IPV6-TCP-MIB DEFINITIONS ::= BEGIN


IMPORTS
   MODULE-COMPLIANCE, OBJECT-GROUP      FROM SNMPv2-CONF
   MODULE-IDENTITY, OBJECT-TYPE,
   mib-2, experimental                  FROM SNMPv2-SMI
   Ipv6Address, Ipv6IfIndexOrZero       FROM IPV6-TC;

ipv6TcpMIB MODULE-IDENTITY
   LAST-UPDATED "9801290000Z"
   ORGANIZATION "IETF IPv6 MIB Working Group"
   CONTACT-INFO
        "       Mike Daniele

                Postal: Compaq Computer Corporation
                        110 Spitbrook Rd
                        Nashua, NH 03062.
                        US

                Phone:  +1 603 884 1423
                Email:  daniele@zk3.dec.com"
   DESCRIPTION
        "The MIB module for entities implementing TCP over IPv6."
   ::= { experimental 86 }






-- objects specific to TCP for IPv6

tcp      OBJECT IDENTIFIER ::= { mib-2 6 }

-- the TCP over IPv6 Connection table

-- This connection table contains information about this
-- entity's existing TCP connections between IPv6 endpoints.
-- Only connections between IPv6 addresses are contained in
-- this table.  This entity's connections between IPv4
-- endpoints are contained in tcpConnTable.

ipv6TcpConnTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF Ipv6TcpConnEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
        "A table containing TCP connection-specific information,
         for only those connections whose endpoints are IPv6 addresses."
   ::= { tcp 16 }

ipv6TcpConnEntry OBJECT-TYPE
   SYNTAX      Ipv6TcpConnEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
        "A conceptual row of the ipv6TcpConnTable containing
         information about a particular current TCP connection.
         Each row of this table is transient, in that it ceases to
         exist when (or soon after) the connection makes the transition
         to the CLOSED state.

         Note that conceptual rows in this table require an additional
         index object compared to tcpConnTable, since IPv6 addresses
         are not guaranteed to be unique on the managed node."
   INDEX   { ipv6TcpConnLocalAddress,
             ipv6TcpConnLocalPort,
             ipv6TcpConnRemAddress,
             ipv6TcpConnRemPort,
             ipv6TcpConnIfIndex }
   ::= { ipv6TcpConnTable 1 }

Ipv6TcpConnEntry ::=
   SEQUENCE { ipv6TcpConnLocalAddress    Ipv6Address,
              ipv6TcpConnLocalPort       INTEGER (0..65535),
              ipv6TcpConnRemAddress      Ipv6Address,
              ipv6TcpConnRemPort         INTEGER (0..65535),
              ipv6TcpConnIfIndex         Ipv6IfIndexOrZero,





              ipv6TcpConnState           INTEGER }

ipv6TcpConnLocalAddress OBJECT-TYPE
   SYNTAX     Ipv6Address
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
        "The local IPv6 address for this TCP connection. In
         the case of a connection in the listen state which
         is willing to accept connections for any IPv6
         address associated with the managed node, the value
         ::0 is used."
   ::= { ipv6TcpConnEntry 1 }

ipv6TcpConnLocalPort OBJECT-TYPE
   SYNTAX     INTEGER (0..65535)
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
        "The local port number for this TCP connection."
   ::= { ipv6TcpConnEntry 2 }

ipv6TcpConnRemAddress OBJECT-TYPE
   SYNTAX     Ipv6Address
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
        "The remote IPv6 address for this TCP connection."
   ::= { ipv6TcpConnEntry 3 }

ipv6TcpConnRemPort OBJECT-TYPE
   SYNTAX     INTEGER (0..65535)
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
        "The remote port number for this TCP connection."
   ::= { ipv6TcpConnEntry 4 }

ipv6TcpConnIfIndex OBJECT-TYPE
   SYNTAX     Ipv6IfIndexOrZero
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
        "An index object used to disambiguate conceptual rows in
         the table, since the connection 4-tuple may not be unique.

         If the connection's remote address (ipv6TcpConnRemAddress)
         is a link-local address and the connection's local address





         (ipv6TcpConnLocalAddress) is not a link-local address, this
         object identifies a local interface on the same link as
         the connection's remote link-local address.

         Otherwise, this object identifies the local interface that
         is associated with the ipv6TcpConnLocalAddress for this
         TCP connection.  If such a local interface cannot be determined,
         this object should take on the value 0.  (A possible example
         of this would be if the value of ipv6TcpConnLocalAddress is ::0.)

         The interface identified by a particular non-0 value of this
         index is the same interface as identified by the same value
         of ipv6IfIndex.

         The value of this object must remain constant during the life
         of the TCP connection."
   ::= { ipv6TcpConnEntry 5 }

ipv6TcpConnState OBJECT-TYPE
   SYNTAX     INTEGER {
        closed(1),
        listen(2),
        synSent(3),
        synReceived(4),
        established(5),
        finWait1(6),
        finWait2(7),
        closeWait(8),
        lastAck(9),
        closing(10),
        timeWait(11),
        deleteTCB(12) }
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
        "The state of this TCP connection.

         The only value which may be set by a management station is
         deleteTCB(12).  Accordingly, it is appropriate for an agent
         to return an error response (`badValue' for SNMPv1, 'wrongValue'
         for SNMPv2) if a management station attempts to set this
         object to any other value.

         If a management station sets this object to the value
         deleteTCB(12), then this has the effect of deleting the TCB
         (as defined in RFC 793) of the corresponding connection on
         the managed node, resulting in immediate termination of the
         connection.





         As an implementation-specific option, a RST segment may be
         sent from the managed node to the other TCP endpoint (note
         however that RST segments are not sent reliably)."
   ::= { ipv6TcpConnEntry 6 }

--
-- conformance information
--

ipv6TcpConformance OBJECT IDENTIFIER ::= { ipv6TcpMIB 2 }

ipv6TcpCompliances OBJECT IDENTIFIER ::= { ipv6TcpConformance 1 }
ipv6TcpGroups      OBJECT IDENTIFIER ::= { ipv6TcpConformance 2 }

-- compliance statements

ipv6TcpCompliance MODULE-COMPLIANCE
   STATUS  current
   DESCRIPTION
        "The compliance statement for SNMPv2 entities which
         implement TCP over IPv6."
   MODULE  -- this module
   MANDATORY-GROUPS { ipv6TcpGroup }
   ::= { ipv6TcpCompliances 1 }

ipv6TcpGroup OBJECT-GROUP
   OBJECTS   { -- these are defined in this module
               -- ipv6TcpConnLocalAddress (not-accessible)
               -- ipv6TcpConnLocalPort (not-accessible)
               -- ipv6TcpConnRemAddress (not-accessible)
               -- ipv6TcpConnRemPort (not-accessible)
               -- ipv6TcpConnIfIndex (not-accessible)
               ipv6TcpConnState }
   STATUS    current
   DESCRIPTION
        "The group of objects providing management of
         TCP over IPv6."
   ::= { ipv6TcpGroups 1 }

END












