SNMP-USM-DH-OBJECTS-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    -- OBJECT-IDENTITY,
    experimental, Integer32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    usmUserEntry
        FROM SNMP-USER-BASED-SM-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB;

snmpUsmDHObjectsMIB MODULE-IDENTITY
    LAST-UPDATED "200003060000Z"  -- 6 March 2000, Midnight
    ORGANIZATION "Excite@Home"
    CONTACT-INFO "Author: Mike StJohns
                  Postal: Excite@Home
                          450 Broadway
                          Redwood City, CA 94063
                  Email:  stjohns@corp.home.net
                  Phone:  +1-650-556-5368"

    DESCRIPTION
        "The management information definitions for providing forward
    secrecy for key changes for the usmUserTable, and for providing a
    method for 'kickstarting' access to the agent via a Diffie-Helman
    key agreement."

    REVISION     "200003060000Z"
    DESCRIPTION
       "Initial version published as RFC 2786."


    ::= { experimental 101 }  -- IANA DHKEY-CHANGE 101

-- Administrative assignments

usmDHKeyObjects OBJECT IDENTIFIER ::= { snmpUsmDHObjectsMIB 1 }
usmDHKeyConformance OBJECT IDENTIFIER ::= { snmpUsmDHObjectsMIB 2 }

-- Textual conventions






DHKeyChange ::=         TEXTUAL-CONVENTION
    STATUS              current
    DESCRIPTION
        "Upon initialization, or upon creation of a row containing an
    object of this type, and after any successful SET of this value, a
    GET of this value returns 'y' where y = g^xa MOD p, and where g is
    the base from usmDHParameters, p is the prime from
    usmDHParameters, and xa is a new random integer selected by the
    agent in the interval 2^(l-1) <= xa < 2^l < p-1.  'l' is the
    optional privateValueLength from usmDHParameters in bits.  If 'l'
    is omitted, then xa (and xr below) is selected in the interval 0
    <= xa < p-1.  y is expressed as an OCTET STRING 'PV' of length 'k'
    which satisfies

              k
        y =  SUM   2^(8(k-i)) PV'i
             i=1

        where PV1,...,PVk are the octets of PV from first to last, and
        where PV1 <> 0.

    A successful SET consists of the value 'y' expressed as an OCTET
    STRING as above concatenated with the value 'z'(expressed as an
    OCTET STRING in the same manner as y) where z = g^xr MOD p, where
    g, p and l are as above, and where xr is a new random integer
    selected by the manager in the interval 2^(l-1) <= xr < 2^l <
    p-1. A SET to an object of this type will fail with the error
    wrongValue if the current 'y' does not match the 'y' portion of
    the value of the varbind for the object. (E.g. GET yout, SET
    concat(yin, z), yout <> yin).

    Note that the private values xa and xr are never transmitted from
    manager to device or vice versa, only the values y and z.
    Obviously, these values must be retained until a successful SET on
    the associated object.

    The shared secret 'sk' is calculated at the agent as sk = z^xa MOD
    p, and at the manager as sk = y^xr MOD p.

    Each object definition of this type MUST describe how to map from
    the shared secret 'sk' to the operational key value used by the
    protocols and operations related to the object.  In general, if n
    bits of key are required, the author suggests using the n
    right-most bits of the shared secret as the operational key value."
    REFERENCE
        "-- Diffie-Hellman Key-Agreement Standard, PKCS #3;
            RSA Laboratories, November 1993"
    SYNTAX              OCTET STRING





-- Diffie Hellman public values

usmDHPublicObjects      OBJECT IDENTIFIER ::= { usmDHKeyObjects 1 }

usmDHParameters OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS read-write
    STATUS  current
    DESCRIPTION
        "The public Diffie-Hellman parameters for doing a Diffie-Hellman
    key agreement for this device.  This is encoded as an ASN.1
    DHParameter per PKCS #3, section 9.  E.g.

        DHParameter ::= SEQUENCE {
           prime   INTEGER,   -- p
           base    INTEGER,   -- g
           privateValueLength  INTEGER OPTIONAL }


    Implementors are encouraged to use either the values from
    Oakley Group 1  or the values of from Oakley Group 2 as specified
    in RFC-2409, The Internet Key Exchange, Section 6.1, 6.2 as the
    default for this object.  Other values may be used, but the
    security properties of those values MUST be well understood and
    MUST meet the requirements of PKCS #3 for the selection of
    Diffie-Hellman primes.

        In addition, any time usmDHParameters changes, all values of
    type DHKeyChange will change and new random numbers MUST be
    generated by the agent for each DHKeyChange object."
    REFERENCE
        "-- Diffie-Hellman Key-Agreement Standard, PKCS #3,
            RSA Laboratories, November 1993
         -- The Internet Key Exchange, RFC 2409, November 1998,
            Sec 6.1, 6.2"
    ::= { usmDHPublicObjects 1 }

usmDHUserKeyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF UsmDHUserKeyEntry
    MAX-ACCESS not-accessible
    STATUS  current
    DESCRIPTION
        "This table augments and extends the usmUserTable and provides
    4 objects which exactly mirror the objects in that table with the
    textual convention of 'KeyChange'.  This extension allows key
    changes to be done in a manner where the knowledge of the current
    secret plus knowledge of the key change data exchanges (e.g. via
    wiretapping)  will not reveal the new key."





    ::= { usmDHPublicObjects 2 }

usmDHUserKeyEntry OBJECT-TYPE
    SYNTAX  UsmDHUserKeyEntry
    MAX-ACCESS not-accessible
    STATUS  current
    DESCRIPTION
        "A row of DHKeyChange objects which augment or replace the
    functionality of the KeyChange objects in the base table row."
    AUGMENTS { usmUserEntry }
    ::= {usmDHUserKeyTable 1 }

UsmDHUserKeyEntry ::= SEQUENCE {
        usmDHUserAuthKeyChange          DHKeyChange,
    usmDHUserOwnAuthKeyChange   DHKeyChange,
        usmDHUserPrivKeyChange          DHKeyChange,
        usmDHUserOwnPrivKeyChange       DHKeyChange
        }

usmDHUserAuthKeyChange OBJECT-TYPE
    SYNTAX  DHKeyChange
    MAX-ACCESS read-create
    STATUS  current
    DESCRIPTION
        "The object used to change any given user's Authentication Key
    using a Diffie-Hellman key exchange.

    The right-most n bits of the shared secret 'sk', where 'n' is the
    number of bits required for the protocol defined by
    usmUserAuthProtocol, are installed as the operational
    authentication key for this row after a successful SET."
    ::= { usmDHUserKeyEntry 1 }

usmDHUserOwnAuthKeyChange OBJECT-TYPE
    SYNTAX  DHKeyChange
    MAX-ACCESS read-create
    STATUS  current
    DESCRIPTION
        "The object used to change the agents own Authentication Key
    using a Diffie-Hellman key exchange.

    The right-most n bits of the shared secret 'sk', where 'n' is the
    number of bits required for the protocol defined by
    usmUserAuthProtocol, are installed as the operational
    authentication key for this row after a successful SET."
    ::= { usmDHUserKeyEntry 2 }

usmDHUserPrivKeyChange OBJECT-TYPE





    SYNTAX  DHKeyChange
    MAX-ACCESS read-create
    STATUS  current
    DESCRIPTION
        "The object used to change any given user's Privacy Key using
    a Diffie-Hellman key exchange.

    The right-most n bits of the shared secret 'sk', where 'n' is the
    number of bits required for the protocol defined by
    usmUserPrivProtocol, are installed as the operational privacy key
    for this row after a successful SET."
    ::= { usmDHUserKeyEntry 3 }

usmDHUserOwnPrivKeyChange OBJECT-TYPE
    SYNTAX  DHKeyChange
    MAX-ACCESS read-create
    STATUS  current
    DESCRIPTION
        "The object used to change the agent's own Privacy Key using a
    Diffie-Hellman key exchange.

    The right-most n bits of the shared secret 'sk', where 'n' is the
    number of bits required for the protocol defined by
    usmUserPrivProtocol, are installed as the operational privacy key
    for this row after a successful SET."
    ::= { usmDHUserKeyEntry 4 }

usmDHKickstartGroup OBJECT IDENTIFIER ::= { usmDHKeyObjects 2 }

usmDHKickstartTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF UsmDHKickstartEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of mappings between zero or more Diffie-Helman key
    agreement values and entries in the usmUserTable.  Entries in this
    table are created by providing the associated device with a
    Diffie-Helman public value and a usmUserName/usmUserSecurityName
    pair during initialization. How these values are provided is
    outside the scope of this MIB, but could be provided manually, or
    through a configuration file.  Valid public value/name pairs
    result in the creation of a row in this table as well as the
    creation of an associated row (with keys derived as indicated) in
    the usmUserTable.  The actual access the related usmSecurityName
    has is dependent on the entries in the VACM tables.  In general,
    an implementor will specify one or more standard security names
    and will provide entries in the VACM tables granting various
    levels of access to those names.  The actual content of the VACM





    table is beyond the scope of this MIB.

    Note: This table is expected to be readable without authentication
    using the usmUserSecurityName 'dhKickstart'.  See the conformance
    statements for details."
    ::= { usmDHKickstartGroup 1 }

usmDHKickstartEntry OBJECT-TYPE
    SYNTAX      UsmDHKickstartEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION

        "An entry in the usmDHKickstartTable.  The agent SHOULD either
    delete this entry or mark it as inactive upon a successful SET of
    any of the KeyChange-typed objects in the usmUserEntry or upon a
    successful SET of any of the DHKeyChange-typed objects in the
    usmDhKeyChangeEntry where the related usmSecurityName (e.g. row of
    usmUserTable or row of ushDhKeyChangeTable) equals this entry's
    usmDhKickstartSecurityName.  In otherwords, once you've changed
    one or more of the keys for a row in usmUserTable with a
    particular security name, the row in this table with that same
    security name is no longer useful or meaningful."

    INDEX   { usmDHKickstartIndex }
    ::= {usmDHKickstartTable 1 }

UsmDHKickstartEntry ::= SEQUENCE  {
        usmDHKickstartIndex     Integer32,
        usmDHKickstartMyPublic  OCTET STRING,
        usmDHKickstartMgrPublic OCTET STRING,
        usmDHKickstartSecurityName      SnmpAdminString
        }

usmDHKickstartIndex OBJECT-TYPE
    SYNTAX      Integer32  (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Index value for this row."
    ::= { usmDHKickstartEntry 1 }

usmDHKickstartMyPublic OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The agent's Diffie-Hellman public value for this row.  At





    initialization, the agent generates a random number and derives
    its public value from that number.  This public value is published
    here.  This public value 'y' equals g^r MOD p where g is the from
    the set of Diffie-Hellman parameters, p is the prime from those
    parameters, and r is a random integer selected by the agent in the
    interval 2^(l-1) <= r < p-1 < 2^l.  If l is unspecified, then r is
    a random integer selected in the interval 0 <= r < p-1

    The public value is expressed as an OCTET STRING 'PV' of length
    'k' which satisfies

              k
        y =  SUM   2^(8(k-i)) PV'i
             i = 1

        where PV1,...,PVk are the octets of PV from first to last, and
        where PV1 != 0.


    The following DH parameters (Oakley group #2, RFC 2409, sec 6.1,
    6.2) are used for this object:

    g = 2
    p = FFFFFFFF FFFFFFFF C90FDAA2 2168C234 C4C6628B 80DC1CD1
        29024E08 8A67CC74 020BBEA6 3B139B22 514A0879 8E3404DD
        EF9519B3 CD3A431B 302B0A6D F25F1437 4FE1356D 6D51C245
        E485B576 625E7EC6 F44C42E9 A637ED6B 0BFF5CB6 F406B7ED
        EE386BFB 5A899FA5 AE9F2411 7C4B1FE6 49286651 ECE65381
        FFFFFFFF FFFFFFFF
    l=1024
    "
    REFERENCE
        "-- Diffie-Hellman Key-Agreement Standard, PKCS#3v1.4;
            RSA Laboratories, November 1993
         -- The Internet Key Exchange, RFC2409;
            Harkins, D., Carrel, D.; November 1998"
    ::= { usmDHKickstartEntry 2 }

usmDHKickstartMgrPublic OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION

        "The manager's Diffie-Hellman public value for this row.  Note
    that this value is not set via the SNMP agent, but may be set via
    some out of band method, such as the device's configuration file.






    The manager calculates this value in the same manner and using the
    same parameter set as the agent does.  E.g. it selects a random
    number 'r', calculates y = g^r mod p and provides 'y' as the
    public number expressed as an OCTET STRING.  See
    usmDHKickstartMyPublic for details.

    When this object is set with a valid value during initialization,
    a row is created in the usmUserTable with the following values:

    usmUserEngineID             localEngineID
    usmUserName                 [value of usmDHKickstartSecurityName]
    usmUserSecurityName         [value of usmDHKickstartSecurityName]
    usmUserCloneFrom            ZeroDotZero
    usmUserAuthProtocol         usmHMACMD5AuthProtocol
    usmUserAuthKeyChange        -- derived from set value
    usmUserOwnAuthKeyChange     -- derived from set value
    usmUserPrivProtocol         usmDESPrivProtocol
    usmUserPrivKeyChange        -- derived from set value
    usmUserOwnPrivKeyChange     -- derived from set value
    usmUserPublic               ''
    usmUserStorageType          permanent
    usmUserStatus               active

    A shared secret 'sk' is calculated at the agent as sk =
    mgrPublic^r mod p where r is the agents random number and p is the
    DH prime from the common parameters.  The underlying privacy key
    for this row is derived from sk by applying the key derivation
    function PBKDF2 defined in PKCS#5v2.0 with a salt of 0xd1310ba6,
    and iterationCount of 500, a keyLength of 16 (for
    usmDESPrivProtocol), and a prf (pseudo random function) of
    'id-hmacWithSHA1'.  The underlying authentication key for this row
    is derived from sk by applying the key derivation function PBKDF2
    with a salt of 0x98dfb5ac , an interation count of 500, a
    keyLength of 16 (for usmHMAC5AuthProtocol), and a prf of
    'id-hmacWithSHA1'.  Note: The salts are the first two words in the
    ks0 [key schedule 0] of the BLOWFISH cipher from 'Applied
    Cryptography' by Bruce Schnier - they could be any relatively
    random string of bits.

    The manager can use its knowledge of its own random number and the
    agent's public value to kickstart its access to the agent in a
    secure manner.  Note that the security of this approach is
    directly related to the strength of the authorization security of
    the out of band provisioning of the managers public value
    (e.g. the configuration file), but is not dependent at all on the
    strength of the confidentiality of the out of band provisioning
    data."
    REFERENCE





        "-- Password-Based Cryptography Standard, PKCS#5v2.0;
            RSA Laboratories, March 1999
         -- Applied Cryptography, 2nd Ed.; B. Schneier,
            Counterpane Systems; John Wiley & Sons, 1996"
    ::= { usmDHKickstartEntry 3 }

usmDHKickstartSecurityName OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The usmUserName and usmUserSecurityName in the usmUserTable
    associated with this row.  This is provided in the same manner and
    at the same time as the usmDHKickstartMgrPublic value -
    e.g. possibly manually, or via the device's configuration file."
    ::= { usmDHKickstartEntry 4 }

-- Conformance Information

usmDHKeyMIBCompliances  OBJECT IDENTIFIER ::= { usmDHKeyConformance 1 }
usmDHKeyMIBGroups       OBJECT IDENTIFIER ::= { usmDHKeyConformance 2 }

-- Compliance statements

usmDHKeyMIBCompliance   MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for this module."
    MODULE
        GROUP usmDHKeyMIBBasicGroup
        DESCRIPTION
        "This group MAY be implemented by any agent which
        implements the usmUserTable and which wishes to provide the
        ability to change user and agent authentication and privacy
        keys via Diffie-Hellman key exchanges."

        GROUP usmDHKeyParamGroup
        DESCRIPTION
            "This group MUST be implemented by any agent which
        implements a MIB containing the DHKeyChange Textual
        Convention defined in this module."

        GROUP usmDHKeyKickstartGroup
        DESCRIPTION
            "This group MAY be implemented by any agent which
        implements the usmUserTable and which wishes the ability to
        populate the USM table based on out-of-band provided DH
        ignition values.





             Any agent implementing this group is expected to provide
        preinstalled entries in the vacm tables as follows:

             In the usmUserTable: This entry allows access to the
        system and dhKickstart groups

        usmUserEngineID         localEngineID
        usmUserName             'dhKickstart'
        usmUserSecurityName     'dhKickstart'
        usmUserCloneFrom        ZeroDotZero
        usmUserAuthProtocol     none
        usmUserAuthKeyChange    ''
        usmUserOwnAuthKeyChange ''
        usmUserPrivProtocol     none
        usmUserPrivKeyChange    ''
        usmUserOwnPrivKeyChange ''
        usmUserPublic           ''
        usmUserStorageType      permanent
        usmUserStatus           active

            In the vacmSecurityToGroupTable: This maps the initial
        user into the accessible objects.

        vacmSecurityModel               3 (USM)
        vacmSecurityName                'dhKickstart'
        vacmGroupName                   'dhKickstart'
        vacmSecurityToGroupStorageType  permanent
        vacmSecurityToGroupStatus       active

            In the vacmAccessTable: Group name to view name translation.

        vacmGroupName                   'dhKickstart'
    vacmAccessContextPrefix             ''
        vacmAccessSecurityModel         3 (USM)
        vacmAccessSecurityLevel         noAuthNoPriv
        vacmAccessContextMatch          exact
        vacmAccessReadViewName          'dhKickRestricted'
        vacmAccessWriteViewName         ''
        vacmAccessNotifyViewName        'dhKickRestricted'
        vacmAccessStorageType           permanent
        vacmAccessStatus                active

            In the vacmViewTreeFamilyTable: Two entries to allow the
        initial entry to access the system and kickstart groups.

        vacmViewTreeFamilyViewName      'dhKickRestricted'
        vacmViewTreeFamilySubtree       1.3.6.1.2.1.1  (system)
        vacmViewTreeFamilyMask          ''





        vacmViewTreeFamilyType          1
        vacmViewTreeFamilyStorageType   permanent
        vacmViewTreeFamilyStatus        active

        vacmViewTreeFamilyViewName      'dhKickRestricted'
        vacmViewTreeFamilySubtree         (usmDHKickstartTable OID)
        vacmViewTreeFamilyMask          ''
        vacmViewTreeFamilyType          1
        vacmViewTreeFamilyStorageType   permanent
        vacmViewTreeFamilyStatus        active
        "

        OBJECT usmDHParameters
        MIN-ACCESS      read-only
        DESCRIPTION
            "It is compliant to implement this object as read-only for
        any device."

    ::= { usmDHKeyMIBCompliances 1 }

-- Units of Compliance

usmDHKeyMIBBasicGroup OBJECT-GROUP
    OBJECTS     {
                  usmDHUserAuthKeyChange,
                  usmDHUserOwnAuthKeyChange,
                  usmDHUserPrivKeyChange,
                  usmDHUserOwnPrivKeyChange
                }
    STATUS      current
    DESCRIPTION
        ""
    ::= { usmDHKeyMIBGroups 1 }

usmDHKeyParamGroup OBJECT-GROUP
    OBJECTS     {
                  usmDHParameters
                }
    STATUS      current
    DESCRIPTION
        "The mandatory object for all MIBs which use the DHKeyChange
    textual convention."
    ::= { usmDHKeyMIBGroups 2 }

usmDHKeyKickstartGroup OBJECT-GROUP
    OBJECTS     {
                  usmDHKickstartMyPublic,
                  usmDHKickstartMgrPublic,





                  usmDHKickstartSecurityName
                }
    STATUS      current
    DESCRIPTION
        "The objects used for kickstarting one or more SNMPv3 USM
    associations via a configuration file or other out of band,
    non-confidential access."
    ::= { usmDHKeyMIBGroups 3 }


END


