ADSL2-LINE-MIB DEFINITIONS ::= BEGIN


   IMPORTS
      MODULE-IDENTITY,
      OBJECT-TYPE,
      transmission,
      Unsigned32,
      NOTIFICATION-TYPE,
      Integer32,
      Counter32
         FROM SNMPv2-SMI

      ifIndex
         FROM IF-MIB

      TruthValue,
      RowStatus
         FROM SNMPv2-TC

      SnmpAdminString
         FROM SNMP-FRAMEWORK-MIB

      HCPerfIntervalThreshold,
      HCPerfTimeElapsed
         FROM  HC-PerfHist-TC-MIB   -- [RFC3705]

      Adsl2Unit,
      Adsl2Direction,
      Adsl2TransmissionModeType,
      Adsl2RaMode,
      Adsl2InitResult,
      Adsl2OperationModes,
      Adsl2PowerMngState,
      Adsl2ConfPmsForce,
      Adsl2LConfProfPmMode,
      Adsl2LineLdsf,
      Adsl2LdsfResult,
      Adsl2SymbolProtection,
      Adsl2MaxBer,
      Adsl2ScMaskDs,
      Adsl2ScMaskUs,
      Adsl2RfiDs,
      Adsl2PsdMaskDs,
      Adsl2PsdMaskUs,
      Adsl2Tssi,
      Adsl2LastTransmittedState,
      Adsl2LineStatus,
      Adsl2ChAtmStatus,





      Adsl2ChPtmStatus
             FROM   ADSL2-LINE-TC-MIB       -- [This document]

      MODULE-COMPLIANCE,
      OBJECT-GROUP,
      NOTIFICATION-GROUP
         FROM SNMPv2-CONF;

   adsl2MIB MODULE-IDENTITY
      LAST-UPDATED "200610040000Z" -- October 4th, 2006
      ORGANIZATION "ADSLMIB Working Group"
      CONTACT-INFO "WG-email:  adslmib@ietf.org
      Info:      https://www1.ietf.org/mailman/listinfo/adslmib


                Chair:     Mike Sneed
                           Sand Channel Systems
                Postal:    P.O. Box 37324
                           Raleigh NC 27627-732
                Email:     sneedmike@hotmail.com
                Phone:     +1 206 600 7022

                Co-Chair & Co-editor:
                           Menachem Dodge
                           ECI Telecom Ltd.
                Postal:    30 Hasivim St.
                           Petach Tikva 49517,
                           Israel.
                Email:     mbdodge@ieee.org
                Phone:     +972 3 926 8421

                Co-editor: Moti Morgenstern
                           ECI Telecom Ltd.
                Postal:    30 Hasivim St.
                           Petach Tikva 49517,
                           Israel.
                Email:     moti.morgenstern@ecitele.com
                Phone:     +972 3 926 6258

                Co-editor: Scott Baillie
                           NEC Australia
                Postal:    649-655 Springvale Road,
                           Mulgrave, Victoria 3170,
                           Australia.
                Email:     scott.baillie@nec.com.au
                Phone:     +61 3 9264 3986

                Co-editor: Umberto Bonollo





                           NEC Australia
                Postal:    649-655 Springvale Road,
                           Mulgrave, Victoria 3170,
                           Australia.
                Email:     umberto.bonollo@nec.com.au
                Phone:     +61 3 9264 3385
               "
      DESCRIPTION
           "
            This document defines a Management Information Base (MIB)
            module for use with network management protocols in the
            Internet community for the purpose of managing ADSL, ADSL2,
            and ADSL2+ lines.  The MIB module described in RFC 2662
            [RFC2662] describes objects used for managing Asymmetric
            Bit-Rate DSL (ADSL) interfaces per [T1E1.413], [G.992.1],
            and [G.992.2].  These object descriptions are based upon the
            specifications for the ADSL Embedded Operations Channel
            (EOC) as defined in American National Standards Institute
            (ANSI) T1E1.413/1995 [T1E1.413] and International
            Telecommunication Union (ITU-T) G.992.1  [G.992.1] and
            G.992.2 [G.992.2].

            This document does not obsolete RFC 2662 [RFC2662], but
            rather provides a more comprehensive management model that
            includes the ADSL2 and ADSL2+ technologies per G.992.3,
            G.992.4, and G.992.5 ([G.992.3], [G.992.4], and [G.992.5],
            respectively).  In addition, objects have been added to
            improve the management of ADSL, ADSL2, and ADSL2+ lines.

           Additionally, the management framework for New Generation
           ADSL lines specified by the Digital Subscriber Line Forum
           (DSLF) has been taken into consideration [TR-90].  That
           framework is based on ITU-T G.997.1 standard [G.997.1] as
           well as two amendments: [G.997.1am1] and [G.997.1am2].

           Note that the revised ITU-T G.997.1 standard also refers to
           the next generation of VDSL technology, known as VDSL2, per
           ITU-T G.993.2 [G.993.2].  However, managing VDSL2 lines is
           currently beyond the scope of this document.

           The MIB module is located in the MIB tree under MIB 2
           transmission, as discussed in the IANA Considerations section
           of this document.

           Copyright (C) The Internet Society (2006).  This version of
           this MIB module is part of RFC 4706: see the RFC itself for
           full legal notices."






      REVISION "200610040000Z" -- October 4th, 2006
      DESCRIPTION "Initial version, published as RFC 4706."
         ::= { transmission 238 }

     adsl2            OBJECT IDENTIFIER ::= { adsl2MIB 1 }
     ------------------------------------------------
     adsl2Line          OBJECT IDENTIFIER ::= { adsl2 1 }
     adsl2Status        OBJECT IDENTIFIER ::= { adsl2 2 }
     adsl2Inventory     OBJECT IDENTIFIER ::= { adsl2 3 }
     adsl2PM            OBJECT IDENTIFIER ::= { adsl2 4 }
     adsl2Profile       OBJECT IDENTIFIER ::= { adsl2 5 }
     adsl2Scalar        OBJECT IDENTIFIER ::= { adsl2 6 }
     adsl2Notifications OBJECT IDENTIFIER ::= { adsl2 0 }
     adsl2Conformance   OBJECT IDENTIFIER ::= { adsl2 7 }
     ------------------------------------------------
     adsl2PMLine      OBJECT IDENTIFIER ::= { adsl2PM 1 }
     adsl2PMChannel   OBJECT IDENTIFIER ::= { adsl2PM 2 }
     ------------------------------------------------
     adsl2ProfileLine      OBJECT IDENTIFIER ::= { adsl2Profile 1 }
     adsl2ProfileChannel   OBJECT IDENTIFIER ::= { adsl2Profile 2 }
     adsl2ProfileAlarmConf OBJECT IDENTIFIER ::= { adsl2Profile 3 }
     ------------------------------------------------
     adsl2ScalarSC         OBJECT IDENTIFIER ::= { adsl2Scalar 1 }
     ------------------------------------------------


   ------------------------------------------------
   --          adsl2LineTable                    --
   ------------------------------------------------
   adsl2LineTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2LineEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineTable contains configuration,
          command, and status parameters of the ADSL2 line.
          The index of this table is an interface index where the
          interface has an ifType of adsl2plus(238).

          Several objects in this table MUST be maintained in a
          persistent manner."
      ::= { adsl2Line 1 }

   adsl2LineEntry  OBJECT-TYPE
      SYNTAX      Adsl2LineEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION





         "The table adsl2LineTable contains configuration,
         commands, and status parameters of the ADSL2 line"
      INDEX  { ifIndex }
      ::= { adsl2LineTable 1 }

   Adsl2LineEntry  ::=
      SEQUENCE {
         adsl2LineCnfgTemplate            SnmpAdminString,
         adsl2LineAlarmCnfgTemplate       SnmpAdminString,
         adsl2LineCmndConfPmsf            Adsl2ConfPmsForce,
         adsl2LineCmndConfLdsf            Adsl2LineLdsf,
         adsl2LineCmndConfLdsfFailReason  Adsl2LdsfResult,
         adsl2LineCmndAutomodeColdStart   TruthValue,
         adsl2LineStatusAtuTransSys       Adsl2TransmissionModeType,
         adsl2LineStatusPwrMngState       Adsl2PowerMngState,
         adsl2LineStatusInitResult        Adsl2InitResult,
         adsl2LineStatusLastStateDs       Adsl2LastTransmittedState,
         adsl2LineStatusLastStateUs       Adsl2LastTransmittedState,
         adsl2LineStatusAtur              Adsl2LineStatus,
         adsl2LineStatusAtuc              Adsl2LineStatus,
         adsl2LineStatusLnAttenDs         Unsigned32,
         adsl2LineStatusLnAttenUs         Unsigned32,
         adsl2LineStatusSigAttenDs        Unsigned32,
         adsl2LineStatusSigAttenUs        Unsigned32,
         adsl2LineStatusSnrMarginDs       Integer32,
         adsl2LineStatusSnrMarginUs       Integer32,
         adsl2LineStatusAttainableRateDs  Unsigned32,
         adsl2LineStatusAttainableRateUs  Unsigned32,
         adsl2LineStatusActPsdDs          Integer32,
         adsl2LineStatusActPsdUs          Integer32,
         adsl2LineStatusActAtpDs          Integer32,
         adsl2LineStatusActAtpUs          Integer32
      }

   adsl2LineCnfgTemplate  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2 Line
          Configuration Templates Table, (adsl2LineConfTemplateTable),
          which applies for this ADSL2 line.

          This object MUST be maintained in a persistent manner."
      REFERENCE    "DSL Forum TR-90, paragraph 5.1.1"
      DEFVAL       { "DEFVAL" }
      ::= { adsl2LineEntry 1 }






   adsl2LineAlarmCnfgTemplate  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2 Line
         Alarm Configuration Template Table,
         (adsl2LineAlarmConfTemplateTable), which applies to this ADSL2
         line.

         This object MUST be maintained in a persistent manner."
      REFERENCE    "DSL Forum TR-90, paragraph 5.1.1"
      DEFVAL       { "DEFVAL" }
      ::= { adsl2LineEntry 2 }

   adsl2LineCmndConfPmsf  OBJECT-TYPE
      SYNTAX      Adsl2ConfPmsForce
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "Power management state forced.  Defines the line states to be
          forced by the near-end ATU on this line.  The various possible
          values are:
             l3toL0(0),
             l0toL2(2), or
             l0orL2toL3(3).

          This object MUST be maintained in a persistent manner."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.1.3"
      DEFVAL       { l3toL0 }
      ::= { adsl2LineEntry 3 }

   adsl2LineCmndConfLdsf  OBJECT-TYPE
      SYNTAX      Adsl2LineLdsf
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "Loop diagnostics mode forced (LDSF).  Defines whether the line
          should be forced into the loop diagnostics mode by the
          near-end ATU on this line or only be responsive to loop
          diagnostics initiated by the far-end ATU.

          This object MUST be maintained in a persistent manner.
          However, in case the operator forces loop diagnostics mode
          then the access node should reset the object (inhibit) when
          loop diagnostics mode procedures are completed."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.1.8"
      DEFVAL       { inhibit }





      ::= { adsl2LineEntry 4 }

   adsl2LineCmndConfLdsfFailReason  OBJECT-TYPE
      SYNTAX      Adsl2LdsfResult
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The status of the recent occasion the Loop diagnostics mode
          forced (LDSF) was issued for the associated line.  Possible
          values are:
             none(1)         - The default value in case LDSF was never
                               requested for the associated line.
             success(2)      - The recent command completed
                               successfully.
             inProgress(3)   - The Loop Diagnostics process is in
                               progress.
             unsupported(4)  - The NE or the line card doesn't support
                               LDSF.
             cannotRun(5)    - The NE cannot initiate the command, due
                               to a nonspecific reason.
             aborted(6)      - The Loop Diagnostics process aborted.
             failed(7)       - The Loop Diagnostics process failed.
             illegalMode(8)  - The NE cannot initiate the command, due
                               to the specific mode of the relevant
                               line.
             adminUp(9)      - The NE cannot initiate the command, as
                               the relevant line is administratively
                               'Up'.
             tableFull(10)   - The NE cannot initiate the command, due
                               to reaching the maximum number of rows
                               in the results table.
             noResources(11) - The NE cannot initiate the command, due
                               to lack of internal memory resources."
      DEFVAL       { none }
      ::= { adsl2LineEntry 5 }

      adsl2LineCmndAutomodeColdStart   OBJECT-TYPE
         SYNTAX      TruthValue
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
            "Automode cold start forced.  This parameter is defined
             in order to improve testing of the performance of ATUs
             supporting automode when it is enabled in the MIB.
             Change the value of this parameter to 'true' indicates
             a change in loop conditions applied to the devices under
             test.  The ATUs shall reset any historical information
             used for automode and for shortening G.994.1 handshake





             and initialization.

             Automode is the case where multiple operation-modes are
             enabled through the adsl2LConfProfAtuTransSysEna object
             in the line configuration profile being used for the
             ADSL line, and where the selection of the actual
             operation-mode depends not only on the common
             capabilities of both ATUs (as exchanged in G.994.1), but
             also on achievable data rates under given loop
             conditions.

             This object MUST be maintained in a persistent manner."

         REFERENCE    "ITU-T G.997.1 (amendment 1), 7.3.1.1.10"
         DEFVAL       { false }
         ::= { adsl2LineEntry 6 }


   adsl2LineStatusAtuTransSys  OBJECT-TYPE
      SYNTAX      Adsl2TransmissionModeType
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The ATU Transmission System (ATS) in use.
          It is coded in a bit-map representation with only a single bit
          set to '1' (the selected coding for the ADSL line).  This
          parameter may be derived from the handshaking procedures
          defined in Recommendation G.994.1.  A set of ADSL2 line
          transmission modes, with one bit per mode."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.1.1"
      ::= { adsl2LineEntry 7 }

   adsl2LineStatusPwrMngState  OBJECT-TYPE
      SYNTAX      Adsl2PowerMngState
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The current power management state.  One of four possible
          power management states:
             L0 - Synchronized and full transmission (i.e., Showtime).
             L1 - Low Power with reduced net data rate (G.992.2 only).
             L2 - Low Power with reduced net data rate (G.992.3 and
                  G.992.4 only).
             L3 - No power.
         The various possible values are: l0(1), l1(2), l2(3), or
         l3(4)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.2"
         ::= { adsl2LineEntry 8 }





   adsl2LineStatusInitResult  OBJECT-TYPE
      SYNTAX      Adsl2InitResult
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Indicates the result of the last full initialization performed
          on the line.  It is an enumeration type with the following
          values: noFail(0), configError(1), configNotFeasible(2),
          commFail(3), noPeerAtu(4), or otherCause(5)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.3"
      ::= { adsl2LineEntry 9 }

   adsl2LineStatusLastStateDs  OBJECT-TYPE
      SYNTAX      Adsl2LastTransmittedState
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The last successful transmitted initialization state in
          the downstream direction in the last full initialization
          performed on the line."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.4"
      ::= { adsl2LineEntry 10 }

   adsl2LineStatusLastStateUs  OBJECT-TYPE
      SYNTAX      Adsl2LastTransmittedState
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The last successful transmitted initialization state in the
          upstream direction in the last full initialization performed
          on the line."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.5"
      ::= { adsl2LineEntry 11 }

   adsl2LineStatusAtur  OBJECT-TYPE
      SYNTAX      Adsl2LineStatus
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Indicates current state (existing failures) of the ATU-R.
          This is a bit-map of possible conditions."
      REFERENCE    "ITU-T G.997.1, paragraph 7.1.1.2"
      ::= { adsl2LineEntry 12 }

   adsl2LineStatusAtuc  OBJECT-TYPE
      SYNTAX      Adsl2LineStatus
      MAX-ACCESS  read-only
      STATUS      current





      DESCRIPTION
         "Indicates current state (existing failures) of the ATU-C.
          This is a bit-map of possible conditions."
      REFERENCE    "ITU-T G.997.1, paragraph 7.1.1.1"
      ::= { adsl2LineEntry 13 }

   adsl2LineStatusLnAttenDs  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The measured difference in the total power transmitted by the
          ATU-C and the total power received by the ATU-R over all sub-
          carriers during diagnostics mode and initialization.  It
          ranges from 0 to 1270 units of 0.1 dB (physical values
          are 0 to 127 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the line
          attenuation is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the line
          attenuation measurement is currently unavailable."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.6"
      ::= { adsl2LineEntry 14 }

   adsl2LineStatusLnAttenUs  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The measured difference in the total power transmitted by the
          ATU-R and the total power received by the ATU-C over all sub-
          carriers during diagnostics mode and initialization.
          It ranges from 0 to 1270 units of 0.1 dB (physical values are
          0 to 127 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the line
          attenuation is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the line
          attenuation measurement is currently unavailable."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.7"
      ::= { adsl2LineEntry 15 }

   adsl2LineStatusSigAttenDs  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION





         "The measured difference in the total power transmitted by the
          ATU-C and the total power received by the ATU-R over all sub-
          carriers during Showtime.  It ranges from 0 to 1270 units of
          0.1 dB (physical values are 0 to 127 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the
          signal attenuation is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the
          signal attenuation measurement is currently unavailable."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.8"
      ::= { adsl2LineEntry 16 }

   adsl2LineStatusSigAttenUs  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The measured difference in the total power transmitted by the
          ATU-R and the total power received by the ATU-C over all sub-
          carriers during Showtime.  It ranges from 0 to 1270 units of
          0.1 dB (physical values are 0 to 127 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the
          signal attenuation is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the
          signal attenuation measurement is currently unavailable."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.9"
      ::= { adsl2LineEntry 17 }

   adsl2LineStatusSnrMarginDs  OBJECT-TYPE
      SYNTAX      Integer32 (-640..630 | 2147483646 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Downstream SNR Margin is the maximum increase in dB of the
          noise power received at the ATU-R, such that the BER
          requirements are met for all downstream bearer channels.  It
          ranges from -640 to 630 units of 0.1 dB (physical values are
          -64 to 63 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the
          SNR Margin is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the
          SNR Margin measurement is currently unavailable."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.10"
      ::= { adsl2LineEntry 18 }

   adsl2LineStatusSnrMarginUs  OBJECT-TYPE
      SYNTAX      Integer32 (-640..630 | 2147483646 | 2147483647)





      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Upstream SNR Margin is the maximum increase in dB of the noise
          power received at the ATU-C, such that the BER requirements
          are met for all downstream bearer channels.  It ranges from
          -640 to 630 units of 0.1 dB (physical values are -64 to
          63 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the
          SNR Margin is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the
          SNR Margin measurement is currently unavailable."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.11"
      ::= { adsl2LineEntry 19 }

   adsl2LineStatusAttainableRateDs  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "bits/second"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Maximum Attainable Data Rate Downstream.
          The maximum downstream net data rate currently attainable by
          the ATU-C transmitter and the ATU-R receiver, coded in
          bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.12"
      ::= { adsl2LineEntry 20 }

   adsl2LineStatusAttainableRateUs  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "bits/second"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Maximum Attainable Data Rate Upstream.
          The maximum upstream net data rate currently attainable by the
          ATU-R transmitter and the ATU-C receiver, coded in
          bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.13"
      ::= { adsl2LineEntry 21 }

   adsl2LineStatusActPsdDs OBJECT-TYPE
      SYNTAX      Integer32 (-900..0 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION





         "Actual Power Spectrum Density (PSD) Downstream.  The average
          downstream transmit PSD over the sub-carriers used for
          downstream.  It ranges from -900 to 0 units of 0.1 dB
          (physical values are -90 to 0 dBm/Hz).
          A value of 0x7FFFFFFF (2147483647) indicates the measurement
          is out of range to be represented."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.14"
      ::= { adsl2LineEntry 22 }

   adsl2LineStatusActPsdUs OBJECT-TYPE
      SYNTAX      Integer32 (-900..0 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Actual Power Spectrum Density (PSD) Upstream.  The average
          upstream transmit PSD over the sub-carriers used for upstream.
          It ranges from -900 to 0 units of 0.1 dB (physical values
          are -90 to 0 dBm/Hz).
          A value of 0x7FFFFFFF (2147483647) indicates the measurement
          is out of range to be represented."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.15"
      ::= { adsl2LineEntry 23 }

   adsl2LineStatusActAtpDs  OBJECT-TYPE
      SYNTAX      Integer32 (-310..310 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Actual Aggregate Transmit Power Downstream.  The total amount
          of transmit power delivered by the ATU-C at the U-C reference
          point, at the instant of measurement.  It ranges from -310 to
          310 units of 0.1 dB (physical values are -31 to 31 dBm).
          A value of 0x7FFFFFFF (2147483647) indicates the measurement
          is out of range to be represented."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.16"
      ::= { adsl2LineEntry 24 }

   adsl2LineStatusActAtpUs  OBJECT-TYPE
      SYNTAX      Integer32 (-310..310 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Actual Aggregate Transmit Power Upstream.  The total amount of
          transmit power delivered by the ATU-R at the U-R
          reference point, at the instant of measurement.  It ranges





          from -310 to 310 units of 0.1 dB (physical values are -31
          to 31 dBm).
          A value of 0x7FFFFFFF (2147483647) indicates the measurement
          is out of range to be represented."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.17"
      ::= { adsl2LineEntry 25 }


   ------------------------------------------------
   --        adsl2ChannelStatusTable             --
   ------------------------------------------------
   adsl2ChannelStatusTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2ChannelStatusEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2ChannelStatusTable contains status
          parameters of the ADSL2 channel.  This table contains live
          data from equipment."
      ::= { adsl2Status 1 }

   adsl2ChannelStatusEntry  OBJECT-TYPE
      SYNTAX      Adsl2ChannelStatusEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2ChannelStatusTable contains status
          parameters of the ADSL2 channel.
          The index of this table consists of an interface index, where
          the interface has an ifType value that is applicable
          for a DSL channel, along with a termination unit."
      INDEX  { ifIndex, adsl2ChStatusUnit }
      ::= { adsl2ChannelStatusTable 1 }

   Adsl2ChannelStatusEntry  ::=
      SEQUENCE {
         adsl2ChStatusUnit                Adsl2Unit,
         adsl2ChStatusChannelNum          Unsigned32,
         adsl2ChStatusActDataRate         Unsigned32,
         adsl2ChStatusPrevDataRate        Unsigned32,
         adsl2ChStatusActDelay            Unsigned32,
         adsl2ChStatusAtmStatus           Adsl2ChAtmStatus,
         adsl2ChStatusPtmStatus           Adsl2ChPtmStatus
      }

   adsl2ChStatusUnit  OBJECT-TYPE
      SYNTAX      Adsl2Unit
      MAX-ACCESS  not-accessible





      STATUS      current
      DESCRIPTION
         "The termination unit atuc(1) or atur(2)."
      ::= { adsl2ChannelStatusEntry 1 }

   adsl2ChStatusChannelNum  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Provides the bearer channel number associated with this
          row (i.e., the channel ifIndex).
          This enables determining the channel configuration profile
          and the channel thresholds profile applicable for this
          bearer channel."
      ::= { adsl2ChannelStatusEntry 2 }

   adsl2ChStatusActDataRate  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The actual net data rate that the bearer channel is operating
          at, if in L0 power management state.  In L1 or L2 states, it
          relates to the previous L0 state.  The data rate is coded in
          bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.2.1"
      ::= { adsl2ChannelStatusEntry 3 }

   adsl2ChStatusPrevDataRate  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The previous net data rate that the bearer channel was
          operating at just before the latest rate change event.  This
          could be a full or short initialization, fast retrain, DRA or
          power management transitions, excluding transitions between L0
          state and L1 or L2 states.  The data rate is coded in
          bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.2.2"
      ::= { adsl2ChannelStatusEntry 4 }

   adsl2ChStatusActDelay  OBJECT-TYPE
      SYNTAX      Unsigned32(0..8176)
      UNITS       "milliseconds"





      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The actual one-way interleaving delay introduced by the
          PMS-TC in the direction of the bearer channel, if in L0
          power management state.  In L1 or L2 states, it relates to
          the previous L0 state.  It is coded in ms (rounded to the
          nearest ms)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.2.3"
      ::= { adsl2ChannelStatusEntry 5 }

   adsl2ChStatusAtmStatus  OBJECT-TYPE
      SYNTAX      Adsl2ChAtmStatus
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Indicates the current state (existing failures) of the ADSL
          channel in case its Data Path is ATM.  This is a bit-map of
          possible conditions.  The various bit positions are:
             noDefect(0),
             noCellDelineation(1), or
             lossOfCellDelineation(2).
         In the case where the channel is not an ATM Data Path, the
         object is set to '0'."
      REFERENCE    "ITU-T G.997.1, paragraph 7.1.4"
      ::= { adsl2ChannelStatusEntry 6 }

   adsl2ChStatusPtmStatus  OBJECT-TYPE
      SYNTAX      Adsl2ChPtmStatus
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Indicates the current state (existing failures) of the ADSL
          channel in case its Data Path is PTM.  This is a bit-map of
          possible conditions.  The various bit positions are:
             noDefect(0), or
             outOfSync(1).
         In the case where the channel is not a PTM Data Path, the
         object is set to '0'."
      REFERENCE    "ITU-T G.997.1, paragraph 7.1.5"
      ::= { adsl2ChannelStatusEntry 7 }


   ------------------------------------------------
   --        Scalars that relate to the adsl2SCStatusTable.
   ------------------------------------------------

   adsl2ScalarSCMaxInterfaces  OBJECT-TYPE





      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This value determines the upper size of adsl2SCStatusTable.
          The maximum number of entries in adsl2SCStatusTable is equal
          to two times the value of this attribute."
      ::= { adsl2ScalarSC 1 }

   adsl2ScalarSCAvailInterfaces  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This value determines the amount of space that is
          currently available in adsl2SCStatusTable.
          The number of entries available in adsl2SCStatusTable is equal
          to two times the value of this attribute."
      ::= { adsl2ScalarSC 2 }

   ------------------------------------------------
   --        adsl2SCStatusTable                --
   ------------------------------------------------

   adsl2SCStatusTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2SCStatusEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2SCStatusTable contains status parameters
          of the ADSL2 sub-carriers.  The following points apply to this
          table:
          1.  The main purpose of this table is to hold the results
              of a DELT.
          2.  This table also holds parameters obtained at line
              initialization time.
          3.  The rows in this table are volatile; that is, they are
              lost if the SNMP agent is rebooted.
          4.  Due to the large OCTET STRING attributes in this table,
              the worst case memory requirements for this table are
              very high.  The manager may use the row status attribute
              of this table to delete rows in order to reclaim memory.
          5.  The manager may create rows in this table.  The SNMP
              agent may create rows in this table.  Only the manager
              may delete rows in this table.
          6.  The maximum number of rows allowable in this table is
              indicated by the scalar attribute
              adsl2ScalarSCMaxInterfaces.





              The number of rows available in this table is indicated
              by the scalar attribute adsl2ScalarSCAvailInterfaces.
          7.  The SNMP agent is permitted to create rows in this table
              when a DELT completes successfully or when line
              initialization occurs.  It is not mandatory for the SNMP
              agent to create rows in this table; hence, it may be
              necessary for the manager to create rows in this table
              before any results can be stored.
          8.  If the manager attempts to create a row in this table
              and there are no more rows available, the creation
              attempt will fail, and the response to the SNMP SET PDU
              will contain the error noCreation(11).
          9.  If the SNMP agent attempts to create a row in this table
              and there are no more rows available, the creation
              attempt will fail, and the attribute
              adsl2LineCmndConfLdsfFailReason will indicate the
              reason for the failure.  The failure reason will be either
              tableFull(10) or noResources(11).
          10. An example of use of this table is as follows:
              Step 1. : The DELT is started by setting the
                      : adsl2LineCmndConfLdsf from inhibit to force.
              Step 2. : The DELT completes, and valid data is
                      : available.
              Step 3. : The row in the adsl2SCStatusTable where the
                      : results will be stored does not yet exist so
                      : the SNMP agent attempts to create the row.
              Step 4. : Due to a low memory condition, a row in the
                      : adsl2SCStatusTable table cannot be created at
                      : this time.
              Step 5. : The reason for the failure, tableFull(10), is
                      : indicated in the adsl2LineCmndConfLdsfFailReason
                      : attribute.
          11. Another example of use of this table is as follows :
              Step 1. : The DELT is started by setting the
                      : adsl2LineCmndConfLdsf from inhibit to force.
              Step 2. : The DELT completes and valid data is
                      : available.
              Step 3. : The row in the adsl2SCStatusTable where the
                      : results will be stored does not yet exist so
                      : the SNMP agent attempts to create the row.
              Step 4. : The row creation is successful.
              Step 5. : The value of the attribute
                      : adsl2LineCmndConfLdsfFailReasonreason is set
                      : to success(2).
          12. Another example of use of this table is as follows:
              Step 1. : The manager creates a row in adsl2SCStatusTable
                      : for a particular ADSL2 line.
              Step 2. : The DELT is started on the above-mentioned





                      : line by setting the adsl2LineCmndConfLdsf from
                      : inhibit to force.
              Step 3. : The DELT completes, and valid data is
                      : available.
              Step 4. : The value of the attribute
                      : adsl2LineCmndConfLdsfFailReasonreason is set
                      : to success(2)."
      ::= { adsl2Status 2 }

   adsl2SCStatusEntry  OBJECT-TYPE
      SYNTAX      Adsl2SCStatusEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table Adsl2SCStatusEntry contains status parameters
          of the ADSL2 sub-carriers.
          The index of this table is an interface index where the
          interface has an ifType of adsl2plus(238)."
      INDEX  { ifIndex, adsl2SCStatusDirection }
      ::= { adsl2SCStatusTable 1 }

   Adsl2SCStatusEntry  ::=
      SEQUENCE {
         adsl2SCStatusDirection         Adsl2Direction,
         adsl2SCStatusMtime             Unsigned32,
         adsl2SCStatusSnr               OCTET STRING,
         adsl2SCStatusBitsAlloc         OCTET STRING,
         adsl2SCStatusGainAlloc         OCTET STRING,
         adsl2SCStatusTssi              Adsl2Tssi,
         adsl2SCStatusLinScale          Unsigned32,
         adsl2SCStatusLinReal           OCTET STRING,
         adsl2SCStatusLinImg            OCTET STRING,
         adsl2SCStatusLogMt             Unsigned32,
         adsl2SCStatusLog               OCTET STRING,
         adsl2SCStatusQlnMt             Unsigned32,
         adsl2SCStatusQln               OCTET STRING,
         adsl2SCStatusLnAtten           Unsigned32,
         adsl2SCStatusSigAtten          Unsigned32,
         adsl2SCStatusSnrMargin         Integer32,
         adsl2SCStatusAttainableRate    Unsigned32,
         adsl2SCStatusActAtp            Integer32,
         adsl2SCStatusRowStatus         RowStatus
      }

   adsl2SCStatusDirection  OBJECT-TYPE
      SYNTAX      Adsl2Direction
      MAX-ACCESS  not-accessible
      STATUS      current





      DESCRIPTION
        "The direction of the sub-carrier is either
        upstream or downstream."
        ::= { adsl2SCStatusEntry 1 }

   adsl2SCStatusMtime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "symbols"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "SNR Measurement Time.  The number of symbols used to
         measure the SNR values on the respective transmission
         direction.  It should correspond to the value specified in the
         recommendation (e.g., the number of symbols in 1 second
         time interval for G.992.3).  This parameter corresponds to
         1 second in loop diagnostic procedure and should be updated
         otherwise."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.20.1 (SNRMTds)
                    and paragraph 7.5.1.20.3 (SNRMTus)"
        ::= { adsl2SCStatusEntry 2 }

   adsl2SCStatusSnr  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..512))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The SNR Margin per sub-carrier, expressing the ratio between
         the received signal power and received noise power per
         subscriber.  It is an array of 512 octets, designed for
         supporting up to 512 (downstream) sub-carriers.
         The number of utilized octets on downstream direction depends
         on NSCds, and on upstream direction it depends on NSCus.  This
         value is referred to here as NSC.
         Octet i (0 <= i < NSC) is set to a value in the range 0 to
         254 to indicate that the respective downstream or upstream sub-
         carrier i has SNR of: (-32 + Adsl2SubcarrierSnr(i)/2) in dB
         (i.e., -32 to 95dB).
         The special value 255 means that no measurement could be done
         for the subcarrier because it is out of the PSD mask passband
         or that the noise PSD is out of range to be represented.
         Each value in this array is 8 bits wide."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.20.2 (SNRpsds)
                    and paragraph 7.5.1.20.4 (SNRpsus)"
        ::= { adsl2SCStatusEntry 3 }

   adsl2SCStatusBitsAlloc  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..256))





      UNITS       "bits"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The bits allocation per sub-carrier.  An array of 256 octets
         (512 nibbles), designed for supporting up to 512 (downstream)
         sub-carriers.
         The number of utilized nibbles on downstream direction depends
         on NSCds, and on upstream direction it depends on NSCus.  This
         value is referred to here as NSC.
         Nibble i (0 <= i < NSC) is set to a value in the range 0
         to 15 to indicate that the respective downstream or upstream
         sub-carrier i has the same amount of bits allocation."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.21.1 (BITSpsds)
                    and paragraph 7.5.1.21.2 (BITSpsus)"
        ::= { adsl2SCStatusEntry 4 }

   adsl2SCStatusGainAlloc  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..1024))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The gain allocation per sub-carrier.  An array of 512 16-bits
        values, designed for supporting up to 512 (downstream) sub-
        carriers.
        The number of utilized octets on downstream direction depends
        on NSCds, and on upstream direction it depends on NSCus.  This
        value is referred to here as NSC.
        Value i (0 <= i < NSC) is in the range 0 to 4093 to indicate
        that the respective downstream or upstream sub-carrier i has the
        same amount of gain value.
        The gain value is represented as a multiple of 1/512 on a
        linear scale.  Each value in this array is 16 bits wide and is
        stored in big endian format."
      REFERENCE    "ITU-T G.997.1, paragraph 7.5.1.21.3 (GAINSpsds)
                    and paragraph 7.5.1.21.4 (GAINSpsus)"
        ::= { adsl2SCStatusEntry 5 }

   adsl2SCStatusTssi  OBJECT-TYPE
      SYNTAX      Adsl2Tssi
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The transmit spectrum shaping (TSSi) breakpoints expressed
        as the set of breakpoints exchanged during G.994.1.
        Each breakpoint is a pair of values occupying 3 octets with the
        following structure:
        First 2 octets - Index of the subcarrier used in the context of





                         the breakpoint.
        Third octet    - The shaping parameter at the breakpoint.
        Subcarrier index is an unsigned number in the range 1 to either
        NSCds (downstream direction) or NSCus (upstream direction).
        The shaping parameter value is in the range 0 to 127 (units of
        -0.5dB).  The special value 127 indicates that the subcarrier
        is not transmitted."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.21.5 (TSSpsds)
                  and paragraph 7.5.1.21.6 (TSSpsus)"
        ::= { adsl2SCStatusEntry 6 }

   adsl2SCStatusLinScale  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The scale factor to be applied to the H(f) linear
        representation values for the respective transmission direction.
        This parameter is only available after a loop diagnostic
        procedure."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.18.1 (HLINSCds)
                  and paragraph 7.5.1.18.5 (HLINSCus)"
        ::= { adsl2SCStatusEntry 7 }

   adsl2SCStatusLinReal  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..1024))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "An array of up to 512 complex H(f) linear representation
        values in linear scale for the respective transmission
        direction.  It is designed to support up to 512 (downstream)
        sub-carriers.
        The number of utilized values on downstream direction depends
        on NSCds, and on upstream direction it depends on NSCus.  This
        value is referred to here as NSC.
        Each array entry represents the real component [referred to here
        as a(i)] of Hlin(f = i*Df) value for a particular sub-carrier
        index i (0 <= i < NSC).
        Hlin(f) is represented as ((scale/2^15)*((a(i)+j*b(i))/2^15)),
        where scale is Adsl2SubcarrierLinScale and a(i) and b(i)
        [provided by the Adsl2SubcarrierLinImg object] are in the range
        (-2^15+1) to (+2^15-1).
        A special value a(i)=b(i)= -2^15 indicates that no measurement
        could be done for the subcarrier because it is out of the
        passband or that the attenuation is out of range to be
        represented.  This parameter is only available after a loop
        diagnostic procedure.





        Each value in this array is 16 bits wide and is stored in big
        endian format."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.18.2 (HLINpsds)
                  and paragraph 7.5.1.18.6 (HLINpsds)"
        ::= { adsl2SCStatusEntry 8 }

   adsl2SCStatusLinImg  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..1024))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "An array of up to 512 complex H(f) linear representation
        values in linear scale for the respective transmission
        direction.  It is designed to support up to 512 (downstream)
        sub-carriers.
        The number of utilized values on downstream direction depends
        on NSCds, and on upstream direction it depends on NSCus.  This
        value is referred to here as NSC.
        Each array entry represents the imaginary component [referred
        to here as b(i)] of Hlin(f = i*Df) value for a particular sub-
        carrier index i (0 <= i < NSC).
        Hlin(f) is represented as ((scale/2^15)*((a(i)+j*b(i))/2^15)),
        where scale is Adsl2SubcarrierLinScale and a(i) [provided by
        the Adsl2SubcarrierLinReal object] and b(i) are in the range
        (-2^15+1) to (+2^15-1).
        A special value a(i)=b(i)= -2^15 indicates that no measurement
        could be done for the subcarrier because it is out of the
        passband or that the attenuation is out of range to be
        represented.  This parameter is only available after a loop
        diagnostic procedure.
        Each value in this array is 16 bits wide and is stored in big
        endian format."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.18.2 (HLINpsds)
                  and paragraph 7.5.1.18.6 (HLINpsds)"
        ::= { adsl2SCStatusEntry 9 }

   adsl2SCStatusLogMt  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The number of symbols used to measure the H(f) logarithmic
        measurement values for the respective transmission direction.
        This parameter should correspond to the value specified in the
        recommendation (e.g., the number of symbols in 1 second
        time interval for G.992.3).  This parameter corresponds to 1
        second in loop diagnostic procedure and should be updated in
        initialization"





      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.18.3 (HLOGMTds)
                  and paragraph 7.5.1.18.7 (HLOGMTus)"
        ::= { adsl2SCStatusEntry 10 }

   adsl2SCStatusLog  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..1024))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "An array of up to 512 real H(f) logarithmic representation
         values in dB for the respective transmission direction.  It is
         designed to support up to 512 (downstream) sub-carriers.
         The number of utilized values on downstream direction depends
         on NSCds, and on upstream direction it depends on NSCus.  This
         value is referred to here as NSC.
         Each array entry represents the real Hlog(f = i*Df) value for a
         particular sub-carrier index i, (0 <= i < NSC).
         The real Hlog(f) value is represented as (6-m(i)/10), with m(i)
         in the range 0 to 1022.  A special value m=1023 indicates that
         no measurement could be done for the subcarrier because it is
         out of the passband or that the attenuation is out of range to
         be represented.  This parameter is applicable in loop
         diagnostic procedure and initialization.
         Each value in this array is 16 bits wide and is stored
         in big endian format."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.18.4 (HLOGpsds)
                  and paragraph 7.5.1.18.8 (HLOGpsus)"
        ::= { adsl2SCStatusEntry 11 }

   adsl2SCStatusQlnMt  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The number of symbols used to measure the Quiet Line Noise
         values on the respective transmission direction.  This
         parameter should correspond to the value specified in the
         recommendation (e.g., the number of symbols in 1 second time
         interval for G.992.3).  This parameter corresponds to 1 second
         in loop diagnostic procedure and should be updated in
         initialization "
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.19.1 (QLNMTds)
                  and paragraph 7.5.1.19.3 (QLNMTus)"
        ::= { adsl2SCStatusEntry 12 }

   adsl2SCStatusQln  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..512))
      UNITS       "dBm/Hz"





      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "An array of up to 512 real Quiet Line Noise values in dBm/Hz
        for the respective transmission direction.  It is designed for
        up to 512 (downstream) sub-carriers.
        The number of utilized values on downstream direction depends
        on NSCds, and on upstream direction it depends on NSCus.  This
        value is referred to here as NSC.
        Each array entry represents the QLN(f = i*Df) value for a
        particular sub-carrier index i, (0 <= i < NSC).
        The QLN(f) is represented as ( -23-n(i)/2), with n(i) in the
        range 0 to 254.  A special value n(i)=255 indicates that no
        measurement could be done for the subcarrier because it is out
        of the passband or that the noise PSD is out of range to be
        represented.
        This parameter is applicable in loop diagnostic procedure and
        initialization.  Each value in this array is 8 bits wide."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.19.2 (QLNpsds)
                  and paragraph 7.5.1.19.4 (QLNpsus)"
        ::= { adsl2SCStatusEntry 13 }

   adsl2SCStatusLnAtten  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "When referring to the downstream direction, it is the measured
          difference in the total power transmitted by the ATU-C and the
          total power received by the ATU-R over all sub-carriers during
          diagnostics mode.
          When referring to the upstream direction, it is the measured
          difference in the total power transmitted by the ATU-R and the
          total power received by the ATU-C over all sub-carriers during
          diagnostics mode.
          It ranges from 0 to 1270 units of 0.1 dB (physical values are
          0 to 127 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the line
          attenuation is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the line
          attenuation measurement is unavailable.
          This object reflects the value of the parameter following the
          most recent DELT performed on the associated line.  Once
          the DELT process is over, the parameter no longer changes
          until the row is deleted or a new DELT process is initiated."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.6 (LATNds)
                  and paragraph 7.5.1.7 (LATNus)"





      ::= { adsl2SCStatusEntry 14 }

   adsl2SCStatusSigAtten  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "When referring to the downstream direction, it is the measured
          difference in the total power transmitted by the
          ATU-C and the total power received by the ATU-R over all sub-
          carriers during Showtime after the diagnostics mode.
          When referring to the upstream direction, it is the measured
          difference in the total power transmitted by the
          ATU-R and the total power received by the ATU-C over all sub-
          carriers during Showtime after the diagnostics mode.
          It ranges from 0 to 1270 units of 0.1 dB (physical values
          are 0 to 127 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the
          signal attenuation is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the
          signal attenuation measurement is unavailable.
          This object reflects the value of the parameter following the
          most recent DELT performed on the associated line.  Once
          the DELT process is over, the parameter no longer changes
          until the row is deleted or a new DELT process is initiated."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.8 (SATNds)
                  and paragraph 7.5.1.9 (SATNus)"
      ::= { adsl2SCStatusEntry 15 }

   adsl2SCStatusSnrMargin  OBJECT-TYPE
      SYNTAX      Integer32 (-640..630 | 2147483646 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "SNR Margin is the maximum increase in dB of the noise power
          received at the ATU (ATU-R on downstream direction and ATU-C
          on upstream direction), such that the BER requirements are met
          for all bearer channels received at the ATU.  It ranges from
          -640 to 630 units of 0.1 dB (physical values are -64 to
          63 dB).
          A special value of 0x7FFFFFFF (2147483647) indicates the
          SNR Margin is out of range to be represented.
          A special value of 0x7FFFFFFE (2147483646) indicates the
          SNR Margin measurement is currently unavailable.
          This object reflects the value of the parameter following the
          most recent DELT performed on the associated line.  Once





          the DELT process is over, the parameter no longer changes
          until the row is deleted or a new DELT process is initiated."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.10 (SNRMds)
                  and paragraph 7.5.1.11 (SNRMus)"
      ::= { adsl2SCStatusEntry 16 }

   adsl2SCStatusAttainableRate  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "bits/second"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Maximum Attainable Data Rate.  The maximum net data rate
          currently attainable by the ATU-C transmitter and ATU-R
          receiver (when referring to downstream direction) or by the
          ATU-R transmitter and ATU-C receiver (when referring to
          upstream direction).  Value is coded in bits/second.
          This object reflects the value of the parameter following the
          most recent DELT performed on the associated line.  Once
          the DELT process is over, the parameter no longer changes
          until the row is deleted or a new DELT process is initiated."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.12 (ATTNDRds)
                  and paragraph 7.5.1.13 (ATTNDRus)"
      ::= { adsl2SCStatusEntry 17 }

   adsl2SCStatusActAtp  OBJECT-TYPE
      SYNTAX      Integer32
      UNITS       "0.1 dB"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Actual Aggregate Transmit Power from the ATU (ATU-R on
          downstream direction and ATU-C on upstream direction), at the
          instant of measurement.  It ranges from -310 to 310 units of
          0.1 dB (physical values are -31 to 31 dBm).  A value of all
          1's indicates the measurement is out of range to be
          represented.
          This object reflects the value of the parameter following the
          most recent DELT performed on the associated line.  Once
          the DELT process is over, the parameter no longer changes
          until the row is deleted or a new DELT process is initiated."
      REFERENCE  "ITU-T G.997.1, paragraph 7.5.1.16 (ACTATPds)
                  and paragraph 7.5.1.17 (ACTATPus)"
      ::= { adsl2SCStatusEntry 18 }

   adsl2SCStatusRowStatus  OBJECT-TYPE
      SYNTAX      RowStatus
      MAX-ACCESS  read-create





      STATUS      current
      DESCRIPTION
         "Row Status.  The manager may create and delete rows
          of this table.  Please see the description of
          adsl2SCStatusTable above for more details."
      ::= { adsl2SCStatusEntry 19 }

   ------------------------------------------------
   --        adsl2LineInventoryTable             --
   ------------------------------------------------
   adsl2LineInventoryTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2LineInventoryEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineInventoryTable contains inventory of the
          ADSL2 units."
      ::= { adsl2Inventory 1 }

   adsl2LineInventoryEntry  OBJECT-TYPE
      SYNTAX      Adsl2LineInventoryEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineInventoryTable contains inventory of the
          ADSL2 units.
          The index of this table is an interface index where the
          interface has an ifType of adsl2plus(238)."
      INDEX  { ifIndex, adsl2LInvUnit }
      ::= { adsl2LineInventoryTable 1 }

   Adsl2LineInventoryEntry  ::=
      SEQUENCE {
         adsl2LInvUnit                      Adsl2Unit,
         adsl2LInvG994VendorId              OCTET STRING,
         adsl2LInvSystemVendorId            OCTET STRING,
         adsl2LInvVersionNumber             OCTET STRING,
         adsl2LInvSerialNumber              OCTET STRING,
         adsl2LInvSelfTestResult            Unsigned32,
         adsl2LInvTransmissionCapabilities  Adsl2TransmissionModeType
      }

   adsl2LInvUnit  OBJECT-TYPE
      SYNTAX      Adsl2Unit
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The termination unit atuc(1) or atur(2)."





      ::= { adsl2LineInventoryEntry 1 }

   adsl2LInvG994VendorId  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(8))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The ATU G.994.1 Vendor ID as inserted in the G.994.1 CL/CLR
          message.  It consists of 8 binary octets, including a country
          code followed by a (regionally allocated) provider code, as
          defined in Recommendation T.35."
      REFERENCE    "ITU-T G.997.1, paragraph 7.4"
      ::= { adsl2LineInventoryEntry 2 }

   adsl2LInvSystemVendorId  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(8))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The ATU System Vendor ID (identifies the ATU system
          integrator) as inserted in the Overhead Messages (both ATUs
          for G.992.3 and G.992.4) or in the Embedded Operations
          Channel (only ATU-R in G.992.1 and G.992.2).  It consists of
          8 binary octets, with the same format as used for
          Adsl2InvG994VendorId."
      REFERENCE    "ITU-T G.997.1, paragraph 7.4"
      ::= { adsl2LineInventoryEntry 3 }

   adsl2LInvVersionNumber  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..16))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The ATU version number (vendor-specific information) as
          inserted in the Overhead Messages (both ATUs for G.992.3 and
          G.992.4) or in the Embedded Operations Channel (only ATU-R in
          G.992.1 and G.992.2).  It consists of up to 16 binary octets."
      REFERENCE    "ITU-T G.997.1, paragraph 7.4"
      ::= { adsl2LineInventoryEntry 4 }

   adsl2LInvSerialNumber  OBJECT-TYPE
      SYNTAX      OCTET STRING  (SIZE(0..32))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The ATU serial number (vendor-specific information) as
          inserted in the Overhead Messages (both ATUs for G.992.3 and
          G.992.4) or in the Embedded Operations Channel (only ATU-R in





          G.992.1 and G.992.2).  It is vendor-specific information.  It
          consists of up to 32 ASCII characters."
      REFERENCE    "ITU-T G.997.1, paragraph 7.4"
      ::= { adsl2LineInventoryEntry 5 }

   adsl2LInvSelfTestResult  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The ATU self-test result, coded as a 32-bit value.  The
          most significant octet of the result is '0' if the self-test
          passed, and '1' if the self-test failed.  The interpretation
          of the other octets is vendor discretionary."
      REFERENCE    "ITU-T G.997.1, paragraph 7.4"
      ::= { adsl2LineInventoryEntry 6 }

   adsl2LInvTransmissionCapabilities  OBJECT-TYPE
      SYNTAX      Adsl2TransmissionModeType
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The ATU transmission system capability list of the different
          coding types.  It is coded in a bit-map representation with 1
          or more bits set.  A bit set to '1' means that the ATU
          supports the respective coding.  The value may be derived
          from the handshaking procedures defined in G.994.1.  A set
          of ADSL2 line transmission modes, with one bit per mode."
      REFERENCE    "ITU-T G.997.1, paragraph 7.4"
      ::= { adsl2LineInventoryEntry 7 }


   ------------------------------------------------
   --        adsl2LineConfTemplateTable          --
   ------------------------------------------------
   adsl2LineConfTemplateTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2LineConfTemplateEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineConfTemplateTable contains ADSL2 line
          configuration templates.

          Entries in this table MUST be maintained in a
          persistent manner."
      ::= { adsl2ProfileLine 1 }

   adsl2LineConfTemplateEntry  OBJECT-TYPE





      SYNTAX      Adsl2LineConfTemplateEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineConfTemplateTable contains the ADSL2 line
          configuration template.
          A default template with an index of 'DEFVAL' will
          always exist, and its parameters will be set to vendor-
          specific values, unless otherwise specified in this document."
      INDEX  { adsl2LConfTempTemplateName }
      ::= { adsl2LineConfTemplateTable 1 }

   Adsl2LineConfTemplateEntry  ::=
      SEQUENCE {
         adsl2LConfTempTemplateName      SnmpAdminString,
         adsl2LConfTempLineProfile       SnmpAdminString,
         adsl2LConfTempChan1ConfProfile  SnmpAdminString,
         adsl2LConfTempChan1RaRatioDs    Unsigned32,
         adsl2LConfTempChan1RaRatioUs    Unsigned32,
         adsl2LConfTempChan2ConfProfile  SnmpAdminString,
         adsl2LConfTempChan2RaRatioDs    Unsigned32,
         adsl2LConfTempChan2RaRatioUs    Unsigned32,
         adsl2LConfTempChan3ConfProfile  SnmpAdminString,
         adsl2LConfTempChan3RaRatioDs    Unsigned32,
         adsl2LConfTempChan3RaRatioUs    Unsigned32,
         adsl2LConfTempChan4ConfProfile  SnmpAdminString,
         adsl2LConfTempChan4RaRatioDs    Unsigned32,
         adsl2LConfTempChan4RaRatioUs    Unsigned32,
         adsl2LConfTempRowStatus         RowStatus
      }

   adsl2LConfTempTemplateName  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This object identifies a row in this table."
      REFERENCE    "DSL Forum TR-90, paragraph 5.1.4"
      ::= { adsl2LineConfTemplateEntry 1 }

   adsl2LConfTempLineProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2 Line
          Configuration Profile Table, (adsl2LineConfProfTable),
          which applies for this ADSL2 line."





      REFERENCE    "DSL Forum TR-90, paragraph 5.1.4"
      DEFVAL       { "DEFVAL" }
      ::= { adsl2LineConfTemplateEntry 2 }

   adsl2LConfTempChan1ConfProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2
          Channel Configuration Profile Table,
          (adsl2ChConfProfileTable) that applies to ADSL2 bearer
          channel #1.  The channel profile name specified here must
          match the name of an existing row in the
          adsl2ChConfProfileTable table."
      DEFVAL       { "DEFVAL" }
      ::= { adsl2LineConfTemplateEntry 3 }

   adsl2LConfTempChan1RaRatioDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..100)
      UNITS       "percent"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Rate Adaptation Ratio.  The ratio (in %) that should be taken
          into account for the bearer channel #1 when performing rate
          adaptation on Downstream.  The ratio refers to the available
          data rate in excess of the Minimum Data Rate, summed over all
          bearer channels.  Also, the 100 -
          adsl2LConfTempChan1RaRatioDs is the ratio of excess data
          rate to be assigned to all other bearer channels on Downstream
          direction.  The sum of rate adaptation ratios over all bearers
          on the same direction shall be equal to 100%."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      DEFVAL       { 100 }
      ::= { adsl2LineConfTemplateEntry 4 }

   adsl2LConfTempChan1RaRatioUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..100)
      UNITS       "percent"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Rate Adaptation Ratio.  The ratio (in %) that should be taken
          into account for the bearer channel #1 when performing rate
          adaptation on Upstream.  The ratio refers to the available
          data rate in excess of the Minimum Data Rate, summed over all
          bearer channels.  Also, the





          100 - adsl2LConfTempChan1RaRatioUs is the ratio of excess
          data rate to be assigned to all other bearer channels on
          Upstream direction.  The sum of rate adaptation ratios over
          all bearers on the same direction shall be equal to 100%."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      DEFVAL       { 100 }
      ::= { adsl2LineConfTemplateEntry 5 }

   adsl2LConfTempChan2ConfProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(0..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2
          Channel Configuration Profile Table
          (adsl2ChConfProfileTable) that applies to ADSL2 bearer
          channel #2.  If the channel is unused, then the object is set
          to a zero-length string.
          This object may be set to a zero-length string only if
          adsl2LConfTempChan3ConfProfile contains a zero-length
          string."

      DEFVAL       { "" }
      ::= { adsl2LineConfTemplateEntry 6 }

   adsl2LConfTempChan2RaRatioDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..100)
      UNITS       "percent"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Rate Adaptation Ratio.  The ratio (in %) that should be taken
          into account for the bearer channel #2 when performing rate
          adaptation on Downstream.  The ratio refers to the available
          data rate in excess of the Minimum Data Rate, summed over all
          bearer channels.  Also, the
          100 - adsl2LConfTempChan2RaRatioDs is the ratio of excess
          data rate to be assigned to all other bearer channels on
          Downstream direction.  The sum of rate adaptation ratios
          over all bearers on the same direction shall be equal to
          100%."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      DEFVAL       { 0 }
      ::= { adsl2LineConfTemplateEntry 7 }

   adsl2LConfTempChan2RaRatioUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..100)
      UNITS       "percent"





      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Rate Adaptation Ratio.  The ratio (in %) that should be taken
          into account for the bearer channel #2 when performing rate
          adaptation on Upstream.  The ratio refers to the available
          data rate in excess of the Minimum Data Rate, summed over all
          bearer channels.  Also, the
          100 - adsl2LConfTempChan2RaRatioUs is the ratio of excess
          data rate to be assigned to all other bearer channels on
          Upstream direction.  The sum of rate adaptation ratios over
          all bearers on the same direction shall be equal to 100%."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      DEFVAL       { 0 }
      ::= { adsl2LineConfTemplateEntry 8 }

   adsl2LConfTempChan3ConfProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(0..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2
          Channel Configuration Profile Table
          (adsl2ChConfProfileTable) that applies to ADSL2 bearer
          channel #3.  If the channel is unused, then the object is set
          to a zero-length string.
          This object may be set to a zero-length string only if
          adsl2LConfTempChan4ConfProfile contains a zero-length
          string.
          This object may be set to a non-zero-length string only if
          adsl2LConfTempChan2ConfProfile contains a non-zero-length
          string."
      DEFVAL       { "" }
      ::= { adsl2LineConfTemplateEntry 9 }

   adsl2LConfTempChan3RaRatioDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..100)
      UNITS       "percent"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Rate Adaptation Ratio.  The ratio (in %) that should be taken
          into account for the bearer channel #3 when performing rate
          adaptation on Downstream.  The ratio refers to the available
          data rate in excess of the Minimum Data Rate, summed over all
          bearer channels.  Also, the 100 -
          adsl2LConfTempChan3RaRatioDs is the ratio of excess data
          rate to be assigned to all other bearer channels on Downstream





          direction.  The sum of rate adaptation ratios over all bearers
          on the same direction shall be equal to 100%."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      DEFVAL       { 0 }
      ::= { adsl2LineConfTemplateEntry 10 }

   adsl2LConfTempChan3RaRatioUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..100)
      UNITS       "percent"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Rate Adaptation Ratio.  The ratio (in %) that should be taken
          into account for the bearer channel #3 when performing rate
          adaptation on Upstream.  The ratio refers to the available
          data rate in excess of the Minimum Data Rate, summed over all
          bearer channels.  Also, the
          100 - adsl2LConfTempChan3RaRatioUs is the ratio of excess
          data rate to be assigned to all other bearer channels on
          Upstream direction.  The sum of rate adaptation ratios over
          all bearers on the same direction shall be equal to 100%."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      DEFVAL       { 0 }
      ::= { adsl2LineConfTemplateEntry 11 }

   adsl2LConfTempChan4ConfProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(0..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2
          Channel Configuration Profile Table
          (adsl2ChConfProfileTable) that applies to ADSL2 bearer
          channel #4.  If the channel is unused, then the object is set
          to a zero-length string.
          This object may be set to a non-zero-length string only if
          adsl2LConfTempChan3ConfProfile contains a non-zero-length
          string."
      DEFVAL       { "" }
      ::= { adsl2LineConfTemplateEntry 12 }

   adsl2LConfTempChan4RaRatioDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..100)
      UNITS       "percent"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Rate Adaptation Ratio.  The ratio (in %) that should be taken





          into account for the bearer channel #4 when performing rate
          adaptation on Downstream.  The ratio refers to the available
          data rate in excess of the Minimum Data Rate, summed over all
          bearer channels.  Also, the 100 -
          adsl2LConfTempChan4RaRatioDs is the ratio of
          excess data rate to be assigned to all other bearer channels.
          The sum of rate adaptation ratios over all bearers on the same
          direction shall sum to 100%."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      DEFVAL       { 0 }
      ::= { adsl2LineConfTemplateEntry 13 }

   adsl2LConfTempChan4RaRatioUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..100)
      UNITS       "percent"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Rate Adaptation Ratio.  The ratio (in %) that should be taken
          into account for the bearer channel #4 when performing rate
          adaptation on Upstream.  The ratio refers to the available
          data rate in excess of the Minimum Data Rate, summed over
          all bearer channels.  Also, the 100 -
          adsl2LConfTempChan4RaRatioUs is the
          ratio of excess data rate to be assigned to all other bearer
          channels.  The sum of rate adaptation ratios over all bearers
          on the same direction shall sum to 100%."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      DEFVAL       { 0 }
      ::= { adsl2LineConfTemplateEntry 14 }

   adsl2LConfTempRowStatus  OBJECT-TYPE
      SYNTAX      RowStatus
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "This object is used to create a new row or to modify or
         delete an existing row in this table.

         A template is activated by setting this object to 'active'.
         When 'active' is set, the system will validate the template.

         Before a template can be deleted or taken out of service
         (by setting this object to 'destroy' or 'notInService'),
         it must first be unreferenced from all associated
         lines."
      ::= { adsl2LineConfTemplateEntry 15 }






   ------------------------------------------
   --        adsl2LineConfProfTable        --
   ------------------------------------------
   adsl2LineConfProfTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2LineConfProfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineConfProfTable contains ADSL2 line profile
          configuration.

          Entries in this table MUST be maintained in a
          persistent manner."
      ::= { adsl2ProfileLine 2 }

   adsl2LineConfProfEntry  OBJECT-TYPE
      SYNTAX      Adsl2LineConfProfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineConfProfTable contains ADSL2 line profile
          configuration.

          A default profile with an index of 'DEFVAL' will
          always exist, and its parameters will be set to vendor-
          specific values, unless otherwise specified in this document."
      INDEX  { adsl2LConfProfProfileName }
      ::= { adsl2LineConfProfTable 1 }

   Adsl2LineConfProfEntry  ::=
      SEQUENCE {
         adsl2LConfProfProfileName          SnmpAdminString,
         adsl2LConfProfScMaskDs             Adsl2ScMaskDs,
         adsl2LConfProfScMaskUs             Adsl2ScMaskUs,
         adsl2LConfProfRfiBandsDs           Adsl2RfiDs,
         adsl2LConfProfRaModeDs             Adsl2RaMode,
         adsl2LConfProfRaModeUs             Adsl2RaMode,
         adsl2LConfProfRaUsNrmDs            Unsigned32,
         adsl2LConfProfRaUsNrmUs            Unsigned32,
         adsl2LConfProfRaUsTimeDs           Unsigned32,
         adsl2LConfProfRaUsTimeUs           Unsigned32,
         adsl2LConfProfRaDsNrmsDs           Unsigned32,
         adsl2LConfProfRaDsNrmsUs           Unsigned32,
         adsl2LConfProfRaDsTimeDs           Unsigned32,
         adsl2LConfProfRaDsTimeUs           Unsigned32,
         adsl2LConfProfTargetSnrmDs         Unsigned32,
         adsl2LConfProfTargetSnrmUs         Unsigned32,
         adsl2LConfProfMaxSnrmDs            Unsigned32,





         adsl2LConfProfMaxSnrmUs            Unsigned32,
         adsl2LConfProfMinSnrmDs            Unsigned32,
         adsl2LConfProfMinSnrmUs            Unsigned32,
         adsl2LConfProfMsgMinUs             Unsigned32,
         adsl2LConfProfMsgMinDs             Unsigned32,
         adsl2LConfProfAtuTransSysEna       Adsl2TransmissionModeType,
         adsl2LConfProfPmMode               Adsl2LConfProfPmMode,
         adsl2LConfProfL0Time               Unsigned32,
         adsl2LConfProfL2Time               Unsigned32,
         adsl2LConfProfL2Atpr               Unsigned32,
         adsl2LConfProfL2Atprt              Unsigned32,
         adsl2LConfProfRowStatus            RowStatus
      }

   adsl2LConfProfProfileName  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This object identifies a row in this table."
        ::= { adsl2LineConfProfEntry 1 }

   adsl2LConfProfScMaskDs  OBJECT-TYPE
      SYNTAX      Adsl2ScMaskDs
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Sub-carriers mask.  A bitmap of 512 bits that allows masking
          up to 512 downstream sub-carriers, depending on NSCds.  If bit
          i (0 <= i < NSCds) is set to '1', the respective
          downstream sub-carrier i is masked, and if set to '0', the
          respective sub-carrier is unmasked.  Note that there should
          always be unmasked sub-carriers (i.e., the object cannot be
          all 1's).  Also note that if NSCds < 512, all bits
          i (NSCds < i <= 512) should be set to '1'."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2.6"
      ::= { adsl2LineConfProfEntry 2 }

   adsl2LConfProfScMaskUs  OBJECT-TYPE
      SYNTAX      Adsl2ScMaskUs
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Sub-carriers mask.  A bitmap of 64 bits that allows masking
          up to 64 downstream sub-carriers, depending on NSCds.  If
          bit i (0 <= i < NSCus) is set to '1', the respective
          upstream sub-carrier i is masked, and if set to '0', the
          respective sub-carrier is unmasked.  Note that there





          should always be unmasked sub-carriers (i.e., the object
          cannot be all 1's).  Also note that if NSCus <
          64, all bits i (NSCus < i <= 64) should be set to '1'."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2.7"
      ::= { adsl2LineConfProfEntry 3 }

   adsl2LConfProfRfiBandsDs  OBJECT-TYPE
      SYNTAX      Adsl2RfiDs
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
          "The subset of downstream PSD mask breakpoints that shall be
          used to notch an RFI band.
          The specific interpolation around these points is defined in
          G.992.5.  It is a bitmap of 512 bits that allows referring to
          up to 512 downstream sub-carriers, depending on NSCds.  If bit
          i (0 <= i < NSCds) is set to '1', the respective downstream
          sub-carrier i is part of a notch filter, and if set to '0',
          the respective sub-carrier is not part of a notch filter.
          This information complements the specification provided by
          adsl2LConfProfPsdMaskDs.
          Note that if NSCds < 512, all bits i (NSCds<i<512)
          should be set to '0'."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2.9"
      ::= { adsl2LineConfProfEntry 4 }

   adsl2LConfProfRaModeDs  OBJECT-TYPE
      SYNTAX      Adsl2RaMode
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The mode of operation of a rate-adaptive ATU-C in the transmit
          direction.  The parameter can take three values:
             manual(1),
             raInit(2), or
             dynamicRa(3)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.1"
      DEFVAL       { manual }
      ::= { adsl2LineConfProfEntry 5 }

   adsl2LConfProfRaModeUs  OBJECT-TYPE
      SYNTAX      Adsl2RaMode
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The mode of operation of a rate-adaptive ATU-R in the transmit
          direction.  The parameter can take three values:
             manual(1),





             raInit(2), or
             dynamicRa(3)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.2"
      DEFVAL       { manual }
      ::= { adsl2LineConfProfEntry 6 }

   adsl2LConfProfRaUsNrmDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..310)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The Downstream Up-Shift Noise Margin value, to be used when
          adsl2LConfProfRaModeDs is set to dynamicRa.  If the downstream
          noise margin is above this value and stays above it for
          more than the time specified by the adsl2LConfProfRaUsTimeDs,
          the ATU-R shall attempt to increase the downstream net data
          rate.  The Downstream Up-Shift Noise Margin ranges from 0 to
          310 units of 0.1 dB (physical values are 0 to 31 dB)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.3"
      DEFVAL       { 10 }
      ::= { adsl2LineConfProfEntry 7 }

   adsl2LConfProfRaUsNrmUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..310)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The Upstream Up-Shift Noise Margin value, to be used when
          adsl2LConfProfRaModeUs is set to dynamicRa.  If the upstream
          noise margin is above this value and stays above it for more
          than the time specified by the adsl2LConfProfRaUsTimeUs, the
          ATU-C shall attempt to increase the upstream net data rate.
          The Upstream Up-Shift Noise Margin ranges from 0 to 310 units
          of 0.1 dB (physical values are 0 to 31 dB)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.4"
      DEFVAL       { 10 }
      ::= { adsl2LineConfProfEntry 8 }

   adsl2LConfProfRaUsTimeDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..16383)
      UNITS       "seconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The Downstream Up-Shift Time Interval, to be used when
          adsl2LConfProfRaModeDs is set to dynamicRa.  The interval of





          time that the downstream noise margin should stay above the
          Downstream Up-Shift Noise Margin before the ATU-R shall
          attempt to increase the downstream net data rate.  The time
          interval ranges from 0 to 16383 seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.5"
      DEFVAL       { 3600 }
      ::= { adsl2LineConfProfEntry 9 }

   adsl2LConfProfRaUsTimeUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..16383)
      UNITS       "seconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The Upstream Up-Shift Time Interval, to be used when
          adsl2LConfProfRaModeUs is set to dynamicRa.  The interval of
          time the upstream noise margin should stay above the
          Upstream Up-Shift Noise Margin before the ATU-C shall
          attempt to increase the upstream net data rate.  The time
          interval ranges from 0 to 16383 seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.6"
      DEFVAL       { 3600 }
      ::= { adsl2LineConfProfEntry 10 }

   adsl2LConfProfRaDsNrmsDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..310)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The Downstream Down-Shift Noise Margin value, to be used when
          adsl2LConfProfRaModeDs is set to dynamicRa.  If the downstream
          noise margin is below this value and stays below that for more
          than the time specified by the adsl2LConfProfRaDsTimeDs, the
          ATU-R shall attempt to decrease the downstream net data rate.
          The Downstream Down-Shift Noise Margin ranges from 0 to 310
          units of 0.1 dB (physical values are 0 to 31 dB)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.7"
      DEFVAL       { 10 }
      ::= { adsl2LineConfProfEntry 11 }

   adsl2LConfProfRaDsNrmsUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..310)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The Upstream Down-Shift Noise Margin value, to be used when





          adsl2LConfProfRaModeUs is set to dynamicRa.  If the upstream
          noise margin is below this value and stays below that for more
          than the time specified by the adsl2LConfProfRaDsTimeUs, the
          ATU-C shall attempt to decrease the upstream net data rate.
          The Upstream Down-Shift Noise Margin ranges from 0 to 310
          units of 0.1 dB (physical values are 0 to 31 dB)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.8"
      DEFVAL       { 10 }
      ::= { adsl2LineConfProfEntry 12 }

   adsl2LConfProfRaDsTimeDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..16383)
      UNITS       "seconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The Downstream Down-Shift Time Interval, to be used when
          adsl2LConfProfRaModeDs is set to dynamicRa.  The interval of
          time the downstream noise margin should stay below the
          Downstream Down-Shift Noise Margin before the ATU-R shall
          attempt to decrease the downstream net data rate.  The time
          interval ranges from 0 to 16383 seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.9"
      DEFVAL       { 3600 }
      ::= { adsl2LineConfProfEntry 13 }

   adsl2LConfProfRaDsTimeUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..16383)
      UNITS       "seconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The Upstream Down-Shift Time Interval, to be used when
          adsl2LConfProfRaModeUs is set to dynamicRa.  The interval of
          time the upstream noise margin should stay below the Upstream
          Down-Shift Noise Margin before the ATU-C shall attempt to
          decrease the upstream net data rate.  The time interval ranges
          from 0 to 16383 seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.4.10"
      DEFVAL       { 3600 }
      ::= { adsl2LineConfProfEntry 14 }

   adsl2LConfProfTargetSnrmDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..310)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION





         "The minimum Noise Margin the ATU-R receiver shall achieve,
          relative to the BER requirement for each of the downstream
          bearer channels, to successfully complete initialization.
          The target noise margin ranges from 0 to 310 units of 0.1 dB
          (physical values are 0 to 31 dB)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.3.1"
      DEFVAL       { 60 }
      ::= { adsl2LineConfProfEntry 15 }

   adsl2LConfProfTargetSnrmUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..310)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The minimum Noise Margin the ATU-C receiver shall achieve,
          relative to the BER requirement for each of the upstream
          bearer channels, to successfully complete initialization.
          The target noise margin ranges from 0 to 310 units of 0.1 dB
          (physical values are 0 to 31 dB)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.3.2"
      DEFVAL       { 60 }
      ::= { adsl2LineConfProfEntry 16 }

   adsl2LConfProfMaxSnrmDs  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..310 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The maximum Noise Margin the ATU-R receiver shall try to
          sustain.  If the Noise Margin is above this level, the ATU-R
          shall request that the ATU-C reduce the ATU-C transmit power
          to get a noise margin below this limit (if this functionality
          is supported).  The maximum noise margin ranges from 0 to 310
          units of 0.1 dB (physical values are 0 to 31 dB).  A value of
          0x7FFFFFFF (2147483647) means that there is no maximum."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.3.3"
      DEFVAL       { 310 }
      ::= { adsl2LineConfProfEntry 17 }

   adsl2LConfProfMaxSnrmUs  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..310 | 2147483647)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The maximum Noise Margin the ATU-C receiver shall try to





          sustain.  If the Noise Margin is above this level, the ATU-C
          shall request that the ATU-R reduce the ATU-R transmit power
          to get a noise margin below this limit (if this functionality
          is supported).  The maximum noise margin ranges from 0 to 310
          units of 0.1 dB (physical values are 0 to 31 dB).  A value of
          0x7FFFFFFF (2147483647) means that there is no maximum."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.3.4"
      DEFVAL       { 310 }
      ::= { adsl2LineConfProfEntry 18 }

   adsl2LConfProfMinSnrmDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..310)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The minimum Noise Margin the ATU-R receiver shall tolerate.
          If the noise margin falls below this level, the ATU-R shall
          request that the ATU-C increase the ATU-C transmit power.
          If an increase to ATU-C transmit power is not possible, a
          loss-of-margin (LOM) defect occurs, the ATU-R shall fail and
          attempt to reinitialize, and the NMS shall be notified.  The
          minimum noise margin ranges from 0 to 310 units of
          0.1 dB (physical values are 0 to 31 dB).  A value of 0 means
          that there is no minimum."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.3.5"
      DEFVAL       { 10 }
      ::= { adsl2LineConfProfEntry 19 }

   adsl2LConfProfMinSnrmUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..310)
      UNITS       "0.1 dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The minimum Noise Margin the ATU-C receiver shall tolerate.
          If the noise margin falls below this level, the ATU-C shall
          request that the ATU-R increase the ATU-R transmit power.
          If an increase of ATU-R transmit power is not possible, a
          loss-of-margin (LOM) defect occurs, the ATU-C shall fail and
          attempt to reinitialize, and the NMS shall be notified.  The
          minimum noise margin ranges from 0 to 310 units of
          0.1 dB (physical values are 0 to 31 dB).  A value of 0 means
          that there is no minimum."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.3.6"
      DEFVAL       { 10 }
      ::= { adsl2LineConfProfEntry 20 }






   adsl2LConfProfMsgMinUs  OBJECT-TYPE
      SYNTAX      Unsigned32(4000..63000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Minimum Overhead Rate Upstream.  Defines the minimum rate of
          the message-based overhead that shall be maintained by the ATU
          in upstream direction.  Expressed in bits per second and
          ranges from 4000 to 63000 bps."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.5.1"
      DEFVAL       { 4000 }
     ::= { adsl2LineConfProfEntry 21 }

   adsl2LConfProfMsgMinDs  OBJECT-TYPE
      SYNTAX      Unsigned32(4000..63000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Minimum Overhead Rate Downstream.  Defines the minimum rate of
          the message-based overhead that shall be maintained by the ATU
          in downstream direction.  Expressed in bits per second and
          ranges from 4000 to 63000 bps."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.5.2"
      DEFVAL       { 4000 }
      ::= { adsl2LineConfProfEntry 22 }

   adsl2LConfProfAtuTransSysEna  OBJECT-TYPE
      SYNTAX      Adsl2TransmissionModeType
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "ATU Transmission System Enabling (ATSE).  A list of the
          different coding types enabled in this profile.  It is coded
          in a bit-map representation with 1 or more bits set.  A bit
          set to  '1' means that the ATUs may apply the respective
          coding for the ADSL line.  A bit set to '0' means that
          the ATUs cannot apply the respective coding for the ADSL
          line.  All 'reserved' bits should be set to '0'."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.1.1"
      ::= { adsl2LineConfProfEntry 23 }

   adsl2LConfProfPmMode  OBJECT-TYPE
      SYNTAX      Adsl2LConfProfPmMode
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION





         "Power management state Enabling.  Defines the power states the
          ATU-C or ATU-R may autonomously transition to on this line.
          The various bit positions are: allowTransitionsToIdle(0) and
          allowTransitionsToLowPower(1).  A bit with a '1' value means
          that the ATU is allowed to transit into the respective state,
          and a '0' value means that the ATU is not allowed
          to transit into the respective state."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.1.4"
      DEFVAL  { { allowTransitionsToIdle, allowTransitionsToLowPower } }
      ::= { adsl2LineConfProfEntry 24 }

   adsl2LConfProfL0Time  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..255)
      UNITS       "seconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "This minimum time (in seconds) between an Exit from the L2
          state and the next Entry into the L2 state.  It ranges from 0
          to 255 seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.1.5"
      DEFVAL       { 255 }
      ::= { adsl2LineConfProfEntry 25 }

   adsl2LConfProfL2Time  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..255)
      UNITS       "seconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "This minimum time (in seconds) between an Entry into the
         L2 state and the first Power Trim in the L2 state and between
         two consecutive Power Trims in the L2 State.
         It ranges from 0 to 255 seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.1.6"
      DEFVAL       { 255 }
      ::= { adsl2LineConfProfEntry 26 }

   adsl2LConfProfL2Atpr  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..31)
      UNITS       "dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The maximum aggregate transmit power reduction (in dB) that
          can be performed at transition of L0 to L2 state or through a
          single Power Trim in the L2 state.
          It ranges from 0 dB to 31 dB."





      REFERENCE    "ITU-T G.997.1 (amendment 1), 7.3.1.1.7"
      DEFVAL       { 10 }
      ::= { adsl2LineConfProfEntry 27 }

   adsl2LConfProfL2Atprt  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..31)
      UNITS       "dB"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The total maximum aggregate transmit power reduction
         (in dB) that can be performed in an L2 state.  This is the
         sum of all reductions of L2 Request (i.e., at transition of
         L0 to L2 state) and Power Trims."
      REFERENCE    "ITU-T G.997.1 (amendment 1), 7.3.1.1.9"
      DEFVAL       { 31 }
      ::= { adsl2LineConfProfEntry 28 }

   adsl2LConfProfRowStatus  OBJECT-TYPE
      SYNTAX      RowStatus
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "This object is used to create a new row or to modify or
         delete an existing row in this table.

         A profile is activated by setting this object to 'active'.
         When 'active' is set, the system will validate the profile.

         Before a profile can be deleted or taken out of service
         (by setting this object to 'destroy' or 'notInService'),
         it must first be unreferenced from all associated
         templates."
      ::= { adsl2LineConfProfEntry 29 }


   ------------------------------------------
   --    adsl2LineConfProfModeSpecTable    --
   ------------------------------------------
   adsl2LineConfProfModeSpecTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2LineConfProfModeSpecEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineConfProfModeSpecTable extends the
          ADSL2 line configuration profile by ADSL Mode Specific
          parameters.
          A row in this table that has an index of





          adsl2LConfProfAdslMode == defMode(1) is called a
          'mandatory' row.
          A row in this table that has an index such that
          adsl2LConfProfAdslMode is not equal to defMode(1)
          is called an 'optional' row.
          When a row in the adsl2LineConfProfTable table
          (the parent row) is created, the SNMP agent will
          automatically create a 'mandatory' row in this table.
          When the parent row is deleted, the SNMP agent will
          automatically delete all associated rows in this table.
          Any attempt to delete the 'mandatory' row using the
          adsl2LConfProfModeSpecRowStatus attribute will be
          rejected by the SNMP agent.
          The manager MAY create an 'optional' row in this table
          using the adsl2LConfProfModeSpecRowStatus attribute if
          the parent row exists.
          The manager MAY delete an 'optional' row in this table
          using the adsl2LConfProfModeSpecRowStatus attribute at
          any time.
          If the actual transmission mode of a DSL line does not
          match one of the 'optional' rows in this table, then
          the line will use the PSD configuration from the
          'mandatory' row.

          Entries in this table MUST be maintained in a
          persistent manner."
      ::= { adsl2ProfileLine 3 }

   adsl2LineConfProfModeSpecEntry  OBJECT-TYPE
      SYNTAX      Adsl2LineConfProfModeSpecEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineConfProfModeSpecTable extends the
          ADSL2 line configuration profile by ADSL Mode Specific
          parameters."
      INDEX  { adsl2LConfProfProfileName, adsl2LConfProfAdslMode }
      ::= { adsl2LineConfProfModeSpecTable 1 }

   Adsl2LineConfProfModeSpecEntry  ::=
      SEQUENCE {
         adsl2LConfProfAdslMode             Adsl2OperationModes,
         adsl2LConfProfMaxNomPsdDs          Integer32,
         adsl2LConfProfMaxNomPsdUs          Integer32,
         adsl2LConfProfMaxNomAtpDs          Unsigned32,
         adsl2LConfProfMaxNomAtpUs          Unsigned32,
         adsl2LConfProfMaxAggRxPwrUs        Integer32,
         adsl2LConfProfPsdMaskDs            Adsl2PsdMaskDs,





         adsl2LConfProfPsdMaskUs            Adsl2PsdMaskUs,
         adsl2LConfProfPsdMaskSelectUs      Unsigned32,
         adsl2LConfProfModeSpecRowStatus    RowStatus
      }

   adsl2LConfProfAdslMode    OBJECT-TYPE
      SYNTAX      Adsl2OperationModes
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The ADSL Mode is a way of categorizing the various ADSL
          transmission modes into groups; each group (ADSL Mode) shares
          the same PSD configuration.
          There should be multiple entries in this table for a given
          line profile in case multiple bits are set in
          adsl2LConfProfAtuTransSysEna for that profile."
      REFERENCE    "DSL Forum TR-90, paragraph 5.1.8"
      ::= { adsl2LineConfProfModeSpecEntry 1 }

   adsl2LConfProfMaxNomPsdDs  OBJECT-TYPE
      SYNTAX      Integer32(-600..-300)
      UNITS       "0.1 dBm/Hz"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The maximum nominal transmit PSD in the downstream
          direction during initialization and Showtime.  It ranges from
          -600 to -300 units of 0.1 dBm/Hz (physical values are -60 to
          -30 dBm/Hz)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2"
      DEFVAL       { -300 }
     ::= { adsl2LineConfProfModeSpecEntry 2 }

   adsl2LConfProfMaxNomPsdUs  OBJECT-TYPE
      SYNTAX      Integer32(-600..-300)
      UNITS       "0.1 dBm/Hz"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The maximum nominal transmit PSD in the upstream direction
          during initialization and Showtime.  It ranges from -600 to
          -300 units of 0.1 dBm/Hz (physical values are -60 to
          -30 dBm/Hz)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2"
      DEFVAL       { -300 }
      ::= { adsl2LineConfProfModeSpecEntry 3 }

   adsl2LConfProfMaxNomAtpDs  OBJECT-TYPE





      SYNTAX      Unsigned32 (0..255)
      UNITS       "0.1 dBm"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The maximum nominal aggregate transmit power in the
          downstream direction during initialization and Showtime.  It
          ranges from 0 to 255 units of 0.1 dBm (physical values are 0
          to 25.5 dBm)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2"
      DEFVAL       { 255 }
      ::= { adsl2LineConfProfModeSpecEntry 4 }

   adsl2LConfProfMaxNomAtpUs  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..255)
      UNITS       "0.1 dBm"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The maximum nominal aggregate transmit power in the upstream
          direction during initialization and Showtime.  It ranges from
          0 to 255 units of 0.1 dBm (physical values are 0 to 25.5
          dBm)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2"
      DEFVAL       { 255 }
      ::= { adsl2LineConfProfModeSpecEntry 5 }

   adsl2LConfProfMaxAggRxPwrUs  OBJECT-TYPE
      SYNTAX      Integer32(-255..255 | 2147483647)
      UNITS       "0.1 dBm"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The maximum upstream aggregate receive power over the relevant
          set of sub-carriers.  The ATU-C should verify that the
          upstream power cutback is such that this maximum aggregate
          receive power value is honored.  It ranges from -255 to 255
          units of 0.1 dBm (physical values are -25.5 to 25.5 dBm).
          A value of 0x7FFFFFFF (2147483647) means that there is no
          limit."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2"
      DEFVAL       { 255 }
      ::= { adsl2LineConfProfModeSpecEntry 6 }

   adsl2LConfProfPsdMaskDs   OBJECT-TYPE
      SYNTAX      Adsl2PsdMaskDs
      MAX-ACCESS  read-create
      STATUS      current





      DESCRIPTION
        "The downstream PSD mask applicable at the U-C2 reference
         point.
        This parameter is used only for G.992.5, and it may impose PSD
        restrictions (breakpoints) in addition to the Limit PSD mask
        defined in G.992.5.
        This is a string of 32 pairs of values in the following
        structure:
        Octets 0+1 - Index of 1st sub-carrier used in the context
                     of a first breakpoint.
        Octet 2    - The PSD reduction for the sub-carrier indicated in
                     octets 0 and 1.
        Octets 3-5 - Same, for a 2nd breakpoint.
        Octets 6-8 - Same, for a 3rd breakpoint.
        This architecture continues until octets 94-95, which are
        associated with a 32nd breakpoint.
        Each subcarrier index is an unsigned number in the range 1 to
        NSCds.  Each PSD reduction value is in the range 0 (0dBm/Hz) to
        255 (-127.5dBm/Hz) with steps of 0.5dBm/Hz.  Valid values are
        in the range 0 to 190 (0 to -95dBm/Hz).
        When the number of breakpoints is less than 32, all remaining
        octets are set to the value 0.  Note that the content of this
        object should be correlated with the sub-carriers mask and with
        the RFI setup."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2"
        ::= { adsl2LineConfProfModeSpecEntry 7 }

   adsl2LConfProfPsdMaskUs   OBJECT-TYPE
      SYNTAX      Adsl2PsdMaskUs
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
        "The upstream PSD mask applicable at the U-R2 reference
         point.
        This parameter is used only for G.992.5, and it may impose PSD
        restrictions (breakpoints) in addition to the Limit PSD mask
        defined in G.992.5.
        This is a string of 4 pairs of values in the following
        structure:
        Octets 0+1 - Index of 1st sub-carrier used in the context
                     of a first breakpoint.
        Octet 2    - The PSD reduction for the sub-carrier indicated in
                     octets 0 and 1.
        Octets 3-5 - Same, for a 2nd breakpoint.
        Octets 6-8 - Same, for a 3rd breakpoint.
        This architecture continues until octets 9-11, which are
        associated with a 4th breakpoint.
        Each subcarrier index is an unsigned number in the range 1 to





        NSCus.  Each PSD reduction value is in the range 0 (0dBm/Hz) to
        255 (-127.5dBm/Hz) with steps of 0.5dBm/Hz.  Valid values are
        in the range 0 to 190 (0 to -95dBm/Hz).
        When the number of breakpoints is less than 4, all remaining
        octets are set to the value 0.  Note that the content of this
        object should be correlated with the sub-carriers mask and with
        the RFI setup."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1.2"
        ::= { adsl2LineConfProfModeSpecEntry 8 }

   adsl2LConfProfPsdMaskSelectUs  OBJECT-TYPE
      SYNTAX      Unsigned32(1..9)
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
        "The selected upstream PSD mask.  This parameter is used only
         for annexes J and M of G.992.3 and G.992.5, and the same
         selection is used for all relevant enabled bits in
         adsl2LConfProfAtuTransSysEna."
      REFERENCE    "ITU-T G.997.1 (amendment 1), 7.3.1.2.10"
      DEFVAL       { 1 }
       ::= { adsl2LineConfProfModeSpecEntry 9 }

   adsl2LConfProfModeSpecRowStatus  OBJECT-TYPE
      SYNTAX      RowStatus
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION

         "This object is used to create a new row or to modify or
         delete an existing row in this table.

         A profile is activated by setting this object to 'active'.
         When 'active' is set, the system will validate the profile.

         Before a profile can be deleted or taken out of service
         (by setting this object to 'destroy' or 'notInService'),
         it must first be unreferenced from all associated
         templates."

      ::= { adsl2LineConfProfModeSpecEntry 10 }

   ------------------------------------------------
   --          adsl2ChConfProfileTable           --
   ------------------------------------------------
   adsl2ChConfProfileTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2ChConfProfileEntry
      MAX-ACCESS  not-accessible





      STATUS      current
      DESCRIPTION
         "The table adsl2ChConfProfileTable contains ADSL2 channel
          profile configuration.

          Entries in this table MUST be maintained in a
          persistent manner."
      ::= { adsl2ProfileChannel 1 }

   adsl2ChConfProfileEntry  OBJECT-TYPE
      SYNTAX      Adsl2ChConfProfileEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2ChConfProfileTable contains ADSL2 channel
          profile configuration.
          A default profile with an index of 'DEFVAL' will
          always exist, and its parameters will be set to vendor-
          specific values, unless otherwise specified in this document."
      INDEX  { adsl2ChConfProfProfileName }
      ::= { adsl2ChConfProfileTable 1 }

   Adsl2ChConfProfileEntry  ::=
      SEQUENCE {
         adsl2ChConfProfProfileName          SnmpAdminString,
         adsl2ChConfProfMinDataRateDs        Unsigned32,
         adsl2ChConfProfMinDataRateUs        Unsigned32,
         adsl2ChConfProfMinResDataRateDs     Unsigned32,
         adsl2ChConfProfMinResDataRateUs     Unsigned32,
         adsl2ChConfProfMaxDataRateDs        Unsigned32,
         adsl2ChConfProfMaxDataRateUs        Unsigned32,
         adsl2ChConfProfMinDataRateLowPwrDs  Unsigned32,
         adsl2ChConfProfMaxDelayDs           Unsigned32,
         adsl2ChConfProfMaxDelayUs           Unsigned32,
         adsl2ChConfProfMinProtectionDs      Adsl2SymbolProtection,
         adsl2ChConfProfMinProtectionUs      Adsl2SymbolProtection,
         adsl2ChConfProfMaxBerDs             Adsl2MaxBer,
         adsl2ChConfProfMaxBerUs             Adsl2MaxBer,
         adsl2ChConfProfUsDataRateDs         Unsigned32,
         adsl2ChConfProfDsDataRateDs         Unsigned32,
         adsl2ChConfProfUsDataRateUs         Unsigned32,
         adsl2ChConfProfDsDataRateUs         Unsigned32,
         adsl2ChConfProfImaEnabled           TruthValue,
         adsl2ChConfProfRowStatus            RowStatus
      }

   adsl2ChConfProfProfileName  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))





      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This object identifies a row in this table."
      ::= { adsl2ChConfProfileEntry 1 }

   adsl2ChConfProfMinDataRateDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Minimum Data Rate on Downstream direction.  The minimum net
          data rate for the bearer channel, coded in bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      ::= { adsl2ChConfProfileEntry 2 }

   adsl2ChConfProfMinDataRateUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Minimum Data Rate on Upstream direction.  The minimum net data
          rate for the bearer channel, coded in bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      ::= { adsl2ChConfProfileEntry 3 }

   adsl2ChConfProfMinResDataRateDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Minimum Reserved Data Rate on Downstream direction.  The
          minimum reserved net data rate for the bearer channel, coded
          in bits/second.  This parameter is used only if the Rate
          Adaptation Mode in the direction of the bearer channel (i.e.,
          adsl2LConfProfRaModeDs) is set to dynamicRa."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      ::= { adsl2ChConfProfileEntry 4 }

   adsl2ChConfProfMinResDataRateUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION





         "Minimum Reserved Data Rate on Upstream direction.  The minimum
          reserved net data rate for the bearer channel, coded in
          bits/second.  This parameter is used only if the Rate
          Adaptation Mode in the direction of the bearer channel (i.e.,
          adsl2LConfProfRaModeUs) is set to dynamicRa."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      ::= { adsl2ChConfProfileEntry 5 }

   adsl2ChConfProfMaxDataRateDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Maximum Data Rate on Downstream direction.  The maximum net
          data rate for the bearer channel, coded in bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      ::= { adsl2ChConfProfileEntry 6 }

   adsl2ChConfProfMaxDataRateUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Maximum Data Rate on Upstream direction.  The maximum net data
          rate for the bearer channel, coded in bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      ::= { adsl2ChConfProfileEntry 7 }

   adsl2ChConfProfMinDataRateLowPwrDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Minimum Data Rate in Low Power state on Downstream direction.
          The minimum net data rate for the bearer channel, coded in
          bits/second, during the low power state (L1 in G.992.2, L2 in
          G.992.3)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.1"
      ::= { adsl2ChConfProfileEntry 8 }

   adsl2ChConfProfMaxDelayDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..63)
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current





      DESCRIPTION
         "Maximum Interleave Delay on Downstream direction.  The maximum
          one-way interleaving delay introduced by the PMS-TC on
          Downstream direction.  The ATUs shall choose the S (factor)
          and D (depth) values such that the actual one-way interleaving
          delay (adsl2ChStatusActDelay) is as close as possible to,
          but less than or equal to, adsl2ChConfProfMaxDelayDs.  The
          delay is coded in ms, with the value 0 indicating no delay
          bound is being imposed."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.2"
      ::= { adsl2ChConfProfileEntry 9 }

   adsl2ChConfProfMaxDelayUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..63)
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Maximum Interleave Delay on Upstream direction.  The maximum
          one-way interleaving delay introduced by the PMS-TC on
          Upstream direction.  The ATUs shall choose the S (factor) and
          D (depth) values such that the actual one-way interleaving
          delay (adsl2ChStatusActDelay) is as close as possible to,
          but less than or equal to, adsl2ChConfProfMaxDelayUs.  The
          delay is coded in ms, with the value 0 indicating no delay
          bound is being imposed."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.2"
      ::= { adsl2ChConfProfileEntry 10 }

   adsl2ChConfProfMinProtectionDs  OBJECT-TYPE
      SYNTAX      Adsl2SymbolProtection
      UNITS       "symbols"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Minimum Impulse Noise Protection on Downstream direction.  The
          minimum impulse noise protection for the bearer channel,
          expressed in symbols.  The parameter can take the following
          values: noProtection (i.e., INP not required), halfSymbol
          (i.e., INP length is 1/2 symbol), and 1-16 symbols in steps
          of 1 symbol."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.3"
      DEFVAL       { noProtection }
      ::= { adsl2ChConfProfileEntry 11 }

   adsl2ChConfProfMinProtectionUs  OBJECT-TYPE
      SYNTAX      Adsl2SymbolProtection
      UNITS       "symbols"





      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Minimum Impulse Noise Protection on Upstream direction.  The
          minimum impulse noise protection for the bearer channel,
          expressed in symbols.  The parameter can take the following
          values: noProtection (i.e., INP not required), halfSymbol
          (i.e., INP length is 1/2 symbol), and 1-16 symbols in steps
          of 1 symbol."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.3"
      DEFVAL       { noProtection }
      ::= { adsl2ChConfProfileEntry 12 }

   adsl2ChConfProfMaxBerDs  OBJECT-TYPE
      SYNTAX      Adsl2MaxBer
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Maximum Bit Error Ratio on Downstream direction.  The maximum
          bit error ratio for the bearer channel.  The parameter can
          take the following values (for 1E-3, 1E-5 or 1E-7):
             eminus3(1),
             eminus5(2), or
             eminus7(3)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.4"
      DEFVAL       { eminus5 }
     ::= { adsl2ChConfProfileEntry 13 }

   adsl2ChConfProfMaxBerUs  OBJECT-TYPE
      SYNTAX      Adsl2MaxBer
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Maximum Bit Error Ratio on Upstream direction.  The maximum
          bit error ratio for the bearer channel.  The parameter can
          take the following values (for 1E-3, 1E-5 or 1E-7):
             eminus3(1),
             eminus5(2), or
             eminus7(3)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.4"
      DEFVAL       { eminus5 }
      ::= { adsl2ChConfProfileEntry 14 }

   adsl2ChConfProfUsDataRateDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current





      DESCRIPTION
         "Data Rate Threshold Up shift for downstream direction.  An
          'Up-shift rate change' event is triggered when the actual
          downstream data rate exceeds, by more than the threshold, the
          data rate at the last entry into Showtime.  The parameter is
          coded in bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.6"
      ::= { adsl2ChConfProfileEntry 15 }

   adsl2ChConfProfDsDataRateDs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Data Rate Threshold Down-shift for downstream direction.  A
          'Down-shift rate change' event is triggered when the actual
          downstream data rate is below the data rate at the last entry
          into Showtime, by more than the threshold.  The parameter is
          coded in bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.6"
      ::= { adsl2ChConfProfileEntry 16 }

   adsl2ChConfProfUsDataRateUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Data Rate Threshold Up shift for upstream direction.  An
          'Up-shift rate change' event is triggered when the actual
          upstream data rate exceeds, by more than the threshold, the
          data rate at the last entry into Showtime.  The parameter is
          coded in bits/second."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.6"
      ::= { adsl2ChConfProfileEntry 17 }

   adsl2ChConfProfDsDataRateUs  OBJECT-TYPE
      SYNTAX      Unsigned32(0..200000000)
      UNITS       "bits/second"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Data Rate Threshold Down-shift for upstream direction.  A
          'Down-shift rate change' event is triggered when the actual
          upstream data rate is below the data rate at the last entry
          into Showtime, by more than the threshold.  The parameter is
          coded in bits/second."





      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2.6"
      ::= { adsl2ChConfProfileEntry 18 }

   adsl2ChConfProfImaEnabled  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "IMA Mode Enable.  The parameter enables the IMA operation mode
          in the ATM Data Path.  Relevant only if the channel is an ATM
          Data Path.  When in 'enable' state, the ATM data path should
          comply with the requirements for IMA transmission."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.4.1"
      DEFVAL       { false }
    ::= { adsl2ChConfProfileEntry 19 }

   adsl2ChConfProfRowStatus  OBJECT-TYPE
      SYNTAX      RowStatus
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "This object is used to create a new row or to modify or
         delete an existing row in this table.

         A profile is activated by setting this object to 'active'.
         When 'active' is set, the system will validate the profile.

         Before a profile can be deleted or taken out of service
         (by setting this object to 'destroy' or 'notInService'),
         it must first be unreferenced from all associated
         templates."
      ::= { adsl2ChConfProfileEntry 20 }

   ------------------------------------------------
   --        adsl2LineAlarmConfTemplateTable          --
   ------------------------------------------------
   adsl2LineAlarmConfTemplateTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2LineAlarmConfTemplateEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineAlarmConfTemplateTable contains
          ADSL2 line configuration templates.

          Entries in this table MUST be maintained in a
          persistent manner."
      ::= { adsl2ProfileAlarmConf 1 }






   adsl2LineAlarmConfTemplateEntry  OBJECT-TYPE
      SYNTAX      Adsl2LineAlarmConfTemplateEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2LineAlarmConfTemplateTable contains ADSL2
         line PM thresholds templates.
         A default template with an index of 'DEFVAL' will
         always exist, and its parameters will be set to vendor-
         specific values, unless otherwise specified in this
         document."
      INDEX  { adsl2LAlarmConfTempTemplateName }
      ::= { adsl2LineAlarmConfTemplateTable 1 }

   Adsl2LineAlarmConfTemplateEntry  ::=
      SEQUENCE {
         adsl2LAlarmConfTempTemplateName      SnmpAdminString,
         adsl2LAlarmConfTempLineProfile       SnmpAdminString,
         adsl2LAlarmConfTempChan1ConfProfile  SnmpAdminString,
         adsl2LAlarmConfTempChan2ConfProfile  SnmpAdminString,
         adsl2LAlarmConfTempChan3ConfProfile  SnmpAdminString,
         adsl2LAlarmConfTempChan4ConfProfile  SnmpAdminString,
         adsl2LAlarmConfTempRowStatus         RowStatus
      }

   adsl2LAlarmConfTempTemplateName  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This object identifies a row in this table."
      ::= { adsl2LineAlarmConfTemplateEntry 1 }

   adsl2LAlarmConfTempLineProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2 Line
          Thresholds Configuration Profile Table
          (adsl2LineAlarmConfProfileTable) that applies to this ADSL2
          line."
      REFERENCE    "DSL Forum TR-90, paragraph 5.4.1"
      DEFVAL       { "DEFVAL" }
      ::= { adsl2LineAlarmConfTemplateEntry 2 }

   adsl2LAlarmConfTempChan1ConfProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(1..32))





      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2
          Channel Thresholds Configuration Profile Table
          (adsl2ChAlarmConfProfileTable) that applies for ADSL2
          bearer channel #1.  The channel profile name specified here
          must match the name of an existing row in the
          adsl2ChAlarmConfProfileTable table."
      REFERENCE    "DSL Forum TR-90, paragraph 5.4.1"
      DEFVAL       { "DEFVAL" }
      ::= { adsl2LineAlarmConfTemplateEntry 3 }

   adsl2LAlarmConfTempChan2ConfProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(0..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2
          Channel Thresholds Configuration Profile Table
          (adsl2ChAlarmConfProfileTable) that applies for ADSL2
          bearer channel #2.  The channel profile name specified here
          must match the name of an existing row in the
          adsl2ChAlarmConfProfileTable table.  If the channel is unused,
          then the object is set to a zero-length string."
      REFERENCE    "DSL Forum TR-90, paragraph 5.4.1"
      DEFVAL       { "" }
      ::= { adsl2LineAlarmConfTemplateEntry 4 }

   adsl2LAlarmConfTempChan3ConfProfile  OBJECT-TYPE
      SYNTAX      SnmpAdminString (SIZE(0..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2
          Channel Thresholds Configuration Profile Table
          (adsl2ChAlarmConfProfileTable) that applies for ADSL2
          bearer channel #3.  The channel profile name specified here
          must match the name of an existing row in the
          adsl2ChAlarmConfProfileTable table.
          This object may be set to a non-zero-length string only if
          adsl2LAlarmConfTempChan2ConfProfile contains a non-zero-
          length string."
      REFERENCE    "DSL Forum TR-90, paragraph 5.4.1"
      DEFVAL       { "" }
      ::= { adsl2LineAlarmConfTemplateEntry 5 }

   adsl2LAlarmConfTempChan4ConfProfile  OBJECT-TYPE





      SYNTAX      SnmpAdminString (SIZE(0..32))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The value of this object identifies the row in the ADSL2
          Channel Thresholds Configuration Profile Table
          (adsl2ChAlarmConfProfileTable) that applies for ADSL2
          bearer channel #4.  The channel profile name specified here
          must match the name of an existing row in the
          adsl2ChAlarmConfProfileTable table.
          This object may be set to a non-zero-length string only if
          adsl2LAlarmConfTempChan3ConfProfile contains a non-zero-
          length string."
      REFERENCE    "DSL Forum TR-90, paragraph 5.4.1"
      DEFVAL       { "" }
      ::= { adsl2LineAlarmConfTemplateEntry 6 }

   adsl2LAlarmConfTempRowStatus  OBJECT-TYPE
      SYNTAX      RowStatus
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "This object is used to create a new row or to modify or
         delete an existing row in this table.

         A template is activated by setting this object to 'active'.
         When 'active' is set, the system will validate the template.

         Before a template can be deleted or taken out of service
         (by setting this object to 'destroy' or 'notInService'),
         it must first be unreferenced from all associated
         lines."
      ::= { adsl2LineAlarmConfTemplateEntry 7 }

   ------------------------------------------------
   --      adsl2LineAlarmConfProfileTable        --
   ------------------------------------------------

   adsl2LineAlarmConfProfileTable  OBJECT-TYPE
        SYNTAX      SEQUENCE  OF  Adsl2LineAlarmConfProfileEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "The table adsl2LineAlarmConfProfileTable contains ADSL2
         line PM thresholds profiles.

          Entries in this table MUST be maintained in a
          persistent manner."





        ::= { adsl2ProfileAlarmConf 2 }

   adsl2LineAlarmConfProfileEntry  OBJECT-TYPE
        SYNTAX      Adsl2LineAlarmConfProfileEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "The table adsl2LineAlarmConfProfileTable contains ADSL2
         line PM thresholds profiles.
         A default profile with an index of 'DEFVAL' will
         always exist, and its parameters will be set to vendor-
         specific values, unless otherwise specified in this
         document."
        INDEX  { adsl2LineAlarmConfProfileName }
        ::= { adsl2LineAlarmConfProfileTable 1 }

   Adsl2LineAlarmConfProfileEntry ::=
        SEQUENCE {
        adsl2LineAlarmConfProfileName                SnmpAdminString,
        adsl2LineAlarmConfProfileAtucThresh15MinFecs
                                             HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAtucThresh15MinEs
                                             HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAtucThresh15MinSes
                                              HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAtucThresh15MinLoss
                                              HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAtucThresh15MinUas
                                              HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAturThresh15MinFecs
                                              HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAturThresh15MinEs
                                              HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAturThresh15MinSes
                                              HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAturThresh15MinLoss
                                              HCPerfIntervalThreshold,
        adsl2LineAlarmConfProfileAturThresh15MinUas
                                              HCPerfIntervalThreshold,

        adsl2LineAlarmConfProfileThresh15MinFailedFullInt   Unsigned32,
        adsl2LineAlarmConfProfileThresh15MinFailedShrtInt   Unsigned32,

        adsl2LineAlarmConfProfileRowStatus                   RowStatus
        }

   adsl2LineAlarmConfProfileName  OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(1..32))





        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
        "This object identifies a row in this table."
        ::= { adsl2LineAlarmConfProfileEntry 1 }

   adsl2LineAlarmConfProfileAtucThresh15MinFecs  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MFecs counter,
        when adsl2PMLCurrUnit is atuc(1).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 2 }

   adsl2LineAlarmConfProfileAtucThresh15MinEs  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MEs counter,
        when adsl2PMLCurrUnit is atuc(1).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 3 }

   adsl2LineAlarmConfProfileAtucThresh15MinSes  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MSes counter,
        when adsl2PMLCurrUnit is atuc(1).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 4 }






   adsl2LineAlarmConfProfileAtucThresh15MinLoss  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MLoss counter,
        when adsl2PMLCurrUnit is atuc(1).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 5 }

   adsl2LineAlarmConfProfileAtucThresh15MinUas  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MUas counter,
        when adsl2PMLCurrUnit is atuc(1).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 6 }

   adsl2LineAlarmConfProfileAturThresh15MinFecs  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MFecs counter,
        when adsl2PMLCurrUnit is atur(2).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 7 }

   adsl2LineAlarmConfProfileAturThresh15MinEs  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION





        "A threshold for the adsl2PMLCurr15MEs counter,
        when adsl2PMLCurrUnit is atur(2).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 8 }

   adsl2LineAlarmConfProfileAturThresh15MinSes  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MSes counter,
        when adsl2PMLCurrUnit is atur(2).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 9 }

   adsl2LineAlarmConfProfileAturThresh15MinLoss  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MLoss counter,
        when adsl2PMLCurrUnit is atur(2).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 10 }

   adsl2LineAlarmConfProfileAturThresh15MinUas  OBJECT-TYPE
        SYNTAX      HCPerfIntervalThreshold
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurr15MUas counter,
        when adsl2PMLCurrUnit is atur(2).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }





        ::= { adsl2LineAlarmConfProfileEntry 11 }

   adsl2LineAlarmConfProfileThresh15MinFailedFullInt  OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurrInit15MfailedFullInits
        counter.
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 12 }

   adsl2LineAlarmConfProfileThresh15MinFailedShrtInt  OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMLCurrInit15MFailedShortInits
        counter.
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.1"
      DEFVAL       { 0 }
        ::= { adsl2LineAlarmConfProfileEntry 13 }

   adsl2LineAlarmConfProfileRowStatus  OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "This object is used to create a new row or to modify or
         delete an existing row in this table.

         A profile is activated by setting this object to 'active'.
         When 'active' is set, the system will validate the profile.

         Before a profile can be deleted or taken out of service
         (by setting this object to 'destroy' or 'notInService'),
         it must first be unreferenced from all associated
         templates."
        ::= { adsl2LineAlarmConfProfileEntry 14 }


   ------------------------------------------------
   --      adsl2ChAlarmConfProfileTable        --





   ------------------------------------------------

   adsl2ChAlarmConfProfileTable  OBJECT-TYPE
        SYNTAX      SEQUENCE  OF  Adsl2ChAlarmConfProfileEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "The table adsl2ChAlarmConfProfileTable contains ADSL2
         channel PM thresholds profiles.

          Entries in this table MUST be maintained in a
          persistent manner."
        ::= { adsl2ProfileAlarmConf 3 }

   adsl2ChAlarmConfProfileEntry  OBJECT-TYPE
        SYNTAX      Adsl2ChAlarmConfProfileEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
         "The table adsl2ChAlarmConfProfileTable contains ADSL2
         channel PM thresholds profiles.
         A default profile with an index of 'DEFVAL' will
         always exist, and its parameters will be set to vendor-
         specific values, unless otherwise specified in this document."
        INDEX  { adsl2ChAlarmConfProfileName }
        ::= { adsl2ChAlarmConfProfileTable 1 }

   Adsl2ChAlarmConfProfileEntry ::=
        SEQUENCE {
        adsl2ChAlarmConfProfileName
                                                        SnmpAdminString,
        adsl2ChAlarmConfProfileAtucThresh15MinCodingViolations
                                                        Unsigned32,
        adsl2ChAlarmConfProfileAtucThresh15MinCorrected Unsigned32,
        adsl2ChAlarmConfProfileAturThresh15MinCodingViolations
                                                        Unsigned32,
        adsl2ChAlarmConfProfileAturThresh15MinCorrected Unsigned32,
        adsl2ChAlarmConfProfileRowStatus                RowStatus
        }

   adsl2ChAlarmConfProfileName  OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(1..32))
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
        "This object identifies a row in this table."
        ::= { adsl2ChAlarmConfProfileEntry 1 }






   adsl2ChAlarmConfProfileAtucThresh15MinCodingViolations OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMChCurr15MCodingViolations
        counter, when adsl2PMChCurrUnit is atuc(1).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2"
      DEFVAL       { 0 }
        ::= { adsl2ChAlarmConfProfileEntry 2 }

   adsl2ChAlarmConfProfileAtucThresh15MinCorrected  OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMChCurr15MCorrectedBlocks
        counter, when adsl2PMChCurrUnit is atuc(1).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2"
      DEFVAL       { 0 }
        ::= { adsl2ChAlarmConfProfileEntry 3 }

   adsl2ChAlarmConfProfileAturThresh15MinCodingViolations  OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMChCurr15MCodingViolations
        counter, when adsl2PMChCurrUnit is atur(2).
        The value 0 means that no threshold is specified for the
        associated counter."
      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2"
      DEFVAL       { 0 }
        ::= { adsl2ChAlarmConfProfileEntry 4 }

   adsl2ChAlarmConfProfileAturThresh15MinCorrected  OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
        "A threshold for the adsl2PMChCurr15MCorrectedBlocks
        counter, when adsl2PMChCurrUnit is atur(2).
        The value 0 means that no threshold is specified for the
        associated counter."





      REFERENCE    "ITU-T G.997.1, paragraph 7.3.2"
      DEFVAL       { 0 }
        ::= { adsl2ChAlarmConfProfileEntry 5 }

   adsl2ChAlarmConfProfileRowStatus  OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
         "This object is used to create a new row or to modify or
         delete an existing row in this table.

         A profile is activated by setting this object to 'active'.
         When 'active' is set, the system will validate the profile.

         Before a profile can be deleted or taken out of service
         (by setting this object to 'destroy' or 'notInService'),
         it must first be unreferenced from all associated
         templates."
        ::= { adsl2ChAlarmConfProfileEntry 6 }

   ------------------------------------------------
   --          PM line current counters          --
   ------------------------------------------------
   adsl2PMLineCurrTable  OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMLineCurrEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineCurrTable contains current Performance
          Monitoring results of ADSL2 lines."
      ::= { adsl2PMLine 1 }

   adsl2PMLineCurrEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMLineCurrEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineCurrTable contains current Performance
          Monitoring results of ADSL2 lines.
          The index of this table consists of an interface index, where
          the interface has an ifType of adsl2plus(238), along with a
          termination unit.
          The PM counters in the table are not reset even when the XTU
          is reinitialized.  They are reinitialized only when the
          agent itself is reset or reinitialized."
      INDEX  { ifIndex, adsl2PMLCurrUnit }
      ::= { adsl2PMLineCurrTable 1 }





   Adsl2PMLineCurrEntry  ::=
      SEQUENCE {
         adsl2PMLCurrUnit                    Adsl2Unit,
         adsl2PMLCurrValidIntervals          Unsigned32,
         adsl2PMLCurrInvalidIntervals        Unsigned32,
         adsl2PMLCurr15MTimeElapsed          HCPerfTimeElapsed,
         adsl2PMLCurr15MFecs                 Counter32,
         adsl2PMLCurr15MEs                   Counter32,
         adsl2PMLCurr15MSes                  Counter32,
         adsl2PMLCurr15MLoss                 Counter32,
         adsl2PMLCurr15MUas                  Counter32,
         adsl2PMLCurr1DayValidIntervals      Unsigned32,
         adsl2PMLCurr1DayInvalidIntervals    Unsigned32,
         adsl2PMLCurr1DayTimeElapsed         HCPerfTimeElapsed,
         adsl2PMLCurr1DayFecs                Counter32,
         adsl2PMLCurr1DayEs                  Counter32,
         adsl2PMLCurr1DaySes                 Counter32,
         adsl2PMLCurr1DayLoss                Counter32,
         adsl2PMLCurr1DayUas                 Counter32
      }

   adsl2PMLCurrUnit  OBJECT-TYPE
      SYNTAX      Adsl2Unit
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The termination unit atuc(1) or atur(2)."
      ::= { adsl2PMLineCurrEntry 1 }

   adsl2PMLCurrValidIntervals  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Valid intervals."
      ::= { adsl2PMLineCurrEntry 2 }

   adsl2PMLCurrInvalidIntervals  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Invalid intervals."
      ::= { adsl2PMLineCurrEntry 3 }

   adsl2PMLCurr15MTimeElapsed  OBJECT-TYPE
      SYNTAX      HCPerfTimeElapsed
      UNITS       "seconds"





      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total elapsed seconds since this PM interval began.
          Note that the PM counters are not reset even when the XTU
          is reinitialized.  They are reinitialized only when the
          agent itself is reset or reinitialized."
      ::= { adsl2PMLineCurrEntry 4 }

   adsl2PMLCurr15MFecs  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was at least
          one FEC correction event for one or more bearer channels in
          this line.  This parameter is inhibited during UAS or SES."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 5 }

   adsl2PMLCurr15MEs  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was:
             ATU-C: CRC-8 >= 1 for one or more bearer channels OR
                    LOS >= 1 OR SEF >=1 OR LPR >= 1
             ATU-R: FEBE >= 1 for one or more bearer channels OR
                    LOS-FE >=1 OR RDI >=1 OR LPR-FE >=1 .
          This parameter is inhibited during UAS."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 6 }

   adsl2PMLCurr15MSes  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was:
             ATU-C: (CRC-8 summed over all bearer channels) >= 18 OR
                    LOS >= 1 OR SEF >= 1 OR LPR >= 1
             ATU-R: (FEBE summed over all bearer channels) >= 18 OR
                    LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1 .
          This parameter is inhibited during UAS."





      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 7 }

   adsl2PMLCurr15MLoss  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was LOS (or
          LOS-FE for ATU-R)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 8 }

   adsl2PMLCurr15MUas  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds in Unavailability State during this
          interval.  Unavailability begins at the onset of 10
          contiguous severely-errored seconds, and ends at the
          onset of 10 contiguous seconds with no severely-errored
          seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 9 }

   adsl2PMLCurr1DayValidIntervals  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Valid intervals."
      ::= { adsl2PMLineCurrEntry 10 }

   adsl2PMLCurr1DayInvalidIntervals  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Invalid intervals."
      ::= { adsl2PMLineCurrEntry 11 }

   adsl2PMLCurr1DayTimeElapsed  OBJECT-TYPE
      SYNTAX      HCPerfTimeElapsed
      UNITS       "seconds"
      MAX-ACCESS  read-only





      STATUS      current
      DESCRIPTION
         "Total elapsed seconds since this PM interval began.
          Note that the PM counters are not reset even when the XTU
          is reinitialized.  They are reinitialized only when the
          agent itself is reset or reinitialized."
      ::= { adsl2PMLineCurrEntry 12 }

   adsl2PMLCurr1DayFecs  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was at least
          one FEC correction event for one or more bearer channels in
          this line.  This parameter is inhibited during UAS or SES."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 13 }

   adsl2PMLCurr1DayEs  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was:
             ATU-C: CRC-8 >= 1 for one or more bearer channels OR
                    LOS >= 1 OR SEF >= 1 OR LPR >= 1
             ATU-R: FEBE >= 1 for one or more bearer channels OR
                    LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1.
          This parameter is inhibited during UAS."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 14 }

   adsl2PMLCurr1DaySes  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was:
             ATU-C: (CRC-8 summed over all bearer channels) >= 18 OR
                     LOS >= 1 OR SEF >= 1 OR LPR >= 1
             ATU-R: (FEBE summed over all bearer channels) >= 18 OR
                    LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1
          This parameter is inhibited during UAS."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"





      ::= { adsl2PMLineCurrEntry 15 }

   adsl2PMLCurr1DayLoss  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was LOS (or
          LOS-FE for ATU-R)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 16 }

   adsl2PMLCurr1DayUas  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds in Unavailability State during this interval.
          Unavailability begins at the onset of 10 contiguous severely-
          errored seconds, and ends at the onset of 10 contiguous
          seconds with no severely-errored seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrEntry 17 }


   ------------------------------------------------
   --          PM line init current counters     --
   ------------------------------------------------

   adsl2PMLineCurrInitTable   OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMLineCurrInitEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineCurrInitTable contains current
          initialization counters of the ADSL2 line.
          The PM counters in the table are not reset even when the XTU
          is reinitialized.  They are reinitialized only when the
          agent itself is reset or reinitialized."
      ::= { adsl2PMLine 2 }

   adsl2PMLineCurrInitEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMLineCurrInitEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION





         "The table adsl2PMLineCurrInitTable contains current
          initialization counters of the ADSL2 line.
          The index of this table consists of an interface index, where
          the interface has an ifType of adsl2plus(238), and a
          termination unit."
      INDEX  { ifIndex }
      ::= { adsl2PMLineCurrInitTable 1 }

   Adsl2PMLineCurrInitEntry  ::=
      SEQUENCE {
         adsl2PMLCurrInit15MTimeElapsed          Unsigned32,
         adsl2PMLCurrInit15MFullInits            Unsigned32,
         adsl2PMLCurrInit15MFailedFullInits      Unsigned32,
         adsl2PMLCurrInit15MShortInits           Unsigned32,
         adsl2PMLCurrInit15MFailedShortInits     Unsigned32,
         adsl2PMLCurrInit1DayTimeElapsed         Unsigned32,
         adsl2PMLCurrInit1DayFullInits           Unsigned32,
         adsl2PMLCurrInit1DayFailedFullInits     Unsigned32,
         adsl2PMLCurrInit1DayShortInits          Unsigned32,
         adsl2PMLCurrInit1DayFailedShortInits    Unsigned32
      }

   adsl2PMLCurrInit15MTimeElapsed  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total elapsed seconds since this PM interval began.
          Note that the PM counters are not reset even when the XTU
          is reinitialized.  They are reinitialized only when the
          agent itself is reset or reinitialized."
      ::= { adsl2PMLineCurrInitEntry 1 }

   adsl2PMLCurrInit15MFullInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of full initializations attempted on the line
          (successful and failed) during this interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrInitEntry 2 }

   adsl2PMLCurrInit15MFailedFullInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current





      DESCRIPTION
         "Count of failed full initializations on the line during this
          interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrInitEntry 3 }

   adsl2PMLCurrInit15MShortInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of short initializations attempted on the line
          (successful and failed) during this interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrInitEntry 4 }

   adsl2PMLCurrInit15MFailedShortInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of failed short initializations on the line during this
          interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrInitEntry 5 }

   adsl2PMLCurrInit1DayTimeElapsed  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total elapsed seconds since this PM interval began.
          Note that the PM counters are not reset even when the XTU
          is reinitialized.  They are reinitialized only when the
          agent itself is reset or reinitialized."
      ::= { adsl2PMLineCurrInitEntry 6 }

   adsl2PMLCurrInit1DayFullInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of full initializations attempted on the line
          (successful and failed) during this interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrInitEntry 7 }






   adsl2PMLCurrInit1DayFailedFullInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of failed full initializations on the line during this
          interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrInitEntry 8 }

   adsl2PMLCurrInit1DayShortInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of short initializations attempted on the line
          (successful and failed) during this interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrInitEntry 9 }

   adsl2PMLCurrInit1DayFailedShortInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of failed short initializations on the line during this
          interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineCurrInitEntry 10 }



   -------------------------------------------
   --       PM line history 15 Minutes      --
   -------------------------------------------
   adsl2PMLineHist15MinTable    OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMLineHist15MinEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineHist15MinTable contains PM line history
         for 15min intervals of the ADSL2 line."
      ::= { adsl2PMLine 3 }

   adsl2PMLineHist15MinEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMLineHist15MinEntry
      MAX-ACCESS  not-accessible
      STATUS      current





      DESCRIPTION
         "The table adsl2PMLineHist15MinTable contains PM line history
          for 15min intervals of the ADSL2 line.
          The index of this table consists of an interface index, where
          the interface has an ifType of adsl2plus(238), along with a
          termination unit, and an interval number."
      INDEX  { ifIndex,
               adsl2PMLHist15MUnit,
               adsl2PMLHist15MInterval }
      ::= { adsl2PMLineHist15MinTable 1 }

   Adsl2PMLineHist15MinEntry  ::=
      SEQUENCE {
         adsl2PMLHist15MUnit                 Adsl2Unit,
         adsl2PMLHist15MInterval             Unsigned32,
         adsl2PMLHist15MMonitoredTime        Unsigned32,
         adsl2PMLHist15MFecs                 Counter32,
         adsl2PMLHist15MEs                   Counter32,
         adsl2PMLHist15MSes                  Counter32,
         adsl2PMLHist15MLoss                 Counter32,
         adsl2PMLHist15MUas                  Counter32,
         adsl2PMLHist15MValidInterval        TruthValue
      }

   adsl2PMLHist15MUnit  OBJECT-TYPE
      SYNTAX      Adsl2Unit
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The termination unit atuc(1) or atur(2)."
      ::= { adsl2PMLineHist15MinEntry 1 }

   adsl2PMLHist15MInterval  OBJECT-TYPE
      SYNTAX      Unsigned32 (1..96)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The interval number."
      ::= { adsl2PMLineHist15MinEntry 2 }

   adsl2PMLHist15MMonitoredTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total seconds monitored in this interval."
      ::= { adsl2PMLineHist15MinEntry 3 }





   adsl2PMLHist15MFecs  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was at least
          one FEC correction event for one or more bearer channels in
          this line.  This parameter is inhibited during UAS or SES."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist15MinEntry 4 }

   adsl2PMLHist15MEs  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was:
             ATU-C: CRC-8 >= 1 for one or more bearer channels OR
                    LOS >= 1 OR SEF >= 1 OR LPR >= 1
             ATU-R: FEBE >= 1 for one or more bearer channels OR
                    LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1.
          This parameter is inhibited during UAS."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist15MinEntry 5 }

   adsl2PMLHist15MSes  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was:
             ATU-C: (CRC-8 summed over all bearer channels) >= 18 OR
                    LOS >= 1 OR SEF >= 1 OR LPR >= 1
             ATU-R: (FEBE summed over all bearer channels) >= 18 OR
                    LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1.
          This parameter is inhibited during UAS."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist15MinEntry 6 }

   adsl2PMLHist15MLoss  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION





         "Count of seconds during this interval where there was LOS (or
          LOS-FE for ATU-R)."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist15MinEntry 7 }

   adsl2PMLHist15MUas  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds in Unavailability State during this interval.
          Unavailability begins at the onset of 10 contiguous severely-
          errored seconds, and ends at the onset of 10 contiguous
          seconds with no severely-errored seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist15MinEntry 8 }

   adsl2PMLHist15MValidInterval  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This variable indicates if the data for this interval is
          valid."
      ::= { adsl2PMLineHist15MinEntry 9 }



   ---------------------------------------
   --       PM line history 1 Day       --
   ---------------------------------------
   adsl2PMLineHist1DayTable     OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMLineHist1DayEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineHist1DayTable contains PM line history
          for 24-hour intervals of the ADSL2 line."
      ::= { adsl2PMLine 4 }

   adsl2PMLineHist1DayEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMLineHist1DayEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineHist1DayTable contains PM line history
          for 24-hour intervals of the ADSL2 line.





          The index of this table consists of an interface index, where
          the interface has an ifType of adsl2plus(238), along with a
          termination unit, and an interval number."
      INDEX  { ifIndex,
               adsl2PMLHist1DUnit,
               adsl2PMLHist1DInterval }
      ::= { adsl2PMLineHist1DayTable 1 }

   Adsl2PMLineHist1DayEntry  ::=
      SEQUENCE {
         adsl2PMLHist1DUnit              Adsl2Unit,
         adsl2PMLHist1DInterval          Unsigned32,
         adsl2PMLHist1DMonitoredTime     Unsigned32,
         adsl2PMLHist1DFecs              Counter32,
         adsl2PMLHist1DEs                Counter32,
         adsl2PMLHist1DSes               Counter32,
         adsl2PMLHist1DLoss              Counter32,
         adsl2PMLHist1DUas               Counter32,
         adsl2PMLHist1DValidInterval     TruthValue
      }

   adsl2PMLHist1DUnit  OBJECT-TYPE
      SYNTAX      Adsl2Unit
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The termination unit."
      ::= { adsl2PMLineHist1DayEntry 1 }

   adsl2PMLHist1DInterval  OBJECT-TYPE
      SYNTAX      Unsigned32 (1..30)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The interval number."
      ::= { adsl2PMLineHist1DayEntry 2 }

   adsl2PMLHist1DMonitoredTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total seconds monitored in this interval."
      ::= { adsl2PMLineHist1DayEntry 3 }

   adsl2PMLHist1DFecs  OBJECT-TYPE
      SYNTAX      Counter32





      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was at least
          one FEC correction event for one or more bearer channels in
          this line.  This parameter is inhibited during UAS or SES."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist1DayEntry 4 }

   adsl2PMLHist1DEs  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was:
             ATU-C: CRC-8 >= 1 for one or more bearer channels OR
                    LOS >= 1 OR SEF >= 1 OR LPR >= 1
             ATU-R: FEBE >= 1 for one or more bearer channels OR
                    LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1.
          This parameter is inhibited during UAS."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist1DayEntry 5 }

   adsl2PMLHist1DSes  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was:
             ATU-C: (CRC-8 summed over all bearer channels) >= 18 OR
                     LOS >= 1 OR SEF >> 1 OR LPR >= 1
             ATU-R: (FEBE summed over all bearer channels) >= 18 OR
                     LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1.
          This parameter is inhibited during UAS."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist1DayEntry 6 }

   adsl2PMLHist1DLoss  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds during this interval where there was LOS (or
          LOS-FE for ATU-R)."





      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist1DayEntry 7 }

   adsl2PMLHist1DUas  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of seconds in Unavailability State during this interval.
          Unavailability begins at the onset of 10 contiguous severely-
          errored seconds, and ends at the onset of 10 contiguous
          seconds with no severely-errored seconds."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineHist1DayEntry 8 }

   adsl2PMLHist1DValidInterval  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This variable indicates if the data for this interval is
          valid."
      ::= { adsl2PMLineHist1DayEntry 9 }




   -------------------------------------------
   --     PM line init history 15 Minutes   --
   -------------------------------------------

   adsl2PMLineInitHist15MinTable      OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMLineInitHist15MinEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineInitHist15MinTable contains PM line
          initialization history for 15-minute intervals of the ADSL2
          line."
      ::= { adsl2PMLine 5 }

   adsl2PMLineInitHist15MinEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMLineInitHist15MinEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineInitHist15MinTable contains PM line





          initialization history for 15 minutes intervals of the ADSL2
          line.
          The index of this table consists of an interface index, where
          the interface has an ifType of adsl2plus(238), and an interval
          number."
      INDEX  { ifIndex,
               adsl2PMLHistInit15MInterval }
      ::= { adsl2PMLineInitHist15MinTable 1 }

   Adsl2PMLineInitHist15MinEntry  ::=
      SEQUENCE {
         adsl2PMLHistInit15MInterval              Unsigned32,
         adsl2PMLHistInit15MMonitoredTime         Unsigned32,
         adsl2PMLHistInit15MFullInits             Unsigned32,
         adsl2PMLHistInit15MFailedFullInits       Unsigned32,
         adsl2PMLHistInit15MShortInits            Unsigned32,
         adsl2PMLHistInit15MFailedShortInits      Unsigned32,
         adsl2PMLHistInit15MValidInterval         TruthValue
      }

   adsl2PMLHistInit15MInterval  OBJECT-TYPE
      SYNTAX      Unsigned32 (1..96)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The interval number."
      ::= { adsl2PMLineInitHist15MinEntry 1 }

   adsl2PMLHistInit15MMonitoredTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total seconds monitored in this interval."
      ::= { adsl2PMLineInitHist15MinEntry 2 }

   adsl2PMLHistInit15MFullInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of full initializations attempted on the line
          (successful and failed) during this interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineInitHist15MinEntry 3 }

   adsl2PMLHistInit15MFailedFullInits  OBJECT-TYPE





      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of failed full initializations on the line during this
          interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineInitHist15MinEntry 4 }

   adsl2PMLHistInit15MShortInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of short initializations attempted on the line
          (successful and failed) during this interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineInitHist15MinEntry 5 }

   adsl2PMLHistInit15MFailedShortInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of failed short initializations on the line during this
          interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineInitHist15MinEntry 6 }

   adsl2PMLHistInit15MValidInterval  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This variable indicates if the data for this interval is
          valid."
      ::= { adsl2PMLineInitHist15MinEntry 7 }



   -------------------------------------------
   --       PM line init history 1 Day      --
   -------------------------------------------
   adsl2PMLineInitHist1DayTable       OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMLineInitHist1DayEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION





         "The table adsl2PMLineInitHist1DayTable contains PM line
          initialization history for 24-hour intervals of the ADSL2
          line."
      ::= { adsl2PMLine 6 }

   adsl2PMLineInitHist1DayEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMLineInitHist1DayEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMLineInitHist1DayTable contains PM line
          initialization history for 24-hour intervals of the ADSL2
          line.
          The index of this table consists of an interface index, where
          the interface has an ifType of adsl2plus(238), and an interval
          number."
      INDEX  { ifIndex,
               adsl2PMLHistinit1DInterval }
      ::= { adsl2PMLineInitHist1DayTable 1 }

   Adsl2PMLineInitHist1DayEntry  ::=
      SEQUENCE {
         adsl2PMLHistinit1DInterval              Unsigned32,
         adsl2PMLHistinit1DMonitoredTime         Unsigned32,
         adsl2PMLHistinit1DFullInits             Unsigned32,
         adsl2PMLHistinit1DFailedFullInits       Unsigned32,
         adsl2PMLHistinit1DShortInits            Unsigned32,
         adsl2PMLHistinit1DFailedShortInits      Unsigned32,
         adsl2PMLHistinit1DValidInterval         TruthValue
      }

   adsl2PMLHistinit1DInterval  OBJECT-TYPE
      SYNTAX      Unsigned32 (1..30)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The interval number."
      ::= { adsl2PMLineInitHist1DayEntry 1 }

   adsl2PMLHistinit1DMonitoredTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total seconds monitored in this interval."
      ::= { adsl2PMLineInitHist1DayEntry 2 }






   adsl2PMLHistinit1DFullInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of full initializations attempted on the line
          (successful and failed) during this interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
       ::= { adsl2PMLineInitHist1DayEntry 3 }

   adsl2PMLHistinit1DFailedFullInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of failed full initializations on the line during this
          interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineInitHist1DayEntry 4 }

   adsl2PMLHistinit1DShortInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of short initializations attempted on the line
          (successful and failed) during this interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineInitHist1DayEntry 5 }

   adsl2PMLHistinit1DFailedShortInits  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of failed short initializations on the line during this
          interval."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.1"
      ::= { adsl2PMLineInitHist1DayEntry 6 }

   adsl2PMLHistinit1DValidInterval  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This variable indicates if the data for this interval is
          valid."
      ::= { adsl2PMLineInitHist1DayEntry 7 }





   ---------------------------------------------------
   --          PM channel current counters          --
   ---------------------------------------------------
   adsl2PMChCurrTable        OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMChCurrEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMChCurrTable contains current Performance
          Monitoring results of the ADSL2 channel.
          The PM counters in the table are not reset even when the XTU
          is reinitialized. They are reinitialized only when the
          agent itself is reset or reinitialized."
      ::= { adsl2PMChannel 1 }

   adsl2PMChCurrEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMChCurrEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMChCurrTable contains current Performance
          Monitoring results of the ADSL2 channel.
          The index of this table consists of an interface index, where
          the interface has an ifType value that is applicable
          for a DSL channel, along with a termination unit."
      INDEX  { ifIndex, adsl2PMChCurrUnit }
      ::= { adsl2PMChCurrTable 1 }

   Adsl2PMChCurrEntry  ::=
      SEQUENCE {
         adsl2PMChCurrUnit                     Adsl2Unit,
         adsl2PMChCurrValidIntervals           Unsigned32,
         adsl2PMChCurrInvalidIntervals         Unsigned32,
         adsl2PMChCurr15MTimeElapsed           HCPerfTimeElapsed,
         adsl2PMChCurr15MCodingViolations      Unsigned32,
         adsl2PMChCurr15MCorrectedBlocks       Unsigned32,
         adsl2PMChCurr1DayValidIntervals       Unsigned32,
         adsl2PMChCurr1DayInvalidIntervals     Unsigned32,
         adsl2PMChCurr1DayTimeElapsed          HCPerfTimeElapsed,
         adsl2PMChCurr1DayCodingViolations     Unsigned32,
         adsl2PMChCurr1DayCorrectedBlocks      Unsigned32
      }

   adsl2PMChCurrUnit  OBJECT-TYPE
      SYNTAX      Adsl2Unit
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION





      "The termination unit."
      ::= { adsl2PMChCurrEntry 1 }

   adsl2PMChCurrValidIntervals  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Valid intervals."
      ::= { adsl2PMChCurrEntry 2 }

   adsl2PMChCurrInvalidIntervals  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Invalid intervals."
       ::= { adsl2PMChCurrEntry 3 }

   adsl2PMChCurr15MTimeElapsed  OBJECT-TYPE
      SYNTAX      HCPerfTimeElapsed
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total elapsed seconds since this PM interval began.
          Note that the PM counters are not reset even when the XTU
          is reinitialized. They are reinitialized only when the
          agent itself is reset or reinitialized."
      ::= { adsl2PMChCurrEntry 4 }

   adsl2PMChCurr15MCodingViolations  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of CRC-8 (FEBE for ATU-R) anomalies occurring in the
          channel during the interval.  This parameter is inhibited
          during UAS or SES.  If the CRC is applied over multiple
          channels, then each related CRC-8 (or FEBE) anomaly should
          increment each of the counters related to the individual
          channels."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.2"
     ::= { adsl2PMChCurrEntry 5 }

   adsl2PMChCurr15MCorrectedBlocks  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only





      STATUS      current
      DESCRIPTION
         "Count of FEC (FFEC for ATU-R) anomalies (corrected code words)
          occurring in the channel during the interval.  This parameter
          is inhibited during UAS or SES.  If the FEC is applied over
          multiple channels, then each related FEC (or FFEC) anomaly
          should increment each of the counters related to the
          individual channels."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.2"
      ::= { adsl2PMChCurrEntry 6 }

   adsl2PMChCurr1DayValidIntervals  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Valid intervals."
      ::= { adsl2PMChCurrEntry 7 }

   adsl2PMChCurr1DayInvalidIntervals  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Invalid intervals."
      ::= { adsl2PMChCurrEntry 8 }

   adsl2PMChCurr1DayTimeElapsed  OBJECT-TYPE
      SYNTAX      HCPerfTimeElapsed
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total elapsed seconds since this PM interval began.
          Note that the PM counters are not reset even when the XTU
          is reinitialized. They are reinitialized only when the
          agent itself is reset or reinitialized."
      ::= { adsl2PMChCurrEntry 9 }

   adsl2PMChCurr1DayCodingViolations  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of CRC-8 (FEBE for ATU-R) anomalies occurring in the
          channel during the interval.  This parameter is inhibited
          during UAS or SES.  If the CRC is applied over multiple
          channels, then each related CRC-8 (or FEBE) anomaly should





          increment each of the counters related to the individual
          channels."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.2"
      ::= { adsl2PMChCurrEntry 10 }

   adsl2PMChCurr1DayCorrectedBlocks  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of FEC (FFEC for ATU-R) anomalies (corrected code words)
          occurring in the channel during the interval.  This parameter
          is inhibited during UAS or SES.  If the FEC is applied over
          multiple channels, then each related FEC (or FFEC) anomaly
          should increment each of the counters related to the
          individual channels."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.2"
      ::= { adsl2PMChCurrEntry 11 }



   -------------------------------------------
   --    PM channel history 15 Minutes      --
   -------------------------------------------
   adsl2PMChHist15MinTable         OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMChHist15MinEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMChCurrTable contains current Performance
          Monitoring results of the ADSL2 channel."
      ::= { adsl2PMChannel 2 }

   adsl2PMChHist15MinEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMChHist15MinEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMChCurrTable contains current Performance
          Monitoring results of the ADSL2 channel.
          The index of this table consists of an interface index, where
          the interface has an ifType value that is applicable
          for a DSL channel, along with a termination unit, and the
          interval number."
      INDEX  { ifIndex,
               adsl2PMChHist15MUnit,
               adsl2PMChHist15MInterval }
      ::= { adsl2PMChHist15MinTable 1 }





   Adsl2PMChHist15MinEntry  ::=
      SEQUENCE {
         adsl2PMChHist15MUnit                     Adsl2Unit,
         adsl2PMChHist15MInterval                 Unsigned32,
         adsl2PMChHist15MMonitoredTime            Unsigned32,
         adsl2PMChHist15MCodingViolations         Unsigned32,
         adsl2PMChHist15MCorrectedBlocks          Unsigned32,
         adsl2PMChHist15MValidInterval            TruthValue
      }

   adsl2PMChHist15MUnit  OBJECT-TYPE
      SYNTAX      Adsl2Unit
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The termination unit."
      ::= { adsl2PMChHist15MinEntry 1 }

   adsl2PMChHist15MInterval  OBJECT-TYPE
      SYNTAX      Unsigned32 (1..96)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The interval number."
      ::= { adsl2PMChHist15MinEntry 2 }

   adsl2PMChHist15MMonitoredTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total seconds monitored in this interval."
      ::= { adsl2PMChHist15MinEntry 3 }

   adsl2PMChHist15MCodingViolations  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of CRC-8 (FEBE for ATU-R) anomalies occurring in the
          channel during the interval.  This parameter is inhibited
          during UAS or SES.  If the CRC is applied over multiple
          channels, then each related CRC-8 (or FEBE) anomaly should
          increment each of the counters related to the individual
          channels."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.2"
      ::= { adsl2PMChHist15MinEntry 4 }





   adsl2PMChHist15MCorrectedBlocks  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of FEC (FFEC for ATU-R) anomalies (corrected code words)
          occurring in the channel during the interval.  This parameter
          is inhibited during UAS or SES.  If the FEC is applied over
          multiple channels, then each related FEC (or FFEC) anomaly
          should increment each of the counters related to the
          individual channels."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.2"
      ::= { adsl2PMChHist15MinEntry 5 }

   adsl2PMChHist15MValidInterval  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This variable indicates if the data for this interval is
          valid."
      ::= { adsl2PMChHist15MinEntry 6 }



   ------------------------------------------
   --        PM channel history 1 Day      --
   ------------------------------------------
   adsl2PMChHist1DTable         OBJECT-TYPE
      SYNTAX      SEQUENCE  OF  Adsl2PMChHist1DEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMChHist1DayTable contains PM channel history
          for 1-day intervals of ADSL2."
      ::= { adsl2PMChannel 3 }

   adsl2PMChHist1DEntry  OBJECT-TYPE
      SYNTAX      Adsl2PMChHist1DEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The table adsl2PMChHist1DayTable contains PM channel history
          for 1-day intervals of ADSL2.
          The index of this table consists of an interface index, where
          the interface has an ifType value that is applicable
          for a DSL channel, along with a termination unit, and the
          interval number."





      INDEX  { ifIndex,
               adsl2PMChHist1DUnit,
               adsl2PMChHist1DInterval }
      ::= { adsl2PMChHist1DTable 1 }

   Adsl2PMChHist1DEntry  ::=
      SEQUENCE {
         adsl2PMChHist1DUnit                      Adsl2Unit,
         adsl2PMChHist1DInterval                  Unsigned32,
         adsl2PMChHist1DMonitoredTime             Unsigned32,
         adsl2PMChHist1DCodingViolations          Unsigned32,
         adsl2PMChHist1DCorrectedBlocks           Unsigned32,
         adsl2PMChHist1DValidInterval             TruthValue
      }

   adsl2PMChHist1DUnit  OBJECT-TYPE
      SYNTAX      Adsl2Unit
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The termination unit."
       ::= { adsl2PMChHist1DEntry 1 }

   adsl2PMChHist1DInterval  OBJECT-TYPE
      SYNTAX      Unsigned32 (1..30)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The interval number."
      ::= { adsl2PMChHist1DEntry 2 }

   adsl2PMChHist1DMonitoredTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "seconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Total seconds monitored in this interval."
      ::= { adsl2PMChHist1DEntry 3 }

   adsl2PMChHist1DCodingViolations  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of CRC-8 (FEBE for ATU-R) anomalies occurring in the
          channel during the interval.  This parameter is inhibited
          during UAS or SES.  If the CRC is applied over multiple





          channels, then each related CRC-8 (or FEBE) anomaly should
          increment each of the counters related to the individual
          channels."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.2"
      ::= { adsl2PMChHist1DEntry 4 }

   adsl2PMChHist1DCorrectedBlocks  OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Count of FEC (FFEC for ATU-R) anomalies (corrected code words)
          occurring in the channel during the interval.  This parameter
          is inhibited during UAS or SES.  If the FEC is applied over
          multiple channels, then each related FEC (or FFEC) anomaly
          should increment each of the counters related to the
          individual channels."
      REFERENCE    "ITU-T G.997.1, paragraph 7.2.2"
      ::= { adsl2PMChHist1DEntry 5 }

   adsl2PMChHist1DValidInterval  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This variable indicates if the data for this interval is
          valid."
      ::= { adsl2PMChHist1DEntry 6 }

   -------------------------------------------
   --          Notifications Group          --
   -------------------------------------------

   adsl2LinePerfFECSThreshAtuc NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurr15MFecs,
      adsl2LineAlarmConfProfileAtucThresh15MinFecs
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the FEC seconds threshold
         has been reached/exceeded for the referred ATU-C."
      ::= { adsl2Notifications 1 }

   adsl2LinePerfFECSThreshAtur NOTIFICATION-TYPE
      OBJECTS
      {





      adsl2PMLCurr15MFecs,
      adsl2LineAlarmConfProfileAturThresh15MinFecs
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the FEC seconds threshold
         has been reached/exceeded for the referred ATU-R."
      ::= { adsl2Notifications 2 }

   adsl2LinePerfESThreshAtuc NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurr15MEs,
      adsl2LineAlarmConfProfileAtucThresh15MinEs
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the errored seconds threshold
         has been reached/exceeded for the referred ATU-C."
      ::= { adsl2Notifications 3 }

   adsl2LinePerfESThreshAtur NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurr15MEs,
      adsl2LineAlarmConfProfileAturThresh15MinEs
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the errored seconds threshold
         has been reached/exceeded for the referred ATU-R."
      ::= { adsl2Notifications 4 }

   adsl2LinePerfSESThreshAtuc NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurr15MSes,
      adsl2LineAlarmConfProfileAtucThresh15MinSes
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the severely-errored seconds
         threshold has been reached/exceeded for the referred ATU-C."
      ::= { adsl2Notifications 5 }

   adsl2LinePerfSESThreshAtur NOTIFICATION-TYPE
      OBJECTS
      {





      adsl2PMLCurr15MSes,
      adsl2LineAlarmConfProfileAturThresh15MinSes
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the severely-errored seconds
         threshold has been reached/exceeded for the referred ATU-R."
      ::= { adsl2Notifications 6 }

   adsl2LinePerfLOSSThreshAtuc NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurr15MLoss,
      adsl2LineAlarmConfProfileAtucThresh15MinLoss
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the LOS seconds
         threshold has been reached/exceeded for the referred ATU-C."
      ::= { adsl2Notifications 7 }

   adsl2LinePerfLOSSThreshAtur NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurr15MLoss,
      adsl2LineAlarmConfProfileAturThresh15MinLoss
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the LOS seconds
         threshold has been reached/exceeded for the referred ATU-R."
      ::= { adsl2Notifications 8 }

   adsl2LinePerfUASThreshAtuc NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurr15MUas,
      adsl2LineAlarmConfProfileAtucThresh15MinUas
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the unavailable seconds
         threshold has been reached/exceeded for the referred ATU-C."
      ::= { adsl2Notifications 9 }

   adsl2LinePerfUASThreshAtur NOTIFICATION-TYPE
      OBJECTS
      {





      adsl2PMLCurr15MUas,
      adsl2LineAlarmConfProfileAturThresh15MinUas
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the unavailable seconds
         threshold has been reached/exceeded for the referred ATU-R."
      ::= { adsl2Notifications 10 }

   adsl2LinePerfCodingViolationsThreshAtuc NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMChCurr15MCodingViolations,
      adsl2ChAlarmConfProfileAtucThresh15MinCodingViolations
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the coding violations
         threshold has been reached/exceeded for the referred ATU-C."
      ::= { adsl2Notifications 11 }

   adsl2LinePerfCodingViolationsThreshAtur NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMChCurr15MCodingViolations,
      adsl2ChAlarmConfProfileAturThresh15MinCodingViolations
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the coding violations
         threshold has been reached/exceeded for the referred ATU-R."
      ::= { adsl2Notifications 12 }

   adsl2LinePerfCorrectedThreshAtuc NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMChCurr15MCorrectedBlocks,
      adsl2ChAlarmConfProfileAtucThresh15MinCorrected
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the corrected blocks
         (FEC events) threshold has been reached/exceeded for the
         referred ATU-C."
      ::= { adsl2Notifications 13 }

   adsl2LinePerfCorrectedThreshAtur NOTIFICATION-TYPE
      OBJECTS





      {
      adsl2PMChCurr15MCorrectedBlocks,
      adsl2ChAlarmConfProfileAturThresh15MinCorrected
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the corrected blocks
         (FEC events) threshold has been reached/exceeded for the
         referred ATU-R."
      ::= { adsl2Notifications 14 }

   adsl2LinePerfFailedFullInitThresh NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurrInit15MFailedFullInits,
      adsl2LineAlarmConfProfileThresh15MinFailedFullInt
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the failed full
         initializations threshold has been reached/exceeded for the
         referred ADSL/ADSL2 or ADSL2+ line."
      ::= { adsl2Notifications 15 }

   adsl2LinePerfFailedShortInitThresh NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2PMLCurrInit15MFailedShortInits,
      adsl2LineAlarmConfProfileThresh15MinFailedShrtInt
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that the failed short
         initializations threshold has been reached/exceeded for the
         referred ADSL/ADSL2 or ADSL2+ line."
      ::= { adsl2Notifications 16 }

   adsl2LineStatusChangeAtuc NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2LineStatusAtuc
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that a status change is
         detected for the referred ATU-C."
      ::= { adsl2Notifications 17 }






   adsl2LineStatusChangeAtur NOTIFICATION-TYPE
      OBJECTS
      {
      adsl2LineStatusAtur
      }
      STATUS     current
      DESCRIPTION
        "This notification indicates that a status change is
         detected for the referred ATU-R."
      ::= { adsl2Notifications 18 }


      -- conformance information

      adsl2Groups OBJECT IDENTIFIER ::= { adsl2Conformance 1 }
      adsl2Compliances OBJECT IDENTIFIER ::= { adsl2Conformance 2 }

      adsl2LineMibCompliance MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
             "The compliance statement for SNMP entities that
             manage ADSL/ADSL2 or ADSL2+ interfaces."
         MODULE  -- this module
         MANDATORY-GROUPS
             {
             adsl2LineGroup,
             adsl2ChannelStatusGroup,
             adsl2SCStatusGroup,
             adsl2LineInventoryGroup,
             adsl2LineConfTemplateGroup,
             adsl2LineConfProfGroup,
             adsl2LineConfProfModeSpecGroup,
             adsl2ChConfProfileGroup,
             adsl2LineAlarmConfTemplateGroup,
             adsl2PMLineCurrGroup,
             adsl2PMLineCurrInitGroup,
             adsl2PMLineHist15MinGroup,
             adsl2PMLineHist1DayGroup,
             adsl2PMLineInitHist15MinGroup,
             adsl2PMLineInitHist1DayGroup,
             adsl2PMChCurrGroup,
             adsl2PMChHist15MinGroup,
             adsl2PMChHist1DGroup
             }

      GROUP  adsl2ChannelStatusAtmGroup
         DESCRIPTION
           "The group of status objects required when the data path





           is ATM."

      GROUP  adsl2ChannelStatusPtmGroup
         DESCRIPTION
           "The group of status objects required when the data path
           is PTM."

      GROUP  adsl2LineConfProfRaGroup
         DESCRIPTION
           "The group of objects required for controlling the rate-
           adaptive behavior of the line."

      GROUP  adsl2LineConfProfMsgMinGroup
         DESCRIPTION
           "The group of objects required for controlling the rate
           reserved for Overhead traffic."

      GROUP  adsl2LineAlarmConfProfileGroup
         DESCRIPTION
           "The group of objects that define the alarm thresholds
           on line-level PM counters."

      GROUP  adsl2ChAlarmConfProfileGroup
         DESCRIPTION
           "The group of objects that define the alarm thresholds
           on channel-level PM counters."

      GROUP  adsl2ChConfProfileAtmGroup
         DESCRIPTION
           "The group of configuration objects required when the data
           path is ATM."

      GROUP  adsl2ChConfProfileMinResGroup
         DESCRIPTION
           "The group of configuration objects required for the
           reserved data rate."

      GROUP  adsl2PMLineCurrInitShortGroup
         DESCRIPTION
           "The group of PM counters for the current interval's
           short initializations."

      GROUP  adsl2PMLineInitHist15MinShortGroup
         DESCRIPTION
           "The group of PM counters for the previous 15-minute
           interval's short initializations."

      GROUP  adsl2PMLineInitHist1DayShortGroup





         DESCRIPTION
           "The group of PM counters for the previous 24-hour
           interval's short initializations."

      GROUP  adsl2ScalarSCGroup
         DESCRIPTION
           "The group of objects that report the available memory
           resources for DELT processes."

      GROUP  adsl2ThreshNotificationGroup
         DESCRIPTION
           "The group of threshold crossing notifications."

      GROUP  adsl2StatusChangeNotificationGroup
         DESCRIPTION
           "The group of status change notifications."

         ::= { adsl2Compliances 1 }

      -- units of conformance

      adsl2LineGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LineCnfgTemplate,
             adsl2LineAlarmCnfgTemplate,
             adsl2LineCmndConfPmsf,
             adsl2LineCmndConfLdsf,
             adsl2LineCmndConfLdsfFailReason,
             adsl2LineCmndAutomodeColdStart,
             adsl2LineStatusAtuTransSys,
             adsl2LineStatusPwrMngState,
             adsl2LineStatusInitResult,
             adsl2LineStatusLastStateDs,
             adsl2LineStatusLastStateUs,
             adsl2LineStatusAtur,
             adsl2LineStatusAtuc,
             adsl2LineStatusLnAttenDs,
             adsl2LineStatusLnAttenUs,
             adsl2LineStatusSigAttenDs,
             adsl2LineStatusSigAttenUs,
             adsl2LineStatusSnrMarginDs,
             adsl2LineStatusSnrMarginUs,
             adsl2LineStatusAttainableRateDs,
             adsl2LineStatusAttainableRateUs,
             adsl2LineStatusActPsdDs,
             adsl2LineStatusActPsdUs,
             adsl2LineStatusActAtpDs,





             adsl2LineStatusActAtpUs
             }
         STATUS     current
         DESCRIPTION
             "The group of configuration, status, and commands objects
             on the line level."
         ::= { adsl2Groups 1 }

      adsl2ChannelStatusGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2ChStatusChannelNum,
             adsl2ChStatusActDataRate,
             adsl2ChStatusPrevDataRate,
             adsl2ChStatusActDelay
             }
         STATUS     current
         DESCRIPTION
             "The group of status objects on the channel level."
         ::= { adsl2Groups 2 }

      adsl2ChannelStatusAtmGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2ChStatusAtmStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of status objects on the data path level
             when it is ATM."
         ::= { adsl2Groups 3 }

      adsl2ChannelStatusPtmGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2ChStatusPtmStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of status objects on the data path level
             when it is PTM."
         ::= { adsl2Groups 4 }

      adsl2SCStatusGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2SCStatusMtime,
             adsl2SCStatusSnr,





             adsl2SCStatusBitsAlloc,
             adsl2SCStatusGainAlloc,
             adsl2SCStatusTssi,
             adsl2SCStatusLinScale,
             adsl2SCStatusLinReal,
             adsl2SCStatusLinImg,
             adsl2SCStatusLogMt,
             adsl2SCStatusLog,
             adsl2SCStatusQlnMt,
             adsl2SCStatusQln,
             adsl2SCStatusLnAtten,
             adsl2SCStatusSigAtten,
             adsl2SCStatusSnrMargin,
             adsl2SCStatusAttainableRate,
             adsl2SCStatusActAtp,
             adsl2SCStatusRowStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of status objects on the sub-carrier level.
             They are updated as a result of a DELT process."
         ::= { adsl2Groups 5 }

      adsl2LineInventoryGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LInvG994VendorId,
             adsl2LInvSystemVendorId,
             adsl2LInvVersionNumber,
             adsl2LInvSerialNumber,
             adsl2LInvSelfTestResult,
             adsl2LInvTransmissionCapabilities
             }
         STATUS     current
         DESCRIPTION
             "The group of inventory objects per XTU."
         ::= { adsl2Groups 6 }

      adsl2LineConfTemplateGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LConfTempLineProfile,
             adsl2LConfTempChan1ConfProfile,
             adsl2LConfTempChan1RaRatioDs,
             adsl2LConfTempChan1RaRatioUs,
             adsl2LConfTempChan2ConfProfile,
             adsl2LConfTempChan2RaRatioDs,
             adsl2LConfTempChan2RaRatioUs,





             adsl2LConfTempChan3ConfProfile,
             adsl2LConfTempChan3RaRatioDs,
             adsl2LConfTempChan3RaRatioUs,
             adsl2LConfTempChan4ConfProfile,
             adsl2LConfTempChan4RaRatioDs,
             adsl2LConfTempChan4RaRatioUs,
             adsl2LConfTempRowStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of objects in a line configuration template."
         ::= { adsl2Groups 7 }

      adsl2LineConfProfGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LConfProfScMaskDs,
             adsl2LConfProfScMaskUs,
             adsl2LConfProfRfiBandsDs,
             adsl2LConfProfRaModeDs,
             adsl2LConfProfRaModeUs,
             adsl2LConfProfTargetSnrmDs,
             adsl2LConfProfTargetSnrmUs,
             adsl2LConfProfMaxSnrmDs,
             adsl2LConfProfMaxSnrmUs,
             adsl2LConfProfMinSnrmDs,
             adsl2LConfProfMinSnrmUs,
             adsl2LConfProfAtuTransSysEna,
             adsl2LConfProfPmMode,
             adsl2LConfProfL0Time,
             adsl2LConfProfL2Time,
             adsl2LConfProfL2Atpr,
             adsl2LConfProfL2Atprt,
             adsl2LConfProfRowStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of objects in a line configuration profile."
         ::= { adsl2Groups 8 }

      adsl2LineConfProfRaGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LConfProfRaUsNrmDs,
             adsl2LConfProfRaUsNrmUs,
             adsl2LConfProfRaUsTimeDs,
             adsl2LConfProfRaUsTimeUs,
             adsl2LConfProfRaDsNrmsDs,





             adsl2LConfProfRaDsNrmsUs,
             adsl2LConfProfRaDsTimeDs,
             adsl2LConfProfRaDsTimeUs
             }
         STATUS     current
         DESCRIPTION
           "The group of objects required for controlling the rate-
           adaptive behavior of the line."
         ::= { adsl2Groups 9 }

      adsl2LineConfProfMsgMinGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LConfProfMsgMinUs,
             adsl2LConfProfMsgMinDs
             }
         STATUS     current
         DESCRIPTION
           "The group of objects required for controlling the rate
           reserved for Overhead traffic."
         ::= { adsl2Groups 10 }

      adsl2LineConfProfModeSpecGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LConfProfMaxNomPsdDs,
             adsl2LConfProfMaxNomPsdUs,
             adsl2LConfProfMaxNomAtpDs,
             adsl2LConfProfMaxNomAtpUs,
             adsl2LConfProfMaxAggRxPwrUs,
             adsl2LConfProfPsdMaskDs,
             adsl2LConfProfPsdMaskUs,
             adsl2LConfProfPsdMaskSelectUs,
             adsl2LConfProfModeSpecRowStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of objects in a line configuration profile
             that have an instance for each operation mode allowed."
         ::= { adsl2Groups 11 }

      adsl2ChConfProfileGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2ChConfProfMinDataRateDs,
             adsl2ChConfProfMinDataRateUs,
             adsl2ChConfProfMaxDataRateDs,
             adsl2ChConfProfMaxDataRateUs,





             adsl2ChConfProfMinDataRateLowPwrDs,
             adsl2ChConfProfMaxDelayDs,
             adsl2ChConfProfMaxDelayUs,
             adsl2ChConfProfMinProtectionDs,
             adsl2ChConfProfMinProtectionUs,
             adsl2ChConfProfMaxBerDs,
             adsl2ChConfProfMaxBerUs,
             adsl2ChConfProfUsDataRateDs,
             adsl2ChConfProfDsDataRateDs,
             adsl2ChConfProfUsDataRateUs,
             adsl2ChConfProfDsDataRateUs,
             adsl2ChConfProfRowStatus
             }
         STATUS     current
         DESCRIPTION
            "The group of objects in a channel configuration profile."
         ::= { adsl2Groups 12 }

      adsl2ChConfProfileAtmGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2ChConfProfImaEnabled,
             adsl2ChStatusAtmStatus
             }
         STATUS     current
         DESCRIPTION
           "The group of configuration objects required when the data
           path is ATM."
         ::= { adsl2Groups 13 }

      adsl2ChConfProfileMinResGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2ChConfProfMinResDataRateDs,
             adsl2ChConfProfMinResDataRateUs
             }
         STATUS     current
         DESCRIPTION
           "The group of configuration objects required for the
           reserved data rate."
         ::= { adsl2Groups 14 }

      adsl2LineAlarmConfTemplateGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LAlarmConfTempLineProfile,
             adsl2LAlarmConfTempChan1ConfProfile,
             adsl2LAlarmConfTempChan2ConfProfile,





             adsl2LAlarmConfTempChan3ConfProfile,
             adsl2LAlarmConfTempChan4ConfProfile,
             adsl2LAlarmConfTempRowStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of objects in a line alarm
              template."
         ::= { adsl2Groups 15 }

      adsl2LineAlarmConfProfileGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2LineAlarmConfProfileAtucThresh15MinFecs,
             adsl2LineAlarmConfProfileAtucThresh15MinEs,
             adsl2LineAlarmConfProfileAtucThresh15MinSes,
             adsl2LineAlarmConfProfileAtucThresh15MinLoss,
             adsl2LineAlarmConfProfileAtucThresh15MinUas,
             adsl2LineAlarmConfProfileAturThresh15MinFecs,
             adsl2LineAlarmConfProfileAturThresh15MinEs,
             adsl2LineAlarmConfProfileAturThresh15MinSes,
             adsl2LineAlarmConfProfileAturThresh15MinLoss,
             adsl2LineAlarmConfProfileAturThresh15MinUas,
             adsl2LineAlarmConfProfileThresh15MinFailedFullInt,
             adsl2LineAlarmConfProfileThresh15MinFailedShrtInt,
             adsl2LineAlarmConfProfileRowStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of objects in a line alarm profile."
         ::= { adsl2Groups 16 }

      adsl2ChAlarmConfProfileGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2ChAlarmConfProfileAtucThresh15MinCodingViolations,
             adsl2ChAlarmConfProfileAtucThresh15MinCorrected,
             adsl2ChAlarmConfProfileAturThresh15MinCodingViolations,
             adsl2ChAlarmConfProfileAturThresh15MinCorrected,
             adsl2ChAlarmConfProfileRowStatus
             }
         STATUS     current
         DESCRIPTION
             "The group of objects in a channel alarm profile."
         ::= { adsl2Groups 17 }

      adsl2PMLineCurrGroup OBJECT-GROUP
         OBJECTS





             {
             adsl2PMLCurrValidIntervals,
             adsl2PMLCurrInvalidIntervals,
             adsl2PMLCurr15MTimeElapsed,
             adsl2PMLCurr15MFecs,
             adsl2PMLCurr15MEs,
             adsl2PMLCurr15MSes,
             adsl2PMLCurr15MLoss,
             adsl2PMLCurr15MUas,
             adsl2PMLCurr1DayValidIntervals,
             adsl2PMLCurr1DayInvalidIntervals,
             adsl2PMLCurr1DayTimeElapsed,
             adsl2PMLCurr1DayFecs,
             adsl2PMLCurr1DayEs,
             adsl2PMLCurr1DaySes,
             adsl2PMLCurr1DayLoss,
             adsl2PMLCurr1DayUas
             }
         STATUS     current
         DESCRIPTION
           "The group of objects that report the line-level
           counters for current PM intervals."
         ::= { adsl2Groups 18 }

      adsl2PMLineCurrInitGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMLCurrInit15MTimeElapsed,
             adsl2PMLCurrInit15MFullInits,
             adsl2PMLCurrInit15MFailedFullInits,
             adsl2PMLCurrInit1DayTimeElapsed,
             adsl2PMLCurrInit1DayFullInits,
             adsl2PMLCurrInit1DayFailedFullInits
             }
         STATUS     current
         DESCRIPTION
           "The group of objects that report the full
           initialization counters for current PM intervals."
         ::= { adsl2Groups 19 }

      adsl2PMLineCurrInitShortGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMLCurrInit15MShortInits,
             adsl2PMLCurrInit15MFailedShortInits,
             adsl2PMLCurrInit1DayShortInits,
             adsl2PMLCurrInit1DayFailedShortInits
             }





         STATUS     current
         DESCRIPTION
           "The group of objects that report the short
           initialization counters for current PM intervals."
         ::= { adsl2Groups 20 }

      adsl2PMLineHist15MinGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMLHist15MMonitoredTime,
             adsl2PMLHist15MFecs,
             adsl2PMLHist15MEs,
             adsl2PMLHist15MSes,
             adsl2PMLHist15MLoss,
             adsl2PMLHist15MUas,
             adsl2PMLHist15MValidInterval
             }
         STATUS     current
         DESCRIPTION
           "The group of line-level PM counters for the previous
           15-minute interval."
         ::= { adsl2Groups 21 }

      adsl2PMLineHist1DayGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMLHist1DMonitoredTime,
             adsl2PMLHist1DFecs,
             adsl2PMLHist1DEs,
             adsl2PMLHist1DSes,
             adsl2PMLHist1DLoss,
             adsl2PMLHist1DUas,
             adsl2PMLHist1DValidInterval
             }
         STATUS     current
         DESCRIPTION
           "The group of line-level PM counters for the previous
           24-hour interval."
         ::= { adsl2Groups 22 }

      adsl2PMLineInitHist15MinGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMLHistInit15MMonitoredTime,
             adsl2PMLHistInit15MFullInits,
             adsl2PMLHistInit15MFailedFullInits,
             adsl2PMLHistInit15MValidInterval
             }





         STATUS     current
         DESCRIPTION
           "The group of PM counters for the previous 15-minute
           interval's full initializations."
         ::= { adsl2Groups 23 }

      adsl2PMLineInitHist15MinShortGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMLHistInit15MShortInits,
             adsl2PMLHistInit15MFailedShortInits
             }
         STATUS     current
         DESCRIPTION
           "The group of PM counters for the previous 15-minute
           interval's short initializations."
         ::= { adsl2Groups 24 }

      adsl2PMLineInitHist1DayGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMLHistinit1DMonitoredTime,
             adsl2PMLHistinit1DFullInits,
             adsl2PMLHistinit1DFailedFullInits,
             adsl2PMLHistinit1DValidInterval
             }
         STATUS     current
         DESCRIPTION
           "The group of PM counters for the previous 24-hour
           interval's full initializations."
         ::= { adsl2Groups 25 }

      adsl2PMLineInitHist1DayShortGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMLHistinit1DShortInits,
             adsl2PMLHistinit1DFailedShortInits
             }
         STATUS     current
         DESCRIPTION
           "The group of PM counters for the previous 24-hour
           interval's short initializations."
         ::= { adsl2Groups 26 }

      adsl2PMChCurrGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMChCurrValidIntervals,





             adsl2PMChCurrInvalidIntervals,
             adsl2PMChCurr15MTimeElapsed,
             adsl2PMChCurr15MCodingViolations,
             adsl2PMChCurr15MCorrectedBlocks,
             adsl2PMChCurr1DayValidIntervals,
             adsl2PMChCurr1DayInvalidIntervals,
             adsl2PMChCurr1DayTimeElapsed,
             adsl2PMChCurr1DayCodingViolations,
             adsl2PMChCurr1DayCorrectedBlocks
             }
         STATUS     current
         DESCRIPTION
           "The group of objects that report the channel-level
           counters for current PM intervals."
         ::= { adsl2Groups 27 }

      adsl2PMChHist15MinGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMChHist15MMonitoredTime,
             adsl2PMChHist15MCodingViolations,
             adsl2PMChHist15MCorrectedBlocks,
             adsl2PMChHist15MValidInterval
             }
         STATUS     current
         DESCRIPTION
           "The group of objects that report the channel-level
           counters for previous 15-minute PM intervals."
         ::= { adsl2Groups 28 }

      adsl2PMChHist1DGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2PMChHist1DMonitoredTime,
             adsl2PMChHist1DCodingViolations,
             adsl2PMChHist1DCorrectedBlocks,
             adsl2PMChHist1DValidInterval
             }
         STATUS     current
         DESCRIPTION
           "The group of objects that report the channel-level
           counters for previous 24-hour PM intervals."
         ::= { adsl2Groups 29 }

      adsl2ScalarSCGroup OBJECT-GROUP
         OBJECTS
             {
             adsl2ScalarSCMaxInterfaces,





             adsl2ScalarSCAvailInterfaces
             }
         STATUS     current
         DESCRIPTION
           "The group of objects that report the available memory
           resources for DELT processes."
         ::= { adsl2Groups 30 }

      adsl2ThreshNotificationGroup NOTIFICATION-GROUP
         NOTIFICATIONS
         {
         adsl2LinePerfFECSThreshAtuc,
         adsl2LinePerfFECSThreshAtur,
         adsl2LinePerfESThreshAtuc,
         adsl2LinePerfESThreshAtur,
         adsl2LinePerfSESThreshAtuc,
         adsl2LinePerfSESThreshAtur,
         adsl2LinePerfLOSSThreshAtuc,
         adsl2LinePerfLOSSThreshAtur,
         adsl2LinePerfUASThreshAtuc,
         adsl2LinePerfUASThreshAtur,
         adsl2LinePerfCodingViolationsThreshAtuc,
         adsl2LinePerfCodingViolationsThreshAtur,
         adsl2LinePerfCorrectedThreshAtuc,
         adsl2LinePerfCorrectedThreshAtur,
         adsl2LinePerfFailedFullInitThresh,
         adsl2LinePerfFailedShortInitThresh
         }
         STATUS      current
         DESCRIPTION
           "This group supports notifications of significant conditions
           associated with ADSL/ADSL2/ADSL2+ lines."
         ::= { adsl2Groups 31 }

      adsl2StatusChangeNotificationGroup NOTIFICATION-GROUP
         NOTIFICATIONS
         {
         adsl2LineStatusChangeAtuc,
         adsl2LineStatusChangeAtur
         }
         STATUS      current
         DESCRIPTION
           "This group supports notifications of threshold crossing
           associated with ADSL/ADSL2/ADSL2+ lines."
         ::= { adsl2Groups 32 }

   END





