RFC1354-MIB DEFINITIONS ::= BEGIN


     IMPORTS
             Gauge, IpAddress
                     FROM RFC1155-SMI
             mib-2, ip
                     FROM RFC1213-MIB
             OBJECT-TYPE
                     FROM RFC-1212;

     --  This MIB module uses the extended OBJECT-TYPE macro as
     --  defined in [9].
     ipForward  OBJECT IDENTIFIER ::= { ip 24 }

         ipForwardNumber OBJECT-TYPE
             SYNTAX   Gauge
             ACCESS   read-only
             STATUS   mandatory
             DESCRIPTION
                "The number of current  ipForwardTable  entries
                that are not invalid."
             ::= { ipForward 1 }


     --  IP Forwarding Table

     --  The IP Forwarding Table obsoletes and replaces the ipRoute
     --  Table current in MIB-I and MIB-II.  It adds knowledge of





     --  the autonomous system of the next hop, multiple next hop
     --  support, and policy routing support.


         ipForwardTable OBJECT-TYPE
             SYNTAX   SEQUENCE OF IpForwardEntry
             ACCESS   not-accessible
             STATUS   mandatory
             DESCRIPTION
                "This entity's IP Routing table."
             REFERENCE
                "RFC 1213 Section 6.6, The IP Group"
             ::= { ipForward 2 }


         ipForwardEntry OBJECT-TYPE
             SYNTAX   IpForwardEntry
             ACCESS   not-accessible
             STATUS   mandatory
             DESCRIPTION
                "A particular route to  a  particular  destina-
                tion, under a particular policy."
             INDEX {
                 ipForwardDest,
                 ipForwardProto,
                 ipForwardPolicy,
                 ipForwardNextHop
                 }
             ::= { ipForwardTable 1 }


         IpForwardEntry ::=
             SEQUENCE {
                 ipForwardDest
                     IpAddress,
                 ipForwardMask
                     IpAddress,
                 ipForwardPolicy
                     INTEGER,
                 ipForwardNextHop
                     IpAddress,
                 ipForwardIfIndex
                     INTEGER,
                 ipForwardType
                     INTEGER,
                 ipForwardProto
                     INTEGER,
                 ipForwardAge





                     INTEGER,
                 ipForwardInfo
                     OBJECT IDENTIFIER,
                 ipForwardNextHopAS
                     INTEGER,
                 ipForwardMetric1
                     INTEGER,
                 ipForwardMetric2
                     INTEGER,
                 ipForwardMetric3
                     INTEGER,
                 ipForwardMetric4
                     INTEGER,
                 ipForwardMetric5
                     INTEGER
             }

         ipForwardDest OBJECT-TYPE
             SYNTAX   IpAddress
             ACCESS   read-only
             STATUS   mandatory
             DESCRIPTION
                "The destination IP address of this route.   An
                entry  with  a value of 0.0.0.0 is considered a
                default route.

                This object may not take a Multicast (Class  D)
                address value.

                Any assignment (implicit or  otherwise)  of  an
                instance  of  this  object to a value x must be
                rejected if the bitwise logical-AND of  x  with
                the  value of the corresponding instance of the
                ipForwardMask object is not equal to x."
             ::= { ipForwardEntry 1 }


         ipForwardMask OBJECT-TYPE
             SYNTAX   IpAddress
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "Indicate the mask to be logical-ANDed with the
                destination  address  before  being compared to
                the value  in  the  ipForwardDest  field.   For
                those  systems  that  do  not support arbitrary
                subnet masks, an agent constructs the value  of
                the  ipForwardMask  by  reference to the IP Ad-





                dress Class.

                Any assignment (implicit or  otherwise)  of  an
                instance  of  this  object to a value x must be
                rejected if the bitwise logical-AND of  x  with
                the  value of the corresponding instance of the
                ipForwardDest object is not equal to ipForward-
                Dest."
             DEFVAL { '00000000'h }      -- 0.0.0.0
             ::= { ipForwardEntry 2 }


         -- The following convention is included for specification
         -- of TOS Field contents.  At this time, the Host Requirements
         -- and the Router Requirements documents disagree on the width
         -- of the TOS field.  This mapping describes the Router
         -- Requirements mapping, and leaves room to widen the TOS field
         -- without impact to fielded systems.

         ipForwardPolicy OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-only
             STATUS   mandatory
             DESCRIPTION
                "The general set of conditions that would cause
                the  selection  of  one multipath route (set of
                next hops for a given destination) is  referred
                to as 'policy'.

                Unless the mechanism indicated by ipForwardPro-
                to specifies otherwise, the policy specifier is
                the IP TOS Field.  The encoding of IP TOS is as
                specified  by  the  following convention.  Zero
                indicates the default path if no more  specific
                policy applies.

                +-----+-----+-----+-----+-----+-----+-----+-----+
                |                 |                       |     |
                |   PRECEDENCE    |    TYPE OF SERVICE    |  0  |
                |                 |                       |     |
                +-----+-----+-----+-----+-----+-----+-----+-----+

                         IP TOS                IP TOS
                    Field     Policy      Field     Policy
                    Contents    Code      Contents    Code
                    0 0 0 0  ==>   0      0 0 0 1  ==>   2
                    0 0 1 0  ==>   4      0 0 1 1  ==>   6
                    0 1 0 0  ==>   8      0 1 0 1  ==>  10





                    0 1 1 0  ==>  12      0 1 1 1  ==>  14
                    1 0 0 0  ==>  16      1 0 0 1  ==>  18
                    1 0 1 0  ==>  20      1 0 1 1  ==>  22
                    1 1 0 0  ==>  24      1 1 0 1  ==>  26
                    1 1 1 0  ==>  28      1 1 1 1  ==>  30

                Protocols defining 'policy' otherwise must  ei-
                ther define a set of values which are valid for
                this  object  or  must  implement  an  integer-
                instanced  policy table for which this object's
                value acts as an index."
             ::= { ipForwardEntry 3 }


         ipForwardNextHop OBJECT-TYPE
             SYNTAX   IpAddress
             ACCESS   read-only
             STATUS   mandatory
             DESCRIPTION
                "On remote routes, the address of the next sys-
                tem en route; Otherwise, 0.0.0.0."
             ::= { ipForwardEntry 4 }


         ipForwardIfIndex OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "The ifIndex value which identifies  the  local
                interface  through  which  the next hop of this
                route should be reached."
             DEFVAL { 0 }
             ::= { ipForwardEntry 5 }


         ipForwardType OBJECT-TYPE
             SYNTAX   INTEGER {
                         other    (1), -- not specified by this MIB
                         invalid  (2), -- logically deleted
                         local    (3), -- local interface
                         remote   (4)  -- remote destination
                      }
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "The type of route.  Note that local(3)  refers
                to  a route for which the next hop is the final





                destination; remote(4) refers to  a  route  for
                which  the  next  hop is not the final destina-
                tion.

                Setting this object to the value invalid(2) has
                the  effect  of  invalidating the corresponding
                entry in the ipForwardTable object.   That  is,
                it  effectively  disassociates  the destination
                identified with said entry from the route iden-
                tified    with    said   entry.    It   is   an
                implementation-specific matter  as  to  whether
                the agent removes an invalidated entry from the
                table.  Accordingly, management  stations  must
                be prepared to receive tabular information from
                agents that corresponds to entries not current-
                ly  in  use.  Proper interpretation of such en-
                tries requires examination of the relevant  ip-
                ForwardType object."
             DEFVAL { invalid }
             ::= { ipForwardEntry 6 }

         ipForwardProto OBJECT-TYPE
             SYNTAX   INTEGER {
                         other     (1),  -- not specified
                         local     (2),  -- local interface
                         netmgmt   (3),  -- static route
                         icmp      (4),  -- result of ICMP Redirect

                                 -- the following are all dynamic
                                 -- routing protocols
                         egp       (5),  -- Exterior Gateway Protocol
                         ggp       (6),  -- Gateway-Gateway Protocol
                         hello     (7),  -- FuzzBall HelloSpeak
                         rip       (8),  -- Berkeley RIP or RIP-II
                         is-is     (9),  -- Dual IS-IS
                         es-is     (10), -- ISO 9542
                         ciscoIgrp (11), -- Cisco IGRP
                         bbnSpfIgp (12), -- BBN SPF IGP
                         ospf      (13), -- Open Shortest Path First
                         bgp       (14), -- Border Gateway Protocol
                         idpr      (15)  -- InterDomain Policy Routing
                      }
             ACCESS   read-only
             STATUS   mandatory
             DESCRIPTION
                "The routing mechanism via which this route was
                learned.  Inclusion of values for gateway rout-
                ing protocols is not  intended  to  imply  that





                hosts should support those protocols."
             ::= { ipForwardEntry 7 }


         ipForwardAge OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-only
             STATUS   mandatory
             DESCRIPTION
                "The number of seconds  since  this  route  was
                last  updated  or  otherwise  determined  to be
                correct.  Note that no semantics of  `too  old'
                can  be implied except through knowledge of the
                routing  protocol  by  which  the   route   was
                learned."
             DEFVAL  { 0 }
             ::= { ipForwardEntry 8 }


         ipForwardInfo OBJECT-TYPE
             SYNTAX   OBJECT IDENTIFIER
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "A reference to MIB definitions specific to the
                particular  routing protocol which is responsi-
                ble for this route, as determined by the  value
                specified  in the route's ipForwardProto value.
                If this information is not present,  its  value
                should be set to the OBJECT IDENTIFIER { 0 0 },
                which is a syntactically valid object  identif-
                ier, and any implementation conforming to ASN.1
                and the Basic Encoding Rules must  be  able  to
                generate and recognize this value."
             DEFVAL  { { 0 0 } } -- 0.0
             ::= { ipForwardEntry 9 }


         ipForwardNextHopAS OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "The Autonomous System Number of the Next  Hop.
                When  this  is  unknown  or not relevant to the
                protocol indicated by ipForwardProto, zero."
             DEFVAL { 0 }
             ::= { ipForwardEntry 10 }





         ipForwardMetric1 OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "The primary routing  metric  for  this  route.
                The  semantics of this metric are determined by
                the routing-protocol specified in  the  route's
                ipForwardProto  value.   If  this metric is not
                used, its value should be set to -1."
             DEFVAL { -1 }
             ::= { ipForwardEntry 11 }


         ipForwardMetric2 OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "An alternate routing metric  for  this  route.
                The  semantics of this metric are determined by
                the routing-protocol specified in  the  route's
                ipForwardProto  value.   If  this metric is not
                used, its value should be set to -1."
             DEFVAL { -1 }
             ::= { ipForwardEntry 12 }


         ipForwardMetric3 OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "An alternate routing metric  for  this  route.
                The  semantics of this metric are determined by
                the routing-protocol specified in  the  route's
                ipForwardProto  value.   If  this metric is not
                used, its value should be set to -1."
             DEFVAL { -1 }
             ::= { ipForwardEntry 13 }


         ipForwardMetric4 OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "An alternate routing metric  for  this  route.





                The  semantics of this metric are determined by
                the routing-protocol specified in  the  route's
                ipForwardProto  value.   If  this metric is not
                used, its value should be set to -1."
             DEFVAL { -1 }
             ::= { ipForwardEntry 14 }


         ipForwardMetric5 OBJECT-TYPE
             SYNTAX   INTEGER
             ACCESS   read-write
             STATUS   mandatory
             DESCRIPTION
                "An alternate routing metric  for  this  route.
                The  semantics of this metric are determined by
                the routing-protocol specified in  the  route's
                ipForwardProto  value.   If  this metric is not
                used, its value should be set to -1."
             DEFVAL { -1 }
             ::= { ipForwardEntry 15 }

     END


