IANA-BFD-TC-STD-MIB DEFINITIONS ::= BEGIN


    IMPORTS
        MODULE-IDENTITY, mib-2
            FROM SNMPv2-SMI                               -- RFC 2578

        TEXTUAL-CONVENTION
            FROM SNMPv2-TC;                               -- RFC 2579





    ianaBfdTCStdMib MODULE-IDENTITY

        LAST-UPDATED
                   "201408120000Z" -- 12 August 2014 00:00:00 GMT
        ORGANIZATION
                   "IANA"
        CONTACT-INFO
                   "Internet Assigned Numbers Authority
                    Postal: 12025 Waterfront Drive, Suite 300
                            Los Angeles, CA  90094-2536
                    Tel:    +1 310 301 5800
                    EMail:  iana@iana.org"

        DESCRIPTION
          "Copyright (c) 2014 IETF Trust and the persons identified as
           authors of the code.  All rights reserved.

           Redistribution and use in source and binary forms, with or
           without modification, is permitted pursuant to, and subject
           to the license terms contained in, the Simplified BSD License
           set forth in Section 4.c of the IETF Trust's Legal Provisions
           Relating to IETF Documents
           (http://trustee.ietf.org/license-info)."

        REVISION
          "201408120000Z" -- 12 August 2014 00:00:00 GMT
        DESCRIPTION
          "Initial version.  Published as RFC 7330."

    ::= { mib-2 224 }

    IANAbfdDiagTC ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
        "A common BFD diagnostic code."
    REFERENCE
        "Katz, D. and D. Ward, Bidirectional Forwarding
         Detection (BFD), RFC 5880, June 2010.

         Allan, D., Swallow, G., and Drake, J., Proactive Connectivity
         Verification, Continuity Check, and Remote Defect
         Indication for the MPLS Transport Profile, RFC 6428,
         November 2011."

    SYNTAX INTEGER {
        noDiagnostic(0),
        controlDetectionTimeExpired(1),
        echoFunctionFailed(2),





        neighborSignaledSessionDown(3),
        forwardingPlaneReset(4),
        pathDown(5),
        concatenatedPathDown(6),
        administrativelyDown(7),
        reverseConcatenatedPathDown(8),
        misConnectivityDefect(9)
    }

    IANAbfdSessTypeTC ::= TEXTUAL-CONVENTION
    STATUS        current
    DESCRIPTION
        "BFD session type"
    REFERENCE
        "Katz, D. and D. Ward, Bidirectional Forwarding
         Detection (BFD), RFC 5880, June 2010.

         Katz, D. and D. Ward, Bidirectional Forwarding
         Detection (BFD) for IPv4 and IPv6 (Single Hop),
         RFC 5881, June 2010.

         Katz, D. and D. Ward, Bidirectional Forwarding
         Detection (BFD) for Multihop Paths, RFC 5883,
         June 2010."
    SYNTAX INTEGER {
        singleHop(1),
        multiHopTotallyArbitraryPaths(2),
        multiHopOutOfBandSignaling(3),
        multiHopUnidirectionalLinks(4)
    }

    IANAbfdSessOperModeTC ::= TEXTUAL-CONVENTION
    STATUS            current
    DESCRIPTION
        "BFD session operating mode"
    REFERENCE
        "Katz, D. and D. Ward, Bidirectional Forwarding
         Detection (BFD), RFC 5880, June 2010."
    SYNTAX INTEGER {
        asyncModeWEchoFunction(1),
        asynchModeWOEchoFunction(2),
        demandModeWEchoFunction(3),
        demandModeWOEchoFunction(4)
    }

    IANAbfdSessStateTC ::= TEXTUAL-CONVENTION
    STATUS         current
    DESCRIPTION





        "BFD session state.  State failing(5) is only applicable if
         corresponding session is running in BFD version 0."

    REFERENCE
        "Katz, D. and D. Ward, Bidirectional Forwarding
         Detection (BFD), RFC 5880, June 2010."
    SYNTAX INTEGER {
        adminDown(1),
        down(2),
        init(3),
        up(4),
        failing(5)
    }

    IANAbfdSessAuthenticationTypeTC ::= TEXTUAL-CONVENTION
    STATUS                      current
    DESCRIPTION
        "BFD authentication type"
    REFERENCE
        "Sections 4.2 - 4.4 from Katz, D. and D. Ward,
         Bidirectional Forwarding Detection (BFD),
         RFC 5880, June 2010."
    SYNTAX INTEGER {
        noAuthentication(-1),
        reserved(0),
        simplePassword(1),
        keyedMD5(2),
        meticulousKeyedMD5(3),
        keyedSHA1(4),
        meticulousKeyedSHA1(5)
    }

    IANAbfdSessAuthenticationKeyTC ::= TEXTUAL-CONVENTION
    DISPLAY-HINT                  "1x "
    STATUS                        current
    DESCRIPTION
        "BFD authentication key type.

         An IANAbfdSessAuthenticationKeyTC is always interpreted
         within the context of an IANAbfdSessAuthenticationTypeTC
         value.  Every usage of the IANAbfdSessAuthenticationTypeTC
         textual convention is required to specify the
         IANAbfdSessAuthenticationKeyTC object that provides the
         context.  It is suggested that the
         IANAbfdSessAuthenticationKeyTC object be logically registered
         before the object(s) that use the
         IANAbfdSessAuthenticationKeyTC textual convention, if they
         appear in the same logical row.





         The value of an IANAbfdSessAuthenticationKeyTC must
         always be consistent with the value of the associated
         IANAbfdSessAuthenticationTypeTC object.  Attempts to set an
         IANAbfdSessAuthenticationKeyTC object to a value inconsistent
         with the associated IANAbfdSessAuthenticationTypeTC must fail
         with an inconsistentValue error.

         The following size constraints for an
         IANAbfdSessAuthenticationKeyTC object are defined for the
         associated IANAbfdSessAuthenticationTypeTC values show below:

         noAuthentication(-1): SIZE(0)
         reserved(0): SIZE(0)
         simplePassword(1): SIZE(1..16)
         keyedMD5(2): SIZE(16)
         meticulousKeyedMD5(3): SIZE(16)
         keyedSHA1(4): SIZE(20)
         meticulousKeyedSHA1(5): SIZE(20)

         When this textual convention is used as the syntax of an
         index object, there may be issues with the limit of 128
         sub-identifiers specified in SMIv2, STD 58.  In this case,
         the object definition MUST include a 'SIZE' clause to limit
         the number of potential instance sub-identifiers; otherwise,
         the applicable constraints MUST be stated in the appropriate
         conceptual row DESCRIPTION clauses, or in the surrounding
         documentation if there is no single DESCRIPTION clause that
         is appropriate."
    REFERENCE
        "Sections 4.2 - 4.4 from Katz, D. and D. Ward, Bidirectional
         Forwarding Detection (BFD), RFC 5880, June 2010."
    SYNTAX OCTET STRING(SIZE(0..252))

    END


