SNMP-SSH-TM-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    OBJECT-IDENTITY, mib-2, snmpDomains,
    Counter32
      FROM SNMPv2-SMI -- RFC 2578
    TEXTUAL-CONVENTION
      FROM SNMPv2-TC -- RFC 2579
    MODULE-COMPLIANCE, OBJECT-GROUP
      FROM SNMPv2-CONF -- RFC 2580
    ;

snmpSshtmMIB MODULE-IDENTITY
    LAST-UPDATED "200906090000Z"
    ORGANIZATION "ISMS Working Group"
    CONTACT-INFO "WG-EMail:   isms@lists.ietf.org
                  Subscribe:  isms-request@lists.ietf.org

                  Chairs:
                    Juergen Quittek
                    NEC Europe Ltd.
                    Network Laboratories
                    Kurfuersten-Anlage 36
                    69115 Heidelberg
                    Germany
                    +49 6221 90511-15
                    quittek@netlab.nec.de

                    Juergen Schoenwaelder
                    Jacobs University Bremen
                    Campus Ring 1
                    28725 Bremen
                    Germany
                    +49 421 200-3587
                    j.schoenwaelder@jacobs-university.de

                  Co-editors:
                    David Harrington
                    Huawei Technologies USA
                    1700 Alma Drive
                    Plano Texas 75075





                    USA
                    +1 603-436-8634
                    ietfdbh@comcast.net

                    Joseph Salowey
                    Cisco Systems
                    2901 3rd Ave
                    Seattle, WA 98121
                    USA
                    jsalowey@cisco.com

                    Wes Hardaker
                    Cobham Analytic Solutions
                    P.O. Box 382
                    Davis, CA  95617
                    USA
                    +1 530 792 1913
                    ietf@hardakers.net
                 "
    DESCRIPTION
       "The Secure Shell Transport Model MIB.

        Copyright (c) 2009 IETF Trust and the persons
        identified as authors of the code.  All rights reserved.

        Redistribution and use in source and binary forms, with or
        without modification, are permitted provided that the
        following conditions are met:

        - Redistributions of source code must retain the above copyright
          notice, this list of conditions and the following disclaimer.

        - Redistributions in binary form must reproduce the above
          copyright notice, this list of conditions and the following
          disclaimer in the documentation and/or other materials
          provided with the distribution.

        - Neither the name of Internet Society, IETF or IETF Trust,
          nor the names of specific contributors, may be used to endorse
          or promote products derived from this software without
          specific prior written permission.

        THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
        CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED WARRANTIES,
        INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
        MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
        DISCLAIMED.  IN NO EVENT SHALL THE COPYRIGHT OWNER OR
        CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,





        SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
        NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
        LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
        HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
        CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR
        OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,
        EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

        This version of this MIB module is part of RFC 5592;
        see the RFC itself for full legal notices."

    REVISION     "200906090000Z"
    DESCRIPTION  "The initial version, published in RFC 5592."

    ::= { mib-2 189 }

-- ---------------------------------------------------------- --
-- subtrees in the SNMP-SSH-TM-MIB
-- ---------------------------------------------------------- --

snmpSshtmNotifications    OBJECT IDENTIFIER ::= { snmpSshtmMIB 0 }
snmpSshtmObjects          OBJECT IDENTIFIER ::= { snmpSshtmMIB 1 }
snmpSshtmConformance      OBJECT IDENTIFIER ::= { snmpSshtmMIB 2 }

-- -------------------------------------------------------------
-- Objects
-- -------------------------------------------------------------

snmpSSHDomain OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The SNMP-over-SSH transport domain.  The corresponding
         transport address is of type SnmpSSHAddress.

         When an SNMP entity uses the snmpSSHDomain Transport
         Model, it must be capable of accepting messages up to
         and including 8192 octets in size.  Implementation of
         larger values is encouraged whenever possible.

         The securityName prefix to be associated with the
         snmpSSHDomain is 'ssh'.  This prefix may be used by Security
         Models or other components to identify which secure transport
         infrastructure authenticated a securityName."
    ::= { snmpDomains 7 }

SnmpSSHAddress ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "1a"
    STATUS      current





    DESCRIPTION
        "Represents either a hostname or IP address, along with a port
         number and an optional user name.

         The beginning of the address specification may contain a
         user name followed by an '@' (US-ASCII character 0x40).  This
         portion of the address will indicate the user name that should
         be used when authenticating to an SSH server.  The user name
         must be encoded in UTF-8 (per [RFC4252]).  If missing, the
         SNMP securityName should be used.  After the optional user
         name field and '@' character comes the hostname or IP
         address.

         The hostname is always in US-ASCII (as per RFC1033);
         internationalized hostnames are encoded in US-ASCII as
         specified in RFC 3490.  The hostname is followed by a colon
         ':' (US-ASCII character 0x3A) and a decimal port number in
         US-ASCII.  The name SHOULD be fully qualified whenever
         possible.

         An IPv4 address must be in dotted decimal format followed
         by a colon ':' (US-ASCII character 0x3A) and a decimal port
         number in US-ASCII.

         An IPv6 address must be in colon-separated format, surrounded
         by square brackets ('[', US-ASCII character 0x5B, and ']',
         US-ASCII character 0x5D), followed by a colon ':' (US-ASCII
         character 0x3A) and a decimal port number in US-ASCII.

         Values of this Textual Convention might not be directly usable
         as transport-layer addressing information and may require
         runtime resolution.  As such, applications that write them
         must be prepared for handling errors if such values are
         not supported or cannot be resolved (if resolution occurs
         at the time of the management operation).

         The DESCRIPTION clause of TransportAddress objects that may
         have snmpSSHAddress values must fully describe how (and
         when) such names are to be resolved to IP addresses and vice
         versa.

         This Textual Convention SHOULD NOT be used directly in
         object definitions since it restricts addresses to a
         specific format.  However, if it is used, it MAY be used
         either on its own or in conjunction with
         TransportAddressType or TransportDomain as a pair.







         When this Textual Convention is used as a syntax of an
         index object, there may be issues with the limit of 128
         sub-identifiers, which is specified in SMIv2 (STD 58).  It
         is RECOMMENDED that all MIB documents using this Textual
         Convention make explicit any limitations on index
         component lengths that management software must observe.
         This may be done either by including SIZE constraints on
         the index components or by specifying applicable
         constraints in the conceptual row DESCRIPTION clause or
         in the surrounding documentation.
        "
    REFERENCE
      "RFC 1033: DOMAIN ADMINISTRATORS OPERATIONS GUIDE
       RFC 3490: Internationalizing Domain Names in Applications
       RFC 3986: Uniform Resource Identifier (URI): Generic Syntax
       RFC 4252: The Secure Shell (SSH) Authentication Protocol"
    SYNTAX      OCTET STRING (SIZE (1..255))

-- The snmpSshtmSession Group

snmpSshtmSession       OBJECT IDENTIFIER ::= { snmpSshtmObjects 1 }

snmpSshtmSessionOpens  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The number of times an openSession() request has been
                 executed as an SSH client, whether it succeeded or
                 failed.
                "
    ::= { snmpSshtmSession 1 }

snmpSshtmSessionCloses  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The number of times a closeSession() request has been
                 executed as an SSH client, whether it succeeded or
                 failed.
                "
    ::= { snmpSshtmSession 2 }

snmpSshtmSessionOpenErrors  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current







    DESCRIPTION "The number of times an openSession() request
                 failed to open a transport connection or failed to
                 authenticate the server.
                "
    ::= { snmpSshtmSession 3 }

snmpSshtmSessionUserAuthFailures  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The number of times an openSession() request
                 failed to open a session as an SSH client due to
                 user-authentication failures.
                "
    ::= { snmpSshtmSession 4 }

snmpSshtmSessionNoChannels  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The number of times an openSession() request
                 failed to open a session as an SSH client due to
                 channel-open failures.
                "
    ::= { snmpSshtmSession 5 }

snmpSshtmSessionNoSubsystems OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The number of times an openSession() request
                 failed to open a session as an SSH client due to
                 inability to connect to the requested subsystem.
                "
    ::= { snmpSshtmSession 6 }

snmpSshtmSessionNoSessions  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The number of times an outgoing message was
                 dropped because the same session was no longer
                 available.
                "
    ::= { snmpSshtmSession 7 }

snmpSshtmSessionInvalidCaches OBJECT-TYPE
    SYNTAX       Counter32





    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The number of outgoing messages dropped because the
                 tmStateReference referred to an invalid cache.
                "
    ::= { snmpSshtmSession 8 }

-- ************************************************
-- snmpSshtmMIB - Conformance Information
-- ************************************************

snmpSshtmCompliances OBJECT IDENTIFIER ::= { snmpSshtmConformance 1 }

snmpSshtmGroups      OBJECT IDENTIFIER ::= { snmpSshtmConformance 2 }

-- ************************************************
-- Compliance statements
-- ************************************************

snmpSshtmCompliance MODULE-COMPLIANCE
    STATUS      current

    DESCRIPTION "The compliance statement for SNMP engines that
                 support the SNMP-SSH-TM-MIB."
    MODULE
        MANDATORY-GROUPS { snmpSshtmGroup }
    ::= { snmpSshtmCompliances 1 }

-- ************************************************
-- Units of conformance
-- ************************************************

snmpSshtmGroup OBJECT-GROUP
    OBJECTS {
      snmpSshtmSessionOpens,
      snmpSshtmSessionCloses,
      snmpSshtmSessionOpenErrors,
      snmpSshtmSessionUserAuthFailures,
      snmpSshtmSessionNoChannels,
      snmpSshtmSessionNoSubsystems,
      snmpSshtmSessionNoSessions,
      snmpSshtmSessionInvalidCaches
    }
    STATUS      current
    DESCRIPTION "A collection of objects for maintaining information
                 of an SNMP engine that implements the SNMP Secure
                 Shell Transport Model.
                "





    ::= { snmpSshtmGroups 2 }

END


