RFC1304-MIB DEFINITIONS ::= BEGIN


               IMPORTS
                       Counter, TimeTicks, IpAddress
                               FROM RFC1155-SMI
                       transmission
                               FROM RFC1213-MIB
                       OBJECT-TYPE
                               FROM RFC-1212;

               --  This MIB module uses the extended OBJECT-TYPE macro
               --  as defined in RFC-1212.

               --  This is the MIB module for the SIP objects.


               sip     OBJECT IDENTIFIER ::= { transmission 31 }

               -- All representations of SMDS addresses in this MIB
               -- module use, as a textual convention (i.e., this
               -- convention does not affect their encoding), the
               -- data type:

               SMDSAddress ::= OCTET STRING (SIZE (8))
               -- the 60-bit SMDS address, preceded by 4 bits with the
               -- following values:
               -- "1100" when representing an individual address
               -- "1110" when representing a group address


               -- The SIP Level 3 group
               -- Implementation of the SIP Level 3 group is mandatory
               -- for all systems implementing SIP Level 3.

               sipL3Table  OBJECT-TYPE
                   SYNTAX  SEQUENCE OF SipL3Entry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                           "This table contains SIP L3 parameters and
                           state variables, one entry per SIP port."





                  ::= { sip 1 }

              sipL3Entry  OBJECT-TYPE
                  SYNTAX  SipL3Entry
                  ACCESS  not-accessible
                  STATUS  mandatory
                  DESCRIPTION
                          "This list contains SIP L3 parameters and
                          state variables."
                 INDEX   { sipL3Index }
                 ::= { sipL3Table 1 }

             SipL3Entry  ::= SEQUENCE {
                 sipL3Index
                     INTEGER,
                 sipL3ReceivedIndividualDAs
                     Counter,
                 sipL3ReceivedGAs
                     Counter,
                 sipL3UnrecognizedIndividualDAs
                     Counter,
                 sipL3UnrecognizedGAs
                     Counter,
                 sipL3SentIndividualDAs
                     Counter,
                 sipL3SentGAs
                     Counter,
                 sipL3Errors
                     Counter,
                 sipL3InvalidSMDSAddressTypes
                     Counter,
                 sipL3VersionSupport
                     INTEGER
                 }

             sipL3Index  OBJECT-TYPE
                 SYNTAX  INTEGER (1..65535)
                 ACCESS  read-only
                 STATUS  mandatory
                 DESCRIPTION
                         "The value of this object identifies the SIP
                         port interface for which this entry contains
                         management information.  The value of this
                         object for a particular interface has the same
                         value as the ifIndex object, defined in RFC
                         1156 and RFC 1213, for the same interface."
                ::= { sipL3Entry 1 }






            sipL3ReceivedIndividualDAs OBJECT-TYPE
                SYNTAX  Counter
                ACCESS  read-only
                STATUS  mandatory
                DESCRIPTION
                        "The total number of individually addressed SIP
                        Level 3 PDUs received from the remote system
                        across the SNI.  The total includes only
                        unerrored L3PDUs."
               ::= { sipL3Entry 2 }

           sipL3ReceivedGAs OBJECT-TYPE
               SYNTAX  Counter
               ACCESS  read-only
               STATUS  mandatory
               DESCRIPTION
                       "The total number of group addressed SIP Level 3
                       PDUs received from the remote system across the
                       SNI.  The total includes only unerrored L3PDUs."
              ::= { sipL3Entry 3 }

          sipL3UnrecognizedIndividualDAs OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of SIP Level 3 PDUs received from the
                      remote system with invalid or unknown individual
                      destination addresses (Destination Address
                      Screening violations are not included).  See SMDS
                      Subscription MIB module."
              ::= { sipL3Entry 4 }

          sipL3UnrecognizedGAs OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of SIP Level 3 PDUs received from the
                      remote system with invalid or unknown group
                      addresses.  (Destination Address Screening
                      violations are not included).  See SMDS
                      Subscription MIB module."
              ::= { sipL3Entry 5 }

          sipL3SentIndividualDAs OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only





              STATUS  mandatory
              DESCRIPTION
                      "The number of individually addressed SIP Level 3
                      PDUs that have been sent by this system across the
                      SNI."
              ::= { sipL3Entry 6 }

          sipL3SentGAs OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of group addressed SIP L3PDUs that
                      have been sent by this system across the SNI."
              ::= { sipL3Entry 7 }

          -- The total number of SIP L3PDU errors can be calculated as
          -- (Syntactic errors + Semantic Service errors )
          -- Syntactic errors include:
          --    sipL3Errors
          -- Latest occurrences of syntactic error types are logged in
          --    sipL3PDUErrorTable.
          -- Semantic Service errors include:
          --    sipL3UnrecognizedIndividualDAs
          --    sipL3UnrecognizedGAs
          --    sipL3InvalidSMDSAddressTypes
          -- Note that public networks supporting SMDS may discard
          -- SIP L3PDUs due to subscription violations.  Related
          -- managed objects are defined in Definitions of Managed
          -- Objects for SMDS Subscription.


          sipL3Errors OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The total number of SIP Level 3 PDUs received
                      from the remote system that were discovered to
                      have errors (including protocol processing and bit
                      errors but excluding addressing-related errors)
                      and were discarded.  Includes both group addressed
                      L3PDUs and L3PDUs containing an individual
                      destination address."
              ::= { sipL3Entry 8 }








          sipL3InvalidSMDSAddressTypes OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of SIP Level 3 PDUs received from the
                      remote system that had the Source or Destination
                      Address_Type subfields, (the four most significant
                      bits of the 64 bit address field), not equal to
                      the value 1100 or 1110.  Also, an error is
                      considered to have occurred if the Address_Type
                      field for a Source Address, the four most
                      significant bits of the 64 bits, is equal to 1110
                      (a group address)."
              ::= { sipL3Entry 9 }

          sipL3VersionSupport  OBJECT-TYPE
              SYNTAX  INTEGER (1..65535)
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "A value which indicates the version(s) of SIP
                      that this interface supports.  The value is a sum.
                      This sum initially takes the value zero.  For each
                      version, V, that this interface supports, 2 raised
                      to (V - 1) is added to the sum. For example, a
                      port supporting versions 1 and 2 would have a
                      value of (2^(1-1)+2^(2-1))=3.  The
                      sipL3VersionSupport is effectively a bit mask with
                      Version 1 equal to the least significant bit
                      (LSB)."
              ::= { sipL3Entry 10 }


          -- The SIP Level 2 group
          -- Implementation of the SIP Level 2 group is mandatory
          -- for all systems implementing SIP Level 2.


          sipL2Table  OBJECT-TYPE
              SYNTAX  SEQUENCE OF SipL2Entry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "This table contains SIP L2PDU parameters and
                      state variables, one entry per SIP port."
              ::= { sip 2 }






          sipL2Entry  OBJECT-TYPE
              SYNTAX  SipL2Entry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "This list contains SIP L2 parameters and state
                      variables."
              INDEX   { sipL2Index }
              ::= { sipL2Table 1 }

          SipL2Entry  ::= SEQUENCE {
              sipL2Index
                  INTEGER,
              sipL2ReceivedCounts
                  Counter,
              sipL2SentCounts
                  Counter,
              sipL2HcsOrCRCErrors
                  Counter,
              sipL2PayloadLengthErrors
                  Counter,
              sipL2SequenceNumberErrors
                  Counter,
              sipL2MidCurrentlyActiveErrors
                  Counter,
              sipL2BomOrSSMsMIDErrors
                  Counter,
              sipL2EomsMIDErrors
                  Counter
              }

          sipL2Index  OBJECT-TYPE
              SYNTAX  INTEGER (1..65535)
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The value of this object identifies the SIP port
                      interface for which this entry contains management
                      information.  The value of this object for a
                      particular interface has the same value as the
                      ifIndex object, defined in RFC 1156 and RFC 1213,
                      for the same interface."
              ::= { sipL2Entry 1 }

          sipL2ReceivedCounts OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory





              DESCRIPTION
                      "The number of SIP Level 2 PDUs received from the
                      remote system across the SNI. The total includes
                      only unerrored L2PDUs."
              ::= { sipL2Entry 2 }

          sipL2SentCounts OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of SIP Level 2 PDUs that have been
                      sent by this system across the SNI."
              ::= { sipL2Entry 3 }

          -- The total number of SIP L2PDU errors can be calculated as
          -- the sum of:
          --    sipL2HcsOrCRCErrors
          --    sipL2PayloadLengthErrors
          --    sipL2SequenceNumberErrors
          --    sipL2MidCurrentlyActiveErrors
          --    sipL2BomOrSSMsMIDErrors
          --    sipL2EomsMIDErrors

          sipL2HcsOrCRCErrors  OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of received SIP Level 2 PDUs that were
                      discovered to have either a Header Check Sequence
                      error or a Payload CRC violation."
              ::= { sipL2Entry 4 }

          sipL2PayloadLengthErrors  OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of received SIP Level 2 PDUs that had
                      Payload Length errors that fall in the following
                      specifications:
                      - SSM L2_PDU payload length field value less
                      - than 28 octets or greater than 44 octets,

                      - BOM or COM L2_PDU payload length field not
                      - equal to 44 octets,






                      - EOM L2_PDU payload length field value less
                      - than 4 octets or greater than 44 octets."
              ::= { sipL2Entry 5 }

          sipL2SequenceNumberErrors  OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of received SIP Level 2 PDUs that had
                      a sequence number within the L2PDU not equal to
                      the expected sequence number of the SMDS SS
                      receive process."
              ::= { sipL2Entry 6 }

          sipL2MidCurrentlyActiveErrors  OBJECT-TYPE
              SYNTAX Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of received SIP Level 2 PDUs that are
                      BOMs for which an active receive process is
                      already started."
              ::= { sipL2Entry 7 }

          sipL2BomOrSSMsMIDErrors  OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of received SIP Level 2 PDUs that are
                      SSMs with a MID not equal to zero or are BOMs with
                      MIDs equal to zero."
              ::= { sipL2Entry 8 }

          sipL2EomsMIDErrors  OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The number of received SIP Level 2 PDUs that are
                      EOMs for which there is no active receive process
                      for the MID (i.e., the receipt of an EOM which
                      does not correspond to a BOM) OR the EOM has a MID
                      equal to zero."
              ::= { sipL2Entry 9 }







          -- The SIP PLCP group
          -- Implementation of one of these groups is mandatory
          -- if the PLCP is implemented.

          sipPLCP OBJECT IDENTIFIER ::= { sip 3 }


          -- The SIP DS1 PLCP group
          -- Implementation of this group is mandatory
          -- if the DS1 PLCP is implemented.

          sipDS1PLCPTable  OBJECT-TYPE
              SYNTAX  SEQUENCE OF SipDS1PLCPEntry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "This table contains SIP DS1 PLCP parameters and
                      state variables, one entry per SIP port."
              ::= { sipPLCP 1 }

          sipDS1PLCPEntry  OBJECT-TYPE
              SYNTAX  SipDS1PLCPEntry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "This list contains SIP DS1 PLCP parameters and
                      state variables."
              INDEX   { sipDS1PLCPIndex }
              ::= { sipDS1PLCPTable 1 }

          SipDS1PLCPEntry  ::= SEQUENCE {
              sipDS1PLCPIndex
                  INTEGER,
              sipDS1PLCPSEFSs
                  Counter,
              sipDS1PLCPAlarmState
                  INTEGER,
              sipDS1PLCPUASs
                  Counter
              }


          sipDS1PLCPIndex  OBJECT-TYPE
              SYNTAX  INTEGER (1..65535)
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The value of this object identifies the SIP port





                      interface for which this entry contains management
                      information.  The value of this object for a
                      particular interface has the same value as the
                      ifIndex object, defined in RFC 1156 and RFC 1213,
                      for the same interface."
              ::= { sipDS1PLCPEntry 1 }


          sipDS1PLCPSEFSs OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "A DS1 Severely Errored Framing Second (SEFS) is a
                      count of one-second intervals containing one or
                      more SEF events.  A Severely Errored Framing (SEF)
                      event is declared when an error in the A1 octet
                      and an error in the A2 octet of a framing octet
                      pair (i.e., errors in both framing octets), or two
                      consecutive invalid and/or nonsequential Path
                      Overhead Identifier octets are detected."
              ::= { sipDS1PLCPEntry 2 }

          sipDS1PLCPAlarmState OBJECT-TYPE
              SYNTAX  INTEGER {
                          noAlarm (1),
                          receivedFarEndAlarm (2),
                          incomingLOF (3)
                      }
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "This variable indicates if there is an alarm
                      present for the DS1 PLCP.  The value
                      receivedFarEndAlarm means that the DS1 PLCP has
                      received an incoming Yellow Signal, the value
                      incomingLOF means that the DS1 PLCP has declared a
                      loss of frame (LOF) failure condition, and the
                      value noAlarm means that there are no alarms
                      present.  See TR-TSV-000773 for a description of
                      alarm states."
              ::= { sipDS1PLCPEntry 3 }


          sipDS1PLCPUASs OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory





              DESCRIPTION
                      "The counter associated with the number of
                      Unavailable Seconds, as defined by TR-TSV-000773,
                      encountered by the PLCP."
              ::= { sipDS1PLCPEntry 4 }


          -- The SIP DS3 PLCP group
          -- Implementation of this group is mandatory
          -- if the DS3 PLCP is implemented.

          sipDS3PLCPTable  OBJECT-TYPE
              SYNTAX  SEQUENCE OF SipDS3PLCPEntry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "This table contains SIP DS3 PLCP parameters and
                      state variables, one entry per SIP port."
              ::= { sipPLCP 2 }

          sipDS3PLCPEntry  OBJECT-TYPE
              SYNTAX  SipDS3PLCPEntry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "This list contains SIP DS3 PLCP parameters and
                      state variables."
              INDEX   { sipDS3PLCPIndex }
              ::= { sipDS3PLCPTable 1 }

          SipDS3PLCPEntry  ::= SEQUENCE {
              sipDS3PLCPIndex
                  INTEGER,
              sipDS3PLCPSEFSs
                  Counter,
              sipDS3PLCPAlarmState
                  INTEGER,
              sipDS3PLCPUASs
                  Counter
              }


          sipDS3PLCPIndex  OBJECT-TYPE
              SYNTAX  INTEGER (1..65535)
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The value of this object identifies the SIP port





                      interface for which this entry contains management
                      information.  The value of this object for a
                      particular interface has the same value as the
                      ifIndex object, defined in RFC 1156 and RFC 1213,
                      for the same interface."
              ::= { sipDS3PLCPEntry 1 }

          sipDS3PLCPSEFSs OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "A DS3 Severely Errored Framing Second (SEFS) is a
                      count of one-second intervals containing one or
                      more SEF events.  A Severely Errored Framing (SEF)
                      event is declared when an error in the A1 octet
                      and an error in the A2 octet of a framing octet
                      pair (i.e., errors in both framing octets), or two
                      consecutive invalid and/or nonsequential Path
                      Overhead Identifier octets are detected."
              ::= { sipDS3PLCPEntry 2 }

          sipDS3PLCPAlarmState OBJECT-TYPE
              SYNTAX  INTEGER {
                          noAlarm (1),
                          receivedFarEndAlarm (2),
                          incomingLOF (3)
                      }
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "This variable indicates if there is an alarm
                      present for the DS3 PLCP.  The value
                      receivedFarEndAlarm means that the DS3 PLCP has
                      received an incoming Yellow Signal, the value
                      incomingLOF means that the DS3 PLCP has declared a
                      loss of frame (LOF) failure condition, and the
                      value noAlarm means that there are no alarms
                      present.  See TR-TSV-000773 for a description of
                      alarm states."
              ::= { sipDS3PLCPEntry 3 }


          sipDS3PLCPUASs OBJECT-TYPE
              SYNTAX  Counter
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION





                      "The counter associated with the number of
                      Unavailable Seconds, as defined by TR-TSV-000773,
                      encountered by the PLCP."
              ::= { sipDS3PLCPEntry 4 }


          -- The SMDS Applications group
          -- Applications that have been identified for this group are:
          --          * IP-over-SMDS (details are specified in RFC 1209)
          -- Implementation of this group is mandatory for systems
          -- that implement IP-over-SMDS Interface Protocol.

          smdsApplications OBJECT IDENTIFIER ::= { sip 4 }

          ipOverSMDS OBJECT IDENTIFIER ::= { smdsApplications 1 }

          -- Although the objects in this group are read-only, at the
          -- agent's discretion they may be made read-write so that the
          -- management station, when appropriately authorized, may
          -- change the addressing information related to the
          -- configuration of a logical IP subnetwork implemented on
          -- top of SMDS.

          -- This table is necessary to support RFC1209 (IP-over-SMDS)
          -- and gives information on the Group Addresses and ARP
          -- Addresses used in the Logical IP subnetwork.
          -- One SMDS address may be associated with multiple IP
          -- addresses.  One SNI may be associated with multiple LISs.

          ipOverSMDSTable OBJECT-TYPE
              SYNTAX  SEQUENCE OF IpOverSMDSEntry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "The table of addressing information relevant to
                      this entity's IP addresses."
              ::= { ipOverSMDS 1 }

          ipOverSMDSEntry OBJECT-TYPE
              SYNTAX  IpOverSMDSEntry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "The addressing information for one of this
                      entity's IP addresses."
              INDEX   { ipOverSMDSIndex, ipOverSMDSAddress }
              ::= { ipOverSMDSTable 1 }






          IpOverSMDSEntry ::=
              SEQUENCE {
                 ipOverSMDSIndex
                     INTEGER,
                 ipOverSMDSAddress
                     IpAddress,
                 ipOverSMDSHA
                     SMDSAddress,
                 ipOverSMDSLISGA
                     SMDSAddress,
                 ipOverSMDSARPReq
                     SMDSAddress
                 }

          ipOverSMDSIndex OBJECT-TYPE
              SYNTAX  INTEGER (1..65535)
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The value of this object identifies the SIP port
                      interface for which this entry contains management
                      information.  The value of this object for a
                      particular interface has the same value as the
                      ifIndex object, defined in RFC 1156 and RFC 1213,
                      for the same interface."
              ::= { ipOverSMDSEntry 1 }

          ipOverSMDSAddress OBJECT-TYPE
               SYNTAX  IpAddress
               ACCESS  read-only
               STATUS  mandatory
               DESCRIPTION
                      "The IP address to which this entry's addressing
                      information pertains."
              ::= { ipOverSMDSEntry 2 }

          ipOverSMDSHA OBJECT-TYPE
              SYNTAX  SMDSAddress
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The SMDS Individual address of the IP station."
              ::= { ipOverSMDSEntry 3 }

          ipOverSMDSLISGA OBJECT-TYPE
              SYNTAX  SMDSAddress
              ACCESS  read-only
              STATUS  mandatory





              DESCRIPTION
                      "The SMDS Group Address that has been configured
                      to identify the SMDS Subscriber-Network Interfaces
                      (SNIs) of all members of the Logical IP Subnetwork
                      (LIS) connected to the network supporting SMDS."
              ::= { ipOverSMDSEntry 4 }

          ipOverSMDSARPReq OBJECT-TYPE
              SYNTAX  SMDSAddress
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The SMDS address (individual or group) to which
                      ARP Requests are to be sent."
              ::= { ipOverSMDSEntry 5 }


          -- The SMDS Carrier Selection group
          -- This group is used as a place holder
          -- for carrier selection objects.

          smdsCarrierSelection OBJECT IDENTIFIER ::= { sip 5}


          -- The SIP Error Log
          -- Implementation of this group is mandatory
          -- for all systems that implement SIP Level 3.

          sipErrorLog OBJECT IDENTIFIER ::= { sip 6 }

          sipL3PDUErrorTable OBJECT-TYPE
              SYNTAX  SEQUENCE OF SipL3PDUErrorEntry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "A table that contains the latest occurrence of
                      the following syntactical SIP L3PDU errors:

                      - Destination Address Field Format Error,

                      The following pertains to the 60 least significant
                      bits of the 64 bit address field.  The 60 bits
                      contained in the address subfield can be used to
                      represent addresses up to 15 decimal digits.  Each
                      decimal digit shall be encoded into four bits
                      using Binary Coded Decimal (BCD), with the most
                      significant digit occurring left-most.  If not all
                      15 digits are required, then the remainder of this





                      field shall be padded on the right with bits set
                      to one.  An error is considered to have occurred:
                      a).  if the first four bits of the address
                      subfield are not BCD, OR b).  if the first four
                      bits of the address subfield are populated with
                      the country code value 0001, AND the 40 bits which
                      follow are not Binary Coded Decimal (BCD) encoded
                      values of the 10 digit addresses, OR the remaining
                      16 least significant bits are not populated with
                      1's, OR c).  if the address subfield is not
                      correct according to another numbering plan which
                      is dependent upon the carrier assigning the
                      numbers and offering SMDS.

                      - Source Address Field Format Error,

                      The description of this parameter is the same as
                      the description of the Destination Address Field
                      Format Error.

                      - Invalid BAsize Field Value,

                      An error is considered to have occurred when the
                      BAsize field of an SIP L3PDU contains a value less
                      that 32, greater than 9220 octets without the
                      CRC32 field present, greater than 9224 octets with
                      the CRC32 field present, or not equal to a
                      multiple of 4 octets,

                      - Invalid Header Extension Length Field Value,

                      An error is considered to have occurred when the
                      Header Extension Length field value is not equal
                      3.

                      - Invalid Header Extension - Element Length,

                      An error is considered to have occurred when the
                      Header Extension - Element Length is greater than
                      12.

                      - Invalid Header Extension - Version Element
                      Position, Length, or Value,

                      An error is considered to have occurred when a
                      Version element with Length=3, Type=0, and Value=1
                      does not appear first within the Header Extension,
                      or an element Type=0 appears somewhere other than





                      within the first three octets in the Header
                      Extension.

                      - Invalid Header Extension - Carrier Selection
                      Element Position, Length, Value or Format,

                      An error is considered to have occurred when a
                      Carrier Selection element does not appear second
                      within the Header Extension, if the Element Type
                      does not equal 1, the Element Length does not
                      equal 4, 6, or 8, the Element Value field is not
                      four BCD encoded decimal digits used in specifying
                      the Carrier Identification Code (CIC), or the
                      identified CIC code is invalid.

                      - Header Extension PAD Error

                      An error is considered to have occurred when the
                      Header Extension PAD is 9 octets in length, or if
                      the Header Extension PAD is greater than zero
                      octets in length and the Header Extension PAD does
                      not follow all Header Extension elements or does
                      not begin with at least one octet of all zeros.

                      - BEtag Mismatch Error,

                      An error is considered to have occurred when the
                      Beginning-End Tags in the SIP L3PDU header and
                      trailer are not equal.

                      - BAsize Field not equal to Length Field Error,

                      An error is considered to have occurred when the
                      value of the BAsize Field does not equal the value
                      of the Length Field.

                      - Incorrect Length Error, and

                      An error is considered to have occurred when the
                      the Length field value is not equal to the portion
                      of the SIP L3PDU which extends from the
                      Destination Address field up to and including the
                      CRC32 field (if present) or up to and including
                      the PAD field (if the CRC32 field is not present).
                      As an optional check, an error is considered to
                      have occurred when the length of a partially
                      received SIP L3PDU exceeds the BAsize value.






                      - MRI Timeout Error.

                      An error is considered to have occurred when the
                      elapsed time between receipt of BOM and
                      corresponding EOM exceeds the value of the MRI
                      (Message Receive Interval) for a particular
                      transport signal format.

                      An entry is indexed by interface number and error
                      type, and contains Source Address, Destination
                      Address and a timestamp. All these errors are
                      counted in the sipL3Errors counter.  When
                      sipL3PDUErrorTimeStamp is equal to zero, the
                      SipL3PDUErrorEntry does not contain any valid
                      information."
              ::= { sipErrorLog 1 }

          sipL3PDUErrorEntry  OBJECT-TYPE
              SYNTAX SipL3PDUErrorEntry
              ACCESS  not-accessible
              STATUS  mandatory
              DESCRIPTION
                      "An entry in the service disagreement table."
              INDEX   { sipL3PDUErrorIndex, sipL3PDUErrorType }
              ::= { sipL3PDUErrorTable 1 }

          SipL3PDUErrorEntry ::= SEQUENCE {
              sipL3PDUErrorIndex
                  INTEGER,
              sipL3PDUErrorType
                  INTEGER,
              sipL3PDUErrorSA
                  SMDSAddress,
              sipL3PDUErrorDA
                  SMDSAddress,
              sipL3PDUErrorTimeStamp
                  TimeTicks
              }

          sipL3PDUErrorIndex OBJECT-TYPE
              SYNTAX  INTEGER (1..65535)
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The value of this object identifies the SIP port
                      interface for which this entry contains management
                      information.   The value of this object for a
                      particular interface has the same value as the





                      ifIndex object, defined in RFC 1156 and RFC 1213,
                      for the same interface."
              ::= { sipL3PDUErrorEntry 1 }

          sipL3PDUErrorType OBJECT-TYPE
              SYNTAX  INTEGER {
                   erroredDAFieldFormat (1),
                   erroredSAFieldFormat (2),
                   invalidBAsizeFieldValue (3),
                   invalidHdrExtLength (4),
                   invalidHdrExtElementLength (5),
                   invalidHdrExtVersionElementPositionLenthOrValue (6),
           invalidHdrExtCarSelectElementPositionLenghtValueOrFormat (7),
                   hePADError (8),
                   beTagMismatch (9),
                   baSizeFieldNotEqualToLengthField (10),
                   incorrectLength (11),
                   mriTimeout (12)
              }
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The type of error."
              ::= { sipL3PDUErrorEntry 2 }

          sipL3PDUErrorSA OBJECT-TYPE
              SYNTAX  SMDSAddress
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "A rejected SMDS source address."
              ::= { sipL3PDUErrorEntry 3 }

          sipL3PDUErrorDA OBJECT-TYPE
              SYNTAX  SMDSAddress
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "A rejected SMDS destination address."
              ::= { sipL3PDUErrorEntry 4 }

          sipL3PDUErrorTimeStamp OBJECT-TYPE
              SYNTAX  TimeTicks
              ACCESS  read-only
              STATUS  mandatory
              DESCRIPTION
                      "The timestamp for the service disagreement.  The
                      timestamp contains the value of sysUpTime at the





                      latest occurrence of this type of service
                      disagreement.  See textual description under
                      sipL3PDUErrorTable for boundary conditions."
              ::= { sipL3PDUErrorEntry 5 }

          END


