IPV6-TC DEFINITIONS ::= BEGIN


-- Copyright (c) 2017 IETF Trust and the persons identified as
-- authors of the code.  All rights reserved.

--   Redistribution and use in source and binary forms, with or without
--   modification, is permitted pursuant to, and subject to the license
--   terms contained in, the Simplified BSD License set forth in Section
--   4.c of the IETF Trust's Legal Provisions Relating to IETF Documents
--   (http://trustee.ietf.org/license-info).

IMPORTS
     Integer32                FROM SNMPv2-SMI
     TEXTUAL-CONVENTION       FROM SNMPv2-TC;

-- definition of textual conventions
Ipv6Address ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "2x:"
     STATUS       obsolete
     DESCRIPTION
       "This data type is used to model IPv6 addresses.
        This is a binary string of 16 octets in network
        byte-order.

        This object is obsoleted by INET-ADDRESS-MIB::InetAddress."
     SYNTAX       OCTET STRING (SIZE (16))

Ipv6AddressPrefix ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "2x:"
     STATUS       obsolete
     DESCRIPTION
       "This data type is used to model IPv6 address
       prefixes.  This is a binary string of up to 16
       octets in network byte-order.
       This object is obsoleted by INET-ADDRESS-MIB::InetAddress."
     SYNTAX       OCTET STRING (SIZE (0..16))

Ipv6AddressIfIdentifier ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "2x:"
     STATUS       obsolete
     DESCRIPTION
       "This data type is used to model IPv6 address
       interface identifiers.  This is a binary string
        of up to 8 octets in network byte-order.

       This object is obsoleted by IP-MIB::Ipv6AddressIfIdentifierTC."





     SYNTAX      OCTET STRING (SIZE (0..8))

Ipv6IfIndex ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "d"
     STATUS       obsolete
     DESCRIPTION
       "A unique value, greater than zero for each
       internetwork-layer interface in the managed
       system.  It is recommended that values are assigned
       contiguously starting from 1.  The value for each
       internetwork-layer interface must remain constant
       at least from one re-initialization of the entity's
       network management system to the next
       re-initialization.

       This object is obsoleted by IF-MIB::InterfaceIndex."
     SYNTAX       Integer32 (1..2147483647)

Ipv6IfIndexOrZero ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "d"
     STATUS       obsolete
     DESCRIPTION
         "This textual convention is an extension of the
         Ipv6IfIndex convention.  The latter defines
         a greater than zero value used to identify an IPv6
         interface in the managed system.  This extension
         permits the additional value of zero.  The value
         zero is object-specific and must therefore be
         defined as part of the description of any object
         which uses this syntax.  Examples of the usage of
         zero might include situations where interface was
         unknown, or when none or all interfaces need to be
         referenced.

         This object is obsoleted by IF-MIB::InterfaceIndexOrZero."
     SYNTAX       Integer32 (0..2147483647)

END














