PW-MPLS-STD-MIB DEFINITIONS ::= BEGIN


   IMPORTS
      MODULE-IDENTITY, OBJECT-TYPE, Unsigned32, mib-2
         FROM SNMPv2-SMI                   -- [RFC2578]

      MODULE-COMPLIANCE, OBJECT-GROUP
         FROM SNMPv2-CONF                  -- [RFC2580]

      StorageType
         FROM SNMPv2-TC                    -- [RFC2579]

      InterfaceIndexOrZero
         FROM IF-MIB                       -- [RFC2863]

      MplsTunnelIndex, MplsTunnelInstanceIndex,
      MplsLdpIdentifier, MplsLsrIdentifier
         FROM MPLS-TC-STD-MIB              -- [RFC3811]

      MplsIndexType
         FROM MPLS-LSR-STD-MIB             -- [RFC3813]

      PwIndexType
         FROM PW-TC-STD-MIB                -- [RFC5542]






      pwIndex                              -- [RFC5601]
         FROM PW-STD-MIB
   ;

   pwMplsStdMIB MODULE-IDENTITY
      LAST-UPDATED "200906120000Z"  --  12 June 2009 00:00:00 GMT
      ORGANIZATION "Pseudowire Emulation Edge-to-Edge (PWE3) Working
                    Group."
      CONTACT-INFO
          "
           David Zelig, Editor
           Email: davidz@corrigent.com

           Thomas D. Nadeau, Editor
           Email:  tom.nadeau@bt.com

           The PWE3 Working Group (email distribution pwe3@ietf.org,
           http://www.ietf.org/html.charters/pwe3-charter.html)
          "
      DESCRIPTION
          "This MIB module complements the PW-STD-MIB module for PW
           operation over MPLS.

           Copyright (c) 2009 IETF Trust and the persons identified as
           authors of the code.  All rights reserved.

           Redistribution and use in source and binary forms, with or
           without modification, are permitted provided that the
           following conditions are met:

           - Redistributions of source code must retain the above
             copyright notice, this list of conditions and the
             following disclaimer.

           - Redistributions in binary form must reproduce the above
             copyright notice, this list of conditions and the following
             disclaimer in the documentation and/or other materials
             provided with the distribution.

           - Neither the name of Internet Society, IETF or IETF Trust,
             nor the names of specific contributors, may be used to
             endorse or promote products derived from this software
             without specific prior written permission.

           THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
           CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED WARRANTIES,
           INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
           MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE





           DISCLAIMED.  IN NO EVENT SHALL THE COPYRIGHT OWNER OR
           CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
           SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
           NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
           LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
           HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
           CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR
           OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
           SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

           This version of this MIB module is part of RFC 5602;
           see the RFC itself for full legal notices.
          "

      -- Revision history.
       REVISION "200906120000Z"  -- 12 June 2009 00:00:00 GMT
       DESCRIPTION
           "First published as RFC 5602. "

     ::= { mib-2 181 }

   -- Top-level components of this MIB.

    -- Notifications
    pwMplsNotifications OBJECT IDENTIFIER
                                  ::= { pwMplsStdMIB 0 }

   -- Tables, Scalars
   pwMplsObjects       OBJECT IDENTIFIER
                                 ::= { pwMplsStdMIB 1 }
   -- Conformance
   pwMplsConformance   OBJECT IDENTIFIER
                                 ::= { pwMplsStdMIB 2 }

   -- PW MPLS table

   pwMplsTable   OBJECT-TYPE
      SYNTAX        SEQUENCE OF PwMplsEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This table controls MPLS-specific parameters when the PW is
           going to be carried over MPLS PSN."
      ::= { pwMplsObjects 1 }

   pwMplsEntry   OBJECT-TYPE
      SYNTAX        PwMplsEntry
      MAX-ACCESS    not-accessible





      STATUS        current
      DESCRIPTION
           "A row in this table represents parameters specific to MPLS
            PSN for a pseudowire (PW).  The row is created
            automatically by the local agent if the pwPsnType is
            mpls(1).  It is indexed by pwIndex, which uniquely
            identifies a singular PW.
            Manual entries in this table SHOULD be preserved after a
            reboot, and the agent MUST ensure the integrity of those
            entries.
            If the set of entries of a specific row were found to be
            nonconsistent after reboot, the PW pwOperStatus MUST be
            declared as down(2).
            Any read-write object in this table MAY be changed at any
            time; however, change of some objects (for example,
            pwMplsMplsType) during PW forwarding state MAY cause traffic
            disruption."

      INDEX  { pwIndex }

         ::= { pwMplsTable 1 }

   PwMplsEntry ::= SEQUENCE {
         pwMplsMplsType             BITS,
         pwMplsExpBitsMode          INTEGER,
         pwMplsExpBits              Unsigned32,
         pwMplsTtl                  Unsigned32,
         pwMplsLocalLdpID           MplsLdpIdentifier,
         pwMplsLocalLdpEntityIndex  Unsigned32,
         pwMplsPeerLdpID            MplsLdpIdentifier,
         pwMplsStorageType          StorageType
      }

   pwMplsMplsType OBJECT-TYPE
      SYNTAX   BITS {
          mplsTe    (0),
          mplsNonTe (1),
          pwOnly    (2)
               }
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
           "This object is set by the operator to indicate the outer
            tunnel types, if existing.  mplsTe(0) is used if the outer
            tunnel is set up by MPLS-TE, and mplsNonTe(1) is used if the
            outer tunnel is set up by LDP or manually.  A combination of
            mplsTe(0) and mplsNonTe(1) MAY exist.
            pwOnly(2) is used if there is no outer tunnel label, i.e.,





            in static provisioning without an MPLS tunnel.  pwOnly(2)
            cannot be combined with mplsNonTe(1) or mplsTe(0).
            An implementation that can identify automatically that the
            peer node is directly connected MAY support the bit
            pwOnly(2) as read-only.
           "
      DEFVAL { { mplsNonTe } }
      ::= { pwMplsEntry 1 }

   pwMplsExpBitsMode OBJECT-TYPE
      SYNTAX   INTEGER {
          outerTunnel      (1),
          specifiedValue   (2),
          serviceDependant (3)
               }

      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
          "This object is set by the operator to determine the PW shim
           label EXP bits.  The value of outerTunnel(1) is used where
           there is an outer tunnel -- pwMplsMplsType equals to
           mplsTe(0) or mplsNonTe(1).  Note that in this case, there
           is no need to mark the PW label with the EXP bits, since the
           PW label is not visible to the intermediate nodes.
           If there is no outer tunnel, specifiedValue(2) SHOULD be used
           to indicate that the value is specified by pwMplsExpBits.
           Setting serviceDependant(3) indicates that the EXP bits are
           set based on a rule that is implementation specific."

      DEFVAL { outerTunnel }
      ::= { pwMplsEntry 2 }

   pwMplsExpBits OBJECT-TYPE
      SYNTAX        Unsigned32 (0..7)
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
           "This object is set by the operator if pwMplsExpBitsMode is
            set to specifiedValue(2) to indicate the MPLS EXP bits to
            be used on the PW shim label.  Otherwise, it SHOULD be set
            to zero."
      DEFVAL { 0 }
      ::= { pwMplsEntry 3 }

   pwMplsTtl OBJECT-TYPE
      SYNTAX        Unsigned32 (0..255)
      MAX-ACCESS    read-write





      STATUS        current
      DESCRIPTION
           "This object is set by the operator to indicate the PW TTL
            value to be used on the PW shim label."
      DEFVAL { 2 }
      ::= { pwMplsEntry 4 }

   pwMplsLocalLdpID OBJECT-TYPE
      SYNTAX        MplsLdpIdentifier
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
           "The LDP identifier of the LDP entity that creates
            this PW in the local node.  As the PW labels are always
            set from the per-platform label space, the last two octets
            in the LDP ID MUST always both be zeros."
      REFERENCE
           "'LDP specifications', RFC 3036, section 2.2.2."
      ::= { pwMplsEntry 5 }

   pwMplsLocalLdpEntityIndex OBJECT-TYPE
      SYNTAX        Unsigned32 (1..4294967295)
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
           "The local node LDP Entity Index of the LDP entity creating
            this PW."
      ::= { pwMplsEntry 6 }

   pwMplsPeerLdpID OBJECT-TYPE
      SYNTAX        MplsLdpIdentifier
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
           "The peer LDP identifier of the LDP session.  This object
            SHOULD return the value zero if LDP is not used or if the
            value is not yet known."
      ::= { pwMplsEntry 7 }

   pwMplsStorageType OBJECT-TYPE
      SYNTAX        StorageType
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
          "This variable indicates the storage type for this row."
      DEFVAL { nonVolatile }
      ::= { pwMplsEntry 8 }






   -- End of PW MPLS Table

   -- Pseudowire MPLS Outbound Tunnel Table

   pwMplsOutboundTable   OBJECT-TYPE
      SYNTAX        SEQUENCE OF PwMplsOutboundEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This table reports and configures the current outbound MPLS
           tunnels (i.e., toward the PSN) or the physical interface in
           the case of a PW label only that carries the PW traffic.  It
           also reports the current outer tunnel and LSP that forward
           the PW traffic."
      ::= { pwMplsObjects 2 }

   pwMplsOutboundEntry OBJECT-TYPE
      SYNTAX        PwMplsOutboundEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "A row in this table configures the outer tunnel used for
           carrying the PW traffic toward the PSN.
           In the case of PW label only, it configures the interface
           that will carry the PW traffic.

           An entry in this table augments the pwMplsEntry, and is
           created automatically when the corresponding row has been
           created by the agent in the pwMplsEntry.

           This table points to the appropriate MPLS MIB module:

           In the MPLS-TE case, the three objects relevant to the
           indexing of a TE tunnel head-end (as used in the
           MPLS-TE-STD-MIB) are to be configured, and the tunnel
           instance indicates the LSP that is currently in use for
           forwarding the traffic.

           In the case of signaled non-TE MPLS (an outer tunnel label
           assigned by LDP), the table points to the XC entry in the
           LSR-STD-MIB.  If the non-TE MPLS tunnel is manually
           configured, the operator configures the XC pointer to this
           tunnel.

           In the case of PW label only (no outer tunnel), the ifIndex
           of the port to carry the PW is configured here.







           It is possible to associate a PW to one TE tunnel head-end
           and a non-TE tunnel together.  An indication in this table
           will report the currently active one.  In addition, in the
           TE case, the table reports the active tunnel instance
           (i.e., the specific LSP in use).
           Any read-write object in this table MAY be changed at any
           time; however, change of some objects (for example,
           MPLS-TE indexes) during PW forwarding state MAY cause traffic
           disruption."

      AUGMENTS { pwMplsEntry }

         ::= { pwMplsOutboundTable 1 }

   PwMplsOutboundEntry ::= SEQUENCE {
         pwMplsOutboundLsrXcIndex           MplsIndexType,
         pwMplsOutboundTunnelIndex          MplsTunnelIndex,
         pwMplsOutboundTunnelInstance       MplsTunnelInstanceIndex,
         pwMplsOutboundTunnelLclLSR         MplsLsrIdentifier,
         pwMplsOutboundTunnelPeerLSR        MplsLsrIdentifier,
         pwMplsOutboundIfIndex              InterfaceIndexOrZero,
         pwMplsOutboundTunnelTypeInUse      INTEGER
         }

   pwMplsOutboundLsrXcIndex      OBJECT-TYPE
      SYNTAX        MplsIndexType
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
          "This object is applicable if the pwMplsMplsType mplsNonTe(1)
           bit is set, and MUST return a value of zero otherwise.
           If the outer tunnel is signaled, the object is read-only
           and indicates the XC index in the MPLS-LSR-STD-MIB of the
           outer tunnel toward the peer.  Otherwise (tunnel is set up
           manually), the operator defines the XC index of the manually
           created outer tunnel through this object.
          "
      ::= { pwMplsOutboundEntry 1 }


   pwMplsOutboundTunnelIndex         OBJECT-TYPE
      SYNTAX        MplsTunnelIndex
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
          "This object is applicable if the pwMplsMplsType mplsTe(0)
           bit is set, and MUST return a value of zero otherwise.
           It is part of the set of indexes for the outbound tunnel.





           The operator sets this object to represent the desired
           tunnel head-end toward the peer for carrying the PW
           traffic.
          "
      ::= { pwMplsOutboundEntry  2 }

   pwMplsOutboundTunnelInstance      OBJECT-TYPE
      SYNTAX        MplsTunnelInstanceIndex
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
          "This object is applicable if the pwMplsMplsType mplsTe(0)
           bit is set, and MUST return a value of zero otherwise.
           It indicates the actual tunnel instance that is currently
           active and carrying the PW traffic.  It SHOULD return the
           value zero if the information from the MPLS-TE
           application is not yet known.
          "
      ::= { pwMplsOutboundEntry   3 }

   pwMplsOutboundTunnelLclLSR        OBJECT-TYPE
      SYNTAX        MplsLsrIdentifier
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
          "This object is applicable if the pwMplsMplsType mplsTe(0)
           bit is set, and MUST return a value of all zeros otherwise.
           It is part of the set of indexes for the outbound tunnel.
           The operator sets this object to represent the desired
           tunnel head-end toward the peer for carrying the PW
           traffic.
          "
      ::= { pwMplsOutboundEntry   4 }

   pwMplsOutboundTunnelPeerLSR       OBJECT-TYPE
      SYNTAX        MplsLsrIdentifier
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION
          "This object is applicable if the pwMplsMplsType mplsTe(0)
           bit is set, and MUST return a value of zero otherwise.
           It is part of the set of indexes for the outbound tunnel.
           Note that in most cases, it equals to pwPeerAddr.
          "
      ::= { pwMplsOutboundEntry   5 }

   pwMplsOutboundIfIndex       OBJECT-TYPE
      SYNTAX         InterfaceIndexOrZero





      MAX-ACCESS     read-write
      STATUS         current
      DESCRIPTION
          "This object is applicable if the pwMplsMplsType pwOnly(0)
           bit is set, and MUST return a value of zero otherwise.
           The operator configures the ifIndex of the outbound port
           in this case.
          "
      ::= { pwMplsOutboundEntry   6 }

   pwMplsOutboundTunnelTypeInUse OBJECT-TYPE
      SYNTAX         INTEGER {
                     notYetKnown (1),
                     mplsTe      (2),
                     mplsNonTe   (3),
                     pwOnly      (4)
      }
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
          "This object indicates the current tunnel that is carrying
           the PW traffic.
           The value of notYetKnown(1) should be used if the agent is
           currently unable to determine which tunnel or interface is
           carrying the PW, for example, because both tunnels are in
           operational status down.
          "
      ::= { pwMplsOutboundEntry   7 }

   -- End of PW MPLS Outbound Tunnel table

   -- PW MPLS inbound table

   pwMplsInboundTable OBJECT-TYPE
      SYNTAX           SEQUENCE OF PwMplsInboundEntry
      MAX-ACCESS       not-accessible
      STATUS           current
      DESCRIPTION
          "This table indicates the PW LDP XC entry in the
           MPLS-LSR-STD-MIB for signaled PWs.
          "
      ::= { pwMplsObjects 3 }

   pwMplsInboundEntry OBJECT-TYPE
      SYNTAX           PwMplsInboundEntry
      MAX-ACCESS       not-accessible
      STATUS           current
      DESCRIPTION





           "A row in this table is created by the agent
            for each signaled PW, and shows the XC index related to
            the PW signaling in the inbound direction in the
            MPLS-LSR-STD-MIB that controls and display the information
            for all the LDP signaling processes in the local node.
           "
      INDEX  { pwIndex }

         ::= { pwMplsInboundTable 1 }

   PwMplsInboundEntry ::= SEQUENCE {
         pwMplsInboundXcIndex           MplsIndexType
      }

   pwMplsInboundXcIndex OBJECT-TYPE
      SYNTAX        MplsIndexType
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
          "The XC index representing this PW in the inbound
           direction.  It MUST return the value zero if the
           information is not yet known."
      ::= { pwMplsInboundEntry 1 }

   -- End of PW MPLS inbound table

   -- PW to Non-TE mapping Table.

   pwMplsNonTeMappingTable OBJECT-TYPE
      SYNTAX           SEQUENCE OF PwMplsNonTeMappingEntry
      MAX-ACCESS       not-accessible
      STATUS           current
      DESCRIPTION
          "This table indicates the PW association to the outbound
           tunnel in non-TE applications, maps the PW to its (inbound)
           XC entry, and indicates the PW-to-physical interface mapping
           for a PW without an outer tunnel.
          "
      ::= { pwMplsObjects 4 }

   pwMplsNonTeMappingEntry OBJECT-TYPE
      SYNTAX           PwMplsNonTeMappingEntry
      MAX-ACCESS       not-accessible
      STATUS           current
      DESCRIPTION
           "A row in this table displays the association
            between the PW and
            - its non-TE MPLS outbound outer tunnel,





            - its XC entry in the MPLS-LSR-STD-MIB, or
            - its physical interface if there is no outer tunnel
              (PW label only) and manual configuration.

            Rows are created in this table by the agent depending on
            the setting of pwMplsMplsType:

            - If the pwMplsMplsType mplsNonTe(1) bit is set, the agent
            creates a row for the outbound direction
            (pwMplsNonTeMappingDirection set to psnBound(1)).
            The pwMplsNonTeMappingXcIndex holds the XC index in the
            MPLS-LSR-STD-MIB of the PSN-bound outer tunnel.
            pwMplsNonTeMappingIfIndex MUST be zero for this row.

            - If the pwMplsMplsType pwOnly(2) bit is set, the agent
            creates a row for the outbound direction
            (pwMplsNonTeMappingDirection set to psnBound(1)).
            The pwMplsNonTeMappingIfIndex holds the ifIndex of the
            physical port this PW will use in the outbound direction.
            pwMplsNonTeMappingXcIndex MUST be zero for this row.

            - If the PW has been set up by a signaling protocol (i.e.,
            pwOwner equal pwIdFecSignaling(2) or
            genFecSignaling(3)), the agent creates a row for the
            inbound direction (pwMplsNonTeMappingDirection set to
            fromPsn(2)).
            The pwMplsNonTeMappingXcIndex holds the XC index in the
            MPLS-LSR-STD-MIB of the PW LDP-generated XC entry.
            pwMplsNonTeMappingIfIndex MUST be zero for this row.

            An application can use this table to quickly retrieve the
            PW carried over specific non-TE MPLS outer tunnel or
            physical interface.
            "

      INDEX  { pwMplsNonTeMappingDirection,
               pwMplsNonTeMappingXcIndex,
               pwMplsNonTeMappingIfIndex,
               pwMplsNonTeMappingPwIndex }

         ::= { pwMplsNonTeMappingTable 1 }

   PwMplsNonTeMappingEntry ::= SEQUENCE {
         pwMplsNonTeMappingDirection         INTEGER,
         pwMplsNonTeMappingXcIndex           MplsIndexType,
         pwMplsNonTeMappingIfIndex           InterfaceIndexOrZero,
         pwMplsNonTeMappingPwIndex           PwIndexType
      }





   pwMplsNonTeMappingDirection OBJECT-TYPE
      SYNTAX        INTEGER {
                    psnBound (1),
                    fromPsn  (2)
      }
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "Index for the conceptual XC row identifying the tunnel-to-PW
           mappings, indicating the direction of the packet flow for
           this entry.
           psnBound(1) indicates that the entry is related to
           packets toward the PSN.
           fromPsn(2) indicates that the entry is related to
           packets coming from the PSN.
          "
      ::= { pwMplsNonTeMappingEntry 1 }

   pwMplsNonTeMappingXcIndex OBJECT-TYPE
      SYNTAX        MplsIndexType
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "See the description clause of pwMplsNonTeMappingEntry for
           the usage guidelines of this object."
      ::= { pwMplsNonTeMappingEntry 2 }

   pwMplsNonTeMappingIfIndex  OBJECT-TYPE
      SYNTAX        InterfaceIndexOrZero
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "See the description clause of pwMplsNonTeMappingEntry for
           the usage guidelines of this object."
      ::= { pwMplsNonTeMappingEntry 3 }

   pwMplsNonTeMappingPwIndex  OBJECT-TYPE
      SYNTAX        PwIndexType
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
          "The value that represents the PW in the pwTable."
      ::= { pwMplsNonTeMappingEntry 4 }

   -- End of PW to Non-TE mapping Table.


   -- PW to TE MPLS tunnels mapping Table.





   pwMplsTeMappingTable OBJECT-TYPE
      SYNTAX           SEQUENCE OF PwMplsTeMappingEntry
      MAX-ACCESS       not-accessible
      STATUS           current
      DESCRIPTION
          "This table reports the PW association to the
           outbound MPLS tunnel for MPLS-TE applications."
      ::= { pwMplsObjects 5 }

   pwMplsTeMappingEntry OBJECT-TYPE
      SYNTAX           PwMplsTeMappingEntry
      MAX-ACCESS       not-accessible
      STATUS           current
      DESCRIPTION
           "A row in this table represents the association
            between a PW and its MPLS-TE outer (head-end) tunnel.

            An application can use this table to quickly retrieve the
            list of the PWs that are configured on a specific MPLS-TE
            outer tunnel.

            The pwMplsTeMappingTunnelInstance reports the actual
            LSP out of the tunnel head-end that is currently
            forwarding the traffic.

            The table is indexed by the head-end indexes of a TE
            tunnel and the PW index.
           "

      INDEX  { pwMplsTeMappingTunnelIndex,
               pwMplsTeMappingTunnelInstance,
               pwMplsTeMappingTunnelPeerLsrID,
               pwMplsTeMappingTunnelLocalLsrID,
               pwMplsTeMappingPwIndex }

         ::= { pwMplsTeMappingTable 1 }

   PwMplsTeMappingEntry ::= SEQUENCE {
         pwMplsTeMappingTunnelIndex       MplsTunnelIndex,
         pwMplsTeMappingTunnelInstance    MplsTunnelInstanceIndex,
         pwMplsTeMappingTunnelPeerLsrID   MplsLsrIdentifier,
         pwMplsTeMappingTunnelLocalLsrID  MplsLsrIdentifier,
         pwMplsTeMappingPwIndex           PwIndexType
      }









   pwMplsTeMappingTunnelIndex OBJECT-TYPE
      SYNTAX        MplsTunnelIndex
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "Primary index for the conceptual row identifying the
           MPLS-TE tunnel that is carrying the PW traffic."
      ::= { pwMplsTeMappingEntry 1 }

   pwMplsTeMappingTunnelInstance OBJECT-TYPE
      SYNTAX        MplsTunnelInstanceIndex
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This object identifies the MPLS-TE LSP that is carrying the
           PW traffic.  It MUST return the value zero if the
           information of the specific LSP is not yet known.
           Note that based on the recommendation in the
           MPLS-TC-STD-MIB, instance index 0 should refer to the
           configured tunnel interface."
      ::= { pwMplsTeMappingEntry 2 }

   pwMplsTeMappingTunnelPeerLsrID  OBJECT-TYPE
      SYNTAX        MplsLsrIdentifier
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This object identifies the peer LSR when the outer tunnel
           is MPLS-TE."
      ::= { pwMplsTeMappingEntry 3 }

   pwMplsTeMappingTunnelLocalLsrID  OBJECT-TYPE
      SYNTAX        MplsLsrIdentifier
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This object identifies the local LSR."
      ::= { pwMplsTeMappingEntry 4 }

   pwMplsTeMappingPwIndex  OBJECT-TYPE
      SYNTAX        PwIndexType
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
          "This object returns the value that represents the PW in the
           pwTable."
      ::= { pwMplsTeMappingEntry 5 }






   -- End of PW to TE MPLS tunnels mapping Table.

   -- conformance information

   pwMplsGroups      OBJECT IDENTIFIER ::= { pwMplsConformance 1 }
   pwMplsCompliances OBJECT IDENTIFIER ::= { pwMplsConformance 2 }

   -- Compliance requirement for fully compliant implementations.

   pwMplsModuleFullCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for agents that provide full
                support for the PW-MPLS-STD-MIB module.  Such devices
                can then be monitored and also be configured using
                this MIB module."

      MODULE  -- this module
      MANDATORY-GROUPS { pwMplsGroup,
                         pwMplsOutboundMainGroup,
                         pwMplsInboundGroup,
                         pwMplsMappingGroup
                        }

      GROUP        pwMplsOutboundTeGroup
      DESCRIPTION "This group MUST be supported if the implementation
                   allows MPLS-TE tunnels to carry PW traffic.
                   "

      OBJECT       pwMplsMplsType
      DESCRIPTION "Support of pwOnly(2) is not required.  At least one
                   of mplsTe(0) or mplsNonTe(1) MUST be supported if
                   signaling of PW is supported.
                   "

      OBJECT       pwMplsExpBitsMode
      DESCRIPTION "Support of specifiedValue(2) and
                   serviceDependant(3) is optional.
                   "

      OBJECT       pwMplsLocalLdpID
      MIN-ACCESS   read-only
      DESCRIPTION "A read-write access is required if the
                   implementation supports more than one LDP entity
                   identifier for PW signaling.
                   "

      OBJECT       pwMplsLocalLdpEntityIndex





      MIN-ACCESS   read-only
      DESCRIPTION "A read-write access is required if the
                   implementation supports more than one LDP entity
                   index for PW signaling.
                   "

      OBJECT       pwMplsOutboundLsrXcIndex
      MIN-ACCESS   read-only
      DESCRIPTION "A value other than zero MUST be supported if the
                   implementation supports non-TE signaling of the
                   outer tunnel.
                   A read-write access MUST be supported if the
                   implementation supports PW label manual setting
                   and carrying them over non-TE tunnels.
                   "

      OBJECT       pwMplsOutboundIfIndex
      MIN-ACCESS   read-only
      DESCRIPTION "A value other than zero and read-write operations
                   MUST be supported if the implementation supports
                   manually configured PW without MPLS outer tunnel.
                   "
       ::= { pwMplsCompliances 1 }

   -- Compliance requirement for Read Only compliant implementations.

   pwMplsModuleReadOnlyCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for agents that provide read-
                only support for the PW-MPLS-STD-MIB module.  Such
                devices can then be monitored but cannot be configured
                using this MIB module."

      MODULE  -- this module
      MANDATORY-GROUPS { pwMplsGroup,
                         pwMplsOutboundMainGroup,
                         pwMplsInboundGroup,
                         pwMplsMappingGroup
                        }

      GROUP        pwMplsOutboundTeGroup
      DESCRIPTION "This group MUST be supported if the implementation
                   allows MPLS-TE tunnels to carry PW traffic.
                   "

      OBJECT       pwMplsMplsType
      MIN-ACCESS   read-only





      DESCRIPTION "Write access is not required.
                   Support of pwOnly(2) is not required.  At least one
                   of mplsTe(0) or mplsNonTe(1) MUST be supported if
                   signaling of PW is supported.
                   "

      OBJECT       pwMplsExpBitsMode
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   Support of specifiedValue(2) and serviceDependant(3)
                   is optional.
                   "
      OBJECT       pwMplsExpBits
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   "
      OBJECT       pwMplsTtl
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   "

      OBJECT       pwMplsLocalLdpID
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   "

      OBJECT       pwMplsLocalLdpEntityIndex
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   "

      OBJECT       pwMplsStorageType
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   "

      OBJECT       pwMplsOutboundLsrXcIndex
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   A value other than zero MUST be supported if the
                   implementation supports non-TE signaling of the
                   outer tunnel.
                   "

      OBJECT       pwMplsOutboundTunnelIndex
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   "





      OBJECT       pwMplsOutboundTunnelLclLSR
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   "

      OBJECT       pwMplsOutboundTunnelPeerLSR
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   "

      OBJECT       pwMplsOutboundIfIndex
      MIN-ACCESS   read-only
      DESCRIPTION "Write access is not required.
                   A value other than zero MUST be supported if the
                   implementation supports manually configured PW
                   without MPLS outer tunnel.
                   "
       ::= { pwMplsCompliances 2 }

   -- Units of conformance.

   pwMplsGroup OBJECT-GROUP
      OBJECTS {
               pwMplsMplsType,
               pwMplsExpBitsMode,
               pwMplsExpBits,
               pwMplsTtl,
               pwMplsLocalLdpID,
               pwMplsLocalLdpEntityIndex,
               pwMplsPeerLdpID,
               pwMplsStorageType
             }

      STATUS  current
      DESCRIPTION
          "Collection of objects needed for PW over MPLS PSN
           configuration."
      ::= { pwMplsGroups 1 }

   pwMplsOutboundMainGroup OBJECT-GROUP
      OBJECTS {
               pwMplsOutboundLsrXcIndex,
               pwMplsOutboundIfIndex,
               pwMplsOutboundTunnelTypeInUse
             }

      STATUS  current
      DESCRIPTION





          "Collection of objects needed for outbound association of
           PW and MPLS tunnel."
      ::= { pwMplsGroups 2 }

   pwMplsOutboundTeGroup OBJECT-GROUP
      OBJECTS {
               pwMplsOutboundTunnelIndex,
               pwMplsOutboundTunnelInstance,
               pwMplsOutboundTunnelLclLSR,
               pwMplsOutboundTunnelPeerLSR
             }

      STATUS  current
      DESCRIPTION
          "Collection of objects needed for outbound association of
           PW and MPLS-TE tunnel."
      ::= { pwMplsGroups 3 }

   pwMplsInboundGroup OBJECT-GROUP
      OBJECTS {
               pwMplsInboundXcIndex
             }

      STATUS  current
      DESCRIPTION
          "Collection of objects needed for inbound PW presentation.
           This group MUST be supported if PW signaling through LDP is
           used."
      ::= { pwMplsGroups 4 }

   pwMplsMappingGroup OBJECT-GROUP
      OBJECTS {
               pwMplsNonTeMappingPwIndex,
               pwMplsTeMappingPwIndex
             }

      STATUS  current
      DESCRIPTION
          "Collection of objects needed for mapping association of
           PW and MPLS tunnel."
      ::= { pwMplsGroups 5 }

   END









