FRNETSERV-MIB DEFINITIONS ::= BEGIN


IMPORTS
              MODULE-IDENTITY, OBJECT-TYPE,
              NOTIFICATION-TYPE, transmission,
              Counter32, Integer32             FROM SNMPv2-SMI
              TimeStamp, RowStatus             FROM SNMPv2-TC
              MODULE-COMPLIANCE, OBJECT-GROUP,
              NOTIFICATION-GROUP               FROM SNMPv2-CONF
              InterfaceIndex, ifIndex          FROM IF-MIB
              SnmpAdminString                  FROM SNMP-FRAMEWORK-MIB;

        frnetservMIB MODULE-IDENTITY
            LAST-UPDATED "200009280000Z" -- September 28, 2000
            ORGANIZATION "IETF Frame Relay Service MIB Working Group"
            CONTACT-INFO
                "WG Charter:
                   http://www.ietf.org/html.charters/frnetmib-charter
                 WG-email:
                   frnetmib@sunroof.eng.sun.com





                 Subscribe:
                   frnetmib-request@sunroof.eng.sun.com
                 Email Archive:
                   ftp://ftp.ietf.org/ietf-mail-archive/frnetmib

                 Chair:      Andy Malis
                             Vivace Networks, Inc.
                 Email:      Andy.Malis@vivacenetworks.com

                 WG editor:  Kenneth Rehbehn
                             Megisto Systems, Inc.
                 Email:      krehbehn@megisto.com

                 Co-author:  David Fowler
                             Syndesis Limited,
                 EMail:      fowler@syndesis.com"

            DESCRIPTION
                 "The MIB module to describe generic objects for
                  Frame Relay Network Service."

            --
            -- Revision History
            --
            REVISION "200009280000Z"
            DESCRIPTION
                 "Published as RFC 2954.

                 The major new features of this revision include:

                     o  Support for read-write capability to
                        provision switch components providing service,

                     o  Support for cross-connection via a frame relay
                        to ATM service interworking function,

                     o  Support for frame relay fragmentation,

                     o  Additional frame counters to track frame
                        loss.

                 Refer to Appendix A for a comprehensive list of
                 changes since RFC 1604."

            REVISION "199311161200Z"
            DESCRIPTION
                 "Published as RFC 1604."
            ::= { transmission 44 }





            frnetservObjects
                OBJECT IDENTIFIER ::= { frnetservMIB 1 }

            frnetservTraps
                OBJECT IDENTIFIER ::= { frnetservMIB 2 }

            frnetservTrapsPrefix
                OBJECT IDENTIFIER ::= { frnetservTraps 0 }

        --
        -- The Frame Relay Service Logical Port
        --
        frLportTable OBJECT-TYPE
            SYNTAX      SEQUENCE OF FrLportEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The Frame Relay Logical Port Information table is
                    an interface-specific addendum to the generic
                    ifTable of the Interface MIB."
            ::= { frnetservObjects 1 }

        frLportEntry OBJECT-TYPE
            SYNTAX      FrLportEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "An entry in the Frame Relay Logical Port
                    Information table."
            INDEX   {   ifIndex }
            ::= { frLportTable 1 }

        FrLportEntry ::=
            SEQUENCE {
                frLportNumPlan            INTEGER,
                frLportContact            SnmpAdminString,
                frLportLocation           SnmpAdminString,
                frLportType               INTEGER,
                frLportAddrDLCILen        INTEGER,
                frLportVCSigProtocol      INTEGER,
                frLportVCSigPointer       OBJECT IDENTIFIER,
                frLportDLCIIndexValue     Integer32,
                frLportTypeAdmin          INTEGER,
                frLportVCSigProtocolAdmin INTEGER,
                frLportFragControl        INTEGER,
                frLportFragSize           Integer32
        }






        frLportNumPlan OBJECT-TYPE
            SYNTAX      INTEGER {
                        other(1),
                        e164(2),
                        x121(3),
                        none(4)
                        }
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the network
                    address numbering plan for this UNI/NNI logical
                    port. The network address is the object
                    ifPhysAddress. The value none(4) implies that
                    there is no ifPhysAddress.  The FRS agent will
                    return an octet string of zero length for
                    ifPhysAddress.  The value other(1) means that an
                    address has been assigned to this interface, but
                    the numbering plan is not enumerated here."
            REFERENCE   "E.164 [29]
                         X.121 [30]"
            ::= { frLportEntry 1 }

        frLportContact  OBJECT-TYPE
            SYNTAX      SnmpAdminString
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the network
                    contact for this UNI/NNI logical port."
            ::= { frLportEntry 2 }

        frLportLocation OBJECT-TYPE
            SYNTAX      SnmpAdminString
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the frame
                    relay network location for this UNI/NNI logical
                    port."
            ::= { frLportEntry 3 }

        frLportType     OBJECT-TYPE
            SYNTAX      INTEGER {
                        uni(1),
                        nni(2)
                        }
            MAX-ACCESS  read-only





            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the type of
                    network interface for this logical port."
            ::= { frLportEntry 4 }

        frLportAddrDLCILen OBJECT-TYPE
            SYNTAX      INTEGER {
                        twoOctets10Bits(1),
                        threeOctets10Bits(2),
                        threeOctets16Bits(3),
                        fourOctets17Bits(4),
                        fourOctets23Bits(5)
                        }
            UNITS       "Octets"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the Q.922
                    Address field length and DLCI length for this
                    UNI/NNI logical port."
            REFERENCE   "Q.922 [25]"
            ::= { frLportEntry 5 }

        frLportVCSigProtocol OBJECT-TYPE
            SYNTAX      INTEGER {
                        none(1),
                        lmi(2),
                        ansiT1617D(3),
                        ansiT1617B(4),
                        ccittQ933A(5)
                        }
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the Local
                    In-Channel Signaling Protocol that is used for
                    this frame relay UNI/NNI logical port.

                    none(1):        Interface does not use a PVC
                                    signaling protocol

                    lmi(2):         Interface operates the Stratacom/
                                    Nortel/DEC Local Management
                                    Interface Specification protocol

                    ansiT1617D(3):  Interface operates the ANSI T1.617
                                    Annex D PVC status protocol





                      ansiT1617B(4):  Interface operates the ANSI
T1.617
                                      Annex B procedures

                      ccittQ933A(5):  Interface operates the ITU Q.933
                                      Annex A PVC status protocol"
              REFERENCE   "LMI [24]
                           T1.617 Annex D [17],
                           Q.933 Annex A [22]"
              ::= { frLportEntry 6 }

        frLportVCSigPointer OBJECT-TYPE
            SYNTAX      OBJECT IDENTIFIER
            MAX-ACCESS  read-only
            STATUS      deprecated
            DESCRIPTION
                    "The value of this object is used as a pointer to
                    the table that contains the Local In-Channel
                    Signaling Protocol parameters and errors for this
                    UNI/NNI logical port.

                    This object has been deprecated to reflect the
                    fact that the local in-channel signaling
                    parameters are accessed from a single table
                    (frMgtVCSigTable) that includes parameters for all
                    possible signaling protocols.  Early design
                    anticipated multiple tables, one for each
                    signaling protocol."
            ::= { frLportEntry 7 }

        frLportDLCIIndexValue OBJECT-TYPE
            SYNTAX      Integer32 (16..4194303)
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "This object contains a hint to be used for
                    frPVCEndptDLCIIndex when creating entries in the
                    frPVCEndptTable.  The SYNTAX of this object
                    matches the SYNTAX of the frPVCEndptDLCIIndex - an
                    object that is restricted to legal Q.922 DLCI
                    values for the size of the address field.

                    The value 0 indicates that no unassigned entries
                    are available.

                    To obtain the frPVCEndptDLCIIndex value for a new
                    entry, the manager issues a management protocol
                    retrieval operation to obtain the current value of





                    this object.  After each retrieval, the agent must
                    modify the value to the next unassigned index to
                    prevent assignment of the same value to multiple
                    management systems.

                    A management system should repeat the read to
                    obtain a new value should an attempt to create the
                    new row using the previously returned hint fail."
            REFERENCE   "Q.922 [25]"
            ::= { frLportEntry 8 }

        frLportTypeAdmin   OBJECT-TYPE
            SYNTAX      INTEGER {
                        uni(1),
                        nni(2)
                        }
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object desired identifies the
                    type of network interface for this logical port."
              ::= { frLportEntry 9 }

        frLportVCSigProtocolAdmin OBJECT-TYPE
            SYNTAX      INTEGER {
                        none(1),
                        lmi(2),
                        ansiT1617D(3),
                        ansiT1617B(4),
                        ccittQ933A(5)
                        }
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    Local In-Channel Signaling Protocol that is used
                    for this frame relay UNI/NNI logical port.  This
                    value must be made the active protocol as soon as
                    possible on the device.

                    Refer to frLportVCSigProtocol for a description of
                    each signaling protocol choices."
            REFERENCE   "LMI [24]
                         T1.617 Annex D [17],
                         Q.933 Annex A [22]"
            ::= { frLportEntry 10 }

        frLportFragControl OBJECT-TYPE





            SYNTAX      INTEGER {
                        on(1),
                        off(2)
                        }
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "This object controls the transmission and
                    reception of fragmentation frames for this UNI or
                    NNI interface.

                    on(1)   Frames are fragmented using the interface
                            fragmentation format
                            Note:  The customer side of the interface
                            must also be configured to fragment
                            frames.

                    off(2)  Frames are not fragmented using the
                            interface fragmentation format."
            REFERENCE   "FRF.12 [21]"
            DEFVAL { off }
            ::= { frLportEntry 11 }

        frLportFragSize OBJECT-TYPE
            SYNTAX      Integer32 (0..4096)
            UNITS       "Octets"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object is the size in octets of
                    the maximum size of each fragment to be sent when
                    fragmenting.  This object is only used by the
                    fragmentation transmitter, and the two sides of
                    the interface may differ.  The fragment size
                    includes the octets for the frame relay header,
                    the UI octet, the NLPID, the fragmentation header,
                    and the fragment payload. If frLportFragControl is
                    set to off, this value should be zero."
            REFERENCE   "FRF.12 [21]"
            DEFVAL { 0 }
            ::= { frLportEntry 12 }

        --
        -- Frame Relay Management VC Signaling
        --

        frMgtVCSigTable OBJECT-TYPE
            SYNTAX      SEQUENCE OF FrMgtVCSigEntry





            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The Frame Relay Management VC Signaling
                    Parameters and Errors table."
            ::= { frnetservObjects 2 }

        frMgtVCSigEntry OBJECT-TYPE
            SYNTAX      FrMgtVCSigEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "An entry in the Frame Relay Management VC
                    Signaling Parameters Errors table."
            INDEX       { ifIndex }
            ::= { frMgtVCSigTable 1 }

        FrMgtVCSigEntry ::=
            SEQUENCE {
                frMgtVCSigProced             INTEGER,
                frMgtVCSigUserN391           INTEGER,
                frMgtVCSigUserN392           INTEGER,
                frMgtVCSigUserN393           INTEGER,
                frMgtVCSigUserT391           INTEGER,
                frMgtVCSigNetN392            INTEGER,
                frMgtVCSigNetN393            INTEGER,
                frMgtVCSigNetT392            INTEGER,
                frMgtVCSigNetnN4             INTEGER,
                frMgtVCSigNetnT3             INTEGER,
                frMgtVCSigUserLinkRelErrors  Counter32,
                frMgtVCSigUserProtErrors     Counter32,
                frMgtVCSigUserChanInactive   Counter32,
                frMgtVCSigNetLinkRelErrors   Counter32,
                frMgtVCSigNetProtErrors      Counter32,
                frMgtVCSigNetChanInactive    Counter32,
                frMgtVCSigProcedAdmin        INTEGER,
                frMgtVCSigUserN391Admin      INTEGER,
                frMgtVCSigUserN392Admin      INTEGER,
                frMgtVCSigUserN393Admin      INTEGER,
                frMgtVCSigUserT391Admin      INTEGER,
                frMgtVCSigNetN392Admin       INTEGER,
                frMgtVCSigNetN393Admin       INTEGER,
                frMgtVCSigNetT392Admin       INTEGER,
                frMgtVCSigNetnT3Admin        INTEGER
        }

        frMgtVCSigProced OBJECT-TYPE
            SYNTAX      INTEGER {





                        u2nnet(1),
                        bidirect(2),
                        u2nuser(3)
                        }
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the local
                    in-channel signaling procedural role that is used
                    for this UNI/NNI logical port.  Bidirectional
                    procedures implies that both user-side and
                    network-side procedural roles are used.

                    u2nnet(1)   Logical port operates user to network
                                procedure in the role of the network
                                side

                    bidirect(2) Logical port operates the
                                bidirectional procedure (both user
                                and network side roles)

                    u2nuser(3)  Logical port operates user to network
                                procedure in the role of the user
                                side"
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            ::= { frMgtVCSigEntry 1 }

        frMgtVCSigUserN391 OBJECT-TYPE
            SYNTAX      INTEGER (1..255)
            UNITS       "Polls"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the User-side
                    N391 full status polling cycle value for this
                    UNI/NNI logical port.  If the logical port is not
                    performing user-side (bidirectional) procedures,
                    then this object is not instantiated and an
                    attempt to read will result in the noSuchInstance
                    exception response."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            DEFVAL { 6 }
            ::= { frMgtVCSigEntry 2 }

        frMgtVCSigUserN392 OBJECT-TYPE
            SYNTAX      INTEGER (1..10)





            UNITS       "Events"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the User-side
                    N392 error threshold value for this UNI/NNI
                    logical port.  If the logical port is not
                    performing user-side (bidirectional) procedures,
                    then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            DEFVAL { 3 }
            ::= { frMgtVCSigEntry 3 }

        frMgtVCSigUserN393 OBJECT-TYPE
            SYNTAX      INTEGER (1..10)
            UNITS       "Events"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the User-side
                    N393 monitored events count value for this UNI/NNI
                    logical port.  If the logical port is not
                    performing user-side (bidirectional) procedures,
                    then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            DEFVAL { 4 }
            ::= { frMgtVCSigEntry 4 }

        frMgtVCSigUserT391 OBJECT-TYPE
            SYNTAX      INTEGER (5..30)
            UNITS       "Seconds"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the User-side
                    T391 link integrity verification polling timer
                    value for this UNI/NNI logical port.  If the
                    logical port is not performing user-side
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            DEFVAL { 10 }
            ::= { frMgtVCSigEntry 5 }

        frMgtVCSigNetN392 OBJECT-TYPE
            SYNTAX      INTEGER (1..10)





            UNITS       "Events"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the Network-
                    side N392 error threshold value (nN2 for LMI) for
                    this UNI/NNI logical port.  If the logical port is
                    not performing network-side procedures, then this
                    object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17],
                         LMI [24]"
            DEFVAL { 3 }
            ::= { frMgtVCSigEntry 6 }

        frMgtVCSigNetN393 OBJECT-TYPE
            SYNTAX      INTEGER (1..10)
            UNITS       "Events"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the Network-
                    side N393 monitored events count value (nN3 for
                    LMI) for this UNI/NNI logical port.  If the
                    logical port is not performing network-side
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17],
                         LMI [24]"
            DEFVAL { 4 }
            ::= { frMgtVCSigEntry 7 }

        frMgtVCSigNetT392 OBJECT-TYPE
            SYNTAX      INTEGER (5..30)
            UNITS       "Seconds"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the Network-
                    side T392 polling verification timer value (nT2
                    for LMI)  for this UNI/NNI logical port.  If the
                    logical port is not performing network-side
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17],
                         LMI [24]"
            DEFVAL { 15 }
            ::= { frMgtVCSigEntry 8 }





        frMgtVCSigNetnN4 OBJECT-TYPE
            SYNTAX      INTEGER (5..5)
            UNITS       "Events"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the Network-
                    side nN4 maximum status enquires received value
                    for this UNI/NNI logical port.  If the logical
                    port is not performing network-side procedures or
                    is not performing LMI procedures, then this object
                    is not instantiated.

                    This object applies only to LMI and always has a
                    value of 5."
            REFERENCE   "LMI [24]"
            ::= { frMgtVCSigEntry 9 }

        frMgtVCSigNetnT3 OBJECT-TYPE
            SYNTAX      INTEGER (5 | 10 | 15 | 20 | 25 | 30)
            UNITS       "Seconds"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the Network-
                    side nT3 timer (for nN4 status enquires received)
                    value for this UNI/NNI logical port.  If the
                    logical port is not performing network-side
                    procedures or is not performing LMI procedures,
                    then this object is not instantiated.

                      This object applies only to LMI."
              REFERENCE   "LMI [24]"
              DEFVAL { 20 }
              ::= { frMgtVCSigEntry 10 }

        frMgtVCSigUserLinkRelErrors OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Errors"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of user-side local in-channel
                    signaling link reliability errors (i.e., non-
                    receipt of Status/Status Enquiry messages or
                    invalid sequence numbers in a Link Integrity
                    Verification Information Element) for this UNI/NNI
                    logical port.  If the logical port is not





                    performing user-side procedures, then this object
                    is not instantiated."
            ::= { frMgtVCSigEntry 11 }

        frMgtVCSigUserProtErrors OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Errors"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of user-side local in-channel
                    signaling protocol errors (i.e., protocol
                    discriminator, unnumbered information, message
                    type, call reference, and mandatory information
                    element errors) for this UNI/NNI logical port. If
                    the logical port is not performing user-side
                    procedures, then this object is not instantiated."
            ::= { frMgtVCSigEntry 12 }

      frMgtVCSigUserChanInactive OBJECT-TYPE
          SYNTAX      Counter32
          UNITS       "Events"
          MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of times the user-side channel was
                    declared inactive (i.e., N392 errors in N393
                    events) for this UNI/NNI logical port. If the
                    logical port is not performing user-side
                    procedures, then this object is not instantiated."
            ::= { frMgtVCSigEntry 13 }

        frMgtVCSigNetLinkRelErrors OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Errors"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of network-side local in-channel
                    signaling link reliability errors (i.e., non-
                    receipt of Status/Status Enquiry messages or
                    invalid sequence numbers in a Link Integrity
                    Verification Information Element) for this UNI/NNI
                    logical port."
            ::= { frMgtVCSigEntry 14 }

        frMgtVCSigNetProtErrors OBJECT-TYPE
            SYNTAX      Counter32





            UNITS       "Errors"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of network-side local in-channel
                    signaling protocol errors (i.e., protocol
                    discriminator, message type, call reference, and
                    mandatory information element errors) for this
                    UNI/NNI logical port."
            ::= { frMgtVCSigEntry 15 }

        frMgtVCSigNetChanInactive OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Events"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of times the network-side channel was
                    declared inactive (i.e., N392 errors in N393
                    events) for this UNI/NNI logical port."
            ::= { frMgtVCSigEntry 16 }

        frMgtVCSigProcedAdmin OBJECT-TYPE
            SYNTAX      INTEGER {
                        u2nnet(1),
                        bidirect(2),
                        u2nuser(3)
                        }
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the local
                    in-channel signaling procedural role that is used
                    for this UNI/NNI logical port.  Bidirectional
                    procedures implies that both user-side and
                    network-side procedural roles are used.

                    u2nnet(1)   Logical port operates user to network
                                procedure in the role of the network
                                side

                    bidirect(2) Logical port operates the
                                bidirectional procedure (both user
                                and network side roles)

                    u2nuser(3)  Logical port operates user to network
                                procedure in the role of the user
                                side"





            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            DEFVAL { u2nnet }
            ::= { frMgtVCSigEntry 17 }

        frMgtVCSigUserN391Admin OBJECT-TYPE
            SYNTAX      INTEGER (1..255)
            UNITS       "Polls"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    User-side N391 full status polling cycle value for
                    this UNI/NNI logical port.  If the logical port is
                    not performing user-side (bidirectional)
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            ::= { frMgtVCSigEntry 18 }

        frMgtVCSigUserN392Admin OBJECT-TYPE
            SYNTAX      INTEGER (1..10)
            UNITS       "Events"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    User-side N392 error threshold value for this
                    UNI/NNI logical port.  If the logical port is not
                    performing user-side (bidirectional) procedures,
                    then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            ::= { frMgtVCSigEntry 19 }

        frMgtVCSigUserN393Admin OBJECT-TYPE
            SYNTAX      INTEGER (1..10)
            UNITS       "Events"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    User-side N393 monitored events count value for
                    this UNI/NNI logical port.  If the logical port is
                    not performing user-side (bidirectional)
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"





            ::= { frMgtVCSigEntry 20 }

        frMgtVCSigUserT391Admin OBJECT-TYPE
            SYNTAX      INTEGER (5..30)
            UNITS       "Seconds"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    User-side T391 link integrity verification polling
                    timer value for this UNI/NNI logical port.  If the
                    logical port is not performing user-side
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17]"
            ::= { frMgtVCSigEntry 21 }

        frMgtVCSigNetN392Admin OBJECT-TYPE
            SYNTAX      INTEGER (1..10)
            UNITS       "Events"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    Network-side N392 error threshold value (nN2 for
                    LMI) for this UNI/NNI logical port.  If the
                    logical port is not performing network-side
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17],
                         LMI [24]"
            ::= { frMgtVCSigEntry 22 }

        frMgtVCSigNetN393Admin OBJECT-TYPE
            SYNTAX      INTEGER (1..10)
            UNITS       "Events"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    Network-side N393 monitored events count value
                    (nN3 for LMI) for this UNI/NNI logical port.  If
                    the logical port is not performing network-side
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17],
                         LMI [24]"
            ::= { frMgtVCSigEntry 23 }





        frMgtVCSigNetT392Admin OBJECT-TYPE
            SYNTAX      INTEGER (5..30)
            UNITS       "Seconds"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    Network-side T392 polling verification timer value
                    (nT2 for LMI)  for this UNI/NNI logical port. If
                    the logical port is not performing network-side
                    procedures, then this object is not instantiated."
            REFERENCE   "Q.933 Annex A [22],
                         T1.617 Annex D [17],
                         LMI [24]"
            ::= { frMgtVCSigEntry 24 }

        frMgtVCSigNetnT3Admin OBJECT-TYPE
            SYNTAX      INTEGER (5 | 10 | 15 | 20 | 25 | 30)
            UNITS       "Seconds"
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    Network-side nT3 timer (for nN4 status enquires
                    received) value for this UNI/NNI logical port. If
                    the logical port is not performing network-side
                    procedures or is not performing LMI procedures,
                    then this object is not instantiated.  This object
                    applies only to LMI."
            REFERENCE   "LMI [24]"
            ::= { frMgtVCSigEntry 25 }

        --
        -- Frame Relay PVC End-points
        --

        frPVCEndptTable OBJECT-TYPE
            SYNTAX      SEQUENCE OF FrPVCEndptEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The Frame Relay PVC End-Point table.  This table
                    is used to model a PVC end-point.  This table
                    contains the traffic parameters and statistics for
                    a PVC end-point.

                    This table is used to identify the traffic
                    parameters for a bi-directional PVC segment end-





                    point, and it also provides statistics for a PVC
                    segment end-point.

                    A PVC segment end-point is identified by a UNI/NNI
                    logical port index value and DLCI index value.

                    If the frame relay service provider allows the
                    frame relay CNM subscriber to create, modify or
                    delete PVCs using SNMP, then this table is used to
                    identify and reserve the requested traffic
                    parameters of each PVC segment end-point.  The
                    Connection table is used to 'connect' the end-
                    points together.  Not all implementations will
                    support the capability of
                    creating/modifying/deleting PVCs using SNMP as a
                    feature of frame relay CNM service.

                    Uni-directional PVCs are modeled with zero valued
                    traffic parameters in one of the directions (In or
                     Out direction) in this table.

                    To create a PVC, the following procedures shall be
                    followed:

                    1)  Create the entries for the PVC segment
                        endpoints in the frPVCEndptTable by specifying
                        the traffic parameters for the bi-directional
                        PVC segment endpoints. As shown in figure 2, a
                        point-to-point PVC has two endpoints, thus two
                        entries in this table.  Uni-directional PVCs
                        are modeled with zero valued traffic
                        parameters in one direction; all the `In'
                        direction parameters for one frame relay PVC
                        End-point or all the `Out' direction
                        parameters for the other frame relay PVC
                        Endpoint.

                        In    _____________________________  Out
                       >>>>>>|                             |>>>>>>>>
                       ______|    Frame Relay Network      |________
                        Out  |                             |  In
                       <<<<<<|_____________________________|<<<<<<<<
                     Frame Relay                         Frame Relay
                         PVC                                 PVC
                       Endpoint                            Endpoint

                                Figure 2, PVC Terminology






                    2)  Go to the Frame Relay Connection Group."
            ::= { frnetservObjects 3 }

        frPVCEndptEntry OBJECT-TYPE
            SYNTAX      FrPVCEndptEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "An entry in the Frame Relay PVC Endpoint table."
            INDEX   { ifIndex, frPVCEndptDLCIIndex }
            ::= { frPVCEndptTable 1 }

        FrPVCEndptEntry ::=
            SEQUENCE {
                frPVCEndptDLCIIndex            Integer32,
                frPVCEndptInMaxFrameSize       Integer32,
                frPVCEndptInBc                 Integer32,
                frPVCEndptInBe                 Integer32,
                frPVCEndptInCIR                Integer32,
                frPVCEndptOutMaxFrameSize      Integer32,
                frPVCEndptOutBc                Integer32,
                frPVCEndptOutBe                Integer32,
                frPVCEndptOutCIR               Integer32,
                frPVCEndptConnectIdentifier    Integer32,
                frPVCEndptRowStatus            RowStatus,
                frPVCEndptRcvdSigStatus        INTEGER,
                frPVCEndptInFrames             Counter32,
                frPVCEndptOutFrames            Counter32,
                frPVCEndptInDEFrames           Counter32,
                frPVCEndptInExcessFrames       Counter32,
                frPVCEndptOutExcessFrames      Counter32,
                frPVCEndptInDiscards           Counter32,
                frPVCEndptInOctets             Counter32,
                frPVCEndptOutOctets            Counter32,
                frPVCEndptInDiscardsDESet      Counter32,
                frPVCEndptInFramesFECNSet      Counter32,
                frPVCEndptOutFramesFECNSet     Counter32,
                frPVCEndptInFramesBECNSet      Counter32,
                frPVCEndptOutFramesBECNSet     Counter32,
                frPVCEndptInCongDiscards       Counter32,
                frPVCEndptInDECongDiscards     Counter32,
                frPVCEndptOutCongDiscards      Counter32,
                frPVCEndptOutDECongDiscards    Counter32,
                frPVCEndptOutDEFrames          Counter32,
                frPVCEndptAtmIwfConnIndex      Integer32

            }






        frPVCEndptDLCIIndex OBJECT-TYPE
            SYNTAX      Integer32 (16..4194303)
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the DLCI
                    value for this PVC end-point.

                    The values are restricted to the legal range for
                    the size of address field supported by the logical
                    port (frLportAddrDLCILen)."
            REFERENCE   "Q.922 [25]"
            ::= { frPVCEndptEntry 1 }

        frPVCEndptInMaxFrameSize OBJECT-TYPE
            SYNTAX      Integer32 (1..4096)
            UNITS       "Octets"
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object is the size in octets of
                    the largest frame relay information field for this
                    PVC end-point in the ingress direction (into the
                    frame relay network).  The value of
                    frPVCEndptInMaxFrameSize must be less than or
                    equal to the corresponding ifMtu for this frame
                    relay UNI/NNI logical port."
            REFERENCE   "FRF.1 [31]
                         Q.922 [25]
                         Q.933 [22]"
            DEFVAL { 1600 }
            ::= { frPVCEndptEntry 2 }

        frPVCEndptInBc OBJECT-TYPE
            SYNTAX      Integer32 (1..2147483647)
            UNITS       "Bits"
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the
                    committed burst size (Bc) parameter (measured in
                    bits) for this PVC end-point in the ingress
                    direction (into the frame relay network).

                    Note that the max value of this range is lower
                    than the max value allowed by Q.933 (16383 *
                    10**6).






                    Note that the value is encoded in bits whilst the
                    Q.933 Link layer core parameters information
                    element encodes this information using octet
                    units."
            REFERENCE   "Q.933 [22]"
            ::= { frPVCEndptEntry 3 }

        frPVCEndptInBe OBJECT-TYPE
            SYNTAX      Integer32 (1..2147483647)
            UNITS       "Bits"
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the excess
                    burst size (Be) parameter (measured in bits) for
                    this PVC end-point in the ingress direction (into
                    the frame relay network).

                    Note that the max value of this range is lower
                    than the max value allowed by Q.933 (16383 *
                    10**6).

                    Note that the value is encoded in bits whilst the
                    Q.933 Link layer core parameters information
                    element encodes this information using octet
                    units."
            REFERENCE   "Q.933 [22]"
            ::= { frPVCEndptEntry 4 }

        frPVCEndptInCIR OBJECT-TYPE
            SYNTAX      Integer32 (1..2147483647)
            UNITS       "Bits per Second"
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the
                    committed information rate (CIR) parameter
                    (measured in bits per second) for this PVC end-
                    point in the ingress direction (into the frame
                    relay network).

                    Note that the max value of this range is lower
                    than the max value allowed by Q.933 (2047 *
                    10**6)."
            REFERENCE   "Q.933 [22]"
            ::= { frPVCEndptEntry 5 }

        frPVCEndptOutMaxFrameSize OBJECT-TYPE





            SYNTAX      Integer32 (1..4096)
            UNITS       "Octets"
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object is the size in octets of
                    the largest frame relay information field for this
                    PVC end-point in the egress direction (out of the
                    frame relay network).  The value of
                    frPVCEndptOutMaxFrameSize must be less than or
                    equal to the corresponding ifMtu for this frame
                    relay UNI/NNI logical port."
            REFERENCE   "FRF.1 [31]
                         Q.922 [25]
                         Q.933 [22]"
            DEFVAL { 1600 }
            ::= { frPVCEndptEntry 6 }

        frPVCEndptOutBc OBJECT-TYPE
            SYNTAX      Integer32 (1..2147483647)
            UNITS       "Bits"
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the
                    committed burst size (Bc) parameter (measured in
                    bits) for this PVC end-point in the egress
                    direction (out of the frame relay network).

                    Note that the max value of this range is lower
                    than the max value allowed by Q.933 (16383 *
                    10**6).

                    Note that the value is encoded in bits whilst the
                    Q.933 Link layer core parameters information
                    element encodes this information using octet
                    units."
            REFERENCE   "Q.933 [22]"
            ::= { frPVCEndptEntry 7 }

        frPVCEndptOutBe OBJECT-TYPE
            SYNTAX      Integer32 (1..2147483647)
            UNITS       "Bits"
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the excess
                    burst size (Be) parameter (measured in bits) for





                    this PVC end-point in the egress direction (out of
                    the frame relay network).

                    Note that the max value of this range is lower
                    than the max value allowed by Q.933 (16383 *
                    10**6).

                    Note that the value is encoded in bits whilst the
                    Q.933 Link layer core parameters information
                    element encodes this information using octet
                    units."
            REFERENCE   "Q.933 [22]"
            ::= { frPVCEndptEntry 8 }

        frPVCEndptOutCIR OBJECT-TYPE
            SYNTAX      Integer32 (1..2147483647)
            UNITS       "Bits per Second"
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the
                    committed information rate (CIR) parameter
                    (measured in bits per second) for this PVC end-
                    point in the egress direction (out of the frame
                    relay network).

                    Note that the max value of this range is lower
                    than the max value allowed by Q.933 (2047 *
                    10**6)."
            REFERENCE   "Q.933 [22]"
            ::= { frPVCEndptEntry 9 }

        frPVCEndptConnectIdentifier OBJECT-TYPE
            SYNTAX      Integer32 (0..2147483647)
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "This object is used to associate PVC end-points
                    as being part of one PVC segment connection. This
                    value of this object is equal to the value of
                    frPVCConnectIndex, which is used as one of the
                    indices into the frPVCConnectTable.

                    A connection that has been cross-connected via the
                    FR/ATM PVC Service IWF cross-connect table will
                    return the value zero when this object is read. In
                    case of these interworked connections, the
                    frPVCEndptAtmIwfConnIndex object must be accessed





                    to select the entry in the FR/ATM PVC Service IWF
                    cross-connect table.

                    The value of this object is provided by the agent,
                    after the associated entries in the
                    frPVCConnectTable or frAtmIwfConnectionTable have
                    been created."
            ::= { frPVCEndptEntry 10 }

        frPVCEndptRowStatus OBJECT-TYPE
            SYNTAX      RowStatus
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "This object is used to create new rows in this
                    table, modify existing rows, and to delete
                    existing rows.  To create a new PVC, the entries
                    for the PVC segment end-points in the
                    frPVCEndptTable must first be created.  Next, the
                    frPVCConnectTable is used to associate the frame
                    relay PVC segment end-points.  In order for the
                    manager to have the necessary error diagnostics,
                    the frPVCEndptRowStatus object must initially be
                    set to `createAndWait(5)'.  While the
                    frPVCEndptRowStatus object is in the
                    `createAndWait(5)' state, the manager can set each
                    columnar object and get the necessary error
                    diagnostics.  The frPVCEndptRowStatus object may
                    not be set to `active(1)' unless the following
                    columnar objects exist in this row:
                    frPVCEndptInMaxFrameSize, frPVCEndptInBc,
                    frPVCEndptInBe, frPVCEndptInCIR,
                    frPVCEndptOutMaxFrameSize, frPVCEndptOutBc,
                    frPVCEndptOutBe, and frPVCEndptOutCIR."
            ::= { frPVCEndptEntry 11 }

        frPVCEndptRcvdSigStatus OBJECT-TYPE
            SYNTAX      INTEGER {
                        deleted(1),
                        active(2),
                        inactive(3),
                        none(4)
                        }
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the PVC
                    status received via the local in-channel signaling





                    procedures for this PVC end-point.  This object is
                    only pertinent for interfaces that perform the
                    bidirectional procedures.

                    Each value has the following meaning:
                      deleted(1):  This PVC is not listed in the full
                                   status reports received from the
                                   user device.  The object retains
                                   this value for as long as the PVC
                                   is not listed in the full status
                                   reports

                    active(2):   This PVC is reported as active, or
                                   operational, by the user device.

                      inactive(3): This PVC is reported as inactive,
                                   or non-operational, by the user
                                   device.

                      none(4):     This interface is only using the
                                   network-side in-channel signaling
                                   procedures, so this object does
                                   not apply."
            ::= { frPVCEndptEntry 12 }

        frPVCEndptInFrames OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames received by the network
                    (ingress) for this PVC end-point. This includes
                    any frames discarded by the network due to
                    submitting more than Bc + Be data or due to any
                    network congestion recovery procedures."
            ::= { frPVCEndptEntry 13 }

        frPVCEndptOutFrames OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames sent by the network (egress)
                    regardless of whether they are Bc or Be frames for
                    this PVC end-point."
            ::= { frPVCEndptEntry 14 }





        frPVCEndptInDEFrames OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames received by the network
                    (ingress) with the DE bit set to (1) for this PVC
                    end-point."
            ::= { frPVCEndptEntry 15 }

        frPVCEndptInExcessFrames OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames received by the network
                    (ingress) for this PVC end-point which were
                    treated as excess traffic.  Frames which are sent
                    to the network with DE set to zero are treated as
                    excess when more than Bc bits are submitted to the
                    network during the Committed Information Rate
                    Measurement Interval (Tc).  Excess traffic may or
                    may not be discarded at the ingress if more than
                    Bc + Be bits are submitted to the network during
                    Tc.  Traffic discarded at the ingress is not
                    recorded in frPVCEndptInExcessFrames.  Frames
                    which are sent to the network with DE set to one
                    are also treated as excess traffic."
            ::= { frPVCEndptEntry 16 }

        frPVCEndptOutExcessFrames OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames sent by the network (egress)
                    for this PVC end-point which were treated as
                    excess traffic.  (The DE bit may be set to one.)"
            ::= { frPVCEndptEntry 17 }

        frPVCEndptInDiscards OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current





            DESCRIPTION
                    "The number of frames received by the network
                    (ingress) that were discarded due to traffic
                    enforcement for this PVC end-point.  Congestion
                    discards are not counted in this object."
            ::= { frPVCEndptEntry 18 }

        frPVCEndptInOctets OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Octets"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of octets received by the network
                    (ingress) for this PVC end-point.  This counter
                    should only count octets from the beginning of the
                    frame relay header field to the end of user data.
                    If the network supporting frame relay can not
                    count octets, then this count should be an
                    approximation."
            ::= { frPVCEndptEntry 19 }

        frPVCEndptOutOctets OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Octets"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of octets sent by the network (egress)
                    for this PVC end-point.  This counter should only
                    count octets from the beginning of the frame relay
                    header field to the end of user data.  If the
                    network supporting frame relay can not count
                    octets, then this count should be an
                    approximation."
            ::= { frPVCEndptEntry 20 }

        frPVCEndptInDiscardsDESet OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames received by the network
                    (ingress) that were discarded with the DE bit set
                    due to traffic enforcement for this PVC end-point.
                    Congestion discards are not counted in this
                    object."





            ::= { frPVCEndptEntry 21 }

        frPVCEndptInFramesFECNSet OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames received by the network
                    (ingress) that have the FECN bit set for this PVC
                    end-point."
            ::= { frPVCEndptEntry 22 }

        frPVCEndptOutFramesFECNSet OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames sent by the network (egress)
                    that have the FECN bit set for this PVC end-
                    point."
            ::= { frPVCEndptEntry 23 }

        frPVCEndptInFramesBECNSet OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames received by the network
                    (ingress) that have the BECN bit set for this PVC
                    end-point."
            ::= { frPVCEndptEntry 24 }

        frPVCEndptOutFramesBECNSet OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames sent by the network (egress)
                    that have the BECN bit set for this PVC end-
                    point."
            ::= { frPVCEndptEntry 25 }

        frPVCEndptInCongDiscards OBJECT-TYPE
            SYNTAX      Counter32





            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames received by the network
                    (ingress) that were discarded due to input buffer
                    congestion, rather than traffic enforcement, for
                    this PVC end-point."
            ::= { frPVCEndptEntry 26 }

        frPVCEndptInDECongDiscards OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames counted by
                    frPVCEndptInCongDiscards with the DE bit set to
                    (1)."
            ::= { frPVCEndptEntry 27 }

        frPVCEndptOutCongDiscards OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames sent by the network (egress)
                    that were discarded due to output buffer
                    congestion for this PVC end-point."
            ::= { frPVCEndptEntry 28 }

        frPVCEndptOutDECongDiscards OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The number of frames counted by
                    frPVCEndptOutCongDiscards with the DE bit set to
                    (1)."
            ::= { frPVCEndptEntry 29 }

        frPVCEndptOutDEFrames OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Frames"
            MAX-ACCESS  read-only
            STATUS      current





            DESCRIPTION
                    "The number of frames sent by the network (egress)
                    with the DE bit set to (1) for this PVC end-
                    point."
            ::= { frPVCEndptEntry 30 }

        frPVCEndptAtmIwfConnIndex OBJECT-TYPE
            SYNTAX      Integer32  (0..2147483647)
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "This object contains the index value of the
                    FR/ATM cross-connect table entry used to link the
                    frame relay PVC with an ATM PVC.

                    Each row of the frPVCEndptTable that is not
                    cross-connected with an ATM PVC must return the
                    value zero when this object is read.

                    The value of this object is initialized by the
                    agent after the associated entries in the
                    frAtmIwfConnectionTable have been created.

                    The value of this object is reset to zero
                    following destruction of the associated entry in
                    the frAtmIwfConnectionTable"
            ::= { frPVCEndptEntry 31 }

        --
        -- Frame Relay PVC Connections
        --

        frPVCConnectIndexValue OBJECT-TYPE
            SYNTAX      INTEGER (0..2147483647)
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "This object returns a hint to be used for
                    frPVCConnectIndex when creating entries in the
                    frPVCConnectTable.

                    The value 0 indicates that no unassigned entries
                    are available.

                    To obtain the frPVCConnectIndex value for a new
                    entry, the manager issues a management protocol
                    retrieval operation to obtain the current value of
                    this object.  After each retrieval, the agent must





                    modify the value to the next unassigned index to
                    prevent assignment of the same value to multiple
                    management systems.

                    A management system should repeat the read to
                    obtain a new value should an attempt to create the
                    new row using the previously returned hint fail."
            ::= { frnetservObjects 4 }

        frPVCConnectTable OBJECT-TYPE
            SYNTAX      SEQUENCE OF FrPVCConnectEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The Frame Relay PVC Connect Table is used to
                    model the bi-directional PVC segment flows
                    including:  point-to-point PVCs, point-to-
                    multipoint PVCs, and multipoint-to-multipoint
                    PVCs.

                    This table has read-create access and is used to
                    associate PVC end-points together as belonging to
                    one connection.  The frPVCConnectIndex is used to
                    associate all the bi-directional flows.  Not all
                    implementations will support the capability of
                    creating/modifying/deleting PVCs using SNMP as a
                    feature of frame relay CNM service.

                    Once the entries in the frPVCEndptTable are
                    created, the following step are used to associate
                    the PVC end-points as belonging to one PVC
                    connection:

                    1)  Obtain a unique frPVCConnectIndex
                        using the frPVCConnectIndexValue object.

                    2)  Connect the PVC segment endpoints together
                        with the applicable frPVCConnectIndex value
                        obtained via  frPVCConnectIndexValue.  The
                        entries in this table are created by using
                        the frPVCConnectRowStatus object.

                    3)  The agent will provide the value of the
                        corresponding instances of
                        frPVCEndptConnectIdentifier with the
                        frPVCConnectIndex value.

                    4)  Set frPVCConnectAdminStatus to `active(1)' in





                        all rows for this PVC segment to turn the
                        PVC on.

                    For example, the Frame Relay PVC Connection Group
                    models a bi-directional, point-to-point PVC
                    segment as one entry in this table.

                    Frame Relay                           Frame Relay
                     Network                                 Network
                     Low Port                               High Port
                             __________________________________
                            |                                  |
                       _____| >> from low to high PVC flow  >> |_____
                            | << from high to low PVC flow  << |
                            |__________________________________|

                    The terms low and high are chosen to represent
                    numerical ordering of a PVC segment's endpoints
                    for representation in this table.  That is, the
                    endpoint with the lower value of ifIndex is termed
                    'low', while the opposite endpoint of the segment
                    is termed 'high'.  This terminology is to provide
                    directional information; for example the
                    frPVCConnectL2hOperStatus and
                    frPVCConnectH2lOperStatus as illustrated above.

                    If the Frame Relay Connection table is used to
                    model a unidirectional PVC, then one direction
                    (either from low to high or from high to low) has
                     its Operational Status equal to down.

                     A PVC segment is a portion of a PVC that traverses
                    one Frame Relay Network, and a PVC segment is
                    identified by its two end-points (UNI/NNI logical
                    port index value and DLCI index value) through one
                    Frame Relay Network."
            ::= { frnetservObjects 5 }

        frPVCConnectEntry OBJECT-TYPE
            SYNTAX      FrPVCConnectEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "An entry in the Frame Relay PVC Connect table.
                    This entry is used to model a PVC segment in two
                    directions."
            INDEX { frPVCConnectIndex,
                    frPVCConnectLowIfIndex,





                    frPVCConnectLowDLCIIndex,
                    frPVCConnectHighIfIndex,
                    frPVCConnectHighDLCIIndex }
            ::= { frPVCConnectTable 1 }

        FrPVCConnectEntry ::=
            SEQUENCE {
                frPVCConnectIndex            Integer32,
                frPVCConnectLowIfIndex       InterfaceIndex,
                frPVCConnectLowDLCIIndex     Integer32,
                frPVCConnectHighIfIndex      InterfaceIndex,
                frPVCConnectHighDLCIIndex    Integer32,
                frPVCConnectAdminStatus      INTEGER,
                frPVCConnectL2hOperStatus    INTEGER,
                frPVCConnectH2lOperStatus    INTEGER,
                frPVCConnectL2hLastChange    TimeStamp,
                frPVCConnectH2lLastChange    TimeStamp,
                frPVCConnectRowStatus        RowStatus,
                frPVCConnectUserName         SnmpAdminString,
                frPVCConnectProviderName     SnmpAdminString
        }

          frPVCConnectIndex OBJECT-TYPE
              SYNTAX      Integer32 (0..2147483647)
              MAX-ACCESS  not-accessible
              STATUS      current
              DESCRIPTION
                      "The value of this object is equal to the
                      frPVCConnectIndexValue obtained to uniquely
                      identify this PVC segment connection."
              ::= { frPVCConnectEntry 1 }

        frPVCConnectLowIfIndex OBJECT-TYPE
            SYNTAX      InterfaceIndex
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to IF-MIB
                    ifIndex value of the UNI/NNI logical port for this
                    PVC segment.  The term low implies that this PVC
                    segment end-point has the numerically lower
                    ifIndex value than the connected/associated PVC
                    segment end-point.

                    RFC 1604 permitted a zero value for this object to
                    identify termination at a non-frame relay
                    interface.  However, this cross-connect table is
                    limited to frame relay connections.  See the frame





                    relay/ATM IWF MIB [28] for the cross-connect table
                    used for those types of connections."
            ::= { frPVCConnectEntry 2 }

        frPVCConnectLowDLCIIndex OBJECT-TYPE
            SYNTAX      Integer32 (16..4194303)
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the DLCI
                    value for this end-point of the PVC segment."
            REFERENCE   "Q.922 [25]"
            ::= { frPVCConnectEntry 3 }

        frPVCConnectHighIfIndex OBJECT-TYPE
            SYNTAX      InterfaceIndex
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to IF-MIB
                    ifIndex value for the UNI/NNI logical port for
                    this PVC segment.  The term high implies that this
                    PVC segment end-point has the numerically higher
                    ifIndex value than the connected/associated PVC
                    segment end-point."
            ::= { frPVCConnectEntry 4 }

        frPVCConnectHighDLCIIndex OBJECT-TYPE
            SYNTAX      Integer32 (16..4194303)
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the egress
                    DLCI value for this end-point of the PVC segment."
            REFERENCE   "Q.922 [25]"
            ::= { frPVCConnectEntry 5 }

        frPVCConnectAdminStatus OBJECT-TYPE
            SYNTAX      INTEGER {
                        active(1),
                        inactive(2),
                        testing(3)
                        }
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the desired
                    administrative status of this bi-directional PVC





                    segment.  The active(1) state means the PVC
                    segment is currently operational; the inactive(2)
                    state means the PVC segment is currently not
                    operational; the testing(3) state means the PVC
                    segment is currently undergoing a test.  This
                    state is set by an administrative entity.  This
                    value affects the PVC status indicated across the
                    ingress NNI/UNI of both end-points of the bi-
                    directional PVC segment.  When a PVC segment
                    connection is created using this table, this
                    object is initially set to `inactive(2)'.  After
                    the frPVCConnectRowStatus object is set to
                    `active(1)' (and the corresponding/associated
                    entries in the frPVCEndptTable have their
                    frPVCEndptRowStatus object set to `active(1)'),
                    the frPVCConnectAdminStatus object may be set to
                    `active(1)' to turn on the PVC segment
                    connection."
            ::= { frPVCConnectEntry 6 }

        frPVCConnectL2hOperStatus OBJECT-TYPE
            SYNTAX      INTEGER {
                        active(1),
                        inactive(2),
                        testing(3),
                        unknown(4)
                        }
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the current
                    operational status of the PVC segment connection
                    in one direction; (i.e., in the low to high
                    direction). This value affects the PVC status
                    indicated across the ingress NNI/UNI (low side) of
                    the PVC segment.

                    The values mean:

                    active(1)   - PVC is currently operational

                    inactive(2) - PVC is currently not operational.
                                  This may be because of an underlying
                                  LMI or DS1 failure.

                    testing(3)  - PVC is currently undergoing a test.
                                  This may be because of an underlying
                                  frLport or DS1 undergoing a test.





                    unknown(4)  - the status of the PVC currently can
                                  not be determined."
            ::= { frPVCConnectEntry 7 }

        frPVCConnectH2lOperStatus OBJECT-TYPE
            SYNTAX      INTEGER {
                        active(1),
                        inactive(2),
                        testing(3),
                        unknown(4)
                        }
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object identifies the current
                    operational status of the PVC segment connection
                    in one direction; (i.e., in the high to low
                    direction)..  This value affects the PVC status
                    indicated across the ingress NNI/UNI (high side)
                    of the PVC segment.

                    The values mean:

                    active(1)   - PVC is currently operational

                    inactive(2) - PVC is currently not operational.
                                  This may be because of an underlying
                                  LMI or DS1 failure.

                    testing(3)  - PVC is currently undergoing a test.
                                  This may be because of an underlying
                                  frLport or DS1 undergoing a test.

                    unknown(4)  - the status of the PVC currently can
                                  not be determined."
            ::= { frPVCConnectEntry 8 }

        frPVCConnectL2hLastChange OBJECT-TYPE
            SYNTAX      TimeStamp
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of the Interface MIB's sysUpTime object
                    at the time this PVC segment entered its current
                    operational state in the low to high direction.
                    If the current state was entered prior to the last
                    re-initialization of the FRS agent, then this
                    object contains a zero value."





            ::= { frPVCConnectEntry 9 }

        frPVCConnectH2lLastChange OBJECT-TYPE
            SYNTAX      TimeStamp
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of the Interface MIB's sysUpTime object
                    at the time this PVC segment entered its current
                    operational state in the high to low direction.
                    If the current state was entered prior to the last
                    re-initialization of the FRS agent, then this
                    object contains a zero value."
            ::= { frPVCConnectEntry 10 }

        frPVCConnectRowStatus OBJECT-TYPE
            SYNTAX      RowStatus
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "The status of this entry in the
                    frPVCConnectTable.  This variable is used to
                    create new connections for the PVC end-points and
                    to change existing connections of the PVC end-
                    points.  This object must be initially set to
                    `createAndWait(5)'. In this state, the agent
                    checks the parameters in the associated entries in
                    the frPVCEndptTable to verify that the PVC end-
                    points can be connected (i.e., the In parameters
                    for one PVC end-point are equal to the Out
                    parameters for the other PVC end-point).  This
                    object can not be set to `active(1)' unless the
                    following columnar object exists in this row:
                    frPVCConnectAdminStatus.  The agent also supplies
                    the associated value of frPVCConnectIndex for the
                    frPVCEndptConnectIdentifier instances.  To turn on
                    a PVC segment connection, the
                    frPVCConnectAdminStatus is set to `active(1)'."
            ::= { frPVCConnectEntry 11 }

        frPVCConnectUserName OBJECT-TYPE
            SYNTAX      SnmpAdminString
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "This is a service user assigned textual
                    representation of a PVC."
            ::= { frPVCConnectEntry 12 }





        frPVCConnectProviderName OBJECT-TYPE
            SYNTAX      SnmpAdminString
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
                    "This is a system supplied textual representation
                    of PVC.  It is assigned by the service provider."
            ::= { frPVCConnectEntry 13 }

        --
        -- The Frame Relay Accounting
        --

        frAccountPVCTable OBJECT-TYPE
            SYNTAX      SEQUENCE OF FrAccountPVCEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The Frame Relay Accounting PVC table.  This table
                    is used to perform accounting on a PVC segment
                    end-point basis."
            ::= { frnetservObjects 6 }

        frAccountPVCEntry OBJECT-TYPE
            SYNTAX      FrAccountPVCEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "An entry in the Frame Relay Accounting PVC
                    table."
            INDEX   {   ifIndex,
                        frAccountPVCDLCIIndex }
            ::= { frAccountPVCTable 1 }

        FrAccountPVCEntry ::=
            SEQUENCE {
                frAccountPVCDLCIIndex            Integer32,
                frAccountPVCSegmentSize          Integer32,
                frAccountPVCInSegments           Counter32,
                frAccountPVCOutSegments          Counter32
            }

        frAccountPVCDLCIIndex OBJECT-TYPE
            SYNTAX      Integer32 (16..4194303)
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the DLCI





                    value for this PVC segment end-point."
            REFERENCE   "Q.922 [25]"
            ::= { frAccountPVCEntry 1 }

        frAccountPVCSegmentSize OBJECT-TYPE
            SYNTAX      Integer32
            UNITS       "Octets"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the Segment
                    Size for this PVC segment end-point."
            ::= { frAccountPVCEntry 2 }

        frAccountPVCInSegments OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Segments"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the number
                    of segments received by this PVC segment end-
                    point."
            ::= { frAccountPVCEntry 3 }

        frAccountPVCOutSegments OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Segments"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the number
                    of segments sent by this PVC segment end-point."
            ::= { frAccountPVCEntry 4 }

        --
        -- Accounting on a Frame Relay Logical Port
        --

        frAccountLportTable OBJECT-TYPE
            SYNTAX      SEQUENCE OF FrAccountLportEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "The Frame Relay Accounting Logical Port table.
                    This table is used to perform accounting on a
                    UNI/NNI Logical Port basis."
            ::= { frnetservObjects 7 }





        frAccountLportEntry OBJECT-TYPE
            SYNTAX      FrAccountLportEntry
            MAX-ACCESS  not-accessible
            STATUS      current
            DESCRIPTION
                    "An entry in the Frame Relay Accounting Logical
                    Port table."
            INDEX   {   ifIndex }
            ::= { frAccountLportTable 1 }

        FrAccountLportEntry ::=
            SEQUENCE {
                frAccountLportSegmentSize
                    Integer32,
                frAccountLportInSegments
                    Counter32,
                frAccountLportOutSegments
                    Counter32
            }

        frAccountLportSegmentSize OBJECT-TYPE
            SYNTAX      Integer32
            UNITS       "Octets"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the Segment
                    Size for this UNI/NNI logical port."
            ::= { frAccountLportEntry 1 }

        frAccountLportInSegments OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Segments"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the number
                    of segments received by this UNI/NNI logical
                    port."
            ::= { frAccountLportEntry 2 }

        frAccountLportOutSegments OBJECT-TYPE
            SYNTAX      Counter32
            UNITS       "Segments"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                    "The value of this object is equal to the number





                    of segments sent by this UNI/NNI logical port."
            ::= { frAccountLportEntry 3 }

          --
          -- Frame Relay Network Service Notifications
          --

        frPVCConnectStatusChange  NOTIFICATION-TYPE
            OBJECTS { frPVCConnectIndex,
                      frPVCConnectLowIfIndex,
                      frPVCConnectLowDLCIIndex,
                      frPVCConnectHighIfIndex,
                      frPVCConnectHighDLCIIndex,
                      frPVCConnectL2hOperStatus,
                      frPVCConnectH2lOperStatus,
                      frPVCEndptRcvdSigStatus }
            STATUS  deprecated
            DESCRIPTION
                    "Refer to the description of the
                    frPVCConnectStatusNotif notification that has
                    replaced this notification.  The notification is
                    deprecated due to the incorrect inclusion of index
                    values and to take advantage of the trap prefix
                    for automatic conversion from SMIv2 to SMIv1 by
                    making the one but last sub-ID a zero (i.e. the
                    so-called trap prefix)."
            ::= { frnetservTraps 1 }

        frPVCConnectStatusNotif  NOTIFICATION-TYPE
            OBJECTS { frPVCConnectL2hOperStatus,
                      frPVCConnectH2lOperStatus,
                      frPVCEndptRcvdSigStatus }
            STATUS  current
            DESCRIPTION
                    "This notification indicates that the indicated
                    PVC has changed state.

                    This notification is not sent if an FR-UNI changes
                    state; a linkDown or linkUp notification should be
                    sent instead.  The first instance of
                    frPVCEndptRcvdSigStatus is for the endpoint with
                    LowIfIndex, LowDLCIIndex.  The second instance of
                    frPVCEndptRcvdSigStatus is for the endpoint with
                    HighIfIndex, HighDLCIIndex"
            ::= { frnetservTrapsPrefix 2 }

        -- Conformance Information






        frnetservConformance  OBJECT IDENTIFIER
            ::= { frnetservMIB 3 }

        frnetservGroups       OBJECT IDENTIFIER
            ::= { frnetservConformance 1 }
        frnetservCompliances  OBJECT IDENTIFIER
            ::= { frnetservConformance 2 }


        --
        --  Service (Read-only) Modules
        --
        frnetservCompliance2 MODULE-COMPLIANCE
            STATUS      current
            DESCRIPTION
                    "The compliance statement for SNMP entities which
                    have Frame Relay Network Service Interfaces.

                    The distinction between 'service' and 'switch' is
                    that a 'switch' is configured via this MIB.
                    Hence, the various read/write objects have write
                    capability.  A 'service' represents a passive
                    monitor-only customer network management
                    interface.  The various read/write objects are
                    restricted to read-only capability."
            MODULE -- this module
                MANDATORY-GROUPS { frnetservLportGroup2,
                                   frnetservMgtVCSigGroup,
                                   frnetservPVCEndptGroup,
                                   frnetservPVCEndptGroup2,
                                   frnetservPVCConnectGroup,
                                   frnetservPVCConnectNamesGroup,
                                   frnetservPVCNotifGroup2 }

                GROUP       frnetservAccountPVCGroup
                DESCRIPTION
                    "This group is optional for frame relay
                    interfaces.  It is mandatory if and only if
                    accounting is performed on a PVC basis this frame
                    relay interface."
                GROUP       frnetservAccountLportGroup
                DESCRIPTION
                    "This group is optional for frame relay
                    interfaces.  It is mandatory if and only if
                    accounting is performed on a logical port basis
                    this frame relay interface."

                OBJECT      frPVCEndptInMaxFrameSize





                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCEndptInBc
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCEndptInBe
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCEndptInCIR
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCEndptOutMaxFrameSize
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCEndptOutBc
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCEndptOutBe
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCEndptOutCIR
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCEndptRowStatus
             -- subset of RowStatus
                SYNTAX      INTEGER { active(1) }
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required, and only one of the
                    six enumerated values for the RowStatus textual
                    convention need be supported, specifically:
                    active(1)."





                OBJECT      frPVCConnectAdminStatus
                MIN-ACCESS  read-only
                DESCRIPTION
                     "Write access is not required."

                OBJECT      frPVCConnectRowStatus
             -- subset of RowStatus
                SYNTAX      INTEGER { active(1) }
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required, and only one of the
                    six enumerated values for the RowStatus textual
                    convention need be supported, specifically:
                    active(1)."

                OBJECT      frLportFragControl
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frLportFragSize
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCConnectUserName
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

                OBJECT      frPVCConnectProviderName
                MIN-ACCESS  read-only
                DESCRIPTION
                      "Write access is not required."

              ::= { frnetservCompliances 2 }

        --
        -- Switch (Configuration) Compliance
        --
        frnetSwitchCompliance MODULE-COMPLIANCE
            STATUS      current
            DESCRIPTION
                    "The compliance statement for SNMP entities which
                    have Frame Relay Network Switch objects.

                    The distinction between 'service' and 'switch' is
                    that a 'switch' is configured via this MIB.





                    Hence, the various read/write objects have write
                    capability.  A 'service' represents a passive
                    monitor-only customer network management
                    interface.  The various read/write objects are
                    restricted to read-only capability."
            MODULE -- this module
                MANDATORY-GROUPS { frnetservLportGroup2,
                                   frnetservLportAdminGroup,
                                   frnetservMgtVCSigGroup,
                                   frnetservMgtVCSigAdminGroup,
                                   frnetservPVCEndptGroup,
                                   frnetservPVCEndptGroup2,
                                   frnetservPVCConnectGroup,
                                   frnetservPVCConnectNamesGroup,
                                   frnetservPVCNotifGroup2 }

                GROUP       frnetservAccountPVCGroup
                DESCRIPTION
                    "This group is optional for frame relay
                    interfaces.  It is mandatory if and only if
                    accounting is performed on a PVC basis this frame
                    relay interface."
                GROUP       frnetservAccountLportGroup
                DESCRIPTION
                    "This group is optional for frame relay
                    interfaces.  It is mandatory if and only if
                    accounting is performed on a logical port basis
                    this frame relay interface."

              ::= { frnetservCompliances 3 }

         --
         -- Historical RFC 1604 Compliance Modules
         --

        frnetservCompliance MODULE-COMPLIANCE
            STATUS  deprecated
            DESCRIPTION
                    "The compliance statement for SNMP entities which
                    have Frame Relay Network Service Interfaces.

                    This compliance statement has been deprecated in
                    favor of frnetservCompliance2.  The new compliance
                    module expands the mandatory groups to include
                    notification and other new objects."

            MODULE -- this module
                MANDATORY-GROUPS { frnetservLportGroup,





                                   frnetservMgtVCSigGroup,
                                   frnetservPVCEndptGroup,
                                   frnetservPVCConnectGroup }

                GROUP       frnetservAccountPVCGroup
                DESCRIPTION
                    "This group is optional for Frame Relay
                    interfaces.  It is mandatory if and only if
                    accounting is performed on a PVC basis this Frame
                    Relay interface."

                GROUP       frnetservAccountLportGroup
                DESCRIPTION
                    "This group is optional for Frame Relay
                    interfaces.  It is mandatory if and only if
                    accounting is performed on a logical port basis
                    this Frame Relay interface."

                OBJECT      frPVCEndptInMaxFrameSize
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."

                OBJECT      frPVCEndptInBc
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."
                OBJECT      frPVCEndptInBe
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."

                OBJECT      frPVCEndptInCIR
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."

                OBJECT      frPVCEndptOutMaxFrameSize
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."

                OBJECT      frPVCEndptOutBc
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."

                OBJECT      frPVCEndptOutBe





                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."

                OBJECT      frPVCEndptOutCIR
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."

                OBJECT      frPVCEndptRowStatus
             -- subset of RowStatus
                SYNTAX      INTEGER { active(1) }
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required, and only one of the
                    six enumerated values for the RowStatus textual
                    convention need be supported, specifically:
                    active(1)."

                OBJECT      frPVCConnectAdminStatus
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required."

                OBJECT      frPVCConnectRowStatus
             -- subset of RowStatus
                SYNTAX      INTEGER { active(1) }
                MIN-ACCESS  read-only
                DESCRIPTION
                    "Write access is not required, and only one of the
                    six enumerated values for the RowStatus textual
                    convention need be supported, specifically:
                    active(1)."
            ::= { frnetservCompliances 1 }

         --
         -- Frame Relay Service MIB Object Groups
         --
         frnetservLportGroup  OBJECT-GROUP
             OBJECTS { frLportNumPlan, frLportContact, frLportLocation,
                       frLportType,
                       frLportAddrDLCILen, frLportVCSigProtocol,
                       frLportVCSigPointer }
             STATUS  deprecated
             DESCRIPTION
                     "A collection of objects providing information
                     applicable to a Frame Relay Logical Port.  This
                     group has been deprecated to eliminate reference





                     to the object frLportVCSigPointer.

                     Use the new group frnetservLportGroup2 as a
                     replacement for this group."
             ::= { frnetservGroups 1 }

        frnetservMgtVCSigGroup  OBJECT-GROUP
            OBJECTS { frMgtVCSigProced,
                      frMgtVCSigUserN391,
                      frMgtVCSigUserN392,
                      frMgtVCSigUserN393,
                      frMgtVCSigUserT391,
                      frMgtVCSigNetN392,
                      frMgtVCSigNetN393,
                      frMgtVCSigNetT392,
                      frMgtVCSigNetnN4,
                      frMgtVCSigNetnT3,
                      frMgtVCSigUserLinkRelErrors,
                      frMgtVCSigUserProtErrors,
                      frMgtVCSigUserChanInactive,
                      frMgtVCSigNetLinkRelErrors,
                      frMgtVCSigNetProtErrors,
                      frMgtVCSigNetChanInactive }
            STATUS  current
            DESCRIPTION
                    "A collection of objects providing information
                    applicable to the Local In-Channel Signaling
                    Procedures used for a UNI/NNI logical port."
            ::= { frnetservGroups 2 }

        frnetservPVCEndptGroup  OBJECT-GROUP
            OBJECTS { frPVCConnectIndexValue,
                      frPVCEndptInMaxFrameSize,
                      frPVCEndptInBc,
                      frPVCEndptInBe,
                      frPVCEndptInCIR,
                      frPVCEndptOutMaxFrameSize,
                      frPVCEndptOutBc,
                      frPVCEndptOutBe,
                      frPVCEndptOutCIR,
                      frPVCEndptConnectIdentifier,
                      frPVCEndptRowStatus,
                      frPVCEndptRcvdSigStatus,
                      frPVCEndptInFrames,
                      frPVCEndptOutFrames,
                      frPVCEndptInDEFrames,
                      frPVCEndptInExcessFrames,
                      frPVCEndptOutExcessFrames,





                      frPVCEndptInDiscards,
                      frPVCEndptInOctets,
                      frPVCEndptOutOctets }
            STATUS  current
            DESCRIPTION
                    "A collection of objects providing information
                    applicable to a Frame Relay PVC end-point."
            ::= { frnetservGroups 3 }

        frnetservPVCConnectGroup  OBJECT-GROUP
            OBJECTS { frPVCConnectAdminStatus,
                      frPVCConnectL2hOperStatus,
                      frPVCConnectH2lOperStatus,
                      frPVCConnectL2hLastChange,
                      frPVCConnectH2lLastChange,
                      frPVCConnectRowStatus }
            STATUS  current
            DESCRIPTION
                    "A collection of objects providing information
                    applicable to a Frame Relay PVC connection."
            ::= { frnetservGroups 4 }

        frnetservAccountPVCGroup  OBJECT-GROUP
            OBJECTS { frAccountPVCSegmentSize,
                      frAccountPVCInSegments,
                      frAccountPVCOutSegments }
            STATUS  current
            DESCRIPTION
                    "A collection of objects providing accounting
                    information application to a Frame Relay PVC end-
                    point."
            ::= { frnetservGroups 5 }

        frnetservAccountLportGroup  OBJECT-GROUP
            OBJECTS { frAccountLportSegmentSize,
                      frAccountLportInSegments,
                      frAccountLportOutSegments }
            STATUS  current
            DESCRIPTION
                    "A collection of objects providing accounting
                    information application to a Frame Relay logical
                    port."
            ::= { frnetservGroups 6 }

        frnetservLportGroup2  OBJECT-GROUP
            OBJECTS { frLportNumPlan,
                      frLportContact,
                      frLportLocation,





                      frLportType,
                      frLportAddrDLCILen,
                      frLportVCSigProtocol,
                      frLportFragControl,
                      frLportFragSize }
            STATUS  current
            DESCRIPTION
                    "A collection of objects providing information
                    applicable to a Frame Relay Logical Port.

                    This new version of the Logical Port Group
                    eliminates the frLportVCSigPointer and adds
                    support for fragmentation."
            ::= { frnetservGroups 7 }

        frnetservPVCEndptGroup2  OBJECT-GROUP
              OBJECTS { frPVCEndptInDiscardsDESet,
                        frPVCEndptInFramesFECNSet,
                        frPVCEndptOutFramesFECNSet,
                        frPVCEndptInFramesBECNSet,
                        frPVCEndptOutFramesBECNSet,
                        frPVCEndptInCongDiscards,
                        frPVCEndptInDECongDiscards,
                        frPVCEndptOutCongDiscards,
                        frPVCEndptOutDECongDiscards,
                        frPVCEndptOutDEFrames,
                        frPVCEndptAtmIwfConnIndex }
              STATUS  current
              DESCRIPTION
                    "Additions to the PVC end-point group.  These
                    additions provide new frame counters to track
                    frame loss.  In addition, the new FR/ATM IWF MIB
                    cross-connect index is included."
              ::= { frnetservGroups 8 }

        frnetservPVCConnectNamesGroup  OBJECT-GROUP
              OBJECTS { frPVCConnectUserName,
                        frPVCConnectProviderName }
              STATUS  current
              DESCRIPTION
                    "Additions to the PVC Connect Group."
              ::= { frnetservGroups 9 }

        frnetservLportAdminGroup OBJECT-GROUP
              OBJECTS { frLportDLCIIndexValue,
                        frLportTypeAdmin,
                        frLportVCSigProtocolAdmin }
              STATUS  current





              DESCRIPTION
                    "Administrative (R/W) objects for creating a
                    switch logical port."
              ::= { frnetservGroups 10 }

        frnetservMgtVCSigAdminGroup OBJECT-GROUP
              OBJECTS { frMgtVCSigProcedAdmin,
                        frMgtVCSigUserN391Admin,
                        frMgtVCSigUserN392Admin,
                        frMgtVCSigUserN393Admin,
                        frMgtVCSigUserT391Admin,
                        frMgtVCSigNetN392Admin,
                        frMgtVCSigNetN393Admin,
                        frMgtVCSigNetT392Admin,
                        frMgtVCSigNetnT3Admin }
              STATUS  current
              DESCRIPTION

                    "A collection of objects providing information
                    applicable to the Local In-Channel Signaling
                    Procedures used for a UNI/NNI logical port."
              ::= { frnetservGroups 11 }

        frnetservPVCNotifGroup NOTIFICATION-GROUP
              NOTIFICATIONS { frPVCConnectStatusChange }
              STATUS    deprecated
              DESCRIPTION
                    "Deprecated notification group.  The
                    frPVCConnectStatusChange notification was flawed
                    because it included redundant indexes and was not
                    properly encoded for SMIv1 conversion."
            ::= { frnetservGroups 12 }

        frnetservPVCNotifGroup2 NOTIFICATION-GROUP
              NOTIFICATIONS { frPVCConnectStatusNotif }
              STATUS    current
              DESCRIPTION
                    "A collection of notifications that apply to frame
                    relay PVC Connections "
            ::= { frnetservGroups 13 }

        END










