NATV2-MIB DEFINITIONS ::= BEGIN


IMPORTS
     MODULE-IDENTITY,
     OBJECT-TYPE,
     Integer32,
     Unsigned32,
     Counter64,
     mib-2,
     NOTIFICATION-TYPE
             FROM SNMPv2-SMI          -- RFC 2578
     TEXTUAL-CONVENTION,
     DisplayString,
     TimeStamp
             FROM SNMPv2-TC           -- RFC 2579
     MODULE-COMPLIANCE,
     NOTIFICATION-GROUP,
     OBJECT-GROUP
             FROM SNMPv2-CONF         -- RFC 2580
     SnmpAdminString
             FROM SNMP-FRAMEWORK-MIB  -- RFC 3411
     InetAddressType,
     InetAddress,
     InetAddressPrefixLength,
     InetPortNumber
             FROM INET-ADDRESS-MIB;   -- RFC 4001

natv2MIB MODULE-IDENTITY
     LAST-UPDATED "201510020000Z" -- 2 October 2015

     ORGANIZATION
             "IETF Behavior Engineering for Hindrance
               Avoidance (BEHAVE) Working Group"
     CONTACT-INFO
             "Working Group Email: behave@ietf.org

              Simon Perreault
              Jive Communications
              Quebec, QC
              Canada

              Email: sperreault@jive.com






              Tina Tsou
              Huawei Technologies
              Bantian, Longgang
              Shenzhen 518129
              China

              Email: tina.tsou.zouting@huawei.com

              Senthil Sivakumar
              Cisco Systems
              7100-8 Kit Creek Road
              Research Triangle Park, North Carolina  27709
              United States

              Phone: +1 919 392 5158
              Email: ssenthil@cisco.com

              Tom Taylor
              PT Taylor Consulting
              Ottawa
              Canada

              Email: tom.taylor.stds@gmail.com"

     DESCRIPTION
             "This MIB module defines the generic managed objects
              for NAT.

              Copyright (c) 2015 IETF Trust and the persons
              identified as authors of the code.  All rights reserved.

              Redistribution and use in source and binary forms, with
              or without modification, is permitted pursuant to, and
              subject to the license terms contained in, the Simplified
              BSD License set forth in Section 4.c of the IETF Trust's
              Legal Provisions Relating to IETF Documents
              (http://trustee.ietf.org/license-info).

              This version of this MIB module is part of RFC 7659;
              see the RFC itself for full legal notices."
     REVISION     "201510020000Z" -- 2 October 2015
     DESCRIPTION
             "Complete rewrite, published as RFC 7659.
              Replaces former version published as RFC 4008."
     ::= { mib-2 234 }

-- Textual conventions






ProtocolNumber ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
        "A protocol number, from the IANA Protocol Numbers
         registry."
    REFERENCE
        "IANA Protocol Numbers,
         <http://www.iana.org/assignments/protocol-numbers>"
    SYNTAX Unsigned32 (0..255)

Natv2SubscriberIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
        "A unique value, greater than zero, for each subscriber
         in the managed system.  The value for each
         subscriber MUST remain constant at least from one
         update of the entity's natv2SubscriberDiscontinuityTime
         object until the next update of that object.  If a
         subscriber is deleted, its assigned index value MUST NOT
         be assigned to another subscriber at least until
         reinitialization of the entity's management system."
    SYNTAX Unsigned32 (1..4294967295)

Natv2SubscriberIndexOrZero ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
        "This textual convention is an extension of the
         Natv2SubscriberIndex convention.  The latter defines a
         greater than zero value used to identify a subscriber in
         the managed system.  This extension permits the additional
         value of zero, which serves as a placeholder when no
         subscriber is associated with the object."
    SYNTAX Unsigned32 (0|1..4294967295)

Natv2InstanceIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
        "A unique value, greater than zero, for each NAT instance
         in the managed system.  It is RECOMMENDED that values are
         assigned contiguously starting from 1.  The value for each
         NAT instance MUST remain constant at least from one
         update of the entity's natv2InstanceDiscontinuityTime
         object until the next update of that object.  If a NAT
         instance is deleted, its assigned index value MUST NOT





         be assigned to another NAT instance at least until
         reinitialization of the entity's management system."
    SYNTAX Unsigned32 (1..4294967295)

Natv2PoolIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
       "A unique value over the containing NAT instance, greater than
        zero, for each address pool supported by that NAT instance.
        It is RECOMMENDED that values are assigned contiguously
        starting from 1.  The value for each address pool MUST remain
        constant at least from one update of the entity's
        natv2PoolDiscontinuityTime object until the next update of
        that object.  If an address pool is deleted, its assigned
        index value MUST NOT be assigned to another address pool for
        the same NAT instance at least until reinitialization of the
        entity's management system."
    SYNTAX Unsigned32 (1..4294967295)

Natv2PoolIndexOrZero ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
        "This textual convention is an extension of the
         Natv2PoolIndex convention.  The latter defines a greater
         than zero value used to identify address pools in the
         managed system.  This extension permits the additional
         value of zero, which serves as a placeholder when the
         implementation does not support address pools or no address
         pool is configured in a given external realm."
    SYNTAX Unsigned32 (0|1..4294967295)

-- Notifications

natv2MIBNotifications OBJECT IDENTIFIER ::= { natv2MIB 0 }

natv2NotificationPoolUsageLow NOTIFICATION-TYPE
    OBJECTS { natv2PoolNotifiedPortMapEntries,
              natv2PoolNotifiedPortMapProtocol  }
    STATUS current
    DESCRIPTION
        "This notification is triggered when an address pool's usage
         becomes less than or equal to the value of the
         natv2PoolThresholdUsageLow object for that pool, unless the
         notification has been disabled by setting the value of the
         threshold to -1.  It is reported subject to the rate
         limitation specified by natv2PortMapNotificationInterval.





         Address pool usage is calculated as the percentage of the
         total number of ports allocated to the address pool that are
         already in use, for the most-mapped protocol at the time
         the notification is triggered.  The two returned objects are
         members of natv2PoolTable indexed by the NAT instance and
         pool indices for which the event is being reported.  They
         give the number of port map entries using external addresses
         configured on the pool for the most-mapped protocol and
         identify that protocol at the time the notification was
         triggered."
    REFERENCE
        "RFC 7659, Sections 3.1.2 and 3.3.6."
    ::= { natv2MIBNotifications 1 }

natv2NotificationPoolUsageHigh NOTIFICATION-TYPE
    OBJECTS { natv2PoolNotifiedPortMapEntries,
              natv2PoolNotifiedPortMapProtocol  }
    STATUS current
    DESCRIPTION
        "This notification is triggered when an address pool's usage
         becomes greater than or equal to the value of the
         natv2PoolThresholdUsageHigh object for that pool, unless
         the notification has been disabled by setting the value of
         the threshold to -1.  It is reported subject to the rate
         limitation specified by natv2PortMapNotificationInterval.

         Address pool usage is calculated as the percentage of the
         total number of ports allocated to the address pool that are
         already in use, for the most-mapped protocol at the time the
         notification is triggered.  The two returned objects are
         members of natv2PoolTable indexed by the NAT instance and
         pool indices for which the event is being reported.  They
         give the number of port map entries using external addresses
         configured on the pool for the most-mapped protocol and
         identify that protocol at the time the notification was
         triggered."
    REFERENCE
        "RFC 7659, Sections 3.1.2 and 3.3.6."
    ::= { natv2MIBNotifications 2 }

natv2NotificationInstanceAddressMapEntriesHigh NOTIFICATION-TYPE
    OBJECTS { natv2InstanceAddressMapEntries,
              natv2InstanceAddressMapCreations }
    STATUS current
    DESCRIPTION
        "This notification is triggered when the value of
         natv2InstanceAddressMapEntries equals or exceeds the value
         of the natv2InstanceThresholdAddressMapEntriesHigh object





         for the NAT instance, unless disabled by setting that
         threshold to -1.  Reporting is subject to the rate limitation
         given by natv2InstanceNotificationInterval.

         natv2InstanceAddressMapEntries and
         natv2InstanceAddressMapCreations are members of table
         natv2InstanceTable indexed by the identifier of the NAT
         instance for which the event is being reported.  The values
         reported are those observed at the moment the notification
         was triggered."
    REFERENCE
        "RFC 7659, Section 3.1.2."
    ::= { natv2MIBNotifications 3 }

natv2NotificationInstancePortMapEntriesHigh NOTIFICATION-TYPE
    OBJECTS { natv2InstancePortMapEntries,
              natv2InstancePortMapCreations }
    STATUS current
    DESCRIPTION
        "This notification is triggered when the value of
         natv2InstancePortMapEntries becomes greater than or equal
         to the value of natv2InstanceThresholdPortMapEntriesHigh,
         unless disabled by setting that threshold to -1.  Reporting
         is subject to the rate limitation given by
         natv2InstanceNotificationInterval.

         natv2InstancePortMapEntries and
         natv2InstancePortMapCreations are members of table
         natv2InstanceTable indexed by the identifier of the NAT
         instance for which the event is being reported.  The values
         reported are those observed at the moment the notification
         was triggered."
    ::= { natv2MIBNotifications 4 }

natv2NotificationSubscriberPortMappingEntriesHigh
NOTIFICATION-TYPE
    OBJECTS { natv2SubscriberPortMapEntries,
              natv2SubscriberPortMapCreations }
    STATUS current
    DESCRIPTION
        "This notification is triggered when the value of
         natv2SubscriberPortMapEntries for an individual subscriber
         becomes greater than or equal to the value of the
         natv2SubscriberThresholdPortMapEntriesHigh object for that
         subscriber, unless disabled by setting that threshold to -1.
         Reporting is subject to the rate limitation given by
         natv2SubscriberNotificationInterval.






         natv2SubscriberPortMapEntries and
         natv2SubscriberPortMapCreations are members of table
         natv2SubscriberTable indexed by the subscriber for
         which the event is being reported.  The values
         reported are those observed at the moment the notification
         was triggered."
    ::= { natv2MIBNotifications 5 }

-- Device-level objects

natv2MIBDeviceObjects OBJECT IDENTIFIER ::= { natv2MIB 1 }

-- Subscriber table

natv2SubscriberTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Natv2SubscriberEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Table of subscribers.  As well as the subscriber index, it
         provides per-subscriber state and counter objects, a last
         discontinuity time object for the counters, and a writable
         threshold value and limit on port consumption."
    REFERENCE
        "RFC 7659, Section 3.3.3."
    ::= { natv2MIBDeviceObjects 1 }

natv2SubscriberEntry OBJECT-TYPE
    SYNTAX Natv2SubscriberEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry describes a single subscriber."
    INDEX { natv2SubscriberIndex }
    ::= { natv2SubscriberTable 1 }

Natv2SubscriberEntry ::=
    SEQUENCE {
        natv2SubscriberIndex                  Natv2SubscriberIndex,
        natv2SubscriberInternalRealm               SnmpAdminString,
        natv2SubscriberInternalPrefixType          InetAddressType,
        natv2SubscriberInternalPrefix              InetAddress,
        natv2SubscriberInternalPrefixLength InetAddressPrefixLength,
-- State
        natv2SubscriberAddressMapEntries           Unsigned32,
        natv2SubscriberPortMapEntries              Unsigned32,







-- Counters and last discontinuity time
        natv2SubscriberTranslations                Counter64,
        natv2SubscriberAddressMapCreations         Counter64,
        natv2SubscriberPortMapCreations            Counter64,
        natv2SubscriberAddressMapFailureDrops      Counter64,
        natv2SubscriberPortMapFailureDrops         Counter64,
        natv2SubscriberDiscontinuityTime           TimeStamp,
-- Read-write controls
        natv2SubscriberLimitPortMapEntries         Unsigned32,
-- Disable notifications by setting threshold to -1
        natv2SubscriberThresholdPortMapEntriesHigh Integer32,
-- Disable limit by setting to 0
        natv2SubscriberNotificationInterval        Unsigned32
    }

natv2SubscriberIndex OBJECT-TYPE
    SYNTAX Natv2SubscriberIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "A unique value, greater than zero, for each subscriber
         in the managed system.  The value for each
         subscriber MUST remain constant at least from one
         update of the entity's natv2SubscriberDiscontinuityTime
         object until the next update of that object.  If a
         subscriber is deleted, its assigned index value MUST NOT
         be assigned to another subscriber at least until
         reinitialization of the entity's management system."
    ::= { natv2SubscriberEntry 1 }

-- Configuration for this subscriber: realm, internal address(es)

natv2SubscriberInternalRealm OBJECT-TYPE
    SYNTAX SnmpAdminString (SIZE(0..32))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The address realm to which this subscriber belongs.  A realm
         defines an address space.  All NATs support at least two
         realms.

         The default realm for subscribers is 'internal'.
         Administrators can set other values for individual
         subscribers when they are configured.  The administrator MAY
         configure a new value of natv2SubscriberRealm at any time
         subsequent to initial configuration of the subscriber.  If
         this happens, it MUST be treated as a point of discontinuity
         requiring an update of natv2SubscriberDiscontinuityTime.





         When the subscriber sends a packet to the NAT through a
         DS-Lite (RFC 6333) tunnel, this is the realm of the outer
         packet header source address.  Other tunneled access is out
         of scope."
    REFERENCE
         "Address realm: RFC 2663.  DS-Lite: RFC 6333."
    DEFVAL
        { "internal" }
    ::= { natv2SubscriberEntry 2 }

natv2SubscriberInternalPrefixType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Subscriber's internal prefix type.  Any value other than
         ipv4(1) or ipv6(2) would be unexpected.  In the case of
         DS-Lite access, this is the prefix type (IPv6(2)) used in
         the outer packet header."
    REFERENCE
        "DS-Lite: RFC 6333."
    ::= { natv2SubscriberEntry 3 }

natv2SubscriberInternalPrefix OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Prefix assigned to a subscriber's Customer Premises Equipment
         (CPE).  The type of this prefix is given by
         natv2SubscriberInternalPrefixType.  Source addresses of packets
         outgoing from the subscriber will be contained within this
         prefix.  In the case of DS-Lite access, the source address
         taken from the prefix will be that of the outer header."
    REFERENCE
        "DS-Lite: RFC 6333."
    ::= { natv2SubscriberEntry 4 }

natv2SubscriberInternalPrefixLength OBJECT-TYPE
    SYNTAX InetAddressPrefixLength
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Length of the prefix assigned to a subscriber's CPE, in
         bits.  If a single address is assigned, this will be 32
         for IPv4 and 128 for IPv6."
    ::= { natv2SubscriberEntry 5 }






-- State objects

natv2SubscriberAddressMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The current number of address map entries for the
         subscriber, including static mappings.  An address map entry
         maps from a given internal address and realm to an external
         address in a particular external realm.  This definition
         includes 'hairpin' mappings, where the external realm is the
         same as the internal one.  Address map entries are also
         tracked per instance and per address pool within the
         instance."
    REFERENCE
        "RFC 7659, Section 3.3.8."
    ::= { natv2SubscriberEntry 6 }

natv2SubscriberPortMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The current number of port map entries in the port map table
         for the subscriber, including static mappings.  A port map
         entry maps from a given external realm, address, and port
         for a given protocol to an internal realm, address, and
         port.  This definition includes 'hairpin' mappings, where the
         external realm is the same as the internal one.  Port map
         entries are also tracked per instance and per protocol and
         address pool within the instance."
    REFERENCE
        "RFC 7659, Section 3.3.9."
    ::= { natv2SubscriberEntry 7 }

-- Counters and last discontinuity time

natv2SubscriberTranslations OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of translated packets received from or
         sent to this subscriber.  This value MUST be monotone
         increasing in the periods between updates of the entity's
         natv2SubscriberDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this





         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2SubscriberDiscontinuityTime."
    ::= { natv2SubscriberEntry 8 }

natv2SubscriberAddressMapCreations OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of address map entries created for
         this subscriber, including static mappings.  Address map
         entries are also tracked per instance and per protocol and
         address pool within the instance.

         This value MUST be monotone increasing in
         the periods between updates of the entity's
         natv2SubscriberDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2SubscriberDiscontinuityTime."
    ::= { natv2SubscriberEntry 9 }

natv2SubscriberPortMapCreations OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of port map entries created for this
         subscriber, including static mappings.  Port map entries are
         also tracked per instance and per protocol and address pool
         within the instance.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2SubscriberDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2SubscriberDiscontinuityTime."
    ::= { natv2SubscriberEntry 10 }

natv2SubscriberAddressMapFailureDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current






    DESCRIPTION
        "The cumulative number of packets originated by this
         subscriber that were dropped because the packet would have
         triggered the creation of a new address map entry, but no
         address could be allocated in the selected external realm
         because all addresses from the selected address pool (or the
         whole realm, if no address pool has been configured for that
         realm) have already been fully allocated.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2SubscriberDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2SubscriberDiscontinuityTime."
    ::= { natv2SubscriberEntry 11 }

natv2SubscriberPortMapFailureDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped because the
         packet would have triggered the creation of a new
         port mapping, but no port could be allocated for the
         protocol concerned.  The usual case for this will be
         for a NAT instance that supports address pooling and
         the 'Paired' pooling behavior recommended by RFC 4787,
         where the internal endpoint has used up all of the
         ports allocated to it for the address it was mapped to
         in the selected address pool in the external realm
         concerned and cannot be given more ports because
         - policy or implementation prevents it from having a
           second address in the same pool, and
         - policy or unavailability prevents it from acquiring
           more ports at its originally assigned address.

         If the NAT instance supports address pooling but its
         pooling behavior is 'Arbitrary' (meaning that
         the NAT instance can allocate a new port mapping for
         the given internal endpoint on any address in the
         selected address pool and is not bound to what it has
         already mapped for that endpoint), then this counter
         is incremented when all ports for the protocol concerned
         over the whole of the selected address pool are already
         in use.






         As a third case, if no address pools have been configured
         for the external realm concerned, then this counter is
         incremented because all ports for the protocol involved over
         the whole set of addresses available for that external realm
         are already in use.

         Finally, this counter is incremented if the packet would
         have triggered the creation of a new port mapping, but the
         current value of natv2SubscriberPortMapEntries equals or
         exceeds the value of natv2SubscriberLimitPortMapEntries
         for this subscriber (unless that limit is disabled).

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2SubscriberDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2SubscriberDiscontinuityTime."
    REFERENCE
        "Pooling behavior: RFC 4787, end of Section 4.1."
    ::= { natv2SubscriberEntry 12 }

natv2SubscriberDiscontinuityTime OBJECT-TYPE
    SYNTAX TimeStamp
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Snapshot of the value of the sysUpTime object at the
         beginning of the latest period of continuity of the
         statistical counters associated with this subscriber."
    ::= { natv2SubscriberEntry 14 }

-- Per-subscriber limit and threshold on port mappings
-- Disabled if set to zero
natv2SubscriberLimitPortMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Limit on total number of port mappings active for this
         subscriber (natv2SubscriberPortMapEntries).  Once this limit
         is reached, packets that might have triggered new port
         mappings are dropped.  The number of such packets dropped is
         counted in natv2InstancePortMapFailureDrops.

         Limit is disabled if set to zero."






    DEFVAL
         { 0 }
    ::= { natv2SubscriberEntry 15 }

natv2SubscriberThresholdPortMapEntriesHigh OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Notification threshold for total number of port mappings
         active for this subscriber.  Whenever
         natv2SubscriberPortMapEntries is updated, if it equals or
         exceeds natv2SubscriberThresholdPortMapEntriesHigh, the
         notification
         natv2NotificationSubscriberPortMappingEntriesHigh is
         triggered, unless the notification is disabled by setting
         the threshold to -1.  Reporting is subject to the minimum
         inter-notification interval given by
         natv2SubscriberNotificationInterval.  If multiple
         notifications are triggered during one interval, the agent
         MUST report only the one containing the highest value of
         natv2SubscriberPortMapEntries and discard the others."
    DEFVAL
         { -1 }
    ::= { natv2SubscriberEntry 16 }

natv2SubscriberNotificationInterval OBJECT-TYPE
    SYNTAX Unsigned32 (1..3600)
    UNITS
        "Seconds"
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Minimum number of seconds between successive
         reporting of notifications for this subscriber.  Controls
         the reporting of
         natv2NotificationSubscriberPortMappingEntriesHigh."
    DEFVAL
         { 60 }
    ::= { natv2SubscriberEntry 17 }

-- Per-NAT-instance objects

natv2MIBInstanceObjects OBJECT IDENTIFIER ::= { natv2MIB 2 }

-- Instance table







natv2InstanceTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Natv2InstanceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Table of NAT instances.  As well as state and counter
         objects, it provides the instance index, instance name, and
         the last discontinuity time object that is applicable to
         the counters.  It also contains writable thresholds for
         reporting of notifications and limits on usage of resources
         at the level of the NAT instance.

         It is assumed that NAT instances can be created and deleted
         dynamically, but this MIB module does not provide the means
         to do so.  For restrictions on assignment and maintenance of
         the NAT index instance, see the description of
         natv2InstanceIndex in the table below.  For the requirements
         on maintenance of the values of the counters in this table,
         see the description of natv2InstanceDiscontinuityTime in
         this table.

         Each NAT instance has its own resources and behavior.  The
         resources include memory as reflected in space for map
         entries, processing power as reflected in the rate of map
         creation and deletion, and mappable addresses in each realm
         that can play the role of an external realm for at least
         some mappings for that instance.  The NAT instance table
         includes limits and notification thresholds that relate to
         memory usage for mapping at the level of the whole instance.
         The limit on number of subscribers with active mappings is a
         limit to some extent on processor usage.

         The mappable 'external' addresses may or may not be
         organized into address pools.  For a definition of address
         pools, see the description of natv2PoolTable.  If the instance
         does support address pools, it also has a pooling behavior.
         Mapping, filtering, and pooling behavior are defined in the
         descriptions of the natv2InstancePortMappingBehavior,
         natv2InstanceFilteringBehavior, and
         natv2InstancePoolingBehavior objects in this table.  The
         instance also has a fragmentation behavior, defined in the
         description of the natv2InstanceFragmentBehavior object."
    REFERENCE
        "RFC 7659, Section 3.3.4.
         NAT behaviors: RFC 4787 (primary, UDP); RFC 5382 (TCP);
         RFC 5508 (ICMP); and RFC 5597 (Datagram Congestion Control
         Protocol (DCCP))."
    ::= { natv2MIBInstanceObjects 1 }





natv2InstanceEntry OBJECT-TYPE
    SYNTAX Natv2InstanceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Objects related to a single NAT instance."
    INDEX { natv2InstanceIndex }
    ::= { natv2InstanceTable 1 }

Natv2InstanceEntry ::=
    SEQUENCE {
         natv2InstanceIndex                    Natv2InstanceIndex,
         natv2InstanceAlias                         DisplayString,
-- Configured behaviors
         natv2InstancePortMappingBehavior           INTEGER,
         natv2InstanceFilteringBehavior             INTEGER,
         natv2InstancePoolingBehavior               INTEGER,
         natv2InstanceFragmentBehavior              INTEGER,
-- State
         natv2InstanceAddressMapEntries              Unsigned32,
         natv2InstancePortMapEntries                 Unsigned32,
-- Statistics and discontinuity time
         natv2InstanceTranslations                   Counter64,
         natv2InstanceAddressMapCreations            Counter64,
         natv2InstancePortMapCreations               Counter64,
         natv2InstanceAddressMapEntryLimitDrops      Counter64,
         natv2InstancePortMapEntryLimitDrops         Counter64,
         natv2InstanceSubscriberActiveLimitDrops     Counter64,
         natv2InstanceAddressMapFailureDrops         Counter64,
         natv2InstancePortMapFailureDrops            Counter64,
         natv2InstanceFragmentDrops                  Counter64,
         natv2InstanceOtherResourceFailureDrops      Counter64,
         natv2InstanceDiscontinuityTime              TimeStamp,
-- Notification thresholds, disabled if set to -1
         natv2InstanceThresholdAddressMapEntriesHigh Integer32,
         natv2InstanceThresholdPortMapEntriesHigh    Integer32,
         natv2InstanceNotificationInterval           Unsigned32,
-- Limits, disabled if set to 0
         natv2InstanceLimitAddressMapEntries         Unsigned32,
         natv2InstanceLimitPortMapEntries            Unsigned32,
         natv2InstanceLimitPendingFragments          Unsigned32,
         natv2InstanceLimitSubscriberActives         Unsigned32
    }

natv2InstanceIndex OBJECT-TYPE
    SYNTAX Natv2InstanceIndex
    MAX-ACCESS not-accessible
    STATUS current





    DESCRIPTION
        "NAT instance index.  It is up to the implementation to
         determine which values correspond to in-service NAT
         instances.  This object is used as an index for all tables
         defined below."
    ::= { natv2InstanceEntry 1 }

natv2InstanceAlias OBJECT-TYPE
    SYNTAX DisplayString (SIZE (0..64))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "This object is an 'alias' name for the NAT instance as
         specified by a network manager and provides a non-volatile
         'handle' for the instance.

         An example of the value that a network manager might store
         in this object for a NAT instance is the name/identifier of
         the interface that brings in internal traffic for this NAT
         instance or the name of the Virtual Routing and Forwarding
         (VRF) for internal traffic."
    ::= { natv2InstanceEntry 2 }

-- Configured behaviors

natv2InstancePortMappingBehavior OBJECT-TYPE
    SYNTAX INTEGER {
           endpointIndependent (0),
           addressDependent (1),
           addressAndPortDependent (2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Port mapping behavior is the policy governing the selection
         of external address and port in a given realm for a given
         five-tuple of source address and port, destination address
         and port, and protocol.

         endpointIndependent(0), the behavior REQUIRED by RFC 4787,
         REQ-1, maps the source address and port to the same
         external address and port for all destination address and
         port combinations reached through the same external realm
         and using the given protocol.









         addressDependent(1) maps to the same external address and
         port for all destination ports at the same destination
         address reached through the same external realm and using
         the given protocol.

         addressAndPortDependent(2) maps to a separate external
         address and port combination for each different
         destination address and port combination reached through
         the same external realm."
    REFERENCE
         "RFC 4787, Section 4.1."
    ::= { natv2InstanceEntry 3 }

natv2InstanceFilteringBehavior OBJECT-TYPE
    SYNTAX INTEGER {
           endpointIndependent (0),
           addressDependent (1),
           addressAndPortDependent (2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Filtering behavior is the policy governing acceptance or
         the dropping of packets incoming from remote sources via a
         given external realm and destined to a specific three-tuple
         of external address, port, and protocol at the NAT instance
         that has been assigned in a port mapping.

         endpointIndependent(0) accepts for translation packets from
         all combinations of remote address and port destined to the
         mapped external address and port via the given external
         realm and using the given protocol.

         addressDependent(1) accepts for translation packets from all
         remote ports from the same remote source address destined to
         the mapped external address and port via the given external
         realm and using the given protocol.

         addressAndPortDependent(2) accepts for translation only
         those packets with the same remote source address, port, and
         protocol incoming from the same external realm as identified
         when the applicable port map entry was created.

         RFC 4787, REQ-8 recommends either endpointIndependent(0) or
         addressDependent(1) filtering behavior depending on whether
         application friendliness or security takes priority."
    REFERENCE
        "RFC 4787, Section 5."





    ::= { natv2InstanceEntry 4 }

natv2InstancePoolingBehavior OBJECT-TYPE
    SYNTAX INTEGER {
           arbitrary (0),
           paired (1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Pooling behavior is the policy used to select the address
         for a new port mapping within a given address pool to which
         the internal address has already been mapped.

         arbitrary(0) pooling behavior means that the NAT instance
         may create the new port mapping using any address in the
         pool that has a free port for the protocol concerned.

         paired(1) pooling behavior, the behavior RECOMMENDED by RFC
         4787, REQ-2, means that once a given internal address has
         been mapped to a particular address in a particular pool,
         further mappings of the same internal address to that pool
         will reuse the previously assigned pool member address."
    REFERENCE
        "RFC 4787, near the end of Section 4.1"
    ::= { natv2InstanceEntry 5 }

natv2InstanceFragmentBehavior OBJECT-TYPE
    SYNTAX INTEGER {
           fragmentNone (0),
           fragmentInOrder (1),
           fragmentOutOfOrder (2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Fragment behavior is the NAT instance's capability to
         receive and translate fragments incoming from remote
         sources.

         fragmentNone(0) implies no capability to translate incoming
         fragments, so all received fragments are dropped.  Each
         dropped fragment is counted in natv2InstanceFragmentDrops.

         fragmentInOrder(1) implies the ability to translate
         fragments only if they are received in order, so that in
         particular the header is in the first packet.  If a fragment






         is received out of order, it is dropped and counted in
         natv2InstanceFragmentDrops.

         fragmentOutOfOrder(2), the capability REQUIRED by RFC 4787,
         REQ-14, implies the capability to translate fragments even
         when they arrive out of order, subject to a protective
         limit natv2InstanceLimitPendingFragments on total number of
         fragments awaiting the first fragment of the chain.  If the
         implementation supports this capability,
         natv2InstanceFragmentDrops is incremented only when a new
         fragment arrives but is dropped because the limit on pending
         fragments has already been reached."
    REFERENCE
        "RFC 4787, Section 11."
    ::= { natv2InstanceEntry 6 }

-- State

natv2InstanceAddressMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The current number of address map entries in total over the
         whole NAT instance, including static mappings.  An address
         map entry maps from a given internal address and realm to an
         external address in a particular external realm.  This
         definition includes 'hairpin' mappings, where the external
         realm is the same as the internal one.  Address map entries
         are also tracked per subscriber and per address pool within
         the instance."
    REFERENCE
        "RFC 7659, Section 3.3.8.
         Hairpinning: RFC 4787, Section 6."
    ::= { natv2InstanceEntry 7 }

natv2InstancePortMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The current number of entries in the port map table in total
         over the whole NAT instance, including static mappings.  A
         port map entry maps from a given external realm, address,
         and port for a given protocol to an internal realm, address,
         and port.  This definition includes 'hairpin' mappings, where
         the external realm is the same as the internal one.  Port map






         entries are also tracked per subscriber and per protocol and
         address pool within the instance."
    REFERENCE
        "RFC 7659, Section 3.3.9.
         Hairpinning: RFC 4787, Section 6."
    ::= { natv2InstanceEntry 8 }

-- Statistics

natv2InstanceTranslations OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of translated packets passing through
         this NAT instance.  This value MUST be monotone increasing in
         the periods between updates of
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2InstanceEntry 9 }

natv2InstanceAddressMapCreations OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of address map entries created by the
         NAT instance, including static mappings.  Address map
         creations are also tracked per address pool within the
         instance and per subscriber.

         This value MUST be monotone increasing in
         the periods between updates of
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2InstanceEntry 10 }

natv2InstancePortMapCreations  OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current






    DESCRIPTION
        "The cumulative number of port map entries created by the
         NAT instance, including static mappings.  Port map
         creations are also tracked per protocol and address pool
         within the instance and per subscriber.

         This value MUST be monotone increasing in
         the periods between updates of
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2InstanceEntry 11 }

natv2InstanceAddressMapEntryLimitDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped rather than
         translated because the packet would have triggered
         the creation of a new address map entry, but the limit
         on number of address map entries for the NAT instance
         given by natv2InstanceLimitAddressMapEntries has
         already been reached.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2InstanceEntry 12 }

natv2InstancePortMapEntryLimitDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped rather than
         translated because the packet would have triggered
         the creation of a new port map entry, but the limit
         on number of port map entries for the NAT instance
         given by natv2InstanceLimitPortMapEntries has
         already been reached.






         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2InstanceEntry 13 }

natv2InstanceSubscriberActiveLimitDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped rather than
         translated because the packet would have triggered the
         creation of a new mapping for a subscriber with no other
         active mappings, but the limit on number of active
         subscribers for the NAT instance given by
         natv2InstanceLimitSubscriberActives has already been
         reached.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2InstanceEntry 14 }

natv2InstanceAddressMapFailureDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped because the packet
         would have triggered the creation of a new address map
         entry, but no address could be allocated in the selected
         external realm because all addresses from the selected
         address pool (or the whole realm, if no address pool has
         been configured for that realm) have already been fully
         allocated.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this





         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2InstanceEntry 15 }

natv2InstancePortMapFailureDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped because the
         packet would have triggered the creation of a new
         port map entry, but no port could be allocated for the
         protocol concerned.  The usual case for this will be
         for a NAT instance that supports address pooling and
         the 'Paired' pooling behavior recommended by RFC 4787,
         where the internal endpoint has used up all of the
         ports allocated to it for the address it was mapped to
         in the selected address pool in the external realm
         concerned and cannot be given more ports because
         - policy or implementation prevents it from having a
           second address in the same pool, and
         - policy or unavailability prevents it from acquiring
           more ports at its originally assigned address.

         If the NAT instance supports address pooling but its
         pooling behavior is 'Arbitrary' (meaning that
         the NAT instance can allocate a new port mapping for
         the given internal endpoint on any address in the
         selected address pool and is not bound to what it has
         already mapped for that endpoint), then this counter
         is incremented when all ports for the protocol concerned
         over the whole of the selected address pool are already
         in use.

         Finally, if no address pools have been configured for the
         external realm concerned, then this counter is incremented
         because all ports for the protocol involved over the whole
         set of addresses available for that external realm are
         already in use.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."





    REFERENCE
        "Pooling behavior: RFC 4787, end of Section 4.1."
    ::= { natv2InstanceEntry 16 }

natv2InstanceFragmentDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of fragments received by the NAT
         instance but dropped rather than translated.  When the NAT
         instance supports the 'Receive Fragment Out of Order'
         capability as required by RFC 4787, this occurs because the
         fragment was received out of order and would be added to the
         queue of fragments awaiting the initial fragment of the
         chain, but the queue has already reached the limit set by
         natv2InstanceLimitsPendingFragments.  Counting in other cases
         is specified in the description of
         natv2InstanceFragmentBehavior.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    REFERENCE
        "RFC 4787, Section 11."
    ::= { natv2InstanceEntry 17 }

natv2InstanceOtherResourceFailureDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped because of
         unavailability of a resource other than an address or port
         that would have been required to process it.  The most likely
         case is where the upper-layer protocol in the packet is not
         supported by the NAT instance.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved





         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2InstanceEntry 18 }

natv2InstanceDiscontinuityTime OBJECT-TYPE
    SYNTAX TimeStamp
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Snapshot of the value of the sysUpTime object at the
         beginning of the latest period of continuity of the
         statistical counters associated with this NAT instance."
    ::= { natv2InstanceEntry 19 }

-- Notification thresholds, disabled by setting to -1.

natv2InstanceThresholdAddressMapEntriesHigh OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Notification threshold for total number of address map
         entries held by this NAT instance.  Whenever
         natv2InstanceAddressMapEntries is updated, if it equals or
         exceeds natv2InstanceThresholdAddressMapEntriesHigh, then
         natv2NotificationInstanceAddressMapEntriesHigh may be
         triggered, unless the notification is disabled by setting
         the threshold to -1.  Reporting is subject to the minimum
         inter-notification interval given by
         natv2InstanceNotificationInterval.  If multiple notifications
         are triggered during one interval, the agent MUST report
         only the one containing the highest value of
         natv2InstanceAddressMapEntries and discard the others."
    DEFVAL
         { -1 }
    ::= { natv2InstanceEntry 20 }

natv2InstanceThresholdPortMapEntriesHigh OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Notification threshold for total number of port map
         entries held by this NAT instance.  Whenever
         natv2InstancePortMapEntries is updated, if it equals or
         exceeds natv2InstanceThresholdPortMapEntriesHigh, then
         natv2NotificationInstancePortMapEntriesHigh may be
         triggered, unless the notification is disabled by setting
         the threshold to -1.  Reporting is subject to the minimum





         inter-notification interval given by
         natv2InstanceNotificationInterval.  If multiple notifications
         are triggered during one interval, the agent MUST report
         only the one containing the highest value of
         natv2InstancePortMapEntries and discard the others."
    DEFVAL
        { -1 }
    ::= { natv2InstanceEntry 21 }

natv2InstanceNotificationInterval OBJECT-TYPE
    SYNTAX Unsigned32 (1..3600)
    UNITS
        "Seconds"
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Minimum number of seconds between successive
         notifications for this NAT instance.  Controls the reporting
         of natv2NotificationInstanceAddressMapEntriesHigh and
         natv2NotificationInstancePortMapEntriesHigh."
    DEFVAL
        { 10 }
    ::= { natv2InstanceEntry 22 }

  -- Limits, disabled if set to 0

natv2InstanceLimitAddressMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Limit on total number of address map entries supported by
         the NAT instance.  When natv2InstanceAddressMapEntries has
         reached this limit, subsequent packets that would normally
         trigger creation of a new address map entry will be dropped
         and counted in natv2InstanceAddressMapEntryLimitDrops.
         Warning of an approach to this limit can be achieved by
         setting natv2InstanceThresholdAddressMapEntriesHigh to a
         non-zero value, for example, 80% of the limit.  The limit is
         disabled by setting its value to zero.

         For further information, please see the descriptions of
         natv2NotificationInstanceAddressMapEntriesHigh and
         natv2InstanceAddressMapEntries."
    DEFVAL
        { 0 }
    ::= { natv2InstanceEntry 23 }






natv2InstanceLimitPortMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Limit on total number of port map entries supported by the
         NAT instance.  When natv2InstancePortMapEntries has reached
         this limit, subsequent packets that would normally trigger
         creation of a new port map entry will be dropped and counted
         in natv2InstancePortMapEntryLimitDrops.  Warning of an
         approach to this limit can be achieved by setting
         natv2InstanceThresholdPortMapEntriesHigh to a non-zero
         value, for example, 80% of the limit.  The limit is disabled
         by setting its value to zero.

         For further information, please see the descriptions of
         natv2NotificationInstancePortMapEntriesHigh and
         natv2InstancePortMapEntries."
    DEFVAL
        { 0 }
    ::= { natv2InstanceEntry 24 }

natv2InstanceLimitPendingFragments OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Limit on number of out-of-order fragments received by the
         NAT instance from remote sources and held until head of
         chain appears.  While the number of held fragments is at this
         limit, subsequent packets that contain fragments not
         relating to those already held will be dropped and counted
         in natv2InstancePendingFragmentLimitDrops.  The limit is
         disabled by setting the value to zero.

         Applicable only when the NAT instance supports 'Receive
         Fragments Out of Order' behavior; leave at default
         otherwise.  See the description of
         natv2InstanceFragmentBehavior."
    REFERENCE
         "RFC 4787, Section 11."
    DEFVAL { 0 }
    ::= { natv2InstanceEntry 25 }

natv2InstanceLimitSubscriberActives OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-write
    STATUS current





    DESCRIPTION
        "Limit on number of total number of active subscribers
         supported by the NAT instance.  An active subscriber is
         defined as any subscriber with at least one map entry,
         including static mappings.  While the number of active
         subscribers is at this limit, subsequent packets that would
         otherwise trigger first mappings for newly active
         subscribers will be dropped and counted in
         natv2InstanceSubscriberActiveLimitDrops.  The limit is
         disabled by setting the value to zero."
    DEFVAL { 0 }
    ::= { natv2InstanceEntry 26 }

-- Table of counters per upper-layer protocol identified by the
-- packet header and supported by the NAT instance.

natv2ProtocolTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF Natv2ProtocolEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Table of protocols with per-protocol counters.  Conceptual
         rows of the table are indexed by the combination of the NAT
         instance number and the IANA-assigned upper-layer protocol
         number as given by the ProtocolNumber Textual Convention
         (TC) and contained in the packet IP header.  It is up to the
         agent implementation to determine and operate upon only
         those upper-layer protocol numbers supported by the NAT
         instance."
    REFERENCE
        "RFC 7659, Section 3.3.5."
    ::= { natv2MIBInstanceObjects 2 }

natv2ProtocolEntry OBJECT-TYPE
    SYNTAX Natv2ProtocolEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Per-protocol counters."
    INDEX { natv2ProtocolInstanceIndex,
            natv2ProtocolNumber }
    ::= { natv2ProtocolTable 1 }

Natv2ProtocolEntry ::=
    SEQUENCE {
        natv2ProtocolInstanceIndex          Natv2InstanceIndex,
        natv2ProtocolNumber                     ProtocolNumber,






-- State
        natv2ProtocolPortMapEntries             Unsigned32,
-- Statistics.  Discontinuity object from instance table reused here.
        natv2ProtocolTranslations               Counter64,
        natv2ProtocolPortMapCreations           Counter64,
        natv2ProtocolPortMapFailureDrops        Counter64
    }

natv2ProtocolInstanceIndex OBJECT-TYPE
    SYNTAX Natv2InstanceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "NAT instance index.  It is up to the implementation to
         determine and operate upon only those values that
         correspond to in-service NAT instances."
    ::= { natv2ProtocolEntry 1 }

natv2ProtocolNumber OBJECT-TYPE
    SYNTAX ProtocolNumber
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Counters in this conceptual row apply to packets indicating
         the upper-layer protocol identified by the value of
         this object.  It is up to the implementation to determine and
         operate upon only those values that correspond to protocols
         supported by the NAT instance."
    REFERENCE
        "RFC 7659, Section 3.3.5.
         IANA Protocol Numbers,
         <http://www.iana.org/assignments/protocol-numbers>"
    ::= { natv2ProtocolEntry 2 }

 -- State
natv2ProtocolPortMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The current number of entries in the port map table in total
         over the whole NAT instance for a given protocol, including
         static mappings.  A port map entry maps from a given external
         realm, address, and port for a given protocol to an internal
         realm, address, and port.  This definition includes 'hairpin'
         mappings, where the external realm is the same as the
         internal one.  Port map entries are also tracked per
         subscriber, per instance, and per address pool within the





         instance."
    REFERENCE
        "RFC 7659, Sections 3.3.5 and 3.3.9.
         Hairpinning: RFC 4787, Section 6."
    ::= { natv2ProtocolEntry 3 }

-- Statistics
natv2ProtocolTranslations OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets translated by the NAT
         instance in either direction for the given protocol.

         This value MUST be monotone increasing in the periods
         between updates of the NAT instance
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2ProtocolEntry 4 }

natv2ProtocolPortMapCreations  OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of port map entries created by the NAT
         instance for the given protocol.

         This value MUST be monotone increasing in the periods
         between updates of the NAT instance
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    ::= { natv2ProtocolEntry 5 }

natv2ProtocolPortMapFailureDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped because the packet
         would have triggered the creation of a new port map entry,





         but no port could be allocated for the protocol concerned.
         The usual case for this will be for a NAT instance that
         supports address pooling and the 'Paired' pooling behavior
         recommended by RFC 4787, where the internal endpoint has
         used up all of the ports allocated to it for the address it
         was mapped to in the selected address pool in the external
         realm concerned and cannot be given more ports because
         - policy or implementation prevents it from having a
           second address in the same pool, and
         - policy or unavailability prevents it from acquiring
           more ports at its originally assigned address.

         If the NAT instance supports address pooling but its
         pooling behavior is 'Arbitrary' (meaning that
         the NAT instance can allocate a new port mapping for
         the given internal endpoint on any address in the
         selected address pool and is not bound to what it has
         already mapped for that endpoint), then this counter
         is incremented when all ports for the protocol concerned
         over the whole of the selected address pool are already
         in use.

         Finally, if the NAT instance has no configured address
         pooling, then this counter is incremented because all
         ports for the protocol concerned over the whole of the
         NAT instance for the external realm concerned are already
         in use.

         This value MUST be monotone increasing in the periods
         between updates of the NAT instance
         natv2InstanceDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2InstanceDiscontinuityTime."
    REFERENCE
        "RFC 4787, end of Section 4.1."
    ::= { natv2ProtocolEntry 6 }

-- pools

natv2PoolTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Natv2PoolEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
       "Table of address pools, applicable only if these are
        supported by the NAT instance.  An address pool is a set of





        addresses and ports in a particular realm, available for
        assignment to the 'external' portion of a mapping.  Where more
        than one pool has been configured for the realm, policy
        determines which subscribers and/or services are mapped to
        which pool.  natv2PoolTable provides basic information, state,
        statistics, and two notification thresholds for each pool.
        natv2PoolRangeTable is an expansion table for natv2PoolTable
        that identifies particular address ranges allocated to the
        pool."
    REFERENCE
        "RFC 7659, Section 3.3.6."
    ::= { natv2MIBInstanceObjects 3 }

natv2PoolEntry OBJECT-TYPE
    SYNTAX Natv2PoolEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Entry in the table of address pools."
    INDEX { natv2PoolInstanceIndex, natv2PoolIndex }
    ::= { natv2PoolTable 1 }

Natv2PoolEntry ::=
    SEQUENCE {
-- Index
         natv2PoolInstanceIndex                 Natv2InstanceIndex,
         natv2PoolIndex                         Natv2PoolIndex,
-- Configuration
         natv2PoolRealm                         SnmpAdminString,
         natv2PoolAddressType                   InetAddressType,
         natv2PoolMinimumPort                   InetPortNumber,
         natv2PoolMaximumPort                   InetPortNumber,
-- State
         natv2PoolAddressMapEntries             Unsigned32,
         natv2PoolPortMapEntries                Unsigned32,
-- Statistics and discontinuity time
         natv2PoolAddressMapCreations           Counter64,
         natv2PoolPortMapCreations              Counter64,
         natv2PoolAddressMapFailureDrops        Counter64,
         natv2PoolPortMapFailureDrops           Counter64,
         natv2PoolDiscontinuityTime             TimeStamp,
-- Notification thresholds and objects returned by notifications
         natv2PoolThresholdUsageLow             Integer32,
         natv2PoolThresholdUsageHigh            Integer32,
         natv2PoolNotifiedPortMapEntries        Unsigned32,
         natv2PoolNotifiedPortMapProtocol       ProtocolNumber,
         natv2PoolNotificationInterval          Unsigned32
    }





natv2PoolInstanceIndex OBJECT-TYPE
    SYNTAX Natv2InstanceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "NAT instance index.  It is up to the agent implementation
         to determine and operate upon only those values that
         correspond to in-service NAT instances."
    ::= { natv2PoolEntry 1 }

natv2PoolIndex OBJECT-TYPE
    SYNTAX Natv2PoolIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Index of an address pool that is unique for a given NAT
         instance.  It is up to the agent implementation to determine
         and operate upon only those values that correspond to
         provisioned pools."
    ::= { natv2PoolEntry 2 }

-- Configuration
natv2PoolRealm OBJECT-TYPE
    SYNTAX SnmpAdminString (SIZE (0..32))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Address realm to which this pool's addresses belong."
    REFERENCE
        "Address realms are discussed in Section 3.3.3 of
         RFC 7659.  The primary reference is RFC 2663, Section 2.1."
    ::= { natv2PoolEntry 3 }

natv2PoolAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Address type supplied by this address pool.  This will be the
         same for all pools in a given realm (by definition of an
         address realm).  Values other than ipv4(1) or ipv6(2) would
         be unexpected."
    REFERENCE
        "InetAddressType in RFC 4001."
    ::= { natv2PoolEntry 4 }

natv2PoolMinimumPort OBJECT-TYPE
    SYNTAX InetPortNumber





    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Minimum port number of the range that can be allocated in
         this pool.  Applies to all protocols supported by the NAT
         instance."
    REFERENCE
        "InetPortNumber in RFC 4001."
    ::= { natv2PoolEntry 5 }

natv2PoolMaximumPort OBJECT-TYPE
    SYNTAX InetPortNumber
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Maximum port number of the range that can be allocated in
         this pool.  Applies to all protocols supported by the NAT
         instance."
    REFERENCE
        "InetPortNumber in RFC 4001."
    ::= { natv2PoolEntry 6 }

-- State
natv2PoolAddressMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The current number of address map entries using external
         addresses drawn from this pool, including static mappings.
         This definition includes 'hairpin' mappings, where the
         external realm is the same as the internal one.  Address map
         entries are also tracked per subscriber and per instance."
    REFERENCE
        "RFC 7659, Section 3.3.8.
         Hairpinning: RFC 4787, Section 6."
    ::= { natv2PoolEntry 7 }

natv2PoolPortMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The current number of entries in the port map table using
         external addresses and ports drawn from this pool, including
         static mappings.  This definition includes 'hairpin'
         mappings, where the external realm is the same as the
         internal one.  Port map entries are also tracked per





         subscriber, per instance, and per protocol within the
         instance."
    REFERENCE
        "RFC 7659, Section 3.3.9.
         Hairpinning: RFC 4787, Section 6."
    ::= { natv2PoolEntry 8 }

-- Statistics and discontinuity time
natv2PoolAddressMapCreations OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of address map entries created in this
         pool, including static mappings.  Address map entries are
         also tracked per instance and per subscriber.

         This value MUST be monotone increasing in
         the periods between updates of the entity's
         natv2PoolDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2PoolDiscontinuityTime."
    ::= { natv2PoolEntry 9 }

natv2PoolPortMapCreations OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of port map entries created in this
         pool, including static mappings.  Port map entries are also
         tracked per instance, per protocol, and per subscriber.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2PoolDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2PoolDiscontinuityTime."
    ::= { natv2PoolEntry 10 }

natv2PoolAddressMapFailureDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current





    DESCRIPTION
        "The cumulative number of packets originated by the
         subscriber that were dropped because the packet would have
         triggered the creation of a new address map entry, but no
         address could be allocated from this address pool because
         all addresses in the pool have already been fully allocated.
         Counters of this event are also provided per instance, per
         protocol, and per subscriber.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2PoolDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this
         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2PoolDiscontinuityTime."
    ::= { natv2PoolEntry 11 }

natv2PoolPortMapFailureDrops OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cumulative number of packets dropped because the packet
         would have triggered the creation of a new port map entry,
         but no port could be allocated for the protocol concerned.
         The usual case for this will be for a NAT instance that
         supports the 'Paired' pooling behavior recommended by RFC
         4787, where the internal endpoint has used up all of the
         ports allocated to it for the address it was mapped to in
         this pool and cannot be given more ports because
         - policy or implementation prevents it from having a
           second address in the same pool, and
         - policy or unavailability prevents it from acquiring
           more ports at its originally assigned address.

         If the NAT instance pooling behavior is 'Arbitrary' (meaning
         that the NAT instance can allocate a new port mapping for
         the given internal endpoint on any address in the selected
         address pool and is not bound to what it has already mapped
         for that endpoint), then this counter is incremented when
         all ports for the protocol concerned over the whole of this
         address pool are already in use.

         This value MUST be monotone increasing in the periods
         between updates of the entity's
         natv2PoolDiscontinuityTime.  If a manager detects a
         change in the latter since the last time it sampled this





         counter, it SHOULD NOT make use of the difference between
         the latest value of the counter and any value retrieved
         before the new value of natv2PoolDiscontinuityTime."
    REFERENCE
        "Pooling behavior: RFC 4787, end of Section 4.1."
    ::= { natv2PoolEntry 12 }


natv2PoolDiscontinuityTime OBJECT-TYPE
    SYNTAX TimeStamp
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Snapshot of the value of the sysUpTime object at the
         beginning of the latest period of continuity of the
         statistical counters associated with this address
         pool.  This MUST be initialized when the address pool
         is configured and MUST be updated whenever the port
         or address ranges allocated to the pool change."
    ::= { natv2PoolEntry 13 }

-- Notification thresholds and objects returned by notifications
natv2PoolThresholdUsageLow OBJECT-TYPE
    SYNTAX Integer32 (-1|0..100)
    UNITS "Percent"
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Threshold for reporting low utilization of the address pool.
         Utilization at a given instant is calculated as the
         percentage of ports allocated in port map entries for the
         most-used protocol at that instant.  If utilization is less
         than or equal to natv2PoolThresholdUsageLow, an instance of
         natv2NotificationPoolUsageLow may be triggered, unless
         disabled by setting it to -1.  Reporting is subject to the
         per-pool notification interval given by
         natv2PoolNotificationInterval.  If multiple notifications
         are triggered during one interval, the agent MUST report
         only the one with the lowest value of
         natv2PoolNotifiedPortMapEntries and discard the others.

         Implementation note: the percentage specified by this object
         can be converted to a number of port map entries at
         configuration time (after port and address ranges have been
         configured or reconfigured) and compared to the current
         value of natv2PoolNotifiedPortMapEntries."
    REFERENCE
        "RFC 7659, Sections 3.1.2 and 3.3.6."





    DEFVAL { -1 }
    ::= { natv2PoolEntry 14 }

natv2PoolThresholdUsageHigh OBJECT-TYPE
    SYNTAX Integer32 (-1|0..100)
    UNITS "Percent"
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Threshold for reporting high utilization of the address
         pool.  Utilization at a given instant is calculated as the
         percentage of ports allocated in port map entries for the
         most-used protocol at that instant.  If utilization is
         greater than or equal to natv2PoolThresholdUsageHigh, an
         instance of natv2NotificationPoolUsageHigh may be triggered,
         unless disabled by setting it to -1.

         Reporting is subject to the per-pool notification interval
         given by natv2PoolNotificationInterval.  If multiple
         notifications are triggered during one interval, the agent
         MUST report only the one with the highest value of
         natv2PoolNotifiedPortMapEntries and discard the others.
         In the rare case where both upper and lower thresholds
         are crossed in the same interval, the agent MUST report only
         the upper-threshold notification.

         Implementation note: the percentage specified by this object
         can be converted to a number of port map entries at
         configuration time (after port and address ranges have been
         configured or reconfigured) and compared to the current
         value of natv2PoolNotifiedPortMapEntries."
    DEFVAL { -1 }
    ::= { natv2PoolEntry 15 }

natv2PoolNotifiedPortMapEntries OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS accessible-for-notify
    STATUS current
    DESCRIPTION
        "Number of port map entries using addresses and ports from
         this address pool for the most-used protocol at a given
         instant.  One of the objects returned by
         natv2NotificationPoolUsageLow and
         natv2NotificationPoolUsageHigh."
    ::= { natv2PoolEntry 16 }

natv2PoolNotifiedPortMapProtocol OBJECT-TYPE
    SYNTAX ProtocolNumber





    MAX-ACCESS accessible-for-notify
    STATUS current
    DESCRIPTION
        "The most-used protocol (i.e., with the largest number of
         port map entries) mapped into this address pool at a given
         instant.  One of the objects returned by
         natv2NotificationPoolUsageLow and
         natv2NotificationPoolUsageHigh."
    ::= { natv2PoolEntry 17 }

natv2PoolNotificationInterval OBJECT-TYPE
    SYNTAX Unsigned32 (1..3600)
    UNITS
        "Seconds"
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Minimum number of seconds between successive
         notifications for this address pool.  Controls the generation
         of natv2NotificationPoolUsageLow and
         natv2NotificationPoolUsageHigh."
    DEFVAL
        { 20 }
    ::= { natv2PoolEntry 18 }


natv2PoolRangeTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Natv2PoolRangeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains address ranges used by pool entries.
         It is an expansion of natv2PoolTable."
    REFERENCE
        "RFC 7659, Section 3.3.7."
    ::= { natv2MIBInstanceObjects 4 }

natv2PoolRangeEntry OBJECT-TYPE
    SYNTAX Natv2PoolRangeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "NAT pool address range."
    INDEX {
         natv2PoolRangeInstanceIndex,
         natv2PoolRangePoolIndex,
         natv2PoolRangeRowIndex
    }





    ::= { natv2PoolRangeTable 1 }

Natv2PoolRangeEntry ::=
    SEQUENCE {
        natv2PoolRangeInstanceIndex    Natv2InstanceIndex,
        natv2PoolRangePoolIndex        Natv2PoolIndex,
        natv2PoolRangeRowIndex         Unsigned32,
        natv2PoolRangeBegin            InetAddress,
        natv2PoolRangeEnd              InetAddress
    }

natv2PoolRangeInstanceIndex OBJECT-TYPE
    SYNTAX Natv2InstanceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Index of the NAT instance on which the address pool and this
         address range are configured.  See Natv2InstanceIndex."
    ::= { natv2PoolRangeEntry 1 }

natv2PoolRangePoolIndex OBJECT-TYPE
    SYNTAX Natv2PoolIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Index of the address pool to which this address range
         belongs.  See Natv2PoolIndex."
    ::= { natv2PoolRangeEntry 2 }

natv2PoolRangeRowIndex OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Row index for successive range entries for the same
         address pool."
    ::= { natv2PoolRangeEntry 3 }

natv2PoolRangeBegin OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Lowest address included in this range.  The type of address
         (IPv4 or IPv6) is given by natv2PoolAddressType
         in natv2PoolTable."
    ::= { natv2PoolRangeEntry 4 }






natv2PoolRangeEnd OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Highest address included in this range.  The type of address
         (IPv4 or IPv6) is given by natv2PoolAddressType
         in natv2PoolTable."
    ::= { natv2PoolRangeEntry 5 }

-- Indexed mapping tables

-- Address Map Table.  Mapped from the internal to external address.

natv2AddressMapTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Natv2AddressMapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Table of mappings from the internal to external address.  By
         definition, this is a snapshot of NAT instance state at a
         given moment.  Indexed by NAT instance, internal realm, and
         internal address in that realm.  Provides the mapped external
         address and, depending on implementation support, identifies
         the address pool from which the external address and port
         were taken and the index of the subscriber to which the
         mapping has been allocated.

         In the case of DS-Lite (RFC 6333), the indexing realm and
         address are those of the IPv6 encapsulation rather than the
         IPv4 inner packet."
    REFERENCE
        "RFC 7659, Section 3.3.8. DS-Lite: RFC 6333"
    ::= { natv2MIBInstanceObjects 5 }

natv2AddressMapEntry OBJECT-TYPE
    SYNTAX Natv2AddressMapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Mapping from internal to external address."
    INDEX { natv2AddressMapInstanceIndex,
            natv2AddressMapInternalRealm,
            natv2AddressMapInternalAddressType,
            natv2AddressMapInternalAddress,
            natv2AddressMapRowIndex }
    ::= { natv2AddressMapTable 1 }






Natv2AddressMapEntry ::=
    SEQUENCE {
        natv2AddressMapInstanceIndex       Natv2InstanceIndex,
        natv2AddressMapInternalRealm       SnmpAdminString,
        natv2AddressMapInternalAddressType  InetAddressType,
        natv2AddressMapInternalAddress      InetAddress,
        natv2AddressMapRowIndex            Unsigned32,
        natv2AddressMapInternalMappedAddressType InetAddressType,
        natv2AddressMapInternalMappedAddress     InetAddress,
        natv2AddressMapExternalRealm       SnmpAdminString,
        natv2AddressMapExternalAddressType InetAddressType,
        natv2AddressMapExternalAddress     InetAddress,
        natv2AddressMapExternalPoolIndex   Natv2PoolIndexOrZero,
        natv2AddressMapSubscriberIndex     Natv2SubscriberIndexOrZero
    }

natv2AddressMapInstanceIndex OBJECT-TYPE
    SYNTAX Natv2InstanceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Index of the NAT instance that generated this address map."
    ::= { natv2AddressMapEntry 1 }

natv2AddressMapInternalRealm OBJECT-TYPE
    SYNTAX SnmpAdminString (SIZE(0..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Realm to which the internal address belongs.  In most cases,
         this is the realm defining the address space of the packet
         being translated.  However, in the case of DS-Lite (RFC
         6333), this realm defines the IPv6 outer header address
         space.  It is the combination of that outer header and
         the inner IPv4 packet header that is remapped to the
         external address and realm.  The corresponding IPv4 realm is
         restricted in scope to the tunnel, so there is no point in
         identifying it.  The mapped IPv4 address will normally be the
         well-known value 192.0.0.2, or at least lie in the reserved
         192.0.0.0/29 range.

         If natv2AddressMapSubscriberIndex in this table is a valid
         subscriber index (i.e., greater than zero), then the value
         of natv2AddressMapInternalRealm MUST be identical to the
         value of natv2SubscriberRealm associated with that index."
    REFERENCE
        "DS-Lite: RFC 6333, Sections 5.7 (for well-known addresses)
         and 6.6 (on the need to have the IPv6 tunnel address in





         the NAT mapping tables)."
    ::= { natv2AddressMapEntry 2 }

natv2AddressMapInternalAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Address type in the header of packets on the
         interior side of this mapping.  Any value other than ipv4(1)
         or ipv6(2) would be unexpected.

         In the DS-Lite case, the address type is ipv6(2)."
    REFERENCE
        "DS-Lite: RFC 6333, Sections 5.7 (for well-known addresses)
         and 6.6 (on the need to have the IPv6 tunnel source
         address in the NAT mapping tables)."
    ::= { natv2AddressMapEntry 3 }

natv2AddressMapInternalAddress OBJECT-TYPE
    SYNTAX InetAddress (SIZE (0..16))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Source address of packets originating from the interior
         of the association provided by this mapping.  The address
         type is given by natv2AddressMapInternalAddressType.

         In the case of DS-Lite (RFC 6333), this is the IPv6 tunnel
         source address.  The mapping in this case is considered to
         be from the combination of the IPv6 tunnel source address
         natv2AddressMapInternalRealmAddress and the well-known IPv4
         inner source address natv2AddressMapInternalMappedAddress to
         the external address."
    REFERENCE
        "DS-Lite: RFC 6333, Sections 5.7 (for well-known addresses)
         and 6.6 (on the need to have the IPv6 tunnel address in
         the NAT mapping tables)."
    ::= { natv2AddressMapEntry 4 }

natv2AddressMapRowIndex OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Index of a conceptual row corresponding to a mapping of the
         given internal realm and address to a single external realm
         and address.  Multiple rows will be present because of a





         promiscuous external address selection policy, policies
         associating the same internal address with different address
         pools, or because the same internal realm-address
         combination is communicating with multiple external address
         realms."
    ::= { natv2AddressMapEntry 5 }

natv2AddressMapInternalMappedAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Internal address type actually translated by this mapping.
         Any value other than ipv4(1) or ipv6(2) would be unexpected.
         In the general case, this is the same as given by
         natv2AddressMapInternalRealmAddressType.  In the
         tunneled case, it is the address type used in the
         encapsulated packet header.  In particular, in the DS-Lite
         case, the mapped address type is ipv4(1)."
    REFERENCE
        "DS-Lite: RFC 6333."
    ::= { natv2AddressMapEntry 6 }

natv2AddressMapInternalMappedAddress OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Internal address actually translated by this mapping.  In the
         general case, this is the same as
         natv2AddressMapInternalRealmAddress.  The address type is
         given by natv2AddressMapInternalMappedAddressType.  In the
         case of DS-Lite (RFC 6333), this is the source address of
         the encapsulated IPv4 packet, normally lying in the well-known
         range 192.0.0.0/29.  The mapping in this case is considered
         to be from the combination of the IPv6 tunnel source address
         natv2AddressMapInternalRealmAddress and the well-known IPv4
         inner source address natv2AddressMapInternalMappedAddress to
         the external address."
    REFERENCE
        "DS-Lite: RFC 6333, Sections 5.7 (for well-known addresses)
         and 6.6 (on the need to have the IPv6 tunnel address in
         the NAT mapping tables)."
    ::= { natv2AddressMapEntry 7 }

natv2AddressMapExternalRealm OBJECT-TYPE
    SYNTAX SnmpAdminString (SIZE(0..32))
    MAX-ACCESS read-only





    STATUS current
    DESCRIPTION
        "External address realm to which this mapping maps the
         internal address.  This can be the same as the internal realm
         in the case of a 'hairpin' connection, but otherwise will be
         different."
    ::= { natv2AddressMapEntry 8 }

natv2AddressMapExternalAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Address type for the external realm.  Any value other than
         ipv4(1) or ipv6(2) would be unexpected."
    ::= { natv2AddressMapEntry 9 }

natv2AddressMapExternalAddress OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "External address to which the internal address is mapped.
         The address type is given by
         natv2AddressMapExternalAddressType.

         In the DS-Lite case, the mapping is from the combination of
         the internal IPv6 tunnel source address as presented in this
         table and the well-known IPv4 source address of the
         encapsulated IPv4 packet."
    REFERENCE
        "DS-Lite: RFC 6333, Sections 5.7 (for well-known addresses)
         and 6.6 (on the need to have the IPv6 tunnel address in
         the NAT mapping tables)."
    ::= { natv2AddressMapEntry 10 }

natv2AddressMapExternalPoolIndex OBJECT-TYPE
    SYNTAX Natv2PoolIndexOrZero
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Index of the address pool in the external realm from which
         the mapped external address given in
         natv2AddressMapExternalAddress was taken.  Zero if the
         implementation does not support address pools but has chosen
         to support this object or if no pool was configured for the
         given external realm."
    ::= { natv2AddressMapEntry 11 }





natv2AddressMapSubscriberIndex OBJECT-TYPE
    SYNTAX Natv2SubscriberIndexOrZero
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Index of the subscriber to which this address mapping
         applies, or zero if no subscribers are configured on
         this NAT instance."
    ::= { natv2AddressMapEntry 12 }

-- natv2PortMapTable

natv2PortMapTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Natv2PortMapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Table of port map entries indexed by the NAT instance,
         protocol, and external realm and address.  A port map entry
         associates an internal upper-layer protocol endpoint with an
         endpoint for the same protocol in the given external realm.
         By definition, this is a snapshot of NAT instance state at
         a given moment.  The table provides the basic mapping
         information.

         In the case of DS-Lite (RFC 6333), the table provides the
         internal IPv6 tunnel source address in
         natv2PortMapInternalRealmAddress and the IPv4 source address
         of the encapsulated packet that is actually translated in
         natv2PortMapInternalMappedAddress.  In the general (non-DS-
         Lite) case, those two objects will have the same value."
    REFERENCE
        "RFC 7659, Section 3.3.9.
         DS-Lite: RFC 6333, Sections 5.7
         (for well-known addresses) and 6.6 (on the need to have the
         IPv6 tunnel address in the NAT mapping tables)."
    ::= { natv2MIBInstanceObjects 6 }

natv2PortMapEntry OBJECT-TYPE
    SYNTAX Natv2PortMapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "A single NAT mapping."
    INDEX { natv2PortMapInstanceIndex,
            natv2PortMapProtocol,
            natv2PortMapExternalRealm,
            natv2PortMapExternalAddressType,





            natv2PortMapExternalAddress,
            natv2PortMapExternalPort }
    ::= { natv2PortMapTable 1 }

Natv2PortMapEntry ::=
    SEQUENCE {
        natv2PortMapInstanceIndex        Natv2InstanceIndex,
        natv2PortMapProtocol             ProtocolNumber,
        natv2PortMapExternalRealm        SnmpAdminString,
        natv2PortMapExternalAddressType  InetAddressType,
        natv2PortMapExternalAddress      InetAddress,
        natv2PortMapExternalPort         InetPortNumber,
        natv2PortMapInternalRealm        SnmpAdminString,
        natv2PortMapInternalAddressType  InetAddressType,
        natv2PortMapInternalAddress      InetAddress,
        natv2PortMapInternalMappedAddressType InetAddressType,
        natv2PortMapInternalMappedAddress     InetAddress,
        natv2PortMapInternalPort         InetPortNumber,
        natv2PortMapExternalPoolIndex    Natv2PoolIndexOrZero,
        natv2PortMapSubscriberIndex      Natv2SubscriberIndexOrZero
    }

natv2PortMapInstanceIndex OBJECT-TYPE
    SYNTAX Natv2InstanceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Index of the NAT instance that created this port map entry."
    ::= { natv2PortMapEntry 1 }

natv2PortMapProtocol OBJECT-TYPE
    SYNTAX ProtocolNumber
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The map entry's upper-layer protocol number."
    ::= { natv2PortMapEntry 2 }

natv2PortMapExternalRealm OBJECT-TYPE
    SYNTAX SnmpAdminString (SIZE(0..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The realm to which natv2PortMapExternalAddress belongs."
    ::= { natv2PortMapEntry 3 }

natv2PortMapExternalAddressType OBJECT-TYPE
    SYNTAX InetAddressType





    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Address type for the external realm.  A value other
         than ipv4(1) or ipv6(2) would be unexpected."
    ::= { natv2PortMapEntry 4 }

natv2PortMapExternalAddress OBJECT-TYPE
    SYNTAX InetAddress (SIZE (0..16))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The mapping's assigned external address.  (This address is
         taken from the address pool identified by
         natv2PortMapExternalPoolIndex, if the implementation
         supports address pools and pools are configured for the
         given external realm.)  This is the source address for
         translated outgoing packets.  The address type is given
         by natv2PortMapExternalAddressType."

    ::= { natv2PortMapEntry 5 }

natv2PortMapExternalPort OBJECT-TYPE
    SYNTAX InetPortNumber
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The mapping's assigned external port number.  This is the
         source port for translated outgoing packets.  If the internal
         port number given by natv2PortMapInternalPort is zero, this
         value MUST also be zero.  Otherwise, this MUST be a non-zero
         value."
    ::= { natv2PortMapEntry 6 }

natv2PortMapInternalRealm OBJECT-TYPE
    SYNTAX SnmpAdminString (SIZE(0..32))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The realm to which natv2PortMapInternalRealmAddress belongs.
         In the general case, this realm contains the address that is
         being translated.  In the DS-Lite (RFC 6333) case, this realm
         defines the IPv6 address space from which the tunnel source
         address is taken.  The realm of the encapsulated IPv4 address
         is restricted in scope to the tunnel, so there is no point
         in identifying it separately."
    REFERENCE
        "DS-Lite: RFC 6333."





    ::= { natv2PortMapEntry 7 }

natv2PortMapInternalAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Address type for addresses in the realm identified by
         natv2PortMapInternalRealm."
    ::= { natv2PortMapEntry 8 }

natv2PortMapInternalAddress OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Source address for packets received under this mapping on
         the internal side of the NAT instance.  In the general case,
         this address is the same as the address given in
         natv2PortMapInternalMappedAddress.  In the DS-Lite case,
         natv2PortMapInternalAddress is the IPv6 tunnel source
         address.  The address type is given
         by natv2PortMapInternalAddressType."
    REFERENCE
        "DS-Lite: RFC 6333, Sections 5.7 (for well-known addresses)
         and 6.6 (on the need to have the IPv6 tunnel address in
         the NAT mapping tables)."
    ::= { natv2PortMapEntry 9 }

natv2PortMapInternalMappedAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Internal address type actually translated by this mapping.
         Any value other than ipv4(1) or ipv6(2) would be unexpected.
         In the general case, this is the same as given by
         natv2AddressMapInternalAddressType.  In the DS-Lite
         case, the address type is ipv4(1)."
    REFERENCE
        "DS-Lite: RFC 6333."
   ::= { natv2PortMapEntry 10 }

natv2PortMapInternalMappedAddress OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION





        "Internal address actually translated by this mapping.  In the
         general case, this is the same as
         natv2PortMapInternalRealmAddress.  The address type is given
         by natv2PortMapInternalMappedAddressType.

         In the case of DS-Lite (RFC 6333), this is the source
         address of the encapsulated IPv4 packet, normally selected
         from the well-known range 192.0.0.0/29.  The mapping in this
         case is considered to be from the external address to the
         combination of the IPv6 tunnel source address
         natv2PortMapInternalRealmAddress and the well-known IPv4
         inner source address natv2PortMapInternalMappedAddress."
    REFERENCE
        "DS-Lite: RFC 6333, Sections 5.7 (for well-known addresses)
         and 6.6 (on the need to have the IPv6 tunnel address in
         the NAT mapping tables)."
    ::= { natv2PortMapEntry 11 }

natv2PortMapInternalPort OBJECT-TYPE
    SYNTAX InetPortNumber
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The mapping's internal port number.  If this is zero, ports
         are not translated (i.e., the NAT instance is a pure NAT
         rather than a Network Address and Port Translator (NAPT))."
    ::= { natv2PortMapEntry 12 }

natv2PortMapExternalPoolIndex OBJECT-TYPE
    SYNTAX Natv2PoolIndexOrZero
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Identifies the address pool from which the external address
         in this port map entry was taken.  Zero if the implementation
         does not support address pools but has chosen to support
         this object or if no pools are configured for the given
         external realm."
    ::= { natv2PortMapEntry 13 }

natv2PortMapSubscriberIndex OBJECT-TYPE
    SYNTAX Natv2SubscriberIndexOrZero
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Subscriber using this map entry.  Zero if the implementation
         does not support subscribers but has chosen to support
         this object."





    ::= { natv2PortMapEntry 14 }

-- Conformance section.  Specifies three cumulatively more extensive
-- applications: basic NAT, pooled NAT, and carrier-grade NAT.

natv2MIBConformance OBJECT IDENTIFIER ::= { natv2MIB 3 }

natv2MIBCompliances OBJECT IDENTIFIER ::= { natv2MIBConformance 1 }
natv2MIBGroups      OBJECT IDENTIFIER ::= { natv2MIBConformance 2 }

natv2MIBBasicCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
        "Describes the requirements for conformance to the basic NAT
         application of NATV2-MIB."
    MODULE  -- this module
        MANDATORY-GROUPS { natv2BasicNotificationGroup,
                           natv2BasicInstanceLevelGroup
                         }
    ::= { natv2MIBCompliances 1 }

natv2MIBPooledNATCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
        "Describes the requirements for conformance to the pooled NAT
         application of NATV2-MIB."
    MODULE  -- this module
        MANDATORY-GROUPS { natv2BasicNotificationGroup,
                           natv2BasicInstanceLevelGroup,
                           natv2PooledNotificationGroup,
                           natv2PooledInstanceLevelGroup
                         }
    ::= { natv2MIBCompliances 2 }

natv2MIBCGNCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
        "Describes the requirements for conformance to the
         carrier-grade NAT application of NATV2-MIB."
    MODULE  -- this module
        MANDATORY-GROUPS { natv2BasicNotificationGroup,
                           natv2BasicInstanceLevelGroup,
                           natv2PooledNotificationGroup,
                           natv2PooledInstanceLevelGroup,
                           natv2CGNNotificationGroup,
                           natv2CGNDeviceLevelGroup,
                           natv2CGNInstanceLevelGroup
                         }





    ::= { natv2MIBCompliances 3 }

-- Groups

natv2BasicNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
         natv2NotificationInstanceAddressMapEntriesHigh,
         natv2NotificationInstancePortMapEntriesHigh
    }
    STATUS  current
    DESCRIPTION
        "Notifications that MUST be supported by all NAT
         applications."
    ::= { natv2MIBGroups 1 }

natv2BasicInstanceLevelGroup OBJECT-GROUP
    OBJECTS {
-- from natv2InstanceTable
              natv2InstanceAlias,
              natv2InstancePortMappingBehavior,
              natv2InstanceFilteringBehavior,
              natv2InstanceFragmentBehavior,
              natv2InstanceAddressMapEntries,
              natv2InstancePortMapEntries,
              natv2InstanceTranslations,
              natv2InstanceAddressMapCreations,
              natv2InstanceAddressMapEntryLimitDrops,
              natv2InstanceAddressMapFailureDrops,
              natv2InstancePortMapCreations,
              natv2InstancePortMapEntryLimitDrops,
              natv2InstancePortMapFailureDrops,
              natv2InstanceFragmentDrops,
              natv2InstanceOtherResourceFailureDrops,
              natv2InstanceDiscontinuityTime,
              natv2InstanceThresholdAddressMapEntriesHigh,
              natv2InstanceThresholdPortMapEntriesHigh,
              natv2InstanceNotificationInterval,
              natv2InstanceLimitAddressMapEntries,
              natv2InstanceLimitPortMapEntries,
              natv2InstanceLimitPendingFragments,
-- from natv2ProtocolTable
              natv2ProtocolPortMapEntries,
              natv2ProtocolTranslations,
              natv2ProtocolPortMapCreations,
              natv2ProtocolPortMapFailureDrops,
-- from natv2AddressMapTable
              natv2AddressMapExternalRealm,
              natv2AddressMapExternalAddressType,





              natv2AddressMapExternalAddress,
-- from natv2PortMapTable
              natv2PortMapInternalRealm,
              natv2PortMapInternalAddressType,
              natv2PortMapInternalAddress,
              natv2PortMapInternalPort
            }
    STATUS current
    DESCRIPTION
        "Per-instance objects that MUST be supported by
         implementations of all NAT applications."
    ::= { natv2MIBGroups 2 }

natv2PooledNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
         natv2NotificationPoolUsageLow,
         natv2NotificationPoolUsageHigh
                  }
    STATUS  current
    DESCRIPTION
        "Notifications that MUST be supported by pooled and
         carrier-grade NAT applications."
    ::= { natv2MIBGroups 3 }

natv2PooledInstanceLevelGroup OBJECT-GROUP
    OBJECTS {
-- from natv2InstanceTable
                    natv2InstancePoolingBehavior,
-- from natv2PoolTable
                    natv2PoolRealm,
                    natv2PoolAddressType,
                    natv2PoolMinimumPort,
                    natv2PoolMaximumPort,
                    natv2PoolAddressMapEntries,
                    natv2PoolPortMapEntries,
                    natv2PoolAddressMapCreations,
                    natv2PoolPortMapCreations,
                    natv2PoolAddressMapFailureDrops,
                    natv2PoolPortMapFailureDrops,
                    natv2PoolDiscontinuityTime,
                    natv2PoolThresholdUsageLow,
                    natv2PoolThresholdUsageHigh,
                    natv2PoolNotifiedPortMapEntries,
                    natv2PoolNotifiedPortMapProtocol,
                    natv2PoolNotificationInterval,
-- from natv2PoolRangeTable
                    natv2PoolRangeBegin,
                    natv2PoolRangeEnd,





-- from natv2AddressMapTable
                    natv2AddressMapExternalPoolIndex,
-- from natv2PortMapTable
                    natv2PortMapExternalPoolIndex
            }
    STATUS current
    DESCRIPTION
        "Per-instance objects that MUST be supported by
         implementations of the pooled and carrier-grade
         NAT applications."
    ::= { natv2MIBGroups 4 }

natv2CGNNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
         natv2NotificationSubscriberPortMappingEntriesHigh
    }
    STATUS  current
    DESCRIPTION
        "Notification that MUST be supported by implementations
         of the carrier-grade NAT application."
    ::= { natv2MIBGroups 5 }

natv2CGNDeviceLevelGroup OBJECT-GROUP
    OBJECTS {
-- from table natv2SubscriberTable
              natv2SubscriberInternalRealm,
              natv2SubscriberInternalPrefixType,
              natv2SubscriberInternalPrefix,
              natv2SubscriberInternalPrefixLength,
              natv2SubscriberAddressMapEntries,
              natv2SubscriberPortMapEntries,
              natv2SubscriberTranslations,
              natv2SubscriberAddressMapCreations,
              natv2SubscriberPortMapCreations,
              natv2SubscriberAddressMapFailureDrops,
              natv2SubscriberPortMapFailureDrops,
              natv2SubscriberDiscontinuityTime,
              natv2SubscriberLimitPortMapEntries,
              natv2SubscriberThresholdPortMapEntriesHigh,
              natv2SubscriberNotificationInterval
            }
    STATUS current
    DESCRIPTION
        "Device-level objects that MUST be supported by the
         carrier-grade NAT application."
    ::= { natv2MIBGroups 6 }

natv2CGNInstanceLevelGroup OBJECT-GROUP





    OBJECTS {
   -- from natv2InstanceTable
              natv2InstanceSubscriberActiveLimitDrops,
              natv2InstanceLimitSubscriberActives,
   -- from natv2AddressMapTable
              natv2AddressMapInternalMappedAddressType,
              natv2AddressMapInternalMappedAddress,
              natv2AddressMapSubscriberIndex,
   -- from natv2PortMapTable
              natv2PortMapInternalMappedAddressType,
              natv2PortMapInternalMappedAddress,
              natv2PortMapSubscriberIndex
            }
    STATUS current
    DESCRIPTION
        "Per-instance objects that MUST be supported by the
         carrier-grade NAT application."
    ::= { natv2MIBGroups 7 }

END


