PINT-MIB DEFINITIONS ::= BEGIN


         IMPORTS
          OBJECT-TYPE, Counter32, MODULE-IDENTITY, mib-2
         FROM   SNMPv2-SMI
         TEXTUAL-CONVENTION
         FROM SNMPv2-TC
         MODULE-COMPLIANCE, OBJECT-GROUP
         FROM SNMPv2-CONF
         sysApplInstallPkgEntry
         FROM SYSAPPL-MIB
         SnmpAdminString
         FROM SNMP-FRAMEWORK-MIB;  -- RFC 2571 [2]

         pintMib MODULE-IDENTITY
         LAST-UPDATED "200102010000Z" -- 1 Feb 2001

ORGANIZATION "IETF PINT Working Group"
CONTACT-INFO "
        Chairs:  Steve Bellovin
                    E-mail: smb@research.att.com

                    Igor Faynberg
                    E-mail: faynberg@lucent.com

        Authors: Murali Krishnaswamy
                     Postal: 20 Corporate Place South
                                Piscataway, NJ 08854
                                Tel:    +1 (732)465-1000





                                E-mail: murali@photuris.com

                                Dan Romascanu
                                Postal: Atidim Technology Park, Bldg 3
                                Tel Aviv, Israel
                                Tel:    +972 3 6458414
                                E-mail: dromasca@avaya.com

        General Discussion:pint@lists.bell-labs.com
        To Subscribe: pint-request@lists.bell-labs.com
        In Body: subscribe your-email-addres
        Archive: http://www.bell-labs.com/mailing-lists/pint/
        "

DESCRIPTION
    "This MIB defines the objects necessary to monitor
     PINT Services"

-- Revision history

REVISION "200102010000Z" -- 1 Feb 2001
DESCRIPTION
    "Initial version, published as RFC 3055."
::= { mib-2 93 }

PintServiceType ::= TEXTUAL-CONVENTION
        STATUS      current
        DESCRIPTION
            "This TC describes the type of a PINT service."
        SYNTAX  INTEGER {
                r2C(1),     -- Request-to-Talk
                r2F(2),     -- Request-to-Fax
                r2FB(3),    -- Request-to-Fax-Back
                r2HC(4)     -- Request-to-Hear-Content
        }

PintPerfStatPeriod ::= TEXTUAL-CONVENTION
STATUS      current
DESCRIPTION
    "This TC describes the statistics period of time.

    Note that the values of the counters indexed with a value
    SinceReboot(4) can be potentially affected by a counter rollover.
    It is the responsibility of the application using this object to
    take into account that the counter has been zeroed each time it
    reached a value of (2**32-1)."
SYNTAX  INTEGER {
last30sec(1),   -- Performance Statics for the last 30 sec





last15min(2),   --    15 min
last24Hr(3),    --    24 Hour
sinceReboot(4)  --    Since the time the pint server was
--      last rebooted
}

pintServerConfig        OBJECT IDENTIFIER ::= { pintMib 1 }
pintServerMonitor       OBJECT IDENTIFIER ::= { pintMib 2 }
pintMibConformance      OBJECT IDENTIFIER ::= { pintMib 3 }

-- pintServerConfig - PINT configuration MIB variables

pintReleaseNumber OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
     "An indication of version of the PINT protocol supported
     by this agent."
    ::= { pintServerConfig 1 }

pintSysContact           OBJECT-TYPE
    SYNTAX        SnmpAdminString
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
     "Contact information related to the administration of the PINT
     services."
    ::= { pintServerConfig 2 }

pintApplInstallPkgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PintApplInstallPkgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Table describing the PINT applications that are installed."
    ::= { pintServerConfig 3 }

pintApplInstallPkgEntry OBJECT-TYPE
    SYNTAX      PintApplInstallPkgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Entries per PINT Application."
    AUGMENTS { sysApplInstallPkgEntry }
    ::= { pintApplInstallPkgTable 1 }

PintApplInstallPkgEntry ::= SEQUENCE {





pintApplInstallPkgDescription    SnmpAdminString
}

pintApplInstallPkgDescription OBJECT-TYPE
    SYNTAX        SnmpAdminString
    MAX-ACCESS  read-only
    STATUS        current
    DESCRIPTION
     "Textual description of the installed PINT application."
    ::= { pintApplInstallPkgEntry 1 }

pintRegisteredGatewayTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PintRegisteredGatewayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Table describing the registered gateway applications."
    ::= { pintServerConfig 4 }

pintRegisteredGatewayEntry OBJECT-TYPE
    SYNTAX      PintRegisteredGatewayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Entries per Registered Gateway Application."
AUGMENTS { sysApplInstallPkgEntry  }
    ::= { pintRegisteredGatewayTable 1 }

PintRegisteredGatewayEntry ::= SEQUENCE {
pintRegisteredGatewayName       SnmpAdminString,
pintRegisteredGatewayDescription SnmpAdminString
}

pintRegisteredGatewayName OBJECT-TYPE
    SYNTAX        SnmpAdminString
    MAX-ACCESS read-only
    STATUS        current
    DESCRIPTION
     "Name of the registered gateway."
    ::= { pintRegisteredGatewayEntry 1 }

pintRegisteredGatewayDescription OBJECT-TYPE
    SYNTAX        SnmpAdminString
    MAX-ACCESS  read-only
    STATUS        current
    DESCRIPTION
     "Textual description of the registered gateway."
    ::= { pintRegisteredGatewayEntry 2 }





-- pintServerMonitor - PINT monitoring statistics MIB variables

pintServerGlobalPerf    OBJECT IDENTIFIER ::= {pintServerMonitor 1 }
pintServerClientPerf    OBJECT IDENTIFIER ::= {pintServerMonitor 2 }
pintServerUserIdPerf    OBJECT IDENTIFIER ::= {pintServerMonitor 3 }
pintServerGatewayPerf   OBJECT IDENTIFIER ::= {pintServerMonitor 4 }

pintServerGlobalStatsTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF PintServerGlobalStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Table displaying the monitored global server statistics."
    ::= { pintServerGlobalPerf 1 }

pintServerGlobalStatsEntry OBJECT-TYPE
    SYNTAX      PintServerGlobalStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Entries in the global statistics table.
     One entry is defined for each monitored service type and
     performance statistics collection period."
    INDEX {pintServerServiceTypeIndex, pintServerPerfStatPeriodIndex}
    ::= { pintServerGlobalStatsTable 1 }

PintServerGlobalStatsEntry      ::=  SEQUENCE {
pintServerServiceTypeIndex                           PintServiceType,
pintServerPerfStatPeriodIndex                        PintPerfStatPeriod,
pintServerGlobalCallsReceived                        Counter32,
pintServerGlobalSuccessfulCalls                      Counter32,
pintServerGlobalDisconnectedCalls                    Counter32,
pintServerGlobalDisCUAutFCalls                       Counter32,
pintServerGlobalDisServProbCalls                     Counter32,
pintServerGlobalDisGatProbCalls         Counter32
}

pintServerServiceTypeIndex OBJECT-TYPE
    SYNTAX     PintServiceType
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
     "The unique identifier of the monitored service."
    ::= { pintServerGlobalStatsEntry 1 }

pintServerPerfStatPeriodIndex OBJECT-TYPE
    SYNTAX     PintPerfStatPeriod
    MAX-ACCESS not-accessible





    STATUS     current
    DESCRIPTION
     "Time period for which the performance statistics are requested
     from the pint server."
    ::= { pintServerGlobalStatsEntry 2 }

pintServerGlobalCallsReceived OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of received global calls."
    ::= { pintServerGlobalStatsEntry 3 }

pintServerGlobalSuccessfulCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of global successful calls."
    ::= { pintServerGlobalStatsEntry 4 }

pintServerGlobalDisconnectedCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of global disconnected (failed) calls."
    ::= { pintServerGlobalStatsEntry 5 }

pintServerGlobalDisCUAutFCalls
OBJECT-TYPE
SYNTAX     Counter32
MAX-ACCESS read-only
STATUS     current
DESCRIPTION
    "Number of global calls that were disconnected because of client
    or user authorization failure."
::= { pintServerGlobalStatsEntry 6 }

pintServerGlobalDisServProbCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of global calls that were disconnected because of
     server problems."
    ::= { pintServerGlobalStatsEntry 7 }





pintServerGlobalDisGatProbCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of global calls that were disconnected because of
     gateway problems."
    ::= { pintServerGlobalStatsEntry 8 }

pintServerClientStatsTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF PintServerClientStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Table displaying the monitored server client statistics."
    ::= { pintServerClientPerf 1 }

pintServerClientStatsEntry OBJECT-TYPE
    SYNTAX      PintServerClientStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Entries in the client server statistics table.
     One entry is defined for each client identified by name,
     monitored service type and performance statistics collection
     period."
    INDEX {pintServerClientAddress, pintServerServiceTypeIndex,
    pintServerPerfStatPeriodIndex}
    ::= { pintServerClientStatsTable 1 }

PintServerClientStatsEntry      ::=  SEQUENCE {
pintServerClientAddress                              SnmpAdminString,
pintServerClientCallsReceived                           Counter32,
pintServerClientSuccessfulCalls                         Counter32,
pintServerClientDisconnectedCalls                       Counter32,
pintServerClientDisCAutFCalls                           Counter32,
pintServerClientDisEFProbCalls                          Counter32
}

pintServerClientAddress OBJECT-TYPE
    SYNTAX     SnmpAdminString
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
     "The unique identifier of the monitored client
     identified by its address represented as as a string."
    ::= { pintServerClientStatsEntry 1 }






pintServerClientCallsReceived OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls received from the specific client."
    ::= { pintServerClientStatsEntry 2 }

pintServerClientSuccessfulCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls from the client successfully completed."
    ::= { pintServerClientStatsEntry 3 }

pintServerClientDisconnectedCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls received from the client, and that were
     disconnected (failed)."
    ::= { pintServerClientStatsEntry 4 }

pintServerClientDisCAutFCalls
OBJECT-TYPE
SYNTAX     Counter32
MAX-ACCESS read-only
STATUS     current
DESCRIPTION
    "Number of calls from the client that were disconnected because of
    client authorization failure."
::= { pintServerClientStatsEntry 5 }

pintServerClientDisEFProbCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls from the client that were disconnected because
     of egress facility problems."
    ::= { pintServerClientStatsEntry 6 }

pintServerUserIdStatsTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF PintServerUserIdStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current





    DESCRIPTION
     "Table displaying the monitored Pint service user statistics."
    ::= { pintServerUserIdPerf 1 }

pintServerUserIdStatsEntry OBJECT-TYPE
    SYNTAX      PintServerUserIdStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Entries in the user statistics table.
     One entry is defined for each user identified by name,
     each monitored service type and performance statistics collection
     period.

      It is assumed that the capabilities of the pint server
      are enough to accommodate the number of entries in this table.
      It is a local server implementation issue if an aging mechanism
      Is implemented in order to avoid scalability problems."
    INDEX {pintServerUserIdName, pintServerServiceTypeIndex,
    pintServerPerfStatPeriodIndex}
    ::= { pintServerUserIdStatsTable 1 }

PintServerUserIdStatsEntry      ::=  SEQUENCE {
pintServerUserIdName                                   SnmpAdminString,
pintServerUserIdCallsReceived                           Counter32,
pintServerUserIdSuccessfulCalls                         Counter32,
pintServerUserIdDisconnectedCalls                       Counter32,
pintServerUserIdDiscUIdAFailCalls                       Counter32,
pintServerUserIdEFProbCalls                             Counter32
}

pintServerUserIdName OBJECT-TYPE
    SYNTAX     SnmpAdminString (SIZE(0..64))
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
     "The unique identifier of the monitored user
     identified by its name."
    ::= { pintServerUserIdStatsEntry 1 }

pintServerUserIdCallsReceived OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls received from the specific user."
    ::= { pintServerUserIdStatsEntry 2 }






pintServerUserIdSuccessfulCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls from the user successfully completed."
    ::= { pintServerUserIdStatsEntry 3 }

pintServerUserIdDisconnectedCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls received from the user that were
     disconnected (failed)."
    ::= { pintServerUserIdStatsEntry 4 }

pintServerUserIdDiscUIdAFailCalls
OBJECT-TYPE
SYNTAX     Counter32
MAX-ACCESS read-only
STATUS     current
DESCRIPTION
    "Number of calls from the user that were disconnected because of
    user authorization failure."
::= { pintServerUserIdStatsEntry 5 }

pintServerUserIdEFProbCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls from the user that were disconnected because of
     egress facility problems."
    ::= { pintServerUserIdStatsEntry 6 }

pintServerGatewayStatsTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF PintServerGatewayStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "Table displaying the monitored gateway statistics."
    ::= { pintServerGatewayPerf 1 }

pintServerGatewayStatsEntry OBJECT-TYPE
    SYNTAX      PintServerGatewayStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current





    DESCRIPTION
     "Entries in the gateway table.
     One entry is defined for each gateway identified by name,
     each monitored service type and performance statistics collection
     period."

    INDEX { pintRegisteredGatewayName, pintServerServiceTypeIndex,
    pintServerPerfStatPeriodIndex }
    ::= { pintServerGatewayStatsTable 1 }

PintServerGatewayStatsEntry     ::=  SEQUENCE {
pintServerGatewayCallsReceived                  Counter32,
pintServerGatewaySuccessfulCalls                Counter32,
pintServerGatewayDisconnectedCalls              Counter32
}

pintServerGatewayCallsReceived OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls received at the specified gateway."
    ::= { pintServerGatewayStatsEntry 1 }

pintServerGatewaySuccessfulCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls successfully completed at the specified gateway."
    ::= { pintServerGatewayStatsEntry 2 }

pintServerGatewayDisconnectedCalls OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
     "Number of calls that were disconnected (failed) at the specified
     gateway."
    ::= { pintServerGatewayStatsEntry 3 }

--
-- Notifications Section
-- (none defined)
--

--
-- Conformance Section





--

pintMibCompliances OBJECT IDENTIFIER ::= { pintMibConformance 1 }
pintMibGroups      OBJECT IDENTIFIER ::= { pintMibConformance 2 }

pintMibCompliance MODULE-COMPLIANCE
STATUS  current
DESCRIPTION
    "Describes the requirements for conformance to the
    PINT MIB."
MODULE  -- this module
MANDATORY-GROUPS { pintMibConfigGroup, pintMibMonitorGroup }
::= { pintMibCompliances 1 }

pintMibConfigGroup OBJECT-GROUP
OBJECTS {
pintReleaseNumber,
pintSysContact,
pintApplInstallPkgDescription,
pintRegisteredGatewayName,
pintRegisteredGatewayDescription
}
STATUS  current
DESCRIPTION
    "A collection of objects providing configuration
    information
    for a PINT Server."
::= { pintMibGroups 1 }

pintMibMonitorGroup OBJECT-GROUP
OBJECTS {
pintServerGlobalCallsReceived,
pintServerGlobalSuccessfulCalls,
pintServerGlobalDisconnectedCalls,
pintServerGlobalDisCUAutFCalls,
pintServerGlobalDisServProbCalls,
pintServerGlobalDisGatProbCalls,
pintServerClientCallsReceived,
pintServerClientSuccessfulCalls,
pintServerClientDisconnectedCalls,
pintServerClientDisCAutFCalls,
pintServerClientDisEFProbCalls,
--pintServerUserIdName,
pintServerUserIdCallsReceived,
pintServerUserIdSuccessfulCalls,
pintServerUserIdDisconnectedCalls,
pintServerUserIdDiscUIdAFailCalls,
pintServerUserIdEFProbCalls,





pintServerGatewayCallsReceived,
pintServerGatewaySuccessfulCalls,
pintServerGatewayDisconnectedCalls
}
STATUS  current
DESCRIPTION
    "A collection of objects providing monitoring
    information
    for a PINT Server."
::= { pintMibGroups 2 }

END


