DOCS-IETF-CABLE-DEVICE-NOTIFICATION-MIB DEFINITIONS ::= BEGIN


     IMPORTS
           MODULE-IDENTITY,
           OBJECT-TYPE,
           NOTIFICATION-TYPE,
           mib-2
                 FROM SNMPv2-SMI -- RFC 2578
           MODULE-COMPLIANCE,





           OBJECT-GROUP,
           NOTIFICATION-GROUP
                 FROM SNMPv2-CONF -- RFC 2580

           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsDevSwFilename,
           docsDevSwServer,
           docsDevServerDhcp,
           docsDevServerTime
                 FROM DOCS-CABLE-DEVICE-MIB -- RFC 2669

           docsIfCmCmtsAddress,
           docsIfCmtsCmStatusMacAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfCmtsCmStatusModulationType
                 FROM DOCS-IF-MIB -- RFC 4546

           ifPhysAddress
                 FROM IF-MIB;  -- RFC 2863

     docsDevNotifMIB MODULE-IDENTITY

           LAST-UPDATED    "200605240000Z" -- May 24, 2006
           ORGANIZATION    "IETF IP over Cable Data Network
                            Working Group"

           CONTACT-INFO
               "        Azlina Ahmad
                Postal: Cisco Systems, Inc.
                        170 West Tasman Drive
                        San Jose, CA 95134, U.S.A.
                Phone:   408 853 7927
                E-mail: azlina@cisco.com

                        Greg Nakanishi
                Postal: Motorola
                        6450 Sequence Drive
                        San Diego, CA 92121, U.S.A.
                Phone:   858 404 2366
                E-mail: gnakanishi@motorola.com

                IETF IPCDN Working Group
                General Discussion: ipcdn@ietf.org





                Subscribe: http://www.ietf.org/mailman/listinfo/ipcdn
                Archive: ftp://ftp.ietf.org/ietf-mail-archive/ipcdn
                Co-chairs: Richard Woundy,
                             richard_woundy@cable.comcast.com
                           Jean-Francois Mule, jf.mule@cablelabs.com"

           DESCRIPTION
               "The Event Notification MIB is an extension of the
               CABLE DEVICE MIB.  It defines various notification
               objects for both cable modem and cable modem termination
               systems.  Two groups of SNMP notification objects are
               defined.  One group is for notifying cable modem events,
               and one group is for notifying cable modem termination
               system events.

               DOCSIS defines numerous events, and each event is
               assigned to a functional category.  This MIB defines
               a notification object for each functional category.
               The varbinding list of each notification includes
               information about the event that occurred on the
               device.

               Copyright (C) The Internet Society (2006).  This version
               of this MIB module is part of RFC 4547; see the RFC
               itself for full legal notices."

           REVISION "200605240000Z" -- May 24, 2006
           DESCRIPTION
               "Initial version, published as RFC 4547."
           ::= { mib-2 132 }

   docsDevNotifControl OBJECT IDENTIFIER ::= { docsDevNotifMIB 1}
   docsDevCmNotifs OBJECT IDENTIFIER ::= { docsDevNotifMIB 2 0 }
   docsDevCmtsNotifs OBJECT IDENTIFIER ::= { docsDevNotifMIB 3 0 }

   docsDevCmNotifControl OBJECT-TYPE
       SYNTAX BITS {
           cmInitTLVUnknownNotif( 0),
           cmDynServReqFailNotif( 1),
           cmDynServRspFailNotif( 2),
           cmDynServAckFailNotif( 3),
           cmBpiInitNotif( 4),
           cmBPKMNotif( 5),
           cmDynamicSANotif( 6),
           cmDHCPFailNotif( 7),
           cmSwUpgradeInitNotif( 8),
           cmSwUpgradeFailNotif( 9),
           cmSwUpgradeSuccessNotif( 10),





           cmSwUpgradeCVCNotif( 11),
           cmTODFailNotif( 12),
           cmDCCReqFailNotif( 13),
           cmDCCRspFailNotif( 14),
           cmDCCAckFailNotif( 15)
       }
      MAX-ACCESS read-write

      STATUS current
      DESCRIPTION
          "The object is used to enable specific CM notifications.
           For example, if the first bit is set, then
           docsDevCmInitTLVUnknownNotif is enabled.  If it is not set,
           the notification is disabled.  Note that notifications are
           also under the control of the MIB modules defined in
           RFC3413.

           If the device is rebooted,the value of this object SHOULD
           revert to the default value.
          "
      DEFVAL { {} }
      ::= { docsDevNotifControl 1 }

   docsDevCmtsNotifControl OBJECT-TYPE
       SYNTAX BITS {
           cmtsInitRegReqFailNotif( 0),
           cmtsInitRegRspFailNotif( 1),
           cmtsInitRegAckFailNotif( 2),
           cmtsDynServReqFailNotif( 3),
           cmtsDynServRspFailNotif( 4),
           cmtsDynServAckFailNotif( 5),
           cmtsBpiInitNotif( 6),
           cmtsBPKMNotif( 7),
           cmtsDynamicSANotif( 8),
           cmtsDCCReqFailNotif( 9),
           cmtsDCCRspFailNotif( 10),
           cmtsDCCAckFailNotif( 11)
       }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
          "The object is used to enable specific CMTS notifications.
           For example, if the first bit is set, then
           docsDevCmtsInitRegRspFailNotif is enabled.  If it is not set,
           the notification is disabled.  Note that notifications are
           also under the control of the MIB modules defined in
           RFC3413.






           If the device is rebooted,the value of this object SHOULD
           revert to the default value.
          "
       DEFVAL { {} }
       ::= { docsDevNotifControl 2 }

   docsDevCmInitTLVUnknownNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "Notification to indicate that an unknown TLV was
             encountered during the TLV parsing process.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 1 }







   docsDevCmDynServReqFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION

           "A notification to report the failure of a dynamic service
            request during the dynamic services process.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected to (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 2 }

   docsDevCmDynServRspFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,





           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           " A notification to report the failure of a dynamic service
            response during the dynamic services process.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 3}

   docsDevCmDynServAckFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION





           "A notification to report the failure of a dynamic service
            acknowledgement during the dynamic services process.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 4}

   docsDevCmBpiInitNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a BPI
            initialization attempt during the registration process.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the





              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 5 }

   docsDevCmBPKMNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a Baseline
            Privacy Key Management (BPKM) operation.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS





              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 6 }

   docsDevCmDynamicSANotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic security
            association operation.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.





            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 7 }

   docsDevCmDHCPFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsDevServerDhcp,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a DHCP operation.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsDevServerDhcp: the IP address of the DHCP server.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 8 }





   docsDevCmSwUpgradeInitNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsDevSwFilename,
           docsDevSwServer,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to indicate that a software upgrade
            has been initiated on the device.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 9 }

   docsDevCmSwUpgradeFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,





           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsDevSwFilename,
           docsDevSwServer,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a software upgrade
            attempt.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsDevSwFilename: the software image file name
            - docsDevSwServer: the IP address of the server that
              the image is retrieved from.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 10 }

   docsDevCmSwUpgradeSuccessNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,





           docsDevSwFilename,
           docsDevSwServer,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the software upgrade success
            status.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsDevSwFilename: the software image file name
            - docsDevSwServer: the IP address of the server that
              the image is retrieved from.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 11 }

   docsDevCmSwUpgradeCVCFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,





           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report that the verification of the
            code file has failed during a secure software upgrade
            attempt.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 12 }

   docsDevCmTODFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsDevServerTime,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a time of day





            operation.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsDevServerTime: the IP address of the time server.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 13 }

   docsDevCmDCCReqFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           " A notification to report the failure of a dynamic channel
            change request during the dynamic channel change process
            on the CM.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.





            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 14 }

   docsDevCmDCCRspFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic channel
            change response during the dynamic channel
            change process on the CM.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable





              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is
              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmStatusModulationType: the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 15 }

   docsDevCmDCCAckFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           ifPhysAddress,
           docsIfCmCmtsAddress,
           docsIfDocsisBaseCapability,
           docsIfCmStatusDocsisOperMode,
           docsIfCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic channel
            change acknowledgement during the dynamic channel
            change process on the CM.

            This notification sends additional information about
            the event by including the following objects in its

            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - ifPhysAddress: the MAC address of the cable
              interface of this cable modem.
            - docsIfCmCmtsAddress: the MAC address of the CMTS
              to which the CM is connected (if there is a cable
              card/interface in the CMTS, then it is actually the
              MAC address of the cable interface to which it is





              connected).
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmStatusDocsisOperMode: the QOS level (1.0, 1.1)
              that the CM is operating in.
            - docsIfCmtsCmStatusModulationType the upstream modulation
              methodology used by the CM.
           "
       ::= { docsDevCmNotifs 16}

   docsDevCmtsInitRegReqFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a registration
            request from a CM during the CM initialization
            process that was detected on the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.





            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 1 }

   docsDevCmtsInitRegRspFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a registration
            response during the CM initialization
            process that was detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 2 }

   docsDevCmtsInitRegAckFailNotif NOTIFICATION-TYPE





       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a registration
            acknowledgement from the CM during the CM
            initialization process that was detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 3 }

   docsDevCmtsDynServReqFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,





           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
        }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic service
            request during the dynamic services process
            that was detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 4 }

   docsDevCmtsDynServRspFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION





           "A notification to report the failure of a dynamic service
            response during the dynamic services process
            that was detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 5 }

   docsDevCmtsDynServAckFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic service
            acknowledgement during the dynamic services
            process that was detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its





            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 6 }


   docsDevCmtsBpiInitNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a BPI
            initialization attempt during the CM registration process
            that was detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.





            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 7 }

   docsDevCmtsBPKMNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a BPKM operation
            that is detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface





              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 8 }

   docsDevCmtsDynamicSANotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic security
            association operation that is detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.

            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.





            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 9 }

   docsDevCmtsDCCReqFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic channel
            change request during the dynamic channel
            change process and is detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 10 }

   docsDevCmtsDCCRspFailNotif NOTIFICATION-TYPE





       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,
           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic channel
            change response during the dynamic channel
            change process and is detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.

            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 11 }

   docsDevCmtsDCCAckFailNotif NOTIFICATION-TYPE
       OBJECTS {
           docsDevEvLevel,
           docsDevEvId,
           docsDevEvText,
           docsIfCmtsCmStatusMacAddress,





           ifPhysAddress,
           docsIfCmtsCmStatusDocsisRegMode,
           docsIfDocsisBaseCapability,
           docsIfCmtsCmStatusModulationType
       }
       STATUS current
       DESCRIPTION
           "A notification to report the failure of a dynamic channel
            change acknowledgement during the dynamic channel
            change process and is detected by the CMTS.

            This notification sends additional information about
            the event by including the following objects in its
            varbinding list.
            - docsDevEvLevel: the priority level associated with the
              event.
            - docsDevEvId: the unique identifier of the event that
              occurred.
            - docsDevEvText: a textual description of the event.
            - docsIfCmtsCmStatusMacAddress: the MAC address of the CM
              with which this notification is associated.
            - ifPhysAddress: the MAC address of the CMTS
              (if there is a cable card/interface in the CMTS,
              then it is actually the MAC address of the cable
              interface that connected to the CM) cable interface
              connected to the CM.
            - docsIfCmtsCmStatusDocsisRegMode: the QOS level (1.0, 1.1)
              that the reporting CM is operating in.
            - docsIfDocsisBaseCapability: the highest
              version of the DOCSIS specification (1.0, 1.1, 2.0)
              that the device is capable of supporting.
            - docsIfCmtsCmStatusModulationType: the upstream
              modulation methodology used by the CM.
           "
       ::= { docsDevCmtsNotifs 12}

   --
   --Conformance definitions
   --

   docsDevNotifConformance OBJECT IDENTIFIER
      ::= { docsDevNotifMIB 4 }
   docsDevNotifGroups OBJECT IDENTIFIER
      ::= { docsDevNotifConformance 1 }
   docsDevNotifCompliances OBJECT IDENTIFIER
      ::= { docsDevNotifConformance 2 }
   docsDevCmNotifCompliance MODULE-COMPLIANCE
       STATUS current





       DESCRIPTION
       "The compliance statement for CM Notifications and Control."

       MODULE --docsDevNotif
         MANDATORY-GROUPS {
                  docsDevCmNotifControlGroup,
                  docsDevCmNotificationGroup
              }
       ::= { docsDevNotifCompliances 1 }

   docsDevCmNotifControlGroup OBJECT-GROUP
       OBJECTS {
           docsDevCmNotifControl
       }
       STATUS current
       DESCRIPTION
           "This group represents objects that allow control
            over CM Notifications."
       ::= { docsDevNotifGroups 1 }

   docsDevCmNotificationGroup NOTIFICATION-GROUP
       NOTIFICATIONS {
           docsDevCmInitTLVUnknownNotif,
           docsDevCmDynServReqFailNotif,
           docsDevCmDynServRspFailNotif,
           docsDevCmDynServAckFailNotif,
           docsDevCmBpiInitNotif,
           docsDevCmBPKMNotif,
           docsDevCmDynamicSANotif,
           docsDevCmDHCPFailNotif,
           docsDevCmSwUpgradeInitNotif,
           docsDevCmSwUpgradeFailNotif,
           docsDevCmSwUpgradeSuccessNotif,
           docsDevCmSwUpgradeCVCFailNotif,
           docsDevCmTODFailNotif,
           docsDevCmDCCReqFailNotif,
           docsDevCmDCCRspFailNotif,
           docsDevCmDCCAckFailNotif
       }
       STATUS current
       DESCRIPTION
           "A collection of CM notifications providing device status
      and control."
       ::= { docsDevNotifGroups 2 }

   docsDevCmtsNotifCompliance MODULE-COMPLIANCE
       STATUS current
       DESCRIPTION





           "The compliance statement for DOCSIS CMTS Notification
            and Control."
       MODULE --docsDevNotif
          MANDATORY-GROUPS {
             docsDevCmtsNotifControlGroup,
             docsDevCmtsNotificationGroup
          }
       ::= { docsDevNotifCompliances 2 }

   docsDevCmtsNotifControlGroup OBJECT-GROUP
       OBJECTS {
           docsDevCmtsNotifControl
       }
       STATUS current
       DESCRIPTION
           "This group represents objects that allow control
            over CMTS Notifications."
       ::= { docsDevNotifGroups 3 }

   docsDevCmtsNotificationGroup NOTIFICATION-GROUP
       NOTIFICATIONS {
           docsDevCmtsInitRegReqFailNotif,
           docsDevCmtsInitRegRspFailNotif,
           docsDevCmtsInitRegAckFailNotif ,
           docsDevCmtsDynServReqFailNotif,
           docsDevCmtsDynServRspFailNotif,
           docsDevCmtsDynServAckFailNotif,
           docsDevCmtsBpiInitNotif,
           docsDevCmtsBPKMNotif,
           docsDevCmtsDynamicSANotif,
           docsDevCmtsDCCReqFailNotif,
           docsDevCmtsDCCRspFailNotif,
           docsDevCmtsDCCAckFailNotif
       }
       STATUS current
       DESCRIPTION
           "A collection of CMTS notifications providing device
            status and control."
       ::= { docsDevNotifGroups 4 }

   END


