SNMPv2-M2M-MIB DEFINITIONS ::= BEGIN


          IMPORTS
              MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
              Integer32, Counter32, snmpModules
                  FROM SNMPv2-SMI
              DisplayString, InstancePointer, RowStatus, TimeStamp
                  FROM SNMPv2-TC
              MODULE-COMPLIANCE, OBJECT-GROUP
                  FROM SNMPv2-CONF
              contextIdentity
                  FROM SNMPv2-PARTY-MIB;


          snmpM2M MODULE-IDENTITY
              LAST-UPDATED "9304010000Z"
              ORGANIZATION "IETF SNMPv2 Working Group"
              CONTACT-INFO
                      "        Steven Waldbusser

                       Postal: Carnegie Mellon University
                               4910 Forbes Ave
                               Pittsburgh, PA  15213

                          Tel: +1 412 268 6628
                          Fax: +1 412 268 4987

                       E-mail: waldbusser@cmu.edu"
              DESCRIPTION
                      "The Manager-to-Manager MIB module."
              ::= { snmpModules 2 }


          snmpM2MObjects OBJECT IDENTIFIER ::= { snmpM2M 1 }














          RFC 1451            Manager-to-Manager MIB          April 1993


          -- the alarm group
          --
          -- a collection of objects allowing the description and
          -- configuration of threshold alarms from a SNMPv2 entity
          -- acting in a dual role.

          snmpAlarm      OBJECT IDENTIFIER ::= { snmpM2MObjects 1 }

          -- This Alarm mechanism periodically takes statistical samples
          -- from variables available via SNMPv2 and compares them to
          -- thresholds that have been configured.  The alarm table
          -- stores configuration entries that each define a variable,
          -- polling period, and threshold parameters.  If a sample is
          -- found to cross the threshold values, an event is generated.
          -- Only variables that resolve to an ASN.1 primitive type of
          -- INTEGER (Integer32, Counter32, Gauge32, TimeTicks,
          -- Counter64, or UInteger32) may be monitored in this way.
          --
          -- This function has a hysteresis mechanism to limit the
          -- generation of events.  This mechanism generates one event
          -- as a threshold is crossed in the appropriate direction.  No
          -- more events are generated for that threshold until the
          -- opposite threshold is crossed.
          --
          -- In the case of sampling a deltaValue, an entity may
          -- implement this mechanism with more precision if it takes a
          -- delta sample twice per period, each time comparing the sum
          -- of the latest two samples to the threshold.  This allows
          -- the detection of threshold crossings that span the sampling
          -- boundary.  Note that this does not require any special
          -- configuration of the threshold value.  It is suggested that
          -- entities implement this more precise algorithm.
          --

















          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmNextIndex OBJECT-TYPE
              SYNTAX     INTEGER (0..65535)
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The index number of the next appropriate
                      unassigned entry in the snmpAlarmTable.  The value
                      0 indicates that no unassigned entries are
                      available.

                      A management station should create new entries in
                      the snmpAlarmTable using this algorithm: first,
                      issue a management protocol retrieval operation to
                      determine the value of snmpAlarmNextIndex; and,
                      second, issue a management protocol set operation
                      to create an instance of the snmpAlarmStatus
                      object setting its value to `createAndGo' or
                      `createAndWait' (as specified in the description
                      of the RowStatus textual convention)."
              ::= { snmpAlarm 1 }

          snmpAlarmTable OBJECT-TYPE
              SYNTAX     SEQUENCE OF SnmpAlarmEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "A list of snmpAlarm entries."
              ::= { snmpAlarm 2 }

          snmpAlarmEntry OBJECT-TYPE
              SYNTAX     SnmpAlarmEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "A list of parameters that set up a periodic
                      sampling query to check for alarm conditions.  The
                      contextIdentity included in the INDEX clause is
                      the context to which the sampling queries are
                      directed."
              INDEX      { contextIdentity, snmpAlarmIndex }
              ::= { snmpAlarmTable 1 }









          RFC 1451            Manager-to-Manager MIB          April 1993


          SnmpAlarmEntry ::= SEQUENCE {
              snmpAlarmIndex                    INTEGER,
              snmpAlarmVariable                 InstancePointer,
              snmpAlarmInterval                 Integer32,
              snmpAlarmSampleType               INTEGER,
              snmpAlarmValue                    Integer32,
              snmpAlarmStartupAlarm             INTEGER,
              snmpAlarmRisingThreshold          Integer32,
              snmpAlarmFallingThreshold         Integer32,
              snmpAlarmRisingEventIndex         INTEGER,
              snmpAlarmFallingEventIndex        INTEGER,
              snmpAlarmUnavailableEventIndex    INTEGER,
              snmpAlarmStatus                   RowStatus
          }

          snmpAlarmIndex OBJECT-TYPE
              SYNTAX     INTEGER (1..65535)
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "An index that uniquely identifies an entry in the
                      snmpAlarm table for a particular sampling context.
                      Each such entry defines a diagnostic sample at a
                      particular interval for a variable in the
                      particular context's object resources."
              ::= { snmpAlarmEntry 1 }
























          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmVariable OBJECT-TYPE
              SYNTAX     InstancePointer
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The object identifier of the particular variable
                      to be sampled.  Only variables that resolve to an
                      ASN.1 primitive type of INTEGER (Integer32,
                      Counter32, Gauge32, TimeTicks, Counter64, or
                      UInteger32) may be sampled.

                      If it is detected by an error response of
                      authorizationError, noSuchObject, or
                      noSuchInstance that the variable name of an
                      established snmpAlarmEntry is no longer available
                      in the sampling context, a single
                      snmpObjectUnavailableAlarm event is generated and
                      the status of this snmpAlarmEntry is set to
                      `destroy'.  Likewise, if the syntax of the
                      variable retrieved by the query is not Integer32,
                      Counter32, Gauge32, TimeTicks, Counter64, or
                      UInteger32, the same actions will be taken.

                      If the SNMPv2 entity acting in a dual role detects
                      that the sampled value can not be obtained due to
                      lack of response to management queries, it should
                      either:

                           1) Set the status of this snmpAlarmEntry to
                           `destroy', if it is determined that further
                           communication is not possible;

                           or,

                           2) Delete the associated snmpAlarmValue
                           instance (but not the entire conceptual row),
                           and continue to attempt to sample the
                           variable and recreate the associated
                           snmpAlarmValue instance should communication
                           be reestablished.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."





          RFC 1451            Manager-to-Manager MIB          April 1993


              ::= { snmpAlarmEntry 2 }

          snmpAlarmInterval OBJECT-TYPE
              SYNTAX     Integer32
              UNITS      "seconds"
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The interval in seconds over which the data is
                      sampled and compared with the rising and falling
                      thresholds.  When setting this object and the
                      sampling type is `deltaValue',  care should be
                      taken to ensure that the change during this
                      interval of the variable being sampled will not
                      exceed the (-2^31...2^31-1) range of the
                      snmpAlarmValue.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."
              ::= { snmpAlarmEntry 3 }




























          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmSampleType OBJECT-TYPE
              SYNTAX     INTEGER {
                             absoluteValue(1),
                             deltaValue(2)
                         }
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The method of sampling the selected variable and
                      calculating the value to be compared against the
                      thresholds.  If the value of this object is
                      `absoluteValue', the value of the selected
                      variable at the end of the sampling interval will
                      be compared directly with both the
                      snmpAlarmRisingThreshold and the
                      snmpAlarmFallingThreshold values.  If the value of
                      this object is `deltaValue', the value of the
                      selected variable at the end of the sampling
                      interval will be subtracted from its value at the
                      end of the previous sampling interval, and the
                      difference compared with both the
                      snmpAlarmRisingThreshold and the
                      snmpAlarmFallingThreshold values.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."
              DEFVAL { deltaValue }
              ::= { snmpAlarmEntry 4 }




















          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmValue OBJECT-TYPE
              SYNTAX     Integer32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The value of the statistic during the last
                      sampling period.  The value during the current
                      sampling period is not made available until the
                      period is completed.  If the value of the
                      statistic does not fit in the signed 32 bit
                      representation of this object, it should be
                      truncated in an implementation specific manner.

                      Note that if the associated snmpAlarmSampleType is
                      set to `deltaValue', the value of this object is
                      the difference in the sampled variable since the
                      last sample.

                      This object will be created by the SNMPv2 entity
                      acting in a dual role when this entry is set to
                      `active', and the first sampling period has
                      completed.  It may be created and deleted at other
                      times by the SNMPv2 entity acting in a dual role
                      when the sampled value can not be obtained, as
                      specified in the snmpAlarmVariable object."
              ::= { snmpAlarmEntry 5 }
























          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmStartupAlarm OBJECT-TYPE
              SYNTAX     INTEGER {
                             risingAlarm(1),
                             fallingAlarm(2),
                             risingOrFallingAlarm(3)
                         }
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The alarm that may be sent when this entry is
                      first set to `active'.  If the first sample after
                      this entry becomes active is greater than or equal
                      to the risingThreshold and snmpAlarmStartupAlarm
                      is equal to `risingAlarm' or
                      `risingOrFallingAlarm', then a single rising alarm
                      will be generated.  If the first sample after this
                      entry becomes active is less than or equal to the
                      fallingThreshold and snmpAlarmStartupAlarm is
                      equal to `fallingAlarm' or `risingOrFallingAlarm',
                      then a single falling alarm will be generated.
                      Note that a snmpObjectUnavailableAlarm is sent
                      upon startup whenever it is applicable,
                      independent of the setting of
                      snmpAlarmStartupAlarm.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."
              DEFVAL { risingOrFallingAlarm }
              ::= { snmpAlarmEntry 6 }



















          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmRisingThreshold OBJECT-TYPE
              SYNTAX     Integer32
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "A threshold for the sampled statistic.  When the
                      current sampled value is greater than or equal to
                      this threshold, and the value at the last sampling
                      interval was less than this threshold, a single
                      event will be generated.  A single event will also
                      be generated if the first sample after this entry
                      becomes active is greater than or equal to this
                      threshold and the associated snmpAlarmStartupAlarm
                      is equal to `risingAlarm' or
                      `risingOrFallingAlarm'.

                      After a rising event is generated, another such
                      event will not be generated until the sampled
                      value falls below this threshold and reaches the
                      snmpAlarmFallingThreshold.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."
              ::= { snmpAlarmEntry 7 }
























          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmFallingThreshold OBJECT-TYPE
              SYNTAX     Integer32
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "A threshold for the sampled statistic.  When the
                      current sampled value is less than or equal to
                      this threshold, and the value at the last sampling
                      interval was greater than this threshold, a single
                      event will be generated.  A single event will also
                      be generated if the first sample after this entry
                      becomes active is less than or equal to this
                      threshold and the associated snmpAlarmStartupAlarm
                      is equal to `fallingAlarm' or
                      `risingOrFallingAlarm'.

                      After a falling event is generated, another such
                      event will not be generated until the sampled
                      value rises above this threshold and reaches the
                      snmpAlarmRisingThreshold.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."
              ::= { snmpAlarmEntry 8 }
























          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmRisingEventIndex OBJECT-TYPE
              SYNTAX     INTEGER (0..65535)
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The index of the snmpEventEntry that is used when
                      a rising threshold is crossed.  The snmpEventEntry
                      identified by a particular value of this index is
                      the same as identified by the same value of the
                      snmpEventIndex object.  If there is no
                      corresponding entry in the snmpEventTable, then no
                      association exists.  In particular, if this value
                      is zero, no associated event will be generated, as
                      zero is not a valid snmpEventIndex.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."
              ::= { snmpAlarmEntry 9 }






























          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmFallingEventIndex OBJECT-TYPE
              SYNTAX     INTEGER (0..65535)
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The index of the snmpEventEntry that is used when
                      a falling threshold is crossed.  The
                      snmpEventEntry identified by a particular value of
                      this index is the same as identified by the same
                      value of the snmpEventIndex object.  If there is
                      no corresponding entry in the snmpEventTable, then
                      no association exists.  In particular, if this
                      value is zero, no associated event will be
                      generated, as zero is not a valid snmpEventIndex.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."
              ::= { snmpAlarmEntry 10 }

          snmpAlarmUnavailableEventIndex OBJECT-TYPE
              SYNTAX     INTEGER (0..65535)
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The index of the snmpEventEntry that is used when
                      a variable becomes unavailable.  The
                      snmpEventEntry identified by a particular value of
                      this index is the same as identified by the same
                      value of the snmpEventIndex object.  If there is
                      no corresponding entry in the snmpEventTable, then
                      no association exists.  In particular, if this
                      value is zero, no associated event will be
                      generated, as zero is not a valid snmpEventIndex.

                      An attempt to modify this object will fail with an
                      `inconsistentValue' error if the associated
                      snmpAlarmStatus object would be equal to `active'
                      both before and after the modification attempt."
              ::= { snmpAlarmEntry 11 }









          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpAlarmStatus OBJECT-TYPE
              SYNTAX     RowStatus
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The status of this snmpAlarm entry.  This object
                      may not be set to `active' unless the following
                      columnar objects exist in this row:
                      snmpAlarmVariable, snmpAlarmInterval,
                      snmpAlarmSampleType, snmpAlarmStartupAlarm,
                      snmpAlarmRisingThreshold,
                      snmpAlarmFallingThreshold,
                      snmpAlarmRisingEventIndex,
                      snmpAlarmFallingEventIndex, and
                      snmpAlarmUnavailableEventIndex."
              ::= { snmpAlarmEntry 12 }


































          RFC 1451            Manager-to-Manager MIB          April 1993


          -- alarm-related notifications

          snmpAlarmNotifications
                         OBJECT IDENTIFIER ::= { snmpAlarm 3 }

          snmpRisingAlarm NOTIFICATION-TYPE
              OBJECTS { snmpAlarmVariable, snmpAlarmSampleType,
                        snmpAlarmValue, snmpAlarmRisingThreshold }
              STATUS  current
              DESCRIPTION
                      "An event that is generated when an alarm entry
                      crosses its rising threshold.  The instances of
                      those objects contained within the varbind list
                      are those of the alarm entry which generated this
                      event."
              ::= { snmpAlarmNotifications 1 }

          snmpFallingAlarm NOTIFICATION-TYPE
              OBJECTS { snmpAlarmVariable, snmpAlarmSampleType,
                        snmpAlarmValue, snmpAlarmFallingThreshold }
              STATUS  current
              DESCRIPTION
                      "An event that is generated when an alarm entry
                      crosses its falling threshold.  The instances of
                      those objects contained within the varbind list
                      are those of the alarm entry which generated this
                      event."
              ::= { snmpAlarmNotifications 2 }

          snmpObjectUnavailableAlarm NOTIFICATION-TYPE
              OBJECTS { snmpAlarmVariable }
              STATUS  current
              DESCRIPTION
                      "An event that is generated when a variable
                      monitored by an alarm entry becomes unavailable.
                      The instance of snmpAlarmVariable contained within
                      the varbind list is the one associated with the
                      alarm entry which generated this event."
              ::= { snmpAlarmNotifications 3 }











          RFC 1451            Manager-to-Manager MIB          April 1993


          -- the event group
          --
          -- a collection of objects allowing the description and
          -- configuration of events from a SNMPv2 entity acting
          -- in a dual role.

          snmpEvent      OBJECT IDENTIFIER ::= { snmpM2MObjects 2 }

          -- The snmpEvent table defines the set of events generated on
          -- a SNMPv2 entity acting in a dual role.  Each entry in the
          -- snmpEventTable associates an event type with the
          -- notification method and associated parameters.  Some
          -- snmpEvent entries are fired by an associated condition in
          -- the snmpAlarmTable.  Others are fired on behalf of
          -- conditions defined in the NOTIFICATION-TYPE macro.  The
          -- snmpNotificationTable defines notifications that should
          -- occur when an associated event is fired.

          snmpEventNextIndex OBJECT-TYPE
              SYNTAX     INTEGER (0..65535)
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The index number of the next appropriate
                      unassigned entry in the snmpEventTable.  The value
                      0 indicates that no unassigned entries are
                      available.

                      A management station should create new entries in
                      the snmpEventTable using this algorithm: first,
                      issue a management protocol retrieval operation to
                      determine the value of snmpEventNextIndex; and,
                      second, issue a management protocol set operation
                      to create an instance of the snmpEventStatus
                      object setting its value to `createAndWait' or
                      'createAndGo'."
              ::= { snmpEvent 1 }













          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpEventTable OBJECT-TYPE
              SYNTAX     SEQUENCE OF SnmpEventEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "A list of events."
              ::= { snmpEvent 2 }

          snmpEventEntry OBJECT-TYPE
              SYNTAX     SnmpEventEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "A set of parameters that describe an event that
                      is generated when certain conditions are met."
              INDEX      { snmpEventIndex }
              ::= { snmpEventTable 1 }

          SnmpEventEntry ::= SEQUENCE {
              snmpEventIndex          INTEGER,
              snmpEventID             OBJECT IDENTIFIER,
              snmpEventDescription    DisplayString,
              snmpEventEvents         Counter32,
              snmpEventLastTimeSent   TimeStamp,
              snmpEventStatus         RowStatus
          }

          snmpEventIndex OBJECT-TYPE
              SYNTAX     INTEGER (1..65535)
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "An index that uniquely identifies an entry in the
                      snmpEvent table.  Each such entry defines an event
                      generated when the appropriate conditions occur."
              ::= { snmpEventEntry 1 }














          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpEventID OBJECT-TYPE
              SYNTAX     OBJECT IDENTIFIER
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The authoritative identification of the event
                      type generated by this entry.  This variable
                      occurs as the second varbind of an InformRequest-
                      PDU.  If this OBJECT IDENTIFIER maps to a
                      NOTIFICATION-TYPE the sender will place the
                      objects listed in the NOTIFICATION-TYPE in the
                      varbind list."
              ::= { snmpEventEntry 2 }

          snmpEventDescription OBJECT-TYPE
              SYNTAX     DisplayString (SIZE (0..127))
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "A comment describing this snmpEvent entry."
              ::= { snmpEventEntry 3 }

          snmpEventEvents OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The number of events caused by event generators
                      associated with this snmpEvent entry."
              ::= { snmpEventEntry 4 }




















          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpEventLastTimeSent OBJECT-TYPE
              SYNTAX     TimeStamp
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The value of sysUpTime at the time this snmpEvent
                      entry last generated an event.  If this entry has
                      not generated any events, this value will be
                      zero."
              DEFVAL { 0 }
              ::= { snmpEventEntry 5 }

          snmpEventStatus OBJECT-TYPE
              SYNTAX     RowStatus
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The status of this snmpEvent entry.  This object
                      may not be set to `active' unless the following
                      columnar objects exist in this row: snmpEventID,
                      snmpEventDescription, snmpEventEvents, and
                      snmpEventLastTimeSent.

                      Setting an instance of this object to the value
                      'destroy' has the effect of invalidating any/all
                      entries in the snmpEventTable, and the
                      snmpEventNotifyTable which reference the
                      corresponding snmpEventEntry."
              ::= { snmpEventEntry 6 }





















          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpEventNotifyMinInterval OBJECT-TYPE
              SYNTAX     Integer32
              UNITS      "seconds"
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The minimum interval that the SNMPv2 entity
                      acting in a dual role will wait before
                      retransmitting an InformRequest-PDU.  This object
                      specifies the minimal value supported by the
                      SNMPv2 entity acting in a dual role, based on
                      resource or implementation constraints.

                      For a particular entry in the
                      snmpEventNotifyTable, if the associated
                      snmpEventNotifyIntervalRequested variable is
                      greater than this object, the
                      snmpEventNotifyIntervalRequested value shall be
                      used as the minimum interval for retransmissions
                      of InformRequest-PDUs sent on behalf of that
                      entry."
              ::= { snmpEvent 3 }

          snmpEventNotifyMaxRetransmissions OBJECT-TYPE
              SYNTAX     Integer32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The maximum number of time that the SNMPv2 entity
                      acting in a dual role will retransmit an
                      InformRequest-PDU.  This object specifies the
                      maximal value supported by the SNMPv2 entity
                      acting in a dual role, based on resource or
                      implementation constraints.

                      For a particular entry in the
                      snmpEventNotifyTable, if the associated
                      snmpEventNotifyRetransmissionsRequested variable
                      is less than this object, the
                      snmpEventNotifyRetransmissionsRequested value
                      shall be used as the retransmission count for
                      InformRequest-PDUs sent on behalf of that entry."
              ::= { snmpEvent 4 }

          -- The snmpEventNotifyTable is used to configure the





          RFC 1451            Manager-to-Manager MIB          April 1993


          -- destination and type of notifications sent by a SNMPv2
          -- entity acting in a manager role when a particular event
          -- is triggered.

          snmpEventNotifyTable OBJECT-TYPE
              SYNTAX     SEQUENCE OF SnmpEventNotifyEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "A list of protocol configuration entries for
                      event notifications from this entity."
              ::= { snmpEvent 5 }

          snmpEventNotifyEntry OBJECT-TYPE
              SYNTAX     SnmpEventNotifyEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "A set of parameters that describe the type and
                      destination of InformRequest-PDUs sent for a
                      particular event.  The snmpEventIndex in this
                      entry's INDEX clause identifies the snmpEventEntry
                      which, when triggered, will generate a
                      notification as configured in this entry.  The
                      contextIdentity in this entry's INDEX clause
                      identifies the context to which a notification
                      will be sent."
              INDEX      { snmpEventIndex, contextIdentity }
              ::= { snmpEventNotifyTable 1 }

          SnmpEventNotifyEntry ::= SEQUENCE {
              snmpEventNotifyIntervalRequested        Integer32,
              snmpEventNotifyRetransmissionsRequested Integer32,
              snmpEventNotifyLifetime                 Integer32,
              snmpEventNotifyStatus                   RowStatus
          }














          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpEventNotifyIntervalRequested OBJECT-TYPE
              SYNTAX     Integer32
              UNITS      "seconds"
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The requested interval for retransmission of
                      Inform PDUs generated on the behalf of this entry.

                      This variable will be the actual interval used
                      unless the snmpEventNotifyMinInterval is greater
                      than this object, in which case the interval shall
                      be equal to snmpEventNotifyMinInterval."
              DEFVAL { 30 }
              ::= { snmpEventNotifyEntry 1 }

          snmpEventNotifyRetransmissionsRequested OBJECT-TYPE
              SYNTAX     Integer32
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The requested number of retransmissions of an
                      InformRequest-PDU generated on behalf of this
                      entry.

                      This variable will be the actual number of
                      retransmissions used unless the
                      snmpEventNotifyMaxRetransmissions is less than
                      this object, in which case the retransmission
                      count shall be equal to
                      snmpEventNotifyMaxRetransmissions."
              DEFVAL { 5 }
              ::= { snmpEventNotifyEntry 2 }

















          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpEventNotifyLifetime OBJECT-TYPE
              SYNTAX     Integer32
              UNITS      "seconds"
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The number of seconds this entry shall live until
                      the corresponding instance of
                      snmpEventNotifyStatus is set to 'destroy'.  This
                      value shall count down to zero, at which time the
                      corresponding instance of snmpEventNotifyStatus
                      will be set to 'destroy'.  Any management station
                      that is using this entry must periodically refresh
                      this value to ensure the continued delivery of
                      events."
              DEFVAL { 86400 }
              ::= { snmpEventNotifyEntry 3 }

          snmpEventNotifyStatus OBJECT-TYPE
              SYNTAX     RowStatus
              MAX-ACCESS read-create
              STATUS     current
              DESCRIPTION
                      "The state of this snmpEventNotifyEntry.  This
                      object may not be set to `active' unless the
                      following columnar objects exist in this row:
                      snmpEventNotifyIntervalRequested,
                      snmpEventNotifyRetransmissionsRequested, and
                      snmpEventNotifyLifetime."
              ::= { snmpEventNotifyEntry 4 }




















          RFC 1451            Manager-to-Manager MIB          April 1993


          -- conformance information

          snmpM2MConformance
                         OBJECT IDENTIFIER ::= { snmpM2M 2 }

          snmpM2MCompliances
                         OBJECT IDENTIFIER ::= { snmpM2MConformance 1 }
          snmpM2MGroups  OBJECT IDENTIFIER ::= { snmpM2MConformance 2 }


          -- compliance statements

          snmpM2MCompliance MODULE-COMPLIANCE
              STATUS  current
              DESCRIPTION
                      "The compliance statement for SNMPv2 entities
                      which implement the Manager-to-Manager MIB."
              MODULE  -- this module
                  MANDATORY-GROUPS { snmpAlarmGroup, snmpEventGroup }
              ::= { snmpM2MCompliances 1 }


          -- units of conformance

          snmpAlarmGroup OBJECT-GROUP
              OBJECTS { snmpAlarmNextIndex,
                        snmpAlarmVariable, snmpAlarmInterval,
                        snmpAlarmSampleType, snmpAlarmValue,
                        snmpAlarmStartupAlarm, snmpAlarmRisingThreshold,
                        snmpAlarmFallingThreshold,
                        snmpAlarmRisingEventIndex,
                        snmpAlarmFallingEventIndex,
                        snmpAlarmUnavailableEventIndex,
                        snmpAlarmStatus }
              STATUS  current
              DESCRIPTION
                      "A collection of objects allowing the description
                      and configuration of threshold alarms from a
                      SNMPv2 entity acting in a dual role."
              ::= { snmpM2MGroups 1 }










          RFC 1451            Manager-to-Manager MIB          April 1993


          snmpEventGroup OBJECT-GROUP
              OBJECTS { snmpEventNextIndex,
                        snmpEventID, snmpEventDescription,
                        snmpEventEvents, snmpEventLastTimeSent,
                        snmpEventStatus, snmpEventNotifyMinInterval,
                        snmpEventNotifyMaxRetransmissions,
                        snmpEventNotifyIntervalRequested,
                        snmpEventNotifyRetransmissionsRequested,
                        snmpEventNotifyLifetime, snmpEventNotifyStatus }
              STATUS  current
              DESCRIPTION
                      "A collection of objects allowing the description
                      and configuration of events from a SNMPv2 entity
                      acting in a dual role."
              ::= { snmpM2MGroups 2 }


          END
































          
