SNMP-TARGET-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY,
       OBJECT-TYPE,
       snmpModules,
       Counter32,
       Integer32
           FROM SNMPv2-SMI

       TEXTUAL-CONVENTION,
       TDomain,
       TAddress,
       TimeInterval,
       RowStatus,
       StorageType,





       TestAndIncr
           FROM SNMPv2-TC

       SnmpSecurityModel,
       SnmpMessageProcessingModel,
       SnmpSecurityLevel,
       SnmpAdminString
           FROM SNMP-FRAMEWORK-MIB

       MODULE-COMPLIANCE,
       OBJECT-GROUP
           FROM SNMPv2-CONF;

   snmpTargetMIB MODULE-IDENTITY
       LAST-UPDATED "200210140000Z"
       ORGANIZATION "IETF SNMPv3 Working Group"
       CONTACT-INFO
           "WG-email:   snmpv3@lists.tislabs.com
            Subscribe:  majordomo@lists.tislabs.com
                        In message body:  subscribe snmpv3

            Co-Chair:   Russ Mundy
                        Network Associates Laboratories
            Postal:     15204 Omega Drive, Suite 300
                        Rockville, MD 20850-4601
                        USA
            EMail:      mundy@tislabs.com
            Phone:      +1 301-947-7107

            Co-Chair:   David Harrington
                        Enterasys Networks
            Postal:     35 Industrial Way
                        P. O. Box 5004
                        Rochester, New Hampshire 03866-5005
                        USA
            EMail:      dbh@enterasys.com
            Phone:      +1 603-337-2614

            Co-editor:  David B. Levi
                        Nortel Networks
            Postal:     3505 Kesterwood Drive
                        Knoxville, Tennessee 37918
            EMail:      dlevi@nortelnetworks.com
            Phone:      +1 865 686 0432

            Co-editor:  Paul Meyer
                        Secure Computing Corporation
            Postal:     2675 Long Lake Road





                        Roseville, Minnesota 55113
            EMail:      paul_meyer@securecomputing.com
            Phone:      +1 651 628 1592

            Co-editor:  Bob Stewart
                        Retired"
       DESCRIPTION
           "This MIB module defines MIB objects which provide
            mechanisms to remotely configure the parameters used
            by an SNMP entity for the generation of SNMP messages.

            Copyright (C) The Internet Society (2002). This
            version of this MIB module is part of RFC 3413;
            see the RFC itself for full legal notices.
           "
       REVISION    "200210140000Z"             -- 14 October 2002
       DESCRIPTION "Fixed DISPLAY-HINTS for UTF-8 strings, fixed hex
                    value of LF characters, clarified meaning of zero
                    length tag values, improved tag list examples.
                    Published as RFC 3413."
       REVISION    "199808040000Z"             -- 4 August 1998
       DESCRIPTION "Clarifications, published as
                    RFC 2573."
       REVISION    "199707140000Z"             -- 14 July 1997
       DESCRIPTION "The initial revision, published as RFC2273."
       ::= { snmpModules 12 }

   snmpTargetObjects       OBJECT IDENTIFIER ::= { snmpTargetMIB 1 }
   snmpTargetConformance   OBJECT IDENTIFIER ::= { snmpTargetMIB 3 }

   SnmpTagValue ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "255t"
       STATUS       current
       DESCRIPTION
           "An octet string containing a tag value.
            Tag values are preferably in human-readable form.

            To facilitate internationalization, this information
            is represented using the ISO/IEC IS 10646-1 character
            set, encoded as an octet string using the UTF-8
            character encoding scheme described in RFC 2279.

            Since additional code points are added by amendments
            to the 10646 standard from time to time,
            implementations must be prepared to encounter any code
            point from 0x00000000 to 0x7fffffff.

            The use of control codes should be avoided, and certain





            control codes are not allowed as described below.

            For code points not directly supported by user
            interface hardware or software, an alternative means
            of entry and display, such as hexadecimal, may be
            provided.

            For information encoded in 7-bit US-ASCII, the UTF-8
            representation is identical to the US-ASCII encoding.

            Note that when this TC is used for an object that
            is used or envisioned to be used as an index, then a
            SIZE restriction must be specified so that the number
            of sub-identifiers for any object instance does not
            exceed the limit of 128, as defined by [RFC1905].

            An object of this type contains a single tag value
            which is used to select a set of entries in a table.

            A tag value is an arbitrary string of octets, but
            may not contain a delimiter character.  Delimiter
            characters are defined to be one of the following:

                -  An ASCII space character (0x20).

                -  An ASCII TAB character (0x09).

                -  An ASCII carriage return (CR) character (0x0D).

                -  An ASCII line feed (LF) character (0x0A).

            Delimiter characters are used to separate tag values
            in a tag list.  An object of this type may only
            contain a single tag value, and so delimiter
            characters are not allowed in a value of this type.

            Note that a tag value of 0 length means that no tag is
            defined.  In other words, a tag value of 0 length would
            never match anything in a tag list, and would never
            select any table entries.

            Some examples of valid tag values are:

                - 'acme'

                - 'router'

                - 'host'





            The use of a tag value to select table entries is
            application and MIB specific."
       SYNTAX       OCTET STRING (SIZE (0..255))

   SnmpTagList ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "255t"
       STATUS       current
       DESCRIPTION
           "An octet string containing a list of tag values.
            Tag values are preferably in human-readable form.

            To facilitate internationalization, this information
            is represented using the ISO/IEC IS 10646-1 character
            set, encoded as an octet string using the UTF-8
            character encoding scheme described in RFC 2279.

            Since additional code points are added by amendments
            to the 10646 standard from time to time,
            implementations must be prepared to encounter any code
            point from 0x00000000 to 0x7fffffff.

            The use of control codes should be avoided, except as
            described below.

            For code points not directly supported by user
            interface hardware or software, an alternative means
            of entry and display, such as hexadecimal, may be
            provided.

            For information encoded in 7-bit US-ASCII, the UTF-8
            representation is identical to the US-ASCII encoding.

            An object of this type contains a list of tag values
            which are used to select a set of entries in a table.

            A tag value is an arbitrary string of octets, but
            may not contain a delimiter character.  Delimiter
            characters are defined to be one of the following:

                -  An ASCII space character (0x20).

                -  An ASCII TAB character (0x09).

                -  An ASCII carriage return (CR) character (0x0D).

                -  An ASCII line feed (LF) character (0x0A).

            Delimiter characters are used to separate tag values





            in a tag list.  Only a single delimiter character may
            occur between two tag values.  A tag value may not
            have a zero length.  These constraints imply certain
            restrictions on the contents of this object:

                - There cannot be a leading or trailing delimiter
                  character.

                - There cannot be multiple adjacent delimiter
                  characters.

            Some examples of valid tag lists are:

                - ''                        -- an empty list

                - 'acme'                    -- list of one tag

                - 'host router bridge'      -- list of several tags

            Note that although a tag value may not have a length of
            zero, an empty string is still valid.  This indicates
            an empty list (i.e. there are no tag values in the list).

            The use of the tag list to select table entries is
            application and MIB specific.  Typically, an application
            will provide one or more tag values, and any entry
            which contains some combination of these tag values
            will be selected."
       SYNTAX       OCTET STRING (SIZE (0..255))

   --
   --
   -- The snmpTargetObjects group
   --
   --

   snmpTargetSpinLock OBJECT-TYPE
       SYNTAX      TestAndIncr
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "This object is used to facilitate modification of table
            entries in the SNMP-TARGET-MIB module by multiple
            managers.  In particular, it is useful when modifying
            the value of the snmpTargetAddrTagList object.

            The procedure for modifying the snmpTargetAddrTagList
            object is as follows:





                1.  Retrieve the value of snmpTargetSpinLock and
                    of snmpTargetAddrTagList.

                2.  Generate a new value for snmpTargetAddrTagList.

                3.  Set the value of snmpTargetSpinLock to the
                    retrieved value, and the value of
                    snmpTargetAddrTagList to the new value.  If
                    the set fails for the snmpTargetSpinLock
                    object, go back to step 1."
       ::= { snmpTargetObjects 1 }

   snmpTargetAddrTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF SnmpTargetAddrEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table of transport addresses to be used in the generation
            of SNMP messages."
       ::= { snmpTargetObjects 2 }

   snmpTargetAddrEntry OBJECT-TYPE
       SYNTAX      SnmpTargetAddrEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A transport address to be used in the generation
            of SNMP operations.

            Entries in the snmpTargetAddrTable are created and
            deleted using the snmpTargetAddrRowStatus object."
       INDEX { IMPLIED snmpTargetAddrName }
       ::= { snmpTargetAddrTable 1 }

   SnmpTargetAddrEntry ::= SEQUENCE {
       snmpTargetAddrName         SnmpAdminString,
       snmpTargetAddrTDomain      TDomain,
       snmpTargetAddrTAddress     TAddress,
       snmpTargetAddrTimeout      TimeInterval,
       snmpTargetAddrRetryCount   Integer32,
       snmpTargetAddrTagList      SnmpTagList,
       snmpTargetAddrParams       SnmpAdminString,
       snmpTargetAddrStorageType  StorageType,
       snmpTargetAddrRowStatus    RowStatus
   }

   snmpTargetAddrName OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE(1..32))





       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The locally arbitrary, but unique identifier associated
            with this snmpTargetAddrEntry."
       ::= { snmpTargetAddrEntry 1 }

   snmpTargetAddrTDomain OBJECT-TYPE
       SYNTAX      TDomain
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object indicates the transport type of the address
            contained in the snmpTargetAddrTAddress object."
       ::= { snmpTargetAddrEntry 2 }

   snmpTargetAddrTAddress OBJECT-TYPE
       SYNTAX      TAddress
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object contains a transport address.  The format of
            this address depends on the value of the
            snmpTargetAddrTDomain object."
       ::= { snmpTargetAddrEntry 3 }

   snmpTargetAddrTimeout OBJECT-TYPE
       SYNTAX      TimeInterval
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object should reflect the expected maximum round
            trip time for communicating with the transport address
            defined by this row.  When a message is sent to this
            address, and a response (if one is expected) is not
            received within this time period, an implementation
            may assume that the response will not be delivered.

            Note that the time interval that an application waits
            for a response may actually be derived from the value
            of this object.  The method for deriving the actual time
            interval is implementation dependent.  One such method
            is to derive the expected round trip time based on a
            particular retransmission algorithm and on the number
            of timeouts which have occurred.  The type of message may
            also be considered when deriving expected round trip
            times for retransmissions.  For example, if a message is
            being sent with a securityLevel that indicates both





            authentication and privacy, the derived value may be
            increased to compensate for extra processing time spent
            during authentication and encryption processing."
       DEFVAL { 1500 }
       ::= { snmpTargetAddrEntry 4 }

   snmpTargetAddrRetryCount OBJECT-TYPE
       SYNTAX      Integer32 (0..255)
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object specifies a default number of retries to be
            attempted when a response is not received for a generated
            message.  An application may provide its own retry count,
            in which case the value of this object is ignored."
       DEFVAL { 3 }
       ::= { snmpTargetAddrEntry 5 }

   snmpTargetAddrTagList OBJECT-TYPE
       SYNTAX      SnmpTagList
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object contains a list of tag values which are
            used to select target addresses for a particular
            operation."
       DEFVAL { "" }
       ::= { snmpTargetAddrEntry 6 }

   snmpTargetAddrParams OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE(1..32))
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The value of this object identifies an entry in the
            snmpTargetParamsTable.  The identified entry
            contains SNMP parameters to be used when generating
            messages to be sent to this transport address."
       ::= { snmpTargetAddrEntry 7 }

   snmpTargetAddrStorageType OBJECT-TYPE
       SYNTAX      StorageType
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The storage type for this conceptual row.
            Conceptual rows having the value 'permanent' need not
            allow write-access to any columnar objects in the row."





       DEFVAL { nonVolatile }
       ::= { snmpTargetAddrEntry 8 }

   snmpTargetAddrRowStatus OBJECT-TYPE
       SYNTAX      RowStatus
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The status of this conceptual row.

            To create a row in this table, a manager must
            set this object to either createAndGo(4) or
            createAndWait(5).

            Until instances of all corresponding columns are
            appropriately configured, the value of the
            corresponding instance of the snmpTargetAddrRowStatus
            column is 'notReady'.

            In particular, a newly created row cannot be made
            active until the corresponding instances of
            snmpTargetAddrTDomain, snmpTargetAddrTAddress, and
            snmpTargetAddrParams have all been set.

            The following objects may not be modified while the
            value of this object is active(1):
                - snmpTargetAddrTDomain
                - snmpTargetAddrTAddress
            An attempt to set these objects while the value of
            snmpTargetAddrRowStatus is active(1) will result in
            an inconsistentValue error."
       ::= { snmpTargetAddrEntry 9 }

   snmpTargetParamsTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF SnmpTargetParamsEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table of SNMP target information to be used
            in the generation of SNMP messages."
       ::= { snmpTargetObjects 3 }

   snmpTargetParamsEntry OBJECT-TYPE
       SYNTAX      SnmpTargetParamsEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A set of SNMP target information.





            Entries in the snmpTargetParamsTable are created and
            deleted using the snmpTargetParamsRowStatus object."
       INDEX { IMPLIED snmpTargetParamsName }
       ::= { snmpTargetParamsTable 1 }

   SnmpTargetParamsEntry ::= SEQUENCE {
       snmpTargetParamsName           SnmpAdminString,
       snmpTargetParamsMPModel        SnmpMessageProcessingModel,
       snmpTargetParamsSecurityModel  SnmpSecurityModel,
       snmpTargetParamsSecurityName   SnmpAdminString,
       snmpTargetParamsSecurityLevel  SnmpSecurityLevel,
       snmpTargetParamsStorageType    StorageType,
       snmpTargetParamsRowStatus      RowStatus
   }

   snmpTargetParamsName OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE(1..32))
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The locally arbitrary, but unique identifier associated
            with this snmpTargetParamsEntry."
       ::= { snmpTargetParamsEntry 1 }

   snmpTargetParamsMPModel OBJECT-TYPE
       SYNTAX      SnmpMessageProcessingModel
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The Message Processing Model to be used when generating
            SNMP messages using this entry."
       ::= { snmpTargetParamsEntry 2 }

   snmpTargetParamsSecurityModel OBJECT-TYPE
       SYNTAX      SnmpSecurityModel (1..2147483647)
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The Security Model to be used when generating SNMP
             messages using this entry.  An implementation may
             choose to return an inconsistentValue error if an
             attempt is made to set this variable to a value
             for a security model which the implementation does
             not support."
       ::= { snmpTargetParamsEntry 3 }

   snmpTargetParamsSecurityName OBJECT-TYPE
       SYNTAX      SnmpAdminString





       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The securityName which identifies the Principal on
            whose behalf SNMP messages will be generated using
            this entry."
       ::= { snmpTargetParamsEntry 4 }

   snmpTargetParamsSecurityLevel OBJECT-TYPE
       SYNTAX      SnmpSecurityLevel
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The Level of Security to be used when generating
            SNMP messages using this entry."
       ::= { snmpTargetParamsEntry 5 }

   snmpTargetParamsStorageType OBJECT-TYPE
       SYNTAX      StorageType
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The storage type for this conceptual row.
            Conceptual rows having the value 'permanent' need not
            allow write-access to any columnar objects in the row."
       DEFVAL { nonVolatile }
       ::= { snmpTargetParamsEntry 6 }

   snmpTargetParamsRowStatus OBJECT-TYPE
       SYNTAX      RowStatus
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The status of this conceptual row.

            To create a row in this table, a manager must
            set this object to either createAndGo(4) or
            createAndWait(5).

            Until instances of all corresponding columns are
            appropriately configured, the value of the
            corresponding instance of the snmpTargetParamsRowStatus
            column is 'notReady'.

            In particular, a newly created row cannot be made
            active until the corresponding
            snmpTargetParamsMPModel,
            snmpTargetParamsSecurityModel,





            snmpTargetParamsSecurityName,
            and snmpTargetParamsSecurityLevel have all been set.

            The following objects may not be modified while the
            value of this object is active(1):
                - snmpTargetParamsMPModel
                - snmpTargetParamsSecurityModel
                - snmpTargetParamsSecurityName
                - snmpTargetParamsSecurityLevel
            An attempt to set these objects while the value of
            snmpTargetParamsRowStatus is active(1) will result in
            an inconsistentValue error."
       ::= { snmpTargetParamsEntry 7 }

   snmpUnavailableContexts OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "The total number of packets received by the SNMP
            engine which were dropped because the context
            contained in the message was unavailable."
       ::= { snmpTargetObjects 4 }

   snmpUnknownContexts OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "The total number of packets received by the SNMP
            engine which were dropped because the context
            contained in the message was unknown."
       ::= { snmpTargetObjects 5 }

   --
   --
   -- Conformance information
   --
   --

   snmpTargetCompliances OBJECT IDENTIFIER ::=
                                           { snmpTargetConformance 1 }
   snmpTargetGroups      OBJECT IDENTIFIER ::=
                                           { snmpTargetConformance 2 }

   --
   --
   -- Compliance statements





   --
   --

   snmpTargetCommandResponderCompliance MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "The compliance statement for SNMP entities which include
            a command responder application."
       MODULE -- This Module
           MANDATORY-GROUPS { snmpTargetCommandResponderGroup }
       ::= { snmpTargetCompliances 1 }

   snmpTargetBasicGroup OBJECT-GROUP
       OBJECTS {
           snmpTargetSpinLock,
           snmpTargetAddrTDomain,
           snmpTargetAddrTAddress,
           snmpTargetAddrTagList,
           snmpTargetAddrParams,
           snmpTargetAddrStorageType,
           snmpTargetAddrRowStatus,
           snmpTargetParamsMPModel,
           snmpTargetParamsSecurityModel,
           snmpTargetParamsSecurityName,
           snmpTargetParamsSecurityLevel,
           snmpTargetParamsStorageType,
           snmpTargetParamsRowStatus
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing basic remote
            configuration of management targets."
       ::= { snmpTargetGroups 1 }

   snmpTargetResponseGroup OBJECT-GROUP
       OBJECTS {
           snmpTargetAddrTimeout,
           snmpTargetAddrRetryCount
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing remote configuration
            of management targets for applications which generate
            SNMP messages for which a response message would be
            expected."
       ::= { snmpTargetGroups 2 }

   snmpTargetCommandResponderGroup OBJECT-GROUP





       OBJECTS {
           snmpUnavailableContexts,
           snmpUnknownContexts
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects required for command responder
            applications, used for counting error conditions."
       ::= { snmpTargetGroups 3 }

   END


