MPLS-ID-STD-MIB DEFINITIONS ::= BEGIN


   IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE
       FROM SNMPv2-SMI                                 -- RFC 2578
    MODULE-COMPLIANCE, OBJECT-GROUP
       FROM SNMPv2-CONF                                -- RFC 2580
    mplsStdMIB
       FROM MPLS-TC-STD-MIB                            -- RFC 3811
    MplsGlobalId, MplsCcId, MplsIccId, MplsNodeId
       FROM MPLS-TC-EXT-STD-MIB
    ;

  mplsIdStdMIB MODULE-IDENTITY
    LAST-UPDATED
        "201502020000Z" -- February 2, 2015
    ORGANIZATION
       "Multiprotocol Label Switching (MPLS) Working Group"

    CONTACT-INFO
       "
              Venkatesan Mahalingam
              Dell Inc,
              5450 Great America Parkway,
              Santa Clara, CA 95054, USA
        Email: venkat.mahalingams@gmail.com

              Kannan KV Sampath
              Redeem,
              India
        Email: kannankvs@gmail.com

              Sam Aldrin
              Huawei Technologies
              2330 Central Express Way,
              Santa Clara, CA 95051, USA
        Email:  aldrin.ietf@gmail.com






              Thomas D. Nadeau
        Email: tnadeau@lucidvision.com
      "
    DESCRIPTION
        "This MIB module contains identifier object definitions for
         MPLS Traffic Engineering in transport networks.

         Copyright (c) 2015 IETF Trust and the persons identified as
         authors of the code.  All rights reserved.

         Redistribution and use in source and binary forms, with or
         without modification, is permitted pursuant to, and subject to
         the license terms contained in, the Simplified BSD License set
         forth in Section 4.c of the IETF Trust's Legal Provisions
         Relating to IETF Documents
         (http://trustee.ietf.org/license-info)."

    -- Revision history.

    REVISION
        "201502020000Z" -- February 2, 2015
    DESCRIPTION
         "This MIB modules defines the MIB objects for MPLS-TP
          identifiers"

    ::= { mplsStdMIB 18 }

    -- notifications
    mplsIdNotifications OBJECT IDENTIFIER ::= { mplsIdStdMIB 0 }
    -- tables, scalars
    mplsIdObjects       OBJECT IDENTIFIER ::= { mplsIdStdMIB 1 }
    -- conformance
    mplsIdConformance   OBJECT IDENTIFIER ::= { mplsIdStdMIB 2 }

    -- MPLS common objects

  mplsIdGlobalId OBJECT-TYPE
       SYNTAX      MplsGlobalId
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "This object allows the operator or service provider to
            assign a unique operator identifier, also called the MPLS-TP
            Global_ID.
            If this value is used in mplsTunnelExtNodeConfigGlobalId
            for mapping Global_ID::Node_ID with the local identifier,
            then this object value MUST NOT be changed."
      ::= { mplsIdObjects 1 }





  mplsIdNodeId OBJECT-TYPE
       SYNTAX      MplsNodeId
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
          "This object allows the operator or service provider to
           assign a unique MPLS-TP Node_ID.  The Node_ID is assigned
           within the scope of the Global_ID/ICC_Operator_ID.
           If this value is used in mplsTunnelExtNodeConfigNodeId
           for mapping Global_ID::Node_ID with the local identifier,
           then this object value SHOULD NOT be changed.
           If this value is used in mplsTunnelExtNodeConfigNodeId
           for mapping ICC_Operator_ID::Node_ID with the local
           identifier, then this object value MUST NOT be changed."
      ::= { mplsIdObjects 2 }

  mplsIdCc OBJECT-TYPE
       SYNTAX      MplsCcId
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
          "This object allows the operator or service provider to
           assign a Country Code (CC) to the node.  Global
           uniqueness of ICC is assured by concatenating the ICC
           with a Country Code (CC).
           If this value is used in mplsTunnelExtNodeConfigCcId
           for mapping ICC_Operator_ID::Node_ID with the local
           identifier, then this object value MUST NOT be changed."
      REFERENCE
           "MPLS-TP Identifiers Following ITU-T Conventions,
            RFC 6923, Section 3"
          ::= { mplsIdObjects 3 }

  mplsIdIcc OBJECT-TYPE
       SYNTAX      MplsIccId
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
          "This object allows the operator or service provider to
           assign a unique MPLS-TP ITU-T Carrier Code (ICC) to
           the node.  Together, the CC and the ICC form
           the ICC_Operator_ID as CC::ICC.
           If this value is used in mplsTunnelExtNodeConfigIccId
           for mapping ICC_Operator_ID::Node_ID with the local
           identifier, then this object value MUST NOT be changed."
      REFERENCE
           "MPLS-TP Identifiers Following ITU-T Conventions,
            RFC 6923, Section 3"





          ::= { mplsIdObjects 4 }

   -- Module compliance.

  mplsIdCompliances
     OBJECT IDENTIFIER ::= { mplsIdConformance 1 }

  mplsIdGroups
     OBJECT IDENTIFIER ::= { mplsIdConformance 2 }

  -- Compliance requirement for fully compliant implementations.

  mplsIdModuleFullCompliance MODULE-COMPLIANCE
     STATUS current
     DESCRIPTION
          "Compliance statement for agents that provide full
            support of the MPLS-ID-STD-MIB module."

     MODULE -- this module

        -- The mandatory group has to be implemented by all LSRs that
        -- originate, terminate, or act as transit for MPLS-TP Tunnels.

        GROUP mplsIdIpOperatorGroup
        DESCRIPTION
            "This group is mandatory for devices that support
             IP-based identifier configuration."

        GROUP mplsIdIccOperatorGroup
        DESCRIPTION
            "This group is mandatory for devices that support
             ICC-based identifier configuration."

         ::= { mplsIdCompliances 1 }

         -- Compliance requirement for read-only implementations.

        mplsIdModuleReadOnlyCompliance MODULE-COMPLIANCE
           STATUS current
           DESCRIPTION
                "Compliance statement for agents that only provide
                 read-only support for the MPLS-ID-STD-MIB module."

        MODULE -- this module









        GROUP mplsIdIpOperatorGroup
        DESCRIPTION
            "This group is mandatory for devices that support
             IP-based identifier configuration."

        GROUP mplsIdIccOperatorGroup
        DESCRIPTION
            "This group is mandatory for devices that support
             ICC-based identifier configuration."

        OBJECT   mplsIdGlobalId
        MIN-ACCESS  read-only
        DESCRIPTION
          "Write access is not required."

        OBJECT   mplsIdNodeId
        MIN-ACCESS  read-only
        DESCRIPTION
          "Write access is not required."

        OBJECT   mplsIdCc
        MIN-ACCESS  read-only
        DESCRIPTION
          "Write access is not required."

        OBJECT   mplsIdIcc
        MIN-ACCESS  read-only
        DESCRIPTION
          "Write access is not required."

        ::= { mplsIdCompliances 2 }

    -- Units of conformance.

        mplsIdIpOperatorGroup OBJECT-GROUP
              OBJECTS { mplsIdGlobalId,
                        mplsIdNodeId
              }
              STATUS  current
              DESCRIPTION
                  "The objects in this group are optional for an
                   ICC-based node."
              ::= { mplsIdGroups 1 }










        mplsIdIccOperatorGroup OBJECT-GROUP
              OBJECTS { mplsIdNodeId,
                        mplsIdCc,
                        mplsIdIcc
              }
              STATUS  current
              DESCRIPTION
                 "The objects in this group are optional for an
                  IP-based node."
              ::= { mplsIdGroups 2 }

   -- MPLS-ID-STD-MIB module ends
   END


