DOCS-BPI-MIB DEFINITIONS ::= BEGIN


IMPORTS
MODULE-IDENTITY, OBJECT-TYPE,
Integer32, Counter32, IpAddress
FROM SNMPv2-SMI
DisplayString, MacAddress, RowStatus, TruthValue, DateAndTime
FROM SNMPv2-TC
OBJECT-GROUP, MODULE-COMPLIANCE
FROM SNMPv2-CONF
ifIndex
FROM IF-MIB
docsIfMib, docsIfCmServiceId, docsIfCmtsServiceId
FROM DOCS-IF-MIB
;

docsBpiMIB      MODULE-IDENTITY
LAST-UPDATED "200103130000Z"
ORGANIZATION "IETF IPCDN Working Group"
CONTACT-INFO "Rich Woundy
              Postal: Cisco Systems
                      250 Apollo Drive
                      Chelmsford, MA 01824 U.S.A.
              Tel: +1 978 244 8000
              E-mail: rwoundy@cisco.com

              IETF IPCDN Working Group
              General Discussion: ipcdn@ietf.org
              Subscribe: http://www.ietf.org/mailman/listinfo/ipcdn
              Archive: ftp://ftp.ietf.org/ietf-mail-archive/ipcdn
              Co-chairs: Richard Woundy, rwoundy@cisco.com
                         Andrew Valentine, a.valentine@eu.hns.com"
DESCRIPTION
"This is the MIB Module for the DOCSIS Baseline Privacy Interface
(BPI) at cable modems (CMs) and cable modem termination systems
(CMTSs). CableLabs requires the implementation of this MIB in
DOCSIS 1.0 cable modems that implement the Baseline Privacy
Interface, as a prerequisite for DOCSIS 1.0 certification."

REVISION "200103130000Z"
DESCRIPTION
"Version published as RFC 3083."

REVISION "200011031930Z"
DESCRIPTION
"Modified by Richard Woundy to fix problems identified by the MIB





doctor. I marked docsBpiCmtsDefaultAuthGraceTime and
docsBpiCmtsDefaultTEKGraceTime as obsolete objects, to prevent OID
reassignment. Several object descriptions were also corrected."

REVISION "200002161930Z"
DESCRIPTION
"Initial version.
CableLabs requires the implementation of this MIB in certified DOCSIS
1.0 cable modems implementing the Baseline Privacy Interface, per
DOCSIS 1.0 engineering change notice oss-n-99027."
::= { docsIfMib 5 }

docsBpiMIBObjects  OBJECT IDENTIFIER ::= { docsBpiMIB 1 }

-- Cable Modem Group

docsBpiCmObjects OBJECT IDENTIFIER ::= { docsBpiMIBObjects 1 }

--
-- The BPI base and authorization table for CMs, indexed by ifIndex
--

docsBpiCmBaseTable      OBJECT-TYPE
SYNTAX                  SEQUENCE OF     DocsBpiCmBaseEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"This table describes the basic and authorization-related Baseline
Privacy attributes of each CM MAC interface."
::= { docsBpiCmObjects 1 }

docsBpiCmBaseEntry      OBJECT-TYPE
SYNTAX                  DocsBpiCmBaseEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"Each entry contains objects describing attributes of one CM MAC
interface. An entry in this table exists for each ifEntry with an
ifType of docsCableMaclayer(127)."
INDEX                   { ifIndex }
::= { docsBpiCmBaseTable 1 }

DocsBpiCmBaseEntry ::= SEQUENCE {
docsBpiCmPrivacyEnable                  TruthValue,
docsBpiCmPublicKey                      OCTET STRING,
docsBpiCmAuthState                      INTEGER,
docsBpiCmAuthKeySequenceNumber          Integer32,
docsBpiCmAuthExpires                    DateAndTime,





docsBpiCmAuthReset                      TruthValue,
docsBpiCmAuthGraceTime                  Integer32,
docsBpiCmTEKGraceTime                   Integer32,
docsBpiCmAuthWaitTimeout                Integer32,
docsBpiCmReauthWaitTimeout              Integer32,
docsBpiCmOpWaitTimeout                  Integer32,
docsBpiCmRekeyWaitTimeout               Integer32,
docsBpiCmAuthRejectWaitTimeout          Integer32,
docsBpiCmAuthRequests                   Counter32,
docsBpiCmAuthReplies                    Counter32,
docsBpiCmAuthRejects                    Counter32,
docsBpiCmAuthInvalids                   Counter32,
docsBpiCmAuthRejectErrorCode            INTEGER,
docsBpiCmAuthRejectErrorString          DisplayString,
docsBpiCmAuthInvalidErrorCode           INTEGER,
docsBpiCmAuthInvalidErrorString         DisplayString
}

docsBpiCmPrivacyEnable  OBJECT-TYPE
SYNTAX                  TruthValue
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"This object identifies whether this CM is provisioned to run
Baseline Privacy. This is analogous to the presence (or absence)
of the Baseline Privacy Configuration Setting option. The status
of each individual SID with respect to Baseline Privacy is
captured in the docsBpiCmTEKPrivacyEnable object."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1."
::= { docsBpiCmBaseEntry 1 }

docsBpiCmPublicKey      OBJECT-TYPE
SYNTAX                  OCTET STRING (SIZE (74 | 106 | 140 | 270))
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is a DER-encoded RSAPublicKey ASN.1 type
string, as defined in the RSA Encryption Standard (PKCS #1) [22],
corresponding to the public key of the CM. The 74, 106, 140, and
270 byte key encoding lengths correspond to 512 bit, 768 bit, 1024
bit, and 2048 public moduli respectively."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.2.4."
::= { docsBpiCmBaseEntry 2 }

docsBpiCmAuthState      OBJECT-TYPE
SYNTAX                  INTEGER {





                                authWait(2),
                                authorized(3),
                                reauthWait(4),
                                authRejectWait(5)
                        }
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the state of the CM authorization
FSM.  The start state indicates that FSM is in its initial state."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.1.2.1."
::= { docsBpiCmBaseEntry 3 }

docsBpiCmAuthKeySequenceNumber  OBJECT-TYPE
SYNTAX                          Integer32 (0..15)
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the authorization key sequence number
for this FSM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.2
and 4.2.2.10."
::= { docsBpiCmBaseEntry 4 }

docsBpiCmAuthExpires    OBJECT-TYPE
SYNTAX                  DateAndTime
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the actual clock time when the current
authorization for this FSM expires. If the CM does not have an active
authorization, then the value is of the expiration date and time of
the last active authorization."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.2
and 4.2.2.9."
::= { docsBpiCmBaseEntry 5 }

docsBpiCmAuthReset      OBJECT-TYPE
SYNTAX                  TruthValue
MAX-ACCESS              read-write
STATUS                  current
DESCRIPTION
"Setting this object to TRUE generates a Reauthorize event in the
authorization FSM. Reading this object always returns FALSE."
REFERENCE





"DOCSIS Baseline Privacy Interface Specification, Section 4.1.2.3.4."
::= { docsBpiCmBaseEntry 6 }

docsBpiCmAuthGraceTime  OBJECT-TYPE
SYNTAX                  Integer32 (1..1800)
UNITS                   "seconds"
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the grace time for an authorization key.
A CM is expected to start trying to get a new authorization key
beginning AuthGraceTime seconds before the authorization key actually
expires."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.3."
::= { docsBpiCmBaseEntry 7 }

docsBpiCmTEKGraceTime   OBJECT-TYPE
SYNTAX                  Integer32 (1..1800)
UNITS                   "seconds"
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the grace time for a TEK.  A CM is
expected to start trying to get a new TEK beginning TEKGraceTime
seconds before the TEK actually expires."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.6."
::= { docsBpiCmBaseEntry 8 }

docsBpiCmAuthWaitTimeout        OBJECT-TYPE
SYNTAX                          Integer32 (1..30)
UNITS                           "seconds"
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the Authorize Wait Timeout."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.1."
::= { docsBpiCmBaseEntry 9 }

docsBpiCmReauthWaitTimeout      OBJECT-TYPE
SYNTAX                          Integer32 (1..30)
UNITS                           "seconds"
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the Reauthorize Wait Timeout in seconds."





REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.2."
::= { docsBpiCmBaseEntry 10 }

docsBpiCmOpWaitTimeout  OBJECT-TYPE
SYNTAX                  Integer32 (1..10)
UNITS                   "seconds"
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the Operational Wait Timeout in seconds."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.4."
::= { docsBpiCmBaseEntry 11 }

docsBpiCmRekeyWaitTimeout       OBJECT-TYPE
SYNTAX                          Integer32 (1..10)
UNITS                           "seconds"
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the Rekey Wait Timeout in seconds."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.5."
::= { docsBpiCmBaseEntry 12 }

docsBpiCmAuthRejectWaitTimeout  OBJECT-TYPE
SYNTAX                          Integer32 (1..600)
UNITS                           "seconds"
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the Authorization Reject Wait Timeout in
seconds."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.7."
::= { docsBpiCmBaseEntry 13 }

docsBpiCmAuthRequests   OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CM has
transmitted an Authorization Request message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.1."
::= { docsBpiCmBaseEntry 14 }





docsBpiCmAuthReplies    OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CM has
received an Authorization Reply message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.2."
::= { docsBpiCmBaseEntry 15 }

docsBpiCmAuthRejects    OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CM has
received an Authorization Reject message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.3."
::= { docsBpiCmBaseEntry 16 }

docsBpiCmAuthInvalids   OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CM has
received an Authorization Invalid message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.7."
::= { docsBpiCmBaseEntry 17 }

docsBpiCmAuthRejectErrorCode    OBJECT-TYPE
SYNTAX                          INTEGER {
                                        none(1),
                                        unknown(2),
                                        unauthorizedCm(3),
                                        unauthorizedSid(4)
                                }
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the enumerated description of the
Error-Code in most recent Authorization Reject message received by
the CM.  This has value unknown(2) if the last Error-Code value was
0, and none(1) if no Authorization Reject message has been received
since reboot."





REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.3
and 4.2.2.16."
::= { docsBpiCmBaseEntry 18 }

docsBpiCmAuthRejectErrorString  OBJECT-TYPE
SYNTAX                          DisplayString (SIZE (0..128))
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the Display-String in most recent
Authorization Reject message received by the CM.  This is a zero
length string if no Authorization Reject message has been received
since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.3
and 4.2.2.6."
::= { docsBpiCmBaseEntry 19 }

docsBpiCmAuthInvalidErrorCode   OBJECT-TYPE
SYNTAX                  INTEGER {
                                none(1),
                                unknown(2),
                                unauthorizedCm(3),
                                unsolicited(5),
                                invalidKeySequence(6),
                                keyRequestAuthenticationFailure(7)
                        }
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the enumerated description of the
Error-Code in most recent Authorization Invalid message received by
the CM.  This has value unknown(2) if the last Error-Code value was
0, and none(1) if no Authorization Invalid message has been received
since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.7
and 4.2.2.16."
::= { docsBpiCmBaseEntry 20 }

docsBpiCmAuthInvalidErrorString OBJECT-TYPE
SYNTAX                          DisplayString (SIZE (0..128))
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the Display-String in most recent
Authorization Invalid message received by the CM.  This is a zero





length string if no Authorization Invalid message has been received
since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.7
and 4.2.2.6."
::= { docsBpiCmBaseEntry 21 }

--
-- The CM TEK Table, indexed by ifIndex and SID
--

docsBpiCmTEKTable       OBJECT-TYPE
SYNTAX                  SEQUENCE OF     DocsBpiCmTEKEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"This table describes the attributes of each CM Traffic Encryption Key
(TEK) association. The CM maintains (no more than) one TEK association
per SID per CM MAC interface."
::= { docsBpiCmObjects 2 }

docsBpiCmTEKEntry       OBJECT-TYPE
SYNTAX                  DocsBpiCmTEKEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"Each entry contains objects describing the TEK association attributes
of one SID. The CM MUST create one entry per unicast SID, regardless
of whether the SID was obtained from a Registration Response message,
or from an Authorization Reply message."
INDEX                   { ifIndex, docsIfCmServiceId }
::= { docsBpiCmTEKTable 1 }

DocsBpiCmTEKEntry ::= SEQUENCE {
docsBpiCmTEKPrivacyEnable               TruthValue,
docsBpiCmTEKState                       INTEGER,
docsBpiCmTEKExpiresOld                  DateAndTime,
docsBpiCmTEKExpiresNew                  DateAndTime,
docsBpiCmTEKKeyRequests                 Counter32,
docsBpiCmTEKKeyReplies                  Counter32,
docsBpiCmTEKKeyRejects                  Counter32,
docsBpiCmTEKInvalids                    Counter32,
docsBpiCmTEKAuthPends                   Counter32,
docsBpiCmTEKKeyRejectErrorCode          INTEGER,
docsBpiCmTEKKeyRejectErrorString        DisplayString,
docsBpiCmTEKInvalidErrorCode            INTEGER,
docsBpiCmTEKInvalidErrorString          DisplayString
}





docsBpiCmTEKPrivacyEnable       OBJECT-TYPE
SYNTAX                          TruthValue
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"This object identifies whether this SID is provisioned to run
Baseline Privacy. This is analogous to enabling Baseline Privacy on
a provisioned SID using the Class-of-Service Privacy Enable option.
Baseline Privacy is not effectively enabled for any SID unless
Baseline Privacy is enabled for the CM, which is managed via the
docsBpiCmPrivacyEnable object."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.2."
::= { docsBpiCmTEKEntry 1 }

docsBpiCmTEKState       OBJECT-TYPE
SYNTAX                  INTEGER {
                                start(1),
                                opWait(2),
                                opReauthWait(3),
                                operational(4),
                                rekeyWait(5),
                                rekeyReauthWait(6)
                        }
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the state of the indicated TEK FSM.
The start(1) state indicates that FSM is in its initial state."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.1.3.1."
::= { docsBpiCmTEKEntry 2 }

docsBpiCmTEKExpiresOld  OBJECT-TYPE
SYNTAX                  DateAndTime
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the actual clock time for expiration
of the immediate predecessor of the most recent TEK for this FSM.
If this FSM has only one TEK, then the value is the time of activation
of this FSM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.5 and
4.2.2.9."
::= { docsBpiCmTEKEntry 3 }

docsBpiCmTEKExpiresNew  OBJECT-TYPE





SYNTAX                  DateAndTime
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the actual clock time for expiration
of the most recent TEK for this FSM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.5 and
4.2.2.9."
::= { docsBpiCmTEKEntry 4 }

docsBpiCmTEKKeyRequests OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CM has transmitted
a Key Request message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.4."
::= { docsBpiCmTEKEntry 5 }

docsBpiCmTEKKeyReplies  OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CM has received
a Key Reply message, including a message whose authentication failed."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.5."
::= { docsBpiCmTEKEntry 6 }

docsBpiCmTEKKeyRejects  OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CM has received
a Key Reject message, including a message whose authentication failed."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.6."
::= { docsBpiCmTEKEntry 7 }

docsBpiCmTEKInvalids    OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current





DESCRIPTION
"The value of this object is the count of times the CM has received
a TEK Invalid message, including a message whose authentication failed."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.8."
::= { docsBpiCmTEKEntry 8 }

docsBpiCmTEKAuthPends   OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times an Authorization
Pending (Auth Pend) event occurred in this FSM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.1.3.3.3."
::= { docsBpiCmTEKEntry 9 }

docsBpiCmTEKKeyRejectErrorCode  OBJECT-TYPE
SYNTAX                          INTEGER {
                                        none(1),
                                        unknown(2),
                                        unauthorizedSid(4)
                                }
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the enumerated description of the
Error-Code in most recent Key Reject message received by the CM. This
has value unknown(2) if the last Error-Code value was 0, and none(1)
if no Key Reject message has been received since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.1.2.6
and 4.2.2.16."
::= { docsBpiCmTEKEntry 10 }

docsBpiCmTEKKeyRejectErrorString        OBJECT-TYPE
SYNTAX                                  DisplayString (SIZE (0..128))
MAX-ACCESS                              read-only
STATUS                                  current
DESCRIPTION
"The value of this object is the Display-String in most recent Key
Reject message received by the CM. This is a zero length string if no
Key Reject message has been received since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.1.2.6
and 4.2.2.6."
::= { docsBpiCmTEKEntry 11 }





docsBpiCmTEKInvalidErrorCode    OBJECT-TYPE
SYNTAX                          INTEGER {
                                        none(1),
                                        unknown(2),
                                        invalidKeySequence(6)
                                }
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the enumerated description of the
Error-Code in most recent TEK Invalid message received by the CM.
This has value unknown(2) if the last Error-Code value was 0, and
none(1) if no TEK Invalid message has been received since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.1.2.8
and 4.2.2.16."
::= { docsBpiCmTEKEntry 12 }

docsBpiCmTEKInvalidErrorString  OBJECT-TYPE
SYNTAX                          DisplayString (SIZE (0..128))
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the Display-String in most recent TEK
Invalid message received by the CM. This is a zero length string if
no TEK Invalid message has been received since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.1.2.8
and 4.2.2.6."
::= { docsBpiCmTEKEntry 13 }

-- Cable Modem Termination System Group

docsBpiCmtsObjects OBJECT IDENTIFIER ::= { docsBpiMIBObjects 2 }

--
-- The BPI base table for CMTSs, indexed by ifIndex
--

docsBpiCmtsBaseTable    OBJECT-TYPE
SYNTAX                  SEQUENCE OF     DocsBpiCmtsBaseEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"This table describes the basic Baseline Privacy attributes of each
CMTS MAC interface."
::= { docsBpiCmtsObjects 1 }






docsBpiCmtsBaseEntry    OBJECT-TYPE
SYNTAX                  DocsBpiCmtsBaseEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"Each entry contains objects describing attributes of one CMTS MAC
interface. An entry in this table exists for each ifEntry with an
ifType of docsCableMaclayer(127)."
INDEX                   { ifIndex }
::= { docsBpiCmtsBaseTable 1 }

DocsBpiCmtsBaseEntry ::= SEQUENCE {
docsBpiCmtsDefaultAuthLifetime  Integer32,
docsBpiCmtsDefaultTEKLifetime   Integer32,
docsBpiCmtsDefaultAuthGraceTime Integer32,
docsBpiCmtsDefaultTEKGraceTime  Integer32,
docsBpiCmtsAuthRequests         Counter32,
docsBpiCmtsAuthReplies          Counter32,
docsBpiCmtsAuthRejects          Counter32,
docsBpiCmtsAuthInvalids         Counter32
}

docsBpiCmtsDefaultAuthLifetime  OBJECT-TYPE
SYNTAX                          Integer32 (1..6048000)
UNITS                           "seconds"
MAX-ACCESS                      read-write
STATUS                          current
DESCRIPTION
"The value of this object is the default lifetime, in seconds, the
CMTS assigns to a new authorization key."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.2."
::= { docsBpiCmtsBaseEntry 1 }

docsBpiCmtsDefaultTEKLifetime   OBJECT-TYPE
SYNTAX                          Integer32 (1..604800)
UNITS                           "seconds"
MAX-ACCESS                      read-write
STATUS                          current
DESCRIPTION
"The value of this object is the default lifetime, in seconds, the
CMTS assigns to a new Traffic Encryption Key (TEK)."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.2."
::= { docsBpiCmtsBaseEntry 2 }

-- Note: the following two objects have been obsoleted from this MIB.






docsBpiCmtsDefaultAuthGraceTime OBJECT-TYPE
SYNTAX                          Integer32 (1..1800)
UNITS                           "seconds"
MAX-ACCESS                      read-write
STATUS                          obsolete
DESCRIPTION
"This object was obsoleted because the provisioning system, not the CMTS,
manages the authorization key grace time for DOCSIS CMs."
::= { docsBpiCmtsBaseEntry 3 }

docsBpiCmtsDefaultTEKGraceTime  OBJECT-TYPE
SYNTAX                          Integer32 (1..1800)
UNITS                           "seconds"
MAX-ACCESS                      read-write
STATUS                          obsolete
DESCRIPTION
"This object was obsoleted because the provisioning system, not the CMTS,
manages the Traffic Encryption Key (TEK) grace time for DOCSIS CMs."
::= { docsBpiCmtsBaseEntry 4 }

docsBpiCmtsAuthRequests OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CMTS has
received an Authorization Request message from any CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.1."
::= { docsBpiCmtsBaseEntry 5 }

docsBpiCmtsAuthReplies  OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CMTS has
transmitted an Authorization Reply message to any CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.2."
::= { docsBpiCmtsBaseEntry 6 }

docsBpiCmtsAuthRejects  OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CMTS has





transmitted an Authorization Reject message to any CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.3."
::= { docsBpiCmtsBaseEntry 7 }

docsBpiCmtsAuthInvalids OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CMTS has
transmitted an Authorization Invalid message to any CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.7."
::= { docsBpiCmtsBaseEntry 8 }

--
-- The CMTS Authorization Table, indexed by ifIndex and CM MAC address
--

docsBpiCmtsAuthTable    OBJECT-TYPE
SYNTAX                  SEQUENCE OF     DocsBpiCmtsAuthEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"This table describes the attributes of each CM authorization
association. The CMTS maintains one authorization association with
each Baseline Privacy-enabled CM on each CMTS MAC interface."
::= { docsBpiCmtsObjects 2 }

docsBpiCmtsAuthEntry    OBJECT-TYPE
SYNTAX                  DocsBpiCmtsAuthEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"Each entry contains objects describing attributes of one
authorization association. The CMTS MUST create one entry per CM per
MAC interface, based on the receipt of an Authorization Request
message, and MUST not delete the entry before the CM authorization
permanently expires."
INDEX                   { ifIndex, docsBpiCmtsAuthCmMacAddress }
::= { docsBpiCmtsAuthTable 1 }

DocsBpiCmtsAuthEntry ::= SEQUENCE {
docsBpiCmtsAuthCmMacAddress             MacAddress,
docsBpiCmtsAuthCmPublicKey              OCTET STRING,
docsBpiCmtsAuthCmKeySequenceNumber      Integer32,
docsBpiCmtsAuthCmExpires                DateAndTime,





docsBpiCmtsAuthCmLifetime               Integer32,
docsBpiCmtsAuthCmGraceTime              Integer32,
docsBpiCmtsAuthCmReset                  INTEGER,
docsBpiCmtsAuthCmRequests               Counter32,
docsBpiCmtsAuthCmReplies                Counter32,
docsBpiCmtsAuthCmRejects                Counter32,
docsBpiCmtsAuthCmInvalids               Counter32,
docsBpiCmtsAuthRejectErrorCode          INTEGER,
docsBpiCmtsAuthRejectErrorString        DisplayString,
docsBpiCmtsAuthInvalidErrorCode         INTEGER,
docsBpiCmtsAuthInvalidErrorString       DisplayString
}

docsBpiCmtsAuthCmMacAddress     OBJECT-TYPE
SYNTAX                          MacAddress
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION
"The value of this object is the physical address of the CM to
which the authorization association applies."
::= { docsBpiCmtsAuthEntry 1 }

docsBpiCmtsAuthCmPublicKey      OBJECT-TYPE
SYNTAX                          OCTET STRING
                                (SIZE (0 | 74 | 106 | 140 | 270))
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is a DER-encoded RSAPublicKey ASN.1 type
string, as defined in the RSA Encryption Standard (PKCS #1) [22],
corresponding to the public key of the CM. The 74, 106, 140, and
270 byte key encoding lengths correspond to 512 bit, 768 bit, 1024
bit, and 2048 public moduli respectively. This is a zero-length
string if the CMTS does not retain the public key."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.2.4."
::= { docsBpiCmtsAuthEntry 2 }

docsBpiCmtsAuthCmKeySequenceNumber      OBJECT-TYPE
SYNTAX                                  Integer32 (0..15)
MAX-ACCESS                              read-only
STATUS                                  current
DESCRIPTION
"The value of this object is the authorization key sequence number
for this CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.2
and 4.2.2.10."





::= { docsBpiCmtsAuthEntry 3 }

docsBpiCmtsAuthCmExpires        OBJECT-TYPE
SYNTAX                          DateAndTime
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the actual clock time when the current
authorization for this CM expires. If this CM does not have an
active authorization, then the value is of the expiration date and
time of the last active authorization."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.2
and 4.2.2.9."
::= { docsBpiCmtsAuthEntry 4 }

docsBpiCmtsAuthCmLifetime       OBJECT-TYPE
SYNTAX                          Integer32 (1..6048000)
UNITS                           "seconds"
MAX-ACCESS                      read-write
STATUS                          current
DESCRIPTION
"The value of this object is the lifetime, in seconds, the CMTS
assigns to an authorization key for this CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.2
and Appendix A.2."
::= { docsBpiCmtsAuthEntry 5 }

docsBpiCmtsAuthCmGraceTime      OBJECT-TYPE
SYNTAX                          Integer32 (1..1800)
UNITS                           "seconds"
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the grace time for the authorization key
in seconds.  The CM is expected to start trying to get a new
authorization key beginning AuthGraceTime seconds before the
authorization key actually expires."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.3."
::= { docsBpiCmtsAuthEntry 6 }

docsBpiCmtsAuthCmReset  OBJECT-TYPE
SYNTAX                  INTEGER {
                                noResetRequested(1),
                                invalidateAuth(2),
                                sendAuthInvalid(3),





                                invalidateTeks(4)
                        }
MAX-ACCESS              read-write
STATUS                  current
DESCRIPTION
"Setting this object to invalidateAuth(2) causes the CMTS to
invalidate the current CM authorization key, but not to transmit an
Authorization Invalid message nor to invalidate unicast TEKs.  Setting
this object to sendAuthInvalid(3) causes the CMTS to invalidate the
current CM authorization key, and to transmit an Authorization Invalid
message to the CM, but not to invalidate unicast TEKs.  Setting this
object to invalidateTeks(4) causes the CMTS to invalidate the current
CM authorization key, to transmit an Authorization Invalid message to
the CM, and to invalidate all unicast TEKs associated with this CM
authorization. Reading this object returns the most-recently-set value
of this object, or returns noResetRequested(1) if the object has not
been set since the last CMTS reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.1.2.3.4,
4.1.2.3.5, and 4.1.3.3.5."
::= { docsBpiCmtsAuthEntry 7 }

docsBpiCmtsAuthCmRequests       OBJECT-TYPE
SYNTAX                          Counter32
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the count of times the CMTS has
received an Authorization Request message from this CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.1."
::= { docsBpiCmtsAuthEntry 8 }

docsBpiCmtsAuthCmReplies        OBJECT-TYPE
SYNTAX                          Counter32
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the count of times the CMTS has
transmitted an Authorization Reply message to this CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.2."
::= { docsBpiCmtsAuthEntry 9 }

docsBpiCmtsAuthCmRejects        OBJECT-TYPE
SYNTAX                          Counter32
MAX-ACCESS                      read-only
STATUS                          current





DESCRIPTION
"The value of this object is the count of times the CMTS has
transmitted an Authorization Reject message to this CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.3."
::= { docsBpiCmtsAuthEntry 10 }

docsBpiCmtsAuthCmInvalids       OBJECT-TYPE
SYNTAX                          Counter32
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the count of times the CMTS has
transmitted an Authorization Invalid message to this CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.7."
::= { docsBpiCmtsAuthEntry 11 }

docsBpiCmtsAuthRejectErrorCode  OBJECT-TYPE
SYNTAX                  INTEGER {
                                none(1),
                                unknown(2),
                                unauthorizedCm(3),
                                unauthorizedSid(4)
                        }
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the enumerated description of the
Error-Code in most recent Authorization Reject message transmitted to
the CM.  This has value unknown(2) if the last Error-Code value was
0, and none(1) if no Authorization Reject message has been transmitted
to the CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.3
and 4.2.2.16."
::= { docsBpiCmtsAuthEntry 12 }

docsBpiCmtsAuthRejectErrorString        OBJECT-TYPE
SYNTAX                                  DisplayString (SIZE (0..128))
MAX-ACCESS                              read-only
STATUS                                  current
DESCRIPTION
"The value of this object is the Display-String in most recent
Authorization Reject message transmitted to the CM.  This is a
zero length string if no Authorization Reject message has been
transmitted to the CM."
REFERENCE





"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.3
and 4.2.2.6."
::= { docsBpiCmtsAuthEntry 13 }

docsBpiCmtsAuthInvalidErrorCode OBJECT-TYPE
SYNTAX                  INTEGER {
                                none(1),
                                unknown(2),
                                unauthorizedCm(3),
                                unsolicited(5),
                                invalidKeySequence(6),
                                keyRequestAuthenticationFailure(7)
                        }
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the enumerated description of the
Error-Code in most recent Authorization Invalid message transmitted
to the CM.  This has value unknown(2) if the last Error-Code value was
0, and none(1) if no Authorization Invalid message has been
transmitted to the CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.7
and 4.2.2.16."
::= { docsBpiCmtsAuthEntry 14 }

docsBpiCmtsAuthInvalidErrorString       OBJECT-TYPE
SYNTAX                                  DisplayString (SIZE (0..128))
MAX-ACCESS                              read-only
STATUS                                  current
DESCRIPTION
"The value of this object is the Display-String in most recent
Authorization Invalid message transmitted to the CM.  This is a
zero length string if no Authorization Invalid message has been
transmitted to the CM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.7
and 4.2.2.6."
::= { docsBpiCmtsAuthEntry 15 }

--
-- The CMTS TEK Table, indexed by ifIndex and SID
--

docsBpiCmtsTEKTable     OBJECT-TYPE
SYNTAX                  SEQUENCE OF     DocsBpiCmtsTEKEntry
MAX-ACCESS              not-accessible
STATUS                  current





DESCRIPTION
"This table describes the attributes of each CM Traffic Encryption
Key (TEK) association. The CMTS maintains one TEK association per BPI
SID on each CMTS MAC interface."
::= { docsBpiCmtsObjects 3 }

docsBpiCmtsTEKEntry     OBJECT-TYPE
SYNTAX                  DocsBpiCmtsTEKEntry
MAX-ACCESS              not-accessible
STATUS                  current
DESCRIPTION
"Each entry contains objects describing attributes of one TEK
association on a particular CMTS MAC interface. The CMTS MUST create
one entry per SID per MAC interface, based on the receipt of an
Key Request message, and MUST not delete the entry before the CM
authorization for the SID permanently expires."
INDEX                   { ifIndex, docsIfCmtsServiceId }
::= { docsBpiCmtsTEKTable 1 }

DocsBpiCmtsTEKEntry ::= SEQUENCE {
docsBpiCmtsTEKLifetime                  Integer32,
docsBpiCmtsTEKGraceTime                 Integer32,
docsBpiCmtsTEKExpiresOld                DateAndTime,
docsBpiCmtsTEKExpiresNew                DateAndTime,
docsBpiCmtsTEKReset                     TruthValue,
docsBpiCmtsKeyRequests                  Counter32,
docsBpiCmtsKeyReplies                   Counter32,
docsBpiCmtsKeyRejects                   Counter32,
docsBpiCmtsTEKInvalids                  Counter32,
docsBpiCmtsKeyRejectErrorCode           INTEGER,
docsBpiCmtsKeyRejectErrorString         DisplayString,
docsBpiCmtsTEKInvalidErrorCode          INTEGER,
docsBpiCmtsTEKInvalidErrorString        DisplayString
}

docsBpiCmtsTEKLifetime  OBJECT-TYPE
SYNTAX                  Integer32 (1..604800)
UNITS                   "seconds"
MAX-ACCESS              read-write
STATUS                  current
DESCRIPTION
"The value of this object is the lifetime, in seconds, the CMTS assigns
to keys for this TEK association."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.5
and Appendix A.2."
::= { docsBpiCmtsTEKEntry 1 }






docsBpiCmtsTEKGraceTime OBJECT-TYPE
SYNTAX                  Integer32 (1..1800)
UNITS                   "seconds"
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the grace time for the TEK in seconds.
The CM is expected to start trying to get a new TEK beginning
TEKGraceTime seconds before the TEK actually expires."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Appendix A.1.1.1.6."
::= { docsBpiCmtsTEKEntry 2 }

docsBpiCmtsTEKExpiresOld        OBJECT-TYPE
SYNTAX                  DateAndTime
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the actual clock time for expiration
of the immediate predecessor of the most recent TEK for this FSM.
If this FSM has only one TEK, then the value is the time of activation
of this FSM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.5
and 4.2.2.9."
::= { docsBpiCmtsTEKEntry 3 }

docsBpiCmtsTEKExpiresNew        OBJECT-TYPE
SYNTAX                          DateAndTime
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the actual clock time for expiration
of the most recent TEK for this FSM."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.5
and 4.2.2.9."
::= { docsBpiCmtsTEKEntry 4 }

docsBpiCmtsTEKReset     OBJECT-TYPE
SYNTAX                  TruthValue
MAX-ACCESS              read-write
STATUS                  current
DESCRIPTION
"Setting this object to TRUE causes the CMTS to invalidate the current
active TEK(s) (plural due to key transition periods), and to generate
a new TEK for the associated SID; the CMTS MAY also generate an
unsolicited TEK Invalid message, to optimize the TEK synchronization





between the CMTS and the CM. Reading this object always returns
FALSE."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.1.3.3.5."
::= { docsBpiCmtsTEKEntry 5 }

docsBpiCmtsKeyRequests  OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CMTS has
received a Key Request message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.4."
::= { docsBpiCmtsTEKEntry 6 }

docsBpiCmtsKeyReplies   OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CMTS has
transmitted a Key Reply message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.5."
::= { docsBpiCmtsTEKEntry 7 }

docsBpiCmtsKeyRejects   OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CMTS has
transmitted a Key Reject message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.6."
::= { docsBpiCmtsTEKEntry 8 }

docsBpiCmtsTEKInvalids  OBJECT-TYPE
SYNTAX                  Counter32
MAX-ACCESS              read-only
STATUS                  current
DESCRIPTION
"The value of this object is the count of times the CMTS has
transmitted a TEK Invalid message."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Section 4.2.1.8."





::= { docsBpiCmtsTEKEntry 9 }

docsBpiCmtsKeyRejectErrorCode   OBJECT-TYPE
SYNTAX                          INTEGER {
                                        none(1),
                                        unknown(2),
                                        unauthorizedSid(4)
                                }
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the enumerated description of the
Error-Code in the most recent Key Reject message sent in response to
a Key Request for this BPI SID. This has value unknown(2) if the last
Error-Code value was 0, and none(1) if no Key Reject message has been
received since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.6
and 4.2.2.16."
::= { docsBpiCmtsTEKEntry 10 }

docsBpiCmtsKeyRejectErrorString OBJECT-TYPE
SYNTAX                          DisplayString (SIZE (0..128))
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the Display-String in the most recent
Key Reject message sent in response to a Key Request for this BPI
SID.  This is a zero length string if no Key Reject message has been
received since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.6
and 4.2.2.6."
::= { docsBpiCmtsTEKEntry 11 }

docsBpiCmtsTEKInvalidErrorCode  OBJECT-TYPE
SYNTAX                          INTEGER {
                                        none(1),
                                        unknown(2),
                                        invalidKeySequence(6)
                                }
MAX-ACCESS                      read-only
STATUS                          current
DESCRIPTION
"The value of this object is the enumerated description of the
Error-Code in the most recent TEK Invalid message sent in association
with this BPI SID.  This has value unknown(2) if the last Error-Code
value was 0, and none(1) if no TEK Invalid message has been received





since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.8
and 4.2.2.16."
::= { docsBpiCmtsTEKEntry 12 }

docsBpiCmtsTEKInvalidErrorString        OBJECT-TYPE
SYNTAX                                  DisplayString (SIZE (0..128))
MAX-ACCESS                              read-only
STATUS                                  current
DESCRIPTION
"The value of this object is the Display-String in the most recent TEK
Invalid message sent in association with this BPI SID.  This is a zero
length string if no TEK Invalid message has been received since reboot."
REFERENCE
"DOCSIS Baseline Privacy Interface Specification, Sections 4.2.1.8
and 4.2.2.6."
::= { docsBpiCmtsTEKEntry 13 }

--
-- The CMTS Multicast Control Group
--

docsBpiMulticastControl OBJECT IDENTIFIER ::= { docsBpiCmtsObjects 4 }

--
-- The CMTS IP Multicast Mapping Table, indexed by IP multicast
-- address and prefix, and by ifindex
--

docsBpiIpMulticastMapTable      OBJECT-TYPE
SYNTAX                          SEQUENCE OF DocsBpiIpMulticastMapEntry
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION
"This table describes the mapping of IP multicast address prefixes to
multicast SIDs on each CMTS MAC interface."
::= { docsBpiMulticastControl 1 }

docsBpiIpMulticastMapEntry      OBJECT-TYPE
SYNTAX                          DocsBpiIpMulticastMapEntry
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION
"Each entry contains objects describing the mapping of one IP
multicast address prefix to one multicast SID on one CMTS MAC
interface. The CMTS uses the mapping when forwarding downstream IP
multicast traffic."





INDEX                           { ifIndex, docsBpiIpMulticastAddress,
                                  docsBpiIpMulticastPrefixLength }
::= { docsBpiIpMulticastMapTable 1 }

DocsBpiIpMulticastMapEntry ::= SEQUENCE {
docsBpiIpMulticastAddress       IpAddress,
docsBpiIpMulticastPrefixLength  Integer32,
docsBpiIpMulticastServiceId     Integer32,
docsBpiIpMulticastMapControl    RowStatus
}

docsBpiIpMulticastAddress       OBJECT-TYPE
SYNTAX                          IpAddress
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION
"This object represents the IP multicast address (prefix) to be
mapped by this row, in conjunction with
docsBpiIpMulticastPrefixLength."
::= { docsBpiIpMulticastMapEntry 1 }

docsBpiIpMulticastPrefixLength  OBJECT-TYPE
SYNTAX                          Integer32 (0..32)
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION
"This object represents the IP multicast address prefix length
for this row. The value of this object represents the length in
bits of docsBpiIpMulticastAddress for multicast address
comparisons, using big-endian ordering. An IP multicast address
matches this row if the (docsBpiIpMulticastPrefixLength) most
significant bits of the IP multicast address and of the
(docsBpiIpMulticastAddress) are identical.
This object is similar in usage to an IP address mask. The value
0 corresponds to IP address mask 0.0.0.0, the value 1 corresponds
to IP address mask 128.0.0.0, the value 8 corresponds to IP
address mask 255.0.0.0, and the value 32 corresponds to IP
address mask 255.255.255.255."
::= { docsBpiIpMulticastMapEntry 2 }

docsBpiIpMulticastServiceId     OBJECT-TYPE
SYNTAX                          Integer32 (8192..16368)
MAX-ACCESS                      read-create
STATUS                          current
DESCRIPTION
"This object represents the multicast SID to be used in this
IP multicast address prefix mapping entry."
-- DEFVAL is an unused multicast SID value chosen by CMTS.





::= { docsBpiIpMulticastMapEntry 3 }

docsBpiIpMulticastMapControl    OBJECT-TYPE
SYNTAX                          RowStatus
MAX-ACCESS                      read-create
STATUS                          current
DESCRIPTION
"This object controls and reflects the IP multicast address prefix
mapping entry. There is no restriction on the ability to change values
in this row while the row is active."
::= { docsBpiIpMulticastMapEntry 4 }

--
-- The CMTS Multicast SID Authorization Table, indexed by ifIndex by
-- multicast SID by CM MAC address
--

docsBpiMulticastAuthTable       OBJECT-TYPE
SYNTAX                          SEQUENCE OF DocsBpiMulticastAuthEntry
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION
"This table describes the multicast SID authorization for each
CM on each CMTS MAC interface."
::= { docsBpiMulticastControl 2 }

docsBpiMulticastAuthEntry       OBJECT-TYPE
SYNTAX                          DocsBpiMulticastAuthEntry
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION
"Each entry contains objects describing the key authorization of one
cable modem for one multicast SID for one CMTS MAC interface."
INDEX                           { ifIndex, docsBpiMulticastServiceId,
                                  docsBpiMulticastCmMacAddress }
::= { docsBpiMulticastAuthTable 1 }

DocsBpiMulticastAuthEntry ::= SEQUENCE {
docsBpiMulticastServiceId       Integer32,
docsBpiMulticastCmMacAddress    MacAddress,
docsBpiMulticastAuthControl     RowStatus
}

docsBpiMulticastServiceId       OBJECT-TYPE
SYNTAX                          Integer32 (8192..16368)
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION





"This object represents the multicast SID for authorization."
::= { docsBpiMulticastAuthEntry 1 }

docsBpiMulticastCmMacAddress    OBJECT-TYPE
SYNTAX                          MacAddress
MAX-ACCESS                      not-accessible
STATUS                          current
DESCRIPTION
"This object represents the MAC address of the CM to which the
multicast SID authorization applies."
::= { docsBpiMulticastAuthEntry 2 }

docsBpiMulticastAuthControl     OBJECT-TYPE
SYNTAX                          RowStatus
MAX-ACCESS                      read-create
STATUS                          current
DESCRIPTION
"This object controls and reflects the CM authorization for each
multicast SID. There is no restriction on the ability to change
values in this row while the row is active."
::= { docsBpiMulticastAuthEntry 3 }

--
-- The BPI MIB Conformance Statements (with a placeholder for
-- notifications)
--

docsBpiNotification     OBJECT IDENTIFIER ::= { docsBpiMIB 2 }
docsBpiConformance      OBJECT IDENTIFIER ::= { docsBpiMIB 3 }
docsBpiCompliances      OBJECT IDENTIFIER ::= { docsBpiConformance 1 }
docsBpiGroups           OBJECT IDENTIFIER ::= { docsBpiConformance 2 }

docsBpiBasicCompliance MODULE-COMPLIANCE
STATUS          current
DESCRIPTION
"This is the compliance statement for devices which implement the
DOCSIS Baseline Privacy Interface."

MODULE  -- docsBpiMIB

-- conditionally mandatory group
GROUP   docsBpiCmGroup
DESCRIPTION
"This group is implemented only in CMs, not in CMTSs."

-- conditionally mandatory group
GROUP   docsBpiCmtsGroup
DESCRIPTION





"This group is implemented only in CMTSs, not in CMs."

-- relaxation on mandatory range (unnecessary since object is read-only)
-- OBJECT       docsBpiCmAuthGraceTime
-- SYNTAX       Integer32 (300..1800)
-- DESCRIPTION
-- "The refined range corresponds to the minimum and maximum values in
-- operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range (unnecessary since object is read-only)
-- OBJECT       docsBpiCmTEKGraceTime
-- SYNTAX       Integer32 (300..1800)
-- DESCRIPTION
-- "The refined range corresponds to the minimum and maximum values in
-- operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range
OBJECT  docsBpiCmtsDefaultAuthLifetime
SYNTAX  Integer32 (86400..6048000)
DESCRIPTION
"The refined range corresponds to the minimum and maximum values in
operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range
OBJECT  docsBpiCmtsDefaultTEKLifetime
SYNTAX  Integer32 (1800..604800)
DESCRIPTION
"The refined range corresponds to the minimum and maximum values in
operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range (object removed from MIB)
-- OBJECT       docsBpiCmtsDefaultAuthGraceTime
-- SYNTAX       INTEGER (300..1800)
-- DESCRIPTION
-- "The refined range corresponds to the minimum and maximum values in
-- operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range  (object removed from MIB)
-- OBJECT       docsBpiCmtsDefaultTEKGraceTime
-- SYNTAX       INTEGER (300..1800)
-- DESCRIPTION
-- "The refined range corresponds to the minimum and maximum values in
-- operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range
OBJECT  docsBpiCmtsAuthCmLifetime
SYNTAX  Integer32 (86400..6048000)
DESCRIPTION





"The refined range corresponds to the minimum and maximum values in
operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range (unnecessary since object is read-only)
-- OBJECT       docsBpiCmtsAuthCmGraceTime
-- SYNTAX       Integer32 (300..1800)
-- DESCRIPTION
-- "The refined range corresponds to the minimum and maximum values in
-- operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range
OBJECT  docsBpiCmtsTEKLifetime
SYNTAX  Integer32 (1800..604800)
DESCRIPTION
"The refined range corresponds to the minimum and maximum values in
operational networks, according to Appendix A.2 in [18]."

-- relaxation on mandatory range (unnecessary since object is read-only)
-- OBJECT       docsBpiCmtsTEKGraceTime
-- SYNTAX       Integer32 (300..1800)
-- DESCRIPTION
-- "The refined range corresponds to the minimum and maximum values in
-- operational networks, according to Appendix A.2 in [18]."

::= { docsBpiCompliances 1 }

docsBpiCmGroup  OBJECT-GROUP
OBJECTS {
docsBpiCmPrivacyEnable,
docsBpiCmPublicKey,
docsBpiCmAuthState,
docsBpiCmAuthKeySequenceNumber,
docsBpiCmAuthExpires,
docsBpiCmAuthReset,
docsBpiCmAuthGraceTime,
docsBpiCmTEKGraceTime,
docsBpiCmAuthWaitTimeout,
docsBpiCmReauthWaitTimeout,
docsBpiCmOpWaitTimeout,
docsBpiCmRekeyWaitTimeout,
docsBpiCmAuthRejectWaitTimeout,
docsBpiCmAuthRequests,
docsBpiCmAuthReplies,
docsBpiCmAuthRejects,
docsBpiCmAuthInvalids,
docsBpiCmAuthRejectErrorCode,
docsBpiCmAuthRejectErrorString,
docsBpiCmAuthInvalidErrorCode,





docsBpiCmAuthInvalidErrorString,
docsBpiCmTEKPrivacyEnable,
docsBpiCmTEKState,
docsBpiCmTEKExpiresOld,
docsBpiCmTEKExpiresNew,
docsBpiCmTEKKeyRequests,
docsBpiCmTEKKeyReplies,
docsBpiCmTEKKeyRejects,
docsBpiCmTEKInvalids,
docsBpiCmTEKAuthPends,
docsBpiCmTEKKeyRejectErrorCode,
docsBpiCmTEKKeyRejectErrorString,
docsBpiCmTEKInvalidErrorCode,
docsBpiCmTEKInvalidErrorString
}
STATUS                  current
DESCRIPTION
"This collection of objects provides CM BPI status and control."
::= { docsBpiGroups 1 }

docsBpiCmtsGroup        OBJECT-GROUP
OBJECTS {
docsBpiCmtsDefaultAuthLifetime,
docsBpiCmtsDefaultTEKLifetime,
docsBpiCmtsAuthRequests,
docsBpiCmtsAuthReplies,
docsBpiCmtsAuthRejects,
docsBpiCmtsAuthInvalids,
docsBpiCmtsAuthCmPublicKey,
docsBpiCmtsAuthCmKeySequenceNumber,
docsBpiCmtsAuthCmExpires,
docsBpiCmtsAuthCmLifetime,
docsBpiCmtsAuthCmGraceTime,
docsBpiCmtsAuthCmReset,
docsBpiCmtsAuthCmRequests,
docsBpiCmtsAuthCmReplies,
docsBpiCmtsAuthCmRejects,
docsBpiCmtsAuthCmInvalids,
docsBpiCmtsAuthRejectErrorCode,
docsBpiCmtsAuthRejectErrorString,
docsBpiCmtsAuthInvalidErrorCode,
docsBpiCmtsAuthInvalidErrorString,
docsBpiCmtsTEKLifetime,
docsBpiCmtsTEKGraceTime,
docsBpiCmtsTEKExpiresOld,
docsBpiCmtsTEKExpiresNew,
docsBpiCmtsTEKReset,
docsBpiCmtsKeyRequests,





docsBpiCmtsKeyReplies,
docsBpiCmtsKeyRejects,
docsBpiCmtsTEKInvalids,
docsBpiCmtsKeyRejectErrorCode,
docsBpiCmtsKeyRejectErrorString,
docsBpiCmtsTEKInvalidErrorCode,
docsBpiCmtsTEKInvalidErrorString,
docsBpiIpMulticastServiceId,
docsBpiIpMulticastMapControl,
docsBpiMulticastAuthControl
}
STATUS          current
DESCRIPTION
"This collection of objects provides CMTS BPI status and control."
::= { docsBpiGroups 2 }

docsBpiObsoleteObjectsGroup     OBJECT-GROUP
OBJECTS {
docsBpiCmtsDefaultAuthGraceTime,
docsBpiCmtsDefaultTEKGraceTime
}
STATUS          obsolete
DESCRIPTION
"This is a collection of obsolete BPI objects."
::= { docsBpiGroups 3 }

END


