RAQMON-RDS-MIB DEFINITIONS ::= BEGIN


      IMPORTS
          MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
          Counter32, Unsigned32
              FROM SNMPv2-SMI

          DateAndTime
              FROM SNMPv2-TC

          rmon
              FROM RMON-MIB

          SnmpAdminString
              FROM SNMP-FRAMEWORK-MIB

          InetAddressType, InetAddress, InetPortNumber
              FROM INET-ADDRESS-MIB

          Dscp
              FROM DIFFSERV-DSCP-TC

          MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
              FROM SNMPv2-CONF;

      raqmonDsMIB MODULE-IDENTITY
          LAST-UPDATED "200610100000Z"      -- October 10, 2006
          ORGANIZATION "RMON Working Group"
          CONTACT-INFO
              "WG EMail: rmonmib@ietf.org
               Subscribe: rmonmib-request@ietf.org

               MIB Editor:
               Eugene Golovinsky
               Postal: BMC Software, Inc.
                       2101 CityWest Boulevard,





                       Houston, TX, 77094
                       USA
               Tel:    +713-918-1816
               Email:  egolovin@bmc.com
              "
          DESCRIPTION
              "This is the RAQMON Data Source notification MIB Module.
               It provides a mapping of RAQMON PDUs to SNMP
               notifications.

               Ds stands for data source.

               Note that all of the object types defined in this module
               are accessible-for-notify and would consequently not be
               available to a browser using simple Get, GetNext, or
               GetBulk requests.

               Copyright (c) The Internet Society (2006).

               This version of this MIB module is part of RFC 4712;
               See the RFC itself for full legal notices."

          REVISION      "200610100000Z"     -- October 10, 2006
          DESCRIPTION
              "Initial version, published as RFC 4712."

                 ::= { rmon 32 }

   -- This OID allocation conforms to [RFC3737]


      raqmonDsNotifications OBJECT IDENTIFIER ::= { raqmonDsMIB 0 }
      raqmonDsMIBObjects OBJECT IDENTIFIER ::= { raqmonDsMIB 1 }
      raqmonDsConformance OBJECT IDENTIFIER ::= { raqmonDsMIB 2 }

      raqmonDsNotificationTable OBJECT-TYPE
          SYNTAX SEQUENCE OF RaqmonDsNotificationEntry
          MAX-ACCESS not-accessible
          STATUS     current
          DESCRIPTION
              "This conceptual table provides the SNMP mapping of
               the RAQMON BASIC PDU.  It is indexed by the RAQMON
               Data Source, sub-session, and address of the peer
               entity.

               Note that there is no concern about the indexation of
               this table exceeding the limits defined by RFC 2578
               Section 3.5.  According to [RFC4710], Section 5.1,





               only IPv4 and IPv6 addresses can be reported as
               participant addresses."
          ::= { raqmonDsMIBObjects 1 }

      raqmonDsNotificationEntry OBJECT-TYPE
          SYNTAX     RaqmonDsNotificationEntry
          MAX-ACCESS not-accessible
          STATUS     current
          DESCRIPTION
              "The entry (row) is not retrievable and is not kept by
               RDSs.  It serves data organization purposes only."
          INDEX { raqmonDsDSRC, raqmonDsRCN, raqmonDsPeerAddrType,
                  raqmonDsPeerAddr }
          ::= { raqmonDsNotificationTable 1 }

      RaqmonDsNotificationEntry ::= SEQUENCE {
              raqmonDsDSRC                      Unsigned32,
              raqmonDsRCN                       Unsigned32,
              raqmonDsPeerAddrType              InetAddressType,
              raqmonDsPeerAddr                  InetAddress,
              raqmonDsAppName                   SnmpAdminString,
              raqmonDsDataSourceDevicePort      InetPortNumber,
              raqmonDsReceiverDevicePort        InetPortNumber,
              raqmonDsSessionSetupDateTime      DateAndTime,
              raqmonDsSessionSetupDelay         Unsigned32,
              raqmonDsSessionDuration           Unsigned32,
              raqmonDsSessionSetupStatus        SnmpAdminString,
              raqmonDsRoundTripEndToEndNetDelay Unsigned32,
              raqmonDsOneWayEndToEndNetDelay    Unsigned32,
              raqmonDsApplicationDelay          Unsigned32,
              raqmonDsInterArrivalJitter        Unsigned32,
              raqmonDsIPPacketDelayVariation    Unsigned32,
              raqmonDsTotalPacketsReceived      Counter32,
              raqmonDsTotalPacketsSent          Counter32,
              raqmonDsTotalOctetsReceived       Counter32,
              raqmonDsTotalOctetsSent           Counter32,
              raqmonDsCumulativePacketLoss      Counter32,
              raqmonDsPacketLossFraction        Unsigned32,
              raqmonDsCumulativeDiscards        Counter32,
              raqmonDsDiscardsFraction          Unsigned32,
              raqmonDsSourcePayloadType         Unsigned32,
              raqmonDsReceiverPayloadType       Unsigned32,
              raqmonDsSourceLayer2Priority      Unsigned32,
              raqmonDsSourceDscp                Dscp,
              raqmonDsDestinationLayer2Priority Unsigned32,
              raqmonDsDestinationDscp           Dscp,
              raqmonDsCpuUtilization            Unsigned32,
              raqmonDsMemoryUtilization         Unsigned32 }





      raqmonDsDSRC OBJECT-TYPE
          SYNTAX     Unsigned32
          MAX-ACCESS not-accessible
          STATUS     current
          DESCRIPTION
              "Data Source identifier represents a unique session
               descriptor that points to a specific session
               between communicating entities.  Identifiers unique for
               sessions conducted between two entities are
               generated by the communicating entities.  Zero is a
               valid value, with no special semantics."
          ::= { raqmonDsNotificationEntry 1 }

      raqmonDsRCN OBJECT-TYPE
           SYNTAX      Unsigned32 (0..15)
           MAX-ACCESS  not-accessible
           STATUS      current
           DESCRIPTION
               "The Record Count Number indicates a sub-session
                within a communication session.  A maximum number of 16
                sub-sessions are supported; this limitation is
                dictated by reasons of compatibility with other
                transport protocols."
           ::= { raqmonDsNotificationEntry 2 }

      raqmonDsPeerAddrType OBJECT-TYPE
          SYNTAX InetAddressType
          MAX-ACCESS not-accessible
          STATUS current
          DESCRIPTION
              "The type of the Internet address of the peer participant
               for this session."
          REFERENCE
              "Section 5.2 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 3 }

      raqmonDsPeerAddr OBJECT-TYPE
          SYNTAX InetAddress
          MAX-ACCESS not-accessible
          STATUS current
          DESCRIPTION
              "The Internet Address of the peer participant for this
               session."
          REFERENCE
              "Section 5.2 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 4 }

      raqmonDsAppName  OBJECT-TYPE





          SYNTAX     SnmpAdminString
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "This is a text string giving the name and possibly the
               version of the application associated with that session,
               e.g., 'XYZ VoIP Agent 1.2'."
          REFERENCE
              "Section 5.28 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 5 }

      raqmonDsDataSourceDevicePort OBJECT-TYPE
          SYNTAX     InetPortNumber
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The port number from which data for this session was sent
               by the Data Source device."
          REFERENCE
              "Section 5.5 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 6 }

      raqmonDsReceiverDevicePort OBJECT-TYPE
          SYNTAX     InetPortNumber
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The port number where the data for this session was
               received."
          REFERENCE
              "Section 5.6 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 7 }

      raqmonDsSessionSetupDateTime OBJECT-TYPE
          SYNTAX     DateAndTime
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The time when session was initiated."
          REFERENCE
              "Section 5.7 of [RFC4710]"
      ::= { raqmonDsNotificationEntry 8 }

      raqmonDsSessionSetupDelay OBJECT-TYPE
          SYNTAX     Unsigned32 (0..65535)
          UNITS      "milliseconds"
          MAX-ACCESS accessible-for-notify
          STATUS     current





          DESCRIPTION
              "Session setup time."
          REFERENCE
              "Section 5.8 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 9 }

      raqmonDsSessionDuration OBJECT-TYPE
          SYNTAX     Unsigned32
          UNITS      "seconds"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Session duration, including setup time.  The SYNTAX of
               this object allows expression of the duration of sessions
               that do not exceed 4660 hours and 20 minutes."
          REFERENCE
              "Section 5.9 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 10 }

      raqmonDsSessionSetupStatus OBJECT-TYPE
          SYNTAX     SnmpAdminString
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Describes appropriate communication session states, e.g.,
               Call Established successfully, RSVP reservation
               failed, etc."
          REFERENCE
              "Section 5.10 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 11 }

      raqmonDsRoundTripEndToEndNetDelay OBJECT-TYPE
          SYNTAX     Unsigned32
          UNITS      "milliseconds"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Most recent available information about the
               round-trip end-to-end network delay."
          REFERENCE
              "Section 5.11 of [RFC4710]"
          ::= { raqmonDsNotificationEntry  12}

      raqmonDsOneWayEndToEndNetDelay OBJECT-TYPE
          SYNTAX     Unsigned32
          UNITS      "milliseconds"
          MAX-ACCESS accessible-for-notify
          STATUS     current





          DESCRIPTION
              "Most recent available information about the
               one-way end-to-end network delay."
          REFERENCE
              "Section 5.12 of [RFC4710]"
          ::= { raqmonDsNotificationEntry  13}

      raqmonDsApplicationDelay OBJECT-TYPE
          SYNTAX     Unsigned32  (0..65535)
          UNITS      "milliseconds"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Most recent available information about the
               application delay."
          REFERENCE
              "Section 5.13 of [RFC4710"
          ::= { raqmonDsNotificationEntry  14}

      raqmonDsInterArrivalJitter OBJECT-TYPE
          SYNTAX     Unsigned32  (0..65535)
          UNITS      "milliseconds"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "An estimate of the inter-arrival jitter."
          REFERENCE
              "Section 5.14 of [RFC4710]"
          ::= { raqmonDsNotificationEntry  15}

      raqmonDsIPPacketDelayVariation OBJECT-TYPE
          SYNTAX     Unsigned32  (0..65535)
          UNITS      "milliseconds"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "An estimate of the inter-arrival delay variation."
          REFERENCE
              "Section 5.15 of [RFC4710]"
          ::= { raqmonDsNotificationEntry  16}

      raqmonDsTotalPacketsReceived OBJECT-TYPE
          SYNTAX     Counter32
          UNITS     "packets"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The number of packets transmitted within a communication





               session by the receiver since the start of the session."
          REFERENCE
              "Section 5.16 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 17 }

      raqmonDsTotalPacketsSent OBJECT-TYPE
          SYNTAX     Counter32
          UNITS     "packets"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The number of packets transmitted within a communication
               session by the sender since the start of the session."
          REFERENCE
              "Section 5.17 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 18 }

      raqmonDsTotalOctetsReceived OBJECT-TYPE
          SYNTAX     Counter32
          UNITS      "octets"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The total number of payload octets (i.e., not including
               header or padding octets) transmitted in packets by the
               receiver within a communication session since the start
               of the session."
          REFERENCE
              "Section 5.18 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 19 }

      raqmonDsTotalOctetsSent OBJECT-TYPE
          SYNTAX     Counter32
          UNITS      "octets"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The number of payload octets (i.e., not including headers
               or padding) transmitted in packets by the sender within
               a communication sub-session since the start of the
               session."
          REFERENCE
              "Section 5.19 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 20 }

      raqmonDsCumulativePacketLoss OBJECT-TYPE
          SYNTAX     Counter32
          UNITS      "packets"





          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The number of packets from this session whose loss
               had been detected since the start of the session."
          REFERENCE
              "Section 5.20 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 21 }

      raqmonDsPacketLossFraction OBJECT-TYPE
          SYNTAX     Unsigned32 (0..100)
          UNITS      "percentage of packets sent"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The percentage of lost packets with respect to the
               overall packets sent.  This is defined to be 100 times
               the number of packets lost divided by the number of
               packets expected."
          REFERENCE
              "Section 5.21 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 22 }

      raqmonDsCumulativeDiscards OBJECT-TYPE
          SYNTAX     Counter32
          UNITS      "packets"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The number of packet discards detected since the
               start of the session."
          REFERENCE
              "Section 5.22 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 23 }

      raqmonDsDiscardsFraction OBJECT-TYPE
          SYNTAX     Unsigned32 (0..100)
          UNITS      "percentage of packets sent"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The percentage of discards with respect to the overall
               packets sent.  This is defined to be 100 times the number
               of discards divided by the number of packets expected."
          REFERENCE
              "Section 5.23 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 24 }






      raqmonDsSourcePayloadType OBJECT-TYPE
          SYNTAX     Unsigned32 (0..127)
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The payload type of the packet sent by this RDS."
          REFERENCE
              "RFC 1890, Section 5.24 of [RFC4710] "
          ::= { raqmonDsNotificationEntry 25 }

      raqmonDsReceiverPayloadType OBJECT-TYPE
          SYNTAX     Unsigned32 (0..127)
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "The payload type of the packet received by this RDS."
          REFERENCE
              "RFC 1890, Section 5.25 of [RFC4710] "
      ::= { raqmonDsNotificationEntry 26 }

      raqmonDsSourceLayer2Priority OBJECT-TYPE
          SYNTAX     Unsigned32 (0..7)
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Source Layer 2 priority used by the data source to send
               packets to the receiver by this data source during this
               communication session."
          REFERENCE
              "Section 5.26 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 27 }

      raqmonDsSourceDscp OBJECT-TYPE
          SYNTAX     Dscp
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Layer 3 TOS/DSCP values used by the Data Source to
               prioritize traffic sent."
          REFERENCE
              "Section 5.27 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 28 }

      raqmonDsDestinationLayer2Priority OBJECT-TYPE
          SYNTAX     Unsigned32 (0..7)
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION





              "Destination Layer 2 priority.  This is the priority used
               by the peer communicating entity to send packets to the
               data source."
          REFERENCE
              "Section 5.28 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 29 }

      raqmonDsDestinationDscp OBJECT-TYPE
          SYNTAX     Dscp
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Layer 3 TOS/DSCP values used by the
               peer communicating entity to prioritize traffic
               sent to the source."
          REFERENCE
              "Section 5.29 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 30 }

      raqmonDsCpuUtilization OBJECT-TYPE
          SYNTAX     Unsigned32 (0..100)
          UNITS      "percent"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Latest available information about the total CPU
               utilization."
          REFERENCE
              "Section 5.30 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 31 }

      raqmonDsMemoryUtilization OBJECT-TYPE
          SYNTAX     Unsigned32 (0..100)
          UNITS      "percent"
          MAX-ACCESS accessible-for-notify
          STATUS     current
          DESCRIPTION
              "Latest available information about the total memory
               utilization."
          REFERENCE
              "Section 5.31 of [RFC4710]"
          ::= { raqmonDsNotificationEntry 32 }

      -- definitions of the notifications
      --
      -- raqmonDsAppName is the only object that MUST be sent by an
      -- RDS every time the static notification is generated.






      -- raqmonDsTotalPacketsReceived is the only object that MUST be
      -- sent by an RD every time the dynamic notification is generated.

      -- Other objects from the raqmonDsNotificationTable may be
      -- included in the variable binding list.  Specifically, a raqmon
      -- notification will include MIB objects that provide information
      -- about metrics that characterize the application session

         raqmonDsStaticNotification NOTIFICATION-TYPE
          OBJECTS { raqmonDsAppName }
          STATUS current
          DESCRIPTION
              "This notification maps the static parameters in the
               BASIC RAQMON PDU onto an SNMP transport.
               This notification is expected to be sent once per
               session, or when a new sub-session is initiated.
               The following objects MAY be carried by the
               raqmonDsStaticNotification:

               raqmonDsDataSourceDevicePort,
               raqmonDsReceiverDevicePort,
               raqmonDsSessionSetupDateTime,
               raqmonDsSessionSetupDelay,
               raqmonDsSessionDuration,
               raqmonDsSourcePayloadType,
               raqmonDsReceiverPayloadType,
               raqmonDsSourceLayer2Priority,
               raqmonDsSourceDscp,
               raqmonDsDestinationLayer2Priority,
               raqmonDsDestinationDscp

               It is RECOMMENDED to keep the size of a notification
               within the MTU size limits in order to avoid
               fragmentation."
          ::= { raqmonDsNotifications  1 }

      raqmonDsDynamicNotification NOTIFICATION-TYPE
          OBJECTS { raqmonDsTotalPacketsReceived }
          STATUS current
          DESCRIPTION
              "This notification maps the dynamic parameters in the
               BASIC RAQMON PDU onto an SNMP transport.

               The following objects MAY be carried by the
               raqmonDsDynamicNotification:

               raqmonDsRoundTripEndToEndNetDelay,
               raqmonDsOneWayEndToEndNetDelay,





               raqmonDsApplicationDelay,
               raqmonDsInterArrivalJitter,
               raqmonDsIPPacketDelayVariation,
               raqmonDsTotalPacketsSent,
               raqmonDsTotalOctetsReceived,
               raqmonDsTotalOctetsSent,
               raqmonDsCumulativePacketLoss,
               raqmonDsPacketLossFraction,
               raqmonDsCumulativeDiscards,
               raqmonDsDiscardsFraction,
               raqmonDsCpuUtilization,
               raqmonDsMemoryUtilization

               It is RECOMMENDED to keep the size of a notification
               within the MTU size limits in order to avoid
               fragmentation."

          ::= { raqmonDsNotifications  2 }

      raqmonDsByeNotification NOTIFICATION-TYPE
          OBJECTS { raqmonDsAppName }
          STATUS current
          DESCRIPTION
              "The BYE Notification.  This Notification is the
               equivalent of the RAQMON NULL PDU, which signals the
               end of a RAQMON session."
          ::= { raqmonDsNotifications  3 }

      --
      -- conformance information
      raqmonDsCompliance OBJECT IDENTIFIER ::=
                                           { raqmonDsConformance 1 }
      raqmonDsGroups OBJECT IDENTIFIER ::= { raqmonDsConformance 2 }

   raqmonDsBasicCompliance MODULE-COMPLIANCE
           STATUS current
           DESCRIPTION
              "The compliance statement for SNMP entities that
               implement this MIB module.

               There are a number of INDEX objects that cannot be
               represented in the form of OBJECT clauses in SMIv2, but
               for which we have the following compliance requirements,
               expressed in OBJECT clause form in this description
               clause:

               -- OBJECT      raqmonDsPeerAddrType
               -- SYNTAX      InetAddressType { ipv4(1), ipv6(2) }





               -- DESCRIPTION
               --     This MIB requires support for only global IPv4
               --     and IPv6 address types.
               --
               -- OBJECT      raqmonDsPeerAddr
               -- SYNTAX      InetAddress (SIZE(4|16))
               -- DESCRIPTION
               --     This MIB requires support for only global IPv4
               --     and IPv6 address types.
               --
              "
           MODULE  -- this module
               MANDATORY-GROUPS { raqmonDsNotificationGroup,
                                  raqmonDsPayloadGroup }
           ::= { raqmonDsCompliance 1 }

      raqmonDsNotificationGroup NOTIFICATION-GROUP
          NOTIFICATIONS { raqmonDsStaticNotification,
                          raqmonDsDynamicNotification,
                          raqmonDsByeNotification }
          STATUS current
          DESCRIPTION
              "Standard RAQMON Data Source Notification group."
          ::= { raqmonDsGroups 1 }

      raqmonDsPayloadGroup OBJECT-GROUP
          OBJECTS { raqmonDsAppName,
                    raqmonDsDataSourceDevicePort,
                    raqmonDsReceiverDevicePort,
                    raqmonDsSessionSetupDateTime,
                    raqmonDsSessionSetupDelay,
                    raqmonDsSessionDuration,
                    raqmonDsSessionSetupStatus,
                    raqmonDsRoundTripEndToEndNetDelay,
                    raqmonDsOneWayEndToEndNetDelay,
                    raqmonDsApplicationDelay,
                    raqmonDsInterArrivalJitter,
                    raqmonDsIPPacketDelayVariation,
                    raqmonDsTotalPacketsReceived,
                    raqmonDsTotalPacketsSent,
                    raqmonDsTotalOctetsReceived,
                    raqmonDsTotalOctetsSent,
                    raqmonDsCumulativePacketLoss,
                    raqmonDsPacketLossFraction,
                    raqmonDsCumulativeDiscards,
                    raqmonDsDiscardsFraction,
                    raqmonDsSourcePayloadType,
                    raqmonDsReceiverPayloadType,





                    raqmonDsSourceLayer2Priority,
                    raqmonDsSourceDscp,
                    raqmonDsDestinationLayer2Priority,
                    raqmonDsDestinationDscp,
                    raqmonDsCpuUtilization,
                    raqmonDsMemoryUtilization }
          STATUS current
          DESCRIPTION
              "Standard RAQMON Data Source payload MIB objects group."
          ::= { raqmonDsGroups 2 }

      END


