TN3270E-RT-MIB DEFINITIONS ::= BEGIN


  IMPORTS
      MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
      Counter32, Unsigned32, Gauge32
                  FROM SNMPv2-SMI
      RowStatus, DateAndTime, TimeStamp, TestAndIncr
                  FROM SNMPv2-TC
      MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
                  FROM SNMPv2-CONF
      tn3270eSrvrConfIndex, tn3270eClientGroupName,
      tn3270eResMapElementType
                  FROM TN3270E-MIB
      IANATn3270eAddrType, IANATn3270eAddress
                  FROM IANATn3270eTC-MIB
      snanauMIB
                  FROM SNA-NAU-MIB;

    tn3270eRtMIB   MODULE-IDENTITY
        LAST-UPDATED "9807270000Z" -- July 27, 1998
        ORGANIZATION "TN3270E Working Group"
        CONTACT-INFO
          "Kenneth White (kennethw@vnet.ibm.com)
           IBM Corp. - Dept. BRQA/Bldg. 501/G114
           P.O. Box 12195





           3039 Cornwallis
           RTP, NC 27709-2195

           Robert Moore (remoore@us.ibm.com)
           IBM Corp. - Dept. BRQA/Bldg. 501/G114
           P.O. Box 12195
           3039 Cornwallis
           RTP, NC 27709-2195
           (919) 254-4436"
       DESCRIPTION
          "This module defines a portion of the management
          information base (MIB) that enables monitoring of
          TN3270 and TN3270E clients' response times by a
          TN3270E server."
       REVISION  "9807270000Z" -- July 27, 1998
       DESCRIPTION
           "RFC nnnn (Proposed Standard)" -- RFC Editor to fill in
  ::= { snanauMIB 9 }
  -- snanauMIB ::= { mib-2 34 }

  -- Top level structure of the MIB

  tn3270eRtNotifications   OBJECT IDENTIFIER  ::= { tn3270eRtMIB 0 }
  tn3270eRtObjects         OBJECT IDENTIFIER  ::= { tn3270eRtMIB 1 }
  tn3270eRtConformance     OBJECT IDENTIFIER  ::= { tn3270eRtMIB 3 }

  -- MIB Objects

  -- Response Time Control Table

  tn3270eRtCollCtlTable  OBJECT-TYPE
      SYNTAX       SEQUENCE OF Tn3270eRtCollCtlEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
        "The response time monitoring collection control table,
        which allows a management application to control the
        types of response time data being collected, and the
        clients for which it is being collected.

        This table is indexed by tn3270eSrvrConfIndex and
        tn3270eClientGroupName imported from the
        TN3270E-MIB.  tn3270eSrvrConfIndex indicates within
        a host which TN3270E server an entry applies to.
        tn3270eClientGroupName it identifies the set of IP
        clients for which response time data is being collected.
        The particular IP clients making up the set are identified
        in the tn3270eClientGroupTable in the TN3270E-MIB."





      ::= { tn3270eRtObjects 1}

  tn3270eRtCollCtlEntry    OBJECT-TYPE
      SYNTAX        Tn3270eRtCollCtlEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
        "An entry in the TN3270E response time monitoring collection
        control table.  To handle the case of multiple TN3270E
        servers on the same host, the first index of this table is
        the tn3270eSrvrConfIndex from the TN3270E-MIB."
      INDEX {
        tn3270eSrvrConfIndex,    -- Server's index
        tn3270eClientGroupName } -- What to collect on
      ::= { tn3270eRtCollCtlTable 1 }

  Tn3270eRtCollCtlEntry ::= SEQUENCE {
      tn3270eRtCollCtlType              BITS,
      tn3270eRtCollCtlSPeriod           Unsigned32,
      tn3270eRtCollCtlSPMult            Unsigned32,
      tn3270eRtCollCtlThreshHigh        Unsigned32,
      tn3270eRtCollCtlThreshLow         Unsigned32,
      tn3270eRtCollCtlIdleCount         Unsigned32,
      tn3270eRtCollCtlBucketBndry1      Unsigned32,
      tn3270eRtCollCtlBucketBndry2      Unsigned32,
      tn3270eRtCollCtlBucketBndry3      Unsigned32,
      tn3270eRtCollCtlBucketBndry4      Unsigned32,
      tn3270eRtCollCtlRowStatus         RowStatus   }

  -- The OID { tn3270eRtCollCtlEntry 1 } is not used

  tn3270eRtCollCtlType  OBJECT-TYPE
      SYNTAX    BITS {
                       aggregate(0),
                       excludeIpComponent(1),
                       ddr(2),
                       average(3),
                       buckets(4),
                       traps(5)
                     }
      MAX-ACCESS   read-create
      STATUS       current
      DESCRIPTION
        "This object controls what types of response time data to
         collect, whether to summarize the data across the members
         of a client group or keep it individually, whether to
         introduce dynamic definite responses, and whether to
         generate traps.





         aggregate(0)          - Aggregate response time data for the
                                 client group as a whole.  If this bit
                                 is set to 0, then maintain response
                                 time data separately for each member
                                 of the client group.
         excludeIpComponent(1) - Do not include the IP-network
                                 component in any response times.
         ddr(2)                - Enable dynamic definite response.
         average(3)            - Produce an average response time
                                 based on a specified collection
                                 interval.
         buckets(4)            - Maintain tn3270eRtDataBucket values in
                                 a corresponding tn3270eRtDataEntry,
                                 based on the bucket boundaries specified
                                 in the tn3270eRtCollCtlBucketBndry
                                 objects          .
         traps(5)              - generate the notifications specified
                                 in this MIB module.  The
                                 tn3270eRtExceeded and tn3270eRtOkay
                                 notifications are generated only if
                                 average(3) is also specified."
      ::= { tn3270eRtCollCtlEntry 2 }

  tn3270eRtCollCtlSPeriod OBJECT-TYPE
      SYNTAX  Unsigned32 (15..86400) -- 15 second min, 24 hour max
      UNITS   "seconds"
      MAX-ACCESS   read-create
      STATUS       current
      DESCRIPTION
        "The number of seconds that defines the sample period.
         The actual interval is defined as tn3270eRtCollCtlSPeriod
         times tn3270eRtCollCtlSPMult.

         The value of this object is used only if the corresponding
         tn3270eRtCollCtlType has the average(3) setting."
      DEFVAL   {20}    -- 20 seconds
      ::= { tn3270eRtCollCtlEntry 3 }

  tn3270eRtCollCtlSPMult OBJECT-TYPE
      SYNTAX  Unsigned32 (1..5760) -- 5760 x SPeriod of 15 is 24 hours
      UNITS   "period"
      MAX-ACCESS   read-create
      STATUS       current
      DESCRIPTION
        "The sample period multiplier; this value is multiplied by
        the sample period, tn3270eRtCollCtlSPeriod, to determine
        the collection interval.






        Sliding-window average calculation can, if necessary, be
        disabled, by setting the sample period multiplier,
        tn3270eRtCollCtlSPMult, to 1, and setting the sample
        period, tn3270eRtCollCtlSPeriod, to the required
        collection interval.

        The value of this object is used only if the corresponding
        tn3270eRtCollCtlType has the average(3) setting."
      DEFVAL   { 30 }    -- yields an interval of 10 minutes when
                         -- used with the default SPeriod value
      ::= { tn3270eRtCollCtlEntry 4 }

  tn3270eRtCollCtlThreshHigh  OBJECT-TYPE
      SYNTAX            Unsigned32
      UNITS             "seconds"
      MAX-ACCESS        read-create
      STATUS            current
      DESCRIPTION
        "The threshold for generating a tn3270eRtExceeded
        notification, signalling that a monitored total response
        time has exceeded the specified limit.  A value of zero
        for this object suppresses generation of this notification.
        The value of this object is used only if the corresponding
        tn3270eRtCollCtlType has average(3) and traps(5) selected.

        A tn3270eRtExceeded notification is not generated again for a
        tn3270eRtDataEntry until an average response time falling below
        the low threshold tn3270eRtCollCtlThreshLow specified for the
        client group has occurred for the entry."

      DEFVAL   { 0 }   -- suppress notifications
      ::= { tn3270eRtCollCtlEntry 5 }

  tn3270eRtCollCtlThreshLow   OBJECT-TYPE
      SYNTAX            Unsigned32
      UNITS             "seconds"
      MAX-ACCESS        read-create
      STATUS            current
      DESCRIPTION
        "The threshold for generating a tn3270eRtOkay notification,
        signalling that a monitored total response time has fallen
        below the specified limit.  A value of zero for this object
        suppresses generation of this notification.  The value of
        this object is used only if the corresponding
        tn3270eRtCollCtlType has average(3) and traps(5) selected.

        A tn3270eRtOkay notification is not generated again for a
        tn3270eRtDataEntry until an average response time





        exceeding the high threshold tn3270eRtCollCtlThreshHigh
        specified for the client group has occurred for the entry."
      DEFVAL   { 0 }   -- suppress notifications
      ::= { tn3270eRtCollCtlEntry 6 }

  tn3270eRtCollCtlIdleCount   OBJECT-TYPE
      SYNTAX            Unsigned32
      UNITS             "transactions"
      MAX-ACCESS        read-create
      STATUS            current
      DESCRIPTION
        "The value of this object is used to determine whether a
        sample that yields an average response time exceeding the
        value of tn3270eRtCollCtlThreshHigh was a statistically
        valid one.  If the following statement is true, then the
        sample was statistically valid, and so a tn3270eRtExceeded
        notification should be generated:

          AvgCountTrans * ((AvgRt/ThreshHigh - 1) ** 2) >=  IdleCount

        This comparison is done only if the corresponding
        tn3270eRtCollCtlType has average(3) and traps(5) selected."
      DEFVAL { 1 }
      ::= { tn3270eRtCollCtlEntry 7 }

  tn3270eRtCollCtlBucketBndry1   OBJECT-TYPE
      SYNTAX            Unsigned32
      UNITS             "tenths of seconds"
      MAX-ACCESS        read-create
      STATUS            current
      DESCRIPTION
        "The value of this object defines the range of transaction
         response times counted in the Tn3270eRtDataBucket1Rts
         object: those less than or equal to this value."
      DEFVAL { 10 }
      ::= { tn3270eRtCollCtlEntry 8 }

  tn3270eRtCollCtlBucketBndry2   OBJECT-TYPE
      SYNTAX            Unsigned32
      UNITS             "tenths of seconds"
      MAX-ACCESS        read-create
      STATUS            current
      DESCRIPTION
        "The value of this object, together with that of the
        tn3270eRtCollCtlBucketBndry1 object, defines the range
        of transaction response times counted in the
        Tn3270eRtDataBucket2Rts object: those greater than the
        value of the tn3270eRtCollCtlBucketBndry1 object, and





        less than or equal to the value of this object."
      DEFVAL { 20 }
      ::= { tn3270eRtCollCtlEntry 9 }

  tn3270eRtCollCtlBucketBndry3   OBJECT-TYPE
      SYNTAX            Unsigned32
      UNITS             "tenths of seconds"
      MAX-ACCESS        read-create
      STATUS            current
      DESCRIPTION
        "The value of this object, together with that of the
        tn3270eRtCollCtlBucketBndry2 object, defines the range of
        transaction response times counted in the
        Tn3270eRtDataBucket3Rts object:  those greater than the
        value of the tn3270eRtCollCtlBucketBndry2 object, and less
        than or equal to the value of this object."
      DEFVAL { 50 }
      ::= { tn3270eRtCollCtlEntry 10 }

  tn3270eRtCollCtlBucketBndry4   OBJECT-TYPE
      SYNTAX            Unsigned32
      UNITS             "tenths of seconds"
      MAX-ACCESS        read-create
      STATUS            current
      DESCRIPTION
        "The value of this object, together with that of the
        tn3270eRtCollCtlBucketBndry3 object, defines the range
        of transaction response times counted in the
        Tn3270eRtDataBucket4Rts object: those greater than the
        value of the tn3270eRtCollCtlBucketBndry3 object, and
        less than or equal to the value of this object.

        The value of this object also defines the range of
        transaction response times counted in the
        Tn3270eRtDataBucket5Rts object: those greater than the
        value of this object."
      DEFVAL { 100 }
      ::= { tn3270eRtCollCtlEntry 11 }

  tn3270eRtCollCtlRowStatus  OBJECT-TYPE
      SYNTAX            RowStatus
      MAX-ACCESS        read-create
      STATUS            current
      DESCRIPTION
        "This object allows entries to be created and deleted
         in the tn3270eRtCollCtlTable.  An entry in this table
         is deleted by setting this object to destroy(6).
         Deleting an entry in this table has the side-effect





         of removing all entries from the tn3270eRtDataTable
         that are associated with the entry being deleted."
      ::= { tn3270eRtCollCtlEntry 12 }


  -- TN3270E Response Time Data Table

  tn3270eRtDataTable  OBJECT-TYPE
      SYNTAX       SEQUENCE OF Tn3270eRtDataEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
        "The response time data table.  Entries in this table are
         created based on entries in the tn3270eRtCollCtlTable."
      ::= { tn3270eRtObjects 2 }

  tn3270eRtDataEntry  OBJECT-TYPE
      SYNTAX        Tn3270eRtDataEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
        "Entries in this table are created based upon the
        tn3270eRtCollCtlTable.  When the corresponding
        tn3270eRtCollCtlType has aggregate(0) specified, a single
        entry is created in this table, with a tn3270eRtDataClientAddrType
        of unknown(0), a zero-length octet string value for
        tn3270eRtDataClientAddress, and a tn3270eRtDataClientPort value of
        0.  When aggregate(0) is not specified, a separate entry is
        created for each client in the group.

        Note that the following objects defined within an entry in this
        table can  wrap:
            tn3270eRtDataTotalRts
            tn3270eRtDataTotalIpRts
            tn3270eRtDataCountTrans
            tn3270eRtDataCountDrs
            tn3270eRtDataElapsRnTrpSq
            tn3270eRtDataElapsIpRtSq
            tn3270eRtDataBucket1Rts
            tn3270eRtDataBucket2Rts
            tn3270eRtDataBucket3Rts
            tn3270eRtDataBucket4Rts
            tn3270eRtDataBucket5Rts"
      INDEX {
         tn3270eSrvrConfIndex,      -- Server's local index
         tn3270eClientGroupName,    -- Collection target
         tn3270eRtDataClientAddrType,
         tn3270eRtDataClientAddress,





         tn3270eRtDataClientPort }
      ::= { tn3270eRtDataTable 1 }

  Tn3270eRtDataEntry ::= SEQUENCE {
         tn3270eRtDataClientAddrType        IANATn3270eAddrType,
         tn3270eRtDataClientAddress         IANATn3270eAddress,
         tn3270eRtDataClientPort            Unsigned32,
         tn3270eRtDataAvgRt                 Gauge32,
         tn3270eRtDataAvgIpRt               Gauge32,
         tn3270eRtDataAvgCountTrans         Gauge32,
         tn3270eRtDataIntTimeStamp          DateAndTime,
         tn3270eRtDataTotalRts              Counter32,
         tn3270eRtDataTotalIpRts            Counter32,
         tn3270eRtDataCountTrans            Counter32,
         tn3270eRtDataCountDrs              Counter32,
         tn3270eRtDataElapsRndTrpSq         Unsigned32,
         tn3270eRtDataElapsIpRtSq           Unsigned32,
         tn3270eRtDataBucket1Rts            Counter32,
         tn3270eRtDataBucket2Rts            Counter32,
         tn3270eRtDataBucket3Rts            Counter32,
         tn3270eRtDataBucket4Rts            Counter32,
         tn3270eRtDataBucket5Rts            Counter32,
         tn3270eRtDataRtMethod              INTEGER,
         tn3270eRtDataDiscontinuityTime     TimeStamp
     }

  tn3270eRtDataClientAddrType   OBJECT-TYPE
      SYNTAX    IANATn3270eAddrType
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
        "Indicates the type of address represented by the value
        of tn3270eRtDataClientAddress.  The value unknown(0) is
        used if aggregate data is being collected for the client
        group."
      ::= { tn3270eRtDataEntry 1 }

  tn3270eRtDataClientAddress   OBJECT-TYPE
      SYNTAX    IANATn3270eAddress
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
        "Contains the IP address of the TN3270 client being
        monitored.  A zero-length octet string is used if
        aggregate data is being collected for the client group."
      ::= { tn3270eRtDataEntry 2 }

  tn3270eRtDataClientPort   OBJECT-TYPE





      SYNTAX       Unsigned32(0..65535)
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
        "Contains the client port number of the TN3270 client being
        monitored.  The value 0 is used if aggregate data is being
        collected for the client group, or if the
        tn3270eRtDataClientAddrType identifies an address type that
        does not support ports."
      ::= { tn3270eRtDataEntry 3 }

  tn3270eRtDataAvgRt OBJECT-TYPE
      SYNTAX       Gauge32
      UNITS        "tenths of seconds"
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The average total response time measured over the last
        collection interval."
      DEFVAL { 0 }
      ::= { tn3270eRtDataEntry 4 }

  tn3270eRtDataAvgIpRt OBJECT-TYPE
      SYNTAX       Gauge32
      UNITS        "tenths of seconds"
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The average IP response time measured over the last
        collection interval."
      DEFVAL { 0 }
      ::= { tn3270eRtDataEntry 5 }

  tn3270eRtDataAvgCountTrans   OBJECT-TYPE
      SYNTAX       Gauge32
      UNITS        "transactions"
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The sliding transaction count used for calculating the
        values of the tn3270eRtDataAvgRt and tn3270eRtDataAvgIpRt
        objects.  The actual transaction count is available in
        the tn3270eRtDataCountTrans object.

        The initial value of this object, before any averages have
        been calculated, is 0."
      ::= { tn3270eRtDataEntry 6 }






  tn3270eRtDataIntTimeStamp   OBJECT-TYPE
      SYNTAX       DateAndTime
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The date and time of the last interval that
        tn3270eRtDataAvgRt, tn3270eRtDataAvgIpRt, and
        tn3270eRtDataAvgCountTrans were calculated.

        Prior to the calculation of the first interval
        averages, this object returns the value
        0x0000000000000000000000.  When this value is
        returned, the remaining objects in the entry have
        no significance."
      ::= { tn3270eRtDataEntry 7 }

  tn3270eRtDataTotalRts   OBJECT-TYPE
      SYNTAX       Counter32
      UNITS        "tenths of seconds"
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The count of the total response times collected.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 8 }

  tn3270eRtDataTotalIpRts   OBJECT-TYPE
      SYNTAX       Counter32
      UNITS        "tenths of seconds"
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The count of the total IP-network response times
        collected.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 9 }

  tn3270eRtDataCountTrans   OBJECT-TYPE
      SYNTAX       Counter32
      UNITS        "transactions"
      MAX-ACCESS   read-only
      STATUS       current





      DESCRIPTION
        "The count of the total number of transactions detected.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 10 }

  tn3270eRtDataCountDrs   OBJECT-TYPE
      SYNTAX       Counter32
      UNITS        "definite responses"
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The count of the total number of definite responses
        detected.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 11 }

  tn3270eRtDataElapsRndTrpSq   OBJECT-TYPE
      SYNTAX       Unsigned32
      UNITS        "tenths of seconds squared"
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The sum of the elapsed round trip time squared.  The sum
        of the squares is kept in order to enable calculation of
        a variance."
      DEFVAL { 0 }
      ::= { tn3270eRtDataEntry 12 }

  tn3270eRtDataElapsIpRtSq   OBJECT-TYPE
      SYNTAX       Unsigned32
      UNITS        "tenths of seconds squared"
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The sum of the elapsed IP round trip time squared.
        The sum of the squares is kept in order to enable
        calculation of a variance."
      DEFVAL { 0 }
      ::= { tn3270eRtDataEntry 13 }

  tn3270eRtDataBucket1Rts   OBJECT-TYPE
      SYNTAX       Counter32





      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The count of the response times falling into bucket 1.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 14 }

  tn3270eRtDataBucket2Rts   OBJECT-TYPE
      SYNTAX       Counter32
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The count of the response times falling into bucket 2.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 15 }

  tn3270eRtDataBucket3Rts   OBJECT-TYPE
      SYNTAX       Counter32
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The count of the response times falling into bucket 3.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 16 }

  tn3270eRtDataBucket4Rts  OBJECT-TYPE
      SYNTAX       Counter32
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The count of the response times falling into bucket 4.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 17 }

  tn3270eRtDataBucket5Rts  OBJECT-TYPE
      SYNTAX       Counter32





      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The count of the response times falling into bucket 5.

        A management application can detect discontinuities in this
        counter by monitoring the tn3270eRtDataDiscontinuityTime
        object."
      ::= { tn3270eRtDataEntry 18 }

  tn3270eRtDataRtMethod OBJECT-TYPE
      SYNTAX       INTEGER {
                             none(0),
                             responses(1),
                             timingMark(2)
                           }
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
        "The value of this object indicates the method that was
        used in calculating the IP network time.

        The value 'none(0) indicates that response times were not
        calculated for the IP network."
      ::= { tn3270eRtDataEntry 19 }

  tn3270eRtDataDiscontinuityTime OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "The value of sysUpTime on the most recent occasion at
          which one or more of this entry's counter objects
          suffered a discontinuity.  This may happen if a TN3270E
          server is stopped and then restarted, and local methods
          are used to set up collection policy
          (tn3270eRtCollCtlTable entries)."
      ::= { tn3270eRtDataEntry 20 }


  tn3270eRtSpinLock OBJECT-TYPE
      SYNTAX      TestAndIncr
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
        "An advisory lock used to allow cooperating TN3270E-RT-MIB
        applications to coordinate their use of the
        tn3270eRtCollCtlTable.





        When creating a new entry or altering an existing entry
        in the tn3270eRtCollCtlTable, an application should make
        use of tn3270eRtSpinLock to serialize application changes
        or additions.

        Since this is an advisory lock, the use of this lock is
        not enforced."
      ::= { tn3270eRtObjects 3 }

  -- Notifications

  tn3270eRtExceeded   NOTIFICATION-TYPE
      OBJECTS {
         tn3270eRtDataIntTimeStamp,
         tn3270eRtDataAvgRt,
         tn3270eRtDataAvgIpRt,
         tn3270eRtDataAvgCountTrans,
         tn3270eRtDataRtMethod
      }
      STATUS  current
      DESCRIPTION
        "This notification is generated when the average response
        time, tn3270eRtDataAvgRt, exceeds
        tn3270eRtCollCtlThresholdHigh at the end of a collection
        interval specified by tn3270eCollCtlSPeriod
        times tn3270eCollCtlSPMult.  Note that the corresponding
        tn3270eCollCtlType must have traps(5) and average(3) set
        for this notification to be generated.  In addition,
        tn3270eRtDataAvgCountTrans, tn3270eRtCollCtlThreshHigh, and
        tn3270eRtDataAvgRt are algorithmically compared to
        tn3270eRtCollCtlIdleCount for determination if this
        notification will be suppressed."
      ::= { tn3270eRtNotifications 1 }

  tn3270eRtOkay   NOTIFICATION-TYPE
      OBJECTS {
         tn3270eRtDataIntTimeStamp,
         tn3270eRtDataAvgRt,
         tn3270eRtDataAvgIpRt,
         tn3270eRtDataAvgCountTrans,
         tn3270eRtDataRtMethod
      }
      STATUS  current
      DESCRIPTION
        "This notification is generated when the average response
        time, tn3270eRtDataAvgRt, falls below
        tn3270eRtCollCtlThresholdLow at the end of a collection
        interval specified by tn3270eCollCtlSPeriod times





        tn3270eCollCtlSPMult, after a tn3270eRtExceeded
        notification was generated.  Note that the corresponding
        tn3270eCollCtlType must have traps(5) and average(3)
        set for this notification to be generated."
      ::= { tn3270eRtNotifications 2 }

  tn3270eRtCollStart NOTIFICATION-TYPE
      OBJECTS {
         tn3270eRtDataRtMethod,       -- type of collection
         tn3270eResMapElementType     -- type of resource
      }
      STATUS  current
      DESCRIPTION
        "This notification is generated when response time data
        collection is enabled for a member of a client group.
        In order for this notification to occur the corresponding
        tn3270eRtCollCtlType must have traps(5) selected.

        tn3270eResMapElementType contains a valid value only if
        tn3270eRtDataClientAddress contains a valid address
        (rather than a zero-length octet string)."
      ::= { tn3270eRtNotifications 3 }

  tn3270eRtCollEnd   NOTIFICATION-TYPE
      OBJECTS {
         tn3270eRtDataDiscontinuityTime,
         tn3270eRtDataAvgRt,
         tn3270eRtDataAvgIpRt,
         tn3270eRtDataAvgCountTrans,
         tn3270eRtDataIntTimeStamp,
         tn3270eRtDataTotalRts,
         tn3270eRtDataTotalIpRts,
         tn3270eRtDataCountTrans,
         tn3270eRtDataCountDrs,
         tn3270eRtDataElapsRndTrpSq,
         tn3270eRtDataElapsIpRtSq,
         tn3270eRtDataBucket1Rts,
         tn3270eRtDataBucket2Rts,
         tn3270eRtDataBucket3Rts,
         tn3270eRtDataBucket4Rts,
         tn3270eRtDataBucket5Rts,
         tn3270eRtDataRtMethod
      }
      STATUS  current
      DESCRIPTION
        "This notification is generated when an tn3270eRtDataEntry
        is deleted after being active (actual data collected), in
        order to enable a management application monitoring an





        tn3270eRtDataEntry to get the entry's final values.  Note
        that the corresponding tn3270eCollCtlType must have traps(5)
        set for this notification to be generated."
      ::= { tn3270eRtNotifications 4 }

  -- Conformance Statement

  tn3270eRtGroups       OBJECT IDENTIFIER ::= { tn3270eRtConformance 1 }
  tn3270eRtCompliances  OBJECT IDENTIFIER ::= { tn3270eRtConformance 2 }

  -- Compliance statements

  tn3270eRtCompliance     MODULE-COMPLIANCE
      STATUS current
      DESCRIPTION
        "The compliance statement for agents that support the
        TN327E-RT-MIB."
      MODULE   -- this module
         MANDATORY-GROUPS { tn3270eRtGroup, tn3270eRtNotGroup }

      OBJECT tn3270eRtCollCtlType
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to support a SET operation to
            this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlSPeriod
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to allow the user to change
            the default value of this object, and is allowed to
            use a different default."

      OBJECT tn3270eRtCollCtlSPMult
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to support a SET operation
            to this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlThreshHigh
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to support a SET operation
            to this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlThreshLow
         MIN-ACCESS  read-only
         DESCRIPTION





            "The agent is not required to support a SET operation
            to this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlIdleCount
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to support a SET operation
            to this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlBucketBndry1
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to support a SET operation
            to this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlBucketBndry2
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to support a SET operation
            to this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlBucketBndry3
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to support a SET operation
            to this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlBucketBndry4
         MIN-ACCESS  read-only
         DESCRIPTION
            "The agent is not required to support a SET operation
            to this object in the absence of adequate security."

      OBJECT tn3270eRtCollCtlRowStatus
         SYNTAX   INTEGER {
                           active(1) -- subset of RowStatus
                          }
         MIN-ACCESS read-only
         DESCRIPTION
            "Write access is not required, and only one of the six
            enumerated values for the RowStatus textual convention
            need be supported, specifically: active(1)."

      ::= {tn3270eRtCompliances 1 }

  -- Group definitions

  tn3270eRtGroup         OBJECT-GROUP





      OBJECTS {
          tn3270eRtCollCtlType,
          tn3270eRtCollCtlSPeriod,
          tn3270eRtCollCtlSPMult,
          tn3270eRtCollCtlThreshHigh,
          tn3270eRtCollCtlThreshLow,
          tn3270eRtCollCtlIdleCount,
          tn3270eRtCollCtlBucketBndry1,
          tn3270eRtCollCtlBucketBndry2,
          tn3270eRtCollCtlBucketBndry3,
          tn3270eRtCollCtlBucketBndry4,
          tn3270eRtCollCtlRowStatus,
          tn3270eRtDataDiscontinuityTime,
          tn3270eRtDataAvgRt,
          tn3270eRtDataAvgIpRt,
          tn3270eRtDataAvgCountTrans,
          tn3270eRtDataIntTimeStamp,
          tn3270eRtDataTotalRts,
          tn3270eRtDataTotalIpRts,
          tn3270eRtDataCountTrans,
          tn3270eRtDataCountDrs,
          tn3270eRtDataElapsRndTrpSq,
          tn3270eRtDataElapsIpRtSq,
          tn3270eRtDataBucket1Rts,
          tn3270eRtDataBucket2Rts,
          tn3270eRtDataBucket3Rts,
          tn3270eRtDataBucket4Rts,
          tn3270eRtDataBucket5Rts,
          tn3270eRtDataRtMethod,
          tn3270eRtSpinLock }
      STATUS  current
      DESCRIPTION
        "This group is mandatory for all implementations that
        support the TN3270E-RT-MIB. "
      ::= { tn3270eRtGroups 1 }

  tn3270eRtNotGroup         NOTIFICATION-GROUP
      NOTIFICATIONS {
          tn3270eRtExceeded,
          tn3270eRtOkay,
          tn3270eRtCollStart,
          tn3270eRtCollEnd
       }










      STATUS  current
      DESCRIPTION
        "The notifications that must be supported when the
        TN3270E-RT-MIB is implemented. "
      ::= { tn3270eRtGroups 2 }

  END



