SIP-UA-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32,
    mib-2
          FROM SNMPv2-SMI             -- RFC 2578

    MODULE-COMPLIANCE,
    OBJECT-GROUP
          FROM SNMPv2-CONF            -- RFC 2580

    applIndex
          FROM NETWORK-SERVICES-MIB   -- RFC 2788

    InetAddressType,
    InetAddress
          FROM INET-ADDRESS-MIB       -- RFC 4001

    SipTCEntityRole
          FROM SIP-TC-MIB;            -- RFC 4780

sipUAMIB MODULE-IDENTITY
    LAST-UPDATED   "200704200000Z"
    ORGANIZATION   "IETF Session Initiation Protocol Working Group"
    CONTACT-INFO
             "SIP WG email: sip@ietf.org

              Co-editor  Kevin Lingle





                         Cisco Systems, Inc.
              postal:    7025 Kit Creek Road
                         P.O. Box 14987
                         Research Triangle Park, NC 27709
                         USA
              email:     klingle@cisco.com
              phone:     +1 919 476 2029

              Co-editor  Joon Maeng
              email:     jmaeng@austin.rr.com

              Co-editor  Jean-Francois Mule
                         CableLabs
              postal:    858 Coal Creek Circle
                         Louisville, CO 80027
                         USA
              email:     jf.mule@cablelabs.com
              phone:     +1 303 661 9100

              Co-editor  Dave Walker
              email:     drwalker@rogers.com"
    DESCRIPTION
       "Session Initiation Protocol (SIP) User Agent (UA) MIB module.

        SIP is an application-layer signaling protocol for creating,
        modifying, and terminating multimedia sessions with one or more
        participants.  These sessions include Internet multimedia
        conferences and Internet telephone calls.  SIP is defined in
        RFC 3261 (June 2002).

        A User Agent is an application that contains both a User Agent
        Client (UAC) and a User Agent Server (UAS).  A UAC is an
        application that initiates a SIP request.  A UAS is an
        application that contacts the user when a SIP request is
        received and that returns a response on behalf of the user.
        The response accepts, rejects, or redirects the request.

        Copyright (C) The IETF Trust (2007).  This version of
        this MIB module is part of RFC 4780; see the RFC itself for
        full legal notices."
    REVISION        "200704200000Z"
    DESCRIPTION
       "Initial version of the IETF SIP-UA-MIB module.  This version
        published as part of RFC 4780."
     ::= { mib-2 150 }

-- Top-Level Components of this MIB.
sipUAMIBObjects        OBJECT IDENTIFIER ::= { sipUAMIB 1 }





sipUAMIBConformance    OBJECT IDENTIFIER ::= { sipUAMIB 2 }

--
-- This MIB contains objects related to SIP User Agents.
--
sipUACfgServer         OBJECT IDENTIFIER ::= { sipUAMIBObjects 1 }

--
-- SIP Server Configuration
--
sipUACfgServerTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SipUACfgServerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table contains SIP server configuration objects applicable
        to each SIP user agent in this system."
    ::= { sipUACfgServer 1 }

sipUACfgServerEntry OBJECT-TYPE
    SYNTAX      SipUACfgServerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A row of server configuration.

        Each row represents those objects for a particular SIP user
        agent present in this system.  applIndex is used to uniquely
        identify these instances of SIP user agents and correlate
        them through the common framework of the NETWORK-SERVICES-MIB
        (RFC 2788).  The same value of applIndex used in the
        corresponding SIP-COMMON-MIB is used here."
    INDEX { applIndex, sipUACfgServerIndex }
    ::= { sipUACfgServerTable 1 }

SipUACfgServerEntry ::= SEQUENCE {
        sipUACfgServerIndex       Unsigned32,
        sipUACfgServerAddressType InetAddressType,
        sipUACfgServerAddress     InetAddress,
        sipUACfgServerRole        SipTCEntityRole
    }

sipUACfgServerIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A unique identifier of a server address when multiple addresses





        are configured by the SIP entity.  If one address isn't
        reachable, then another can be tried."
    ::= { sipUACfgServerEntry 1 }

sipUACfgServerAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the type of address contained in the
        associated instance of sipUACfgServerAddress."
    REFERENCE
       "INET-ADDRESS-MIB (RFC 4001)"
    ::= { sipUACfgServerEntry 2 }

sipUACfgServerAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the address of a SIP server this user
        agent will use to proxy/redirect calls.  The type of this
        address is determined by the value of the
        sipUACfgServerAddressType object."
    REFERENCE "INET-ADDRESS-MIB (RFC 4001)"
    ::= { sipUACfgServerEntry 3 }

sipUACfgServerRole OBJECT-TYPE
    SYNTAX      SipTCEntityRole
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the function of the SIP server this user
        agent should communicate with: registrar, proxy (outbound
        proxy), etc."
    ::= { sipUACfgServerEntry 4 }

--
-- Conformance
--
sipUAMIBCompliances OBJECT IDENTIFIER ::= { sipUAMIBConformance 1 }
sipUAMIBGroups      OBJECT IDENTIFIER ::= { sipUAMIBConformance 2 }

--
-- Compliance Statements
--
sipUACompliance MODULE-COMPLIANCE
    STATUS      current





    DESCRIPTION
       "The compliance statement for SIP entities that implement the
        SIP-UA-MIB module."
    MODULE -- this module
        MANDATORY-GROUPS { sipUAConfigGroup }

    ::= { sipUAMIBCompliances 1 }

--
-- Units of Conformance
--
sipUAConfigGroup OBJECT-GROUP
    OBJECTS {
            sipUACfgServerAddressType,
            sipUACfgServerAddress,
            sipUACfgServerRole
    }
    STATUS  current
    DESCRIPTION
       "A collection of objects providing information about the
        configuration of SIP User Agents."
    ::= { sipUAMIBGroups 1 }

END


