T11-FC-ROUTE-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Unsigned32, mib-2                   FROM SNMPv2-SMI  -- [RFC2578]
    MODULE-COMPLIANCE, OBJECT-GROUP     FROM SNMPv2-CONF -- [RFC2580]
    RowStatus, TimeStamp,
    StorageType                         FROM SNMPv2-TC   -- [RFC2579]
    InterfaceIndex, InterfaceIndexOrZero  FROM IF-MIB    -- [RFC2863]
    fcmInstanceIndex, fcmSwitchIndex,
    FcAddressIdOrZero, FcDomainIdOrZero FROM FC-MGMT-MIB -- [FC-MGMT]
    T11FabricIndex                      FROM T11-TC-MIB; -- [RFC4439]

t11FcRouteMIB MODULE-IDENTITY
    LAST-UPDATED "200608140000Z"
    ORGANIZATION "T11"
    CONTACT-INFO
              "     Claudio DeSanti
                    Cisco Systems, Inc.
                    170 West Tasman Drive
                    San Jose, CA 95134 USA
                    EMail: cds@cisco.com


                    Keith McCloghrie
                    Cisco Systems, Inc.
                    170 West Tasman Drive
                    San Jose, CA USA 95134
                    Email: kzm@cisco.com"
    DESCRIPTION
           "The MIB module for configuring and displaying Fibre
           Channel Route Information.

           Copyright (C) The Internet Society (2006).  This version
           of this MIB module is part of RFC 4625;  see the RFC
           itself for full legal notices."
    REVISION     "200608140000Z"





    DESCRIPTION
           "Initial version of this MIB module, published as RFC4625."

    ::= {mib-2 144 }

t11FcRouteNotifications OBJECT IDENTIFIER ::= { t11FcRouteMIB 0 }
t11FcRouteObjects       OBJECT IDENTIFIER ::= { t11FcRouteMIB 1 }
t11FcRouteConformance   OBJECT IDENTIFIER ::= { t11FcRouteMIB 2 }

--
-- Per-Fabric routing information
--
t11FcRouteFabricTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF T11FcRouteFabricEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The table containing Fibre Channel Routing information
           that is specific to a Fabric."
    ::= { t11FcRouteObjects 1 }

t11FcRouteFabricEntry OBJECT-TYPE
    SYNTAX      T11FcRouteFabricEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "Each entry contains routing information specific to a
           particular Fabric on a particular switch (identified by
           values of fcmInstanceIndex and fcmSwitchIndex)."
    INDEX      { fcmInstanceIndex, fcmSwitchIndex,
                 t11FcRouteFabricIndex }
    ::= { t11FcRouteFabricTable 1 }

T11FcRouteFabricEntry ::=
    SEQUENCE {
        t11FcRouteFabricIndex      T11FabricIndex,
        t11FcRouteFabricLastChange TimeStamp
    }

t11FcRouteFabricIndex OBJECT-TYPE
    SYNTAX      T11FabricIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "A unique index value that uniquely identifies a
           particular Fabric.

           In a Fabric conformant to FC-SW-3, only a single Fabric





           can operate within a physical infrastructure, and thus
           the value of this Fabric Index will always be 1.

           In a Fabric conformant to FC-SW-4, multiple Virtual Fabrics
           can operate within one (or more) physical infrastructures.
           In such a case, index value is used to uniquely identify a
           particular Fabric within a physical infrastructure."
    ::= { t11FcRouteFabricEntry 1 }

t11FcRouteFabricLastChange OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The value of sysUpTime at the most recent time when any
           corresponding row in the t11FcRouteTable was created,
           modified, or deleted.  A corresponding row in the
           t11FcRouteTable is for the same management instance,
           the same switch, and same Fabric as the row in this table.

           If no change has occurred since the last restart of the
           management system, then the value of this object is 0."
    ::= { t11FcRouteFabricEntry 2 }

--
-- Fibre Channel Routing table
--
t11FcRouteTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF T11FcRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The Fibre Channel Routing tables for the
           locally managed switches.  This table lists all the
           routes that are configured in and/or computed by any
           local switch for any Fabric.

           Such routes are used by a switch to forward frames (of user
           data) on a Fabric.  The conceptual process is based on
           extracting the Destination Fibre Channel Address Identifier
           (D_ID) out of a received frame (of user data) and comparing
           it to each entry of this table that is applicable to the
           given switch and Fabric.  Such comparison consists of first
           performing a logical-AND of the extracted D_ID with a mask
           (the value of t11FcRouteDestMask) and second comparing the
           result of that 'AND' operation to the value of
           t11FcRouteDestAddrId.  A similar comparison is made of the
           Source Fibre Channel Address Identifier (S_ID) of a frame





           against the t11FcRouteSrcAddrId and t11FcRouteSrcMask values
           of an entry.  If an entry's value of t11FcRouteInInterface
           is non-zero, then a further comparison determines if the
           frame was received on the appropriate interface.  If all of
           these comparisons for a particular entry are successful,
           then that entry represents a potential route for forwarding
           the received frame.

           For entries configured by a user, t11FcRouteProto has
           the value 'netmgmt'; only entries of this type can be
           deleted by the user."
    ::= { t11FcRouteObjects 2 }

t11FcRouteEntry OBJECT-TYPE
    SYNTAX      T11FcRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "Each entry contains a route to a particular destination,
           possibly from a particular subset of source addresses,
           on a particular Fabric via a particular output interface
           and learned in a particular manner."
    INDEX       { fcmInstanceIndex, fcmSwitchIndex,
                  t11FcRouteFabricIndex,
                  t11FcRouteDestAddrId, t11FcRouteDestMask,
                  t11FcRouteSrcAddrId, t11FcRouteSrcMask,
                  t11FcRouteInInterface, t11FcRouteProto,
                  t11FcRouteOutInterface }
    ::= { t11FcRouteTable 1 }
T11FcRouteEntry ::=
    SEQUENCE {
        t11FcRouteDestAddrId   FcAddressIdOrZero,
        t11FcRouteDestMask     FcAddressIdOrZero,
        t11FcRouteSrcAddrId    FcAddressIdOrZero,
        t11FcRouteSrcMask      FcAddressIdOrZero,
        t11FcRouteInInterface  InterfaceIndexOrZero,
        t11FcRouteProto        INTEGER,
        t11FcRouteOutInterface InterfaceIndex,
        t11FcRouteDomainId     FcDomainIdOrZero,
        t11FcRouteMetric       Unsigned32,
        t11FcRouteType         INTEGER,
        t11FcRouteIfDown       INTEGER,
        t11FcRouteStorageType  StorageType,
        t11FcRouteRowStatus    RowStatus
    }

t11FcRouteDestAddrId OBJECT-TYPE
    SYNTAX      FcAddressIdOrZero (SIZE (3))





    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The destination Fibre Channel Address Identifier of
           this route.  A zero-length string for this field is
           not allowed."
    ::= { t11FcRouteEntry 1 }

t11FcRouteDestMask OBJECT-TYPE
    SYNTAX      FcAddressIdOrZero
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The mask to be logical-ANDed with a destination
           Fibre Channel Address Identifier before it is compared
           to the value in the t11FcRouteDestAddrId field.
           Allowed values are 255.255.255, 255.255.0, or 255.0.0.
           FSPF's definition generates routes to a Domain_ID,
           so the mask for all FSPF-generated routes is 255.0.0.
           The zero-length value has the same meaning as 0.0.0."
    ::= { t11FcRouteEntry 2 }

t11FcRouteSrcAddrId OBJECT-TYPE
    SYNTAX      FcAddressIdOrZero
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The source Fibre Channel Address Identifier of this
           route.  Note that if this object and the corresponding
           instance of t11FcRouteSrcMask both have a value of 0.0.0,
           then this route matches all source addresses.  The
           zero-length value has the same meaning as 0.0.0."
    ::= { t11FcRouteEntry 3 }

t11FcRouteSrcMask OBJECT-TYPE
    SYNTAX      FcAddressIdOrZero
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The mask to be logical-ANDed with a source
           Fibre Channel Address Identifier before it is compared
           to the value in the t11FcRouteSrcAddrId field.  Allowed
           values are 255.255.255, 255.255.0, 255.0.0, or 0.0.0.
           The zero-length value has the same meaning as 0.0.0."
    ::= { t11FcRouteEntry 4 }

t11FcRouteInInterface OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero





    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "If the value of this object is non-zero, it is the
           value of ifIndex that identifies the local
           Fibre Channel interface through which a frame
           must have been received in order to match with
           this entry.  If the value of this object is zero,
           the matching does not require that the frame be
           received on any specific interface."
    ::= { t11FcRouteEntry 5 }

t11FcRouteProto OBJECT-TYPE
    SYNTAX   INTEGER {
                 other(1),
                 local(2),
                 netmgmt(3),
                 fspf(4)
              }
    MAX-ACCESS not-accessible
    STATUS   current
    DESCRIPTION
           "The mechanism via which this route was learned:
                other(1)  - not specified
                local(2)  - local interface
                netmgmt(3)- static route
                fspf(4)   - Fibre Shortest Path First
           "
    ::= { t11FcRouteEntry 6 }

t11FcRouteOutInterface OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The value of ifIndex that identifies the local
           Fibre Channel interface through which the next hop
           of this route is to be reached."
    ::= { t11FcRouteEntry 7 }

t11FcRouteDomainId OBJECT-TYPE
    SYNTAX      FcDomainIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The domain_ID of next hop switch.

           This object can have a value of zero if the value





           of t11FcRouteProto is 'local'."
    ::= { t11FcRouteEntry 8 }

t11FcRouteMetric OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65536)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The routing metric for this route.

           The use of this object is dependent on t11FcRouteProto."
    ::= { t11FcRouteEntry 9 }

t11FcRouteType OBJECT-TYPE
    SYNTAX      INTEGER {
                    local(1),
                    remote(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The type of route.

           local(1)  - a route for which the next Fibre Channel
                       port is the final destination;
           remote(2) - a route for which the next Fibre Channel
                      port is not the final destination."
    DEFVAL {local}
    ::= { t11FcRouteEntry 10 }

t11FcRouteIfDown OBJECT-TYPE
    SYNTAX      INTEGER {
                    remove(1),
                    retain(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The value of this object indicates what happens to
           this route when the output interface (given by the
           corresponding value of t11FcRouteOutInterface) is
           operationally 'down'.  If this object's value is 'retain',
           the route is to be retained in this table.  If this
           object's value is 'remove', the route is to be removed
           from this table."
    DEFVAL  { retain }
    ::= { t11FcRouteEntry 11 }






t11FcRouteStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The storage type for this conceptual row.
           Conceptual rows having the value 'permanent' need not
           allow write-access to any columnar objects in the row."
       DEFVAL { nonVolatile }
    ::= { t11FcRouteEntry 12 }

t11FcRouteRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The status of this conceptual row.
           The only rows that can be deleted by setting this object to
           'destroy' are those for which t11FcRouteProto has the value
           'netmgmt'."
    ::= { t11FcRouteEntry 13 }

--
-- Conformance
--
t11FcRouteCompliances OBJECT IDENTIFIER
                         ::= { t11FcRouteConformance 1 }
t11FcRouteGroups      OBJECT IDENTIFIER
                         ::= { t11FcRouteConformance 2 }


t11FcRouteCompliance  MODULE-COMPLIANCE
    STATUS    current
    DESCRIPTION
           "The compliance statement for entities that
           implement the T11-FC-ROUTE-MIB.
--
-- Note: The next four OBJECT clauses are for auxiliary objects, and the
-- SMIv2 does not permit inclusion of objects that are not accessible
-- in an OBJECT clause (see Sections 3.1 & 5.4.3 in STD 58, RFC 2580).
-- Thus, these four clauses cannot be included below in the normal
-- location for OBJECT clauses.
--
--      OBJECT     t11FcRouteSrcAddrId
--      SYNTAX     FcAddressIdOrZero (SIZE (0))
--      DESCRIPTION
--             'Support is not required for routes that
--             match only a subset of possible source





--             addresses.'
--
--      OBJECT     t11FcRouteSrcMask
--      SYNTAX     FcAddressIdOrZero (SIZE (0))
--      DESCRIPTION
--             'Support is not required for routes that
--             match only a subset of possible source
--             addresses.'
--
--      OBJECT     t11FcRouteDestMask
--      DESCRIPTION
--             'Support is mandatory only for FSPF-generated
--             routes.  Since FSPF's definition generates
--             routes to a Domain_ID, the mask for all
--             FSPF-generated routes is 255.0.0.  Thus,
--             support is only required for 255.0.0.'
--
--      OBJECT     t11FcRouteInInterface
--      SYNTAX     InterfaceIndexOrZero (0)
--      DESCRIPTION
--             'Support for routes specific to particular
--             source interfaces is not required.'
          "

    MODULE  -- this module
        MANDATORY-GROUPS { t11FcRouteGroup }

        OBJECT     t11FcRouteIfDown
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcRouteDomainId
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcRouteMetric
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcRouteType
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcRouteStorageType





        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcRouteRowStatus
        SYNTAX     INTEGER { active(1) }
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

    ::= { t11FcRouteCompliances 1 }
t11FcRouteGroup  OBJECT-GROUP
    OBJECTS  { t11FcRouteFabricLastChange,
               t11FcRouteDomainId,
               t11FcRouteMetric,
               t11FcRouteType,
               t11FcRouteIfDown,
               t11FcRouteStorageType,
               t11FcRouteRowStatus
             }
    STATUS   current
    DESCRIPTION
           "A collection of objects for displaying and configuring
           routes."
    ::= { t11FcRouteGroups 1 }

END

























