DISMAN-TRACEROUTE-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32,
    Gauge32, Unsigned32, mib-2,
    NOTIFICATION-TYPE,
    OBJECT-IDENTITY
        FROM SNMPv2-SMI                  -- RFC2578
    RowStatus, StorageType,
    TruthValue, DateAndTime
        FROM SNMPv2-TC                   -- RFC2579
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF                 -- RFC2580
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB          -- RFC2571
    InterfaceIndexOrZero                 -- RFC2863
        FROM IF-MIB
    InetAddressType, InetAddress
        FROM INET-ADDRESS-MIB            -- RFC2851
    OperationResponseStatus
        FROM DISMAN-PING-MIB;            -- RFC2925

 traceRouteMIB MODULE-IDENTITY
    LAST-UPDATED "200009210000Z"         -- 21 September 2000

    ORGANIZATION "IETF Distributed Management Working Group"
    CONTACT-INFO
        "Kenneth White

        International Business Machines Corporation
        Network Computing Software Division
        Research Triangle Park, NC, USA






        E-mail: wkenneth@us.ibm.com"
    DESCRIPTION
        "The Traceroute MIB (DISMAN-TRACEROUTE-MIB) provides
        access to the traceroute capability at a remote host."

     --  Revision history

     REVISION     "200009210000Z"         -- 21 September 2000
     DESCRIPTION
         "Initial version, published as RFC 2925."

    ::= { mib-2 81 }

 -- Top level structure of the MIB

 traceRouteNotifications  OBJECT IDENTIFIER ::= { traceRouteMIB 0 }
 traceRouteObjects        OBJECT IDENTIFIER ::= { traceRouteMIB 1 }
 traceRouteConformance    OBJECT IDENTIFIER ::= { traceRouteMIB 2 }

 -- The registration node (point) for traceroute implementation types

 traceRouteImplementationTypeDomains OBJECT IDENTIFIER
 ::= { traceRouteMIB 3 }

 traceRouteUsingUdpProbes OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Indicates that an implementation is using UDP probes to
        perform the traceroute operation."
    ::= { traceRouteImplementationTypeDomains 1 }


 -- Simple Object Definitions

 traceRouteMaxConcurrentRequests OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "requests"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The maximum number of concurrent active traceroute requests
       that are allowed within an agent implementation.  A value
       of 0 for this object implies that there is no limit for
       the number of concurrent active requests in effect."
    DEFVAL { 10 }
    ::= { traceRouteObjects 1 }







  -- Traceroute Control Table

 traceRouteCtlTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TraceRouteCtlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines the Remote Operations Traceroute Control Table for
        providing the capability of invoking traceroute from a remote
        host.  The results of traceroute operations can be stored in
        the traceRouteResultsTable, traceRouteProbeHistoryTable, and
        the traceRouteHopsTable."
   ::= { traceRouteObjects 2 }

 traceRouteCtlEntry OBJECT-TYPE
    SYNTAX      TraceRouteCtlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines an entry in the traceRouteCtlTable.  The first
        index element, traceRouteCtlOwnerIndex, is of type
        SnmpAdminString, a textual convention that allows for
        use of the SNMPv3 View-Based Access Control Model
        (RFC 2575 [11], VACM) and allows an management
        application to identify its entries.  The second index,
        traceRouteCtlTestName (also an SnmpAdminString),
        enables the same management application to have
        multiple requests outstanding."
    INDEX {
            traceRouteCtlOwnerIndex,
            traceRouteCtlTestName
          }
    ::= { traceRouteCtlTable 1 }

 TraceRouteCtlEntry ::=
    SEQUENCE {
      traceRouteCtlOwnerIndex         SnmpAdminString,
      traceRouteCtlTestName           SnmpAdminString,
      traceRouteCtlTargetAddressType  InetAddressType,
      traceRouteCtlTargetAddress      InetAddress,
      traceRouteCtlByPassRouteTable   TruthValue,
      traceRouteCtlDataSize           Unsigned32,
      traceRouteCtlTimeOut            Unsigned32,
      traceRouteCtlProbesPerHop       Unsigned32,
      traceRouteCtlPort               Unsigned32,
      traceRouteCtlMaxTtl             Unsigned32,
      traceRouteCtlDSField            Unsigned32,
      traceRouteCtlSourceAddressType  InetAddressType,





      traceRouteCtlSourceAddress      InetAddress,
      traceRouteCtlIfIndex            InterfaceIndexOrZero,
      traceRouteCtlMiscOptions        SnmpAdminString,
      traceRouteCtlMaxFailures        Unsigned32,
      traceRouteCtlDontFragment       TruthValue,
      traceRouteCtlInitialTtl         Unsigned32,
      traceRouteCtlFrequency          Unsigned32,
      traceRouteCtlStorageType        StorageType,
      traceRouteCtlAdminStatus        INTEGER,
      traceRouteCtlMaxRows            Unsigned32,
      traceRouteCtlTrapGeneration     BITS,
      traceRouteCtlDescr              SnmpAdminString,
      traceRouteCtlCreateHopsEntries  TruthValue,
      traceRouteCtlType               OBJECT IDENTIFIER,
      traceRouteCtlRowStatus          RowStatus
    }

 traceRouteCtlOwnerIndex OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "To facilitate the provisioning of access control by a
       security administrator using the View-Based Access
       Control Model (RFC 2575, VACM) for tables in which
       multiple users may need to independently create or
       modify entries, the initial index is used as an 'owner
       index'.  Such an initial index has a syntax of
       SnmpAdminString, and can thus be trivially mapped to a
       securityName or groupName as defined in VACM, in
       accordance with a security policy.

       When used in conjunction with such a security policy
       all entries in the table belonging to a particular user
       (or group) will have the same value for this initial
       index.  For a given user's entries in a particular
       table, the object identifiers for the information in
       these entries will have the same subidentifiers (except
       for the 'column' subidentifier) up to the end of the
       encoded owner index. To configure VACM to permit access
       to this portion of the table, one would create
       vacmViewTreeFamilyTable entries with the value of
       vacmViewTreeFamilySubtree including the owner index
       portion, and vacmViewTreeFamilyMask 'wildcarding' the
       column subidentifier.  More elaborate configurations
       are possible."
    ::= { traceRouteCtlEntry 1 }






  traceRouteCtlTestName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of a traceroute test.  This is locally unique,
        within the scope of an traceRouteCtlOwnerIndex."
    ::= { traceRouteCtlEntry 2 }

 traceRouteCtlTargetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the type of host address to be used on the
        traceroute request at the remote host."
    DEFVAL { ipv4 }
    ::= { traceRouteCtlEntry 3 }

 traceRouteCtlTargetAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the host address used on the
        traceroute request at the remote host.  The
        host address type can be determined by the
        examining the value of the corresponding
        traceRouteCtlTargetAddressType index element.

        A value for this object MUST be set prior to
        transitioning its corresponding traceRouteCtlEntry to
        active(1) via traceRouteCtlRowStatus."
    ::= { traceRouteCtlEntry 4 }

 traceRouteCtlByPassRouteTable OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The purpose of this object is to optionally enable
       bypassing the route table.  If enabled, the remote
       host will bypass the normal routing tables and send
       directly to a host on an attached network.  If the
       host is not on a directly-attached network, an
       error is returned.  This option can be used to perform
       the traceroute operation to a local host through an
       interface that has no route defined (e.g., after the





       interface was dropped by routed)."
    DEFVAL { false }
    ::= { traceRouteCtlEntry 5 }

 traceRouteCtlDataSize OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65507)
    UNITS       "octets"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the size of the data portion of a traceroute
        request in octets.  A traceroute request is essentially
        transmitted by encoding a UDP datagram into a
        IP packet. So subtracting the size of a UDP header
        (8 octets) and the size of a IP header (20 octets)
        yields a maximum of 65507 octets."
    DEFVAL { 0 }
    ::= { traceRouteCtlEntry 6 }

 traceRouteCtlTimeOut OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the time-out value, in seconds, for
        a traceroute request."
    DEFVAL { 3 }
    ::= { traceRouteCtlEntry 7 }

 traceRouteCtlProbesPerHop OBJECT-TYPE
    SYNTAX      Unsigned32 (1..10)
    UNITS       "probes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the number of times to reissue a traceroute
        request with the same time-to-live (TTL) value."
    DEFVAL { 3 }
    ::= { traceRouteCtlEntry 8 }

 traceRouteCtlPort OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    UNITS       "UDP Port"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the UDP port to send the traceroute





        request to.  Need to specify a port that is not in
        use at the destination (target) host.  The default
        value for this object is the IANA assigned port,
        33434, for the traceroute function."
    DEFVAL { 33434 }
    ::= { traceRouteCtlEntry 9 }

 traceRouteCtlMaxTtl OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    UNITS       "time-to-live value"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum time-to-live value."
    DEFVAL { 30 }
    ::= { traceRouteCtlEntry 10 }

 traceRouteCtlDSField OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the value to store in the Differentiated
        Services (DS) Field in the IP packet used to
        encapsulate the traceroute probe.  The DS Field is
        defined as the Type of Service (TOS) octet in a IPv4
        header or as the Traffic Class octet in a IPv6 header.

        The value of this object must be a decimal integer
        in the range from 0 to 255.  This option can be used
        to determine what effect an explicit DS Field setting
        has on a traceroute response.  Not all values are legal
        or meaningful.  DS Field usage is often not supported
        by IP implementations.  A value of 0 means that the
     function represented by this option is not supported.
     Useful TOS octet values are probably '16' (low delay)
     and '8' ( high throughput)."
    REFERENCE
        "Refer to RFC 2474 for the definition of the
        Differentiated Services Field and to RFC 1812
        Section 5.3.2 for Type of Service (TOS)."
    DEFVAL { 0 }
    ::= { traceRouteCtlEntry 11 }

 traceRouteCtlSourceAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current





    DESCRIPTION
        "Specifies the type of the source address,
        traceRouteCtlSourceAddress, to be used at a remote host
        when performing a traceroute operation."
    DEFVAL { unknown }
    ::= { traceRouteCtlEntry 12 }

 traceRouteCtlSourceAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Use the specified IP address (which must be given
        as an IP number, not a hostname) as the source
        address in outgoing probe packets. On hosts with
        more than one IP address, this option can be used
        to force the source address to be something other
        than the primary IP address of the interface the
        probe packet is sent on.  If the IP address is not
        one of this machine's interface addresses, an error
        is returned and nothing is sent.  A zero length
        octet string value for this object disables source
        address specification.

        The address type (InetAddressType) that relates to
        this object is specified by the corresponding value
        of traceRouteCtlSourceAddressType."
    DEFVAL { ''H }
    ::= { traceRouteCtlEntry 13 }

 traceRouteCtlIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Setting this object to an interface's ifIndex prior
        to starting a remote traceroute operation directs
        the traceroute probes to be transmitted over the
        specified interface.  A value of zero for this object
        implies that this option is not enabled."
    DEFVAL { 0 }
    ::= { traceRouteCtlEntry 14 }

 traceRouteCtlMiscOptions OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION





        "Enables an application to specify implementation
        dependent options."
    DEFVAL { ''H }
    ::= { traceRouteCtlEntry 15 }

 traceRouteCtlMaxFailures OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    UNITS       "timeouts"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object indicates the maximum number
        of consecutive timeouts allowed before terminating
        a remote traceroute request.  A value of either 255 (maximum
        hop count/possible TTL value) or a 0 indicates that the
        function of terminating a remote traceroute request when a
        specific number of successive timeouts are detected is
        disabled."
    DEFVAL { 5 }
    ::= { traceRouteCtlEntry 16 }

 traceRouteCtlDontFragment OBJECT-TYPE
    SYNTAX         TruthValue
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "This object enables setting of the don't fragment flag (DF)
        in the IP header for a probe.  Use of this object enables
        performing a manual PATH MTU test."
    DEFVAL  { false }
    ::= { traceRouteCtlEntry 17 }

 traceRouteCtlInitialTtl OBJECT-TYPE
    SYNTAX         Unsigned32 (0..255)
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The value of this object specifies the initial TTL value to
        use.  This enables bypassing the initial (often well known)
        portion of a path."
    DEFVAL { 1 }
    ::= { traceRouteCtlEntry 18 }

 traceRouteCtlFrequency  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current





    DESCRIPTION
        "The number of seconds to wait before repeating a
        traceroute test as defined by the value of the
        various objects in the corresponding row.

        The number of hops in a single traceroute test
        is determined by the value of the corresponding
        traceRouteCtlProbesPerHop object.  After a
        single test completes the number of seconds as defined
        by the value of traceRouteCtlFrequency MUST elapse
        before the next traceroute test is started.

        A value of 0 for this object implies that the test
        as defined by the corresponding entry will not be
        repeated."
    DEFVAL { 0 }
    ::= { traceRouteCtlEntry 19 }

 traceRouteCtlStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this conceptual row.
        Conceptual rows having the value 'permanent' need not
        allow write-access to any columnar objects in the row."
    DEFVAL { nonVolatile }
    ::= { traceRouteCtlEntry 20 }

 traceRouteCtlAdminStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                          enabled(1), -- operation should be started
                          disabled(2) -- operation should be stopped
                        }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Reflects the desired state that an traceRouteCtlEntry
        should be in:

           enabled(1)  - Attempt to activate the test as defined by
                         this traceRouteCtlEntry.
           disabled(2) - Deactivate the test as defined by this
                         traceRouteCtlEntry.

        Refer to the corresponding traceRouteResultsOperStatus to
        determine the operational state of the test defined by
        this entry."





     DEFVAL { disabled }
    ::= { traceRouteCtlEntry 21 }

 traceRouteCtlDescr OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The purpose of this object is to provide a
        descriptive name of the remote traceroute
        test."
    DEFVAL { '00'H }
    ::= { traceRouteCtlEntry 22 }

 traceRouteCtlMaxRows OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "rows"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The maximum number of entries allowed in the
        traceRouteProbeHistoryTable.  An implementation of
        this MIB will remove the oldest entry in the
        traceRouteProbeHistoryTable to allow the addition
        of an new entry once the number of rows in the
        traceRouteProbeHistoryTable reaches this value.

        Old entries are not removed when a new test is
        started.  Entries are added to the
        traceRouteProbeHistoryTable until traceRouteCtlMaxRows
        is reached before entries begin to be removed.

        A value of 0 for this object disables creation of
        traceRouteProbeHistoryTable entries."
    DEFVAL      { 50 }
    ::= { traceRouteCtlEntry 23 }

 traceRouteCtlTrapGeneration OBJECT-TYPE
    SYNTAX      BITS {
                  pathChange(0),
                  testFailure(1),
                  testCompletion(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object determines when and if to
        to generate a notification for this entry:





        pathChange(0)     - Generate a traceRoutePathChange
            notification when the current path varies from a
            previously determined path.
        testFailure(1)    - Generate a traceRouteTestFailed
            notification when the full path to a target
            can't be determined.
        testCompletion(2) - Generate a traceRouteTestCompleted
            notification when the path to a target has been
            determined.

        The value of this object defaults to zero, indicating
        that none of the above options have been selected."
    ::= { traceRouteCtlEntry 24 }

 traceRouteCtlCreateHopsEntries OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The current path for a traceroute test is kept in the
        traceRouteHopsTable on a per hop basis when the value of
        this object is true(1)."
    DEFVAL { false }
    ::= { traceRouteCtlEntry 25 }

 traceRouteCtlType OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object is used either to report or
        select the implementation method to be used for
        performing a traceroute operation. The value of this
        object may be selected from
        traceRouteImplementationTypeDomains.

        Additional implementation types should be allocated as
        required by implementers of the DISMAN-TRACEROUTE-MIB
        under their enterprise specific registration point and
        not beneath traceRouteImplementationTypeDomains."
    DEFVAL { traceRouteUsingUdpProbes }
    ::= { traceRouteCtlEntry 26 }

 traceRouteCtlRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION





        "This object allows entries to be created and deleted
        in the traceRouteCtlTable.  Deletion of an entry in
        this table results in all corresponding (same
        traceRouteCtlOwnerIndex and traceRouteCtlTestName
        index values) traceRouteResultsTable,
        traceRouteProbeHistoryTable, and traceRouteHopsTable
        entries being deleted.

        A value MUST be specified for traceRouteCtlTargetAddress
        prior to a transition to active(1) state being
        accepted.

        Activation of a remote traceroute operation is
        controlled via traceRouteCtlAdminStatus and not
        by transitioning of this object's value to active(1).

        Transitions in and out of active(1) state are not
        allowed while an entry's traceRouteResultsOperStatus
        is active(1) with the exception that deletion of
        an entry in this table by setting its RowStatus
        object to destroy(6) will stop an active
        traceroute operation.

        The operational state of an traceroute operation
        can be determined by examination of the corresponding
        traceRouteResultsOperStatus object."
    REFERENCE
        "See definition of RowStatus in RFC 2579, 'Textual
        Conventions for SMIv2.'"
    ::= { traceRouteCtlEntry 27 }


 -- Traceroute Results Table

 traceRouteResultsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TraceRouteResultsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines the Remote Operations Traceroute Results Table for
        keeping track of the status of a traceRouteCtlEntry.

        An entry is added to the traceRouteResultsTable when an
        traceRouteCtlEntry is started by successful transition
        of its traceRouteCtlAdminStatus object to enabled(1).
        An entry is removed from the traceRouteResultsTable when
        its corresponding traceRouteCtlEntry is deleted."
   ::= { traceRouteObjects 3 }





 traceRouteResultsEntry OBJECT-TYPE
    SYNTAX      TraceRouteResultsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines an entry in the traceRouteResultsTable.  The
        traceRouteResultsTable has the same indexing as the
        traceRouteCtlTable in order for a traceRouteResultsEntry
        to correspond to the traceRouteCtlEntry that caused it to
        be created."
    INDEX {
            traceRouteCtlOwnerIndex,
            traceRouteCtlTestName
          }
    ::= { traceRouteResultsTable 1 }

 TraceRouteResultsEntry ::=
    SEQUENCE {
      traceRouteResultsOperStatus       INTEGER,
      traceRouteResultsCurHopCount      Gauge32,
      traceRouteResultsCurProbeCount    Gauge32,
      traceRouteResultsIpTgtAddrType    InetAddressType,
      traceRouteResultsIpTgtAddr        InetAddress,
      traceRouteResultsTestAttempts     Unsigned32,
      traceRouteResultsTestSuccesses    Unsigned32,
      traceRouteResultsLastGoodPath     DateAndTime
    }

 traceRouteResultsOperStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                          enabled(1), -- test is in progress
                          disabled(2) -- test has stopped
                        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reflects the operational state of an traceRouteCtlEntry:

           enabled(1)  - Test is active.
           disabled(2) - Test has stopped."
    ::= { traceRouteResultsEntry 1 }

 traceRouteResultsCurHopCount OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "hops"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION





        "Reflects the current TTL value (range from 1 to
        255) for a remote traceroute operation.
        Maximum TTL value is determined by
        traceRouteCtlMaxTtl."
    ::= { traceRouteResultsEntry 2 }

 traceRouteResultsCurProbeCount OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "probes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reflects the current probe count (1..10) for
        a remote traceroute operation. The maximum
        probe count is determined by
        traceRouteCtlProbesPerHop."
    ::= { traceRouteResultsEntry 3 }

 traceRouteResultsIpTgtAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This objects indicates the type of address stored
        in the corresponding traceRouteResultsIpTgtAddr
        object."
    ::= { traceRouteResultsEntry 4 }

 traceRouteResultsIpTgtAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This objects reports the IP address associated
        with a traceRouteCtlTargetAddress value when the
        destination address is specified as a DNS name.
        The value of this object should be a zero length
        octet string when a DNS name is not specified or
        when a specified DNS name fails to resolve."
    ::= { traceRouteResultsEntry 5 }

 traceRouteResultsTestAttempts OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "tests"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current number of attempts to determine a path





        to a target.  The value of this object MUST be started
        at 0."
    ::= { traceRouteResultsEntry 6 }

 traceRouteResultsTestSuccesses OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "tests"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current number of attempts to determine a path
        to a target that have succeeded.  The value of this
        object MUST be reported as 0 when no attempts have
        succeeded."
    ::= { traceRouteResultsEntry 7 }

 traceRouteResultsLastGoodPath OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The date and time when the last complete path
        was determined."
    ::= { traceRouteResultsEntry 8 }

 -- Trace Route Probe History Table

 traceRouteProbeHistoryTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TraceRouteProbeHistoryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines the Remote Operations Traceroute Results Table for
        storing the results of a traceroute operation.

        An implementation of this MIB will remove the oldest
        entry in the traceRouteProbeHistoryTable to allow the
        addition of an new entry once the number of rows in
        the traceRouteProbeHistoryTable reaches the value specified
        by traceRouteCtlMaxRows."
   ::= { traceRouteObjects 4 }

 traceRouteProbeHistoryEntry OBJECT-TYPE
    SYNTAX      TraceRouteProbeHistoryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines a table for storing the results of a traceroute





        operation.  Entries in this table are limited by
        the value of the corresponding traceRouteCtlMaxRows
        object.

        The first two index elements identify the
        traceRouteCtlEntry that a traceRouteProbeHistoryEntry
        belongs to.  The third index element selects a single
        traceroute operation result.  The fourth and fifth indexes
        select the hop and the probe for a particular
        traceroute operation."
    INDEX {
             traceRouteCtlOwnerIndex,
             traceRouteCtlTestName,
             traceRouteProbeHistoryIndex,
             traceRouteProbeHistoryHopIndex,
             traceRouteProbeHistoryProbeIndex
          }
    ::= { traceRouteProbeHistoryTable 1 }

 TraceRouteProbeHistoryEntry ::=
    SEQUENCE {
      traceRouteProbeHistoryIndex         Unsigned32,
      traceRouteProbeHistoryHopIndex      Unsigned32,
      traceRouteProbeHistoryProbeIndex    Unsigned32,
      traceRouteProbeHistoryHAddrType     InetAddressType,
      traceRouteProbeHistoryHAddr         InetAddress,
      traceRouteProbeHistoryResponse      Unsigned32,
      traceRouteProbeHistoryStatus        OperationResponseStatus,
      traceRouteProbeHistoryLastRC        Integer32,
      traceRouteProbeHistoryTime          DateAndTime
    }

 traceRouteProbeHistoryIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..'ffffffff'h)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in this table is created when the result of
        a traceroute probe is determined.  The initial 2 instance
        identifier index values identify the traceRouteCtlEntry
        that a probe result (traceRouteProbeHistoryEntry) belongs
        to.  An entry is removed from this table when
        its corresponding traceRouteCtlEntry is deleted.

        An implementation MUST start assigning
        traceRouteProbeHistoryIndex values at 1 and wrap after
        exceeding the maximum possible value as defined by the
        limit of this object ('ffffffff'h)."





    ::= { traceRouteProbeHistoryEntry 1 }

 traceRouteProbeHistoryHopIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Indicates which hop in a traceroute path that the probe's
       results are for.  The value of this object is initially
       determined by the value of traceRouteCtlInitialTtl."
    ::= { traceRouteProbeHistoryEntry 2 }

 traceRouteProbeHistoryProbeIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..10)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Indicates the index of a probe for a particular
       hop in a traceroute path.  The number of probes per
       hop is determined by the value of the corresponding
       traceRouteCtlProbesPerHop object."
    ::= { traceRouteProbeHistoryEntry 3 }

 traceRouteProbeHistoryHAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This objects indicates the type of address stored
        in the corresponding traceRouteProbeHistoryHAddr
        object."
    ::= { traceRouteProbeHistoryEntry 4 }

 traceRouteProbeHistoryHAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The address of a hop in a traceroute path.  This object
       is not allowed to be a DNS name.  The value of the
       corresponding object, traceRouteProbeHistoryHAddrType,
       indicates this object's IP address type."
    ::= { traceRouteProbeHistoryEntry 5 }

 traceRouteProbeHistoryResponse OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only





    STATUS      current
    DESCRIPTION
        "The amount of time measured in milliseconds from when
        a probe was sent to when its response was received or
        when it timed out.  The value of this object is reported
        as 0 when it is not possible to transmit a probe."
    ::= { traceRouteProbeHistoryEntry 6 }

 traceRouteProbeHistoryStatus OBJECT-TYPE
    SYNTAX      OperationResponseStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The result of a traceroute operation made by a remote
        host for a particular probe."
    ::= { traceRouteProbeHistoryEntry 7 }

 traceRouteProbeHistoryLastRC OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The last implementation method specific reply code received.

        Traceroute is usually implemented by transmitting a series of
        probe packets with increasing time-to-live values.  A probe
        packet is a UDP datagram encapsulated into an IP packet.
        Each hop in a path to the target (destination) host rejects
        the probe packets (probe's TTL too small, ICMP reply) until
        either the maximum TTL is exceeded or the target host is
        received."
    ::= { traceRouteProbeHistoryEntry 8 }

 traceRouteProbeHistoryTime OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Timestamp for when this probe results were determined."
    ::= { traceRouteProbeHistoryEntry 9 }

 -- Traceroute Hop Results Table

 traceRouteHopsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TraceRouteHopsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION





        "Defines the Remote Operations Traceroute Hop Table for
        keeping track of the results of traceroute tests on a
        per hop basis."
    ::= { traceRouteObjects 5 }

 traceRouteHopsEntry OBJECT-TYPE
    SYNTAX      TraceRouteHopsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines an entry in the traceRouteHopsTable.

        The first two index elements identify the
        traceRouteCtlEntry that a traceRouteHopsEntry
        belongs to.  The third index element,
        traceRouteHopsHopIndex, selects a
        hop in a traceroute path."
    INDEX {
            traceRouteCtlOwnerIndex,
            traceRouteCtlTestName,
            traceRouteHopsHopIndex
          }
    ::= { traceRouteHopsTable 1 }

 TraceRouteHopsEntry ::=
    SEQUENCE {
        traceRouteHopsHopIndex         Unsigned32,
        traceRouteHopsIpTgtAddressType InetAddressType,
        traceRouteHopsIpTgtAddress     InetAddress,
        traceRouteHopsMinRtt           Unsigned32,
        traceRouteHopsMaxRtt           Unsigned32,
        traceRouteHopsAverageRtt       Unsigned32,
        traceRouteHopsRttSumOfSquares  Unsigned32,
        traceRouteHopsSentProbes       Unsigned32,
        traceRouteHopsProbeResponses   Unsigned32,
        traceRouteHopsLastGoodProbe    DateAndTime
      }

 traceRouteHopsHopIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Specifies the hop index for a traceroute hop.  Values
        for this object with respect to the same
        traceRouteCtlOwnerIndex and traceRouteCtlTestName
        MUST start at 1 and increase monotonically.






        The traceRouteHopsTable keeps the current traceroute
        path per traceRouteCtlEntry if enabled by
        setting the corresponding traceRouteCtlCreateHopsEntries
        to true(1).

        All hops (traceRouteHopsTable entries) in a traceroute
        path MUST be updated at the same time when a traceroute
        operation completes.  Care needs to be applied when either
        a path changes or can't be determined.  The initial portion
        of the path, up to the first hop change, MUST retain the
        same traceRouteHopsHopIndex values.  The remaining portion
        of the path SHOULD be assigned new traceRouteHopsHopIndex
        values."
    ::= { traceRouteHopsEntry 1 }

 traceRouteHopsIpTgtAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This objects indicates the type of address stored
        in the corresponding traceRouteHopsIpTargetAddress
        object."
    ::= { traceRouteHopsEntry 2 }

 traceRouteHopsIpTgtAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reports the IP address associated with
        the hop.  A value for this object should be reported
        as a numeric IP address and not as a DNS name."
    ::= { traceRouteHopsEntry 3 }

 traceRouteHopsMinRtt OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minimum traceroute round-trip-time (RTT) received for
        this hop.  A value of 0 for this object implies that no
        RTT has been received."
    ::= { traceRouteHopsEntry 4 }

 traceRouteHopsMaxRtt OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only





    STATUS      current
    DESCRIPTION
        "The maximum traceroute round-trip-time (RTT) received for
        this hop.  A value of 0 for this object implies that no
        RTT has been received."
    ::= { traceRouteHopsEntry 5 }

 traceRouteHopsAverageRtt OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current average traceroute round-trip-time (RTT) for
        this hop."
    ::= { traceRouteHopsEntry 6 }

 traceRouteHopsRttSumOfSquares OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object contains the sum of all traceroute responses
        received for this hop.  Its purpose is to enable standard
        deviation calculation."
    ::= { traceRouteHopsEntry 7 }

 traceRouteHopsSentProbes OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of this object reflects the number of probes sent
        for this hop during this traceroute test.  The value of this
        object should start at 0."
    ::= { traceRouteHopsEntry 8 }

 traceRouteHopsProbeResponses OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of responses received for this hop during this
        traceroute test.  This value of this object should start
        at 0."
    ::= { traceRouteHopsEntry 9 }

 traceRouteHopsLastGoodProbe OBJECT-TYPE
    SYNTAX      DateAndTime





    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Date and time was the last response was received for a probe
        for this hop during this traceroute test."
    ::= { traceRouteHopsEntry 10 }

 -- Notification Definition section

 traceRoutePathChange NOTIFICATION-TYPE
      OBJECTS {
        traceRouteCtlTargetAddressType,
        traceRouteCtlTargetAddress,
        traceRouteResultsIpTgtAddrType,
        traceRouteResultsIpTgtAddr
      }
      STATUS  current
      DESCRIPTION
          "The path to a target has changed."
      ::= { traceRouteNotifications 1 }

 traceRouteTestFailed NOTIFICATION-TYPE
      OBJECTS {
        traceRouteCtlTargetAddressType,
        traceRouteCtlTargetAddress,
        traceRouteResultsIpTgtAddrType,
        traceRouteResultsIpTgtAddr
      }
      STATUS  current
      DESCRIPTION
          "Could not determine the path to a target."
      ::= { traceRouteNotifications 2 }

 traceRouteTestCompleted NOTIFICATION-TYPE
      OBJECTS {
        traceRouteCtlTargetAddressType,
        traceRouteCtlTargetAddress,
        traceRouteResultsIpTgtAddrType,
        traceRouteResultsIpTgtAddr
      }
      STATUS  current
      DESCRIPTION
          "The path to a target has just been determined."
      ::= { traceRouteNotifications 3 }

 -- Conformance information
 -- Compliance statements






 traceRouteCompliances OBJECT IDENTIFIER ::= { traceRouteConformance 1 }
 traceRouteGroups      OBJECT IDENTIFIER ::= { traceRouteConformance 2 }

 -- Compliance statements

 traceRouteCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for the DISMAN-TRACEROUTE-MIB."
    MODULE  -- this module
        MANDATORY-GROUPS {
                            traceRouteGroup
                          }
        GROUP traceRouteTimeStampGroup
        DESCRIPTION
            "This group is mandatory for implementations that have
            access to a system clock and are capable of setting
            the values for DateAndTime objects."

        GROUP traceRouteNotificationsGroup
        DESCRIPTION
            "This group defines a collection of optional
            notifications."

        GROUP traceRouteHopsTableGroup
        DESCRIPTION
            "This group lists the objects that make up a
            traceRouteHopsEntry.  Support of the traceRouteHopsTable
            is optional."

        OBJECT traceRouteMaxConcurrentRequests
        MIN-ACCESS  read-only
        DESCRIPTION
            "The agent is not required to support SET
            operations to this object."

        OBJECT traceRouteCtlByPassRouteTable
        MIN-ACCESS  read-only
        DESCRIPTION
            "This object is not required by implementations that
            are not capable of its implementation.  The function
            represented by this object is implementable if the
            setsockopt SOL_SOCKET SO_DONTROUTE option is
            supported."

        OBJECT traceRouteCtlSourceAddressType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        MIN-ACCESS  read-only





        DESCRIPTION
            "This object is not required by implementations that
            are not capable of binding the send socket with a
            source address. An implementation is only required to
            support IPv4 and IPv6 addresses."

        OBJECT traceRouteCtlSourceAddress
        SYNTAX  InetAddress (SIZE(0|4|16))
        MIN-ACCESS  read-only
        DESCRIPTION
            "This object is not required by implementations that
            are not capable of binding the send socket with a
            source address. An implementation is only required to
            support IPv4 and globally unique IPv6 addresses."

        OBJECT traceRouteCtlIfIndex
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  When write access is
            not supported return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlMiscOptions
        MIN-ACCESS  read-only
        DESCRIPTION
            "Support of this object is optional.  When not
            supporting do not allow write access and return a
            zero length octet string as the value of the object."

        OBJECT traceRouteCtlStorageType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  It is also allowed
            for implementations to support only the volatile
            StorageType enumeration."

        OBJECT traceRouteCtlDSField
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.   When write access is
            not supported return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlType
        MIN-ACCESS  read-only
        DESCRIPTION





            "Write access is not required.  In addition, the only
            value that is RECOMMENDED to be supported by an
            implementation is traceRouteUsingUdpProbes."

        OBJECT traceRouteResultsIpTgtAddrType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteResultsIpTgtAddr
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteProbeHistoryHAddrType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."
        OBJECT traceRouteProbeHistoryHAddr
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteHopsIpTgtAddressType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteHopsIpTgtAddress
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."
    ::= { traceRouteCompliances 1 }

 -- MIB groupings

 traceRouteGroup OBJECT-GROUP
   OBJECTS {
             traceRouteMaxConcurrentRequests,
             traceRouteCtlTargetAddressType,
             traceRouteCtlTargetAddress,
             traceRouteCtlByPassRouteTable,





             traceRouteCtlDataSize,
             traceRouteCtlTimeOut,
             traceRouteCtlProbesPerHop,
             traceRouteCtlPort,
             traceRouteCtlMaxTtl,
             traceRouteCtlDSField,
             traceRouteCtlSourceAddressType,
             traceRouteCtlSourceAddress,
             traceRouteCtlIfIndex,
             traceRouteCtlMiscOptions,
             traceRouteCtlMaxFailures,
             traceRouteCtlDontFragment,
             traceRouteCtlInitialTtl,
             traceRouteCtlFrequency,
             traceRouteCtlStorageType,
             traceRouteCtlAdminStatus,
             traceRouteCtlMaxRows,
             traceRouteCtlTrapGeneration,
             traceRouteCtlDescr,
             traceRouteCtlCreateHopsEntries,
             traceRouteCtlType,
             traceRouteCtlRowStatus,
             traceRouteResultsOperStatus,
             traceRouteResultsCurHopCount,
             traceRouteResultsCurProbeCount,
             traceRouteResultsIpTgtAddrType,
             traceRouteResultsIpTgtAddr,
             traceRouteResultsTestAttempts,
             traceRouteResultsTestSuccesses,
             traceRouteProbeHistoryHAddrType,
             traceRouteProbeHistoryHAddr,
             traceRouteProbeHistoryResponse,
             traceRouteProbeHistoryStatus,
             traceRouteProbeHistoryLastRC
          }
   STATUS  current
   DESCRIPTION
       "The group of objects that comprise the remote traceroute
       operation."
   ::= { traceRouteGroups 1 }

 traceRouteTimeStampGroup OBJECT-GROUP
   OBJECTS {
             traceRouteResultsLastGoodPath,
             traceRouteProbeHistoryTime
           }
   STATUS  current
   DESCRIPTION





       "The group of DateAndTime objects."
    ::= { traceRouteGroups 2 }

 traceRouteNotificationsGroup NOTIFICATION-GROUP
   NOTIFICATIONS {
             traceRoutePathChange,
             traceRouteTestFailed,
             traceRouteTestCompleted
          }
   STATUS   current
   DESCRIPTION
       "The notifications which are required to be supported by
       implementations of this MIB."
   ::= { traceRouteGroups 3 }

 traceRouteHopsTableGroup OBJECT-GROUP
   OBJECTS {
             traceRouteHopsIpTgtAddressType,
             traceRouteHopsIpTgtAddress,
             traceRouteHopsMinRtt,
             traceRouteHopsMaxRtt,
             traceRouteHopsAverageRtt,
             traceRouteHopsRttSumOfSquares,
             traceRouteHopsSentProbes,
             traceRouteHopsProbeResponses,
             traceRouteHopsLastGoodProbe
           }
    STATUS   current
    DESCRIPTION
        "The group of objects that comprise the traceRouteHopsTable."
  ::= { traceRouteGroups 4 }

END


