IPV6-TC DEFINITIONS ::= BEGIN


        IMPORTS
             Integer32                FROM SNMPv2-SMI
             TEXTUAL-CONVENTION       FROM SNMPv2-TC;


        -- definition of textual conventions
        Ipv6Address ::= TEXTUAL-CONVENTION
             DISPLAY-HINT "2x:"
             STATUS       current
             DESCRIPTION
               "This data type is used to model IPv6 addresses.
                This is a binary string of 16 octets in network
                byte-order."
             SYNTAX       OCTET STRING (SIZE (16))

        Ipv6AddressPrefix ::= TEXTUAL-CONVENTION
             DISPLAY-HINT "2x:"
             STATUS       current
             DESCRIPTION
               "This data type is used to model IPv6 address
               prefixes. This is a binary string of up to 16
               octets in network byte-order."
             SYNTAX       OCTET STRING (SIZE (0..16))

        Ipv6AddressIfIdentifier ::= TEXTUAL-CONVENTION
             DISPLAY-HINT "2x:"
             STATUS       current
             DESCRIPTION
               "This data type is used to model IPv6 address
               interface identifiers. This is a binary string
                of up to 8 octets in network byte-order."
             SYNTAX      OCTET STRING (SIZE (0..8))

        Ipv6IfIndex ::= TEXTUAL-CONVENTION
             DISPLAY-HINT "d"
             STATUS       current
             DESCRIPTION
               "A unique value, greater than zero for each
               internetwork-layer interface in the managed
               system. It is recommended that values are assigned
               contiguously starting from 1. The value for each
               internetwork-layer interface must remain constant
               at least from one re-initialization of the entity's
               network management system to the next





               re-initialization."
             SYNTAX       Integer32 (1..2147483647)

        Ipv6IfIndexOrZero ::= TEXTUAL-CONVENTION
             DISPLAY-HINT "d"
             STATUS       current
             DESCRIPTION
                 "This textual convention is an extension of the
                 Ipv6IfIndex convention.  The latter defines
                 a greater than zero value used to identify an IPv6
                 interface in the managed system.  This extension
                 permits the additional value of zero.  The value
                 zero is object-specific and must therefore be
                 defined as part of the description of any object
                 which uses this syntax.  Examples of the usage of
                 zero might include situations where interface was
                 unknown, or when none or all interfaces need to be
                 referenced."
             SYNTAX       Integer32 (0..2147483647)

        END


