SFLOW-MIB DEFINITIONS ::= BEGIN


IMPORTS

MODULE-IDENTITY, OBJECT-TYPE, Integer32, enterprises
        FROM SNMPv2-SMI
SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
OwnerString
        FROM RMON-MIB
InetAddressType, InetAddress
        FROM INET-ADDRESS-MIB
MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF;

sFlowMIB  MODULE-IDENTITY
  LAST-UPDATED "200105150000Z"   -- May 15, 2001
  ORGANIZATION "InMon Corp."
  CONTACT-INFO





         "Peter Phaal
          InMon Corp.
          http://www.inmon.com/

          Tel:  +1-415-661-6343
          Email: peter_phaal@inmon.com"
  DESCRIPTION
          "The MIB module for managing the generation and transportation
           of sFlow data records."

  --
  -- Revision History
  --
  REVISION    "200105150000Z"     -- May 15, 2001
  DESCRIPTION
          "Version 1.2

           Brings MIB into SMI v2 compliance."

  REVISION    "200105010000Z"      -- May 1, 2001
  DESCRIPTION
           "Version 1.1

            Adds sFlowDatagramVersion."
  ::= { enterprises 4300 1 }

sFlowAgent OBJECT IDENTIFIER ::= { sFlowMIB 1 }

sFlowVersion OBJECT-TYPE
     SYNTAX      SnmpAdminString
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
       "Uniquely identifies the version and implementation of this MIB.
        The version string must have the following structure:
           <MIB Version>;<Organization>;<Software Revision>
        where:
           <MIB Version>  must be '1.2', the version of this MIB.
           <Organization> the name of the organization responsible
                            for the agent implementation.
           <Revision>     the specific software build of this agent.

        As an example, the string '1.2;InMon Corp.;2.1.1' indicates
        that this agent implements version '1.2' of the SFLOW MIB, that
        it was developed by 'InMon Corp.' and that the software build
        is '2.1.1'.

        The MIB Version will change with each revision of the SFLOW





        MIB.

        Management entities must check the MIB Version and not attempt
        to manage agents with MIB Versions greater than that for which
        they were designed.

        Note: The sFlow Datagram Format has an independent version
              number which may change independently from <MIB Version>.
              <MIB Version> applies to the structure and semantics of
              the SFLOW MIB only."
     DEFVAL { "1.2;;" }
     ::= { sFlowAgent 1 }

sFlowAgentAddressType OBJECT-TYPE
     SYNTAX      InetAddressType
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
       "The address type of the address associated with this agent.
        Only ipv4 and ipv6 types are supported."
     ::= { sFlowAgent 2 }

sFlowAgentAddress OBJECT-TYPE
     SYNTAX      InetAddress
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
       "The IP address associated with this agent.  In the case of a
        multi-homed agent, this should be the loopback address of the
        agent.  The sFlowAgent address must provide SNMP connectivity
        to the agent.  The address should be an invariant that does not
        change as interfaces are reconfigured, enabled, disabled,
        added or removed.  A manager should be able to use the
        sFlowAgentAddress as a unique key that will identify this
        agent over extended periods of time so that a history can
        be maintained."
    ::= { sFlowAgent 3 }

sFlowTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF SFlowEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
       "A table of the sFlow samplers within a device."
     ::= { sFlowAgent 4 }

sFlowEntry OBJECT-TYPE
     SYNTAX      SFlowEntry





     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
       "Attributes of an sFlow sampler."
     INDEX { sFlowDataSource }
     ::= { sFlowTable 1 }

SFlowEntry ::= SEQUENCE {
     sFlowDataSource               OBJECT IDENTIFIER,
     sFlowOwner                    OwnerString,
     sFlowTimeout                  Integer32,
     sFlowPacketSamplingRate       Integer32,
     sFlowCounterSamplingInterval  Integer32,
     sFlowMaximumHeaderSize        Integer32,
     sFlowMaximumDatagramSize      Integer32,
     sFlowCollectorAddressType     InetAddressType,
     sFlowCollectorAddress         InetAddress,
     sFlowCollectorPort            Integer32,
     sFlowDatagramVersion          Integer32
}

sFlowDataSource OBJECT-TYPE
     SYNTAX      OBJECT IDENTIFIER
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
       "Identifies the source of the data for the sFlow sampler.
       The following data source types are currently defined:

       - ifIndex.<I>
       DataSources of this traditional form are called 'port-based'.
       Ideally the sampling entity will perform sampling on all flows
       originating from or destined to the specified interface.
       However, if the switch architecture only permits input or
       output sampling then the sampling agent is permitted to only
       sample input flows input or output flows.  Each packet must
       only be considered once for sampling, irrespective of the
       number of ports it will be forwarded to.

       Note: Port 0 is used to indicate that all ports on the device
             are represented by a single data source.
             - sFlowPacketSamplingRate applies to all ports on the
               device capable of packet sampling.
             - sFlowCounterSamplingInterval applies to all ports.

       - smonVlanDataSource.<V>
       A dataSource of this form refers to a 'Packet-based VLAN'
       and is called a 'VLAN-based' dataSource.  <V> is the VLAN





       ID as defined by the IEEE 802.1Q standard.  The
       value is between 1 and 4094 inclusive, and it represents
       an 802.1Q VLAN-ID with global scope within a given
       bridged domain.
       Sampling is performed on all packets received that are part
       of the specified VLAN (no matter which port they arrived on).
       Each packet will only be considered once for sampling,
       irrespective of the number of ports it will be forwarded to.

       - entPhysicalEntry.<N>
       A dataSource of this form refers to a physical entity within
       the agent (e.g., entPhysicalClass = backplane(4)) and is called
       an 'entity-based' dataSource.
       Sampling is performed on all packets entering the resource (e.g.
       If the backplane is being sampled, all packets transmitted onto
       the backplane will be considered as single candidates for
       sampling irrespective of the number of ports they ultimately
       reach).

       Note: Since each DataSource operates independently, a packet
             that crosses multiple DataSources may generate multiple
             flow records."
     ::= { sFlowEntry 1 }

sFlowOwner OBJECT-TYPE
     SYNTAX      OwnerString
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
       "The entity making use of this sFlow sampler.  The empty string
        indicates that the sFlow sampler is currently unclaimed.
        An entity wishing to claim an sFlow sampler must make sure
        that the sampler is unclaimed before trying to claim it.
        The sampler is claimed by setting the owner string to identify
        the entity claiming the sampler.  The sampler must be claimed
        before any changes can be made to other sampler objects.

        In order to avoid a race condition, the entity taking control
        of the sampler must set both the owner and a value for
        sFlowTimeout in the same SNMP set request.

        When a management entity is finished using the sampler,
        it should set its value back to unclaimed.  The agent
        must restore all other entities this row to their
        default values when the owner is set to unclaimed.

        This mechanism provides no enforcement and relies on the
        cooperation of management entities in order to ensure that





        competition for a sampler is fairly resolved."
     DEFVAL { "" }
     ::= { sFlowEntry 2 }

sFlowTimeout OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
       "The time (in seconds) remaining before the sampler is released
        and stops sampling.  When set, the owner establishes control
        for the specified period.  When read, the remaining time in the
        interval is returned.

        A management entity wanting to maintain control of the sampler
        is responsible for setting a new value before the old one
        expires.

        When the interval expires, the agent is responsible for
        restoring all other entities in this row to their default
        values."
     DEFVAL { 0 }
     ::= { sFlowEntry 3 }

sFlowPacketSamplingRate OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
       "The statistical sampling rate for packet sampling from this
        source.

        Set to N to sample 1/Nth of the packets in the monitored flows.
        An agent should choose its own algorithm introduce variance
        into the sampling so that exactly every Nth packet is not
        counted.  A sampling rate of 1 counts all packets.  A sampling
        rate of 0 disables sampling.

        The agent is permitted to have minimum and maximum allowable
        values for the sampling rate.  A minimum rate lets the agent
        designer set an upper bound on the overhead associated with
        sampling, and a maximum rate may be the result of hardware
        restrictions (such as counter size).  In addition not all values
        between the maximum and minimum may be realizable as the
        sampling rate (again because of implementation considerations).

        When the sampling rate is set the agent is free to adjust the
        value so that it lies between the maximum and minimum values





        and has the closest achievable value.

        When read, the agent must return the actual sampling rate it
        will be using (after the adjustments previously described).  The
        sampling algorithm must converge so that over time the number
        of packets sampled approaches 1/Nth of the total number of
        packets in the monitored flows."
     DEFVAL { 0 }
     ::= { sFlowEntry 4 }

sFlowCounterSamplingInterval OBJECT-TYPE
  SYNTAX      Integer32
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
       "The maximum number of seconds between successive samples of the
        counters associated with this data source.  A sampling interval
        of 0 disables counter sampling."
     DEFVAL { 0 }
     ::= { sFlowEntry 5 }

sFlowMaximumHeaderSize OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
       "The maximum number of bytes that should be copied from a
        sampled packet.  The agent may have an internal maximum and
        minimum permissible sizes.  If an attempt is made to set this
        value outside the permissible range then the agent should
        adjust the value to the closest permissible value."
     DEFVAL { 128 }
     ::= { sFlowEntry 6 }

sFlowMaximumDatagramSize OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "The maximum number of data bytes that can be sent in a single
         sample datagram.  The manager should set this value to avoid
         fragmentation of the sFlow datagrams."
     DEFVAL { 1400 }
     ::= { sFlowEntry 7 }

sFlowCollectorAddressType OBJECT-TYPE
     SYNTAX      InetAddressType
     MAX-ACCESS  read-write





     STATUS      current
     DESCRIPTION
       "The type of sFlowCollectorAddress."
     DEFVAL { ipv4 }
     ::= { sFlowEntry 8 }

sFlowCollectorAddress OBJECT-TYPE
     SYNTAX      InetAddress
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
       "The IP address of the sFlow collector.
        If set to 0.0.0.0 all sampling is disabled."
     DEFVAL { "0.0.0.0" }
     ::= { sFlowEntry 9 }

sFlowCollectorPort OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
       "The destination port for sFlow datagrams."
     DEFVAL { 6343 }
     ::= { sFlowEntry 10 }

sFlowDatagramVersion OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
       "The version of sFlow datagrams that should be sent.

        When set to a value not support by the agent, the agent should
        adjust the value to the highest supported value less than the
        requested value, or return an error if no such values exist."
     DEFVAL { 4 }
     ::= { sFlowEntry 11 }

 --
 -- Compliance Statements
 --

sFlowMIBConformance OBJECT IDENTIFIER ::= { sFlowMIB 2 }
sFlowMIBGroups      OBJECT IDENTIFIER ::= { sFlowMIBConformance 1 }
sFlowMIBCompliances OBJECT IDENTIFIER ::= { sFlowMIBConformance 2 }

sFlowCompliance MODULE-COMPLIANCE
     STATUS      current





     DESCRIPTION
       "Compliance statements for the sFlow Agent."

     MODULE -- this module
         MANDATORY-GROUPS { sFlowAgentGroup }
         OBJECT     sFlowAgentAddressType
         SYNTAX     InetAddressType { ipv4(1) }
         DESCRIPTION
           "Agents need only support ipv4."

         OBJECT sFlowCollectorAddressType
         SYNTAX InetAddressType { ipv4(1) }
         DESCRIPTION
           "Agents need only support ipv4."

     ::= { sFlowMIBCompliances 1 }

sFlowAgentGroup OBJECT-GROUP
     OBJECTS { sFlowVersion, sFlowAgentAddressType, sFlowAgentAddress,
               sFlowDataSource, sFlowOwner, sFlowTimeout,
               sFlowPacketSamplingRate, sFlowCounterSamplingInterval,
               sFlowMaximumHeaderSize, sFlowMaximumDatagramSize,
               sFlowCollectorAddressType, sFlowCollectorAddress,
               sFlowCollectorPort, sFlowDatagramVersion }
      STATUS current
      DESCRIPTION
        "A collection of objects for managing the generation and
         transportation of sFlow data records."
       ::= { sFlowMIBGroups 1 }

END

   
