IANA-PWE3-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, mib-2
          FROM SNMPv2-SMI -- [RFC2578]

       TEXTUAL-CONVENTION
          FROM SNMPv2-TC; -- [RFC2579]

   ianaPwe3MIB  MODULE-IDENTITY
       LAST-UPDATED "200906110000Z"  -- 11 June 2009 00:00:00 GMT
       ORGANIZATION "IANA"
       CONTACT-INFO
            "Internet Assigned Numbers Authority
            Internet Corporation for Assigned Names and Numbers
            4676 Admiralty Way, Suite 330
            Marina del Rey, CA 90292-6601

            Phone: +1 310 823 9358
            EMail: iana@iana.org"
       DESCRIPTION
           "This MIB module defines the IANAPwTypeTC and
           IANAPwPsnTypeTC textual conventions for use in PWE3
           MIB modules.

           Any additions or changes to the contents of this MIB
           module require either publication of an RFC, Designated
           Expert Review as defined in RFC 5226, Guidelines for
           Writing an IANA Considerations Section in RFCs, and should
           be based on the procedures defined in [RFC4446].  The
           Designated Expert will be selected by the IESG Area
           Director(s) of the internet Area.

           Copyright (c) 2009 IETF Trust and the persons identified as
           authors of the code.  All rights reserved.

           Redistribution and use in source and binary forms, with or
           without modification, are permitted provided that the





           following conditions are met:

           - Redistributions of source code must retain the above
             copyright notice, this list of conditions and the
             following disclaimer.

           - Redistributions in binary form must reproduce the above
             copyright notice, this list of conditions and the
             following disclaimer in the documentation and/or other
             materials provided with the distribution.

           - Neither the name of Internet Society, IETF or IETF Trust,
             nor the names of specific contributors, may be used to
             endorse or promote products derived from this software
             without specific prior written permission.

           THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
           CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED WARRANTIES,
           INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
           MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
           DISCLAIMED.  IN NO EVENT SHALL THE COPYRIGHT OWNER OR
           CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
           INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
           (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE
           GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR
           BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF
           LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
           (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT
           OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
           POSSIBILITY OF SUCH DAMAGE. "

       REVISION     "200906110000Z"  -- 11 June 2009 00:00:00 GMT
       DESCRIPTION  "Original version, published as part of RFC 5601."
       ::= { mib-2 174 }

   IANAPwTypeTC ::= TEXTUAL-CONVENTION
      STATUS     current
      DESCRIPTION
         "Indicates the PW type (i.e., the carried service). "
    SYNTAX   INTEGER {
       other(0),
       frameRelayDlciMartiniMode(1),
       atmAal5SduVcc(2),
       atmTransparent(3),
       ethernetTagged(4),
       ethernet(5),
       hdlc(6),
       ppp(7),





       cem(8),  -- Historic type
       atmCellNto1Vcc(9),
       atmCellNto1Vpc(10),
       ipLayer2Transport(11),
       atmCell1to1Vcc(12),
       atmCell1to1Vpc(13),
       atmAal5PduVcc(14),
       frameRelayPortMode(15),
       cep(16),
       e1Satop(17),
       t1Satop(18),
       e3Satop(19),
       t3Satop(20),
       basicCesPsn(21),
       basicTdmIp(22),
       tdmCasCesPsn(23),
       tdmCasTdmIp(24),
       frDlci(25),
       wildcard (32767)
        }

   IANAPwPsnTypeTC ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Identifies the PSN type that the PW will use over the
          network."
      SYNTAX   INTEGER {
         mpls        (1),
         l2tp        (2),
         udpOverIp   (3),
         mplsOverIp  (4),
         mplsOverGre (5),
         other       (6)
         }

   IANAPwCapabilities ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "This TC describes a collection of capabilities related to
          a specific PW.
          Values may be added in the future based on new capabilities
          introduced in IETF documents.
         "
     SYNTAX   BITS {
       pwStatusIndication (0), -- Applicable only if maintenance
                               -- protocol is in use.
       pwVCCV             (1)
     }





   END


