RFC1231-MIB DEFINITIONS ::= BEGIN


          --                 IEEE 802.5 Token Ring MIB

          IMPORTS
                  experimental
                          FROM RFC1155-SMI
                  OBJECT-TYPE
                          FROM RFC-1212;

          --  This MIB Module uses the extended OBJECT-TYPE macro as
          --  defined in [9].



          dot5    OBJECT IDENTIFIER ::= { experimental 4 }

          -- All representations of MAC addresses in this MIB Module
          -- use, as a textual convention (i.e. this convention does
          -- not affect their encoding), the data type:

          MacAddress ::= OCTET STRING (SIZE (6))    -- a 6 octet
                                                    -- address in the
                                                    -- "canonical" order
          -- defined by IEEE 802.1a, i.e., as if it were transmitted
          -- least significant bit first, even though 802.5 (in
          -- contrast to other 802.x protocols) requires MAC addresses
          -- to be transmitted most significant bit first.
          --
          -- 16-bit addresses, if needed, are represented by setting
          -- their upper 4 octets to all 0's, i.e., AAFF would be
          -- represented as 00000000AAFF.



          -- The Interface Table

          -- This table contains state and parameter information which
          -- is specific to 802.5 interfaces.  It is mandatory that
          -- systems having 802.5 interfaces implement this table in
          -- addition to the generic interfaces table [4,6] and its
          -- generic extensions [11].





          dot5Table  OBJECT-TYPE
                     SYNTAX  SEQUENCE OF Dot5Entry
                     ACCESS  not-accessible
                     STATUS  mandatory
                     DESCRIPTION
                             "This table contains Token Ring interface
                             parameters and state variables, one entry
                             per 802.5 interface."
                     ::= { dot5 1 }

          dot5Entry  OBJECT-TYPE
                     SYNTAX  Dot5Entry
                     ACCESS  not-accessible
                     STATUS  mandatory
                     DESCRIPTION
                             "A list of Token Ring status and parameter
                              values for an 802.5 interface."
                     INDEX   { dot5IfIndex }
                     ::= { dot5Table 1 }

          Dot5Entry
              ::= SEQUENCE {
                      dot5IfIndex
                          INTEGER,
                      dot5Commands
                          INTEGER,
                      dot5RingStatus
                          INTEGER,
                      dot5RingState
                          INTEGER,
                      dot5RingOpenStatus
                          INTEGER,
                      dot5RingSpeed
                          INTEGER,
                      dot5UpStream
                          MacAddress,
                      dot5ActMonParticipate
                          INTEGER,
                      dot5Functional
                          MacAddress
                  }

          dot5IfIndex  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The value of this object identifies the





                              802.5 interface for which this entry
                              contains management information.  The
                              value of this object for a particular
                              interface has the same value as the
                              ifIndex object, defined in [4,6],
                              for the same interface."
                     ::= { dot5Entry 1 }

          dot5Commands  OBJECT-TYPE
                     SYNTAX  INTEGER {
                                   no-op(1),
                                   open(2),
                                   reset(3),
                                   close(4)
                             }
                     ACCESS  read-write
                     STATUS  mandatory
                     DESCRIPTION
                             "When this object is set to the value of
                              open(2), the station should go into the
                              open state.  The progress and success of
                              the open is given by the values of the
                              objects dot5RingState and
                              dot5RingOpenStatus.
                                  When this object is set to the value
                              of reset(3), then the station should do
                              a reset.  On a reset, all MIB counters
                              should retain their values, if possible.
                              Other side affects are dependent on the
                              hardware chip set.
                                  When this object is set to the value
                              of close(4), the station should go into
                              the stopped state by removing itself
                              from the ring.
                                  Setting this object to a value of
                              no-op(1) has no effect.
                                  When read, this object always has a
                              value of no-op(1)."
                     ::= { dot5Entry 2 }

          dot5RingStatus OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The current interface status which can
                             be used to diagnose fluctuating problems
                             that can occur on token rings, after a





                             station has successfully been added to
                             the ring.
                                Before an open is completed, this
                             object has the value for the 'no status'
                             condition.  The dot5RingState and
                             dot5RingOpenStatus objects provide for
                             debugging problems when the station
                             can not even enter the ring.
                                 The object's value is a sum of
                             values, one for each currently applicable
                             condition.  The following values are
                             defined for various conditions:

                                     0 = No Problems detected
                                    32 = Ring Recovery
                                    64 = Single Station
                                   256 = Remove Received
                                   512 = reserved
                                  1024 = Auto-Removal Error
                                  2048 = Lobe Wire Fault
                                  4096 = Transmit Beacon
                                  8192 = Soft Error
                                 16384 = Hard Error
                                 32768 = Signal Loss
                                131072 = no status, open not completed."
                     ::= { dot5Entry 3 }

          dot5RingState  OBJECT-TYPE
                     SYNTAX  INTEGER {
                                   opened(1),
                                   closed(2),
                                   opening(3),
                                   closing(4),
                                   openFailure(5),
                                   ringFailure(6)
                             }
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The current interface state with respect
                             to entering or leaving the ring."
                     ::= { dot5Entry 4 }

          dot5RingOpenStatus  OBJECT-TYPE
                     SYNTAX  INTEGER {
                                   noOpen(1),     -- no open attempted
                                   badParam(2),
                                   lobeFailed(3),





                                   signalLoss(4),
                                   insertionTimeout(5),
                                   ringFailed(6),
                                   beaconing(7),
                                   duplicateMAC(8),
                                   requestFailed(9),
                                   removeReceived(10),
                                   open(11)      -- last open successful
                             }
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This object indicates the success, or the
                             reason for failure, of the station's most
                             recent attempt to enter the ring."
                     ::= { dot5Entry 5 }

          dot5RingSpeed  OBJECT-TYPE
                     SYNTAX  INTEGER {
                                   unknown(1),
                                   oneMegabit(2),
                                   fourMegabit(3),
                                   sixteenMegabit(4)
                             }
                     ACCESS  read-write
                     STATUS  mandatory
                     DESCRIPTION
                             "The ring's bandwidth."
                     ::= { dot5Entry 6 }

          dot5UpStream  OBJECT-TYPE
                     SYNTAX  MacAddress
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The MAC-address of the up stream neighbor
                              station in the ring."
                     ::= { dot5Entry 7 }

          dot5ActMonParticipate OBJECT-TYPE
                     SYNTAX  INTEGER {
                                   true(1),
                                   false(2)
                             }
                     ACCESS  read-write
                     STATUS  mandatory
                     DESCRIPTION
                             "If this object has a value of true(1) then





                             this interface will participate in the
                             active monitor selection process.  If the
                             value is false(2) then it will not.
                             Setting this object might not have an
                             effect until the next time the interface
                             is opened."
                     ::= { dot5Entry 8 }

          dot5Functional OBJECT-TYPE
                     SYNTAX  MacAddress
                     ACCESS  read-write
                     STATUS  mandatory
                     DESCRIPTION
                             "The bit mask of all Token Ring functional
                             addresses for which this interface will
                             accept frames."
                     ::= { dot5Entry 9 }



          --   The Statistics Table

          -- This table contains statistics and error counter which are
          -- specific to 802.5 interfaces.  It is mandatory that systems
          -- having 802.5 interfaces implement this table.

          dot5StatsTable  OBJECT-TYPE
                     SYNTAX  SEQUENCE OF Dot5StatsEntry
                     ACCESS  not-accessible
                     STATUS  mandatory
                     DESCRIPTION
                             "A table containing Token Ring statistics,
                             one entry per 802.5 interface.
                                 All the statistics are defined using
                             the syntax Counter as 32-bit wrap around
                             counters.  Thus, if an interface's
                             hardware maintains these statistics in
                             16-bit counters, then the agent must read
                             the hardware's counters frequently enough
                             to prevent loss of significance, in order
                             to maintain 32-bit counters in software."
                     ::= { dot5 2 }

          dot5StatsEntry  OBJECT-TYPE
                     SYNTAX  Dot5StatsEntry
                     ACCESS  not-accessible
                     STATUS  mandatory
                     DESCRIPTION





                             "An entry contains the 802.5 statistics
                              for a particular interface."
                     INDEX   { dot5StatsIfIndex }
                     ::= { dot5StatsTable 1 }

          Dot5StatsEntry
              ::= SEQUENCE {
                      dot5StatsIfIndex
                          INTEGER,
                      dot5StatsLineErrors
                          Counter,
                      dot5StatsBurstErrors
                          Counter,
                      dot5StatsACErrors
                          Counter,
                      dot5StatsAbortTransErrors
                          Counter,
                      dot5StatsInternalErrors
                          Counter,
                      dot5StatsLostFrameErrors
                          Counter,
                      dot5StatsReceiveCongestions
                          Counter,
                      dot5StatsFrameCopiedErrors
                          Counter,
                      dot5StatsTokenErrors
                          Counter,
                      dot5StatsSoftErrors
                          Counter,
                      dot5StatsHardErrors
                          Counter,
                      dot5StatsSignalLoss
                          Counter,
                      dot5StatsTransmitBeacons
                          Counter,
                      dot5StatsRecoverys
                          Counter,
                      dot5StatsLobeWires
                          Counter,
                      dot5StatsRemoves
                          Counter,
                      dot5StatsSingles
                          Counter,
                      dot5StatsFreqErrors
                          Counter
                  }







          dot5StatsIfIndex  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The value of this object identifies the
                             802.5 interface for which this entry
                             contains management information.  The
                             value of this object for a particular
                             interface has the same value as the
                             ifIndex object, defined in [4,6], for
                             the same interface."
                     ::= { dot5StatsEntry 1 }

          dot5StatsLineErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a frame
                             or token is copied or repeated by a
                             station, the E bit is zero in the frame
                             or token and one of the following
                             conditions exists: 1) there is a
                             non-data bit (J or K bit) between the SD
                             and the ED of the frame or token, or
                             2) there is an FCS error in the frame."
                     ::= { dot5StatsEntry 2 }

          dot5StatsBurstErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a station
                             detects the absence of transitions for five
                             half-bit timers (burst-five error)."
                     ::= { dot5StatsEntry 3 }

          dot5StatsACErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a station
                             receives an AMP or SMP frame in which A is
                             equal to C is equal to 0, and then receives
                             another SMP frame with A is equal to C is





                             equal to 0 without first receiving an AMP
                             frame. It denotes a station that cannot set
                             the AC bits properly."
                     ::= { dot5StatsEntry 4 }

          dot5StatsAbortTransErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a station
                             transmits an abort delimiter while
                             transmitting."
                     ::= { dot5StatsEntry 5 }

          dot5StatsInternalErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a station
                             recognizes an internal error."
                     ::= { dot5StatsEntry 6 }

          dot5StatsLostFrameErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a station
                             is transmitting and its TRR timer expires.
                             This condition denotes a condition where a
                             transmitting station in strip mode does not
                             receive the trailer of the frame before the
                             TRR timer goes off."
                     ::= { dot5StatsEntry 7 }

          dot5StatsReceiveCongestions OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a station
                             recognizes a frame addressed to its
                             specific address, but has no available
                             buffer space indicating that the station
                             is congested."
                     ::= { dot5StatsEntry 8 }





          dot5StatsFrameCopiedErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a station
                             recognizes a frame addressed to its
                             specific address and detects that the FS
                             field A bits are set to 1 indicating a
                             possible line hit or duplicate address."
                     ::= { dot5StatsEntry 9 }

          dot5StatsTokenErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "This counter is incremented when a station
                             acting as the active monitor recognizes an
                             error condition that needs a token
                             transmitted."
                     ::= { dot5StatsEntry 10 }

          dot5StatsSoftErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The number of Soft Errors the interface
                             has detected. It directly corresponds to
                             the number of Report Error MAC frames
                             that this interface has transmitted.
                             Soft Errors are those which are
                             recoverable by the MAC layer protocols."
                     ::= { dot5StatsEntry 11 }

          dot5StatsHardErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The number of times this interface has
                             detected an immediately recoverable
                             fatal error.  It denotes the number of
                             times this interface is either
                             transmitting or receiving beacon MAC
                             frames."
                     ::= { dot5StatsEntry 12 }





          dot5StatsSignalLoss OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The number of times this interface has
                             detected the loss of signal condition from
                             the ring."
                     ::= { dot5StatsEntry 13 }

          dot5StatsTransmitBeacons OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The number of times this interface has
                             transmitted a beacon frame."
                     ::= { dot5StatsEntry 14 }

          dot5StatsRecoverys OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The number of Claim Token MAC frames
                             received or transmitted after the interface
                             has received a Ring Purge MAC frame.  This
                             counter signifies the number of times the
                             ring has been purged and is being recovered
                             back into a normal operating state."
                     ::= { dot5StatsEntry 15 }

          dot5StatsLobeWires OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The number of times the interface has
                             detected an open or short circuit in the
                             lobe data path.  The adapter will be closed
                             and dot5RingState will signify this
                             condition."
                     ::= { dot5StatsEntry 16 }

          dot5StatsRemoves OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory





                     DESCRIPTION
                             "The number of times the interface has
                             received a Remove Ring Station MAC frame
                             request.  When this frame is received
                             the interface will enter the close state
                             and dot5RingState will signify this
                             condition."
                     ::= { dot5StatsEntry 17 }

          dot5StatsSingles OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The number of times the interface has
                             sensed that it is the only station on the
                             ring.  This will happen if the interface
                             is the first one up on a ring, or if
                             there is a hardware problem."
                     ::= { dot5StatsEntry 18 }

          dot5StatsFreqErrors OBJECT-TYPE
                     SYNTAX  Counter
                     ACCESS  read-only
                     STATUS  optional
                     DESCRIPTION
                             "The number of times the interface has
                             detected that the frequency of the
                             incoming signal differs from the expected
                             frequency by more than that specified by
                             the IEEE 802.5 standard, see chapter 7
                             in [10]."
                     ::= { dot5StatsEntry 19 }


          -- The Timer Table

          -- This group contains the values of the timers defined in
          -- [10] for 802.5 interfaces.  It is optional that systems
          -- having 802.5 interfaces implement this group.

          dot5TimerTable  OBJECT-TYPE
                     SYNTAX  SEQUENCE OF Dot5TimerEntry
                     ACCESS  not-accessible
                     STATUS  mandatory
                     DESCRIPTION
                             "This table contains Token Ring interface
                             timer values, one entry per 802.5





                             interface."
                     ::= { dot5 5 }

          dot5TimerEntry  OBJECT-TYPE
                     SYNTAX  Dot5TimerEntry
                     ACCESS  not-accessible
                     STATUS  mandatory
                     DESCRIPTION
                             "A list of Token Ring timer values for an
                             802.5 interface."
                     INDEX   { dot5TimerIfIndex }
                     ::= { dot5TimerTable 1 }

          Dot5TimerEntry
              ::= SEQUENCE {
                     dot5TimerIfIndex
                         INTEGER,
                     dot5TimerReturnRepeat
                         INTEGER,
                     dot5TimerHolding
                         INTEGER,
                     dot5TimerQueuePDU
                         INTEGER,
                     dot5TimerValidTransmit
                         INTEGER,
                     dot5TimerNoToken
                         INTEGER,
                     dot5TimerActiveMon
                         INTEGER,
                     dot5TimerStandbyMon
                         INTEGER,
                     dot5TimerErrorReport
                         INTEGER,
                     dot5TimerBeaconTransmit
                         INTEGER,
                     dot5TimerBeaconReceive
                         INTEGER
                 }

          dot5TimerIfIndex  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The value of this object identifies the
                              802.5 interface for which this entry
                              contains timer values.  The value of
                              this object for a particular interface





                              has the same value as the ifIndex
                              object, defined in [4,6], for the same
                              interface."
                     ::= { dot5TimerEntry 1 }

          dot5TimerReturnRepeat  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value used to ensure the
                             interface will return to Repeat State, in
                             units of 100 micro-seconds.  The value
                             should be greater than the maximum ring
                             latency.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 2 }

          dot5TimerHolding  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "Maximum period of time a station is
                             permitted to transmit frames after capturing
                             a token, in units of 100 micro-seconds.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 3 }

          dot5TimerQueuePDU  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value for enqueuing of an SMP
                             PDU after reception of an AMP or SMP
                             frame in which the A and C bits were
                             equal to 0, in units of 100
                             micro-seconds.
                                 Implementors are encouraged to provide





                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 4 }

          dot5TimerValidTransmit OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value used by the active
                             monitor to detect the absence of valid
                             transmissions, in units of 100
                             micro-seconds.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 5 }

          dot5TimerNoToken  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value used to recover from
                             various-related error situations [9].
                             If N is the maximum number of stations on
                             the ring, the value of this timer is
                             normally:
                             dot5TimerReturnRepeat + N*dot5TimerHolding.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 6 }

          dot5TimerActiveMon  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value used by the active
                             monitor to stimulate the enqueuing of an
                             AMP PDU for transmission, in units of





                             100 micro-seconds.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 7 }

          dot5TimerStandbyMon  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value used by the stand-by
                             monitors to ensure that there is an active
                             monitor on the ring and to detect a
                             continuous stream of tokens, in units of
                             100 micro-seconds.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 8 }

          dot5TimerErrorReport  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value which determines how
                             often a station shall send a Report Error
                             MAC frame to report its error counters,
                             in units of 100 micro-seconds.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 9 }

          dot5TimerBeaconTransmit  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value which determines how
                             long a station shall remain in the state





                             of transmitting Beacon frames before
                             entering the Bypass state, in units of
                             100 micro-seconds.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 10 }

          dot5TimerBeaconReceive  OBJECT-TYPE
                     SYNTAX  INTEGER
                     ACCESS  read-only
                     STATUS  mandatory
                     DESCRIPTION
                             "The time-out value which determines how
                             long a station shall receive Beacon
                             frames from its downstream neighbor
                             before entering the Bypass state, in
                             units of 100 micro-seconds.
                                 Implementors are encouraged to provide
                             read-write access to this object if that is
                             possible/useful in their system, but giving
                             due consideration to the dangers of
                             write-able timers."
                     ::= { dot5TimerEntry 11 }


          --                      802.5 Interface Tests

          dot5Tests         OBJECT IDENTIFIER ::= { dot5 3 }

          -- The extensions to the interfaces table proposed in [11]
          -- define a table object, ifExtnsTestTable, through which a
          -- network manager can instruct an agent to test an interface
          -- for various faults.  A test to be performed is identified
          -- (as the value of ifExtnsTestType) via an OBJECT IDENTIFIER.
          --
          -- The Full-Duplex Loop Back Test is a common test, defined
          -- in [11] as:
          --
          --    testFullDuplexLoopBack
          --
          -- Invoking this test on a 802.5 interface causes the
          -- interface to check the path from memory through the
          -- chip set's internal logic and back to memory, thus
          -- checking the proper functioning of the systems's
          -- interface to the chip set.





          -- The Insert Function test is defined by:

          testInsertFunc    OBJECT IDENTIFIER ::= { dot5Tests 1 }

          -- Invoking this test causes the station to test the insert
          -- ring logic of the hardware if the station's lobe media
          -- cable is connected to a wiring concentrator.  Note that
          -- this command inserts the station into the network, and
          -- thus, could cause problems if the station is connected
          -- to a operational network.

          --                 802.5 Hardware Chip Sets

          dot5ChipSets   OBJECT IDENTIFIER ::= { dot5 4 }

          -- The extensions to the interfaces table proposed in [11]
          -- define an object, ifExtnsChipSet, with the syntax of
          -- OBJECT IDENTIFIER, to identify the hardware chip set in
          -- use by an interface.  That definition specifies just
          -- one applicable object identifier:
          --
          --    unknownChipSet
          --
          -- for use as the value of ifExtnsChipSet when the specific
          -- chip set is unknown.
          --
          -- This MIB defines the following for use as values of
          -- ifExtnsChipSet:

             -- IBM 16/4 Mb/s
          chipSetIBM16       OBJECT IDENTIFIER ::= { dot5ChipSets 1 }

             -- TI 4Mb/s
          chipSetTItms380    OBJECT IDENTIFIER ::= { dot5ChipSets 2 }

             -- TI 16/4 Mb/s
          chipSetTItms380c16 OBJECT IDENTIFIER ::= { dot5ChipSets 3 }

          END


