SNMPv2-USEC-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter32, Unsigned32,
    snmpModules
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF;


usecMIB MODULE-IDENTITY
    LAST-UPDATED "9601120000Z"
    ORGANIZATION "IETF SNMPv2 Working Group"
    CONTACT-INFO
            "        Glenn W. Waters

             Postal: Bell-Northern Research, Ltd.
                     P.O. Box 3511, Station C
                     Ottawa, ON, K1Y 4H7
                     Canada

                Tel: +1 613 763 3933

             E-mail: gwaters@bnr.ca"
    DESCRIPTION
            "The MIB module for SNMPv2 entities implementing the user-
            based security model."
    ::= { snmpModules 6 }


usecMIBObjects OBJECT IDENTIFIER ::= { usecMIB 1 }


-- Textual Conventions

AgentID ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
            "An agent's administratively-unique identifier.

            The value for this object may not be all zeros or all 'ff'H.

            The initial value for this object may be configured via an
            operator console entry or via an algorithmic function.  In





            the later case, the following guidelines are recommended:

              1) The first four octets are set to the binary equivalent
                 of the agent's SNMP network management private
                 enterprise number as assigned by the Internet Assigned
                 Numbers Authority (IANA).  For example, if Acme
                 Networks has been assigned { enterprises 696 }, the
                 first four octets would be assigned '000002b8'H.

              2) The remaining eight octets are the cookie whose
                 contents are determined via one or more enterprise-
                 specific methods.  Such methods must be designed so as
                 to maximize the possibility that the value of this
                 object will be unique in the agent's administrative
                 domain.  For example, the cookie may be the IP address
                 of the agent, or the MAC address of one of the
                 interfaces, with each address suitably padded with
                 random octets.  If multiple methods are defined, then
                 it is recommended that the cookie be further divided
                 into one octet that indicates the method being used and
                 seven octets which are a function of the method."
    SYNTAX     OCTET STRING (SIZE (12))


-- the USEC Basic group
--
-- a collection of objects providing basic instrumentation of
-- the SNMPv2 entity implementing the user-based security model


usecAgent       OBJECT IDENTIFIER ::= { usecMIBObjects 1 }

agentID OBJECT-TYPE
    SYNTAX     AgentID
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The agent's administratively-unique identifier."
    ::= { usecAgent 1 }

agentBoots OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of times that the agent has re-initialized
            itself since its initial configuration."
    ::= { usecAgent 2 }





agentTime OBJECT-TYPE
    SYNTAX     Unsigned32 (0..2147483647)
    UNITS      "seconds"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of seconds since the agent last incremented the
            agentBoots object."
    ::= { usecAgent 3 }

agentSize OBJECT-TYPE
    SYNTAX     INTEGER (484..65507)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The maximum length in octets of an SNMPv2 message which
            this agent will accept using any transport mapping."
    ::= { usecAgent 4 }


-- USEC statistics
--
-- a collection of objects providing basic instrumentation of
-- the SNMPv2 entity implementing the user-based security model

usecStats      OBJECT IDENTIFIER ::= { usecMIBObjects 2 }


usecStatsUnsupportedQoS OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The total number of packets received by the SNMPv2 entity
            which were dropped because they requested a quality-of-
            service that was unknown to the agent or otherwise
            unavailable."
    ::= { usecStats 1 }

usecStatsNotInWindows OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The total number of packets received by the SNMPv2 entity
            which were dropped because they appeared outside of the
            agent's window."
    ::= { usecStats 2 }





usecStatsUnknownUserNames OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The total number of packets received by the SNMPv2 entity
            which were dropped because they referenced a user that was
            not known to the agent."
    ::= { usecStats 3 }

usecStatsWrongDigestValues OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The total number of packets received by the SNMPv2 entity
            which were dropped because they didn't contain the expected
            digest value."
    ::= { usecStats 4 }

usecStatsUnknownContexts OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The total number of packets received by the SNMPv2 entity
            which were dropped because they referenced a context that
            was not known to the agent."
    ::= { usecStats 5 }

usecStatsBadParameters OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The total number of packets received by the SNMPv2 entity
            which were dropped because the <parameters> field was
            improperly encoded or had invalid syntax."
    ::= { usecStats 6 }

usecStatsUnauthorizedOperations OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The total number of packets received by the SNMPv2 entity
            which were dropped because the PDU type referred to an
            operation that is invalid or not authorized."





    ::= { usecStats 7 }


-- conformance information

usecMIBConformance
               OBJECT IDENTIFIER ::= { usecMIB 2 }

usecMIBCompliances
               OBJECT IDENTIFIER ::= { usecMIBConformance 1 }
usecMIBGroups  OBJECT IDENTIFIER ::= { usecMIBConformance 2 }


-- compliance statements

usecMIBCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for SNMPv2 entities which
            implement the SNMPv2 USEC model."
    MODULE  -- this module
        MANDATORY-GROUPS { usecBasicGroup,
                          usecStatsGroup }
    ::= { usecMIBCompliances 1 }


-- units of conformance

usecBasicGroup OBJECT-GROUP
    OBJECTS { agentID,
              agentBoots,
              agentTime,
              agentSize }
    STATUS  current
    DESCRIPTION
            "A collection of objects providing identification, clocks,
            and capabilities of an SNMPv2 entity which implements the
            SNMPv2 USEC model."
    ::= { usecMIBGroups 1 }

usecStatsGroup OBJECT-GROUP
    OBJECTS { usecStatsUnsupportedQoS,
              usecStatsNotInWindows,
              usecStatsUnknownUserNames,
              usecStatsWrongDigestValues,
              usecStatsUnknownContexts,
              usecStatsBadParameters,
              usecStatsUnauthorizedOperations }





    STATUS  current
    DESCRIPTION
            "A collection of objects providing basic error statistics of
            an SNMPv2 entity which implements the SNMPv2 USEC model."
    ::= { usecMIBGroups 2 }

END


