PCE-PCEP-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY,
       OBJECT-TYPE,
       mib-2,
       NOTIFICATION-TYPE,
       Unsigned32,
       Counter32
              FROM SNMPv2-SMI             -- RFC 2578
       TruthValue,
       TimeStamp
              FROM SNMPv2-TC              -- RFC 2579
       MODULE-COMPLIANCE,
       OBJECT-GROUP,
       NOTIFICATION-GROUP
              FROM SNMPv2-CONF            -- RFC 2580
       InetAddressType,
       InetAddress
              FROM INET-ADDRESS-MIB;      -- RFC 4001

   pcePcepMIB MODULE-IDENTITY
       LAST-UPDATED
           "201412171200Z" -- 17 December 2014
       ORGANIZATION
           "IETF Path Computation Element (PCE) Working Group"
       CONTACT-INFO
           "Email: pce@ietf.org
            WG charter:
                     http://datatracker.ietf.org/wg/pce/charter/"

       DESCRIPTION
         "This MIB module defines a collection of objects for managing
          the Path Computation Element Communication Protocol (PCEP).

          Copyright (c) 2014 IETF Trust and the persons identified as
          authors of the code.  All rights reserved.

          Redistribution and use in source and binary forms, with or
          without modification, is permitted pursuant to, and subject
          to the license terms contained in, the Simplified BSD License
          set forth in Section 4.c of the IETF Trust's Legal Provisions
          Relating to IETF Documents
          (http://trustee.ietf.org/license-info)."





       REVISION
           "201412171200Z" -- 17 December 2014
       DESCRIPTION
           "Initial version, published as RFC 7420."
       ::= { mib-2 227 }

   pcePcepNotifications OBJECT IDENTIFIER ::= { pcePcepMIB 0 }
   pcePcepObjects       OBJECT IDENTIFIER ::= { pcePcepMIB 1 }
   pcePcepConformance   OBJECT IDENTIFIER ::= { pcePcepMIB 2 }

   --
   -- PCEP Entity Objects
   --

   pcePcepEntityTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF PcePcepEntityEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "This table contains information about local PCEP entities.
            The entries in this table are read-only."
       ::= { pcePcepObjects 1 }

   pcePcepEntityEntry OBJECT-TYPE
       SYNTAX      PcePcepEntityEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "This entry represents a local PCEP entity."
       INDEX       {  pcePcepEntityIndex  }
       ::= { pcePcepEntityTable 1 }

   PcePcepEntityEntry ::= SEQUENCE {
       pcePcepEntityIndex                Unsigned32,
       pcePcepEntityAdminStatus          INTEGER,
       pcePcepEntityOperStatus           INTEGER,
       pcePcepEntityAddrType             InetAddressType,
       pcePcepEntityAddr                 InetAddress,
       pcePcepEntityConnectTimer         Unsigned32,
       pcePcepEntityConnectMaxRetry      Unsigned32,
       pcePcepEntityInitBackoffTimer     Unsigned32,
       pcePcepEntityMaxBackoffTimer      Unsigned32,
       pcePcepEntityOpenWaitTimer        Unsigned32,
       pcePcepEntityKeepWaitTimer        Unsigned32,
       pcePcepEntityKeepAliveTimer       Unsigned32,
       pcePcepEntityDeadTimer            Unsigned32,
       pcePcepEntityAllowNegotiation     TruthValue,
       pcePcepEntityMaxKeepAliveTimer    Unsigned32,





       pcePcepEntityMaxDeadTimer         Unsigned32,
       pcePcepEntityMinKeepAliveTimer    Unsigned32,
       pcePcepEntityMinDeadTimer         Unsigned32,
       pcePcepEntitySyncTimer            Unsigned32,
       pcePcepEntityRequestTimer         Unsigned32,
       pcePcepEntityMaxSessions          Unsigned32,
       pcePcepEntityMaxUnknownReqs       Unsigned32,
       pcePcepEntityMaxUnknownMsgs       Unsigned32
   }

   pcePcepEntityIndex OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "This index is used to uniquely identify the PCEP entity."
       ::= { pcePcepEntityEntry 1 }

   pcePcepEntityAdminStatus OBJECT-TYPE
       SYNTAX      INTEGER {
                     adminStatusUp(1),
                     adminStatusDown(2)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The administrative status of this PCEP entity.

            This is the desired operational status as currently set by
            an operator or by default in the implementation.  The value
            of pcePcepEntityOperStatus represents the current status of
            an attempt to reach this desired status."
       ::= { pcePcepEntityEntry 2 }

   pcePcepEntityOperStatus OBJECT-TYPE
       SYNTAX      INTEGER {
                     operStatusUp(1),
                     operStatusDown(2),
                     operStatusGoingUp(3),
                     operStatusGoingDown(4),
                     operStatusFailed(5),
                     operStatusFailedPerm(6)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The operational status of the PCEP entity.  It takes one of
            the following values.





            - operStatusUp(1): the PCEP entity is active.
            - operStatusDown(2): the PCEP entity is inactive.
            - operStatusGoingUp(3): the PCEP entity is activating.
            - operStatusGoingDown(4): the PCEP entity is deactivating.
            - operStatusFailed(5): the PCEP entity has failed and will
              recover when possible.
            - operStatusFailedPerm(6): the PCEP entity has failed and
              will not recover without operator intervention."
       ::= { pcePcepEntityEntry 3 }

   pcePcepEntityAddrType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The type of the PCEP entity's Internet address.  This object
            specifies how the value of the pcePcepEntityAddr object
            should be interpreted.  Only values unknown(0), ipv4(1), or
            ipv6(2) are supported."
       ::= { pcePcepEntityEntry 4 }

   pcePcepEntityAddr OBJECT-TYPE
       SYNTAX      InetAddress
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The local Internet address of this PCEP entity.  The type is
            given by pcePcepEntityAddrType.

            If operating as a PCE server, the PCEP entity listens on
            this address.  If operating as a PCC, the PCEP entity binds
            outgoing TCP connections to this address.

            It is possible for the PCEP entity to operate both as a PCC
            and a PCE server, in which case it uses this address both to
            listen for incoming TCP connections and to bind outgoing
            TCP connections."
       ::= { pcePcepEntityEntry 5 }

   pcePcepEntityConnectTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (1..65535)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current









       DESCRIPTION
           "The time that the PCEP entity will wait to establish a TCP
            connection with a peer.  If a TCP connection is not
            established within this time, then PCEP aborts the session
            setup attempt."
       ::= { pcePcepEntityEntry 6 }

   pcePcepEntityConnectMaxRetry OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The maximum number of times the system tries to establish
            a TCP connection to a peer before the session with the peer
            transitions to the idle state.

            When the session transitions to the idle state:
            - pcePcepPeerSessionExists transitions to false(2).
            - the associated PcePcepSessEntry is deleted.
            - a backoff timer runs before the session is tried again."
       ::= { pcePcepEntityEntry 7 }

   pcePcepEntityInitBackoffTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (1..65535)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The initial backoff time for retrying a failed session
            setup attempt to a peer.

            The backoff time increases for each failed session setup
            attempt, until a maximum backoff time is reached.  The
            maximum backoff time is pcePcepEntityMaxBackoffTimer."
       ::= { pcePcepEntityEntry 8 }

   pcePcepEntityMaxBackoffTimer OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The maximum backoff time for retrying a failed session
            setup attempt to a peer.









            The backoff time increases for each failed session setup
            attempt, until this maximum value is reached.  Session
            setup attempts then repeats periodically without any
            further increase in backoff time."
       ::= { pcePcepEntityEntry 9 }

   pcePcepEntityOpenWaitTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (1..65535)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The time that the PCEP entity will wait to receive an Open
            message from a peer after the TCP connection has come up.
            If no Open message is received within this time, then PCEP
            terminates the TCP connection and deletes the associated
            PcePcepSessEntry."
       ::= { pcePcepEntityEntry 10 }

   pcePcepEntityKeepWaitTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (1..65535)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The time that the PCEP entity will wait to receive a
            Keepalive or PCErr message from a peer during session
            initialization after receiving an Open message.  If no
            Keepalive or PCErr message is received within this time,
            then PCEP terminates the TCP connection and deletes the
            associated PcePcepSessEntry."
       ::= { pcePcepEntityEntry 11 }

   pcePcepEntityKeepAliveTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The Keepalive transmission timer that this PCEP entity will
            propose in the initial OPEN message of each session it is
            involved in.  This is the maximum time between two
            consecutive messages sent to a peer.  Zero means that
            the PCEP entity prefers not to send Keepalives at all.

            Note that the actual Keepalive transmission intervals, in
            either direction of an active PCEP session, are determined
            by negotiation between the peers as specified by RFC





            5440, and so may differ from this configured value.  For
            the actually negotiated values (per session), see
            pcePcepSessKeepaliveTimer and
            pcePcepSessPeerKeepaliveTimer."
       ::= { pcePcepEntityEntry 12 }

   pcePcepEntityDeadTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The DeadTimer that this PCEP entity will propose in the
            initial OPEN message of each session it is involved in.
            This is the time after which a peer should declare a
            session down if it does not receive any PCEP messages.
            Zero suggests that the peer does not run a DeadTimer at
            all."
       ::= { pcePcepEntityEntry 13 }

   pcePcepEntityAllowNegotiation OBJECT-TYPE
       SYNTAX      TruthValue
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Whether the PCEP entity will permit negotiation of session
            parameters."
       ::= { pcePcepEntityEntry 14 }

   pcePcepEntityMaxKeepAliveTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "In PCEP session parameter negotiation, the maximum value
            that this PCEP entity will accept from a peer for the
            interval between Keepalive transmissions.  Zero means that
            the PCEP entity will allow no Keepalive transmission at
            all."
       ::= { pcePcepEntityEntry 15 }

   pcePcepEntityMaxDeadTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current






       DESCRIPTION
           "In PCEP session parameter negotiation, the maximum value
            that this PCEP entity will accept from a peer for the
            DeadTimer.  Zero means that the PCEP entity will allow not
            running a DeadTimer."
       ::= { pcePcepEntityEntry 16 }

   pcePcepEntityMinKeepAliveTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "In PCEP session parameter negotiation, the minimum value
            that this PCEP entity will accept for the interval between
            Keepalive transmissions.  Zero means that the PCEP entity
            insists on no Keepalive transmission at all."
       ::= { pcePcepEntityEntry 17 }

   pcePcepEntityMinDeadTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "In PCEP session parameter negotiation, the minimum value
            that this PCEP entity will accept for the DeadTimer.  Zero
            means that the PCEP entity insists on not running a
            DeadTimer."
       ::= { pcePcepEntityEntry 18 }

   pcePcepEntitySyncTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..65535)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of SyncTimer is used in the case of a synchronized
            path computation request using the SVEC object.

            Consider the case where a PCReq message is received by a PCE
            that contains the SVEC object referring to M synchronized
            path computation requests.  If after the expiration of the
            SyncTimer all the M path computation requests have not been
            received, a protocol error is triggered and the PCE MUST
            cancel the whole set of path computation requests.







            The aim of the SyncTimer is to avoid the storage of unused
            synchronized requests should one of them get lost for some
            reason (for example, a misbehaving PCC).

            A value of zero is returned if and only if the entity does
            not use the SyncTimer."
       ::= { pcePcepEntityEntry 19 }

   pcePcepEntityRequestTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (1..65535)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The maximum time that the PCEP entity will wait for a
            response to a PCReq message."
       ::= { pcePcepEntityEntry 20 }

   pcePcepEntityMaxSessions OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The maximum number of sessions involving this PCEP entity
            that can exist at any time."
       ::= { pcePcepEntityEntry 21 }

   pcePcepEntityMaxUnknownReqs OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The maximum number of unrecognized requests and replies that
            any session on this PCEP entity is willing to accept per
            minute before terminating the session.

            A PCRep message contains an unrecognized reply if it
            contains an RP object whose request ID does not correspond
            to any in-progress request sent by this PCEP entity.

            A PCReq message contains an unrecognized request if it
            contains an RP object whose request ID is zero."
       ::= { pcePcepEntityEntry 22 }

   pcePcepEntityMaxUnknownMsgs OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current





       DESCRIPTION
           "The maximum number of unknown messages that any session
            on this PCEP entity is willing to accept per minute before
            terminating the session."
       ::= { pcePcepEntityEntry 23 }

   --
   -- The PCEP Peer Table
   --

   pcePcepPeerTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF PcePcepPeerEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "This table contains information about peers known by
            the local PCEP entity.  The entries in this table are
            read-only.

            This table gives peer information that spans PCEP
            sessions.  Information about current PCEP sessions can be
            found in the pcePcepSessTable table."
       ::= { pcePcepObjects 2 }

   pcePcepPeerEntry OBJECT-TYPE
       SYNTAX      PcePcepPeerEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Information about a single peer that spans all PCEP
            sessions to that peer."
       INDEX { pcePcepEntityIndex,
               pcePcepPeerAddrType,
               pcePcepPeerAddr }
       ::= { pcePcepPeerTable 1 }

   PcePcepPeerEntry ::= SEQUENCE {
       pcePcepPeerAddrType                 InetAddressType,
       pcePcepPeerAddr                     InetAddress,
       pcePcepPeerRole                     INTEGER,
       pcePcepPeerDiscontinuityTime        TimeStamp,
       pcePcepPeerInitiateSession          TruthValue,
       pcePcepPeerSessionExists            TruthValue,
       pcePcepPeerNumSessSetupOK           Counter32,
       pcePcepPeerNumSessSetupFail         Counter32,
       pcePcepPeerSessionUpTime            TimeStamp,
       pcePcepPeerSessionFailTime          TimeStamp,
       pcePcepPeerSessionFailUpTime        TimeStamp,





       pcePcepPeerAvgRspTime               Unsigned32,
       pcePcepPeerLWMRspTime               Unsigned32,
       pcePcepPeerHWMRspTime               Unsigned32,
       pcePcepPeerNumPCReqSent             Counter32,
       pcePcepPeerNumPCReqRcvd             Counter32,
       pcePcepPeerNumPCRepSent             Counter32,
       pcePcepPeerNumPCRepRcvd             Counter32,
       pcePcepPeerNumPCErrSent             Counter32,
       pcePcepPeerNumPCErrRcvd             Counter32,
       pcePcepPeerNumPCNtfSent             Counter32,
       pcePcepPeerNumPCNtfRcvd             Counter32,
       pcePcepPeerNumKeepaliveSent         Counter32,
       pcePcepPeerNumKeepaliveRcvd         Counter32,
       pcePcepPeerNumUnknownRcvd           Counter32,
       pcePcepPeerNumCorruptRcvd           Counter32,
       pcePcepPeerNumReqSent               Counter32,
       pcePcepPeerNumSvecSent              Counter32,
       pcePcepPeerNumSvecReqSent           Counter32,
       pcePcepPeerNumReqSentPendRep        Counter32,
       pcePcepPeerNumReqSentEroRcvd        Counter32,
       pcePcepPeerNumReqSentNoPathRcvd     Counter32,
       pcePcepPeerNumReqSentCancelRcvd     Counter32,
       pcePcepPeerNumReqSentErrorRcvd      Counter32,
       pcePcepPeerNumReqSentTimeout        Counter32,
       pcePcepPeerNumReqSentCancelSent     Counter32,
       pcePcepPeerNumReqSentClosed         Counter32,
       pcePcepPeerNumReqRcvd               Counter32,
       pcePcepPeerNumSvecRcvd              Counter32,
       pcePcepPeerNumSvecReqRcvd           Counter32,
       pcePcepPeerNumReqRcvdPendRep        Counter32,
       pcePcepPeerNumReqRcvdEroSent        Counter32,
       pcePcepPeerNumReqRcvdNoPathSent     Counter32,
       pcePcepPeerNumReqRcvdCancelSent     Counter32,
       pcePcepPeerNumReqRcvdErrorSent      Counter32,
       pcePcepPeerNumReqRcvdCancelRcvd     Counter32,
       pcePcepPeerNumReqRcvdClosed         Counter32,
       pcePcepPeerNumRepRcvdUnknown        Counter32,
       pcePcepPeerNumReqRcvdUnknown        Counter32
   }

   pcePcepPeerAddrType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  not-accessible
       STATUS      current









       DESCRIPTION
           "The type of the peer's Internet address.  This object
            specifies how the value of the pcePcepPeerAddr object should
            be interpreted.  Only values unknown(0), ipv4(1), or
            ipv6(2) are supported."
       ::= { pcePcepPeerEntry 1 }

   pcePcepPeerAddr OBJECT-TYPE
       SYNTAX      InetAddress
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The Internet address of the peer.  The type is given by
            pcePcepPeerAddrType."
       ::= { pcePcepPeerEntry 2 }

   pcePcepPeerRole OBJECT-TYPE
       SYNTAX      INTEGER {
                     unknown(0),
                     pcc(1),
                     pce(2),
                     pccAndPce(3)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The role that this peer took the last time a session was
            established.  It takes one of the following values.
            - unknown(0): this peer's role is not known.
            - pcc(1): this peer is a Path Computation Client (PCC).
            - pce(2): this peer is a Path Computation Element (PCE).
            - pccAndPce(3): this peer is both a PCC and a PCE."
       ::= { pcePcepPeerEntry 3 }

   pcePcepPeerDiscontinuityTime OBJECT-TYPE
       SYNTAX      TimeStamp
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of sysUpTime at the time that the information and
            statistics in this row were last reset."
       ::= { pcePcepPeerEntry 4 }

   pcePcepPeerInitiateSession OBJECT-TYPE
       SYNTAX      TruthValue
       MAX-ACCESS  read-only
       STATUS      current






       DESCRIPTION
           "Indicates whether the local PCEP entity initiates sessions
            to this peer or waits for the peer to initiate a session."
       ::= { pcePcepPeerEntry 5 }

   pcePcepPeerSessionExists OBJECT-TYPE
       SYNTAX      TruthValue
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Indicates whether a session with this peer currently
            exists."
       ::= { pcePcepPeerEntry 6 }

   pcePcepPeerNumSessSetupOK OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCEP sessions successfully established with
            the peer, including any current session.  This counter is
            incremented each time a session with this peer is
            successfully established."
       ::= { pcePcepPeerEntry 7 }

   pcePcepPeerNumSessSetupFail OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCEP sessions with the peer that have been
            attempted but failed before being fully established.
            This counter is incremented each time a session retry to
            this peer fails."
       ::= { pcePcepPeerEntry 8 }

   pcePcepPeerSessionUpTime OBJECT-TYPE
       SYNTAX      TimeStamp
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of sysUpTime the last time a session with this
            peer was successfully established.

            If pcePcepPeerNumSessSetupOK is zero, then this object
            contains zero."
       ::= { pcePcepPeerEntry 9 }






   pcePcepPeerSessionFailTime OBJECT-TYPE
       SYNTAX      TimeStamp
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of sysUpTime the last time a session with this
            peer failed to be established.

            If pcePcepPeerNumSessSetupFail is zero, then this object
            contains zero."
       ::= { pcePcepPeerEntry 10 }

   pcePcepPeerSessionFailUpTime OBJECT-TYPE
       SYNTAX      TimeStamp
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of sysUpTime the last time a session with this
            peer failed from active.

            If pcePcepPeerNumSessSetupOK is zero, then this object
            contains zero."
       ::= { pcePcepPeerEntry 11 }

   pcePcepPeerAvgRspTime OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "milliseconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The average response time for this peer.

            If an average response time has not been calculated for this
            peer, then this object has the value zero.

            If pcePcepPeerRole is pcc, then this field is meaningless
            and is set to zero."
       ::= { pcePcepPeerEntry 12 }

   pcePcepPeerLWMRspTime OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "milliseconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The smallest (low-water mark) response time seen from this
            peer.






            If no responses have been received from this peer, then this
            object has the value zero.

            If pcePcepPeerRole is pcc, then this field is meaningless
            and is set to zero."
       ::= { pcePcepPeerEntry 13 }

   pcePcepPeerHWMRspTime OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "milliseconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The greatest (high-water mark) response time seen from this
            peer.

            If no responses have been received from this peer, then this
            object has the value zero.

            If pcePcepPeerRole is pcc, then this field is meaningless
            and is set to zero."
       ::= { pcePcepPeerEntry 14 }

   pcePcepPeerNumPCReqSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCReq messages sent to this peer."
       ::= { pcePcepPeerEntry 15 }

   pcePcepPeerNumPCReqRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCReq messages received from this peer."
       ::= { pcePcepPeerEntry 16 }

   pcePcepPeerNumPCRepSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCRep messages sent to this peer."
       ::= { pcePcepPeerEntry 17 }







   pcePcepPeerNumPCRepRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCRep messages received from this peer."
       ::= { pcePcepPeerEntry 18 }

   pcePcepPeerNumPCErrSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCErr messages sent to this peer."
       ::= { pcePcepPeerEntry 19 }

   pcePcepPeerNumPCErrRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCErr messages received from this peer."
       ::= { pcePcepPeerEntry 20 }

   pcePcepPeerNumPCNtfSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCNtf messages sent to this peer."
       ::= { pcePcepPeerEntry 21 }

   pcePcepPeerNumPCNtfRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCNtf messages received from this peer."
       ::= { pcePcepPeerEntry 22 }

   pcePcepPeerNumKeepaliveSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of Keepalive messages sent to this peer."
       ::= { pcePcepPeerEntry 23 }






   pcePcepPeerNumKeepaliveRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of Keepalive messages received from this peer."
       ::= { pcePcepPeerEntry 24 }

   pcePcepPeerNumUnknownRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of unknown messages received from this peer."
       ::= { pcePcepPeerEntry 25 }

   pcePcepPeerNumCorruptRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of corrupted PCEP messages received from this
            peer."
       ::= { pcePcepPeerEntry 26 }

   pcePcepPeerNumReqSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests sent to this peer.  A request
            corresponds 1:1 with an RP object in a PCReq message.

            This might be greater than pcePcepPeerNumPCReqSent because
            multiple requests can be batched into a single PCReq
            message."
       ::= { pcePcepPeerEntry 27 }

   pcePcepPeerNumSvecSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of SVEC objects sent to this peer in PCReq
            messages.  An SVEC object represents a set of synchronized
            requests."
       ::= { pcePcepPeerEntry 28 }






   pcePcepPeerNumSvecReqSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests sent to this peer that appeared in
            one or more SVEC objects."
       ::= { pcePcepPeerEntry 29 }

   pcePcepPeerNumReqSentPendRep OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that have been sent to this peer for
            which a response is still pending."
       ::= { pcePcepPeerEntry 30 }

   pcePcepPeerNumReqSentEroRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that have been sent to this peer for
            which a response with an ERO was
            received.  Such responses indicate that a path was
            successfully computed by the peer."
       ::= { pcePcepPeerEntry 31 }

   pcePcepPeerNumReqSentNoPathRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that have been sent to this peer for
            which a response with a NO-PATH object was received.  Such
            responses indicate that the peer could not find a path to
            satisfy the request."
       ::= { pcePcepPeerEntry 32 }

   pcePcepPeerNumReqSentCancelRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that were canceled by the peer with
            a PCNtf message.






            This might be different than pcePcepPeerNumPCNtfRcvd because
            not all PCNtf messages are used to cancel requests, and a
            single PCNtf message can cancel multiple requests."
       ::= { pcePcepPeerEntry 33 }

   pcePcepPeerNumReqSentErrorRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that were rejected by the peer with a
            PCErr message.

            This might be different than pcePcepPeerNumPCErrRcvd because
            not all PCErr messages are used to reject requests, and a
            single PCErr message can reject multiple requests."
       ::= { pcePcepPeerEntry 34 }

   pcePcepPeerNumReqSentTimeout OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that have been sent to a peer and
            have been abandoned because the peer has taken too long to
            respond to them."
       ::= { pcePcepPeerEntry 35 }

   pcePcepPeerNumReqSentCancelSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that were sent to the peer and
            explicitly canceled by the local PCEP entity sending a
            PCNtf."
       ::= { pcePcepPeerEntry 36 }

   pcePcepPeerNumReqSentClosed OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that were sent to the peer and
            implicitly canceled when the session they were sent over was
            closed."
       ::= { pcePcepPeerEntry 37 }






   pcePcepPeerNumReqRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests received from this peer.  A request
            corresponds 1:1 with an RP object in a PCReq message.

            This might be greater than pcePcepPeerNumPCReqRcvd because
            multiple requests can be batched into a single PCReq
            message."
       ::= { pcePcepPeerEntry 38 }

   pcePcepPeerNumSvecRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of SVEC objects received from this peer in PCReq
            messages.  An SVEC object represents a set of synchronized
            requests."
       ::= { pcePcepPeerEntry 39 }

   pcePcepPeerNumSvecReqRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests received from this peer that appeared
            in one or more SVEC objects."
       ::= { pcePcepPeerEntry 40 }

   pcePcepPeerNumReqRcvdPendRep OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that have been received from this
            peer for which a response is still pending."
       ::= { pcePcepPeerEntry 41 }

   pcePcepPeerNumReqRcvdEroSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current








       DESCRIPTION
           "The number of requests that have been received from this
            peer for which a response with an ERO was sent.  Such
            responses indicate that a path was successfully computed by
            the local PCEP entity."
       ::= { pcePcepPeerEntry 42 }

   pcePcepPeerNumReqRcvdNoPathSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that have been received from this
            peer for which a response with a NO-PATH object was sent.
            Such responses indicate that the local PCEP entity could
            not find a path to satisfy the request."
       ::= { pcePcepPeerEntry 43 }

   pcePcepPeerNumReqRcvdCancelSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests received from this peer that were
            canceled by the local PCEP entity sending a PCNtf message.

            This might be different than pcePcepPeerNumPCNtfSent because
            not all PCNtf messages are used to cancel requests, and a
            single PCNtf message can cancel multiple requests."
       ::= { pcePcepPeerEntry 44 }

   pcePcepPeerNumReqRcvdErrorSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests received from this peer that were
            rejected by the local PCEP entity sending a PCErr message.

            This might be different than pcePcepPeerNumPCErrSent because
            not all PCErr messages are used to reject requests, and a
            single PCErr message can reject multiple requests."
       ::= { pcePcepPeerEntry 45 }

   pcePcepPeerNumReqRcvdCancelRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current





       DESCRIPTION
           "The number of requests that were received from the peer and
            explicitly canceled by the peer sending a PCNtf."
       ::= { pcePcepPeerEntry 46 }

   pcePcepPeerNumReqRcvdClosed OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that were received from the peer and
            implicitly canceled when the session they were received over
            was closed."
       ::= { pcePcepPeerEntry 47 }

   pcePcepPeerNumRepRcvdUnknown OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of responses to unknown requests received from
            this peer.  A response to an unknown request is a response
            whose RP object does not contain the request ID of any
            request that is currently outstanding on the session."
       ::= { pcePcepPeerEntry 48 }

   pcePcepPeerNumReqRcvdUnknown OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of unknown requests that have been received from
            a peer.  An unknown request is a request whose RP object
            contains a request ID of zero."
       ::= { pcePcepPeerEntry 49 }

   --
   -- The PCEP Sessions Table
   --

   pcePcepSessTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF PcePcepSessEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table of PCEP sessions that involve the local PCEP
            entity.  Each entry in this table represents a single
            session.  The entries in this table are read-only.





            An entry appears in this table when the corresponding PCEP
            session transitions out of idle state.  If the PCEP session
            transitions back into an idle state, then the corresponding
            entry in this table is removed."
       ::= { pcePcepObjects 3 }

   pcePcepSessEntry OBJECT-TYPE
       SYNTAX      PcePcepSessEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "This entry represents a single PCEP session in which the
            local PCEP entity participates.

            This entry exists only if the corresponding PCEP session has
            been initialized by some event, such as manual user
            configuration, auto-discovery of a peer, or an incoming TCP
            connection."
       INDEX { pcePcepEntityIndex,
               pcePcepPeerAddrType,
               pcePcepPeerAddr,
               pcePcepSessInitiator }
       ::= { pcePcepSessTable 1 }

   PcePcepSessEntry ::= SEQUENCE {
       pcePcepSessInitiator                INTEGER,
       pcePcepSessStateLastChange          TimeStamp,
       pcePcepSessState                    INTEGER,
       pcePcepSessConnectRetry             Counter32,
       pcePcepSessLocalID                  Unsigned32,
       pcePcepSessRemoteID                 Unsigned32,
       pcePcepSessKeepaliveTimer           Unsigned32,
       pcePcepSessPeerKeepaliveTimer       Unsigned32,
       pcePcepSessDeadTimer                Unsigned32,
       pcePcepSessPeerDeadTimer            Unsigned32,
       pcePcepSessKAHoldTimeRem            Unsigned32,
       pcePcepSessOverloaded               TruthValue,
       pcePcepSessOverloadTime             Unsigned32,
       pcePcepSessPeerOverloaded           TruthValue,
       pcePcepSessPeerOverloadTime         Unsigned32,
       pcePcepSessDiscontinuityTime        TimeStamp,
       pcePcepSessAvgRspTime               Unsigned32,
       pcePcepSessLWMRspTime               Unsigned32,
       pcePcepSessHWMRspTime               Unsigned32,
       pcePcepSessNumPCReqSent             Counter32,
       pcePcepSessNumPCReqRcvd             Counter32,
       pcePcepSessNumPCRepSent             Counter32,
       pcePcepSessNumPCRepRcvd             Counter32,





       pcePcepSessNumPCErrSent             Counter32,
       pcePcepSessNumPCErrRcvd             Counter32,
       pcePcepSessNumPCNtfSent             Counter32,
       pcePcepSessNumPCNtfRcvd             Counter32,
       pcePcepSessNumKeepaliveSent         Counter32,
       pcePcepSessNumKeepaliveRcvd         Counter32,
       pcePcepSessNumUnknownRcvd           Counter32,
       pcePcepSessNumCorruptRcvd           Counter32,
       pcePcepSessNumReqSent               Counter32,
       pcePcepSessNumSvecSent              Counter32,
       pcePcepSessNumSvecReqSent           Counter32,
       pcePcepSessNumReqSentPendRep        Counter32,
       pcePcepSessNumReqSentEroRcvd        Counter32,
       pcePcepSessNumReqSentNoPathRcvd     Counter32,
       pcePcepSessNumReqSentCancelRcvd     Counter32,
       pcePcepSessNumReqSentErrorRcvd      Counter32,
       pcePcepSessNumReqSentTimeout        Counter32,
       pcePcepSessNumReqSentCancelSent     Counter32,
       pcePcepSessNumReqRcvd               Counter32,
       pcePcepSessNumSvecRcvd              Counter32,
       pcePcepSessNumSvecReqRcvd           Counter32,
       pcePcepSessNumReqRcvdPendRep        Counter32,
       pcePcepSessNumReqRcvdEroSent        Counter32,
       pcePcepSessNumReqRcvdNoPathSent     Counter32,
       pcePcepSessNumReqRcvdCancelSent     Counter32,
       pcePcepSessNumReqRcvdErrorSent      Counter32,
       pcePcepSessNumReqRcvdCancelRcvd     Counter32,
       pcePcepSessNumRepRcvdUnknown        Counter32,
       pcePcepSessNumReqRcvdUnknown        Counter32
   }

   pcePcepSessInitiator OBJECT-TYPE
       SYNTAX      INTEGER {
                      local(1),
                      remote(2)
                   }
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The initiator of the session; that is, whether the TCP
            connection was initiated by the local PCEP entity or the
            peer.

            There is a window during session initialization where two
            sessions can exist between a pair of PCEP speakers, each
            initiated by one of the speakers.  One of these sessions is
            always discarded before it leaves OpenWait state.  However,
            before it is discarded, two sessions to the given peer





            appear transiently in this MIB module.  The sessions are
            distinguished by who initiated them, and so this field is an
            index for pcePcepSessTable."
       ::= { pcePcepSessEntry 1 }

   pcePcepSessStateLastChange OBJECT-TYPE
       SYNTAX      TimeStamp
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of sysUpTime at the time this session entered its
            current state as denoted by the pcePcepSessState object."
       ::= { pcePcepSessEntry 2 }

   pcePcepSessState OBJECT-TYPE
       SYNTAX      INTEGER {
                      tcpPending(1),
                      openWait(2),
                      keepWait(3),
                      sessionUp(4)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The current state of the session.

            The set of possible states excludes the idle state since
            entries do not exist in this table in the idle state."
       ::= { pcePcepSessEntry 3 }

   pcePcepSessConnectRetry OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of times that the local PCEP entity has
            attempted to establish a TCP connection for this session
            without success.  The PCEP entity gives up when this
            reaches pcePcepEntityConnectMaxRetry."
       ::= { pcePcepSessEntry 4 }

   pcePcepSessLocalID OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of the PCEP session ID used by the local PCEP
            entity in the Open message for this session.





            If pcePcepSessState is tcpPending, then this is the session
            ID that will be used in the Open message.  Otherwise, this
            is the session ID that was sent in the Open message."
       ::= { pcePcepSessEntry 5 }

   pcePcepSessRemoteID OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of the PCEP session ID used by the peer in its
            Open message for this session.

            If pcePcepSessState is tcpPending or openWait, then this
            field is not used and MUST be set to zero."
       ::= { pcePcepSessEntry 6 }

   pcePcepSessKeepaliveTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The agreed maximum interval at which the local PCEP entity
            transmits PCEP messages on this PCEP session.  Zero means
            that the local PCEP entity never sends Keepalives on this
            session.

            This field is used if and only if pcePcepSessState is
            sessionUp.  Otherwise, it is not used and MUST be set to
            zero."
       ::= { pcePcepSessEntry 7 }

   pcePcepSessPeerKeepaliveTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The agreed maximum interval at which the peer transmits PCEP
            messages on this PCEP session.  Zero means that the peer
            never sends Keepalives on this session.

            This field is used if and only if pcePcepSessState is
            sessionUp.  Otherwise, it is not used and MUST be set to
            zero."
       ::= { pcePcepSessEntry 8 }






   pcePcepSessDeadTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The DeadTimer interval for this PCEP session."
       ::= { pcePcepSessEntry 9 }

   pcePcepSessPeerDeadTimer OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The peer's DeadTimer interval for this PCEP session.

            If pcePcepSessState is tcpPending or openWait, then this
            field is not used and MUST be set to zero."
       ::= { pcePcepSessEntry 10 }

   pcePcepSessKAHoldTimeRem OBJECT-TYPE
       SYNTAX      Unsigned32 (0..255)
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The Keepalive hold time remaining for this session.

            If pcePcepSessState is tcpPending or openWait, then this
            field is not used and MUST be set to zero."
       ::= { pcePcepSessEntry 11 }

   pcePcepSessOverloaded OBJECT-TYPE
       SYNTAX      TruthValue
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "If the local PCEP entity has informed the peer that it is
            currently overloaded, then this is set to true.  Otherwise,
            it is set to false."
       ::= { pcePcepSessEntry 12 }

   pcePcepSessOverloadTime OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current





       DESCRIPTION
           "The interval of time that is remaining until the local PCEP
            entity will cease to be overloaded on this session.

            This field is only used if pcePcepSessOverloaded is set to
            true.  Otherwise, it is not used and MUST be set to zero."
       ::= { pcePcepSessEntry 13 }

   pcePcepSessPeerOverloaded OBJECT-TYPE
       SYNTAX      TruthValue
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "If the peer has informed the local PCEP entity that it is
            currently overloaded, then this is set to true.  Otherwise,
            it is set to false."
       ::= { pcePcepSessEntry 14 }

   pcePcepSessPeerOverloadTime OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The interval of time that is remaining until the peer will
            cease to be overloaded.  If it is not known how long the
            peer will stay in overloaded state, this field is set to
            zero.

            This field is only used if pcePcepSessPeerOverloaded is set
            to true.  Otherwise, it is not used and MUST be set to
            zero."
       ::= { pcePcepSessEntry 15 }

   pcePcepSessDiscontinuityTime OBJECT-TYPE
       SYNTAX      TimeStamp
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of sysUpTime at the time that the statistics in
            this row were last reset."
       ::= { pcePcepSessEntry 16 }

   pcePcepSessAvgRspTime OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "milliseconds"
       MAX-ACCESS  read-only
       STATUS      current





       DESCRIPTION
           "The average response time for this peer on this session.

            If an average response time has not been calculated for this
            peer, then this object has the value zero."
       ::= { pcePcepSessEntry 17 }

   pcePcepSessLWMRspTime OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "milliseconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The smallest (low-water mark) response time seen from this
            peer on this session.

            If no responses have been received from this peer, then this
            object has the value zero."
       ::= { pcePcepSessEntry 18 }

   pcePcepSessHWMRspTime OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "milliseconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The greatest (high-water mark) response time seen from this
            peer on this session.

            If no responses have been received from this peer, then this
            object has the value zero."
       ::= { pcePcepSessEntry 19 }

   pcePcepSessNumPCReqSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCReq messages sent on this session."
       ::= { pcePcepSessEntry 20 }

   pcePcepSessNumPCReqRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCReq messages received on this session."
       ::= { pcePcepSessEntry 21 }





   pcePcepSessNumPCRepSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCRep messages sent on this session."
       ::= { pcePcepSessEntry 22 }

   pcePcepSessNumPCRepRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCRep messages received on this session."
       ::= { pcePcepSessEntry 23 }

   pcePcepSessNumPCErrSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCErr messages sent on this session."
       ::= { pcePcepSessEntry 24 }

   pcePcepSessNumPCErrRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCErr messages received on this session."
       ::= { pcePcepSessEntry 25 }

   pcePcepSessNumPCNtfSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCNtf messages sent on this session."
       ::= { pcePcepSessEntry 26 }

   pcePcepSessNumPCNtfRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of PCNtf messages received on this session."
       ::= { pcePcepSessEntry 27 }






   pcePcepSessNumKeepaliveSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of Keepalive messages sent on this session."
       ::= { pcePcepSessEntry 28 }

   pcePcepSessNumKeepaliveRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of Keepalive messages received on this session."
       ::= { pcePcepSessEntry 29 }

   pcePcepSessNumUnknownRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of unknown messages received on this session."
       ::= { pcePcepSessEntry 30 }

   pcePcepSessNumCorruptRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of corrupted PCEP messages received on this
            session."
       ::= { pcePcepSessEntry 31 }

   pcePcepSessNumReqSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests sent on this session.  A request
            corresponds 1:1 with an RP object in a PCReq message.

            This might be greater than pcePcepSessNumPCReqSent because
            multiple requests can be batched into a single PCReq
            message."
       ::= { pcePcepSessEntry 32 }








   pcePcepSessNumSvecSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of SVEC objects sent on this session in PCReq
            messages.  An SVEC object represents a set of synchronized
            requests."
       ::= { pcePcepSessEntry 33 }

   pcePcepSessNumSvecReqSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests sent on this session that appeared in
            one or more SVEC objects."
       ::= { pcePcepSessEntry 34 }

   pcePcepSessNumReqSentPendRep OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that have been sent on this session
            for which a response is still pending."
       ::= { pcePcepSessEntry 35 }

   pcePcepSessNumReqSentEroRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of successful responses received on this session.
            A response corresponds 1:1 with an RP object in a PCRep
            message.  A successful response is a response for which an
            ERO was successfully computed."
       ::= { pcePcepSessEntry 36 }

   pcePcepSessNumReqSentNoPathRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of unsuccessful responses received on this
            session.  A response corresponds 1:1 with an RP object in a
            PCRep message.  An unsuccessful response is a response with
            a NO-PATH object."





       ::= { pcePcepSessEntry 37 }

   pcePcepSessNumReqSentCancelRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests sent on this session that were
            canceled by the peer with a PCNtf message.

            This might be different than pcePcepSessNumPCNtfRcvd because
            not all PCNtf messages are used to cancel requests, and a
            single PCNtf message can cancel multiple requests."
       ::= { pcePcepSessEntry 38 }

   pcePcepSessNumReqSentErrorRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests sent on this session that were
            rejected by the peer with a PCErr message.

            This might be different than pcePcepSessNumPCErrRcvd because
            not all PCErr messages are used to reject requests, and a
            single PCErr message can reject multiple requests."
       ::= { pcePcepSessEntry 39 }

   pcePcepSessNumReqSentTimeout OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests sent on this session that have been
            sent to a peer and have been abandoned because the peer has
            taken too long to respond to them."
       ::= { pcePcepSessEntry 40 }

   pcePcepSessNumReqSentCancelSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests sent on this session that were sent
            to the peer and explicitly canceled by the local PCEP
            entity sending a PCNtf."
       ::= { pcePcepSessEntry 41 }






   pcePcepSessNumReqRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests received on this session.  A request
            corresponds 1:1 with an RP object in a PCReq message.

            This might be greater than pcePcepSessNumPCReqRcvd because
            multiple requests can be batched into a single PCReq
            message."
       ::= { pcePcepSessEntry 42 }

   pcePcepSessNumSvecRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of SVEC objects received on this session in PCReq
            messages.  An SVEC object represents a set of synchronized
            requests."
       ::= { pcePcepSessEntry 43 }

   pcePcepSessNumSvecReqRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests received on this session that
            appeared in one or more SVEC objects."
       ::= { pcePcepSessEntry 44 }

   pcePcepSessNumReqRcvdPendRep OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that have been received on this
            session for which a response is still pending."
       ::= { pcePcepSessEntry 45 }

   pcePcepSessNumReqRcvdEroSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of successful responses sent on this session.  A
            response corresponds 1:1 with an RP object in a PCRep





            message.  A successful response is a response for which an
            ERO was successfully computed."
       ::= { pcePcepSessEntry 46 }

   pcePcepSessNumReqRcvdNoPathSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of unsuccessful responses sent on this session.
            A response corresponds 1:1 with an RP object in a PCRep
            message.  An unsuccessful response is a response with a
            NO-PATH object."
       ::= { pcePcepSessEntry 47 }

   pcePcepSessNumReqRcvdCancelSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests received on this session that were
            canceled by the local PCEP entity sending a PCNtf message.

            This might be different than pcePcepSessNumPCNtfSent because
            not all PCNtf messages are used to cancel requests, and a
            single PCNtf message can cancel multiple requests."
       ::= { pcePcepSessEntry 48 }

   pcePcepSessNumReqRcvdErrorSent OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests received on this session that were
            rejected by the local PCEP entity sending a PCErr message.

            This might be different than pcePcepSessNumPCErrSent because
            not all PCErr messages are used to reject requests, and a
            single PCErr message can reject multiple requests."
       ::= { pcePcepSessEntry 49 }

   pcePcepSessNumReqRcvdCancelRcvd OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests that were received on this session
            and explicitly canceled by the peer sending a PCNtf."





       ::= { pcePcepSessEntry 50 }

   pcePcepSessNumRepRcvdUnknown OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of responses to unknown requests received on this
            session.  A response to an unknown request is a response
            whose RP object does not contain the request ID of any
            request that is currently outstanding on the session."
       ::= { pcePcepSessEntry 51 }

   pcePcepSessNumReqRcvdUnknown OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of unknown requests that have been received on
            this session.  An unknown request is a request whose RP
            object contains a request ID of zero."
       ::= { pcePcepSessEntry 52 }

   ---
   --- Notifications Configuration
   ---

   pcePcepNotificationsMaxRate OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
           "This variable indicates the maximum number of
            notifications issued per second.  If events occur
            more rapidly, the implementation may simply fail to
            emit these notifications during that period or may
            queue them until an appropriate time.  A value of zero
            means no notifications are emitted and all should be
            discarded (that is, not queued)."
       ::= { pcePcepObjects 4 }

   ---
   --- Notifications
   ---

   pcePcepSessUp NOTIFICATION-TYPE
       OBJECTS     {
                      pcePcepSessState,





                      pcePcepSessStateLastChange
                   }
       STATUS      current
       DESCRIPTION
           "This notification is sent when the value of
            pcePcepSessState enters the sessionUp state."
       ::= { pcePcepNotifications 1 }

   pcePcepSessDown NOTIFICATION-TYPE
       OBJECTS     {
                      pcePcepSessState,
                      pcePcepSessStateLastChange
                   }
       STATUS      current
       DESCRIPTION
           "This notification is sent when the value of
            pcePcepSessState leaves the sessionUp state."
       ::= { pcePcepNotifications 2 }

   pcePcepSessLocalOverload NOTIFICATION-TYPE
       OBJECTS     {
                      pcePcepSessOverloaded,
                      pcePcepSessOverloadTime
                   }
       STATUS      current
       DESCRIPTION
           "This notification is sent when the local PCEP entity enters
            overload state for a peer."
       ::= { pcePcepNotifications 3 }

   pcePcepSessLocalOverloadClear NOTIFICATION-TYPE
       OBJECTS     {
                      pcePcepSessOverloaded
                   }
       STATUS      current
       DESCRIPTION
           "This notification is sent when the local PCEP entity leaves
            overload state for a peer."
       ::= { pcePcepNotifications 4 }

   pcePcepSessPeerOverload NOTIFICATION-TYPE
       OBJECTS     {
                      pcePcepSessPeerOverloaded,
                      pcePcepSessPeerOverloadTime
                   }
       STATUS      current







       DESCRIPTION
           "This notification is sent when a peer enters overload
            state."
       ::= { pcePcepNotifications 5 }

   pcePcepSessPeerOverloadClear NOTIFICATION-TYPE
       OBJECTS     {
                      pcePcepSessPeerOverloaded
                   }
       STATUS      current
       DESCRIPTION
           "This notification is sent when a peer leaves overload
            state."
       ::= { pcePcepNotifications 6 }

   --
   -- Module Conformance Statement
   --

   pcePcepCompliances
       OBJECT IDENTIFIER ::= { pcePcepConformance 1 }

   pcePcepGroups
       OBJECT IDENTIFIER ::= { pcePcepConformance 2 }

   --
   -- Read-Only Compliance
   --

   pcePcepModuleReadOnlyCompliance MODULE-COMPLIANCE
       STATUS current
       DESCRIPTION
           "The module is implemented with support for read-only.  In
            other words, only monitoring is available by implementing
            this MODULE-COMPLIANCE."

       MODULE -- this module
           MANDATORY-GROUPS    {
                                 pcePcepGeneralGroup,
                                 pcePcepNotificationsGroup
                               }

       OBJECT       pcePcepEntityAddrType
       SYNTAX       InetAddressType { unknown(0), ipv4(1), ipv6(2) }
       DESCRIPTION  "Only unknown(0), ipv4(1), and ipv6(2) support
                     is required."







-- The following restriction is commented out because of a limitation
-- in SMIv2 which does not allow index objects to be restricted in
-- scope.  Nevertheless, this object is intended to be restricted in
-- scope, as follows.
--
--     OBJECT       pcePcepPeerAddrType
--     SYNTAX       InetAddressType { unknown(0), ipv4(1), ipv6(2) }
--     DESCRIPTION  "Only unknown(0), ipv4(1), and ipv6(2) support
--                   is required."

       ::= { pcePcepCompliances 1 }

   -- units of conformance

   pcePcepGeneralGroup OBJECT-GROUP
       OBJECTS { pcePcepEntityAdminStatus,
                 pcePcepEntityOperStatus,
                 pcePcepEntityAddrType,
                 pcePcepEntityAddr,
                 pcePcepEntityConnectTimer,
                 pcePcepEntityConnectMaxRetry,
                 pcePcepEntityInitBackoffTimer,
                 pcePcepEntityMaxBackoffTimer,
                 pcePcepEntityOpenWaitTimer,
                 pcePcepEntityKeepWaitTimer,
                 pcePcepEntityKeepAliveTimer,
                 pcePcepEntityDeadTimer,
                 pcePcepEntityAllowNegotiation,
                 pcePcepEntityMaxKeepAliveTimer,
                 pcePcepEntityMaxDeadTimer,
                 pcePcepEntityMinKeepAliveTimer,
                 pcePcepEntityMinDeadTimer,
                 pcePcepEntitySyncTimer,
                 pcePcepEntityRequestTimer,
                 pcePcepEntityMaxSessions,
                 pcePcepEntityMaxUnknownReqs,
                 pcePcepEntityMaxUnknownMsgs,
                 pcePcepPeerRole,
                 pcePcepPeerDiscontinuityTime,
                 pcePcepPeerInitiateSession,
                 pcePcepPeerSessionExists,
                 pcePcepPeerNumSessSetupOK,
                 pcePcepPeerNumSessSetupFail,
                 pcePcepPeerSessionUpTime,
                 pcePcepPeerSessionFailTime,
                 pcePcepPeerSessionFailUpTime,
                 pcePcepPeerAvgRspTime,
                 pcePcepPeerLWMRspTime,





                 pcePcepPeerHWMRspTime,
                 pcePcepPeerNumPCReqSent,
                 pcePcepPeerNumPCReqRcvd,
                 pcePcepPeerNumPCRepSent,
                 pcePcepPeerNumPCRepRcvd,
                 pcePcepPeerNumPCErrSent,
                 pcePcepPeerNumPCErrRcvd,
                 pcePcepPeerNumPCNtfSent,
                 pcePcepPeerNumPCNtfRcvd,
                 pcePcepPeerNumKeepaliveSent,
                 pcePcepPeerNumKeepaliveRcvd,
                 pcePcepPeerNumUnknownRcvd,
                 pcePcepPeerNumCorruptRcvd,
                 pcePcepPeerNumReqSent,
                 pcePcepPeerNumSvecSent,
                 pcePcepPeerNumSvecReqSent,
                 pcePcepPeerNumReqSentPendRep,
                 pcePcepPeerNumReqSentEroRcvd,
                 pcePcepPeerNumReqSentNoPathRcvd,
                 pcePcepPeerNumReqSentCancelRcvd,
                 pcePcepPeerNumReqSentErrorRcvd,
                 pcePcepPeerNumReqSentTimeout,
                 pcePcepPeerNumReqSentCancelSent,
                 pcePcepPeerNumReqSentClosed,
                 pcePcepPeerNumReqRcvd,
                 pcePcepPeerNumSvecRcvd,
                 pcePcepPeerNumSvecReqRcvd,
                 pcePcepPeerNumReqRcvdPendRep,
                 pcePcepPeerNumReqRcvdEroSent,
                 pcePcepPeerNumReqRcvdNoPathSent,
                 pcePcepPeerNumReqRcvdCancelSent,
                 pcePcepPeerNumReqRcvdErrorSent,
                 pcePcepPeerNumReqRcvdCancelRcvd,
                 pcePcepPeerNumReqRcvdClosed,
                 pcePcepPeerNumRepRcvdUnknown,
                 pcePcepPeerNumReqRcvdUnknown,
                 pcePcepSessStateLastChange,
                 pcePcepSessState,
                 pcePcepSessConnectRetry,
                 pcePcepSessLocalID,
                 pcePcepSessRemoteID,
                 pcePcepSessKeepaliveTimer,
                 pcePcepSessPeerKeepaliveTimer,
                 pcePcepSessDeadTimer,
                 pcePcepSessPeerDeadTimer,
                 pcePcepSessKAHoldTimeRem,
                 pcePcepSessOverloaded,
                 pcePcepSessOverloadTime,





                 pcePcepSessPeerOverloaded,
                 pcePcepSessPeerOverloadTime,
                 pcePcepSessDiscontinuityTime,
                 pcePcepSessAvgRspTime,
                 pcePcepSessLWMRspTime,
                 pcePcepSessHWMRspTime,
                 pcePcepSessNumPCReqSent,
                 pcePcepSessNumPCReqRcvd,
                 pcePcepSessNumPCRepSent,
                 pcePcepSessNumPCRepRcvd,
                 pcePcepSessNumPCErrSent,
                 pcePcepSessNumPCErrRcvd,
                 pcePcepSessNumPCNtfSent,
                 pcePcepSessNumPCNtfRcvd,
                 pcePcepSessNumKeepaliveSent,
                 pcePcepSessNumKeepaliveRcvd,
                 pcePcepSessNumUnknownRcvd,
                 pcePcepSessNumCorruptRcvd,
                 pcePcepSessNumReqSent,
                 pcePcepSessNumSvecSent,
                 pcePcepSessNumSvecReqSent,
                 pcePcepSessNumReqSentPendRep,
                 pcePcepSessNumReqSentEroRcvd,
                 pcePcepSessNumReqSentNoPathRcvd,
                 pcePcepSessNumReqSentCancelRcvd,
                 pcePcepSessNumReqSentErrorRcvd,
                 pcePcepSessNumReqSentTimeout,
                 pcePcepSessNumReqSentCancelSent,
                 pcePcepSessNumReqRcvd,
                 pcePcepSessNumSvecRcvd,
                 pcePcepSessNumSvecReqRcvd,
                 pcePcepSessNumReqRcvdPendRep,
                 pcePcepSessNumReqRcvdEroSent,
                 pcePcepSessNumReqRcvdNoPathSent,
                 pcePcepSessNumReqRcvdCancelSent,
                 pcePcepSessNumReqRcvdErrorSent,
                 pcePcepSessNumReqRcvdCancelRcvd,
                 pcePcepSessNumRepRcvdUnknown,
                 pcePcepSessNumReqRcvdUnknown,
                 pcePcepNotificationsMaxRate
               }
       STATUS current
       DESCRIPTION
           "Objects that apply to all PCEP MIB module implementations."
       ::= { pcePcepGroups 1 }








   pcePcepNotificationsGroup NOTIFICATION-GROUP
       NOTIFICATIONS { pcePcepSessUp,
                       pcePcepSessDown,
                       pcePcepSessLocalOverload,
                       pcePcepSessLocalOverloadClear,
                       pcePcepSessPeerOverload,
                       pcePcepSessPeerOverloadClear
                     }
       STATUS   current
       DESCRIPTION
           "The notifications for a PCEP MIB module implementation."
       ::= { pcePcepGroups 2 }

   END


