PW-ENET-STD-MIB DEFINITIONS ::= BEGIN


IMPORTS
   OBJECT-TYPE, MODULE-IDENTITY, Unsigned32, mib-2
       FROM SNMPv2-SMI                    -- [RFC2578]

   MODULE-COMPLIANCE, OBJECT-GROUP
       FROM SNMPv2-CONF                   -- [RFC2580]

   StorageType, RowStatus
       FROM SNMPv2-TC                     -- [RFC2579]

   InterfaceIndexOrZero
       FROM IF-MIB                        -- [RFC2863]

   ZeroBasedCounter32
       FROM RMON2-MIB                     -- [RFC4502]

   pwIndex
       FROM PW-STD-MIB                    -- [RFC5601]

   VlanIdOrAnyOrNone
       FROM Q-BRIDGE-MIB;                 -- [RFC4363]

pwEnetStdMIB MODULE-IDENTITY
    LAST-UPDATED "200906150000Z"  -- 15 June 2009 00:00:00 GMT

    ORGANIZATION "Pseudowire Edge-to-Edge Emulation (PWE3) Working
                 Group"





    CONTACT-INFO
         "David Zelig
          Email: davidz@oversi.com

          Thomas D. Nadeau
          Email:  tom.nadeau@bt.com
         "
    DESCRIPTION
        "This MIB module describes a model for managing Ethernet
         point-to-point pseudowire services over a Packet
         Switched Network (PSN).

         Copyright (c) 2009 IETF Trust and the persons identified
         as authors of the code.  All rights reserved.

         Redistribution and use in source and binary forms, with or
         without modification, are permitted provided that the following
         conditions are met:

         - Redistributions of source code must retain the above
           copyright notice, this list of conditions and the following
           disclaimer.

         - Redistributions in binary form must reproduce the above
           copyright notice, this list of conditions and the following
           disclaimer in the documentation and/or other materials
           provided with the distribution.

         - Neither the name of Internet Society, IETF or IETF Trust, nor
           the names of specific contributors, may be used to endorse or
           promote products derived from this software without specific
           prior written permission.

         THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
         CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED WARRANTIES,
         INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
         MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
         DISCLAIMED.  IN NO EVENT SHALL THE COPYRIGHT OWNER OR
         CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
         SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
         NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
         LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
         HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
         CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR
         OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,
         EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

         This version of this MIB module is part of RFC 5603;





         see the RFC itself for full legal notices."

   -- Revision history
   REVISION "200906150000Z"  -- 15 June 2009 00:00:00 GMT
   DESCRIPTION "Initial version published as part of RFC 5603."

      ::= { mib-2 180 }

pwEnetObjects        OBJECT IDENTIFIER ::= { pwEnetStdMIB 1 }
pwEnetConformance    OBJECT IDENTIFIER ::= { pwEnetStdMIB 2 }

--
-- Ethernet PW table
--

pwEnetTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF PwEnetEntry
    MAX-ACCESS  not-accessible
    STATUS     current
    DESCRIPTION
        "This table contains the index to the Ethernet tables
        associated with this Ethernet PW, the VLAN configuration,
        and the VLAN mode."
    ::= { pwEnetObjects 1 }

pwEnetEntry  OBJECT-TYPE
    SYNTAX     PwEnetEntry
    MAX-ACCESS  not-accessible
    STATUS     current
    DESCRIPTION
        "This table is indexed by the same index that was created
        for the associated entry in the PW generic table in the

        PW-STD-MIB module.
        The pwIndex and the pwEnetPwInstance are used as indexes
        to allow multiple VLANs to exist on the same PW.

        An entry is created in this table by the agent for every
        entry in the pwTable with a pwType of 'ethernetTagged'
        or 'ethernet'.  Additional rows may be created by the
        operator or the agent if multiple entries are required for
        the same PW.

        The value of pwEnetPwInstance can be arbitrarily selected
        to make the row unique; however, implementations that know
        the VLAN field value when the row is created MAY use the
        value of the VLAN itself for better readability and
        backward compatibility with older versions of this MIB





        module.

        This table provides Ethernet port mapping and VLAN
        configuration for each Ethernet PW.

        All read-create objects in this table MAY be changed at any
        time; however, change of some objects (for example,
        pwEnetVlanMode) during the PW forwarding state MAY cause traffic
        disruption.

        Manual entries in this table SHOULD be preserved after a
        reboot, and the agent MUST ensure the integrity of those
        entries.  If the set of entries of a specific row is found to
        be inconsistent after reboot, the PW pwOperStatus MUST be
        declared as notPresent(5).
        "

    INDEX { pwIndex, pwEnetPwInstance }
    ::= { pwEnetTable 1 }

PwEnetEntry ::= SEQUENCE {
       pwEnetPwInstance    Unsigned32,
       pwEnetPwVlan        VlanIdOrAnyOrNone,
       pwEnetVlanMode      INTEGER,
       pwEnetPortVlan      VlanIdOrAnyOrNone,

       pwEnetPortIfIndex   InterfaceIndexOrZero,
       pwEnetPwIfIndex     InterfaceIndexOrZero,

       pwEnetRowStatus     RowStatus,
       pwEnetStorageType   StorageType
   }

pwEnetPwInstance  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "If multiple rows are mapped to the same PW, this index is
         used to uniquely identify the individual row.
         If the value of the VLAN field is known at the time of
         row creation, the value of pwEnetPwVlan MAY be used
         for better readability and backward compatibility with
         older versions of this MIB module.  Otherwise, the value
         1 SHOULD be set to the first row for each pwIndex
         for better readability and in order that the management
         application will know in advance how to access the
         first row when it was created by the agent.





        "
    ::= { pwEnetEntry 1 }

pwEnetPwVlan  OBJECT-TYPE
    SYNTAX      VlanIdOrAnyOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object defines the (service-delimiting) VLAN field
        value on the PW.  The value 4095 MUST be used if the
        object is not applicable, for example, when mapping all
        packets from an Ethernet port to this PW (raw mode).
        The value 0 MUST be set to indicate untagged frames
        (from the PW point of view), i.e., when pwEnetVlanMode
        equals 'noChange' and pwEnetPortVlan equals 0."
    ::= { pwEnetEntry 2 }

pwEnetVlanMode  OBJECT-TYPE
    SYNTAX     INTEGER {
             other(0),
             portBased(1),
             noChange(2),
             changeVlan(3),
             addVlan(4),
             removeVlan(5)
    }
    MAX-ACCESS  read-create
    STATUS     current
    DESCRIPTION
        "This object indicates the mode of VLAN handling between the
         port or the virtual port associated with the PW and the
         PW encapsulation.

       - 'other' indicates an operation that is not defined by
          this MIB module.

        - 'portBased' indicates that the forwarder will forward
          packets between the port and the PW independent of their
          structure (i.e., there are no service-delimiting VLAN tags
          from the PE standpoint).

        - 'noChange' indicates that the PW contains the original
           user VLAN, as specified in pwEnetPortVlan; i.e., the
           VLAN on the PE-CE link is the service-delimiting tag
           and is kept 'as is' on the PW.

        - 'changeVlan' indicates that the VLAN field on the PW
          may be different than the VLAN field on the user's





          port.  The VLAN on the PE-CE link is the service-delimiting
          tag but has a different value on the PW.

        - 'addVlan' indicates that a VLAN field will be added
          on the PSN-bound direction (i.e., on the PW). pwEnetPwVlan
          indicates the value that will be added.

        - 'removeVlan' indicates that the encapsulation on the
          PW does not include the service-delimiting VLAN field.
          Note that PRI bits transparency is lost in this case.

        - Implementation of 'portsbased', 'removeVlan', 'addVlan'
          'other', and 'changeVlan' is OPTIONAL.
        "
    DEFVAL { noChange }
    ::= { pwEnetEntry 3 }

pwEnetPortVlan  OBJECT-TYPE
    SYNTAX     VlanIdOrAnyOrNone
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "This object defines if the mapping between the original port
        (physical port or VPLS virtual port) to the PW is VLAN based
        or not.  In case of VLAN mapping, this object indicates the
        VLAN value on the original port.

        The value of '4095' MUST be used if the whole original port
        traffic is mapped to the same PW.  Note that a pwType of
        'ethernetTagged' can still be used if service-delimiting tag
        is added on the PW (pwEnetVlanMode equals 'addVlan').

        This object MUST be equal to pwEnetPwVlan if pwEnetVlanMode
        equals 'noChange'.

        The value 0 indicates that packets without a VLAN field
        (i.e., untagged frames) on the port are associated to this
        PW.  This allows the same behavior as assigning 'Default
        VLAN' to untagged frames.
        "
    DEFVAL  { 4095 }
    ::= { pwEnetEntry 4 }

pwEnetPortIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION





        "This object is used to specify the ifIndex of the Ethernet
         port associated with this PW for point-to-point Ethernet
         service, or the ifIndex of the virtual interface of the
         VPLS instance associated with the PW if the service is
         VPLS.  Two rows in this table can point to the same ifIndex
         only if there is no overlap of VLAN values specified in
         pwEnetPortVlan that are associated with this port.

         A value of zero indicates that association to an ifIndex is
         not yet known."

    ::= { pwEnetEntry 5 }

pwEnetPwIfIndex  OBJECT-TYPE
    SYNTAX     InterfaceIndexOrZero
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "If the PW is modeled as an ifIndex in the ifTable, this
         object indicates the value of the ifIndex representing the
         Ethernet PW on the PSN side in the Etherlike-MIB.  Note that
         this value may be different from the value of pwIfIndex
         that represents the ifIndex of the PW for ifType 'pw'."
     DEFVAL { 0 }
    ::= { pwEnetEntry 6 }

pwEnetRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object enables creating, deleting, and modifying this
         row."
   ::= { pwEnetEntry 7 }

pwEnetStorageType  OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the storage type of this row."
    DEFVAL { nonVolatile }
    ::= { pwEnetEntry 8 }

--
-- Ethernet PW Statistics Table
--






pwEnetStatsTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF PwEnetStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains statistical counters specific for
         Ethernet PW."
    ::= { pwEnetObjects 2 }

pwEnetStatsEntry  OBJECT-TYPE
    SYNTAX      PwEnetStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry represents the statistics gathered for the
         PW carrying the Ethernet."
    INDEX { pwIndex }
    ::= { pwEnetStatsTable 1 }


PwEnetStatsEntry ::= SEQUENCE {
    pwEnetStatsIllegalVlan        ZeroBasedCounter32,
    pwEnetStatsIllegalLength      ZeroBasedCounter32
}

pwEnetStatsIllegalVlan  OBJECT-TYPE
    SYNTAX     ZeroBasedCounter32
    MAX-ACCESS  read-only
    STATUS     current
    DESCRIPTION
        "The number of packets received (from the PSN) on this PW
         with either an illegal VLAN field, a missing VLAN field
         when one was expected, or an excessive VLAN field when
         it was not expected.  This counter may not be applicable
         in some cases, and MUST return the value of zero in
         such a case."
    ::= { pwEnetStatsEntry 1 }

pwEnetStatsIllegalLength  OBJECT-TYPE
    SYNTAX     ZeroBasedCounter32
    MAX-ACCESS  read-only
    STATUS     current
    DESCRIPTION
        "The number of packets that were received with an illegal
         Ethernet packet length on this PW.  An illegal length is
         defined as being greater than the value in the advertised
         MTU supported, or shorter than the allowed Ethernet packet
         size."





    ::= { pwEnetStatsEntry 2 }

---
--- Conformance description
---

pwEnetGroups      OBJECT IDENTIFIER ::= { pwEnetConformance 1 }
pwEnetCompliances OBJECT IDENTIFIER ::= { pwEnetConformance 2 }

-- Compliance requirement for fully compliant implementations

pwEnetModuleFullCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for agents that provides full
             support for the PW-ENET-STD-MIB module.  Such devices
             can then be monitored and also be configured using
             this MIB module."
    MODULE  -- this module
      MANDATORY-GROUPS {
                         pwEnetGroup,
                         pwEnetStatsGroup
                        }

   OBJECT       pwEnetVlanMode
   DESCRIPTION "An implementation MUST support at least the value
                noChange(2)."

   OBJECT       pwEnetPwIfIndex
   MIN-ACCESS   read-only
   DESCRIPTION "Write access and values other than zero are
                required only for implementations that support
                modeling the Ethernet PW in the Etherlike-MIB."
   OBJECT       pwEnetRowStatus
   SYNTAX       RowStatus { active(1), notInService(2),
                            notReady(3) }
   WRITE-SYNTAX RowStatus { active(1), notInService(2),
                            createAndGo(4), destroy(6)
                          }
   MIN-ACCESS   read-only
   DESCRIPTION "Support for createAndWait is not required.  Support
                of notReady is not required for implementations that
                do not support signaling.
                Support of read-write is not required for
                implementations that do not support more than one
                VLAN mapping to the same PW."
    ::= { pwEnetCompliances 1 }






-- Compliance requirement for read-only compliant implementations

pwEnetModuleReadOnlyCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for agents that provide read-
             only support for the PW-ENET-STD-MIB module.  Such
             devices can then be monitored but cannot be configured
             using this MIB module."

    MODULE  -- this module
      MANDATORY-GROUPS { pwEnetGroup,
                         pwEnetStatsGroup
                         }

   OBJECT       pwEnetPwVlan
   MIN-ACCESS   read-only
   DESCRIPTION "Write access is not required."

   OBJECT       pwEnetVlanMode
   MIN-ACCESS   read-only
   DESCRIPTION "Write access is not required.  An implementation
                MUST support at least the value noChange(2)."

   OBJECT       pwEnetPortVlan
   MIN-ACCESS   read-only
   DESCRIPTION "Write access is not required."

   OBJECT       pwEnetPortIfIndex
   MIN-ACCESS   read-only
   DESCRIPTION "Write access is not required."

   OBJECT       pwEnetPwIfIndex
   MIN-ACCESS   read-only
   DESCRIPTION "Write access is not required.  Values other than
                zero are required only for implementations that
                support modeling the Ethernet PW in the
                Etherlike-MIB."

   OBJECT       pwEnetRowStatus
   SYNTAX       RowStatus { active(1), notInService(2),
                            notReady(3) }
   MIN-ACCESS   read-only
   DESCRIPTION "Write access is not required.  Support
                of notReady is not required for implementations that
                do not support signaling."

   OBJECT       pwEnetStorageType





   MIN-ACCESS   read-only
   DESCRIPTION "Write access is not required."

    ::= { pwEnetCompliances 2 }

-- Units of conformance

pwEnetGroup OBJECT-GROUP
   OBJECTS {
            pwEnetPwVlan,
            pwEnetVlanMode,
            pwEnetPortVlan,
            pwEnetPortIfIndex,
            pwEnetPwIfIndex,
            pwEnetRowStatus,
            pwEnetStorageType
   }
   STATUS  current
   DESCRIPTION
       "Collection of objects for basic Ethernet PW configuration."
   ::= { pwEnetGroups 1 }

pwEnetStatsGroup OBJECT-GROUP
   OBJECTS {
            pwEnetStatsIllegalVlan,
            pwEnetStatsIllegalLength
   }
   STATUS  current
   DESCRIPTION
       "Collection of objects counting various PW level errors."
   ::= { pwEnetGroups 2 }

END


