ISDN-MIB DEFINITIONS ::= BEGIN


IMPORTS
        MODULE-IDENTITY,
        NOTIFICATION-TYPE,
        OBJECT-TYPE,
        Counter32,
        Gauge32,
        Integer32
                FROM SNMPv2-SMI
        DisplayString,
        TruthValue,
        TimeStamp,
        RowStatus,
        TestAndIncr,
        TEXTUAL-CONVENTION
                 FROM SNMPv2-TC
        MODULE-COMPLIANCE,
        OBJECT-GROUP,
        NOTIFICATION-GROUP
                FROM SNMPv2-CONF
        ifIndex,
        InterfaceIndex
                FROM IF-MIB
        IANAifType
                FROM IANAifType-MIB
        transmission
                FROM RFC1213-MIB;

isdnMib MODULE-IDENTITY
        LAST-UPDATED    "9609231642Z" -- Sep 23, 1996
        ORGANIZATION    "IETF ISDN MIB Working Group"
        CONTACT-INFO
            "        Guenter Roeck
             Postal: cisco Systems
                     170 West Tasman Drive
                     San Jose, CA 95134
                     U.S.A.
             Phone:  +1 408 527 3143
             E-mail: groeck@cisco.com"
        DESCRIPTION
            "The MIB module to describe the
             management of ISDN interfaces."
        ::= { transmission 20 }

-- The ISDN hardware interface (BRI or PRI) is represented





-- by a media specific ifEntry.
--
-- For basic rate lines, the media specifics for the physical interface
-- is defined in the physical interface group of the ISDN MIB.
-- The ifType for physical basic rate interfaces is isdns(75)
-- or isdnu(76), whichever is appropriate.
--
-- For primary rate, the media specifics are defined in the Trunk
-- MIB and the ifType has a value of ds1(18).

-- Each signaling channel is represented by an entry
-- in the isdnSignalingTable.
-- The signaling channel has an ifType value of isdn(63).
-- Each B channel is also represented as an entry
-- in the ifTable. The B channels have an ifType value
-- of ds0(81).
-- This model is used while defining objects and tables
-- for management.
-- The ISDN MIB allows sub-layers. For example, the data transfer
-- over a B channel may take place with PPP encapsulation. While the
-- ISDN MIB describes the D and B channels, a media specific MIB
-- for PPP can be used on a layered basis. This is as per
-- the interfaces MIB.

-- Textual conventions

IsdnSignalingProtocol ::= TEXTUAL-CONVENTION
        STATUS      current
        DESCRIPTION
            "This data type is used as the syntax of the
             isdnSignalingProtocol object in the
             definition of ISDN-MIB's isdnSignalingTable.

             The definition of this textual convention with the
             addition of newly assigned values is published
             periodically by the IANA, in either the Assigned
             Numbers RFC, or some derivative of it specific to
             Internet Network Management number assignments.  (The
             latest arrangements can be obtained by contacting the
             IANA.)

             Requests for new values should be made to IANA via
             email (iana@iana.org)."
        SYNTAX      INTEGER {
             other(1),          -- none of the following
             dss1(2),           -- ITU DSS1 (formerly CCITT) Q.931
             etsi(3),           -- Europe / ETSI ETS300-102
                                -- plus supplementary services





                                -- (ETSI 300-xxx)
                                -- note that NET3, NET5 define
                                -- test procedures for ETS300-102
                                -- and have been replaced by
                                -- I-CTR 3 and I-CTR 4.
             dass2(4),          -- U.K.   / DASS2 (PRI)
             ess4(5),           -- U.S.A. / AT&T 4ESS
             ess5(6),           -- U.S.A. / AT&T 5ESS
             dms100(7),         -- U.S.A. / Northern Telecom DMS100
             dms250(8),         -- U.S.A. / Northern Telecom DMS250
             ni1(9),            -- U.S.A. / National ISDN 1 (BRI)
             ni2(10),           -- U.S.A. / National ISDN 2 (BRI, PRI)
             ni3(11),           -- U.S.A. / next one
             vn2(12),           -- France / VN2
             vn3(13),           -- France / VN3
             vn4(14),           -- France / VN4 (ETSI with changes)
             vn6(15),           -- France / VN6 (ETSI with changes)
                                -- delta document CSE P 10-21 A
                                -- test document  CSE P 10-20 A
             kdd(16),           -- Japan  / KDD
             ins64(17),         -- Japan  / NTT INS64
             ins1500(18),       -- Japan  / NTT INS1500
             itr6(19),          -- Germany/ 1TR6 (BRI, PRI)
             cornet(20),        -- Germany/ Siemens HiCom CORNET
             ts013(21),         -- Australia / TS013
                                -- (formerly TPH 1962, BRI)
             ts014(22),         -- Australia / TS014
                                -- (formerly TPH 1856, PRI)
             qsig(23),          -- Q.SIG
             swissnet2(24),     -- SwissNet-2
             swissnet3(25)      -- SwissNet-3
        }

-- Isdn Mib objects definitions

isdnMibObjects OBJECT IDENTIFIER ::= { isdnMib 1 }

-- ISDN physical interface group

-- This group describes physical basic rate interfaces.

isdnBasicRateGroup      OBJECT IDENTIFIER ::= { isdnMibObjects 1 }

isdnBasicRateTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IsdnBasicRateEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION





            "Table containing configuration and operational
             parameters for all physical Basic Rate
             interfaces on this managed device."
        ::= { isdnBasicRateGroup 1 }

isdnBasicRateEntry OBJECT-TYPE
        SYNTAX      IsdnBasicRateEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the ISDN Basic Rate Table."
        INDEX { ifIndex }
        ::= { isdnBasicRateTable 1 }

IsdnBasicRateEntry ::= SEQUENCE {
            isdnBasicRateIfType         INTEGER,
            isdnBasicRateLineTopology   INTEGER,
            isdnBasicRateIfMode         INTEGER,
            isdnBasicRateSignalMode     INTEGER
        }

isdnBasicRateIfType OBJECT-TYPE
        SYNTAX      INTEGER {
            isdns(75),
            isdnu(76)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The physical interface type. For 'S/T' interfaces,
             also called 'Four-wire Basic Access Interface',
             the value of this object is isdns(75).
             For 'U' interfaces, also called 'Two-wire Basic
             Access Interface', the value of this object is
             isdnu(76)."
        ::= { isdnBasicRateEntry 1 }

isdnBasicRateLineTopology OBJECT-TYPE
        SYNTAX      INTEGER {
            pointToPoint(1),
            pointToMultipoint(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The line topology to be used for this interface.
             Note that setting isdnBasicRateIfType to isdns(75)
             does not necessarily mean a line topology of





             point-to-multipoint."
        ::= { isdnBasicRateEntry 2 }

isdnBasicRateIfMode OBJECT-TYPE
        SYNTAX      INTEGER {
            te(1),
            nt(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The physical interface mode. For TE mode, the value
             of this object is te(1). For NT mode, the value
             of this object is nt(2)."
        ::= { isdnBasicRateEntry 3 }

isdnBasicRateSignalMode OBJECT-TYPE
        SYNTAX      INTEGER {
            active(1),
            inactive(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The signaling channel operational mode for this interface.
             If active(1) there is a signaling channel on this
             interface. If inactive(2) a signaling channel is
             not available."
        ::= { isdnBasicRateEntry 4 }

-- The B channel (bearer channel) group

-- Note that disconnects can explicitely be handled using the
-- ifStack table. If a connection is to be disconnected,
-- the according ifStack entry has to be removed.
-- More specifically, the ifStackTable entry which binds the high-layer
-- ifTable entry (and related dialCtlNbrCfgTable entry) to the
-- B channel ifTable entry (and related isdnBearerTable entry)
-- during an active call has to be removed.

isdnBearerGroup OBJECT IDENTIFIER ::= { isdnMibObjects 2 }

isdnBearerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IsdnBearerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This table defines port specific operational, statistics





             and active call data for ISDN B channels. Each entry
             in this table describes one B (bearer) channel."
        ::= { isdnBearerGroup 1 }

isdnBearerEntry OBJECT-TYPE
        SYNTAX      IsdnBearerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "Operational and statistics information relating to
             one port. A port is a single B channel."
        INDEX { ifIndex }
        ::= { isdnBearerTable 1 }

IsdnBearerEntry ::=
        SEQUENCE {
            isdnBearerChannelType           INTEGER,
            isdnBearerOperStatus            INTEGER,
            isdnBearerChannelNumber         INTEGER,
            isdnBearerPeerAddress           DisplayString,
            isdnBearerPeerSubAddress        DisplayString,
            isdnBearerCallOrigin            INTEGER,
            isdnBearerInfoType              INTEGER,
            isdnBearerMultirate             TruthValue,
            isdnBearerCallSetupTime         TimeStamp,
            isdnBearerCallConnectTime       TimeStamp,
            isdnBearerChargedUnits          Gauge32
        }

isdnBearerChannelType           OBJECT-TYPE
        SYNTAX INTEGER {
            dialup(1),
            leased(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The B channel type. If the B channel is connected
             to a dialup line, this object has a value of
             dialup(1). In this case, it is controlled by
             an associated signaling channel. If the B channel
             is connected to a leased line, this object has
             a value of leased(2). For leased line B channels, there
             is no signaling channel control available."
        ::= { isdnBearerEntry 1 }

isdnBearerOperStatus            OBJECT-TYPE
        SYNTAX INTEGER {





            idle(1),
            connecting(2),
            connected(3),
            active(4)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current call control state for this port.
             idle(1):       The B channel is idle.
                            No call or call attempt is going on.
             connecting(2): A connection attempt (outgoing call)
                            is being made on this interface.
             connected(3):  An incoming call is in the process
                            of validation.
             active(4):     A call is active on this interface."
        ::= { isdnBearerEntry 2 }

isdnBearerChannelNumber         OBJECT-TYPE
        SYNTAX INTEGER (1..30)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The identifier being used by a signaling protocol
             to identify this B channel, also referred to as
             B channel number. If the Agent also supports the DS0 MIB,
             the values of isdnBearerChannelNumber and dsx0Ds0Number
             must be identical for a given B channel."
        ::= { isdnBearerEntry 3 }

isdnBearerPeerAddress           OBJECT-TYPE
        SYNTAX   DisplayString
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
            "The ISDN address the current or last call is or was
             connected to.

             In some cases, the format of this information can not
             be predicted, since it largely depends on the type
             of switch or PBX the device is connected to. Therefore,
             the detailed format of this information is not
             specified and is implementation dependent.

             If possible, the agent should supply this information
             using the E.164 format. In this case, the number must
             start with '+'. Otherwise, IA5 number digits must be used.






             If the peer ISDN address is not available,
             this object has a length of zero."
        REFERENCE
            "ITU-T E.164, Q.931 chapter 4.5.10"
        ::= { isdnBearerEntry 4 }

isdnBearerPeerSubAddress        OBJECT-TYPE
        SYNTAX   DisplayString
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
            "The ISDN subaddress the current or last call is or was
             connected to.

             The subaddress is an user supplied string of up to 20
             IA5 characters and is transmitted transparently through
             the network.

             If the peer subaddress is not available, this object
             has a length of zero."
        REFERENCE
             "ITU-T I.330, Q.931 chapter 4.5.11"
        ::= { isdnBearerEntry 5 }

isdnBearerCallOrigin            OBJECT-TYPE
          SYNTAX   INTEGER {
            unknown(1),
            originate(2),
            answer(3),
            callback(4)
        }
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
            "The call origin for the current or last call. If since
             system startup there was no call on this interface,
             this object has a value of unknown(1)."
        ::= { isdnBearerEntry 6 }

isdnBearerInfoType              OBJECT-TYPE
        SYNTAX      INTEGER {
            unknown(1),
            speech(2),
            unrestrictedDigital(3),       -- as defined in Q.931
            unrestrictedDigital56(4),     -- with 56k rate adaption
            restrictedDigital(5),
            audio31(6),                   -- 3.1 kHz audio
            audio7(7),                    -- 7 kHz audio





            video(8),
            packetSwitched(9)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The Information Transfer Capability for the current
             or last call.

             speech(2) refers to a non-data connection, whereas
             audio31(6) and audio7(7) refer to data mode connections.

             Note that Q.931, chapter 4.5.5, originally defined
             audio7(7) as '7 kHz audio' and now defines it as
             'Unrestricted digital information with tones/
             announcements'.

             If since system startup there has been no call on this
             interface, this object has a value of unknown(1)."
        REFERENCE
            "Q.931 [8], chapter 4.5.5, octet 3 of bearer capability
             information element, combined with the User Rate
             (as defined in octets 5 and 5a to 5d), if rate adaption
             is being used."
        ::= { isdnBearerEntry 7 }

isdnBearerMultirate             OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This flag indicates if the current or last call used
             multirate. The actual information transfer rate,
             in detail specified in octet 4.1 (rate multiplier),
             is the sum of all B channel ifSpeed values for
             the hyperchannel.

             If since system startup there was no call on this
             interface, this object has a value of false(2)."
        REFERENCE
            "Q.931 [8], chapter 4.5.5."
        ::= { isdnBearerEntry 8 }

isdnBearerCallSetupTime         OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION





            "The value of sysUpTime when the ISDN setup message for
             the current or last call was sent or received. If since
             system startup there has been no call on this interface,
             this object has a value of zero."
        ::= { isdnBearerEntry 9 }

isdnBearerCallConnectTime       OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The value of sysUpTime when the ISDN connect message for
             the current or last call was sent or received. If since
             system startup there has been no call on this interface,
             this object has a value of zero."
        ::= { isdnBearerEntry 10 }

isdnBearerChargedUnits          OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of charged units for the current or last
             connection. For incoming calls or if charging information
             is not supplied by the switch, the value of this object
             is zero."
        ::= { isdnBearerEntry 11 }

-- ISDN signaling group

isdnSignalingGroup OBJECT IDENTIFIER ::= { isdnMibObjects 3 }

-- signaling channel configuration table
-- There is one entry in this table for each Terminal Endpoint
-- (link layer connection to the switch).
-- Usually, there is one endpoint per D channel. In some
-- cases, however, there can be multiple endpoints.
-- Thus, entries in this table can be created and deleted.
-- This also means the creation of an associated ifEntry.
--
-- D channel backup and NFAS trunks are handled using the
-- ifStack table.
-- In case of D channel backup, there are multiple
-- Data Link Layer (LAPD) interfaces. Only one interface is
-- active; all others are dormant(5).
-- In case of NFAS trunks, one lower interface is the
-- LAPD interface, while the other lower interfaces are physical
-- interfaces.





-- If directory number and calling address differ from each other
-- or multiple directory numbers are being used,
-- the isdnDirectoryTable has to be used to enter such
-- directory numbers.

isdnSignalingGetIndex OBJECT-TYPE
        SYNTAX      TestAndIncr
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The recommended procedure for selecting a new index for
             isdnSignalingTable row creation is to GET the value of
             this object, and then to SET the object with the same
             value. If the SET operation succeeds, the manager can use
             this value as an index to create a new row in this table."
        REFERENCE
            "RFC1903, TestAndIncr textual convention."
        ::= { isdnSignalingGroup 1 }

isdnSignalingTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IsdnSignalingEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "ISDN signaling table containing configuration and
             operational parameters for all ISDN signaling
             channels on this managed device."
        ::= { isdnSignalingGroup 2 }

isdnSignalingEntry OBJECT-TYPE
        SYNTAX      IsdnSignalingEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the ISDN Signaling Table. To create a new
             entry, only isdnSignalingProtocol needs to be specified
             before isdnSignalingStatus can become active(1)."
        INDEX { isdnSignalingIndex }
        ::= { isdnSignalingTable 1 }

IsdnSignalingEntry ::= SEQUENCE {
            isdnSignalingIndex          INTEGER,
            isdnSignalingIfIndex        InterfaceIndex,
            isdnSignalingProtocol       IsdnSignalingProtocol,
            isdnSignalingCallingAddress DisplayString,
            isdnSignalingSubAddress     DisplayString,
            isdnSignalingBchannelCount  Integer32,
            isdnSignalingInfoTrapEnable INTEGER,





            isdnSignalingStatus         RowStatus
        }

isdnSignalingIndex OBJECT-TYPE
        SYNTAX      INTEGER (1..2147483647)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The index value which uniquely identifies an entry
             in the isdnSignalingTable."
        ::= { isdnSignalingEntry 1 }

isdnSignalingIfIndex OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The ifIndex value of the interface associated with this
             signaling channel."
        ::= { isdnSignalingEntry 2 }

isdnSignalingProtocol OBJECT-TYPE
        SYNTAX      IsdnSignalingProtocol
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The particular protocol type supported by the
             switch providing access to the ISDN network
             to which this signaling channel is connected."
        ::= { isdnSignalingEntry 3 }

isdnSignalingCallingAddress OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The ISDN Address to be assigned to this signaling
             channel. More specifically, this is the 'Calling Address
             information element' as being passed to the switch
             in outgoing call setup messages.

             It can be an EAZ (1TR6), a calling number (DSS1, ETSI)
             or any other number necessary to identify a signaling
             interface. If there is no such number defined or required,
             this is a zero length string. It is represented in
             DisplayString form.

             Incoming calls can also be identified by this number.





             If the Directory Number, i.e. the Called Number in
             incoming calls, is different to this number, the
             isdnDirectoryTable has to be used to specify all
             possible Directory Numbers.

             The format of this information largely depends on the type
             of switch or PBX the device is connected to. Therefore,
             the detailed format of this information is not
             specified and is implementation dependent.

             If possible, the agent should implement this information
             using the E.164 number format. In this case, the number
             must start with '+'. Otherwise, IA5 number digits must
             be used."
        REFERENCE
            "ITU-T E.164, Q.931 chapter 4.5.10"
        DEFVAL { "" }
        ::= { isdnSignalingEntry 4 }

isdnSignalingSubAddress OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "Supplementary information to the ISDN address assigned
             to this signaling channel. Usually, this is the
             subaddress as defined in Q.931.
             If there is no such number defined or required, this is
             a zero length string.
             The subaddress is used for incoming calls as well as
             for outgoing calls.
             The subaddress is an user supplied string of up to 20
             IA5 characters and is transmitted transparently through
             the network."
        REFERENCE
            "ITU-T I.330, Q.931 chapter 4.5.11"
        DEFVAL { "" }
        ::= { isdnSignalingEntry 5 }

isdnSignalingBchannelCount OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The total number of B channels (bearer channels)
             managed by this signaling channel. The default value
             of this object depends on the physical interface type
             and is either 2 for Basic Rate interfaces or





             24 (30) for Primary Rate interfaces."
        ::= { isdnSignalingEntry 6 }

isdnSignalingInfoTrapEnable    OBJECT-TYPE
        SYNTAX      INTEGER {
            enabled(1),
            disabled(2)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "Indicates whether isdnMibCallInformation traps
             should be generated for calls on this signaling
             channel."
        DEFVAL      { disabled }
        ::= { isdnSignalingEntry 7 }

isdnSignalingStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "This object is used to create and delete rows in the
             isdnSignalingTable."
        ::= { isdnSignalingEntry 8 }

-- Signaling channel statistics table
-- There is one entry for each signaling connection
-- in this table.
-- Note that the ifEntry also has some statistics information.

isdnSignalingStatsTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IsdnSignalingStatsEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "ISDN signaling table containing statistics
             information for all ISDN signaling channels
             on this managed device.
             Only statistical information which is not already being
             counted in the ifTable is being defined in this table."
        ::= { isdnSignalingGroup 3 }

isdnSignalingStatsEntry OBJECT-TYPE
        SYNTAX      IsdnSignalingStatsEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION





            "An entry in the ISDN Signaling statistics Table."
        AUGMENTS { isdnSignalingEntry }
        ::= { isdnSignalingStatsTable 1 }

IsdnSignalingStatsEntry ::= SEQUENCE {
            isdnSigStatsInCalls         Counter32,
            isdnSigStatsInConnected     Counter32,
            isdnSigStatsOutCalls        Counter32,
            isdnSigStatsOutConnected    Counter32,
            isdnSigStatsChargedUnits    Counter32
        }

isdnSigStatsInCalls OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of incoming calls on this interface."
        ::= { isdnSignalingStatsEntry 1 }

isdnSigStatsInConnected OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of incoming calls on this interface
             which were actually connected."
        ::= { isdnSignalingStatsEntry 2 }

isdnSigStatsOutCalls OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of outgoing calls on this interface."
        ::= { isdnSignalingStatsEntry 3 }

isdnSigStatsOutConnected OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of outgoing calls on this interface
             which were actually connected."
        ::= { isdnSignalingStatsEntry 4 }

isdnSigStatsChargedUnits OBJECT-TYPE
        SYNTAX      Counter32





        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of charging units on this interface since
             system startup.
             Only the charging units applying to the local interface,
             i.e. for originated calls or for calls with 'Reverse
             charging' being active, are counted here."
        ::= { isdnSignalingStatsEntry 5 }

--
-- The LAPD table

isdnLapdTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IsdnLapdEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "Table containing configuration and statistics
             information for all LAPD (D channel Data Link)
             interfaces on this managed device.
             Only statistical information which is not already being
             counted in the ifTable is being defined in this table."
        ::= { isdnSignalingGroup 4 }

isdnLapdEntry OBJECT-TYPE
        SYNTAX      IsdnLapdEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the LAPD Table."
        INDEX { ifIndex }
        ::= { isdnLapdTable 1 }

IsdnLapdEntry ::= SEQUENCE {
            isdnLapdPrimaryChannel  TruthValue,
            isdnLapdOperStatus      INTEGER,
            isdnLapdPeerSabme       Counter32,
            isdnLapdRecvdFrmr       Counter32
        }

isdnLapdPrimaryChannel OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "If set to true(1), this D channel is the designated
             primary D channel if D channel backup is active.





             There must be exactly one primary D channel
             configured. If D channel backup is not used, this
             object has a value of true(1)."
        REFERENCE
            "Q.931 [8], Annex F, D channel backup procedures."
        ::= { isdnLapdEntry 1 }

isdnLapdOperStatus OBJECT-TYPE
        SYNTAX      INTEGER {
            inactive(1),
            l1Active(2),
            l2Active(3)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The operational status of this interface:

             inactive  all layers are inactive
             l1Active  layer 1 is activated,
                       layer 2 datalink not established
             l2Active  layer 1 is activated,
                       layer 2 datalink established."
        ::= { isdnLapdEntry 2 }

isdnLapdPeerSabme OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of peer SABME frames received on this
             interface. This is the number of peer-initiated
             new connections on this interface."
        ::= { isdnLapdEntry 3 }

isdnLapdRecvdFrmr OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of LAPD FRMR response frames received.
             This is the number of framing errors on this
             interface."
        ::= { isdnLapdEntry 4 }

--
-- Optional groups follow here.






-- The Terminal Endpoint group and table

-- This table is required only if TEI values or SPID numbers
-- have to be entered.
-- The ifIndex values for this table are identical to those of
-- the isdnSignalingChannel table.

isdnEndpointGroup OBJECT IDENTIFIER ::= { isdnMibObjects 4 }

isdnEndpointGetIndex OBJECT-TYPE
        SYNTAX      TestAndIncr
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The recommended procedure for selecting a new index for
             isdnEndpointTable row creation is to GET the value of
             this object, and then to SET the object with the same
             value. If the SET operation succeeds, the manager can use
             this value as an index to create a new row in this table."
        REFERENCE
            "RFC1903, TestAndIncr textual convention."
        ::= { isdnEndpointGroup 1 }

isdnEndpointTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IsdnEndpointEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "Table containing configuration for Terminal
             Endpoints."
        ::= { isdnEndpointGroup 2 }

isdnEndpointEntry OBJECT-TYPE
        SYNTAX      IsdnEndpointEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the Terminal Endpoint Table. The value
             of isdnEndpointIfType must be supplied for a row
             in this table to become active."
        INDEX { isdnEndpointIndex }
        ::= { isdnEndpointTable 1 }

IsdnEndpointEntry ::= SEQUENCE {
            isdnEndpointIndex       INTEGER,
            isdnEndpointIfIndex     InterfaceIndex,
            isdnEndpointIfType      IANAifType,
            isdnEndpointTeiType     INTEGER,





            isdnEndpointTeiValue    INTEGER,
            isdnEndpointSpid        DisplayString,
            isdnEndpointStatus      RowStatus
        }

isdnEndpointIndex OBJECT-TYPE
        SYNTAX      INTEGER (1..2147483647)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The index value which uniquely identifies an entry
             in the isdnEndpointTable."
        ::= { isdnEndpointEntry 1 }

isdnEndpointIfIndex OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The ifIndex value of the interface associated with this
             Terminal Endpoint."
        ::= { isdnEndpointEntry 2 }

isdnEndpointIfType OBJECT-TYPE
        SYNTAX      IANAifType
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The interface type for this Terminal Endpoint.
             Interface types of x25ple(40) and isdn(63) are allowed.
             The interface type is identical to the value of
             ifType in the associated ifEntry."
        ::= { isdnEndpointEntry 3 }

isdnEndpointTeiType OBJECT-TYPE
        SYNTAX      INTEGER {
            dynamic(1),
            static(2)
        }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The type of TEI (Terminal Endpoint Identifier)
             used for this Terminal Endpoint. In case of dynamic(1),
             the TEI value is selected by the switch. In
             case of static(2), a valid TEI value has to be
             entered in the isdnEndpointTeiValue object.
             The default value for this object depends on the





             interface type as well as the Terminal Endpoint type.
             On Primary Rate interfaces the default value is
             static(2). On Basic Rate interfaces the default value
             is dynamic(1) for isdn(63) Terminal Endpoints and
             static(2) for x25ple(40) Terminal Endpoints."
        ::= { isdnEndpointEntry 4 }

isdnEndpointTeiValue OBJECT-TYPE
        SYNTAX      INTEGER ( 0..255 )
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The TEI (Terminal Endpoint Identifier) value
             for this Terminal Endpoint. If isdnEndpointTeiType
             is set to static(2), valid numbers are 0..63,
             while otherwise the value is set internally.
             The default value of this object is 0 for static
             TEI assignment.
             The default value for dynamic TEI assignment is also
             0 as long as no TEI has been assigned. After TEI
             assignment, the assigned TEI value is returned."
        ::= { isdnEndpointEntry 5 }

isdnEndpointSpid OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The Service profile IDentifier (SPID) information
             for this Terminal Endpoint.

             The SPID is composed of 9-20 numeric characters.

             This information has to be defined in addition to
             the local number for some switch protocol types,
             e.g. Bellcore NI-1 and NI-2.

             If this object is not required, it is a
             zero length string."
        REFERENCE
            "Bellcore SR-NWT-001953, Generic Guidelines for ISDN
             Terminal Equipment on Basic Access Interfaces,
             Chapter 8.5.1."
        DEFVAL { "" }
        ::= { isdnEndpointEntry 6 }

isdnEndpointStatus OBJECT-TYPE
        SYNTAX      RowStatus





        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "This object is used to create and delete rows in the
             isdnEndpointTable."
        ::= { isdnEndpointEntry 7 }

--
-- The Directory Number group
--

isdnDirectoryGroup OBJECT IDENTIFIER ::= { isdnMibObjects 5 }

isdnDirectoryTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IsdnDirectoryEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "Table containing Directory Numbers."
        ::= { isdnDirectoryGroup 1 }

isdnDirectoryEntry OBJECT-TYPE
        SYNTAX      IsdnDirectoryEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the Directory Number Table. All objects
             in an entry must be set for a new row to become active."
        INDEX { isdnDirectoryIndex }
        ::= { isdnDirectoryTable 1 }

IsdnDirectoryEntry ::= SEQUENCE {
            isdnDirectoryIndex      INTEGER,
            isdnDirectoryNumber     DisplayString,
            isdnDirectorySigIndex   INTEGER,
            isdnDirectoryStatus     RowStatus
        }

isdnDirectoryIndex OBJECT-TYPE
        SYNTAX      INTEGER ( 1..'7fffffff'h )
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The index value which uniquely identifies an entry
             in the isdnDirectoryTable."
        ::= { isdnDirectoryEntry 1 }

isdnDirectoryNumber OBJECT-TYPE





        SYNTAX      DisplayString
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "A Directory Number. Directory Numbers are used
             to identify incoming calls on the signaling
             channel given in isdnDirectorySigIndex.

             The format of this information largely depends on the type
             of switch or PBX the device is connected to. Therefore,
             the detailed format of this information is not
             specified and is implementation dependent.

             If possible, the agent should implement this information
             using the E.164 number format. In this case, the number
             must start with '+'. Otherwise, IA5 number digits must
             be used."
        REFERENCE
            "ITU-T E.164, Q.931 chapter 4.5.10"
        ::= { isdnDirectoryEntry 2 }

isdnDirectorySigIndex OBJECT-TYPE
        SYNTAX      INTEGER (1..2147483647)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "An index pointing to an ISDN signaling channel.
             Incoming calls are accepted on this
             signaling channel if the isdnDirectoryNumber is
             presented as Called Number in the SETUP message."
        ::= { isdnDirectoryEntry 3 }

isdnDirectoryStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "This object is used to create and delete rows in the
             isdnDirectoryTable."
        ::= { isdnDirectoryEntry 4 }

-- Traps

isdnMibTrapPrefix OBJECT IDENTIFIER ::= { isdnMib 2 }
isdnMibTraps OBJECT IDENTIFIER ::= { isdnMibTrapPrefix 0 }

isdnMibCallInformation NOTIFICATION-TYPE
        OBJECTS {





            ifIndex,                    -- isdnBearerTable ifIndex
            isdnBearerOperStatus,
            isdnBearerPeerAddress,
            isdnBearerPeerSubAddress,
            isdnBearerCallSetupTime,
            isdnBearerInfoType,
            isdnBearerCallOrigin
        }
        STATUS      current
        DESCRIPTION
            "This trap/inform is sent to the manager under the
             following condidions:
             - on incoming calls for each call which is rejected for
               policy reasons (e.g. unknown neighbor or access
               violation)
             - on outgoing calls whenever a call attempt is determined
               to have ultimately failed. In the event that call retry
               is active, then this will be after all retry attempts
               have failed.
             - whenever a call connects. In this case, the object
               isdnBearerCallConnectTime should be included in the
               trap.

             Only one such trap is sent in between successful or
             unsuccessful call attempts from or to a single neighbor;
             subsequent call attempts result in no trap.

             If the Dial Control MIB objects dialCtlNbrCfgId and
             dialCtlNbrCfgIndex are known by the entity generating
             this trap, both objects should be included in the trap
             as well. The receipt of this trap with no dial neighbor
             information indicates that the manager must poll the
             callHistoryTable of the Dial Control MIB to see what
             changed."
        ::= { isdnMibTraps 1 }

--
-- conformance information
--

isdnMibConformance OBJECT IDENTIFIER ::= { isdnMib 2 }
isdnMibCompliances OBJECT IDENTIFIER ::= { isdnMibConformance 1 }
isdnMibGroups      OBJECT IDENTIFIER ::= { isdnMibConformance 2 }

-- compliance statements

isdnMibCompliance MODULE-COMPLIANCE
        STATUS      current





        DESCRIPTION
            "The compliance statement for entities which implement
             the ISDN MIB."
        MODULE       -- this module

-- unconditionally mandatory groups
        MANDATORY-GROUPS {
            isdnMibSignalingGroup,
            isdnMibBearerGroup,
            isdnMibNotificationsGroup
        }

-- conditionally mandatory group
        GROUP       isdnMibBasicRateGroup
        DESCRIPTION
            "The isdnMibBasicRateGroup is mandatory for entities
             supporting ISDN Basic Rate interfaces."

-- optional groups
        GROUP       isdnMibEndpointGroup
        DESCRIPTION
            "Implementation of this group is optional for all systems
             that attach to ISDN interfaces."

        GROUP       isdnMibDirectoryGroup
        DESCRIPTION
            "Implementation of this group is optional for all systems
             that attach to ISDN interfaces."

        OBJECT      isdnBasicRateIfType
        MIN-ACCESS  read-only
        DESCRIPTION
            "It is conformant to implement this object as read-only."

        OBJECT      isdnBasicRateLineTopology
        MIN-ACCESS  read-only
        DESCRIPTION
            "It is conformant to implement this object as read-only."

        OBJECT      isdnBasicRateIfMode
        MIN-ACCESS  read-only
        DESCRIPTION
            "It is conformant to implement this object as read-only."

        OBJECT      isdnBasicRateSignalMode
        MIN-ACCESS  read-only
        DESCRIPTION
            "It is conformant to implement this object as read-only."





        ::= { isdnMibCompliances 1 }

-- units of conformance

isdnMibBasicRateGroup OBJECT-GROUP
        OBJECTS {
            isdnBasicRateIfType,
            isdnBasicRateLineTopology,
            isdnBasicRateIfMode,
            isdnBasicRateSignalMode
        }
        STATUS      current
        DESCRIPTION
            "A collection of objects required for ISDN Basic Rate
             physical interface configuration and statistics."
        ::= { isdnMibGroups 1 }

isdnMibBearerGroup OBJECT-GROUP
        OBJECTS {
            isdnBearerChannelType,
            isdnBearerOperStatus,
            isdnBearerChannelNumber,
            isdnBearerPeerAddress,
            isdnBearerPeerSubAddress,
            isdnBearerCallOrigin,
            isdnBearerInfoType,
            isdnBearerMultirate,
            isdnBearerCallSetupTime,
            isdnBearerCallConnectTime,
            isdnBearerChargedUnits
        }
        STATUS      current
        DESCRIPTION
            "A collection of objects required for ISDN Bearer channel
             control and statistics."
        ::= { isdnMibGroups 2 }

isdnMibSignalingGroup OBJECT-GROUP
        OBJECTS {
            isdnSignalingGetIndex,
            isdnSignalingIfIndex,
            isdnSignalingProtocol,
            isdnSignalingCallingAddress,
            isdnSignalingSubAddress,
            isdnSignalingBchannelCount,
            isdnSignalingInfoTrapEnable,
            isdnSignalingStatus,
            isdnSigStatsInCalls,





            isdnSigStatsInConnected,
            isdnSigStatsOutCalls,
            isdnSigStatsOutConnected,
            isdnSigStatsChargedUnits,
            isdnLapdPrimaryChannel,
            isdnLapdOperStatus,
            isdnLapdPeerSabme,
            isdnLapdRecvdFrmr
        }
        STATUS      current
        DESCRIPTION
            "A collection of objects required for ISDN D channel
             configuration and statistics."
        ::= { isdnMibGroups 3 }

isdnMibEndpointGroup OBJECT-GROUP
        OBJECTS {
            isdnEndpointGetIndex,
            isdnEndpointIfIndex,
            isdnEndpointIfType,
            isdnEndpointTeiType,
            isdnEndpointTeiValue,
            isdnEndpointSpid,
            isdnEndpointStatus
        }
        STATUS      current
        DESCRIPTION
            "A collection of objects describing Terminal Endpoints."
        ::= { isdnMibGroups 4 }

isdnMibDirectoryGroup OBJECT-GROUP
        OBJECTS {
            isdnDirectoryNumber,
            isdnDirectorySigIndex,
            isdnDirectoryStatus
        }
        STATUS      current
        DESCRIPTION
            "A collection of objects describing directory numbers."
        ::= { isdnMibGroups 5 }

isdnMibNotificationsGroup NOTIFICATION-GROUP
    NOTIFICATIONS { isdnMibCallInformation }
    STATUS        current
    DESCRIPTION
            "The notifications which a ISDN MIB entity is
             required to implement."
    ::= { isdnMibGroups 6 }





END



