VM-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, TimeTicks,
       Counter64, Integer32, mib-2
           FROM SNMPv2-SMI
       OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP
           FROM SNMPv2-CONF
       TEXTUAL-CONVENTION, PhysAddress, TruthValue
           FROM SNMPv2-TC
       SnmpAdminString
           FROM SNMP-FRAMEWORK-MIB
       UUIDorZero
           FROM UUID-TC-MIB
       InterfaceIndexOrZero
           FROM IF-MIB





       IANAStorageMediaType
           FROM IANA-STORAGE-MEDIA-TYPE-MIB;

   vmMIB MODULE-IDENTITY
       LAST-UPDATED "201510120000Z"        -- 12 October 2015
       ORGANIZATION "IETF Operations and Management Area Working Group"
       CONTACT-INFO
               "WG Email: opsawg@ietf.org
               Mailing list subscription info:
               https://www.ietf.org/mailman/listinfo/opsawg

               Hirochika Asai
               The University of Tokyo
               7-3-1 Hongo
               Bunkyo-ku, Tokyo  113-8656
               Japan
               Phone: +81 3 5841 6748
               Email: panda@hongo.wide.ad.jp

               Michael MacFaden
               VMware Inc.
               Email: mrm@vmware.com

               Juergen Schoenwaelder
               Jacobs University
               Campus Ring 1
               Bremen 28759
               Germany
               Email: j.schoenwaelder@jacobs-university.de

               Keiichi Shima
               IIJ Innovation Institute Inc.
               3-13 Kanda-Nishikicho
               Chiyoda-ku, Tokyo  101-0054
               Japan
               Email: keiichi@iijlab.net

               Tina Tsou
               Huawei Technologies (USA)
               2330 Central Expressway
               Santa Clara, CA 95050
               United States
               Email: tina.tsou.zouting@huawei.com"

       DESCRIPTION
               "This MIB module is for use in managing a hypervisor and
               virtual machines controlled by the hypervisor.






               Copyright (c) 2015 IETF Trust and the persons identified
               as authors of the code.  All rights reserved.

               Redistribution and use in source and binary forms, with
               or without modification, is permitted pursuant to, and
               subject to the license terms contained in, the
               Simplified BSD License set forth in Section 4.c of the
               IETF Trust's Legal Provisions Relating to IETF Documents
               (http://trustee.ietf.org/license-info)."

       REVISION "201510120000Z"        -- 12 October 2015
       DESCRIPTION
               "The initial version of this MIB, published as
               RFC 7666."
       ::= { mib-2 236 }

   vmNotifications OBJECT IDENTIFIER ::= { vmMIB 0 }
   vmObjects       OBJECT IDENTIFIER ::= { vmMIB 1 }
   vmConformance   OBJECT IDENTIFIER ::= { vmMIB 2 }


   -- Textual conversion definitions
   --
   VirtualMachineIndex ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d"
       STATUS       current
       DESCRIPTION
               "A unique value, greater than zero, identifying a
               virtual machine.  The value for each virtual machine
               MUST remain constant at least from one re-initialization
               of the hypervisor to the next re-initialization."
       SYNTAX       Integer32 (1..2147483647)

   VirtualMachineIndexOrZero ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d"
       STATUS       current
       DESCRIPTION
               "This textual convention is an extension of the
               VirtualMachineIndex convention.  This extension permits
               the additional value of zero.  The meaning of the value
               zero is object-specific and MUST therefore be defined as
               part of the description of any object that uses this
               syntax.  Examples of the usage of zero might include
               situations where a virtual machine is unknown, or when
               none or all virtual machines need to be referenced."
       SYNTAX       Integer32 (0..2147483647)

   VirtualMachineAdminState ::= TEXTUAL-CONVENTION





       STATUS      current
       DESCRIPTION
               "The administrative state of a virtual machine:

               running(1)    The administrative state of the virtual
                             machine indicating the virtual machine
                             is currently online or should be brought
                             online.

               suspended(2)  The administrative state of the virtual
                             machine where its memory and CPU execution
                             state has been saved to persistent store
                             and will be restored at next running(1).

               paused(3)     The administrative state indicating the
                             virtual machine is resident in memory but
                             is no longer scheduled to execute by the
                             hypervisor.

               shutdown(4)   The administrative state of the virtual
                             machine indicating the virtual machine
                             is currently offline or should be
                             shutting down."
       SYNTAX       INTEGER {
                       running(1),
                       suspended(2),
                       paused(3),
                       shutdown(4)
                    }

   VirtualMachineOperState ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
               "The operational state of a virtual machine:

               unknown(1)     The operational state of the virtual
                              machine is unknown, e.g., because the
                              implementation failed to obtain the state
                              from the hypervisor.

               other(2)       The operational state of the virtual
                              machine indicating that an operational
                              state is obtained from the hypervisor, but
                              it is not a state defined in this MIB
                              module.

               preparing(3)   The operational state of the virtual
                              machine indicating the virtual machine is





                              currently in the process of preparation,
                              e.g., allocating and initializing virtual
                              storage after creating (defining) the
                              virtual machine.

               running(4)     The operational state of the virtual
                              machine indicating the virtual machine is
                              currently executed, but it is not in the
                              process of preparing(3), suspending(5),
                              resuming(7), migrating(9), and
                              shuttingdown(10).

               suspending(5)  The operational state of the virtual
                              machine indicating the virtual machine is
                              currently in the process of suspending
                              to save its memory and CPU execution
                              state to persistent store.  This is a
                              transient state from running(4) to
                              suspended(6).

               suspended(6)   The operational state of the virtual
                              machine indicating the virtual machine is
                              currently suspended, which means the
                              memory and CPU execution state of the
                              virtual machine are saved to persistent
                              store.  During this state, the virtual
                              machine is not scheduled to execute by
                              the hypervisor.

               resuming(7)    The operational state of the virtual
                              machine indicating the virtual machine is
                              currently in the process of resuming
                              to restore its memory and CPU execution
                              state from persistent store.  This is a
                              transient state from suspended(6) to
                              running(4).

               paused(8)      The operational state of the virtual
                              machine indicating the virtual machine is
                              resident in memory but no longer
                              scheduled to execute by the hypervisor.

               migrating(9)   The operational state of the virtual
                              machine indicating the virtual machine is
                              currently in the process of migration
                              from/to another hypervisor.

               shuttingdown(10)





                              The operational state of the virtual
                              machine indicating the virtual machine is
                              currently in the process of shutting
                              down.  This is a transient state from
                              running(4) to shutdown(11).

               shutdown(11)   The operational state of the virtual
                              machine indicating the virtual machine is
                              down, and CPU execution is no longer
                              scheduled by the hypervisor and its
                              memory is not resident in the hypervisor.

               crashed(12)    The operational state of the virtual
                              machine indicating the virtual machine
                              has crashed."
       SYNTAX       INTEGER {
                       unknown(1),
                       other(2),
                       preparing(3),
                       running(4),
                       suspending(5),
                       suspended(6),
                       resuming(7),
                       paused(8),
                       migrating(9),
                       shuttingdown(10),
                       shutdown(11),
                       crashed(12)
                    }

   VirtualMachineAutoStart ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
               "The autostart configuration of a virtual machine:

               unknown(1)     The autostart configuration is unknown,
                              e.g., because the implementation failed
                              to obtain the autostart configuration
                              from the hypervisor.

               enabled(2)     The autostart configuration of the
                              virtual machine is enabled.  The virtual
                              machine should be automatically brought
                              online at the next re-initialization of
                              the hypervisor.

               disabled(3)    The autostart configuration of the
                              virtual machine is disabled.  The virtual





                              machine should not be automatically
                              brought online at the next
                              re-initialization of the hypervisor."
       SYNTAX      INTEGER {
                       unknown(1),
                       enabled(2),
                       disabled(3)
                   }

   VirtualMachinePersistent ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
               "This value indicates whether a virtual machine has a
               persistent configuration, which means the virtual machine
               will still exist after shutting down:

               unknown(1)     The persistent configuration is unknown,
                              e.g., because the implementation failed
                              to obtain the persistent configuration
                              from the hypervisor. (read-only)

               persistent(2)  The virtual machine is persistent, i.e.,
                              the virtual machine will exist after it
                              shuts down.

               transient(3)   The virtual machine is transient, i.e.,
                              the virtual machine will not exist after
                              it shuts down."
       SYNTAX       INTEGER {
                       unknown(1),
                       persistent(2),
                       transient(3)
                    }

   VirtualMachineCpuIndex ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d"
       STATUS       current
       DESCRIPTION
               "A unique value for each virtual machine, greater than
               zero, identifying a virtual CPU assigned to a virtual
               machine.  The value for each virtual CPU MUST remain
               constant at least from one re-initialization of the
               hypervisor to the next re-initialization."
        SYNTAX      Integer32 (1..2147483647)

   VirtualMachineStorageIndex ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d"
       STATUS       current





       DESCRIPTION
               "A unique value for each virtual machine, greater than
               zero, identifying a virtual storage device allocated to
               a virtual machine.  The value for each virtual storage
               device MUST remain constant at least from one
               re-initialization of the hypervisor to the next
               re-initialization."
        SYNTAX      Integer32 (1..2147483647)

   VirtualMachineStorageSourceType ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
               "The source type of a virtual storage device:

               unknown(1)     The source type is unknown, e.g., because
                              the implementation failed to obtain the
                              media type from the hypervisor.

               other(2)       The source type is other than those
                              defined in this conversion.

               block(3)       The source type is a block device.

               raw(4)         The source type is a raw-formatted file.

               sparse(5)      The source type is a sparse file.

               network(6)     The source type is a network device."
       SYNTAX       INTEGER {
                       unknown(1),
                       other(2),
                       block(3),
                       raw(4),
                       sparse(5),
                       network(6)
                    }

   VirtualMachineStorageAccess ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
               "The access permission of a virtual storage:

               unknown(1)     The access permission of the virtual
                              storage is unknown.

               readwrite(2)   The virtual storage is a read-write
                              device.






               readonly(3)    The virtual storage is a read-only
                              device."
       SYNTAX       INTEGER {
                       unknown(1),
                       readwrite(2),
                       readonly(3)
                    }

   VirtualMachineNetworkIndex ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d"
       STATUS       current
       DESCRIPTION
               "A unique value for each virtual machine, greater than
               zero, identifying a virtual network interface allocated
               to the virtual machine.  The value for each virtual
               network interface MUST remain constant at least from one
               re-initialization of the hypervisor to the next
               re-initialization."
        SYNTAX      Integer32 (1..2147483647)

   VirtualMachineList ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "1x"
       STATUS       current
       DESCRIPTION
               "Each octet within this value specifies a set of eight
               virtual machine vmIndex values, with the first octet
               specifying virtual machine 1 through 8, the second octet
               specifying virtual machine 9 through 16, etc.  Within
               each octet, the most significant bit represents the
               lowest-numbered vmIndex, and the least significant bit
               represents the highest-numbered vmIndex.  Thus, each
               virtual machine of the host is represented by a single
               bit within the value of this object.  If that bit has
               a value of '1', then that virtual machine is included
               in the set of virtual machines; the virtual machine is
               not included if its bit has a value of '0'."
       SYNTAX      OCTET STRING

   -- The hypervisor group
   --
   -- A collection of objects common to all hypervisors.
   --
   vmHypervisor    OBJECT IDENTIFIER ::= { vmObjects 1 }

   vmHvSoftware OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (0..255))
       MAX-ACCESS   read-only
       STATUS       current





       DESCRIPTION
               "A textual description of the hypervisor software.  This
               value SHOULD NOT include its version as it SHOULD be
               included in 'vmHvVersion'."
       ::= { vmHypervisor 1 }

   vmHvVersion OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (0..255))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "A textual description of the version of the hypervisor
               software."
       ::= { vmHypervisor 2 }

   vmHvObjectID OBJECT-TYPE
       SYNTAX       OBJECT IDENTIFIER
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The vendor's authoritative identification of the
               hypervisor software contained in the entity.  This value
               is allocated within the SMI enterprises
               subtree (1.3.6.1.4.1).  Note that this is different from
               sysObjectID in the SNMPv2-MIB (RFC 3418) because
               sysObjectID is not the identification of the hypervisor
               software but the device, firmware, or management
               operating system."
       ::= { vmHypervisor 3 }

   vmHvUpTime OBJECT-TYPE
       SYNTAX       TimeTicks
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The time (in centiseconds) since the hypervisor was
               last re-initialized.  Note that this is different from
               sysUpTime in the SNMPv2-MIB (RFC 3418) and hrSystemUptime
               in the HOST-RESOURCES-MIB (RFC 2790) because sysUpTime is
               the uptime of the network management portion of the
               system, and hrSystemUptime is the uptime of the
               management operating system but not the hypervisor
               software."
       ::= { vmHypervisor 4 }


   -- The virtual machine information
   --





   -- A collection of objects common to all virtual machines.
   --
   vmNumber  OBJECT-TYPE
       SYNTAX       Integer32 (0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The number of virtual machines (regardless of their
               current state) present on this hypervisor."
       ::= { vmObjects 2 }

   vmTableLastChange  OBJECT-TYPE
       SYNTAX       TimeTicks
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The value of vmHvUpTime at the time of the last creation
               or deletion of an entry in the vmTable."
       ::= { vmObjects 3 }

   vmTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VmEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "A list of virtual machine entries.  The number of
               entries is given by the value of vmNumber."
       ::= { vmObjects 4 }

   vmEntry OBJECT-TYPE
       SYNTAX       VmEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "An entry containing management information applicable
               to a particular virtual machine."
       INDEX   { vmIndex }
       ::= { vmTable 1 }

   VmEntry ::=
       SEQUENCE {
           vmIndex                 VirtualMachineIndex,
           vmName                  SnmpAdminString,
           vmUUID                  UUIDorZero,
           vmOSType                SnmpAdminString,
           vmAdminState            VirtualMachineAdminState,
           vmOperState             VirtualMachineOperState,
           vmAutoStart             VirtualMachineAutoStart,





           vmPersistent            VirtualMachinePersistent,
           vmCurCpuNumber          Integer32,
           vmMinCpuNumber          Integer32,
           vmMaxCpuNumber          Integer32,
           vmMemUnit               Integer32,
           vmCurMem                Integer32,
           vmMinMem                Integer32,
           vmMaxMem                Integer32,
           vmUpTime                TimeTicks,
           vmCpuTime               Counter64
       }

   vmIndex OBJECT-TYPE
       SYNTAX       VirtualMachineIndex
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "A unique value, greater than zero, identifying the
               virtual machine.  The value assigned to a given virtual
               machine may not persist across re-initialization of the
               hypervisor.  A command generator MUST use the vmUUID to
               identify a given virtual machine of interest."
       ::= { vmEntry 1 }

   vmName OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (0..255))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "A textual name of the virtual machine."
       ::= { vmEntry 2 }

   vmUUID OBJECT-TYPE
       SYNTAX       UUIDorZero
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The virtual machine's 128-bit Universally Unique
               Identifier (UUID) or the zero-length string when a
               UUID is not available.  If set, the UUID MUST uniquely
               identify a virtual machine from all other virtual
               machines in an administrative domain.  A zero-length
               octet string is returned if no UUID information is
               known."
       ::= { vmEntry 3 }

   vmOSType OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (0..255))





       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "A textual description containing operating system
               information installed on the virtual machine.  This
               value corresponds to the operating system the hypervisor
               assumes to be running when the virtual machine is
               started.  This may differ from the actual operating
               system in case the virtual machine boots into a
               different operating system."
       ::= { vmEntry 4 }

   vmAdminState OBJECT-TYPE
       SYNTAX       VirtualMachineAdminState
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The administrative state of the virtual machine."
       ::= { vmEntry 5 }

   vmOperState OBJECT-TYPE
       SYNTAX       VirtualMachineOperState
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The operational state of the virtual machine."
       ::= { vmEntry 6 }

   vmAutoStart OBJECT-TYPE
       SYNTAX       VirtualMachineAutoStart
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The autostart configuration of the virtual machine.  If
               this value is enable(2), the virtual machine
               automatically starts at the next initialization of the
               hypervisor."
       ::= { vmEntry 7 }

   vmPersistent OBJECT-TYPE
       SYNTAX       VirtualMachinePersistent
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "This value indicates whether the virtual machine has a
               persistent configuration, which means the virtual machine
               will still exist after its shutdown."
       ::= { vmEntry 8 }





   vmCurCpuNumber OBJECT-TYPE
       SYNTAX       Integer32 (0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The number of virtual CPUs currently assigned to the
               virtual machine."
       ::= { vmEntry 9 }

   vmMinCpuNumber OBJECT-TYPE
       SYNTAX       Integer32 (-1|0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The minimum number of virtual CPUs that are assigned to
               the virtual machine when it is in a power-on state.  The
               value -1 indicates that there is no hard boundary for
               the minimum number of virtual CPUs."
       ::= { vmEntry 10 }

   vmMaxCpuNumber OBJECT-TYPE
       SYNTAX       Integer32 (-1|0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The maximum number of virtual CPUs that are assigned to
               the virtual machine when it is in a power-on state.  The
               value -1 indicates that there is no limit."
       ::= { vmEntry 11 }

   vmMemUnit OBJECT-TYPE
       SYNTAX       Integer32 (1..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The multiplication unit in bytes for vmCurMem, vmMinMem,
               and vmMaxMem.  For example, when this value is 1024, the
               memory size unit for vmCurMem, vmMinMem, and vmMaxMem is
               KiB."
       ::= { vmEntry 12 }

   vmCurMem OBJECT-TYPE
       SYNTAX       Integer32 (0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The current memory size currently allocated to the
               virtual memory module in the unit designated by





               vmMemUnit."
       ::= { vmEntry 13 }

   vmMinMem OBJECT-TYPE
       SYNTAX       Integer32 (-1|0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The minimum memory size defined to the virtual machine
               in the unit designated by vmMemUnit.  The value -1
               indicates that there is no hard boundary for the minimum
               memory size."
       ::= { vmEntry 14 }

   vmMaxMem OBJECT-TYPE
       SYNTAX       Integer32 (-1|0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The maximum memory size defined to the virtual machine
               in the unit designated by vmMemUnit.  The value -1
               indicates that there is no limit."
       ::= { vmEntry 15 }


   vmUpTime OBJECT-TYPE
       SYNTAX       TimeTicks
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The time (in centiseconds) since the administrative
               state of the virtual machine was last changed from
               shutdown(4) to running(1)."
       ::= { vmEntry 16 }

   vmCpuTime OBJECT-TYPE
       SYNTAX       Counter64
       UNITS        "microsecond"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The total CPU time used in microseconds.  If the number
               of virtual CPUs is larger than 1, vmCpuTime may exceed
               real time.

               Discontinuities in the value of this counter can occur
               at re-initialization of the hypervisor and
               administrative state (vmAdminState) changes of the





               virtual machine."
       ::= { vmEntry 17 }

   -- The virtual CPU on each virtual machines
   vmCpuTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VmCpuEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "The table of virtual CPUs provided by the hypervisor."
       ::= { vmObjects 5 }

   vmCpuEntry OBJECT-TYPE
       SYNTAX       VmCpuEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "An entry for one virtual processor assigned to a
               virtual machine."
       INDEX { vmIndex, vmCpuIndex }
       ::= { vmCpuTable 1 }

   VmCpuEntry ::=
       SEQUENCE {
           vmCpuIndex              VirtualMachineCpuIndex,
           vmCpuCoreTime           Counter64
       }

   vmCpuIndex OBJECT-TYPE
       SYNTAX       VirtualMachineCpuIndex
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "A unique value identifying a virtual CPU assigned to
               the virtual machine."
       ::= { vmCpuEntry 1 }

   vmCpuCoreTime OBJECT-TYPE
       SYNTAX       Counter64
       UNITS        "microsecond"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The total CPU time used by this virtual CPU in
               microseconds.

               Discontinuities in the value of this counter can occur
               at re-initialization of the hypervisor and





               administrative state (vmAdminState) changes of the
               virtual machine."
       ::= { vmCpuEntry 2 }

   -- The virtual CPU affinity on each virtual machines

   vmCpuAffinityTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VmCpuAffinityEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "A list of CPU affinity entries of a virtual CPU."
       ::= { vmObjects 6 }

   vmCpuAffinityEntry OBJECT-TYPE
       SYNTAX       VmCpuAffinityEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "An entry containing CPU affinity associated with a
               particular virtual machine."
       INDEX   { vmIndex, vmCpuIndex, vmCpuPhysIndex }
       ::= { vmCpuAffinityTable 1 }

   VmCpuAffinityEntry ::=
       SEQUENCE {
           vmCpuPhysIndex          Integer32,
           vmCpuAffinity           INTEGER
       }

   vmCpuPhysIndex OBJECT-TYPE
       SYNTAX       Integer32 (1..2147483647)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "A value identifying a physical CPU on the hypervisor.
               On systems implementing the HOST-RESOURCES-MIB, the
               value MUST be the same value that is used as the index
               in the hrProcessorTable (hrDeviceIndex)."
       ::= { vmCpuAffinityEntry 2 }

   vmCpuAffinity OBJECT-TYPE
       SYNTAX       INTEGER {
                       unknown(0),   -- unknown
                       enable(1),    -- enabled
                       disable(2)    -- disabled
                    }
       MAX-ACCESS   read-only





       STATUS       current
       DESCRIPTION
               "The CPU affinity of this virtual CPU to the physical
               CPU represented by 'vmCpuPhysIndex'."
       ::= { vmCpuAffinityEntry 3 }

   -- The virtual storage devices on each virtual machine.  This
   -- document defines some overlapped objects with hrStorage in
   -- HOST-RESOURCES-MIB (RFC 2790), because virtual resources are
   -- allocated from the hypervisor's resources, which is the 'host
   -- resources'.
   vmStorageTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VmStorageEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "The conceptual table of virtual storage devices
               attached to the virtual machine."
       ::= { vmObjects 7 }

   vmStorageEntry OBJECT-TYPE
       SYNTAX       VmStorageEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "An entry for one virtual storage device attached to the
               virtual machine."
       INDEX { vmStorageVmIndex, vmStorageIndex }
       ::= { vmStorageTable 1 }

   VmStorageEntry ::=
       SEQUENCE {
           vmStorageVmIndex        VirtualMachineIndexOrZero,
           vmStorageIndex          VirtualMachineStorageIndex,
           vmStorageParent         Integer32,
           vmStorageSourceType     VirtualMachineStorageSourceType,
           vmStorageSourceTypeString
                                   SnmpAdminString,
           vmStorageResourceID     SnmpAdminString,
           vmStorageAccess         VirtualMachineStorageAccess,
           vmStorageMediaType      IANAStorageMediaType,
           vmStorageMediaTypeString
                                   SnmpAdminString,
           vmStorageSizeUnit       Integer32,
           vmStorageDefinedSize    Integer32,
           vmStorageAllocatedSize  Integer32,
           vmStorageReadIOs        Counter64,
           vmStorageWriteIOs       Counter64,





           vmStorageReadOctets     Counter64,
           vmStorageWriteOctets    Counter64,
           vmStorageReadLatency    Counter64,
           vmStorageWriteLatency   Counter64
       }

   vmStorageVmIndex OBJECT-TYPE
       SYNTAX       VirtualMachineIndexOrZero
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "This value identifies the virtual machine (guest) this
               storage device has been allocated to.  The value zero
               indicates that the storage device is currently not
               allocated to any virtual machines."
       ::= { vmStorageEntry 1 }

   vmStorageIndex OBJECT-TYPE
       SYNTAX       VirtualMachineStorageIndex
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "A unique value identifying a virtual storage device
               allocated to the virtual machine."
       ::= { vmStorageEntry 2 }

   vmStorageParent OBJECT-TYPE
       SYNTAX       Integer32 (0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The value of hrStorageIndex, which is the parent (i.e.,
               physical) device of this virtual device on systems
               implementing the HOST-RESOURCES-MIB.  The value zero
               denotes this virtual device is not any child
               represented in the hrStorageTable."
       ::= { vmStorageEntry 3 }

   vmStorageSourceType OBJECT-TYPE
       SYNTAX       VirtualMachineStorageSourceType
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The source type of the virtual storage device."
       ::= { vmStorageEntry 4 }

   vmStorageSourceTypeString OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (0..255))





       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "A (detailed) textual string of the source type of the
               virtual storage device.  For example, this represents
               the specific format name of the sparse file."
       ::= { vmStorageEntry 5 }

   vmStorageResourceID OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (0..255))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "A textual string that represents the resource
               identifier of the virtual storage.  For example, this
               contains the path to the disk image file that
               corresponds to the virtual storage."
       ::= { vmStorageEntry 6 }

   vmStorageAccess OBJECT-TYPE
       SYNTAX       VirtualMachineStorageAccess
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The access permission of the virtual storage device."
       ::= { vmStorageEntry 7 }

   vmStorageMediaType OBJECT-TYPE
       SYNTAX       IANAStorageMediaType
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The media type of the virtual storage device."
       ::= { vmStorageEntry 8 }

   vmStorageMediaTypeString OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (0..255))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "A (detailed) textual string of the virtual storage
               media.  For example, this represents the specific driver
               name of the emulated media such as 'IDE' and 'SCSI'."
       ::= { vmStorageEntry 9 }

   vmStorageSizeUnit OBJECT-TYPE
       SYNTAX       Integer32 (1..2147483647)
       MAX-ACCESS   read-only





       STATUS       current
       DESCRIPTION
               "The multiplication unit in bytes for
               vmStorageDefinedSize and vmStorageAllocatedSize.  For
               example, when this value is 1048576, the storage size
               unit for vmStorageDefinedSize and vmStorageAllocatedSize
               is MiB."
       ::= { vmStorageEntry 10 }

   vmStorageDefinedSize OBJECT-TYPE
       SYNTAX       Integer32 (-1|0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The defined virtual storage size defined in the unit
               designated by vmStorageSizeUnit.  If this information is
               not available, this value MUST be -1."
       ::= { vmStorageEntry 11 }

   vmStorageAllocatedSize OBJECT-TYPE
       SYNTAX       Integer32 (-1|0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The storage size allocated to the virtual storage from
               a physical storage in the unit designated by
               vmStorageSizeUnit.  When the virtual storage is block
               device or raw file, this value and vmStorageDefinedSize
               are supposed to equal.  This value MUST NOT be different
               from vmStorageDefinedSize when vmStorageSourceType is
               'block' or 'raw'.  If this information is not available,
               this value MUST be -1."
       ::= { vmStorageEntry 12 }

   vmStorageReadIOs OBJECT-TYPE
       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The number of read I/O requests.

               Discontinuities in the value of this counter can occur
               at re-initialization of the hypervisor and
               administrative state (vmAdminState) changes of the
               virtual machine."
       ::= { vmStorageEntry 13 }

   vmStorageWriteIOs OBJECT-TYPE





       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The number of write I/O requests.

               Discontinuities in the value of this counter can occur
               at re-initialization of the hypervisor and
               administrative state (vmAdminState) changes of the
               virtual machine."
       ::= { vmStorageEntry 14 }

   vmStorageReadOctets OBJECT-TYPE
       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The total number of bytes read from this device.

               Discontinuities in the value of this counter can occur
               at re-initialization of the hypervisor and
               administrative state (vmAdminState) changes of the
               virtual machine."
       ::= { vmStorageEntry 15 }

   vmStorageWriteOctets OBJECT-TYPE
       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The total number of bytes written to this device.

               Discontinuities in the value of this counter can occur
               at re-initialization of the hypervisor and
               administrative state (vmAdminState) changes of the
               virtual machine."
       ::= { vmStorageEntry 16 }

   vmStorageReadLatency OBJECT-TYPE
       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The total number of microseconds read requests have
               been queued for this device.

               This would typically be implemented by storing the high
               precision system timestamp of when the request is





               received from the virtual machine with the request, the
               difference between this initial timestamp and the time
               at which the requested operation has completed SHOULD be
               converted to microseconds and accumulated.

               Discontinuities in the value of this counter can occur at
               re-initialization of the hypervisor and administrative
               state (vmAdminState) changes of the virtual machine."
       ::= { vmStorageEntry 17 }

   vmStorageWriteLatency OBJECT-TYPE
       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The total number of microseconds write requests have
               been queued for this device.

               This would typically be implemented by storing the high
               precision system timestamp of when the request is
               received from the virtual machine with the request; the
               difference between this initial timestamp and the time
               at which the requested operation has completed SHOULD be
               converted to microseconds and accumulated.

               Discontinuities in the value of this counter can occur
               at re-initialization of the hypervisor and
               administrative state (vmAdminState) changes of the
               virtual machine."
       ::= { vmStorageEntry 18 }


   -- The virtual network interfaces on each virtual machine.
   vmNetworkTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VmNetworkEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "The conceptual table of virtual network interfaces
               attached to the virtual machine."
       ::= { vmObjects 8 }

   vmNetworkEntry OBJECT-TYPE
       SYNTAX       VmNetworkEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "An entry for one virtual network interface attached to





               the virtual machine."
       INDEX { vmIndex, vmNetworkIndex }
       ::= { vmNetworkTable 1 }

   VmNetworkEntry ::=
       SEQUENCE {
           vmNetworkIndex          VirtualMachineNetworkIndex,
           vmNetworkIfIndex        InterfaceIndexOrZero,
           vmNetworkParent         InterfaceIndexOrZero,
           vmNetworkModel          SnmpAdminString,
           vmNetworkPhysAddress    PhysAddress
       }

   vmNetworkIndex OBJECT-TYPE
       SYNTAX       VirtualMachineNetworkIndex
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
               "A unique value identifying a virtual network interface
               allocated to the virtual machine."
       ::= { vmNetworkEntry 1 }

   vmNetworkIfIndex OBJECT-TYPE
       SYNTAX       InterfaceIndexOrZero
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The value of ifIndex, which corresponds to this virtual
               network interface.  If this device is not represented in
               the ifTable, then this value MUST be zero."
       ::= { vmNetworkEntry 2 }

   vmNetworkParent OBJECT-TYPE
       SYNTAX       InterfaceIndexOrZero
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The value of ifIndex, which corresponds to the parent
               (i.e., physical) device of this virtual device.  The
               value zero denotes this virtual device is not any
               child represented in the ifTable."
       ::= { vmNetworkEntry 3 }

   vmNetworkModel OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (0..255))
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION





               "A textual string containing the (emulated) model of the
               virtual network interface.  For example, this value is
               'virtio' when the emulation driver model is virtio."
       ::= { vmNetworkEntry 4 }

   vmNetworkPhysAddress OBJECT-TYPE
       SYNTAX       PhysAddress
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
               "The Media Access Control (MAC) address of the virtual
               network interface."
       ::= { vmNetworkEntry 5 }


   -- Notification definitions:

   vmPerVMNotificationsEnabled OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
               "Indicates if the notification generator will send
               notifications per virtual machine.  Changes to this
               object MUST NOT persist across re-initialization of
               the management system, e.g., SNMP agent."
       ::= { vmObjects 9 }

   vmBulkNotificationsEnabled OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
               "Indicates if the notification generator will send
               notifications per set of virtual machines.  Changes to
               this object MUST NOT persist across re-initialization of
               the management system, e.g., SNMP agent."
       ::= { vmObjects 10 }

   vmAffectedVMs OBJECT-TYPE
       SYNTAX       VirtualMachineList
       MAX-ACCESS   accessible-for-notify
       STATUS       current
       DESCRIPTION
               "A complete list of virtual machines whose state has
               changed.  This object is the only object sent with bulk
               notifications."
       ::= { vmObjects 11 }





   vmRunning NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of a virtual machine has been changed to
               running(4) from some other state.  The other state is
               indicated by the included value of vmOperState."
       ::= { vmNotifications 1 }

   vmShuttingdown NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of a virtual machine has been changed to
               shuttingdown(10) from some other state.  The other state
               is indicated by the included value of vmOperState."
       ::= { vmNotifications 2 }

   vmShutdown NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of a virtual machine has been changed to
               shutdown(11) from some other state.  The other state is
               indicated by the included value of vmOperState."
       ::= { vmNotifications 3 }

   vmPaused NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }





       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of a virtual machine has been changed to
               paused(8) from some other state.  The other state is
               indicated by the included value of vmOperState."
       ::= { vmNotifications 4 }

   vmSuspending NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of a virtual machine has been changed to
               suspending(5) from some other state.  The other state is
               indicated by the included value of vmOperState."
       ::= { vmNotifications 5 }

   vmSuspended NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of a virtual machine has been changed to
               suspended(6) from some other state.  The other state is
               indicated by the included value of vmOperState."
       ::= { vmNotifications 6 }

   vmResuming NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of a virtual machine has been changed to
               resuming(7) from some other state.  The other state is
               indicated by the included value of vmOperState."





       ::= { vmNotifications 7 }

   vmMigrating NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of a virtual machine has been changed to
               migrating(9) from some other state.  The other state is
               indicated by the included value of vmOperState."
       ::= { vmNotifications 8 }

   vmCrashed NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when a virtual machine
               has been crashed.  The previous state of the virtual
               machine is indicated by the included value of
               vmOperState."
       ::= { vmNotifications 9 }

   vmDeleted NOTIFICATION-TYPE
       OBJECTS      {
                       vmName,
                       vmUUID,
                       vmOperState,
                       vmPersistent
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when a virtual machine
               has been deleted.  The prior state of the virtual
               machine is indicated by the included value of
               vmOperState."
       ::= { vmNotifications 10 }

   vmBulkRunning NOTIFICATION-TYPE
       OBJECTS      {
                       vmAffectedVMs





                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of one or more virtual machines has been changed
               to running(4) from any prior state, except for
               running(4).  Management stations are encouraged to
               subsequently poll the subset of virtual machines of
               interest for vmOperState."
       ::= { vmNotifications 11 }

   vmBulkShuttingdown NOTIFICATION-TYPE
       OBJECTS      {
                      vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of one or more virtual machines has been changed
               to shuttingdown(10) from a state other than
               shuttingdown(10).  Management stations are encouraged to
               subsequently poll the subset of virtual machines of
               interest for vmOperState."
       ::= { vmNotifications 12 }

   vmBulkShutdown NOTIFICATION-TYPE
       OBJECTS      {
                      vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of one or more virtual machine has been changed to
               shutdown(11) from a state other than shutdown(11).
               Management stations are encouraged to subsequently poll
               the subset of virtual machines of interest for
               vmOperState."
       ::= { vmNotifications 13 }

   vmBulkPaused NOTIFICATION-TYPE
       OBJECTS      {
                       vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of one or more virtual machines has been changed
               to paused(8) from a state other than paused(8).





               Management stations are encouraged to subsequently poll
               the subset of virtual machines of interest for
               vmOperState."
       ::= { vmNotifications 14 }

   vmBulkSuspending NOTIFICATION-TYPE
       OBJECTS      {
                       vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of one or more virtual machines has been changed
               to suspending(5) from a state other than suspending(5).
               Management stations are encouraged to subsequently poll
               the subset of virtual machines of interest for
               vmOperState."
       ::= { vmNotifications 15 }

   vmBulkSuspended NOTIFICATION-TYPE
       OBJECTS      {
                       vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of one or more virtual machines has been changed
               to suspended(6) from a state other than suspended(6).
               Management stations are encouraged to subsequently poll
               the subset of virtual machines of interest for
               vmOperState."
       ::= { vmNotifications 16 }

   vmBulkResuming NOTIFICATION-TYPE
       OBJECTS      {
                       vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of one or more virtual machines has been changed
               to resuming(7) from a state other than resuming(7).
               Management stations are encouraged to subsequently poll
               the subset of virtual machines of interest for
               vmOperState."
       ::= { vmNotifications 17 }

   vmBulkMigrating NOTIFICATION-TYPE





       OBJECTS      {
                       vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when the operational
               state of one or more virtual machines has been changed
               to migrating(9) from a state other than migrating(9).
               Management stations are encouraged to subsequently poll
               the subset of virtual machines of interest for
               vmOperState."
       ::= { vmNotifications 18 }

   vmBulkCrashed NOTIFICATION-TYPE
       OBJECTS      {
                       vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when one or more virtual
               machines have been crashed.  Management stations are
               encouraged to subsequently poll the subset of virtual
               machines of interest for vmOperState."
       ::= { vmNotifications 19 }

   vmBulkDeleted NOTIFICATION-TYPE
       OBJECTS      {
                       vmAffectedVMs
                    }
       STATUS       current
       DESCRIPTION
               "This notification is generated when one or more virtual
               machines have been deleted.  Management stations are
               encouraged to subsequently poll the subset of virtual
               machines of interest for vmOperState."
       ::= { vmNotifications 20 }

   -- Compliance definitions:
   vmCompliances  OBJECT IDENTIFIER ::= { vmConformance 1 }
   vmGroups       OBJECT IDENTIFIER ::= { vmConformance 2 }

   vmFullCompliances MODULE-COMPLIANCE
       STATUS       current
       DESCRIPTION
               "Compliance statement for implementations supporting
               read/write access, according to the object definitions."
       MODULE     -- this module
       MANDATORY-GROUPS {





           vmHypervisorGroup,
           vmVirtualMachineGroup,
           vmCpuGroup,
           vmCpuAffinityGroup,
           vmStorageGroup,
           vmNetworkGroup
       }
       GROUP  vmPerVMNotificationOptionalGroup
       DESCRIPTION
               "Support for per-VM notifications is optional.  If not
               implemented, then vmPerVMNotificationsEnabled MUST report
               false(2)."
       GROUP  vmBulkNotificationsVariablesGroup
       DESCRIPTION
               "Necessary only if vmPerVMNotificationOptionalGroup is
               implemented."
       GROUP  vmBulkNotificationOptionalGroup
       DESCRIPTION
               "Support for bulk notifications is optional.  If not
               implemented, then vmBulkNotificationsEnabled MUST report
               false(2)."

       ::= { vmCompliances 1 }

   vmReadOnlyCompliances MODULE-COMPLIANCE
       STATUS       current
       DESCRIPTION
               "Compliance statement for implementations supporting
               only read-only access."
       MODULE     -- this module
       MANDATORY-GROUPS {
           vmHypervisorGroup,
           vmVirtualMachineGroup,
           vmCpuGroup,
           vmCpuAffinityGroup,
           vmStorageGroup,
           vmNetworkGroup
       }

       OBJECT vmPerVMNotificationsEnabled
       MIN-ACCESS   read-only
       DESCRIPTION
               "Write access is not required."

       OBJECT vmBulkNotificationsEnabled
       MIN-ACCESS   read-only
       DESCRIPTION
               "Write access is not required."





       ::= { vmCompliances 2 }

   vmHypervisorGroup OBJECT-GROUP
       OBJECTS {
           vmHvSoftware,
           vmHvVersion,
           vmHvObjectID,
           vmHvUpTime,
           vmNumber,
           vmTableLastChange,
           vmPerVMNotificationsEnabled,
           vmBulkNotificationsEnabled
       }
       STATUS       current
       DESCRIPTION
               "A collection of objects providing insight into the
               hypervisor itself."
        ::= { vmGroups 1 }

   vmVirtualMachineGroup OBJECT-GROUP
       OBJECTS {
           -- vmIndex
           vmName,
           vmUUID,
           vmOSType,
           vmAdminState,
           vmOperState,
           vmAutoStart,
           vmPersistent,
           vmCurCpuNumber,
           vmMinCpuNumber,
           vmMaxCpuNumber,
           vmMemUnit,
           vmCurMem,
           vmMinMem,
           vmMaxMem,
           vmUpTime,
           vmCpuTime
       }
       STATUS       current
       DESCRIPTION
               "A collection of objects providing insight into the
               virtual machines controlled by a hypervisor."
       ::= { vmGroups 2 }

   vmCpuGroup OBJECT-GROUP
       OBJECTS {
           -- vmCpuIndex,





           vmCpuCoreTime
       }
       STATUS       current
       DESCRIPTION
               "A collection of objects providing insight into the
               virtual machines controlled by a hypervisor."
       ::= { vmGroups 3 }

   vmCpuAffinityGroup OBJECT-GROUP
       OBJECTS {
           -- vmCpuPhysIndex,
           vmCpuAffinity
       }
       STATUS       current
       DESCRIPTION
               "A collection of objects providing insight into the
               virtual machines controlled by a hypervisor."
       ::= { vmGroups 4 }

   vmStorageGroup OBJECT-GROUP
       OBJECTS {
           -- vmStorageVmIndex,
           -- vmStorageIndex,
           vmStorageParent,
           vmStorageSourceType,
           vmStorageSourceTypeString,
           vmStorageResourceID,
           vmStorageAccess,
           vmStorageMediaType,
           vmStorageMediaTypeString,
           vmStorageSizeUnit,
           vmStorageDefinedSize,
           vmStorageAllocatedSize,
           vmStorageReadIOs,
           vmStorageWriteIOs,
           vmStorageReadOctets,
           vmStorageWriteOctets,
           vmStorageReadLatency,
           vmStorageWriteLatency
       }
       STATUS       current
       DESCRIPTION
               "A collection of objects providing insight into the
               virtual storage devices controlled by a hypervisor."
       ::= { vmGroups 5 }

   vmNetworkGroup OBJECT-GROUP
       OBJECTS {





           -- vmNetworkIndex,
           vmNetworkIfIndex,
           vmNetworkParent,
           vmNetworkModel,
           vmNetworkPhysAddress
       }
       STATUS       current
       DESCRIPTION
               "A collection of objects providing insight into the
               virtual network interfaces controlled by a hypervisor."
       ::= { vmGroups 6 }

   vmPerVMNotificationOptionalGroup NOTIFICATION-GROUP
       NOTIFICATIONS {
           vmRunning,
           vmShuttingdown,
           vmShutdown,
           vmPaused,
           vmSuspending,
           vmSuspended,
           vmResuming,
           vmMigrating,
           vmCrashed,
           vmDeleted
       }
       STATUS       current
       DESCRIPTION
               "A collection of notifications for per-VM notification
               of changes to virtual machine state (vmOperState) as
               reported by a hypervisor."
       ::= { vmGroups 7 }

   vmBulkNotificationsVariablesGroup OBJECT-GROUP
       OBJECTS {
           vmAffectedVMs
       }
       STATUS       current
       DESCRIPTION
               "The variables used in vmBulkNotificationOptionalGroup
               virtual network interfaces controlled by a hypervisor."
       ::= { vmGroups 8 }

   vmBulkNotificationOptionalGroup NOTIFICATION-GROUP
       NOTIFICATIONS {
           vmBulkRunning,
           vmBulkShuttingdown,
           vmBulkShutdown,
           vmBulkPaused,





           vmBulkSuspending,
           vmBulkSuspended,
           vmBulkResuming,
           vmBulkMigrating,
           vmBulkCrashed,
           vmBulkDeleted
       }
       STATUS       current
       DESCRIPTION
               "A collection of notifications for bulk notification of
               changes to virtual machine state (vmOperState) as
               reported by a given hypervisor."
       ::= { vmGroups 9 }

   END


