DOCS-IETF-SUBMGT-MIB  DEFINITIONS ::= BEGIN


   IMPORTS
           MODULE-IDENTITY,
           OBJECT-TYPE,
           Integer32,
           mib-2
                   FROM SNMPv2-SMI
           RowStatus,
           TruthValue,
           TimeStamp,
           StorageType
                   FROM SNMPv2-TC
           OBJECT-GROUP,
           MODULE-COMPLIANCE
                   FROM SNMPv2-CONF
           InetAddressType,
           InetAddress
                   FROM INET-ADDRESS-MIB
           docsIfCmtsCmStatusIndex,
           docsIfCmtsCmStatusEntry
                   FROM DOCS-IF-MIB  -- RFC2670
           diffServMIBDataPathGroup,
           diffServMIBClfrGroup,
           diffServMIBClfrElementGroup,
           diffServMIBMultiFieldClfrGroup,





           diffServMIBActionGroup,
           diffServMIBAlgDropGroup,
           diffServMIBCounterGroup,
           diffServDataPathStatus,
           diffServClfrStatus,
           diffServClfrElementStatus,
           diffServMultiFieldClfrAddrType,
           diffServMultiFieldClfrSrcAddr,
           diffServMultiFieldClfrDstAddr,
           diffServAlgDropStatus,
           diffServDataPathStorage,
           diffServClfrStorage,
           diffServClfrElementStorage,
           diffServMultiFieldClfrStorage,
           diffServActionStorage,
           diffServCountActStorage,
           diffServAlgDropStorage,
           diffServAlgDropType
                   FROM DIFFSERV-MIB  -- RFC3289
        ;

   docsSubMgt MODULE-IDENTITY
       LAST-UPDATED    "200503290000Z" -- March 29, 2005
       ORGANIZATION    "IETF IP over Cable Data Network (IPCDN) Working
                        Group"
       CONTACT-INFO
           "        Wilson Sawyer
            Postal: 50 Kelly Brook Lane
                    East Hampstead, NH 03826
                    U.S.A.

            Phone:  +1 603 382 7080
            E-mail: wsawyer@ieee.org

            IETF IPCDN Working Group
            General Discussion: ipcdn@ietf.org
            Subscribe: http://www.ietf.org/mailman/listinfo/ipcdn
            Archive: ftp://ftp.ietf.org/ietf-mail-archive/ipcdn
            Co-chairs: Richard Woundy, Richard_Woundy@cable.comcast.com
                       Jean-Francois Mule, jf.mule@cablelabs.com"
       DESCRIPTION
           "This is the CMTS centric subscriber management MIB for
       DOCSIS-compliant CMTS.  It provides the objects to allow a Cable
       Modem Termination operator to control the IP addresses and
       protocols associated with subscribers' cable modems.








       Copyright (C) The Internet Society (2005).  This version of this
       MIB module is part of RFC 4036; see the RFC itself for full legal
       notices."
       REVISION "200503290000Z" -- March 29, 2005
       DESCRIPTION
          "Initial version, published as RFC 4036.  Note that the
          compliance statements in this version apply only to
          implementations that support DOCSIS 1.0/1.1/2.0, which
          are not IPv6-capable."
       ::= { mib-2 125 }

   docsSubMgtObjects OBJECT IDENTIFIER ::= { docsSubMgt 1 }

   docsSubMgtCpeControlTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF DocsSubMgtCpeControlEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "This table AUGMENTs the docsIfCmtsCmStatusTable, adding
       four WRITEable objects, as well as a read-only object, all of
       which reflect the state of subscriber management on a particular
       CM."
       ::= { docsSubMgtObjects 1 }

   docsSubMgtCpeControlEntry OBJECT-TYPE
       SYNTAX  DocsSubMgtCpeControlEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "A row in the docsSubMgtCpeControlTable.  All values are set
       at successful modem registration, either from the system default,
       or from objects included in the DOCSIS registration request sent
       upstream to the CMTS from the CM.  The contents of this entry are
       meaningless unless the corresponding docsIfCmtsCmStatusValue (see
       reference) is registrationComplete(6).  The persistence of this
       row is determined solely by the lifespan of the corresponding
       docsIfCmtsCmStatusEntry (normally StorageType=volatile)."

       REFERENCE
           "RFC 2670"
       AUGMENTS { docsIfCmtsCmStatusEntry }
       ::= {docsSubMgtCpeControlTable 1 }

   DocsSubMgtCpeControlEntry ::= SEQUENCE
       {
       docsSubMgtCpeControlMaxCpeIp        Integer32,
       docsSubMgtCpeControlActive          TruthValue,
       docsSubMgtCpeControlLearnable       TruthValue,





       docsSubMgtCpeControlReset           TruthValue,
       docsSubMgtCpeControlLastReset       TimeStamp
       }

   docsSubMgtCpeControlMaxCpeIp OBJECT-TYPE
       SYNTAX  Integer32(0..2147483647)
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "The number of simultaneous IP addresses permitted behind
       the CM.  If this is set to zero, all CPE traffic from the CM is
       dropped.  If the provisioning object corresponding to
       docsSubMgtCpeIpTable includes more CPE IP address entries for
       this modem than the value of this object, then this object is
       set to the count of the number of rows in docsSubMgtCpeIpTable
       that have the same docsIfCmtsCmStatusIndex value.  (For example,
       if the CM has 5 IP addresses specified for it, this value is 5.)
       This limit applies to learned and DOCSIS-provisioned entries
       but not to entries added through some administrative
       process at the CMTS.  If not set through DOCSIS provisioning,
       this object defaults to docsSubMgtCpeMaxIpDefault.  Note that
       this object is only meaningful if docsSubMgtCpeControlActive
       is true."
       ::= { docsSubMgtCpeControlEntry 1 }

   docsSubMgtCpeControlActive OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "Controls the application of subscriber management to
       this cable modem.  If this is set to true, CMTS-based CPE
       control is active, and all the actions required by the various
       filter tables and controls apply at the CMTS.  If this is set
       to false, no subscriber management filtering is done at the
       CMTS (but other filters may apply).  If not set through DOCSIS
       provisioning, this object defaults to
       docsSubMgtCpeActiveDefault."
       ::= { docsSubMgtCpeControlEntry 2 }

   docsSubMgtCpeControlLearnable OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "Controls whether the CMTS may learn (and pass traffic
       for) CPE IP addresses associated with a cable modem.  If this is
       set to true, the CMTS may learn up to docsSubMgtMaxCpeIp





       addresses (less any DOCSIS-provisioned entries) related to this
       CM.  Those IP addresses are added (by internal process) to the
       docsSubMgtCpeIpTable.  The nature of the learning mechanism is
       not specified here.

       If not set through DOCSIS provisioning, this object defaults to
       docsSubMgtCpeLearnableDefault.  Note that this object is only
       meaningful if docsSubMgtCpeControlActive is true."
       ::= { docsSubMgtCpeControlEntry 3 }

   docsSubMgtCpeControlReset OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "This object always returns false on read.  If this object is
       set to true, the rows with 'learned' addresses in
       docsSubMgtCpeIpTable for this CM are deleted from that table."
       ::= { docsSubMgtCpeControlEntry 4 }

   docsSubMgtCpeControlLastReset OBJECT-TYPE
       SYNTAX  TimeStamp
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "The value of sysUpTime when docsSubMgtCpeControlReset was
       last set true.  Zero if never reset."
       DEFVAL { 0 }
       ::= { docsSubMgtCpeControlEntry 5 }

   docsSubMgtCpeMaxIpDefault OBJECT-TYPE
       SYNTAX  Integer32(0..2147483647)
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "The default value for docsSubMgtCpeControlMaxCpeIp if not
       signaled in the DOCSIS Registration request.  This value should
       be treated as nonvolatile; if set, its value should persist
       across device resets."
       DEFVAL { 16 }
       ::= { docsSubMgtObjects 2 }

   docsSubMgtCpeActiveDefault OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "The default value for docsSubMgtCpeControlActive if not





       signaled in the DOCSIS Registration request.  This value should
       be treated as nonvolatile; if set, its value should persist
       across device resets."
       DEFVAL { false }
       ::= { docsSubMgtObjects 3 }

   docsSubMgtCpeLearnableDefault OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "The default value for docsSubMgtCpeControlLearnable if not
       signaled in the DOCSIS Registration request.  This value should
       be treated as nonvolatile; if set, its value should persist
       across device resets."
       DEFVAL { true }
       ::= { docsSubMgtObjects 4 }

   docsSubMgtCpeIpTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF DocsSubMgtCpeIpEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table of CPE IP addresses known on a per-CM basis."
       ::= { docsSubMgtObjects 5 }

   docsSubMgtCpeIpEntry OBJECT-TYPE
       SYNTAX      DocsSubMgtCpeIpEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry in the docsSubMgtCpeIpTable.  The first index is
       the specific modem we're referring to, and the second index is
       the specific CPE IP entry."
       INDEX   { docsIfCmtsCmStatusIndex,
                 docsSubMgtCpeIpIndex }
       ::= {docsSubMgtCpeIpTable 1 }

   DocsSubMgtCpeIpEntry ::= SEQUENCE
       {
       docsSubMgtCpeIpIndex        Integer32,
       docsSubMgtCpeIpAddressType  InetAddressType,
       docsSubMgtCpeIpAddr         InetAddress,
       docsSubMgtCpeIpLearned      TruthValue
       }

   docsSubMgtCpeIpIndex OBJECT-TYPE
       SYNTAX      Integer32(1..2147483647)





       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The index of this CPE IP address relative to the indexed CM.
       An entry is created either through the included CPE IP addresses
       in the provisioning object, or via learning.

       If docsSubMgtCpeControlActive is true and a CMTS receives
       an IP packet from a CM that contains a source IP address that
       does not match one of the docsSubMgtCpeIpAddr entries for this
       CM, one of two things occurs.  If the number of entries is less
       than docsSubMgtCpeControlMaxCpeIp, the source address is added to
       the table and the packet is forwarded.  If the number of entries
       equals the docsSubMgtCpeControlMaxCpeIp, then the packet is
       dropped."
       ::= { docsSubMgtCpeIpEntry 1 }

   docsSubMgtCpeIpAddressType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The type of internet address of docsSubMgtCpeIpAddr."
       ::= { docsSubMgtCpeIpEntry 2 }

   docsSubMgtCpeIpAddr OBJECT-TYPE
       SYNTAX      InetAddress
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The IP address either set from provisioning or learned via
       address gleaning or other forwarding means.  See
       docsSubMgtCpeIpIndex for the mechanism.

       The type of this address is determined by the value of
       docsSubMgtCpeIpAddressType."
       ::= { docsSubMgtCpeIpEntry 3 }

   docsSubMgtCpeIpLearned OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "If true, this entry was learned from IP packets sent
       upstream rather than from the provisioning objects."
       ::= { docsSubMgtCpeIpEntry 4 }

   docsSubMgtCmFilterTable OBJECT-TYPE





       SYNTAX  SEQUENCE OF DocsSubMgtCmFilterEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Binds filter groups to modems, identifying for each modem
       the upstream and downstream filter groups that apply to packets
       for that modem.  Normally, this table reflects the filter group
       values signaled by DOCSIS Registration, although values may be
       overridden by management action.

       For each of the columns in this table, zero is a distinguished
       value, indicating that the default filtering action is to be
       taken rather than that associated with a filter group number.
       Zero is used if the filter group is not signaled by DOCSIS
       registration."
       ::= { docsSubMgtObjects 6 }

   docsSubMgtCmFilterEntry OBJECT-TYPE
       SYNTAX  DocsSubMgtCmFilterEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Binds a filter group to each direction of traffic for a
       modem.  The filters in this entry apply if
       docsSubMgtCpeControlActive is true.

       The contents of this entry are meaningless unless the
       corresponding docsIfCmtsCmStatusValue (see reference) is
       registrationComplete(6).  The persistence of this row is
       determined solely by the lifespan of the corresponding
       docsIfCmtsCmStatusEntry (normally StorageType=volatile)."
       REFERENCE
           "RFC 2670"
       AUGMENTS { docsIfCmtsCmStatusEntry }
       ::= {docsSubMgtCmFilterTable 1 }

   DocsSubMgtCmFilterEntry ::= SEQUENCE
       {
       docsSubMgtCmFilterSubDownstream        Integer32,
       docsSubMgtCmFilterSubUpstream          Integer32,
       docsSubMgtCmFilterCmDownstream         Integer32,
       docsSubMgtCmFilterCmUpstream           Integer32
   }

   docsSubMgtCmFilterSubDownstream OBJECT-TYPE
       SYNTAX  Integer32(0..65535)
       MAX-ACCESS read-write
       STATUS  current





       DESCRIPTION
           "The filter group applied to traffic destined for subscribers
       attached to the referenced CM.  Upon row creation, this is set
       either to zero (use default classification, the
       diffServClfrElementSpecific=zeroDotZero row of
       diffServClfrElementTable) or to the value in the provisioning
       object sent upstream from the CM to the CMTS during registration.
       The value of this object is the same as that of the filter group
       index appearing as docsSubMgtFilterGroupIndex."
       ::= { docsSubMgtCmFilterEntry 1 }

   docsSubMgtCmFilterSubUpstream OBJECT-TYPE
       SYNTAX  Integer32(0..65535)
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "The filter group applied to traffic originating from
       subscribers attached to the referenced CM.  Upon row creation
       this is set to either zero (use default classification, the
       diffServClfrElementSpecific=zeroDotZero row of
       diffServClfrElementTable), or to the value in the provisioning
       object sent upstream from the CM to the CMTS.  The value of this
       object is the same as that of the filter group index appearing as
       docsSubMgtFilterGroupIndex."
       ::= { docsSubMgtCmFilterEntry 2 }

   docsSubMgtCmFilterCmDownstream OBJECT-TYPE
       SYNTAX  Integer32(0..65535)
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "The filter group applied to traffic destined for the
       referenced CM itself.  Upon row creation this is set either to
       zero (use default classification, the
       diffServClfrElementSpecific=zeroDotZero row of
       diffServClfrElementTable), or to the value in the provisioning
       object sent upstream from the CM to the CMTS during registration.
       The value of this object is the same as that of the filter group
       index appearing as docsSubMgtFilterGroupIndex."
       ::= { docsSubMgtCmFilterEntry 3 }

   docsSubMgtCmFilterCmUpstream OBJECT-TYPE
       SYNTAX  Integer32(0..65535)
       MAX-ACCESS read-write
       STATUS  current
       DESCRIPTION
           "The filter group applied to traffic originating from the
       referenced CM itself.  This is set upon row creation to either





       zero (use default classification, the
       diffServClfrElementSpecific=zeroDotZero row of
       diffServClfrElementTable), or to the value in the provisioning
       object sent upstream from the CM to the CMTS during registration.
       The value of this object is the same as the filter group index
       appearing as docsSubMgtFilterGroupIndex."
       ::= { docsSubMgtCmFilterEntry 4 }

   docsSubMgtFilterGroupTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF DocsSubMgtFilterGroupEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Provides a collection of referenceable entries to which
       diffServClfrElementSpecific refers.  This table provides filter
       group indices that can be compared with those signaled during
       DOCSIS registration.  A packet matches an entry from this table
       if the packet originated from or is destined to a cable modem
       that registered this index as one of its four filter groups
       (see docsSubMgtCmFilterTable), and if the packet direction and
       MAC address select the use of this index among the four."
       ::= { docsSubMgtObjects 7 }

   docsSubMgtFilterGroupEntry OBJECT-TYPE
       SYNTAX  DocsSubMgtFilterGroupEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "An entry only exists if needed by the
       diffServClfrElementEntry.  A packet matches this entry if the
       packet's cable modem registered this index as one of its four
       filter groups (see docsSubMgtCmFilterTable) and if the packet
       direction and MAC address select the use of this index among
       the four."
       INDEX { docsSubMgtFilterGroupIndex }
       ::= { docsSubMgtFilterGroupTable 1 }

   DocsSubMgtFilterGroupEntry ::= SEQUENCE
       {
       docsSubMgtFilterGroupIndex    Integer32
       }

   docsSubMgtFilterGroupIndex OBJECT-TYPE
       SYNTAX  Integer32(1..65535)
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "The filter group index, from the set signaled at DOCSIS





       Registration.  Provides a referenceable entry to which
       diffServClfrElementSpecific points.  A packet matches this
       classifier entry if the packet's cable modem registered this
       index value as one of its four filter groups, and if the packet
       direction and MAC address select the use of this index among
       the four.  Because this is the only field in this table, it is
       read-only, contrary to the usual SMI custom of making indices
       not-accessible.

       Note that although zero may be signaled (or defaulted) at DOCSIS
       Registration to indicate a default filtering group, no such entry
       appears in this table, as diffServClfrElementSpecific will
       use a zeroDotZero pointer for that classification."
       ::= { docsSubMgtFilterGroupEntry 1 }

   docsSubMgtConformance OBJECT IDENTIFIER ::= { docsSubMgt 2 }
   docsSubMgtCompliances OBJECT IDENTIFIER ::=
                                           { docsSubMgtConformance 1 }
   docsSubMgtGroups OBJECT IDENTIFIER      ::=
                                           { docsSubMgtConformance 2 }

   docsSubMgtBasicCompliance MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "The compliance statement for CMTS devices that implement
       CMTS centric subscriber management.

       This compliance statement applies to implementations that
       support DOCSIS 1.0/1.1/2.0, which are not IPv6 capable."


   MODULE DIFFSERV-MIB -- RFC3289
     MANDATORY-GROUPS {
              diffServMIBDataPathGroup,
              diffServMIBClfrGroup,
              diffServMIBClfrElementGroup,
              diffServMIBMultiFieldClfrGroup,
              diffServMIBActionGroup,
              diffServMIBAlgDropGroup,
              diffServMIBCounterGroup
              }

   OBJECT diffServDataPathStatus  -- same as RFC3289
       SYNTAX RowStatus { active(1) }
       WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
       DESCRIPTION
           "Support for createAndWait and notInService is not required."






   OBJECT diffServClfrStatus  -- same as RFC3289
       SYNTAX RowStatus { active(1) }
       WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
       DESCRIPTION
           "Support for createAndWait and notInService is not required."

   OBJECT diffServClfrElementStatus  -- same as RFC3289
       SYNTAX RowStatus { active(1) }
       WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
       DESCRIPTION
           "Support for createAndWait and notInService is not required."

   OBJECT diffServMultiFieldClfrAddrType
       SYNTAX  InetAddressType { ipv4(1) }
       DESCRIPTION
           "An implementation is only required to support IPv4
       addresses."

   OBJECT diffServMultiFieldClfrSrcAddr
       SYNTAX  InetAddress (SIZE(4))
       DESCRIPTION
           "An implementation is only required to support IPv4
       addresses."

   OBJECT diffServMultiFieldClfrDstAddr
       SYNTAX  InetAddress (SIZE(4))
       DESCRIPTION
           "An implementation is only required to support IPv4
       addresses."

   OBJECT diffServAlgDropStatus  -- same as RFC3289
       SYNTAX RowStatus { active(1) }
       WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
       DESCRIPTION
           "Support for createAndWait and notInService is not required."

   OBJECT diffServDataPathStorage
       SYNTAX StorageType { nonVolatile(3) }
       DESCRIPTION
           "An implementation is only required to support nonvolatile
       storage."

   OBJECT diffServClfrStorage
       SYNTAX StorageType { nonVolatile(3) }
       DESCRIPTION
           "An implementation is only required to support nonvolatile
       storage."






   OBJECT diffServClfrElementStorage
       SYNTAX StorageType { nonVolatile(3) }
       DESCRIPTION
           "An implementation is only required to support nonvolatile
       storage."

   OBJECT diffServMultiFieldClfrStorage
       SYNTAX StorageType { nonVolatile(3) }
       DESCRIPTION
           "An implementation is only required to support nonvolatile
       storage."

   OBJECT diffServActionStorage
       SYNTAX StorageType { nonVolatile(3) }
       DESCRIPTION
           "An implementation is only required to support nonvolatile
       storage."

   OBJECT diffServCountActStorage
       SYNTAX StorageType { nonVolatile(3) }
       DESCRIPTION
           "An implementation is only required to support nonvolatile
       storage."

   OBJECT diffServAlgDropStorage
       SYNTAX StorageType { nonVolatile(3) }
       DESCRIPTION
           "An implementation is only required to support nonvolatile
       storage."

   OBJECT diffServAlgDropType
       SYNTAX  INTEGER { alwaysDrop(5) }
       DESCRIPTION
           "For DOCSIS subscriber management, this object is
       only used to provide packet filtering.  Implementations
       need not support other values of this enumeration."

   MODULE -- This module i.e., DOCS-IETF-SUBMGT-MIB

   MANDATORY-GROUPS {
           docsSubMgtGroup
           }

   OBJECT docsSubMgtCpeControlMaxCpeIp
       SYNTAX Integer32(0..16)
       DESCRIPTION
           "An implementation is only required to support up to
       sixteen addresses per modem."





   OBJECT docsSubMgtCpeMaxIpDefault
       SYNTAX Integer32(0..16)
       DESCRIPTION
           "An implementation is only required to support up to
       sixteen addresses per modem."

   OBJECT docsSubMgtCpeIpAddressType
       SYNTAX InetAddressType { ipv4(1) }
       DESCRIPTION
           "An implementation is only required to support IPv4
       addresses."

   OBJECT docsSubMgtCpeIpAddr
       SYNTAX  InetAddress (SIZE(4))
       DESCRIPTION
           "An implementation is only required to support IPv4
       addresses."

   OBJECT docsSubMgtCmFilterSubDownstream
       SYNTAX  Integer32(0..30)
       DESCRIPTION
           "An implementation is only required to support thirty
       filter groups."

   OBJECT docsSubMgtCmFilterSubUpstream
       SYNTAX  Integer32(0..30)
       DESCRIPTION
           "An implementation is only required to support thirty
       filter groups."

   OBJECT docsSubMgtCmFilterCmDownstream
       SYNTAX  Integer32(0..30)
       DESCRIPTION
           "An implementation is only required to support thirty
       filter groups."

   OBJECT docsSubMgtCmFilterCmUpstream
       SYNTAX  Integer32(0..30)
       DESCRIPTION
           "An implementation is only required to support thirty
       filter groups."

           ::= { docsSubMgtCompliances 1 }

   docsSubMgtGroup OBJECT-GROUP
           OBJECTS {
               docsSubMgtCpeControlMaxCpeIp,
               docsSubMgtCpeControlActive,





               docsSubMgtCpeControlLearnable,
               docsSubMgtCpeControlReset,
               docsSubMgtCpeControlLastReset,
               docsSubMgtCpeMaxIpDefault,
               docsSubMgtCpeActiveDefault,
               docsSubMgtCpeLearnableDefault,
               docsSubMgtCpeIpAddressType,
               docsSubMgtCpeIpAddr,
               docsSubMgtCpeIpLearned,
               docsSubMgtCmFilterSubDownstream,
               docsSubMgtCmFilterSubUpstream,
               docsSubMgtCmFilterCmDownstream,
               docsSubMgtCmFilterCmUpstream,
               docsSubMgtFilterGroupIndex
               }
               STATUS      current
               DESCRIPTION
                   "The objects used to manage host-based cable modems
               via a set of CMTS enforced controls."
               ::= {  docsSubMgtGroups 1 }

   END


