T11-FC-SP-AUTHENTICATION-MIB  DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, OBJECT-IDENTITY,
    NOTIFICATION-TYPE,
    mib-2, Counter32, Unsigned32
                                      FROM SNMPv2-SMI  -- [RFC2578]
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP
                                      FROM SNMPv2-CONF -- [RFC2580]
    StorageType, AutonomousType,
    TruthValue, TimeStamp             FROM SNMPv2-TC   -- [RFC2579]
    InterfaceIndex                    FROM IF-MIB      -- [RFC2863]
    fcmInstanceIndex,
    FcNameIdOrZero                    FROM FC-MGMT-MIB -- [RFC4044]
    t11FamLocalSwitchWwn
                       FROM T11-FC-FABRIC-ADDR-MGR-MIB -- [RFC4439]
    T11FabricIndex                    FROM T11-TC-MIB  -- [RFC4439]
    T11FcSpDhGroups,
    T11FcSpHashFunctions,
    T11FcSpSignFunctions,
    T11FcSpLifetimeLeft,
    T11FcSpLifetimeLeftUnits,
    T11FcSpAuthRejectReasonCode,
    T11FcSpAuthRejReasonCodeExp       FROM T11-FC-SP-TC-MIB;

t11FcSpAuthenticationMIB  MODULE-IDENTITY
    LAST-UPDATED  "200808200000Z"
    ORGANIZATION  "This MIB module was developed through the





                  coordinated effort of two organizations:
                  T11 began the development and the IETF (in
                  the IMSS Working Group) finished it."
    CONTACT-INFO
            "     Claudio DeSanti
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA 95134 USA
                  EMail: cds@cisco.com

                  Keith McCloghrie
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA 95134 USA
                  Email: kzm@cisco.com"
    DESCRIPTION
           "This MIB module specifies the management information
           required to manage the Authentication Protocols defined by
           Fibre Channel's FC-SP specification.

           This MIB module defines three tables:

            - t11FcSpAuEntityTable is a table of Fibre Channel
              entities that can be authenticated using FC-SP's
              Authentication Protocols.

            - t11FcSpAuIfStatTable is a table with one row for each
              mapping of an Authentication entity onto an interface,
              containing statistics information.

            - t11FcSpAuRejectTable is a table of volatile information
              about FC-SP Authentication Protocol transactions
              that were most recently rejected.

           Copyright (C) The IETF Trust (2008).  This version
           of this MIB module is part of RFC 5324;  see the RFC
           itself for full legal notices."
    REVISION  "200808200000Z"
    DESCRIPTION
           "Initial version of this MIB module, published as RFC 5324."
    ::= { mib-2 176 }

t11FcSpAuMIBNotifications
                   OBJECT IDENTIFIER ::= { t11FcSpAuthenticationMIB 0 }
t11FcSpAuMIBObjects
                   OBJECT IDENTIFIER ::= { t11FcSpAuthenticationMIB 1 }
t11FcSpAuMIBConformance
                   OBJECT IDENTIFIER ::= { t11FcSpAuthenticationMIB 2 }





t11FcSpAuMIBIdentities
                   OBJECT IDENTIFIER ::= { t11FcSpAuthenticationMIB 3 }

--
-- OIDs defined for use as values of t11FcSpAuServerProtocol
--

t11FcSpAuServerProtocolRadius OBJECT-IDENTITY
    STATUS       current
    DESCRIPTION
           "This OID identifies RADIUS as the protocol used
           to communicate with an External Server as part of
           the process by which identities are verified.
           In this case, information about the RADIUS Servers
           is likely to be provided in radiusAuthServerExtTable
           defined in the RADIUS-AUTH-CLIENT-MIB."
    REFERENCE
           "radiusAuthServerExtTable in 'RADIUS Authentication
            Client MIB', RFC 4668, August 2006."
    ::= { t11FcSpAuMIBIdentities 1 }

t11FcSpAuServerProtocolDiameter OBJECT-IDENTITY
    STATUS       current
    DESCRIPTION
           "This OID identifies Diameter as the protocol used
           to communicate with an External Server as part of
           the process by which identities are verified."
    REFERENCE
           "RFC 3588, September 2003."
    ::= { t11FcSpAuMIBIdentities 2 }

t11FcSpAuServerProtocolTacacs OBJECT-IDENTITY
    STATUS       current
    DESCRIPTION
           "This OID identifies TACACS as the protocol used
           to communicate with an External Server as part of
           the process by which identities are verified."
    REFERENCE
           "RFC 1492, July 1993."
    ::= { t11FcSpAuMIBIdentities 3 }

--
-- Configuration for the Authentication Protocols
--

t11FcSpAuEntityTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FcSpAuEntityEntry
    MAX-ACCESS   not-accessible





    STATUS       current
    DESCRIPTION
           "A table of Fibre Channel entities that can be authenticated
           using FC-SP's Authentication Protocols.

           The purpose of an FC-SP Authentication Protocol is to verify
           that a claimed name is associated with the claiming entity.
           The Authentication Protocols can be used to authenticate
           Nx_Ports, B_Ports, or Switches."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 3.2.25."
    ::= { t11FcSpAuMIBObjects 1 }

t11FcSpAuEntityEntry OBJECT-TYPE
    SYNTAX       T11FcSpAuEntityEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "Information about the configuration and capabilities of an
           FC-SP entity (which is managed within the Fibre Channel
           management instance identified by fcmInstanceIndex) on a
           particular Fabric with respect to FC-SP's Authentication
           Protocols."
    INDEX   { fcmInstanceIndex, t11FcSpAuEntityName,
              t11FcSpAuFabricIndex }
    ::= { t11FcSpAuEntityTable 1 }

T11FcSpAuEntityEntry ::= SEQUENCE {
    t11FcSpAuEntityName             FcNameIdOrZero,
    t11FcSpAuFabricIndex            T11FabricIndex,
    t11FcSpAuServerProtocol         AutonomousType,
                                                   -- Config parameters
    t11FcSpAuStorageType            StorageType,
    t11FcSpAuSendRejNotifyEnable    TruthValue,
    t11FcSpAuRcvRejNotifyEnable     TruthValue,
    t11FcSpAuDefaultLifetime        T11FcSpLifetimeLeft,
    t11FcSpAuDefaultLifetimeUnits   T11FcSpLifetimeLeftUnits,
    t11FcSpAuRejectMaxRows          Unsigned32,
                                                   -- Capabilities
    t11FcSpAuDhChapHashFunctions    T11FcSpHashFunctions,
    t11FcSpAuDhChapDhGroups         T11FcSpDhGroups,
    t11FcSpAuFcapHashFunctions      T11FcSpHashFunctions,
    t11FcSpAuFcapCertsSignFunctions T11FcSpSignFunctions,
    t11FcSpAuFcapDhGroups           T11FcSpDhGroups,
    t11FcSpAuFcpapHashFunctions     T11FcSpHashFunctions,
    t11FcSpAuFcpapDhGroups          T11FcSpDhGroups





}

t11FcSpAuEntityName OBJECT-TYPE
    SYNTAX     FcNameIdOrZero (SIZE (8))
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
           "The name used to identify the FC-SP entity.

           For entities that are Fibre Channel Switches, this value
           corresponds to the Switch's value of fcmSwitchWWN.  For
           entities other than Fibre Channel Switches, this value
           corresponds to the value of fcmInstanceWwn for the
           corresponding Fibre Channel management instance."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.3.3.
            - fcmInstanceWwn & fcmSwitchWWN,
              'Fibre Channel Management MIB', RFC 4044, May 2005."
    ::= { t11FcSpAuEntityEntry 1 }

t11FcSpAuFabricIndex OBJECT-TYPE
    SYNTAX       T11FabricIndex
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "An index value that uniquely identifies a
           particular Fabric to which the entity is attached."
    ::= { t11FcSpAuEntityEntry 2 }

t11FcSpAuServerProtocol OBJECT-TYPE
    SYNTAX       AutonomousType
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The protocol, if any, used by the entity to communicate
           with a third party (i.e., an External Server) as part of
           the process by which it verifies DH-CHAP responses.  For
           example, if the entity is using an external RADIUS server
           to verify DH-CHAP responses, then this object will have
           the value t11FcSpAuServerProtocolRadius.

           The value, zeroDotZero, is used to indicate that no
           protocol is being used to communicate with a third
           party to verify DH-CHAP responses.

           When no protocol is being used, or if the third party is





           unreachable via the specified protocol, then locally
           configured information (if any) may be used instead."
    ::= { t11FcSpAuEntityEntry 3 }

t11FcSpAuStorageType OBJECT-TYPE
    SYNTAX       StorageType
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "This object specifies the memory realization of
           configuration information related to an FC-SP
           Entity on a particular Fabric: specifically, for
           MIB objects in the row containing this object.

           Even if an instance of this object has the value
           'permanent(4)', none of the information in the
           corresponding row of this table needs to be writable."
    ::= { t11FcSpAuEntityEntry 4 }

t11FcSpAuSendRejNotifyEnable OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
           "An indication of whether or not the entity should issue
           t11FcSpAuRejectSentNotify notifications when sending
           AUTH_Reject/SW_RJT/LS_RJT to reject an AUTH message.

           If the value of the object is 'true', then this type of
           notification is generated.  If the value is 'false',
           this type of notification is not generated."
    DEFVAL { false }
    ::= { t11FcSpAuEntityEntry 5 }

t11FcSpAuRcvRejNotifyEnable OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
           "An indication of whether or not the entity should issue
           t11FcSpAuRejectReceivedNotify notifications on the receipt
           of AUTH_Reject/SW_RJT/LS_RJT messages.

           If the value of the object is 'true', then this type of
           notification is generated.  If the value is 'false',
           this type of notification is not generated."
    DEFVAL { false }
    ::= { t11FcSpAuEntityEntry 6 }





t11FcSpAuDefaultLifetime OBJECT-TYPE
    SYNTAX       T11FcSpLifetimeLeft
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "When the value of this object is non-zero, it specifies the
           default value of a lifetime, specified in units given by
           the corresponding instance of t11FcSpAuDefaultLifetimeUnits.
           This default lifetime is to be used for any Security
           Association that has no explicitly specified value for its
           lifetime.

           An SA's lifetime is either the time interval or the number
           of passed bytes, after which the SA has to be terminated and
           (if necessary) replaced with a new SA.

           If this object is zero, then there is no default value for
           lifetime."
    DEFVAL       { 28800 }         -- 8 hours (in units of seconds)
     ::= { t11FcSpAuEntityEntry 7 }

t11FcSpAuDefaultLifetimeUnits OBJECT-TYPE
    SYNTAX       T11FcSpLifetimeLeftUnits
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "The units in which the value of the corresponding
           instance of t11FcSpAuDefaultLifetime specifies a
           default lifetime for a Security Association that has
           no explicitly-specified value for its lifetime."
    DEFVAL       { seconds }
    ::= { t11FcSpAuEntityEntry 8 }

t11FcSpAuRejectMaxRows OBJECT-TYPE
    SYNTAX       Unsigned32 (0..1000)
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "The maximum number of rows in the t11FcSpAuRejectTable for
           this entity on this Fabric.  If and when an AUTH message is
           rejected, and the t11FcSpAuRejectTable already contains this
           maximum number of rows for the specific entity and Fabric,
           the row containing the oldest information is discarded and
           replaced by a row containing information about the new
           rejection.

           There will be less than this maximum number of rows in
           the t11FcSpAuRejectTable in exceptional circumstances,





           e.g., after an agent restart.

           In an implementation that does not support the
           t11FcSpAuRejectTable, this object will always be zero."
    ::= { t11FcSpAuEntityEntry 9 }

t11FcSpAuDhChapHashFunctions OBJECT-TYPE
    SYNTAX     T11FcSpHashFunctions
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The hash functions that the entity supports when using
           the DH-CHAP algorithm."
    ::= { t11FcSpAuEntityEntry 10 }

t11FcSpAuDhChapDhGroups OBJECT-TYPE
    SYNTAX     T11FcSpDhGroups
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The DH Groups that the entity supports when using the
           DH-CHAP algorithm in FC-SP."
    ::= { t11FcSpAuEntityEntry 11 }

t11FcSpAuFcapHashFunctions OBJECT-TYPE
    SYNTAX     T11FcSpHashFunctions
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The hash functions that the entity supports when
           specified as Protocol Parameters in the AUTH_Negotiate
           message for FCAP in FC-SP."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.5.2.1 and table 28."
    ::= { t11FcSpAuEntityEntry 12 }

t11FcSpAuFcapCertsSignFunctions OBJECT-TYPE
    SYNTAX     T11FcSpSignFunctions
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The signature functions used within certificates that
           the entity supports when using FCAP in FC-SP."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),





              February 2007, section 5.5.4.2 and tables 38 & 39."
    ::= { t11FcSpAuEntityEntry 13 }

t11FcSpAuFcapDhGroups OBJECT-TYPE
    SYNTAX     T11FcSpDhGroups
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The DH Groups that the entity supports when using the
           FCAP algorithm in FC-SP."
    ::= { t11FcSpAuEntityEntry 14 }

t11FcSpAuFcpapHashFunctions OBJECT-TYPE
    SYNTAX     T11FcSpHashFunctions
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The hash functions that the entity supports when using
           the FCPAP algorithm in FC-SP."
    ::= { t11FcSpAuEntityEntry 15 }

t11FcSpAuFcpapDhGroups OBJECT-TYPE
    SYNTAX     T11FcSpDhGroups
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The DH Groups that the entity supports when using the
           FCPAP algorithm in FC-SP."
    ::= { t11FcSpAuEntityEntry 16 }

--
-- The Mapping of Authentication Entities onto Interfaces
-- and Statistics
--

t11FcSpAuIfStatTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FcSpAuIfStatEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "Each FC-SP Authentication entity can operate on one or more
           interfaces, but at most one of them can operate on each
           interface.  A row in this table exists for each interface
           to each Fabric on which each Authentication entity operates.

           The objects within this table contain statistics information
           related to FC-SP's Authentication Protocols."
    ::= { t11FcSpAuMIBObjects 2 }





t11FcSpAuIfStatEntry OBJECT-TYPE
    SYNTAX       T11FcSpAuIfStatEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "A set of Authentication Protocols statistics for an FC-SP
           Authentication entity (identified by t11FcSpAuEntityName) on
           one of its interfaces to a particular Fabric, which is
           managed within the Fibre Channel management instance
           identified by fcmInstanceIndex."
    INDEX   { fcmInstanceIndex, t11FcSpAuEntityName,
              t11FcSpAuIfStatInterfaceIndex,
              t11FcSpAuIfStatFabricIndex }
    ::= { t11FcSpAuIfStatTable 1 }

T11FcSpAuIfStatEntry ::= SEQUENCE {
    t11FcSpAuIfStatInterfaceIndex        InterfaceIndex,
    t11FcSpAuIfStatFabricIndex           T11FabricIndex,
    t11FcSpAuIfStatTimeouts              Counter32,
    t11FcSpAuIfStatInAcceptedMsgs        Counter32,
    t11FcSpAuIfStatInLsSwRejectedMsgs    Counter32,
    t11FcSpAuIfStatInAuthRejectedMsgs    Counter32,
    t11FcSpAuIfStatOutAcceptedMsgs       Counter32,
    t11FcSpAuIfStatOutLsSwRejectedMsgs   Counter32,
    t11FcSpAuIfStatOutAuthRejectedMsgs   Counter32
}

t11FcSpAuIfStatInterfaceIndex OBJECT-TYPE
    SYNTAX       InterfaceIndex
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "The interface on which the FC-SP Authentication entity
           operates and for which the statistics are collected."
    ::= { t11FcSpAuIfStatEntry 1 }

t11FcSpAuIfStatFabricIndex OBJECT-TYPE
    SYNTAX       T11FabricIndex
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "An index value identifying the particular Fabric for
           which the statistics are collected."
    ::= { t11FcSpAuIfStatEntry 2 }

t11FcSpAuIfStatTimeouts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only





    STATUS       current
    DESCRIPTION
           "The number of FC-SP Authentication Protocol messages sent
           by the particular entity on the particular Fabric on the
           particular interface, for which no response was received
           within a timeout period.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.11."
    ::= { t11FcSpAuIfStatEntry 3 }

t11FcSpAuIfStatInAcceptedMsgs OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of FC-SP Authentication Protocol messages
           received and accepted by the particular entity on the
           particular Fabric on the particular interface.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.1."
    ::= { t11FcSpAuIfStatEntry 4 }

t11FcSpAuIfStatInLsSwRejectedMsgs OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of FC-SP Authentication Protocol messages
           received by the particular entity on the particular Fabric
           on the particular interface, and rejected by a lower-level
           (SW_RJT or LS_RJT) reject.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.1."





    ::= { t11FcSpAuIfStatEntry 5 }

t11FcSpAuIfStatInAuthRejectedMsgs OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of FC-SP Authentication Protocol messages
           received by the particular entity on the particular Fabric
           on the particular interface, and rejected by an AUTH_Reject
           message.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.1."
    ::= { t11FcSpAuIfStatEntry 6 }

t11FcSpAuIfStatOutAcceptedMsgs OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of FC-SP Authentication Protocol messages sent
           by the particular entity on the particular Fabric on the
           particular interface, which were accepted by the
           neighboring entity, i.e., not rejected by an AUTH_Reject
           message, nor by a lower-level (SW_RJT or LS_RJT) reject.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.1."
    ::= { t11FcSpAuIfStatEntry 7 }

t11FcSpAuIfStatOutLsSwRejectedMsgs OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of FC-SP Authentication Protocol messages sent
           by the particular entity on the particular Fabric on the
           particular interface, which were rejected by a lower-level
           (SW_RJT or LS_RJT) reject.





           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.1."
    ::= { t11FcSpAuIfStatEntry 8 }

t11FcSpAuIfStatOutAuthRejectedMsgs OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of FC-SP Authentication Protocol messages sent
           by the particular entity on the particular Fabric on the
           particular interface, which were rejected by an
           AUTH_Reject message.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, section 5.1."
    ::= { t11FcSpAuIfStatEntry 9 }

--
-- Information about Authentication Protocol Transactions
-- which were recently rejected
--

t11FcSpAuRejectTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FcSpAuRejectEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "A table of volatile information about FC-SP Authentication
           Protocol transactions that were recently rejected with
           an AUTH_Reject message, or with an SW_RJT/LS_RJT.

           The maximum number of rows in this table for a specific
           entity on a specific Fabric is given by the value of the
           corresponding instance of t11FcSpAuRejectMaxRows.

           The syntax of t11FcSpAuRejTimestamp is TimeStamp, and thus
           its value rolls over to zero after approximately 497 days.
           To avoid any confusion due to such a rollover, rows should
           be deleted from this table before they are 497 days old.





           This table will be empty if no AUTH_Reject messages,
           nor any SW_RJT/LS_RJT's rejecting an AUTH message,
           have been sent or received since the last
           re-initialization of the agent."
    ::= { t11FcSpAuMIBObjects 3 }

t11FcSpAuRejectEntry OBJECT-TYPE
    SYNTAX       T11FcSpAuRejectEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "Information about one AUTH message (either an
           AUTH_ELS or an AUTH_ILS) that was rejected with an
           AUTH_Reject, SW_RJT or LS_RJT message, sent/received by
           the entity identified by values of fcmInstanceIndex and
           t11FcSpAuEntityName, on an interface to a particular
           Fabric."
    INDEX   { fcmInstanceIndex, t11FcSpAuEntityName,
              t11FcSpAuRejInterfaceIndex, t11FcSpAuRejFabricIndex,
              t11FcSpAuRejTimestamp }
    ::= { t11FcSpAuRejectTable 1 }

T11FcSpAuRejectEntry ::= SEQUENCE {
    t11FcSpAuRejInterfaceIndex        InterfaceIndex,
    t11FcSpAuRejFabricIndex           T11FabricIndex,
    t11FcSpAuRejTimestamp             TimeStamp,
    t11FcSpAuRejDirection             INTEGER,
    t11FcSpAuRejType                  INTEGER,
    t11FcSpAuRejAuthMsgString         OCTET STRING,
    t11FcSpAuRejReasonCode            T11FcSpAuthRejectReasonCode,
    t11FcSpAuRejReasonCodeExp         T11FcSpAuthRejReasonCodeExp
}

t11FcSpAuRejInterfaceIndex OBJECT-TYPE
    SYNTAX       InterfaceIndex
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "The interface on which the rejected AUTH message was
           sent or received."
    ::= { t11FcSpAuRejectEntry 1 }

t11FcSpAuRejFabricIndex OBJECT-TYPE
    SYNTAX       T11FabricIndex
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "An index value identifying the particular Fabric on





           which the rejected AUTH message was sent or received."
    ::= { t11FcSpAuRejectEntry 2 }

t11FcSpAuRejTimestamp OBJECT-TYPE
    SYNTAX       TimeStamp
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "The time at which the AUTH message was rejected.  If two
           rows have the same value of this object for the same
           entity on the same interface and Fabric, the value of
           this object for the later one is incremented by one."
    ::= { t11FcSpAuRejectEntry 3 }

t11FcSpAuRejDirection OBJECT-TYPE
    SYNTAX       INTEGER { sent(1), received(2) }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "An indication of whether the rejection was sent or
           received by the identified entity.

           The value 'sent(1)' corresponds to a notification of
           type t11FcSpAuRejectSentNotify; the value 'received(2)'
           corresponds to t11FcSpAuRejectReceivedNotify."
    ::= { t11FcSpAuRejectEntry 4 }

t11FcSpAuRejType OBJECT-TYPE
    SYNTAX       INTEGER {
                     authReject(1),
                     swRjt(2),
                     lsRjt(3)
                 }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "An indication of whether the rejection was an
           AUTH_Reject, an SW_RJT or an LS_RJT."
    ::= { t11FcSpAuRejectEntry 5 }

t11FcSpAuRejAuthMsgString OBJECT-TYPE
    SYNTAX       OCTET STRING (SIZE(0..255))
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The binary content of the AUTH message that was
           rejected, formatted as an octet string (in network
           byte order) containing the content of the message.





           If the binary content is unavailable, then the
           length is zero.  Otherwise, the first octet of the
           message identifies the type of message:

              '90'h - an AUTH_ELS, see Table 6 in FC-SP,
              '40'h - an AUTH_ILS, see Table 3 in FC-SP, or
              '41'h - an B_AUTH_ILS, see Table 5 in FC-SP.

           and the remainder of the message may be truncated."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, Tables 3, 5 and 6."
    ::= { t11FcSpAuRejectEntry 6 }

t11FcSpAuRejReasonCode OBJECT-TYPE
    SYNTAX       T11FcSpAuthRejectReasonCode
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The reason code with which this AUTH message was
           rejected."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, Table 17, 48, 52."
    ::= { t11FcSpAuRejectEntry 7 }

t11FcSpAuRejReasonCodeExp OBJECT-TYPE
    SYNTAX       T11FcSpAuthRejReasonCodeExp
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The reason code explanation with which this AUTH
           message was rejected."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, Table 17, 48, 52."
    ::= { t11FcSpAuRejectEntry 8 }

--
-- Notifications
--

t11FcSpAuRejectSentNotify NOTIFICATION-TYPE
    OBJECTS   { t11FamLocalSwitchWwn,
                t11FcSpAuRejAuthMsgString,





                t11FcSpAuRejType,
                t11FcSpAuRejReasonCode,
                t11FcSpAuRejReasonCodeExp }
    STATUS       current
    DESCRIPTION
           "This notification indicates that a Switch (identified
           by the value of t11FamLocalSwitchWwn) has sent a reject
           message of the type indicated by t11FcSpAuRejType in
           response to an AUTH message.

           The content of the rejected AUTH message is given by the
           value of t11FcSpAuRejAuthMsgString.  The values of the
           Reason Code and Reason Code Explanation in the
           AUTH_Reject/SW_RJT/LS_RJT are indicated by the values of
           t11FcSpAuRejReasonCode and t11FcSpAuRejReasonCodeExp."
    ::= { t11FcSpAuMIBNotifications 1 }

t11FcSpAuRejectReceivedNotify NOTIFICATION-TYPE
    OBJECTS   { t11FamLocalSwitchWwn,
                t11FcSpAuRejAuthMsgString,
                t11FcSpAuRejType,
                t11FcSpAuRejReasonCode,
                t11FcSpAuRejReasonCodeExp }
    STATUS       current
    DESCRIPTION
           "This notification indicates that a Switch (identified
           by the value of t11FamLocalSwitchWwn) has received a
           reject message of the type indicated by t11FcSpAuRejType
           in response to an AUTH message.

           The content of the rejected AUTH message is given by the
           value of t11FcSpAuRejAuthMsgString.  The values of the
           Reason Code and Reason Code Explanation in the
           AUTH_Reject/SW_RJT/LS_RJT are indicated by the values of
           t11FcSpAuRejReasonCode and t11FcSpAuRejReasonCodeExp."
    ::= { t11FcSpAuMIBNotifications 2 }

--
-- Conformance
--

t11FcSpAuMIBCompliances
                  OBJECT IDENTIFIER ::= { t11FcSpAuMIBConformance 1 }
t11FcSpAuMIBGroups
                  OBJECT IDENTIFIER ::= { t11FcSpAuMIBConformance 2 }

t11FcSpAuMIBCompliance MODULE-COMPLIANCE
    STATUS       current





    DESCRIPTION
           "The compliance statement for entities that
           implement one or more of the Authentication Protocols
           defined in FC-SP."

    MODULE  -- this module
        MANDATORY-GROUPS { t11FcSpAuGeneralGroup,
                           t11FcSpAuRejectedGroup,
                           t11FcSpAuNotificationGroup }

        GROUP      t11FcSpAuIfStatsGroup
        DESCRIPTION
               "These counters, of particular FC-SP messages and
               events, are mandatory only for those systems that
               count such messages/events."

-- Write access is not required for any objects in this MIB module:

        OBJECT     t11FcSpAuStorageType
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcSpAuSendRejNotifyEnable
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcSpAuRcvRejNotifyEnable
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcSpAuDefaultLifetime
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcSpAuDefaultLifetimeUnits
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FcSpAuRejectMaxRows
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."






        ::= { t11FcSpAuMIBCompliances 1 }

-- Units of Conformance

t11FcSpAuGeneralGroup OBJECT-GROUP
    OBJECTS  { t11FcSpAuServerProtocol,
               t11FcSpAuStorageType,
               t11FcSpAuSendRejNotifyEnable,
               t11FcSpAuRcvRejNotifyEnable,
               t11FcSpAuDefaultLifetime,
               t11FcSpAuDefaultLifetimeUnits,
               t11FcSpAuRejectMaxRows,
               t11FcSpAuDhChapHashFunctions,
               t11FcSpAuDhChapDhGroups,
               t11FcSpAuFcapHashFunctions,
               t11FcSpAuFcapCertsSignFunctions,
               t11FcSpAuFcapDhGroups,
               t11FcSpAuFcpapHashFunctions,
               t11FcSpAuFcpapDhGroups,
               t11FcSpAuIfStatTimeouts }
    STATUS   current
    DESCRIPTION
           "A collection of objects for the capabilities and
           configuration parameters of FC-SP's Authentication
           Protocols.  The inclusion of t11FcSpAuIfStatTimeouts
           in this group provides information on mappings of
           Authentication entities onto interfaces."
    ::= { t11FcSpAuMIBGroups 1 }

t11FcSpAuIfStatsGroup OBJECT-GROUP
    OBJECTS  { t11FcSpAuIfStatInAcceptedMsgs,
               t11FcSpAuIfStatInLsSwRejectedMsgs,
               t11FcSpAuIfStatInAuthRejectedMsgs,
               t11FcSpAuIfStatOutAcceptedMsgs,
               t11FcSpAuIfStatOutLsSwRejectedMsgs,
               t11FcSpAuIfStatOutAuthRejectedMsgs }
    STATUS   current
    DESCRIPTION
           "A collection of objects for monitoring the
           operations of FC-SP's Authentication Protocols."
    ::= { t11FcSpAuMIBGroups 2 }

t11FcSpAuRejectedGroup OBJECT-GROUP
    OBJECTS  { t11FcSpAuRejDirection,
               t11FcSpAuRejType,
               t11FcSpAuRejAuthMsgString,
               t11FcSpAuRejReasonCode,
               t11FcSpAuRejReasonCodeExp }





    STATUS   current
    DESCRIPTION
           "A collection of objects holding information concerning
           FC-SP Authentication Protocol transactions that were
           recently rejected with an AUTH_Reject, with an SW_RJT,
           or with an LS_RJT."
    ::= { t11FcSpAuMIBGroups 3 }

t11FcSpAuNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS  { t11FcSpAuRejectSentNotify,
                     t11FcSpAuRejectReceivedNotify }
    STATUS   current
    DESCRIPTION
           "A collection of notifications for use in the management
           of FC-SP's Authentication Protocols."
    ::= { t11FcSpAuMIBGroups 4 }

END


