CMOT DEFINITIONS ::= BEGIN


   IMPORTS OBJECT-TYPE FROM RFC1065-SMI;

   IMPORTS mib FROM RFC1066-MIB;

     cmot  OBJECT IDENTIFIER ::= { mib 9 }

     -- The following assignments are made for the purpose of
     -- identification within CMOT and do not refer to MIB objects.

     cmotVersion              OBJECT IDENTIFIER ::= { cmot 1 }

     cmotAcseInfo             OBJECT IDENTIFIER ::= { cmot 2 }
     cmotAcseAccessControl    OBJECT IDENTIFIER ::= { cmotAcseInfo 1 }

     -- The following definition is made for use in referencing a
     -- managed system (for the purpose of proxy management) in the
     -- CMIP Object Instance field. It does not represent a MIB
     -- object.

     cmotSystemID OBJECT-TYPE
             SYNTAX  CmotSystemID
             ACCESS  not-accessible
             STATUS  optional
             ::= { cmot 3 }

     CmotSystemID ::= CHOICE {
             arbitrary     [0] IMPLICIT OCTET STRING,
             proxyIndex    [1] IMPLICIT INTEGER,
             inetAddr      [2] IMPLICIT IpAddress,
             domainName    [3] IMPLICIT OCTET STRING,
             mac802Addr    [4] IMPLICIT OCTET STRING,
             x121Addr      [5] IMPLICIT OCTET STRING,
             nsap          [6] IMPLICIT OCTET STRING,
             netbiosName   [7] IMPLICIT OCTET STRING,
             snaName       [8] IMPLICIT OCTET STRING,
             adminId       [9] IMPLICIT OBJECT IDENTIFIER
     }

      -- All addresses should be conveyed in network-byte order.

   END







