IANA-IPPM-METRICS-REGISTRY-MIB DEFINITIONS ::= BEGIN


   IMPORTS





       OBJECT-IDENTITY, MODULE-IDENTITY, mib-2
           FROM SNMPv2-SMI;

   ianaIppmMetricsRegistry MODULE-IDENTITY
   LAST-UPDATED "200507280000Z"    -- July 28, 2005
   ORGANIZATION "IANA"
   CONTACT-INFO "Internet Assigned Numbers Authority

            Postal: ICANN
                4676 Admiralty Way, Suite 330
                Marina del Rey, CA 90292

            Tel:    +1 310 823 9358
            E-Mail: iana@iana.org"

   DESCRIPTION
      "This module defines a registry for IP Performance Metrics.

      Registrations are done sequentially by IANA in the ianaIppmMetrics
      subtree on the basis of 'Specification Required', as defined in
      [RFC2434].

      The reference of the specification must point to a stable document
      including a title, a revision, and a date.

      The name always starts with the name of the organization and must
      respect the SMIv2 rules for descriptors defined in section 3.1 of
      [RFC2578].

      A document that creates new metrics would have an IANA
      considerations section in which it would describe new metrics to
      be registered.

      An OBJECT IDENTITY assigned to a metric is definitive and cannot
      be reused.  If a new version of a metric is produced, then it is
      assigned with a new name and a new identifier.

      Copyright (C) The Internet Society (2005).  The initial version of
      this MIB module was published in RFC 4148; for full legal notices
      see the RFC itself or
      http://www.ietf.org/copyrights/ianamib.html."

   REVISION      "200507280000Z"    -- July 28, 2005
   DESCRIPTION
       "Initial version of the IPPM metrics registry module.
        This version published as RFC 4148."
   ::= { mib-2 128 }






   ianaIppmMetrics OBJECT-IDENTITY
       STATUS       current
       DESCRIPTION
           "Registration point for IP Performance Metrics."
       ::= { ianaIppmMetricsRegistry 1 }

   --
   -- Registry of the metrics of the IPPM WG RFCs
   --

   --
   -- RFC 2678 "IPPM Metrics for Measuring Connectivity"
   --

   ietfInstantUnidirConnectivity OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Instantaneous-Unidirectional-Connectivity"
       REFERENCE "RFC2678, section 2."
       ::= { ianaIppmMetrics 1}

   ietfInstantBidirConnectivity OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Instantaneous-Bidirectional-Connectivity"
       REFERENCE "RFC2678, section 3."
       ::= { ianaIppmMetrics 2}

   ietfIntervalUnidirConnectivity OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Interval-Unidirectional-Connectivity"
       REFERENCE "RFC2678, section 4."
       ::= { ianaIppmMetrics 3 }

   ietfIntervalBidirConnectivity OBJECT-IDENTITY
       STATUS current
       DESCRIPTION
           "Type-P-Interval-Bidirectional-Connectivity"
       REFERENCE "RFC2678, section 5."
       ::= { ianaIppmMetrics 4 }

   ietfIntervalTemporalConnectivity OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P1-P2-Interval-Temporal-Connectivity"
       REFERENCE "RFC2678, section 6."
       ::= { ianaIppmMetrics 5 }





   --
   -- RFC 2679 "A One-way Delay Metric for IPPM"
   --

   ietfOneWayDelay OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Delay"
       REFERENCE "RFC2679, section 3."
       ::= { ianaIppmMetrics 6 }

   ietfOneWayDelayPoissonStream OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Delay-Poisson-Stream"
       REFERENCE "RFC2679, section 4."
       ::= { ianaIppmMetrics 7 }

   ietfOneWayDelayPercentile OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Delay-Percentile"
       REFERENCE "RFC2679, section 5.1."
       ::= { ianaIppmMetrics 8 }

   ietfOneWayDelayMedian OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Delay-Median"
       REFERENCE "RFC2679, section 5.2."
       ::= { ianaIppmMetrics 9 }

   ietfOneWayDelayMinimum OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Delay-Minimum"
       REFERENCE "RFC2679, section 5.3."
       ::= { ianaIppmMetrics 10 }

   ietfOneWayDelayInversePercentile OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Delay-Inverse-Percentile"
       REFERENCE "RFC2679, section 5.4."
       ::= { ianaIppmMetrics 11 }








   --
   -- RFC 2680 "One-way Packet Loss Metric for IPPM"
   --

   ietfOneWayPktLoss OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Packet-Loss"
       REFERENCE "RFC2680, section 2."
       ::= { ianaIppmMetrics 12 }

   ietfOneWayPktLossPoissonStream OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Packet-Loss-Poisson-Stream"
       REFERENCE "RFC2680, section 3."
       ::= { ianaIppmMetrics 13 }

   ietfOneWayPktLossAverage OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Packet-Loss-Average"
       REFERENCE "RFC2680, section 4."
       ::= { ianaIppmMetrics 14 }

   --
   -- RFC 2681 "A Round-trip Delay Metric for IPPM"
   --

   ietfRoundTripDelay OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Round-trip-Delay"
       REFERENCE " section 2 of the rfc2681."
       ::= { ianaIppmMetrics 15 }

   ietfRoundTripDelayPoissonStream OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Round-trip-Delay-Poisson-Stream"
       REFERENCE "RFC2681, section 4."
       ::= { ianaIppmMetrics 16 }

   ietfRoundTripDelayPercentile OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Round-trip-Delay-Percentile"
       REFERENCE "RFC2681, section 4.1."





       ::= { ianaIppmMetrics 17 }

   ietfRoundTripDelayMedian OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Round-trip-Delay-Median"
       REFERENCE "RFC2681, section 4.2."
       ::= { ianaIppmMetrics 18 }

   ietfRoundTripDelayMinimum OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Round-trip-Delay-Minimum"
       REFERENCE "RFC2681, section 4.3."
       ::= { ianaIppmMetrics 19 }

   ietfRoundTripDelayInvPercentile OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-Round-trip-Inverse-Percentile"
       REFERENCE "RFC2681, section 4.4."
       ::= { ianaIppmMetrics 20 }

   --
   -- RFC 3357: "One-way Loss Pattern Sample Metrics"
   --

   ietfOneWayLossDistanceStream OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-Way-Loss-Distance-Stream"
       REFERENCE " RFC3357, section 5.4.1."
       ::={ ianaIppmMetrics 21}

   ietfOneWayLossPeriodStream OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-Way-Loss-Period-Stream"
       REFERENCE " RFC3357, section 5.4.2."
       ::={ ianaIppmMetrics 22}

   ietfOneWayLossNoticeableRate OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-Way-Loss-Noticeable-Rate"
       REFERENCE " RFC3357, section 6.1."
       ::= { ianaIppmMetrics 23 }






   ietfOneWayLossPeriodTotal OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-Way-Loss-Period-Total"
       REFERENCE " RFC3357, section 6.2."
       ::= { ianaIppmMetrics 24 }

   ietfOneWayLossPeriodLengths OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-Way-Loss-Period-Lengths"
       REFERENCE " RFC3357, section 6.3."
       ::= { ianaIppmMetrics 25 }

   ietfOneWayInterLossPeriodLengths OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-Way-Inter-Loss-Period-Lengths"
       REFERENCE " RFC3357, section 6.4."
       ::= { ianaIppmMetrics 26 }

   --
   -- RFC 3393: "IP Packet Delay Variation Metric
   --           for IP Performance Metrics (IPPM)"

   ietfOneWayIpdv OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-ipdv"
       REFERENCE " RFC3393, section 2."
       ::= { ianaIppmMetrics 27 }

   ietfOneWayIpdvPoissonStream OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-ipdv-Poisson-stream"
       REFERENCE " RFC3393, section 3."
       ::= { ianaIppmMetrics 28 }

   ietfOneWayIpdvPercentile OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
         "Type-P-One-way-ipdv-percentile"
       REFERENCE " RFC3393, section 4.3."
       ::= { ianaIppmMetrics 29 }

   ietfOneWayIpdvInversePercentile OBJECT-IDENTITY
       STATUS     current





       DESCRIPTION
           "Type-P-One-way-ipdv-inverse-percentile"
       REFERENCE " RFC3393, section 4.4."
       ::= { ianaIppmMetrics 30 }

   ietfOneWayIpdvJitter OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-ipdv-jitter"
       REFERENCE " RFC3393, section 4.5."
       ::= { ianaIppmMetrics 31 }

   ietfOneWayPeakToPeakIpdv OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-peak-to-peak-ipdv"
       REFERENCE " RFC3393, section 4.6."
       ::= { ianaIppmMetrics 32 }

   --
   -- RFC 3432: "Network performance measurement with periodic streams"
   --

   ietfOneWayDelayPeriodicStream OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
           "Type-P-One-way-Delay-Periodic-Stream"
       REFERENCE " RFC3432, section 4."
       ::= { ianaIppmMetrics 33 }

   END


