LISP-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    mib-2, Unsigned32, Counter64,
    Integer32, TimeTicks            FROM SNMPv2-SMI        -- RFC 2578
    TruthValue, TEXTUAL-CONVENTION,
    TimeStamp                       FROM SNMPv2-TC         -- RFC 2579
    MODULE-COMPLIANCE, OBJECT-GROUP FROM SNMPv2-CONF       -- RFC 2580
    MplsL3VpnName
                 FROM MPLS-L3VPN-STD-MIB                   -- RFC 4382
    AddressFamilyNumbers
                 FROM IANA-ADDRESS-FAMILY-NUMBERS-MIB;
       -- http://www.iana.org/assignments/ianaaddressfamilynumbers-mib

lispMIB MODULE-IDENTITY
    LAST-UPDATED "201310210000Z" -- 21 October 2013
    ORGANIZATION
            "IETF Locator/ID Separation Protocol (LISP) Working Group"
    CONTACT-INFO
            "Email: lisp@ietf.org
             WG charter:
             http://datatracker.ietf.org/wg/lisp/charter/"
    DESCRIPTION
            "This MIB module contains managed objects to support
             monitoring devices that support the Locator/ID Separation
             Protocol (LISP).

             Copyright (c) 2013 IETF Trust and the persons identified
             as authors of the code.  All rights reserved.

             Redistribution and use in source and binary forms, with
             or without modification, is permitted pursuant to, and
             subject to the license terms contained in, the Simplified
             BSD License set forth in Section 4.c of the IETF Trust's
             Legal Provisions Relating to IETF Documents
             (http://trustee.ietf.org/license-info)."
    REVISION     "201310210000Z" -- 21 October 2013
    DESCRIPTION  "Initial version of the IETF LISP-MIB module.
                  Published as RFC 7052."
     ::= { mib-2 220 }

--
-- Textual Conventions
--






LispAddressType ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "39a"
    STATUS current
    DESCRIPTION
      "LISP architecture can be applied to a wide variety of
       address-families.  This textual-convention is a generalization
       for representing addresses belonging to those address-families.
       For convenience, this document refers to any such address as a
       LISP address.  LispAddressType textual-convention consists of
       the following four-tuple:
       1. IANA Address Family Number: A field of length 2 octets,
          whose value is of the form following the assigned
          AddressFamilyNumbers textual-convention described in
          IANA-ADDRESS-FAMILY-NUMBERS-MIB DEFINITIONS, available from
          http://www.iana.org/assignments/ianaaddressfamilynumbers-mib.
          The enumerations are also listed in [IANA].  Note that this
          list of address family numbers is maintained by IANA.
       2. Length of LISP address: A field of length 1 octet, whose
          value indicates the octet-length of the next (third)
          field of this LispAddressType four-tuple.
       3. LISP address: A field of variable length as indicated in
          the previous (second) field, whose value is an address
          of the IANA Address Family indicated in the first field
          of this LispAddressType four-tuple.  Note that any of
          the IANA Address Families can be represented.
          Particularly when the address family is LISP Canonical
          Address Format (LCAF)
          with IANA-assigned Address Family Number 16387, then the
          first octet of this field indicates the LCAF type, and the
          rest of this field is same as the encoding format of the
          LISP Canonical Address after the length field, as defined
          in LCAF document.
       4. Mask-length of address: A field of length 1 octet, whose
          value is the mask-length to be applied to the LISP
          address specified in the previous (third) field.

       To illustrate the use of this object, consider the LISP MIB
       Object below titled lispMapCacheEntry.  This object begins
       with the following entities:

       lispMapCacheEntry ::= SEQUENCE {
          lispMapCacheEidLength          INTEGER,
          lispMapCacheEid                LispAddressType,
           ... [skip] ...









       Example 1: Suppose that the IPv4 EID-Prefix stored is
       192.0.2.0/24.  In this case, the values within
       lispMapCacheEntry would be:

          lispMapCacheEidLength  = 8
          lispMapCacheEid = 1, 4, 192.0.2.0, 24
          ... [skip] ...

       where 8 is the total length in octets of the next object
       (lispMapCacheEID of type LispAddressType).  Then, the value
       1 indicates the IPv4 AF (per the
       IANA-ADDRESS-FAMILY-NUMBERS-MIB), the value 4 indicates that
       the AF is 4 octets in length, 192.0.2.0 is the IPv4 address,
       and the value 24 is the mask-length in bits.  Note that the
       lispMapCacheEidLength value of 8 is used to compute the
       length of the fourth (last) field in lispMapCacheEid to be 1
       octet -- as computed by 8 - (2 + 1 + 4) = 1.

       Example 2: Suppose that the IPv6 EID-Prefix stored is
       2001:db8:a::/48.  In this case, the values within
       lispMapCacheEntry would be:

          lispMapCacheEidLength  = 20
          lispMapCacheEid = 2, 16, 2001:db8:a::, 48
          ... [skip] ...

       where 20 is the total length in octets of the next object
       (lispMapCacheEID of type LispAddressType).  Then, the value
       2 indicates the IPv6 AF (per the
       IANA-ADDRESS-FAMILY-NUMBERS-MIB), the value 16 indicates
       that the AF is 16 octets in length, 2001:db8:a:: is the IPv6
       address, and the value 48 is the mask-length in bits.  Note
       that the lispMapCacheEidLength value of 20 is used to
       compute the length of the fourth (last) field in
       lispMapCacheEid to be 1 octet -- as computed by
       20 - (2 + 1 + 16) = 1.

       Example 3: As an example where LCAF is used, suppose
       that the IPv4 EID-Prefix stored is 192.0.2.0/24 and it
       is part of LISP Instance ID 101.  In this case, the values
       within lispMapCacheEntry would be:

          lispMapCacheEidLength  = 11
          lispMapCacheEid = 16387, 7, 2, 101, 1, 192.0.2.0, 24
          ... [skip] ...








       where 11 is the total length in octets of the next object
       (lispMapCacheEID of type LispAddressType).  Then, the value
       16387 indicates the LCAF AF (see the
       IANA-ADDRESS-FAMILY-NUMBERS-MIB), the value 7 indicates that
       the LCAF AF is 7 octets in length in this case, 2 indicates
       that LCAF Type 2 encoding is used (see the LCAF document), 101
       gives the Instance ID, 1 gives the AFI (per the
       IANA-ADDRESS-FAMILY-NUMBERS-MIB) for an IPv4 address, 192.0.2.0
       is the IPv4 address, and 24 is the mask-length in bits.  Note
       that the lispMapCacheEidLength value of 11 octets is used to
       compute the length of the last field in lispMapCacheEid to be 1
       octet -- as computed by 11 - (2 + 1 + 1 + 1 + 1 + 4) = 1.

       Note: all LISP header formats and locations of specific
       flags, bits, and fields are as given in the base LISP
       references of RFC 6830, RFC 6832, and RFC 6833."

    REFERENCE
        "RFC 6830, Section 14.2 and
         LISP Canonical Address Format (LCAF), Work in Progress,
         March 2013."
    SYNTAX OCTET STRING (SIZE (5..39))

--
-- Top-level components of this MIB.
--
lispObjects       OBJECT IDENTIFIER ::= { lispMIB 1 }
lispConformance   OBJECT IDENTIFIER ::= { lispMIB 2 }

   lispFeaturesTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispFeaturesEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table represents the ON/OFF status of the
           various LISP features that can be enabled on LISP devices."
       REFERENCE
           "RFC 6830, Section 4, Section 5.5., Section 6.3."
       ::= { lispObjects 1 }














   lispFeaturesEntry OBJECT-TYPE
       SYNTAX     LispFeaturesEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the lispFeaturesTable."
       INDEX      { lispFeaturesInstanceID,
                    lispFeaturesAddressFamily }
       ::= { lispFeaturesTable 1 }

   LispFeaturesEntry ::= SEQUENCE {
       lispFeaturesInstanceID                     Unsigned32,
       lispFeaturesAddressFamily                  AddressFamilyNumbers,
       lispFeaturesItrEnabled                     TruthValue,
       lispFeaturesEtrEnabled                     TruthValue,
       lispFeaturesProxyItrEnabled                TruthValue,
       lispFeaturesProxyEtrEnabled                TruthValue,
       lispFeaturesMapServerEnabled               TruthValue,
       lispFeaturesMapResolverEnabled             TruthValue,
       lispFeaturesMapCacheSize                   Unsigned32,
       lispFeaturesMapCacheLimit                  Unsigned32,
       lispFeaturesEtrMapCacheTtl                 Unsigned32,
       lispFeaturesRlocProbeEnabled               TruthValue,
       lispFeaturesEtrAcceptMapDataEnabled        TruthValue,
       lispFeaturesEtrAcceptMapDataVerifyEnabled  TruthValue,
       lispFeaturesRouterTimeStamp                TimeStamp
   }

   lispFeaturesInstanceID OBJECT-TYPE
       SYNTAX     Unsigned32 (0..16777215)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This represents the Instance ID of the LISP header.
           An Instance ID in the LISP address encoding helps
           uniquely identify the AFI-based address space to which
           a given EID belongs.  Its default value is 0."
        DEFVAL { 0 }
        ::= { lispFeaturesEntry 1 }

   lispFeaturesAddressFamily OBJECT-TYPE
       SYNTAX     AddressFamilyNumbers
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "The IANA Address Family Number of destination address
           of packets that this LISP device is enabled to process."
        ::= { lispFeaturesEntry 2 }





   lispFeaturesItrEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of ITR role on this device.  If
           this object is true, then the ITR feature is enabled."
       ::= { lispFeaturesEntry 3 }

   lispFeaturesEtrEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of ETR role on this device.  If
           this object is true, then the ETR feature is enabled."
       ::= { lispFeaturesEntry 4 }

   lispFeaturesProxyItrEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of Proxy-ITR role on this device.
           If this object is true, then the Proxy-ITR feature is
           enabled."
       ::= { lispFeaturesEntry 5 }

   lispFeaturesProxyEtrEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of Proxy-ETR role on this device.
           If this object is true, then the Proxy-ETR feature is
           enabled."
       ::= { lispFeaturesEntry 6 }

   lispFeaturesMapServerEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of Map Server role on this device.
           If this object is true, then the Map-Server feature is
           enabled."
       ::= { lispFeaturesEntry 7 }






   lispFeaturesMapResolverEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of Map Resolver role on this device.
           If this object is true, then Map-Resolver feature is
           enabled."
       ::= { lispFeaturesEntry 8 }

   lispFeaturesMapCacheSize OBJECT-TYPE
       SYNTAX     Unsigned32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Size of EID-to-RLOC map-cache on this device."
       ::= { lispFeaturesEntry 9 }

   lispFeaturesMapCacheLimit OBJECT-TYPE
       SYNTAX     Unsigned32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Maximum permissible entries in EID-to-RLOC map-cache on
           this device."
       ::= { lispFeaturesEntry 10 }

   lispFeaturesEtrMapCacheTtl OBJECT-TYPE
       SYNTAX     Unsigned32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The stored Record TTL of the EID-to-RLOC map record in
           the map-cache."
       ::= { lispFeaturesEntry 11 }

   lispFeaturesRlocProbeEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of RLOC-Probing feature on this
           device.  If this object is true, then this feature is
           enabled."
       ::= { lispFeaturesEntry 12 }








   lispFeaturesEtrAcceptMapDataEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of accepting piggybacked mapping
           data received in a map-request on this device.  If this
           object is true, then this device accepts piggybacked
           mapping data."
       ::= { lispFeaturesEntry 13 }

   lispFeaturesEtrAcceptMapDataVerifyEnabled OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the status of verifying accepted piggybacked
           mapping data received in a map-request on this device.
           If this object is true, then this device verifies
           accepted piggybacked mapping data."
       ::= { lispFeaturesEntry 14 }

   lispFeaturesRouterTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the LISP feature was
           enabled on this device.

           If this information was present at the most recent
           reinitialization of the local management subsystem,
           then this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispFeaturesEntry 15 }

   lispIidToVrfTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispIidToVrfEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table represents the mapping of a LISP Instance ID
           to a VRF."
       REFERENCE
           "RFC 6830, Section 5.5., and RFC 4382, Section 7."
       ::= { lispObjects 2 }







   lispIidToVrfEntry OBJECT-TYPE
       SYNTAX     LispIidToVrfEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the lispIidToVrfTable."
       INDEX      { lispFeaturesInstanceID }
       ::= { lispIidToVrfTable 1 }

   LispIidToVrfEntry ::= SEQUENCE {
       lispIidToVrfName                    MplsL3VpnName
   }

   lispIidToVrfName OBJECT-TYPE
       SYNTAX     MplsL3VpnName
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The identifier for each VPN that is mapped to the
           given LISP Instance ID."
           ::= { lispIidToVrfEntry 1 }

   lispGlobalStatsTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispGlobalStatsEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table provides global statistics for a given
           Instance ID per address family on a LISP device."
       REFERENCE
           "RFC 6830, Section 6.1."
       ::= { lispObjects 3 }

   lispGlobalStatsEntry OBJECT-TYPE
       SYNTAX     LispGlobalStatsEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispGlobalStatsTable."
       INDEX      { lispFeaturesInstanceID,
                    lispFeaturesAddressFamily }
       ::= { lispGlobalStatsTable 1 }










   LispGlobalStatsEntry ::= SEQUENCE {
       lispGlobalStatsMapRequestsIn        Counter64,
       lispGlobalStatsMapRequestsOut       Counter64,
       lispGlobalStatsMapRepliesIn         Counter64,
       lispGlobalStatsMapRepliesOut        Counter64,
       lispGlobalStatsMapRegistersIn       Counter64,
       lispGlobalStatsMapRegistersOut      Counter64
   }

   lispGlobalStatsMapRequestsIn OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Total number of map requests received by this device for
           any EID-Prefix of the given address family and Instance ID.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispFeaturesRouterTimeStamp."
       ::= { lispGlobalStatsEntry 1 }

   lispGlobalStatsMapRequestsOut OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Total number of map requests sent by this device for any
           EID-Prefix of the given address family and Instance ID.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispFeaturesRouterTimeStamp."
       ::= { lispGlobalStatsEntry 2 }

   lispGlobalStatsMapRepliesIn OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Total number of map replies received by this device for any
           EID-Prefix of the given address family and Instance ID.







           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispFeaturesRouterTimeStamp."
       ::= { lispGlobalStatsEntry 3 }

   lispGlobalStatsMapRepliesOut OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Total number of map replies sent by this device for any EID
           prefix of the given address family and Instance ID.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispFeaturesRouterTimeStamp."
       ::= { lispGlobalStatsEntry 4 }

   lispGlobalStatsMapRegistersIn OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Total number of map registers received by this device for
           any EID-Prefix of the given address family and Instance ID.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispFeaturesRouterTimeStamp."
       ::= { lispGlobalStatsEntry 5 }

   lispGlobalStatsMapRegistersOut OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Total number of map registers sent by this device for any
           EID-Prefix of the given address family and Instance ID.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features





           being removed, which can be detected by observing the value
           of lispFeaturesRouterTimeStamp."
       ::= { lispGlobalStatsEntry 6 }

   lispMappingDatabaseTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispMappingDatabaseEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table represents the EID-to-RLOC mapping database
            that contains the EID-Prefix to RLOC mappings configured
            on an ETR.

           This table represents all such mappings for the given LISP
           site to which this device belongs."
       REFERENCE
           "RFC 6830, Section 6."
       ::= { lispObjects 4 }

   lispMappingDatabaseEntry OBJECT-TYPE
       SYNTAX     LispMappingDatabaseEntry

       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in lispMappingDatabaseTable."
       INDEX   { lispMappingDatabaseEidLength,
                 lispMappingDatabaseEid }
       ::= { lispMappingDatabaseTable 1 }

   LispMappingDatabaseEntry ::= SEQUENCE {
       lispMappingDatabaseEidLength        Integer32,
       lispMappingDatabaseEid              LispAddressType,
       lispMappingDatabaseLsb              Unsigned32,
       lispMappingDatabaseEidPartitioned   TruthValue,
       lispMappingDatabaseTimeStamp        TimeStamp,
       lispMappingDatabaseDecapOctets      Counter64,
       lispMappingDatabaseDecapPackets     Counter64,
       lispMappingDatabaseEncapOctets      Counter64,
       lispMappingDatabaseEncapPackets     Counter64
   }












   lispMappingDatabaseEidLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object gives the octet-length of
           lispMappingDatabaseEid."
       ::= { lispMappingDatabaseEntry 1 }

   lispMappingDatabaseEid OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "The EID-Prefix of the mapping database."
       ::= { lispMappingDatabaseEntry 2 }

   lispMappingDatabaseLsb OBJECT-TYPE
       SYNTAX     Unsigned32 (0..4294967295)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The locator status bits for this EID-Prefix."
       ::= { lispMappingDatabaseEntry 3 }

   lispMappingDatabaseEidPartitioned OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only

       STATUS     current
       DESCRIPTION
           "Indicates if this device is partitioned from the site that
           contains this EID-Prefix.  If this object is true, then it
           means this device is partitioned from the site."
       ::= { lispMappingDatabaseEntry 4 }

   lispMappingDatabaseTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the EID Prefix information
           represented by this mapping database entry was configured
           on this device.









           If this information was present at the most recent
           reinitialization of the local management subsystem, then
           this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispMappingDatabaseEntry 5 }

   lispMappingDatabaseDecapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets, after decapsulation, of LISP packets
           that were decapsulated by this device addressed to a host
           within this EID-Prefix.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispMappingDatabaseTimeStamp."
       ::= { lispMappingDatabaseEntry 6 }

   lispMappingDatabaseDecapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were decapsulated by this
           device addressed to a host within this EID-Prefix.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispMappingDatabaseTimeStamp."
       ::= { lispMappingDatabaseEntry 7 }

   lispMappingDatabaseEncapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets, before encapsulation, of LISP packets
           that were encapsulated by this device, whose inner header
           source address matched this EID-Prefix.








           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispMappingDatabaseTimeStamp."
       ::= { lispMappingDatabaseEntry 8 }

   lispMappingDatabaseEncapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were encapsulated by this
           device whose inner header source address matched this EID
           prefix.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of LISP features
           being removed, which can be detected by observing the value
           of lispMappingDatabaseTimeStamp."
       ::= { lispMappingDatabaseEntry 9 }

   lispMappingDatabaseLocatorTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispMappingDatabaseLocatorEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table represents the set of routing locators per EID
           prefix contained in the EID-to-RLOC database configured on
           this ETR."
       REFERENCE
           "RFC 6830, Section 6.2."
       ::= { lispObjects 5 }

   lispMappingDatabaseLocatorEntry OBJECT-TYPE
       SYNTAX     LispMappingDatabaseLocatorEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispMappingDatabaseLocatorTable."
       INDEX  { lispMappingDatabaseEidLength,
                lispMappingDatabaseEid,
                lispMappingDatabaseLocatorRlocLength,
                lispMappingDatabaseLocatorRloc }
       ::= { lispMappingDatabaseLocatorTable 1 }






   LispMappingDatabaseLocatorEntry ::= SEQUENCE {
       lispMappingDatabaseLocatorRlocLength        Integer32,
       lispMappingDatabaseLocatorRloc              LispAddressType,
       lispMappingDatabaseLocatorRlocPriority      Integer32,
       lispMappingDatabaseLocatorRlocWeight        Integer32,
       lispMappingDatabaseLocatorRlocMPriority     Integer32,
       lispMappingDatabaseLocatorRlocMWeight       Integer32,
       lispMappingDatabaseLocatorRlocState         INTEGER,
       lispMappingDatabaseLocatorRlocLocal         INTEGER,
       lispMappingDatabaseLocatorRlocTimeStamp     TimeStamp,
       lispMappingDatabaseLocatorRlocDecapOctets   Counter64,
       lispMappingDatabaseLocatorRlocDecapPackets  Counter64,
       lispMappingDatabaseLocatorRlocEncapOctets   Counter64,
       lispMappingDatabaseLocatorRlocEncapPackets  Counter64
   }

   lispMappingDatabaseLocatorRlocLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispMappingDatabaseLocatorRloc."
       ::= { lispMappingDatabaseLocatorEntry 1 }

   lispMappingDatabaseLocatorRloc OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is a locator for the given EID-Prefix in
           the mapping database."
       ::= { lispMappingDatabaseLocatorEntry 2 }

   lispMappingDatabaseLocatorRlocPriority OBJECT-TYPE
       SYNTAX     Integer32 (0..255)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The unicast priority of the RLOC."
       ::= { lispMappingDatabaseLocatorEntry 3 }

   lispMappingDatabaseLocatorRlocWeight OBJECT-TYPE
       SYNTAX     Integer32 (0..100)
       MAX-ACCESS read-only
       STATUS     current







       DESCRIPTION
           "The unicast weight of the RLOC."
       ::= { lispMappingDatabaseLocatorEntry 4 }

   lispMappingDatabaseLocatorRlocMPriority OBJECT-TYPE
       SYNTAX     Integer32 (0..255)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The multicast priority of the RLOC."
       ::= { lispMappingDatabaseLocatorEntry 5 }

   lispMappingDatabaseLocatorRlocMWeight OBJECT-TYPE
       SYNTAX     Integer32 (0..100)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The multicast weight of the RLOC."
       ::= { lispMappingDatabaseLocatorEntry 6 }

   lispMappingDatabaseLocatorRlocState OBJECT-TYPE
       SYNTAX     INTEGER {
                     up (1),
                     down (2),
                     unreachable (3)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The state of this RLOC as per this device.
           (1 = RLOC is up; 2 = RLOC is down; 3 = RLOC is unreachable)."
       ::= { lispMappingDatabaseLocatorEntry 7 }

   lispMappingDatabaseLocatorRlocLocal OBJECT-TYPE
       SYNTAX     INTEGER {
                     siteself (1),
                     sitelocal (2)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates whether the RLOC is local to this device
           (or remote, meaning local to another device in the same LISP
           site).  (1 = RLOC is an address on this device; 2 = RLOC is
           an address on another device)."
       ::= { lispMappingDatabaseLocatorEntry 8 }







   lispMappingDatabaseLocatorRlocTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the RLOC of the EID Prefix
           represented by this mapping database entry was configured
           on this device.

           If this information was present at the most recent
           reinitialization of the local management subsystem, then
           this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispMappingDatabaseLocatorEntry 9 }

   lispMappingDatabaseLocatorRlocDecapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets of LISP packets that were
           addressed to this RLOC of the EID-Prefix and
           were decapsulated.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of database
           mappings getting reconfigured or RLOC status changes, which
           can be detected by observing the value of
           lispMappingDatabaseLocatorRlocTimeStamp."
       ::= { lispMappingDatabaseLocatorEntry 10 }

   lispMappingDatabaseLocatorRlocDecapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were addressed to this RLOC
           of the EID-Prefix and were decapsulated.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.

           Discontinuities can also occur as a result of database
           mappings getting reconfigured or RLOC status changes, which
           can be detected by observing the value of
           lispMappingDatabaseLocatorRlocTimeStamp."
       ::= { lispMappingDatabaseLocatorEntry 11 }





   lispMappingDatabaseLocatorRlocEncapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets of LISP packets that were encapsulated
           by this device using this RLOC address as the source, and
           that were sourced by an address of this EID-Prefix.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of database
           mappings getting reconfigured or RLOC status changes, which
           can be detected by observing the value of
           lispMappingDatabaseLocatorRlocTimeStamp."
       ::= { lispMappingDatabaseLocatorEntry 12 }

   lispMappingDatabaseLocatorRlocEncapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were encapsulated by this
           device using this RLOC address as the source and that were
           sourced by an address of this EID-Prefix.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of database
           mappings getting reconfigured or RLOC status changes, which
           can be detected by observing the value of
           lispMappingDatabaseLocatorRlocTimeStamp."
       ::= { lispMappingDatabaseLocatorEntry 13 }

   lispMapCacheTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispMapCacheEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table represents the short-lived, on-demand table on
           an ITR that stores, tracks, and is responsible for
           timing-out and otherwise validating EID-to-RLOC mappings."
       REFERENCE
           "RFC 6830, Sections 6 and Section 12."
       ::= { lispObjects 6 }








   lispMapCacheEntry OBJECT-TYPE
       SYNTAX     LispMapCacheEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispMapCacheTable."
       INDEX      { lispMapCacheEidLength,
                    lispMapCacheEid }
       ::= { lispMapCacheTable 1 }

   LispMapCacheEntry ::= SEQUENCE {
       lispMapCacheEidLength           Integer32,
       lispMapCacheEid                 LispAddressType,
       lispMapCacheEidTimeStamp        TimeStamp,
       lispMapCacheEidExpiryTime       TimeTicks,
       lispMapCacheEidState            TruthValue,
       lispMapCacheEidAuthoritative    TruthValue,
       lispMapCacheEidDecapOctets      Counter64,
       lispMapCacheEidDecapPackets     Counter64,
       lispMapCacheEidEncapOctets      Counter64,
       lispMapCacheEidEncapPackets     Counter64
   }

   lispMapCacheEidLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispMapCacheEid."
       ::= { lispMapCacheEntry 1 }

   lispMapCacheEid OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "The EID-Prefix in the mapping cache."
       ::= { lispMapCacheEntry 2 }

   lispMapCacheEidTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the EID Prefix information
           represented by this entry was learned by this device.





           If this information was present at the most recent
           reinitialization of the local management subsystem, then
           this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispMapCacheEntry 3 }

   lispMapCacheEidExpiryTime OBJECT-TYPE
       SYNTAX     TimeTicks
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The time remaining before the ITR times-out this
           EID-Prefix."
       ::= { lispMapCacheEntry 4 }

   lispMapCacheEidState OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "This object is used to indicate the activity of this EID
           prefix.  If this object is true, then it means this EID
           prefix is seeing activity."
       ::= { lispMapCacheEntry 5 }

   lispMapCacheEidAuthoritative OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "This object is used to indicate whether the EID-Prefix was
           installed by an authoritative map-reply.  If this object is
           true, then it means this EID-Prefix was installed by an
           authoritative map-reply."
       ::= { lispMapCacheEntry 6 }

   lispMapCacheEidDecapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets of LISP packets that were decapsulated
           by this device and were sourced from a remote host within
           this EID-Prefix.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of cache being





           removed and replaced, which can be detected by observing the
           value of lispMapCacheEidTimeStamp."
       ::= { lispMapCacheEntry 7 }

   lispMapCacheEidDecapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were decapsulated by this
           device and were sourced from a remote host within this
           EID-Prefix.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of cache being
           removed and replaced, which can be detected by observing the
           value of lispMapCacheEidTimeStamp."
       ::= { lispMapCacheEntry 8 }

   lispMapCacheEidEncapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets of LISP packets that were encapsulated
           by this device using the given EID-Prefix in the map-cache.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of cache being
           removed and replaced, which can be detected by observing the
           value of lispMapCacheEidTimeStamp."
       ::= { lispMapCacheEntry 9 }

   lispMapCacheEidEncapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were encapsulated by this
           device using the given EID-Prefix in the map-cache.











           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of cache being
           removed and replaced, which can be detected by observing the
           value of lispMapCacheEidTimeStamp."
       ::= { lispMapCacheEntry 10 }

   lispMapCacheLocatorTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispMapCacheLocatorEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table represents the set of locators per EID-Prefix
           contained in the map-cache table of an ITR."
       REFERENCE
           "RFC 6830, Section 6.3."
       ::= { lispObjects 7 }

   lispMapCacheLocatorEntry OBJECT-TYPE
       SYNTAX     LispMapCacheLocatorEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispMapCacheLocatorTable."
       INDEX      { lispMapCacheEidLength,
                    lispMapCacheEid,
                    lispMapCacheLocatorRlocLength,
                    lispMapCacheLocatorRloc }
       ::= { lispMapCacheLocatorTable 1 }

   LispMapCacheLocatorEntry ::= SEQUENCE {
       lispMapCacheLocatorRlocLength              Integer32,
       lispMapCacheLocatorRloc                    LispAddressType,
       lispMapCacheLocatorRlocPriority            Integer32,
       lispMapCacheLocatorRlocWeight              Integer32,
       lispMapCacheLocatorRlocMPriority           Integer32,
       lispMapCacheLocatorRlocMWeight             Integer32,
       lispMapCacheLocatorRlocState               INTEGER,
       lispMapCacheLocatorRlocTimeStamp           TimeStamp,
       lispMapCacheLocatorRlocLastPriorityChange  TimeTicks,
       lispMapCacheLocatorRlocLastWeightChange    TimeTicks,
       lispMapCacheLocatorRlocLastMPriorityChange TimeTicks,
       lispMapCacheLocatorRlocLastMWeightChange   TimeTicks,
       lispMapCacheLocatorRlocLastStateChange     TimeTicks,
       lispMapCacheLocatorRlocRtt                 TimeTicks,
       lispMapCacheLocatorRlocDecapOctets         Counter64,
       lispMapCacheLocatorRlocDecapPackets        Counter64,





       lispMapCacheLocatorRlocEncapOctets         Counter64,
       lispMapCacheLocatorRlocEncapPackets        Counter64
   }

   lispMapCacheLocatorRlocLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispMapCacheLocatorRloc."
       ::= { lispMapCacheLocatorEntry 1 }

   lispMapCacheLocatorRloc OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "The locator for the EID-Prefix in the mapping cache."
       ::= { lispMapCacheLocatorEntry 2 }

   lispMapCacheLocatorRlocPriority OBJECT-TYPE
       SYNTAX     Integer32 (0..255)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The unicast priority of the RLOC for this EID-Prefix
           (0-255); lower is more preferred."
       ::= { lispMapCacheLocatorEntry 3 }

   lispMapCacheLocatorRlocWeight OBJECT-TYPE
       SYNTAX     Integer32 (0..100)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The unicast weight of the RLOC for this EID-Prefix
           (0 - 100) percentage."
       ::= { lispMapCacheLocatorEntry 4 }

   lispMapCacheLocatorRlocMPriority OBJECT-TYPE
       SYNTAX     Integer32 (0..255)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The multicast priority of the RLOC for this EID-Prefix
           (0-255); lower is more preferred."
       ::= { lispMapCacheLocatorEntry 5 }






   lispMapCacheLocatorRlocMWeight OBJECT-TYPE
       SYNTAX     Integer32 (0..100)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The multicast weight of the RLOC for this EID-Prefix
           (0 - 100) percentage."
       ::= { lispMapCacheLocatorEntry 6 }

   lispMapCacheLocatorRlocState OBJECT-TYPE
       SYNTAX     INTEGER {
                    up (1),
                    down (2),
                    unreachable (3)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The state of this RLOC as per this device
           (1 = RLOC is up; 2 = RLOC is down; 3 = RLOC is unreachable)."
       ::= { lispMapCacheLocatorEntry 7 }

   lispMapCacheLocatorRlocTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the RLOC of EID-Prefix
           information represented by this entry was learned by
           this device.

           If this information was present at the most recent
           reinitialization of the local management subsystem,
           then this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispMapCacheLocatorEntry 8 }

   lispMapCacheLocatorRlocLastPriorityChange OBJECT-TYPE
       SYNTAX     TimeTicks
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Time elapsed since the last change of the unicast priority
           of the RLOC for this EID-Prefix.  Note that this is
           independent of lispMapCacheLocatorRlocTimeStamp."
       ::= { lispMapCacheLocatorEntry 9 }







   lispMapCacheLocatorRlocLastWeightChange OBJECT-TYPE
       SYNTAX     TimeTicks
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Time elapsed since the last change of the unicast weight
           of the RLOC for this EID-Prefix.  Note that this is
           independent of lispMapCacheLocatorRlocTimeStamp."
       ::= { lispMapCacheLocatorEntry 10 }

   lispMapCacheLocatorRlocLastMPriorityChange OBJECT-TYPE
       SYNTAX     TimeTicks
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Time since the last change of the multicast priority of the
           RLOC for this EID-Prefix."
       ::= { lispMapCacheLocatorEntry 11 }

   lispMapCacheLocatorRlocLastMWeightChange OBJECT-TYPE
       SYNTAX     TimeTicks
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Time since the last change of the multicast weight of the
           RLOC for this EID-Prefix."
       ::= { lispMapCacheLocatorEntry 12 }

   lispMapCacheLocatorRlocLastStateChange OBJECT-TYPE
       SYNTAX     TimeTicks
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Time since the last change of the up/down state of the
           RLOC for this EID-Prefix."
       ::= { lispMapCacheLocatorEntry 13 }

   lispMapCacheLocatorRlocRtt OBJECT-TYPE
       SYNTAX     TimeTicks
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Round-trip time of RLOC probe and map-reply for this RLOC
           address for this prefix."
       ::= { lispMapCacheLocatorEntry 14 }








   lispMapCacheLocatorRlocDecapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets of LISP packets that were decapsulated
           by this device and were sourced from a remote host within
           this EID-Prefix and were encapsulated for this RLOC.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of RLOC of cache
           being removed and replaced, which can be detected by
           observing the value of lispMapCacheLocatorRlocTimeStamp."
       ::= { lispMapCacheLocatorEntry 15 }

   lispMapCacheLocatorRlocDecapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were decapsulated by this
           device and were sourced from a remote host within this
           EID-Prefix and were encapsulated for this RLOC.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of RLOC of cache
           being removed and replaced, which can be detected by
           observing the value of lispMapCacheLocatorRlocTimeStamp."
       ::= { lispMapCacheLocatorEntry 16 }

   lispMapCacheLocatorRlocEncapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets of LISP packets that matched this
           EID-Prefix and were encapsulated using this RLOC address.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of RLOC of cache
           being removed and replaced, which can be detected by
           observing the value of lispMapCacheLocatorRlocTimeStamp."
       ::= { lispMapCacheLocatorEntry 17 }







   lispMapCacheLocatorRlocEncapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that matched this EID-Prefix
           and were encapsulated using this RLOC address.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of RLOC of cache
           being removed and replaced, which can be detected by
           observing the value of lispMapCacheLocatorRlocTimeStamp."
       ::= { lispMapCacheLocatorEntry 18 }

   lispConfiguredLocatorTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispConfiguredLocatorEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table represents the set of routing locators
           configured on this device.  Note that the addresses
           configured by Proxy-ITR are treated as routing locators
           and therefore can be part of this table."
       REFERENCE
           "RFC 6830, Section 6.3."
       ::= { lispObjects 8 }

   lispConfiguredLocatorEntry OBJECT-TYPE
       SYNTAX     LispConfiguredLocatorEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispConfiguredLocatorTable."
       INDEX  { lispConfiguredLocatorRlocLength,
                lispConfiguredLocatorRloc }
       ::= { lispConfiguredLocatorTable 1 }

   LispConfiguredLocatorEntry ::= SEQUENCE {
       lispConfiguredLocatorRlocLength        Integer32,
       lispConfiguredLocatorRloc              LispAddressType,
       lispConfiguredLocatorRlocState         INTEGER,
       lispConfiguredLocatorRlocLocal         INTEGER,
       lispConfiguredLocatorRlocTimeStamp     TimeStamp,
       lispConfiguredLocatorRlocDecapOctets   Counter64,
       lispConfiguredLocatorRlocDecapPackets  Counter64,
       lispConfiguredLocatorRlocEncapOctets   Counter64,





       lispConfiguredLocatorRlocEncapPackets  Counter64
   }

   lispConfiguredLocatorRlocLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispConfiguredLocatorRloc."
       ::= { lispConfiguredLocatorEntry 1 }

   lispConfiguredLocatorRloc OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is an RLOC address configured on this device.
           It can be an RLOC that is local to this device or can be an
           RLOC that belongs to another ETR within the same site.
           Proxy-ITR address is treated as an RLOC."
       ::= { lispConfiguredLocatorEntry 2 }

   lispConfiguredLocatorRlocState OBJECT-TYPE
       SYNTAX     INTEGER {
                     up (1),
                     down (2),
                     unreachable (3)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The state of this RLOC as per this device.  (1 = RLOC is up;
           2 = RLOC is down; 3 = RLOC is unreachable)."
       ::= { lispConfiguredLocatorEntry 3 }

   lispConfiguredLocatorRlocLocal OBJECT-TYPE
       SYNTAX     INTEGER {
                     siteself (1),
                     sitelocal (2)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates whether the RLOC is local to this device (or
           remote, meaning local to another device in the same LISP
           site).  (1 = RLOC is an address on this device; 2 = RLOC is
           an address on another device)."





       ::= { lispConfiguredLocatorEntry 4 }

   lispConfiguredLocatorRlocTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the RLOC was configured on
           this device.

           If this information was present at the most recent
           reinitialization of the local management subsystem, then
           this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispConfiguredLocatorEntry 5 }

   lispConfiguredLocatorRlocDecapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets of LISP packets that were addressed to
           this RLOC and were decapsulated.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of configured
           RLOC being removed and replaced, which can be detected by
           observing the value of lispConfiguredLocatorRlocTimeStamp."
       ::= { lispConfiguredLocatorEntry 6 }

   lispConfiguredLocatorRlocDecapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were addressed to this RLOC
           and were decapsulated.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of configured
           RLOC being removed and replaced, which can be detected by
           observing the value of lispConfiguredLocatorRlocTimeStamp."
       ::= { lispConfiguredLocatorEntry 7 }








   lispConfiguredLocatorRlocEncapOctets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of octets of LISP packets that were encapsulated
           by this device using this RLOC address as the source.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of configured
           RLOC being removed and replaced, which can be detected by
           observing the value of lispConfiguredLocatorRlocTimeStamp."
       ::= { lispConfiguredLocatorEntry 8 }

   lispConfiguredLocatorRlocEncapPackets OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of LISP packets that were encapsulated by this
           device using this RLOC address as the source.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of configured
           RLOC being removed and replaced, which can be detected by
           observing the value of lispConfiguredLocatorRlocTimeStamp."
       ::= { lispConfiguredLocatorEntry 9 }

   lispEidRegistrationTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispEidRegistrationEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table provides the properties of each LISP EID-Prefix
           that is registered with this device when configured to be
           a Map-Server."
       REFERENCE
           "RFC 6833, Section 4."
       ::= { lispObjects 9 }

   lispEidRegistrationEntry OBJECT-TYPE
       SYNTAX     LispEidRegistrationEntry
       MAX-ACCESS not-accessible
       STATUS     current







       DESCRIPTION
           "An entry (conceptual row) in the lispEidRegistrationTable."
       INDEX      { lispEidRegistrationEidLength,
                    lispEidRegistrationEid }
       ::= { lispEidRegistrationTable 1 }

   LispEidRegistrationEntry ::= SEQUENCE {
       lispEidRegistrationEidLength                 Integer32,
       lispEidRegistrationEid                       LispAddressType,
       lispEidRegistrationSiteName                  OCTET STRING,
       lispEidRegistrationSiteDescription           OCTET STRING,
       lispEidRegistrationIsRegistered              TruthValue,
       lispEidRegistrationFirstTimeStamp            TimeStamp,
       lispEidRegistrationLastTimeStamp             TimeStamp,
       lispEidRegistrationLastRegisterSenderLength  Integer32,
       lispEidRegistrationLastRegisterSender        LispAddressType,
       lispEidRegistrationAuthenticationErrors      Counter64,
       lispEidRegistrationRlocsMismatch             Counter64
   }

   lispEidRegistrationEidLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispEidRegistrationEid."
       ::= { lispEidRegistrationEntry 1 }

   lispEidRegistrationEid OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "The EID-Prefix that is being registered."
        ::= { lispEidRegistrationEntry 2 }

   lispEidRegistrationSiteName OBJECT-TYPE
       SYNTAX     OCTET STRING (SIZE(0..63))
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Site name used by a Map-Server to distinguish different
           LISP sites that are registering with it."
       ::= { lispEidRegistrationEntry 3 }

   lispEidRegistrationSiteDescription OBJECT-TYPE
       SYNTAX     OCTET STRING (SIZE(0..255))





       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Description for a site name used by a Map-Server.  The EID
           prefix that is being registered belongs to this site."
       ::= { lispEidRegistrationEntry 4 }

   lispEidRegistrationIsRegistered OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates the registration status of the given EID-Prefix.
           If this object is true, then it means the EID-Prefix is
           registered.

           The value false implies the EID-Prefix is not registered
           with the Map Server.  There are multiple scenarios when this
           could happen like authentication failures, routing problems,
           misconfigs to name a few."
       ::= { lispEidRegistrationEntry 5 }

   lispEidRegistrationFirstTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the first valid register
           message for the EID Prefix information represented by this
           entry was received by this device.

           If this information was present at the most recent
           reinitialization of the local management subsystem, then
           this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispEidRegistrationEntry 6 }

   lispEidRegistrationLastTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the last valid register
           message for the EID Prefix information represented by this
           entry was received by this device.








           If this information was present at the most recent
           reinitialization of the local management subsystem, then
           this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispEidRegistrationEntry 7 }

   lispEidRegistrationLastRegisterSenderLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispEidRegistrationLastRegisterSender, the next
           object."
       ::= { lispEidRegistrationEntry 8 }

   lispEidRegistrationLastRegisterSender OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Source address of the last valid register message for the
           given EID-Prefix that was received by this device."
       ::= { lispEidRegistrationEntry 9 }

   lispEidRegistrationAuthenticationErrors OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Count of total authentication errors of map-registers
           received for the given EID-Prefix.

           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of site config
           changes, which can be detected by observing the value of
           lispEidRegistrationFirstTimeStamp."
       ::= { lispEidRegistrationEntry 10 }

   lispEidRegistrationRlocsMismatch OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Count of total map-registers received that had at least one
           RLOC that was not in the allowed list of RLOCs for the given
           EID-Prefix.





           Discontinuities in this monotonically increasing value occur
           at reinitialization of the management system.
           Discontinuities can also occur as a result of site config
           changes, which can be detected by observing the value of
           lispEidRegistrationFirstTimeStamp."
       ::= { lispEidRegistrationEntry 11 }

   lispEidRegistrationEtrTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispEidRegistrationEtrEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table provides the properties of ETRs that register
           the given EID-Prefix with this device when configured to
           be a Map-Server."
       REFERENCE
           "RFC 6830, Section 6.1."
       ::= { lispObjects 10 }

   lispEidRegistrationEtrEntry OBJECT-TYPE
       SYNTAX     LispEidRegistrationEtrEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispEidRegistrationEtrTable."
       INDEX      { lispEidRegistrationEidLength,
                    lispEidRegistrationEid,
                    lispEidRegistrationEtrSenderLength,
                    lispEidRegistrationEtrSender }
       ::= { lispEidRegistrationEtrTable 1 }

   LispEidRegistrationEtrEntry ::= SEQUENCE {
       lispEidRegistrationEtrSenderLength           Integer32,
       lispEidRegistrationEtrSender                 LispAddressType,
       lispEidRegistrationEtrLastTimeStamp          TimeStamp,
       lispEidRegistrationEtrTtl                    Unsigned32,
       lispEidRegistrationEtrProxyReply             TruthValue,
       lispEidRegistrationEtrWantsMapNotify         TruthValue
   }

   lispEidRegistrationEtrSenderLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispEidRegistrationEtrSender."





       ::= { lispEidRegistrationEtrEntry 1 }

   lispEidRegistrationEtrSender OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "Source address of the ETR that is sending valid register
           messages for this EID-Prefix to this device."
       ::= { lispEidRegistrationEtrEntry 2 }

   lispEidRegistrationEtrLastTimeStamp OBJECT-TYPE
       SYNTAX     TimeStamp
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The value of sysUpTime at which the last valid register
           message from this ETR for the EID Prefix information
           represented by this entry was received by this device.

           If this information was present at the most recent
           reinitialization of the local management subsystem,
           then this object contains a zero value."
       DEFVAL { 0 }
       ::= { lispEidRegistrationEtrEntry 3 }

   lispEidRegistrationEtrTtl OBJECT-TYPE
       SYNTAX     Unsigned32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The Record TTL of the registering ETR device for this
           EID-Prefix."
       ::= { lispEidRegistrationEtrEntry 4 }

   lispEidRegistrationEtrProxyReply OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates proxy-replying status of the registering ETR for
           this EID-Prefix.  If this object is true, then it means the
           Map-Server can proxy-reply."
       ::= { lispEidRegistrationEtrEntry 5 }

   lispEidRegistrationEtrWantsMapNotify OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only





       STATUS     current
       DESCRIPTION
           "Indicates whether the EID-Prefix wants Map-Notifications.
           If this object is true, then it means the EID-Prefix wants
           Map-Notifications."
       ::= { lispEidRegistrationEtrEntry 6 }

   lispEidRegistrationLocatorTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispEidRegistrationLocatorEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table provides the properties of all locators per
           LISP site that are served by this device when configured
           to be a Map-Server."
       REFERENCE
           "RFC 6830, Section 6.1."
       ::= { lispObjects 11 }

   lispEidRegistrationLocatorEntry OBJECT-TYPE
       SYNTAX     LispEidRegistrationLocatorEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispEidRegistrationLocatorTable."
       INDEX      { lispEidRegistrationEidLength,
                    lispEidRegistrationEid,
                    lispEidRegistrationEtrSenderLength,
                    lispEidRegistrationEtrSender,
                    lispEidRegistrationLocatorRlocLength,
                    lispEidRegistrationLocatorRloc }
       ::= { lispEidRegistrationLocatorTable 1 }

   LispEidRegistrationLocatorEntry ::= SEQUENCE {
       lispEidRegistrationLocatorRlocLength         Integer32,
       lispEidRegistrationLocatorRloc               LispAddressType,
       lispEidRegistrationLocatorRlocState          INTEGER,
       lispEidRegistrationLocatorIsLocal            TruthValue,
       lispEidRegistrationLocatorPriority           Integer32,
       lispEidRegistrationLocatorWeight             Integer32,
       lispEidRegistrationLocatorMPriority          Integer32,
       lispEidRegistrationLocatorMWeight            Integer32
   }

   lispEidRegistrationLocatorRlocLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible





       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispEidRegistrationLocatorRloc."
       ::= { lispEidRegistrationLocatorEntry 1 }

   lispEidRegistrationLocatorRloc OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "The locator of the given EID-Prefix being registered by the
           given ETR with this device."
       ::= { lispEidRegistrationLocatorEntry 2 }

   lispEidRegistrationLocatorRlocState OBJECT-TYPE
       SYNTAX     INTEGER {
                     up (1),
                     down (2)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The cached state of this RLOC received in map-register from
           the ETR by the device, in the capacity of a Map-Server.
           Value 1 refers to up, value 2 refers to down."
       ::= { lispEidRegistrationLocatorEntry 3 }

   lispEidRegistrationLocatorIsLocal OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Indicates if the given locator is local to the registering
           ETR.  If this object is true,  it means the locator is
           local."
       ::= { lispEidRegistrationLocatorEntry 4 }

   lispEidRegistrationLocatorPriority OBJECT-TYPE
       SYNTAX     Integer32 (0..255)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The unicast priority of the RLOC for this EID-Prefix in the
           register message sent by the given ETR."
       ::= { lispEidRegistrationLocatorEntry 5 }







   lispEidRegistrationLocatorWeight OBJECT-TYPE
       SYNTAX     Integer32 (0..100)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The unicast weight of the RLOC for this EID-Prefix in the
           register message sent by the given ETR."
       ::= { lispEidRegistrationLocatorEntry 6 }

   lispEidRegistrationLocatorMPriority OBJECT-TYPE
       SYNTAX     Integer32 (0..255)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The multicast priority of the RLOC for this EID-Prefix in
           the register message sent by the given ETR."
       ::= { lispEidRegistrationLocatorEntry 7 }

   lispEidRegistrationLocatorMWeight OBJECT-TYPE
       SYNTAX     Integer32 (0..100)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The multicast weight of the RLOC for this EID-Prefix in the
           register message sent by the given ETR."
       ::= { lispEidRegistrationLocatorEntry 8 }

   lispUseMapServerTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispUseMapServerEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table provides the properties of the Map-Server(s)
           with which this device is configured to register."
       REFERENCE
           "RFC 6833, Section 4.3."
       ::= { lispObjects 12 }

   lispUseMapServerEntry OBJECT-TYPE
       SYNTAX     LispUseMapServerEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the lispUseMapServerTable."
       INDEX      { lispUseMapServerAddressLength,
                    lispUseMapServerAddress }
       ::= { lispUseMapServerTable 1 }






   LispUseMapServerEntry ::= SEQUENCE {
       lispUseMapServerAddressLength Integer32,
       lispUseMapServerAddress       LispAddressType,
       lispUseMapServerState         INTEGER
   }

   lispUseMapServerAddressLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispUseMapServerAddress."
       ::= { lispUseMapServerEntry 1 }

   lispUseMapServerAddress OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "Address of a Map-Server configured on this device."
       ::= { lispUseMapServerEntry 2 }

   lispUseMapServerState OBJECT-TYPE
       SYNTAX     INTEGER {
                     up (1),
                     down (2),
                     unreachable (3)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "State of this Map-Server configured on this device
           (1 = Map-Server is up; 2 = Map-Server is down)."
       ::= { lispUseMapServerEntry 3 }

   lispUseMapResolverTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispUseMapResolverEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This table provides the properties of the Map-Resolver(s)
           this device is configured to use."
       REFERENCE
           "RFC 6833, Section 4.4."
       ::= { lispObjects 13 }

   lispUseMapResolverEntry OBJECT-TYPE





       SYNTAX     LispUseMapResolverEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispUseMapResolverTable."
       INDEX      { lispUseMapResolverAddressLength,
                    lispUseMapResolverAddress }
       ::= { lispUseMapResolverTable 1 }

   LispUseMapResolverEntry ::= SEQUENCE {
       lispUseMapResolverAddressLength   Integer32,
       lispUseMapResolverAddress         LispAddressType,
       lispUseMapResolverState           INTEGER
   }

   lispUseMapResolverAddressLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispUseMapResolverAddress."
       ::= { lispUseMapResolverEntry 1 }

   lispUseMapResolverAddress OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "Address of Map-Resolver configured on this device."
       ::= { lispUseMapResolverEntry 2 }

   lispUseMapResolverState OBJECT-TYPE
       SYNTAX     INTEGER {
                     up (1),
                     down (2)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "State of this Map-Resolver configured on this device
           (1 = Map-Resolver is up; 2 = Map-Resolver is down)."
       ::= { lispUseMapResolverEntry 3 }

   lispUseProxyEtrTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF LispUseProxyEtrEntry
       MAX-ACCESS not-accessible





       STATUS     current
       DESCRIPTION
           "This table provides the properties of all Proxy ETRs that
           this device is configured to use."
       REFERENCE
           "RFC 6830, Section 6."
       ::= { lispObjects 14 }

   lispUseProxyEtrEntry OBJECT-TYPE
       SYNTAX     LispUseProxyEtrEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An entry (conceptual row) in the
           lispUseProxyEtrTable."
       INDEX      { lispUseProxyEtrAddressLength,
                    lispUseProxyEtrAddress }
       ::= { lispUseProxyEtrTable 1 }

   LispUseProxyEtrEntry ::= SEQUENCE {
       lispUseProxyEtrAddressLength        Integer32,
       lispUseProxyEtrAddress              LispAddressType,
       lispUseProxyEtrPriority             Integer32,
       lispUseProxyEtrWeight               Integer32,
       lispUseProxyEtrMPriority            Integer32,
       lispUseProxyEtrMWeight              Integer32,
       lispUseProxyEtrState                INTEGER
   }

   lispUseProxyEtrAddressLength OBJECT-TYPE
       SYNTAX     Integer32 (5..39)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "This object is used to get the octet-length of
           lispUseProxyEtrAddress."
       ::= { lispUseProxyEtrEntry 1 }

   lispUseProxyEtrAddress OBJECT-TYPE
       SYNTAX     LispAddressType
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "Address of Proxy ETR configured on this device."
       ::= { lispUseProxyEtrEntry 2 }

   lispUseProxyEtrPriority OBJECT-TYPE
       SYNTAX     Integer32 (0..255)





       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The unicast priority of the PETR locator."
       ::= { lispUseProxyEtrEntry 3 }

   lispUseProxyEtrWeight OBJECT-TYPE
       SYNTAX     Integer32 (0..100)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The unicast weight of the PETR locator."
       ::= { lispUseProxyEtrEntry 4 }

   lispUseProxyEtrMPriority OBJECT-TYPE
       SYNTAX     Integer32 (0..255)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The multicast priority of the PETR locator."
       ::= { lispUseProxyEtrEntry 5 }

   lispUseProxyEtrMWeight OBJECT-TYPE
       SYNTAX     Integer32 (0..100)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The multicast weight of the PETR locator."
       ::= { lispUseProxyEtrEntry 6 }

   lispUseProxyEtrState OBJECT-TYPE
       SYNTAX     INTEGER {
                     down (0),
                     up (1)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "State of this Proxy ETR configured on this device
           (0 = Proxy ETR is down; 1 = Proxy ETR is up)."
       ::= { lispUseProxyEtrEntry 7 }

   --
   -- Conformance Information
   --

   lispCompliances OBJECT IDENTIFIER ::= { lispConformance 1 }
   lispGroups      OBJECT IDENTIFIER ::= { lispConformance 2 }





   --
   -- Compliance Statements
   --

   lispMIBComplianceEtr MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for LISP ETRs.  It conveys
               whether the device supports the ETR feature, and,
               if so, the relevant state associated with that feature."
       MODULE  -- this module
       MANDATORY-GROUPS { lispMIBEtrGroup }

         GROUP   lispMIBItrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPetrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPitrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapResolverGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEtrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBTuningParametersGroup
         DESCRIPTION
             "This group is optional."





         GROUP   lispMIBEncapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDecapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDiagnosticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBVrfGroup
         DESCRIPTION
             "This group is optional."

       ::= { lispCompliances 1 }

   lispMIBComplianceItr MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for LISP ITRs.  It conveys
               whether the device supports the ITR feature, and,
               if so, the relevant state associated with that feature."
       MODULE  -- this module
       MANDATORY-GROUPS { lispMIBItrGroup }

         GROUP   lispMIBEtrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPetrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPitrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapResolverGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEtrExtendedGroup





         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBTuningParametersGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEncapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDecapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDiagnosticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBVrfGroup
         DESCRIPTION
             "This group is optional."

       ::= { lispCompliances 2 }

   lispMIBCompliancePetr MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for LISP Proxy-ETRs.  It
               conveys whether the device supports the Proxy-ETR
               feature, and, if so, the relevant state associated
               with that feature."
       MODULE  -- this module
       MANDATORY-GROUPS { lispMIBPetrGroup }

         GROUP   lispMIBEtrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrGroup





         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPitrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapResolverGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEtrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBTuningParametersGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEncapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDecapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDiagnosticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBVrfGroup
         DESCRIPTION
             "This group is optional."

       ::= { lispCompliances 3 }





   lispMIBCompliancePitr MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for LISP Proxy-ITRs.  It
               conveys whether the device supports the Proxy-ITR
               feature, and, if so, the relevant state associated
               with that feature."
       MODULE  -- this module
       MANDATORY-GROUPS { lispMIBPitrGroup }

         GROUP   lispMIBEtrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPetrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapResolverGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEtrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBTuningParametersGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEncapStatisticsGroup






         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDecapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDiagnosticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBVrfGroup
         DESCRIPTION
             "This group is optional."

       ::= { lispCompliances 4 }

   lispMIBComplianceMapServer MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for LISP Map Servers.  It
               conveys whether the device supports the Map Server
               feature, and, if so, the relevant state associated
               with that feature."
       MODULE  -- this module
       MANDATORY-GROUPS { lispMIBMapServerGroup }

         GROUP   lispMIBEtrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPetrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPitrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapResolverGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEtrExtendedGroup





         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBTuningParametersGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEncapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDecapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDiagnosticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBVrfGroup
         DESCRIPTION
             "This group is optional."

       ::= { lispCompliances 5 }

   lispMIBComplianceMapResolver MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for LISP Map Resolvers.  It
               conveys whether the device supports the Map Resolver
               feature, and, if so, the relevant state associated
               with that feature."
       MODULE  -- this module
       MANDATORY-GROUPS { lispMIBMapResolverGroup }

         GROUP   lispMIBEtrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrGroup





         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPetrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBPitrGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEtrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBItrExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBMapServerExtendedGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBTuningParametersGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBEncapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDecapStatisticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBDiagnosticsGroup
         DESCRIPTION
             "This group is optional."

         GROUP   lispMIBVrfGroup
         DESCRIPTION
             "This group is optional."

       ::= { lispCompliances 6 }





   --
   -- Units of Conformance
   --

   lispMIBEtrGroup OBJECT-GROUP
       OBJECTS { lispFeaturesEtrEnabled,
                 lispMappingDatabaseLsb,
                 lispMappingDatabaseLocatorRlocPriority,
                 lispMappingDatabaseLocatorRlocWeight,
                 lispMappingDatabaseLocatorRlocMPriority,
                 lispMappingDatabaseLocatorRlocMWeight,
                 lispMappingDatabaseLocatorRlocState,
                 lispMappingDatabaseLocatorRlocLocal,
                 lispConfiguredLocatorRlocState,
                 lispConfiguredLocatorRlocLocal,
                 lispUseMapServerState
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects to support reporting of basic
                LISP ETR parameters."
       ::= { lispGroups 1 }

   lispMIBItrGroup OBJECT-GROUP
       OBJECTS { lispFeaturesItrEnabled,
                 lispFeaturesMapCacheSize,
                 lispMappingDatabaseLsb,
                 lispMapCacheLocatorRlocPriority,
                 lispMapCacheLocatorRlocWeight,
                 lispMapCacheLocatorRlocMPriority,
                 lispMapCacheLocatorRlocMWeight,
                 lispMapCacheLocatorRlocState,
                 lispMapCacheEidTimeStamp,
                 lispMapCacheEidExpiryTime,
                 lispUseMapResolverState,
                 lispUseProxyEtrPriority,
                 lispUseProxyEtrWeight,
                 lispUseProxyEtrMPriority,
                 lispUseProxyEtrMWeight,
                 lispUseProxyEtrState
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects to support reporting of basic
                LISP ITR parameters."
       ::= { lispGroups 2 }







   lispMIBPetrGroup OBJECT-GROUP
       OBJECTS { lispFeaturesProxyEtrEnabled
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects to support reporting of basic
                LISP Proxy-ETR parameters."
       ::= { lispGroups 3 }

   lispMIBPitrGroup OBJECT-GROUP
       OBJECTS { lispFeaturesProxyItrEnabled,
                 lispConfiguredLocatorRlocState,
                 lispConfiguredLocatorRlocLocal
               }

       STATUS  current
       DESCRIPTION
               "A collection of objects to support reporting of basic
                LISP Proxy-ITR parameters."
       ::= { lispGroups 4 }

   lispMIBMapServerGroup OBJECT-GROUP
       OBJECTS { lispFeaturesMapServerEnabled,
                 lispEidRegistrationIsRegistered,
                 lispEidRegistrationLocatorRlocState
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects to support reporting of basic
                LISP Map Server parameters."
       ::= { lispGroups 5 }

   lispMIBMapResolverGroup OBJECT-GROUP
       OBJECTS { lispFeaturesMapResolverEnabled
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects to support reporting of basic
                LISP Map Resolver parameters."
       ::= { lispGroups 6 }

   lispMIBEtrExtendedGroup OBJECT-GROUP
       OBJECTS { lispFeaturesRlocProbeEnabled,
                 lispFeaturesEtrAcceptMapDataEnabled,
                 lispFeaturesEtrAcceptMapDataVerifyEnabled,
                 lispMappingDatabaseEidPartitioned
               }
       STATUS  current





       DESCRIPTION
               "A collection of objects to support reporting of
                LISP features and properties on ETRs."
       ::= { lispGroups 7 }

   lispMIBItrExtendedGroup OBJECT-GROUP
       OBJECTS { lispFeaturesRlocProbeEnabled,
                 lispMapCacheEidState,
                 lispMapCacheEidAuthoritative,
                 lispMapCacheLocatorRlocTimeStamp,
                 lispMapCacheLocatorRlocLastPriorityChange,
                 lispMapCacheLocatorRlocLastWeightChange,
                 lispMapCacheLocatorRlocLastMPriorityChange,
                 lispMapCacheLocatorRlocLastMWeightChange,
                 lispMapCacheLocatorRlocLastStateChange,
                 lispMapCacheLocatorRlocRtt
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects to support reporting of
                LISP features and properties on ITRs."
       ::= { lispGroups 8 }

   lispMIBMapServerExtendedGroup OBJECT-GROUP
       OBJECTS { lispEidRegistrationSiteName,
                 lispEidRegistrationSiteDescription,
                 lispEidRegistrationIsRegistered,
                 lispEidRegistrationFirstTimeStamp,
                 lispEidRegistrationLastTimeStamp,
                 lispEidRegistrationLastRegisterSenderLength,
                 lispEidRegistrationLastRegisterSender,
                 lispEidRegistrationEtrLastTimeStamp,
                 lispEidRegistrationEtrTtl,
                 lispEidRegistrationEtrProxyReply,
                 lispEidRegistrationEtrWantsMapNotify,
                 lispEidRegistrationLocatorIsLocal,
                 lispEidRegistrationLocatorPriority,
                 lispEidRegistrationLocatorWeight,
                 lispEidRegistrationLocatorMPriority,
                 lispEidRegistrationLocatorMWeight
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects to support the reporting of
                LISP features and properties on Map Servers
                related to EID registrations."
       ::= { lispGroups 9 }






   lispMIBTuningParametersGroup OBJECT-GROUP
       OBJECTS { lispFeaturesMapCacheLimit,
                 lispFeaturesEtrMapCacheTtl
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects used to support the reporting of
                parameters used to control LISP behavior and to tune
                performance."
       ::= { lispGroups 10 }

   lispMIBEncapStatisticsGroup OBJECT-GROUP
       OBJECTS { lispMappingDatabaseTimeStamp,
                 lispMappingDatabaseEncapOctets,
                 lispMappingDatabaseEncapPackets,
                 lispMappingDatabaseLocatorRlocTimeStamp,
                 lispMappingDatabaseLocatorRlocEncapOctets,
                 lispMappingDatabaseLocatorRlocEncapPackets,
                 lispMapCacheEidTimeStamp,
                 lispMapCacheEidEncapOctets,
                 lispMapCacheEidEncapPackets,
                 lispMapCacheLocatorRlocTimeStamp,
                 lispMapCacheLocatorRlocEncapOctets,
                 lispMapCacheLocatorRlocEncapPackets,
                 lispConfiguredLocatorRlocTimeStamp,
                 lispConfiguredLocatorRlocEncapOctets,
                 lispConfiguredLocatorRlocEncapPackets
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects used to support the reporting of
                LISP encapsulation statistics for the device."
       ::= { lispGroups 11 }

   lispMIBDecapStatisticsGroup OBJECT-GROUP
       OBJECTS { lispMappingDatabaseTimeStamp,
                 lispMappingDatabaseDecapOctets,
                 lispMappingDatabaseDecapPackets,
                 lispMappingDatabaseLocatorRlocTimeStamp,
                 lispMappingDatabaseLocatorRlocDecapOctets,
                 lispMappingDatabaseLocatorRlocDecapPackets,
                 lispMapCacheEidTimeStamp,
                 lispMapCacheEidDecapOctets,
                 lispMapCacheEidDecapPackets,
                 lispMapCacheLocatorRlocTimeStamp,
                 lispMapCacheLocatorRlocDecapOctets,
                 lispMapCacheLocatorRlocDecapPackets,
                 lispConfiguredLocatorRlocTimeStamp,





                 lispConfiguredLocatorRlocDecapOctets,
                 lispConfiguredLocatorRlocDecapPackets
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects used to support the reporting of
                LISP decapsulation statistics for the device."
       ::= { lispGroups 12 }

   lispMIBDiagnosticsGroup OBJECT-GROUP
       OBJECTS { lispFeaturesRouterTimeStamp,
                 lispGlobalStatsMapRequestsIn,
                 lispGlobalStatsMapRequestsOut,
                 lispGlobalStatsMapRepliesIn,
                 lispGlobalStatsMapRepliesOut,
                 lispGlobalStatsMapRegistersIn,
                 lispGlobalStatsMapRegistersOut,
                 lispEidRegistrationAuthenticationErrors,
                 lispEidRegistrationRlocsMismatch
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects used to support the reporting of
                additional diagnostics related to the LISP control-plane
                state of a LISP device."
       ::= { lispGroups 13 }

   lispMIBVrfGroup OBJECT-GROUP
       OBJECTS { lispIidToVrfName
               }
       STATUS  current
       DESCRIPTION
               "A collection of objects used to support reporting of
                VRF-related information on a LISP device."
       ::= { lispGroups 14 }
END


