IPATM-IPMC-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-COMPLIANCE, NOTIFICATION-GROUP, OBJECT-GROUP
           FROM SNMPv2-CONF
       snmpModules, MODULE-IDENTITY, NOTIFICATION-TYPE, Counter32,
           Integer32, Unsigned32, OBJECT-TYPE, IpAddress
           FROM SNMPv2-SMI
       AtmAddr
           FROM ATM-TC-MIB
       TruthValue, RowStatus
           FROM SNMPv2-TC
       ipAdEntAddr
           FROM RFC1213-MIB
       InterfaceIndex
           FROM IF-MIB;

      marsMIB MODULE-IDENTITY
          LAST-UPDATED "9809010000Z" -- 01 September 1998
          ORGANIZATION "Internetworking Over NBMA (ion) Working Group"
          CONTACT-INFO
              "        Chris Chung (chihschung@aol.com)
                       Independent Consultant

               Editor: Maria Greene
               Postal: Independent Contractor
               E-mail: maria@xedia.com
              "
          DESCRIPTION
              "This module defines a portion of the managed information
               base (MIB) for managing classical IP multicast address
               resolution server (MARS) and related entities as
               described in the RFC2022.  This MIB is meant to be
               used in conjunction with the ATM-MIB (RFC1695),
               MIB-II (RFC1213), and optionally the IF-MIB (RFC1573).
              "
          REVISION     "9809010000Z" -- 01 September 1998
          DESCRIPTION  "Published as RFC 2417. Changes/fixes:
                        - reroot this MIB from snmpModules to mib-2
                          to be consistent with location of other MIBs.
                        - obsoletes RFC2366."
          REVISION     "9804150145Z" -- 15 April 1998
          DESCRIPTION  "Initial version, published as RFC 2366"
          ::= { mib-2 57 }

   --***************************************************************





   --  IP ATM MARS Client Object Definitions
   --***************************************************************

   marsClientObjects  OBJECT IDENTIFIER ::= { marsMIB 1 }

   marsClientTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsClientEntry
       MAX-ACCESS  not-accessible
       STATUS current
       DESCRIPTION
           "The objects defined in this table are used for
            the management of MARS clients, ATM attached
            endpoints."
       ::= { marsClientObjects 1 }

   marsClientEntry OBJECT-TYPE
       SYNTAX  MarsClientEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry contains a MARS client and its associated
            attributes.  An entry in the marsClientTable has
            a corresponding entry in the ipAddrTable defined in
            RFC1213. Association between the ipAddrTable and
            the marsClientTable is made through the index,
            ipAdEntAddr."
       INDEX { ipAdEntAddr, marsClientIndex }
       ::= { marsClientTable 1 }

   MarsClientEntry ::=
       SEQUENCE {
           marsClientIndex                    Integer32,
           marsClientAddr                     AtmAddr,
           marsClientDefaultMarsAddr          AtmAddr,
           marsClientHsn                      Unsigned32,
           marsClientRegistration             INTEGER,
           marsClientCmi                      INTEGER,
           marsClientDefaultMtu               INTEGER,
           marsClientFailureTimer             INTEGER,
           marsClientRetranDelayTimer         INTEGER,
           marsClientRdmMulReqAddRetrTimer    INTEGER,
           marsClientRdmVcRevalidateTimer     INTEGER,
           marsClientJoinLeaveRetrInterval    INTEGER,
           marsClientJoinLeaveRetrLimit       INTEGER,
           marsClientRegWithMarsRdmTimer      INTEGER,
           marsClientForceWaitTimer           INTEGER,
           marsClientLmtToMissRedirMapTimer   INTEGER,
           marsClientIdleTimer                INTEGER,





           marsClientRowStatus                RowStatus
       }

   marsClientIndex OBJECT-TYPE
       SYNTAX  Integer32(1..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The auxiliary variable used to identify instances of
            the columnar objects in the MARS MarsClientTable."
       ::= { marsClientEntry 1 }

   marsClientAddr OBJECT-TYPE
       SYNTAX  AtmAddr
          MAX-ACCESS read-create
          STATUS  current
          DESCRIPTION
              "The ATM address associated with the ATM Client."
          ::= { marsClientEntry 2 }

   marsClientDefaultMarsAddr OBJECT-TYPE
       SYNTAX  AtmAddr
          MAX-ACCESS read-create
          STATUS  current
          DESCRIPTION
              "The default MARS ATM address which is needed to
               setup the initial signalling path between a MARS
               client and its associated MARS."
          ::= { marsClientEntry 3 }

   marsClientHsn OBJECT-TYPE
       SYNTAX  Unsigned32
       MAX-ACCESS read-create
          STATUS  current
          DESCRIPTION
              "The cluster membership own 32 bit Host Sequence
               Number.  When a new cluster member starts up, it is
               initialized to zero.  When the cluster member sends
               the MARS_JOIN to register, the HSN will be correctly
               set to the current cluster sequence number (CSN) when
               the Client receives the copy of its MARS_JOIN from
               the MARS.  It is is used to track the MARS sequence
               number."
          ::= { marsClientEntry 4 }

   marsClientRegistration OBJECT-TYPE
       SYNTAX  INTEGER {
             notRegistered (1),





             registering (2),
             registered (3),
             reRegisteringFault (4),
             reRegisteringRedirMap (5)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "An indication with regards to the registration
            status of this client. The registration codes
            of 'notRegistered (1)', 'registered (2)', and
            registered (3) are self-explanatory. The
            'reRegisteringFault (4)' indicates the client is
            in the process of re-registering with a MARS due
            to some fault conditions.  The 'reRegisteringRedMap
            (5)' status code shows that client is re-registering
            because it has received a MARS_REDIRECT_MAP message
            and was told to register with a different MARS from
            the current MARS."
       ::= { marsClientEntry 5 }

   marsClientCmi OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "16 bit Cluster member identifier (CMI) assigned by the
            MARS which uniquely identifies each endpoint attached
            to the cluster.  The value becomes valid after the
            'marsClientRegistration' is set to the value
            of 'registered (1)'."
       ::= { marsClientEntry 6 }

   marsClientDefaultMtu OBJECT-TYPE
       SYNTAX  INTEGER (1..65535)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The default maximum transmission unit (MTU) used for
            this cluster.  Note that the actual size used for a
            VC between two members of the cluster may be negotiated
            during connection setup and may be different than this
            value.  Default value = 9180 bytes."
       DEFVAL { 9180 }
       ::= { marsClientEntry 7 }

   marsClientFailureTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)





       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "A timer used to flag the failure of last MARS_MULTI
            to arrive.  Default value = 10 seconds (recommended)."
       DEFVAL { 10 }
       ::= { marsClientEntry 8 }

   marsClientRetranDelayTimer OBJECT-TYPE
       SYNTAX  INTEGER (5..10)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The delay timer for sending out new MARS_REQUEST
            for the group after the client learned that there
            is no other group in the cluster.  The timer must
            be set between 5 and 10 seconds inclusive."
       ::= { marsClientEntry 9 }

   marsClientRdmMulReqAddRetrTimer OBJECT-TYPE
       SYNTAX  INTEGER (5..10)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The initial random L_MULTI_RQ/ADD retransmit timer
            which can be set between 5 and 10 seconds inclusive."
       ::= { marsClientEntry 10 }

   marsClientRdmVcRevalidateTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..10)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The random time to set VC_revalidate flag.  The
            timer value ranges between 1 and 10 seconds
            inclusive."
       ::= { marsClientEntry 11 }

   marsClientJoinLeaveRetrInterval OBJECT-TYPE
       SYNTAX  INTEGER(5..2147483647)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION





           "MARS_JOIN/LEAVE retransmit interval. The minimum
            and recommended values are 5 and 10 seconds,
            respectively."
       DEFVAL { 10 }
       ::= { marsClientEntry 12 }

   marsClientJoinLeaveRetrLimit OBJECT-TYPE
       SYNTAX  INTEGER (0..5)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "MARS_JOIN/LEAVE retransmit limit. The maximum
            value is 5."
       ::= { marsClientEntry 13 }

   marsClientRegWithMarsRdmTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..10)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Random time to register with MARS."
       ::= { marsClientEntry 14 }

   marsClientForceWaitTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)
       UNITS   "minutes"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Force wait if MARS re-registration is looping.
            The minimum value is 1 minute."
       ::= { marsClientEntry 15 }

   marsClientLmtToMissRedirMapTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..4)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Timer limit for client to miss MARS_REDIRECT_MAPS."
       ::= { marsClientEntry 16 }

   marsClientIdleTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)
       UNITS   "minutes"
       MAX-ACCESS read-create
       STATUS  current





       DESCRIPTION


           "The configurable inactivity timer associated with a
            client. When a VC is created at this client, it gets
            the idle timer value from this configurable timer.
            The minimum suggested value is 1 minute and the
            recommended default value is 20 minutes."
       DEFVAL { 20 }
       ::= { marsClientEntry 17 }

   marsClientRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.

            A row cannot be made 'active' until instances of
            all corresponding columns in the row of this table
            are appropriately configured and until the agent
            has also created a corresponding row in the
            marsClientStatTable.

            When this object has a value of 'active', the
            following columnar objects can not be modified:

              marsClientDefaultMarsAddr,
              marsClientHsn,
              marsClientRegstration,
              marsClientCmi,
              marsClientDefaultMtu

            while other objects in this conceptual row can be
            modified irrespective of the value of this object.

            Deletion of this row is allowed regardless of
            whether or not a row in any associated tables
            (i.e., marsClientVcTable) still exists or is in
            use. Once this row is deleted, it is recommended
            that the agent or the SNMP management station
            (if possible) through the set command deletes
            any stale rows that are associated with this
            row."
       ::= { marsClientEntry 18 }

   --****************************************************************





   -- IP ATM MARS Client Multicast Group Address Object Definitions
   --****************************************************************

   marsClientMcGrpTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsClientMcGrpEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains a list of IP multicast group address
            blocks associated with a MARS client.  Entries in this
            table are used by the client that needs to receive or
            transmit packets from/to the specified range of
            multicast addresses.
            Each row can be created or deleted via configuration."
       ::= {  marsClientObjects 2 }

   marsClientMcGrpEntry OBJECT-TYPE
       SYNTAX  MarsClientMcGrpEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry represents a consecutive block of multicast
            group addresses."
       INDEX { ipAdEntAddr,
               marsClientIndex,
               marsClientMcMinGrpAddr,
               marsClientMcMaxGrpAddr }
       ::= { marsClientMcGrpTable 1 }

   MarsClientMcGrpEntry ::=
       SEQUENCE {
           marsClientMcMinGrpAddr           IpAddress,
           marsClientMcMaxGrpAddr           IpAddress,
           marsClientMcGrpRowStatus         RowStatus
       }

   marsClientMcMinGrpAddr OBJECT-TYPE
       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Minimum multicast group address - the min and max
            multicast forms multi-group block.  If the MinGrpAddr
            and MaxGrpAddr are the same, it indicates that this
            block contains a single group address."
       ::= { marsClientMcGrpEntry 1 }

   marsClientMcMaxGrpAddr OBJECT-TYPE





       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Maximum multicast group address - the min and max
            multicast forms a multi-group block.  If the MinGrpAddr
            and MaxGrpAddr are the same, it indicates that this
            block contains a single group address."
       ::= { marsClientMcGrpEntry 2 }

   marsClientMcGrpRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create or delete a row in this
            table.

            Since other objects in this row are not-accessible
            'index-objects', the value of this object has no
            effect on whether those objects in this conceptual
            row can be modified."
       ::= { marsClientMcGrpEntry 3 }

   --****************************************************************
   -- IP ATM MARS Client Backup MARS Object Definitions
   --****************************************************************

   marsClientBackupMarsTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsClientBackupMarsEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains a list of backup MARS addresses that
            a client can connect to in case of failure for connecting
            to the primary server. The list of addresses is in
            descending order of preference. It should be noted that
            the backup list provided by the MARS to the client via
            the MARS_REDIRECT_MAP message has a higher preference than
            addresses that are manually configured into the client.
            When such a list is received from the MARS, this information
            should be inserted at the top of the list.
            Each row can be created or deleted via configuration."
       ::= {  marsClientObjects 3 }

   marsClientBackupMarsEntry OBJECT-TYPE
       SYNTAX  MarsClientBackupMarsEntry
       MAX-ACCESS not-accessible





       STATUS  current
       DESCRIPTION
           "Each entry represents an ATM address of a backup MARS."
       INDEX { ipAdEntAddr,
               marsClientIndex,
               marsClientBackupMarsPriority,
               marsClientBackupMarsAddr }
       ::= { marsClientBackupMarsTable 1 }

   MarsClientBackupMarsEntry ::=
       SEQUENCE {
           marsClientBackupMarsPriority     Unsigned32,
           marsClientBackupMarsAddr         AtmAddr,
           marsClientBackupMarsRowStatus    RowStatus
       }

   marsClientBackupMarsPriority OBJECT-TYPE
       SYNTAX  Unsigned32(0..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The priority associated with a backup MARS. A lower
            priority value inidcates a higher preference."
       ::= { marsClientBackupMarsEntry 1 }

   marsClientBackupMarsAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The ATM address associated with a backup MARS."
       ::= { marsClientBackupMarsEntry 2 }

   marsClientBackupMarsRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create or delete a row in this
            table.

            Since other objects in this row are not-accessible
            'index-objects', the value of this object has no effect
            on whether those objects in this conceptual row can be
            modified."
       ::= { marsClientBackupMarsEntry 3 }

   --***************************************************************





   --  IP ATM MARS Client VC Object Definition Table
   --***************************************************************

   marsClientVcTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsClientVcEntry
       MAX-ACCESS  not-accessible
       STATUS current
       DESCRIPTION
           "This table contains information about open virtual
            circuits (VCs) that a client has.  For point to point
            circuit, each entry represents a single VC connection
            between this client ATM address to another party ATM
            address.  In the case of point to multipoint connection
            where a single source address is associated with
            multiple destinations, several entries are used to
            represent the relationship.  An example of point to
            multi-point VC represented in a table is shown below.

                   Client    VPI/VCI    Grp Addr1/Addr2    Part Addr
                     1         0,1          g1,g2             p1
                     1         0,1          g1,g2             p2
                     1         0,1          g1,g2             p3

            Note:  This table assumes the IP multicast address
                   groups (min, max) defined in each entry are
                   always consecutive.  In the case of that a
                   client receives a JOIN/LEAVE with
                   mars$flag.punched set, each pair of the IP
                   groups will first be broken into several
                   pairs of consecutive IP groups before each
                   entry row corresponding to a pair of IP group
                   is created."
       ::= { marsClientObjects 4 }

   marsClientVcEntry OBJECT-TYPE
       SYNTAX  MarsClientVcEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The objects contained in the entry are VC related
            attributes such as VC signalling type, control VC
            type, idle timer, negotiated MTU size, etc."
       INDEX { ipAdEntAddr,
               marsClientIndex,
               marsClientVcVpi,
               marsClientVcVci,
               marsClientVcMinGrpAddr,
               marsClientVcMaxGrpAddr,





               marsClientVcPartyAddr }
       ::= { marsClientVcTable 1 }

   MarsClientVcEntry ::=
       SEQUENCE {
           marsClientVcVpi            INTEGER,
           marsClientVcVci            INTEGER,
           marsClientVcMinGrpAddr     IpAddress,
           marsClientVcMaxGrpAddr     IpAddress,
           marsClientVcPartyAddr      AtmAddr,
           marsClientVcPartyAddrType  INTEGER,
           marsClientVcType           INTEGER,
           marsClientVcCtrlType       INTEGER,
           marsClientVcIdleTimer      INTEGER,
           marsClientVcRevalidate     TruthValue,
           marsClientVcEncapsType     INTEGER,
           marsClientVcNegotiatedMtu  INTEGER,
           marsClientVcRowStatus      RowStatus
       }

   marsClientVcVpi OBJECT-TYPE
       SYNTAX  INTEGER (0..4095)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The value of virtual path identifier (VPI). Since
            a VPI can be numbered 0, this sub-index can take
            a value of 0."
       ::= { marsClientVcEntry 1 }

   marsClientVcVci OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The value of virtual circuit identifier (VCI). Since
            a VCI can be numbered 0, this sub-index can take
            a value of 0."
       ::= { marsClientVcEntry 2 }

   marsClientVcMinGrpAddr OBJECT-TYPE
       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Minimum IP multicast group address - the min and
            max multicast forms a multi-group consecutive
            block which is associated with a table entry.





            if the MinGrpAddr and MaxGrpAddr are the same, it
            indicates that the size of multi-group block is 1,
            a single IP group."
       ::= { marsClientVcEntry 3 }

   marsClientVcMaxGrpAddr OBJECT-TYPE
       SYNTAX  IpAddress


       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Maximum IP multicast group address - the min and
            max multicast forms a multi-group consecutive
            block which is associated with a table entry.
            if the MinGrpAddr and MaxGrpAddr are the same, it
            indicates that the size of multi-group block is 1,
            a single IP group."
       ::= { marsClientVcEntry 4 }

   marsClientVcPartyAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "An ATM party address in which this VC is linked.
            The party type is identified by the
            marsClientVcPartyAddrType."
       ::= { marsClientVcEntry 5 }

   marsClientVcPartyAddrType OBJECT-TYPE
       SYNTAX  INTEGER {
             called (1),
             calling (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The party type is associated with the party address.
            The 'called (1)' indicates that the party address is
            a destination address which implies that VC is
            originated from this client.  The 'calling (2)'
            indicates the VC was initiated externally to this
            client. In this case, the party address is the
            source address."
       ::= { marsClientVcEntry 6 }

   marsClientVcType OBJECT-TYPE





       SYNTAX  INTEGER {
             pvc (1),
             svc (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Circuit Connection type: permanent virtual circuit or
            switched virtual circuit."
       ::= { marsClientVcEntry 7 }

   marsClientVcCtrlType OBJECT-TYPE
       SYNTAX  INTEGER {
              pointToPointVC (1),
              clusterControlVC (2),
              pointToMultiPointVC (3)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Control VC type used to specify a particular connection.
              pointToPointVC (1):
                used by the ATM Clients for the registration and
                queries.  This VC or the initial signalling path
                is set up from the source Client to a MARS. It is
                bi-directional.
              clusterControlVC (2):
                used by a MARS to issue asynchronous updates to an
                ATM Client.  This VC is established from the MARS
                to the ATM Client.
              pointToMultiPointVC (3):
                used by the client to transfer multicast data
                packets from layer 3.  This VC is established
                from the source ATM Client to a destination ATM
                endpoint which can be a multicast group member
                or an MCS.  The destination endpoint was obtained
                from the MARS."
       ::= { marsClientVcEntry 8 }

   marsClientVcIdleTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)
       UNITS   "minutes"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The idle timer associated with this VC.  The minimum
            suggested value is 1 minute and the recommended
            default value is 20 minutes."





       DEFVAL { 20 }
       ::= { marsClientVcEntry 9 }

   marsClientVcRevalidate OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "A flag associated with an open and active multipoint
            VC.  It is checked every time a packet is queued for
            transmission on that VC. The object has the value of
            true (1) if revalidate is required and the value
            false (2) otherwise."
       ::= { marsClientVcEntry 10 }

    marsClientVcEncapsType OBJECT-TYPE
       SYNTAX  INTEGER {
             other (1),
             llcSnap (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The encapsulation type used when communicating over
            this VC."
       ::= { marsClientVcEntry 11 }

   marsClientVcNegotiatedMtu OBJECT-TYPE
       SYNTAX  INTEGER (1..65535)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The negotiated MTU when communicating over this VC."
       ::= { marsClientVcEntry 12 }

   marsClientVcRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.

            A row cannot be made 'active' until instances of
            all corresponding columns in the row of this table
            are appropriately configured.

            While objects: marsClientVcIdleTimer and





            marsClientVcRevalidate in this conceptual
            row can be modified irrespective of the value
            of this object, all other objects in the row can
            not be modified when this object has a value
            of 'active'.

            It is possible for an SNMP management station
            to set the row to 'notInService' and modify
            the entry and then set it back to 'active'

            with the following exception. That is, rows
            for which the corresponding instance of
            marsClientVcType has a value of 'svc' can not
            be modified or deleted."
       ::= { marsClientVcEntry 13 }

   --***************************************************************
   --  IP ATM MARS Client Statistic Object Definition Table
   --***************************************************************

   marsClientStatTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsClientStatEntry
       MAX-ACCESS  not-accessible
       STATUS current
       DESCRIPTION
           "The table contains statistics collected at MARS
            clients."
       ::= { marsClientObjects 5 }

   marsClientStatEntry OBJECT-TYPE
       SYNTAX  MarsClientStatEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry contains statistics collected at one MARS
            client."
       INDEX { ipAdEntAddr, marsClientIndex }
       ::= { marsClientStatTable 1 }

   MarsClientStatEntry ::=
       SEQUENCE {
           marsClientStatTxReqMsgs        Counter32,
           marsClientStatTxJoinMsgs       Counter32,
           marsClientStatTxLeaveMsgs      Counter32,
           marsClientStatTxGrpLstReqMsgs  Counter32,
           marsClientStatRxJoinMsgs       Counter32,
           marsClientStatRxLeaveMsgs      Counter32,
           marsClientStatRxMultiMsgs      Counter32,





           marsClientStatRxNakMsgs        Counter32,
           marsClientStatRxMigrateMsgs    Counter32,
           marsClientStatRxGrpLstRplyMsgs Counter32,
           marsClientStatFailMultiMsgs    Counter32
       }

   marsClientStatTxReqMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_REQUEST messages transmitted
            from a client."
       ::= { marsClientStatEntry 1 }

   marsClientStatTxJoinMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_JOIN messages transmitted from
            a client."
       ::= { marsClientStatEntry 2 }

   marsClientStatTxLeaveMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_LEAVE messages transmitted from
            a client."
       ::= { marsClientStatEntry 3 }

   marsClientStatTxGrpLstReqMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_GROUPLIST_REQUEST messages
            transmitted from a client."
       ::= { marsClientStatEntry 4 }

   marsClientStatRxJoinMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_JOIN messages received by





            a client."
       ::= { marsClientStatEntry 5 }

   marsClientStatRxLeaveMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_LEAVE messages received by
            a client."
       ::= { marsClientStatEntry 6 }

   marsClientStatRxMultiMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MULTI messages received by
            a client."
       ::= { marsClientStatEntry 7 }

   marsClientStatRxNakMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_NAK messages received by
            a client."
       ::= { marsClientStatEntry 8 }

   marsClientStatRxMigrateMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MIGRATE messages received by
            a client."
       ::= { marsClientStatEntry 9 }

       marsClientStatRxGrpLstRplyMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_GROUPLIST_REPLY messages
            received by a client."
       ::= { marsClientStatEntry 10 }






   marsClientStatFailMultiMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of timeouts occurred indicating
            failure of the last MARS_MULTI to arrive."
       ::= { marsClientStatEntry 11 }

   --***************************************************************
   --  IP ATM MARS Object Definitions
   --***************************************************************

   marsObjects    OBJECT IDENTIFIER ::= { marsMIB 2 }

   marsTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsEntry
       MAX-ACCESS  not-accessible
       STATUS current
       DESCRIPTION
           "The objects defined in this table are used for the
            management of MARS servers."
       ::= {  marsObjects 1 }

   marsEntry OBJECT-TYPE
       SYNTAX  MarsEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry contains a MARS and its associated
            attributes."
       INDEX { marsIndex, marsIfIndex }
       ::= { marsTable 1 }

   MarsEntry ::=
       SEQUENCE {
           marsIndex              Integer32,
           marsIfIndex            InterfaceIndex,
           marsAddr               AtmAddr,
           marsLocal              TruthValue,
           marsServStatus         INTEGER,
           marsServType           INTEGER,
           marsServPriority       Unsigned32,
           marsRedirMapMsgTimer   INTEGER,
           marsCsn                Unsigned32,
           marsSsn                Unsigned32,
           marsRowStatus          RowStatus
       }





   marsIndex OBJECT-TYPE
       SYNTAX  Integer32(1..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The auxiliary variable used to identify instances of
            the columnar objects in the MARS table."
       ::= { marsEntry 1 }

   marsIfIndex OBJECT-TYPE
       SYNTAX  InterfaceIndex
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The ifIndex of the interface that the MARS is
            associated with."
       ::= { marsEntry 2 }

   marsAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The ATM address associated with the MARS."
       ::= { marsEntry 3 }

   marsLocal OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "A flag associated with a MARS entry.  The object has
            the value of true (1) if the MARS whose interface
            is local to the machine that implements this MIB;
            otherwise the object has the value of false (2)."
       ::= { marsEntry 4 }

   marsServStatus OBJECT-TYPE
       SYNTAX  INTEGER {
             active (1),
             inactive (2),
             faulted (3)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The current status of MARS."
       ::= { marsEntry 5 }





   marsServType OBJECT-TYPE
       SYNTAX  INTEGER {
             primary (1),
             backup (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Types of MARS servers: primary or backup."
       ::= { marsEntry 6 }

   marsServPriority OBJECT-TYPE
       SYNTAX  Unsigned32(0..65535)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Priority associated with a backup MARS server.
            A backup MARS server with lower priority value
            indicates a higher preference than other backup
            MARS servers to be used as the MARS server when
            the primary server fails."
       ::= { marsEntry 7 }

   marsRedirMapMsgTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2)
       UNITS   "minutes"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Periodic interval on which a multi-part
            MARS_REDIRECT_MAP is sent from this MARS."
          DEFVAL { 1 }
       ::= { marsEntry 8 }

   marsCsn OBJECT-TYPE
       SYNTAX  Unsigned32
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Current cluster sequence number (CSN) which is global
            within the context of a given protocol.  The CSN is
            incremented by the MARS on every transmission of a
            message on ClusterControlVC.  A cluster member uses
            the CSN to track the message loss on ClusterControlVC
            or to monitor a membership change."
       ::= { marsEntry 9 }

   marsSsn OBJECT-TYPE





       SYNTAX  Unsigned32
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Current server sequence number (SSN) which is global
            within the context of a given protocol.  The SSN is
            incremented by the MARS on every transmission of a
            message on ServerControlVC.  A MCS uses the SSN to
            track the message loss on ServerControlVC or to
            monitor a membership change."
       ::= { marsEntry 10 }

   marsRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.

            A row cannot be made 'active' until instances of
            all corresponding columns in the row of this table
            are appropriately configured and until the agent
            has also created a corresponding row in the
            marsStatTable.

            When this object has a value of 'active', the
            following columnar objects can not be modified:

              marsAddr,
              marsAddrLocal,
              marsServStatus,
              marsServType,
              marsCsn,
              marsSsn

            while other objects in this conceptual row can be
            modified irrespective of the value of this object.

            Deletion of this row is allowed regardless of
            whether or not a row in any associated tables
            (i.e., marsVcTable) still exists or is in use.
            Once this row is deleted, it is recommended that
            the agent or the SNMP management station (if
            possible) through the set command deletes any
            stale rows that are associated with this row."
       ::= { marsEntry 11 }






   --****************************************************************
   -- IP ATM MARS Multicast Group Address Object Definitions
   --****************************************************************

   marsMcGrpTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsMcGrpEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains a list of IP multicast address
            blocks associated with a MARS.  Entries in this table
            are used by the MARS host map table and the server map
            table.  They should be created prior to being referenced
            as indices by those tables.
            Each row can be created or deleted via configuration."
       ::= { marsObjects 2 }

   marsMcGrpEntry OBJECT-TYPE
       SYNTAX  MarsMcGrpEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry represents a consecutive block of multicast
            group addresses."
       INDEX { marsIndex,
               marsIfIndex,
               marsMcMinGrpAddr,
               marsMcMaxGrpAddr }
       ::= { marsMcGrpTable 1 }

   MarsMcGrpEntry ::=
       SEQUENCE {
           marsMcMinGrpAddr           IpAddress,
           marsMcMaxGrpAddr           IpAddress,
           marsMcGrpAddrUsage         INTEGER,
           marsMcGrpRxLayer3GrpSets   Counter32,
           marsMcGrpRxLayer3GrpResets Counter32,
           marsMcGrpRowStatus         RowStatus
       }

   marsMcMinGrpAddr OBJECT-TYPE
       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Minimum multicast group address - the min and max
            multicast forms multi-group block.  If the MinGrpAddr
            and MaxGrpAddr are the same, it indicates that this





            block contains a single group address."
       ::= { marsMcGrpEntry 1 }

   marsMcMaxGrpAddr OBJECT-TYPE
       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Maximum multicast group address - the min and max
            multicast forms a multi-group block.  If The
            MinGrpAddr and MaxGrpAddr are the same, it indicates
            that this block contains a single group address."
       ::= { marsMcGrpEntry 2 }

   marsMcGrpAddrUsage OBJECT-TYPE
       SYNTAX  INTEGER {
             hostMap (1),
             serverMap (2),
             hostServerMap (3)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Usage of the multicast address block.  The hostMap (1)
            indicates that the address block is only used in the
            MARS host map table. The serverMap (2) indicates
            that the address block is only used in the MARS
            server map table.  The hostServerMap (3) indicates
            that the address block is used in both the host map
            and the server map tables."
       ::= { marsMcGrpEntry 3 }

   marsMcGrpRxLayer3GrpSets OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Number of MARS_JOIN messages received with
            mars$flags.layer3grp flag set."
       ::= { marsMcGrpEntry 4 }

   marsMcGrpRxLayer3GrpResets OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Number of MARS_JOIN messages received with
            mars$flags.layer3grp flag reset."





       ::= { marsMcGrpEntry 5 }

   marsMcGrpRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.

            The value of this object has no effect on whether
            other objects in this conceptual row can be modified."
       ::= { marsMcGrpEntry 6 }

   --***************************************************************
   --  IP ATM MARS Host Map Object Definitions
   --***************************************************************

   marsHostMapTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsHostMapEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table caches mappings between IP multicast
            address to a list of ATM addresses that are
            configured or dynamically learned from the MARS.
            This address resolution is used for the host map.
            It supports the mapping of a block of multicast
            group addresses to a cluster member address.  In
            the case where a group block is associated with
            multiple cluster members, several entries are
            used to representing the relationship."
       ::= { marsObjects 3 }

   marsHostMapEntry OBJECT-TYPE
       SYNTAX  MarsHostMapEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry row contains attributes associated with
            the mapping between a multicast group block and an
            ATM address."
       INDEX { marsIndex,
               marsIfIndex,
               marsMcMinGrpAddr,
               marsMcMaxGrpAddr,
               marsHostMapAtmAddr }
       ::= { marsHostMapTable 1 }





   MarsHostMapEntry ::=
       SEQUENCE {
           marsHostMapAtmAddr     AtmAddr,
           marsHostMapRowType     INTEGER,
           marsHostMapRowStatus   RowStatus
       }

   marsHostMapAtmAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The mapped cluster member ATM address."
       ::= { marsHostMapEntry 1 }

   marsHostMapRowType OBJECT-TYPE
       SYNTAX  INTEGER {
             static (1),
             dynamic (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Method in which this entry row is created. The
            static (1) indicates that this row is created
            through configuration.  The dynamic (2) indicates
            that the row is created as the result of group
            address updates received at this MARS."
       ::= { marsHostMapEntry 2 }

   marsHostMapRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.

            This object must not be set to 'active' until
            instances of all corresponding columns in the
            row of this table are appropriately configured.

            It is possible for an SNMP management station
            to set the row to 'notInService' and modify
            the entry and then set it back to 'active'
            with the following exception. That is, rows
            for which the corresponding instance of
            marsHostMapRowType has a value of 'dynamic'





            can not be modified or deleted."
       ::= { marsHostMapEntry 3 }

   --***************************************************************
   --  IP ATM MARS Server Map Object Definitions
   --***************************************************************

   marsServerMapTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsServerMapEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table caches mappings between IP multicast
            address to a list of MCS ATM addresses that are
            configured or dynamically learned from the MARS.
            This address resolution is used for the server map.
            It supports the mapping of a block of multicast
            group addresses to a MCS address.  In the case
            where a group block is associated with multiple
            MCSs, several entries are used to representing the
            relationship."
       ::= { marsObjects 4 }

   marsServerMapEntry OBJECT-TYPE
       SYNTAX  MarsServerMapEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry row contains attributes associated with
            the mapping between a multicast group block and an
            MCS address."
       INDEX { marsIndex,
               marsIfIndex,
               marsMcMinGrpAddr,
               marsMcMaxGrpAddr,
               marsServerMapAtmAddr }
       ::= { marsServerMapTable 1 }

   MarsServerMapEntry ::=
       SEQUENCE {
           marsServerMapAtmAddr   AtmAddr,
           marsServerMapRowType   INTEGER,
           marsServerMapRowStatus RowStatus
       }

   marsServerMapAtmAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS not-accessible





       STATUS  current
       DESCRIPTION
           "The mapped MCS ATM address."
       ::= { marsServerMapEntry 1 }

   marsServerMapRowType OBJECT-TYPE
       SYNTAX  INTEGER {
               static (1),
               dynamic (2)
             }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Method in which this entry row is created. The
            'static (1)' indicates that this row is created
            through configuration.  The 'dynamic (2)' indicates
            that the row is created as the result of group
            address updates received at this MARS."
       ::= { marsServerMapEntry 2 }

   marsServerMapRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.

            This object must not be set to 'active' until
            instances of all corresponding columns in the
            row of this table are appropriately configured.

            It is possible for an SNMP management station
            to set the row to 'notInService' and modify
            the entry and then set it back to 'active'
            with the following exception. That is, rows
            for which the corresponding instance of
            marsServerMapRowType has a value of 'dynamic'
            can not be modified or deleted."
       ::= { marsServerMapEntry 3 }

   --***************************************************************
   --  IP ATM MARS VC Object Definition Table
   --***************************************************************

   marsVcTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsVcEntry
       MAX-ACCESS  not-accessible





       STATUS current
       DESCRIPTION
           "This table contains information about open virtual circuits
            (VCs) that a MARS has.  For point to point circuit, each
            entry represents a single VC connection between this MARS
            ATM address to another party's ATM address.  In the case of
            point to multipoint connection where a ControlVc is attached
            with multiple leaf nodes, several entries are used  to
            represent the relationship.  An example of point to
            multi-point VC represented in a table is shown below.

                 MARS     VPI/VCI    MARS Addr     Party Addr
                   1         0,1         m1            p1
                   1         0,1         m1            p2
                   1         0,1         m1            p3"
       ::= { marsObjects 5 }

   marsVcEntry OBJECT-TYPE
       SYNTAX  MarsVcEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The objects contained in the entry are VC related attributes
            such as VC signalling type, control VC type, idle timer,
            negotiated MTU size, etc."
       INDEX { marsIndex,
               marsIfIndex,
               marsVcVpi,
               marsVcVci,
               marsVcPartyAddr }
       ::= { marsVcTable 1 }

   MarsVcEntry ::=
       SEQUENCE {
           marsVcVpi              INTEGER,
           marsVcVci              INTEGER,
           marsVcPartyAddr        AtmAddr,
           marsVcPartyAddrType    INTEGER,
           marsVcType             INTEGER,
           marsVcCtrlType         INTEGER,
           marsVcIdleTimer        INTEGER,
           marsVcCmi              INTEGER,
           marsVcEncapsType       INTEGER,
           marsVcNegotiatedMtu    INTEGER,
           marsVcRowStatus        RowStatus
         }

   marsVcVpi OBJECT-TYPE





       SYNTAX  INTEGER (0..4095)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The value of virtual path identifier (VPI). Since
            a VPI can be numbered 0, this sub-index can take
            a value of 0."
       ::= { marsVcEntry 1 }

   marsVcVci OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
            "The value of virtual circuit identifier (VCI).
             Since a VCI can be numbered 0, this sub-index
             can take a value of 0."
       ::= { marsVcEntry 2 }

   marsVcPartyAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "An ATM party address in which this VC is linked. The
            party type is identified by the marsVcPartyAddrType."
       ::= { marsVcEntry 5 }

   marsVcPartyAddrType OBJECT-TYPE
       SYNTAX  INTEGER {
             called (1),
             calling (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The party type is associated with the party address.  The
            'called (1)' indicates that the party address is a
            destination address which implies that VC is originated
            from this MARS. The 'calling (2)' indicates the VC was
            initiated externally to this MARS.  The party address is
            the source address."
       ::= { marsVcEntry 6 }

   marsVcType OBJECT-TYPE
       SYNTAX  INTEGER {
                pvc (1),
                svc (2)





              }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Circuit Connection type: permanent virtual circuit or
            switched virtual circuit."
       ::= { marsVcEntry 7 }

   marsVcCtrlType OBJECT-TYPE
       SYNTAX  INTEGER {
              pointToPointVC (1),
              clusterControlVC (2),
              serverControlVC (3)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Control VC type used to specify a particular connection.
              pointToPointVC (1):
                used by the ATM endpoints (clients) or the MCS for
                registration and queries.  This VC is set up from
                a MARS client and MCS to this MARS.  It is a
                bi-directional VC.
              clusterControlVC (2):
                used by MARS to issue asynchronous updates to ATM
                an ATM client.  This VC is established from the
                MARs to the ATM client.
              serverControlVC (3):
                used by MARS to issue asynchronous update to ATM
                multicast servers.  This type of VC exists when at
                least a MCS is being used."
       ::= { marsVcEntry 8 }

   marsVcIdleTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)
       UNITS   "minutes"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The idle timer associated with this VC.  The minimum
            suggested value is 1 minute and the recommended default
            value is 20 minutes."
       DEFVAL { 20 }
       ::= { marsVcEntry 9 }

   marsVcCmi OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       MAX-ACCESS read-create





       STATUS  current
       DESCRIPTION
           "Cluster member identifier (CMI) which uniquely identifies
            each endpoint attached to the cluster.  This variable
            applies to each 'leaf node' of an outgoing control VC."
       ::= { marsVcEntry 10 }

   marsVcEncapsType OBJECT-TYPE
       SYNTAX  INTEGER {
             other (1),
             llcSnap (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The encapsulation type used when communicating over
            this VC."
       ::= { marsVcEntry 11 }

   marsVcNegotiatedMtu OBJECT-TYPE
       SYNTAX  INTEGER (1..65535)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The negotiated MTU when communicating over this VC."
       ::= { marsVcEntry 12 }

   marsVcRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.

            A row cannot be made 'active' until instances of
            all corresponding columns in the row of this table
            are appropriately configured.

            While the marsVcIdleTimer in this conceptual
            row can be modified irrespective of the value
            of this object, all other objects in the row can
            not be modified when this object has a value
            of 'active'.

            It is possible for an SNMP management station
            to set the row to 'notInService' and modify
            the entry and then set it back to 'active'





            with the following exception. That is, rows
            for which the corresponding instance of
            marsVcType has a value of 'svc' can not be
            modified or deleted."
       ::= { marsVcEntry 13 }

   --***************************************************************
   --  IP ATM MARS Registered Cluster Member List Table
   --***************************************************************

   marsRegClientTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsRegClientEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains ATM identities of all the currently
            registered cluster members at a MARS.  Each entry represents
            one set of ATM identities associated with one cluster member
            or the MARS client."
       ::= { marsObjects 6 }

   marsRegClientEntry OBJECT-TYPE
       SYNTAX  MarsRegClientEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry row contains attributes associated with one
            register cluster member."
       INDEX { marsIndex,
               marsIfIndex,
               marsRegClientCmi}
       ::= { marsRegClientTable 1 }

   MarsRegClientEntry ::=
       SEQUENCE {
           marsRegClientCmi       INTEGER,
           marsRegClientAtmAddr   AtmAddr
       }

   marsRegClientCmi OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "This cluster member identifier is used as an auxiliary index
            for the entry in this table."
       ::= { marsRegClientEntry 1 }






   marsRegClientAtmAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "The registered client's ATM address."
       ::= { marsRegClientEntry 2 }


   --***************************************************************
   --  IP ATM MARS Registered Server Member List Table
   --***************************************************************

   marsRegMcsTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsRegMcsEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains ATM identities of all the currently
            registered MCSs at a MARS. Each entry represents one set
            of ATM identities associated with one MCS."
       ::= { marsObjects 7 }

   marsRegMcsEntry OBJECT-TYPE
       SYNTAX  MarsRegMcsEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry row contains attributes associated with one
            registered MCS."
       INDEX { marsIndex,
               marsIfIndex,
               marsRegMcsAtmAddr
             }
       ::= { marsRegMcsTable 1 }

   MarsRegMcsEntry ::=
       SEQUENCE {
           marsRegMcsAtmAddr  AtmAddr
       }

   marsRegMcsAtmAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "The registered MCS's ATM address."
       ::= { marsRegMcsEntry 1 }





   --***************************************************************
   --  IP ATM MARS Statistics Object Definition Table
   --***************************************************************

   marsStatTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsStatEntry
       MAX-ACCESS not-accessible
       STATUS current


       DESCRIPTION
           "The table contains statistics collected at MARS."
       ::= {  marsObjects 8 }

   marsStatEntry OBJECT-TYPE
       SYNTAX  MarsStatEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry contains statistics collected at one MARS."
       INDEX { marsIndex, marsIfIndex }
       ::= { marsStatTable 1 }

   MarsStatEntry ::=
       SEQUENCE {
           marsStatTxMultiMsgs        Counter32,
           marsStatTxGrpLstRplyMsgs   Counter32,
           marsStatTxRedirectMapMsgs  Counter32,
           marsStatTxMigrateMsgs      Counter32,
           marsStatTxNakMsgs          Counter32,
           marsStatTxJoinMsgs         Counter32,
           marsStatTxLeaveMsgs        Counter32,
           marsStatTxSjoinMsgs        Counter32,
           marsStatTxSleaveMsgs       Counter32,
           marsStatTxMservMsgs        Counter32,
           marsStatTxUnservMsgs       Counter32,
           marsStatRxReqMsgs          Counter32,
           marsStatRxGrpLstReqMsgs    Counter32,
           marsStatRxJoinMsgs         Counter32,
           marsStatRxLeaveMsgs        Counter32,
           marsStatRxMservMsgs        Counter32,
           marsStatRxUnservMsgs       Counter32,
           marsStatRxBlkJoinMsgs      Counter32,
           marsStatRegMemGroups       Counter32,
           marsStatRegMcsGroups       Counter32
       }

   marsStatTxMultiMsgs OBJECT-TYPE





       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MULTI transmitted by this MARS."
       ::= { marsStatEntry 1 }

   marsStatTxGrpLstRplyMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_GROUPLIST_REPLY messages transmitted
            by this MARS."
       ::= { marsStatEntry 2 }

   marsStatTxRedirectMapMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_REDIRECT_MAP messages transmitted by
            this MARS."
       ::= { marsStatEntry 3 }

   marsStatTxMigrateMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MIGRATE messages transmitted by
            this MARS."
       ::= { marsStatEntry 4 }

   marsStatTxNakMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_NAK messages transmitted by this MARS."
       ::= { marsStatEntry 5 }

   marsStatTxJoinMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_JOIN messages transmitted by this





            MARS."
       ::= { marsStatEntry 6 }

   marsStatTxLeaveMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_LEAVE messages transmitted by this
            MARS."
       ::= { marsStatEntry 7 }

   marsStatTxSjoinMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_SJOIN messages transmitted by this
            MARS."
       ::= { marsStatEntry 8 }

   marsStatTxSleaveMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_SLEAVE messages transmitted by this
            MARS."
       ::= { marsStatEntry 9 }

   marsStatTxMservMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MSERV messages transmitted by this
            MARS."
       ::= { marsStatEntry 10 }

   marsStatTxUnservMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_UNSERV messages transmitted by this
            MARS."
       ::= { marsStatEntry 11 }






   marsStatRxReqMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_REQUEST messages received by this
            MARS."
       ::= { marsStatEntry 12 }

   marsStatRxGrpLstReqMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_GROUPLIST_REQUEST messages received
            by this MARS."
       ::= { marsStatEntry 13 }

   marsStatRxJoinMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_JOINS messages received by this MARS."
       ::= { marsStatEntry 14 }

   marsStatRxLeaveMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_LEAVES messages received by this MARS."
       ::= { marsStatEntry 15 }

   marsStatRxMservMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MSERV messages received by this MARS."
       ::= { marsStatEntry 16 }

   marsStatRxUnservMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_UNSERV messages received by this MARS."





       ::= { marsStatEntry 17 }

   marsStatRxBlkJoinMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of block joins messages received by this MARS."
       ::= { marsStatEntry 18 }

   marsStatRegMemGroups OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of IP multicast groups with 1 or more joined
            cluster members."
       ::= { marsStatEntry 19 }

   marsStatRegMcsGroups OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of IP multicast groups with 1 or more joined
            MCSs."
       ::= { marsStatEntry 20 }

   --***************************************************************
   --  IP ATM MARS MCS Object Definitions
   --***************************************************************

   marsMcsObjects OBJECT IDENTIFIER ::= { marsMIB 3 }

   marsMcsTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsMcsEntry
       MAX-ACCESS  not-accessible
       STATUS current
       DESCRIPTION
           "The objects defined in this table are used for
            the management of a multicast server (MCS)."
       ::= {  marsMcsObjects 1 }

   marsMcsEntry OBJECT-TYPE
       SYNTAX  MarsMcsEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION





           "Each entry contains a MCS and its associated
            attributes."
       INDEX { marsMcsIndex, marsMcsIfIndex }
       ::= { marsMcsTable 1 }

   MarsMcsEntry ::=
       SEQUENCE {
           marsMcsIndex                    Integer32,
           marsMcsIfIndex                  InterfaceIndex,
           marsMcsAddr                     AtmAddr,
           marsMcsDefaultMarsAddr          AtmAddr,
           marsMcsRegistration             INTEGER,
           marsMcsSsn                      Unsigned32,
           marsMcsDefaultMtu               INTEGER,
           marsMcsFailureTimer             INTEGER,
           marsMcsRetranDelayTimer         INTEGER,
           marsMcsRdmMulReqAddRetrTimer    INTEGER,
           marsMcsRdmVcRevalidateTimer     INTEGER,
           marsMcsRegisterRetrInterval     INTEGER,
           marsMcsRegisterRetrLimit        INTEGER,
           marsMcsRegWithMarsRdmTimer      INTEGER,
           marsMcsForceWaitTimer           INTEGER,
           marsMcsIdleTimer                INTEGER,
           marsMcsLmtToMissRedirMapTimer   INTEGER,
           marsMcsRowStatus                RowStatus
       }

   marsMcsIndex OBJECT-TYPE
       SYNTAX  Integer32(1..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The auxiliary variable used to identify instances
            of the columnar objects in the MCS table."
       ::= { marsMcsEntry 1 }

   marsMcsIfIndex OBJECT-TYPE
       SYNTAX  InterfaceIndex
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The ifIndex of the interface that the MCS is
            associated with."
       ::= { marsMcsEntry 2 }

   marsMcsAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS read-create





       STATUS  current
       DESCRIPTION
           "The ATM address associated with the MCS."
       ::= { marsMcsEntry 3 }

   marsMcsDefaultMarsAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The default MARS ATM address which is needed to
            setup the initial signalling path between a MCS
            and its associated MARS."
       ::= { marsMcsEntry 4 }

   marsMcsRegistration OBJECT-TYPE
       SYNTAX  INTEGER {
             notRegistered (1),
             registering (2),
             registered (3),
             reRegisteringFault (4),
             reRegisteringRedirMap (5)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "An indication with regards to the registration
            STATUS of this MCS. The registration codes of
            'notRegistered (1)', 'registered (2)', and
            registered (3) are self-explanatory. The
            'reRegisteringFault (4)' indicates the MCS is
            in the process of re-registering with a MARS due
            to some fault conditions.  The 'reRegisteringRedMap
            (5)' status code shows that MCS is re-registering
            because it has received a MARS_REDIRECT_MAP message
            and was told to register with a shift MARS."
       ::= { marsMcsEntry 5 }

   marsMcsSsn OBJECT-TYPE
       SYNTAX  Unsigned32
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The MCS own 32 bit Server Sequence Number.  It
            is used to track the Mars sequence number."
       ::= { marsMcsEntry 6 }

   marsMcsDefaultMtu OBJECT-TYPE





       SYNTAX  INTEGER (1..65535)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The default maximum transmission unit (MTU) used
            for this cluster.  Note that the actual size used
            for a VC between two members of the cluster may be
            negotiated during connection setup and may be
            different than this value.
            Default value = 9180 bytes."
       DEFVAL { 9180 }
       ::= { marsMcsEntry 7 }

   marsMcsFailureTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "A timer used to flag the failure of last MARS_MULTI
            to arrive.  Default value = 10 seconds (recommended)."
       DEFVAL { 10 }
       ::= { marsMcsEntry 8 }

   marsMcsRetranDelayTimer OBJECT-TYPE
       SYNTAX  INTEGER (5..10)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The delay timer for sending out new MARS_REQUEST
            for the group after the MCS learned that there
            is no other group in the cluster.  The timer must
            be set between 5 and 10 seconds inclusive."
       ::= { marsMcsEntry 9 }

   marsMcsRdmMulReqAddRetrTimer OBJECT-TYPE
       SYNTAX  INTEGER (5..10)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The initial random L_MULTI_RQ/ADD retransmit timer
            which can be set between 5 and 10 seconds inclusive."
       ::= { marsMcsEntry 10 }

   marsMcsRdmVcRevalidateTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..10)





       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The random time to set VC_revalidate flag.  The
            timer value ranges between 1 and 10 seconds
               inclusive."
       ::= { marsMcsEntry 11 }

   marsMcsRegisterRetrInterval OBJECT-TYPE
       SYNTAX  INTEGER(5..2147483647)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "MARS_MSERV/UNSERV retransmit interval. The minimum
            and recommended values are 5 and 10 seconds,
            respectively."
       DEFVAL { 10 }
       ::= { marsMcsEntry 12 }

   marsMcsRegisterRetrLimit OBJECT-TYPE
       SYNTAX  INTEGER (0..5)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "MARS_MSERV/UNSERV retransmit limit. The maximum value
            is 5."
       ::= { marsMcsEntry 13 }

   marsMcsRegWithMarsRdmTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..10)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Random time for a MCS to register with a MARS."
       ::= { marsMcsEntry 14 }

   marsMcsForceWaitTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)
       UNITS   "minutes"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Force wait if MARS re-registration is looping.
            The minimum value is 1 minute."
       ::= { marsMcsEntry 15 }





   marsMcsLmtToMissRedirMapTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..4)
       UNITS   "seconds"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Timer limit for MCS to miss MARS_REDIRECT_MAPS."
       ::= { marsMcsEntry 16 }

   marsMcsIdleTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)
       UNITS   "minutes"
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The configurable inactivity timer associated with a
            MCS. When a VC is created at this MCS, it gets
            the idle timer value from this configurable timer.
            The minimum suggested value is 1 minute and the
            recommended default value is 20 minutes."
       DEFVAL { 20 }
       ::= { marsMcsEntry 17 }

   marsMcsRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.

            A row cannot be made 'active' until instances of
            all corresponding columns in the row of this table
            are appropriately configured and until the agent
            has also created a corresponding row in the
            marsMcsStatTable.

            When this object has a value of 'active', the
            following columnar objects can not be modified:

              marsMcsDefaultMarsAddr,
              marsMcsSsn,
              marsMcsRegstration,
              marsMcsDefaultMtu

            while other objects in this conceptual row can be
            modified irrespective of the value of this object.






            Deletion of this row is allowed regardless of
            whether or not a row in any associated tables
            (i.e., marsMcsVcTable) still exists or is in
            use. Once this row is deleted, it is recommended
            that the agent or the SNMP management station
            (if possible) through the set command deletes
            any stale rows that are associated with this
            row."
       ::= { marsMcsEntry 18 }


   --****************************************************************
   -- IP ATM MARS MCS Multicast Group Address Object Definitions
   --****************************************************************

   marsMcsMcGrpTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsMcsMcGrpEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains a list of IP multicast group address
            blocks associated by a MARS MCS.  The MCS uses the
            information contained in list to advertise its multicast
            group service to the MARS.
            Each row can be created or deleted via configuration."
       ::= { marsMcsObjects 2 }

   marsMcsMcGrpEntry OBJECT-TYPE
       SYNTAX  MarsMcsMcGrpEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry represents a consecutive block of multicast
            group addresses."
       INDEX { marsMcsIndex,
               marsMcsIfIndex,
               marsMcsMcMinGrpAddr,
               marsMcsMcMaxGrpAddr }
       ::= { marsMcsMcGrpTable 1 }

   MarsMcsMcGrpEntry ::=
       SEQUENCE {
           marsMcsMcMinGrpAddr           IpAddress,
           marsMcsMcMaxGrpAddr           IpAddress,
           marsMcsMcGrpRowStatus         RowStatus
       }

   marsMcsMcMinGrpAddr OBJECT-TYPE





       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Minimum multicast group address - the min and max
            multicast forms multi-group block.  If the MinGrpAddr
            and MaxGrpAddr are the same, it indicates that this
            block contains a single group address.   Since the
            block joins are no allowed by a MCS as implied in
            the RFC2022, the MinGrpAddr and MaxGrpAddress should
            be set to the same value at this time when an entry
            row is created."
       ::= { marsMcsMcGrpEntry 1 }

   marsMcsMcMaxGrpAddr OBJECT-TYPE
       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Maximum multicast group address - the min and max
            multicast forms a multi-group block.  If the
            MinGrpAddr and MaxGrpAddr are the same, it indicates
            that this block contains a single group address.
            Since the block joins are no allowed by a MCS as
            implied in the RFC2022, the MinGrpAddr and
            MaxGrpAddress should be set to the same value at
            this time when an entry row is created."
       ::= { marsMcsMcGrpEntry 2 }

   marsMcsMcGrpRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create or delete a row in this
            table.

            Since other objects in this row are not-accessible
            'index-objects', the value of this object has no
            effect on whether those objects in this conceptual
            row can be modified."
       ::= { marsMcsMcGrpEntry 3 }

   --****************************************************************
   -- IP ATM MARS MCS Backup MARS Object Definitions
   --****************************************************************

   marsMcsBackupMarsTable OBJECT-TYPE





       SYNTAX  SEQUENCE OF MarsMcsBackupMarsEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "This table contains a list of backup MARS addresses that
            a MCS can make contact to in case of failure for
            connecting to the primary server. The list of addresses
            is in descending order of preference. It should be noted
            that the backup list provided by the MARS to the MCS
            via the MARS_REDIRECT_MAP message has a higher preference
            than addresses that are manually configured into the MCS.
            When such a list is received from the MARS, this information
            should be inserted at the top of the list.
            Each row can be created or deleted via configuration."
       ::= {  marsMcsObjects 3 }

   marsMcsBackupMarsEntry OBJECT-TYPE
       SYNTAX  MarsMcsBackupMarsEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry represents an ATM address of a backup MARS."
       INDEX { marsMcsIndex,
               marsMcsIfIndex,
               marsMcsBackupMarsPriority,
               marsMcsBackupMarsAddr }
       ::= { marsMcsBackupMarsTable 1 }

   MarsMcsBackupMarsEntry ::=
       SEQUENCE {
           marsMcsBackupMarsPriority     Unsigned32,
           marsMcsBackupMarsAddr         AtmAddr,
           marsMcsBackupMarsRowStatus    RowStatus
       }

   marsMcsBackupMarsPriority OBJECT-TYPE
       SYNTAX  Unsigned32(0..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The priority associated with a backup MARS. A lower
            priority value inidcates a higher preference."
       ::= { marsMcsBackupMarsEntry 1 }

   marsMcsBackupMarsAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS not-accessible
       STATUS  current





       DESCRIPTION
           "The ATM address associated with a backup MARS."
       ::= { marsMcsBackupMarsEntry 2 }

   marsMcsBackupMarsRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create or delete a row in this
            table.

            Since other objects in this row are not-accessible
            'index-objects', the value of this object has no
            effect on whether those objects in this conceptual
            row can be modified."
       ::= { marsMcsBackupMarsEntry 3 }

   --***************************************************************
   --  IP ATM MARS MCS VC Object Definition Table
   --***************************************************************

   marsMcsVcTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsMcsVcEntry
       MAX-ACCESS  not-accessible
       STATUS current
       DESCRIPTION
           "This table contains information about open virtual
            circuits (VCs) that a MCS has.  For point to
            point circuit, each entry represents a single VC
            connection between this MCS ATM address to another
            party ATM address.  In the case of point to
            multipoint connection where a single source address
            is associated with multiple destinations, several
            entries are used to represent the relationship.  An
            example of point to multi-point VC represented in a
            table is shown below.

               MCS      VPI/VCI    Grp Addr1/Addr2    Part Addr
                1         0,1          g1,g2             p1
                1         0,1          g1,g2             p2
                1         0,1          g1,g2             p3"
       ::= {  marsMcsObjects 4 }

   marsMcsVcEntry OBJECT-TYPE
       SYNTAX  MarsMcsVcEntry
       MAX-ACCESS not-accessible
       STATUS  current





       DESCRIPTION
           "The objects contained in the entry are VC related
            attributes such as VC signalling type, control VC
            type, idle timer, negotiated MTU size, etc."
       INDEX { marsMcsIndex,
               marsMcsIfIndex,
               marsMcsVcVpi,
               marsMcsVcVci,
               marsMcsVcMinGrpAddr,
               marsMcsVcMaxGrpAddr,
               marsMcsVcPartyAddr }
       ::= { marsMcsVcTable 1 }

   MarsMcsVcEntry ::=
       SEQUENCE {
           marsMcsVcVpi           INTEGER,
           marsMcsVcVci           INTEGER,
           marsMcsVcMinGrpAddr    IpAddress,
           marsMcsVcMaxGrpAddr    IpAddress,
           marsMcsVcPartyAddr     AtmAddr,
           marsMcsVcPartyAddrType INTEGER,
           marsMcsVcType          INTEGER,
           marsMcsVcCtrlType      INTEGER,
           marsMcsVcIdleTimer     INTEGER,
           marsMcsVcRevalidate    TruthValue,
           marsMcsVcEncapsType    INTEGER,
           marsMcsVcNegotiatedMtu INTEGER,
           marsMcsVcRowStatus     RowStatus
       }

   marsMcsVcVpi OBJECT-TYPE
       SYNTAX  INTEGER (0..4095)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "The value of virtual path identifier (VPI). Since
            a VPI can be numbered 0, this sub-index can take
            a value of 0."
       ::= { marsMcsVcEntry 1 }

   marsMcsVcVci OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
            "The value of virtual circuit identifier (VCI). Since
            a VCI can be numbered 0, this sub-index can take
            a value of 0."





        ::= { marsMcsVcEntry 2 }

   marsMcsVcMinGrpAddr OBJECT-TYPE
       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Minimum IP multicast group address - the min and
            max multicast forms a multi-group block which is
            associated with a VC.  If the MinGrpAddr and
            MaxGrpAddr are the same, it indicates that the
            size of multi-group block is 1, a single IP group."
       ::= { marsMcsVcEntry 3 }

   marsMcsVcMaxGrpAddr OBJECT-TYPE


       SYNTAX  IpAddress
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Maximum IP multicast group address - the min
            and max multicast forms a multi-group block
            which is associated with a VC. If the MinGrpAddr
            and MaxGrpAddr are the same, it indicates that the
            size of multi-group block is 1, a single IP group."
       ::= { marsMcsVcEntry 4 }

   marsMcsVcPartyAddr OBJECT-TYPE
       SYNTAX  AtmAddr
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "An ATM party address in which this VC is linked.
            The party type is identified by the
            marsMcsVcPartyAddrType."
       ::= { marsMcsVcEntry 5 }

   marsMcsVcPartyAddrType OBJECT-TYPE
       SYNTAX  INTEGER {
             called (1),
             calling (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The party type is associated with the party address.
            The called (1) indicates that the party address is





            a destination address which implies that VC is
            originated from this MCS.  The calling (2) indicates
            the VC was initiated externally to this MCS.  In this
            case, the party address is the source address."
       ::= { marsMcsVcEntry 6 }

   marsMcsVcType OBJECT-TYPE
       SYNTAX  INTEGER {
             pvc (1),
             svc (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Circuit Connection type: permanent virtual circuit or
            switched virtual circuit."
       ::= { marsMcsVcEntry 7 }


   marsMcsVcCtrlType OBJECT-TYPE
       SYNTAX  INTEGER {
              pointToPointVC (1),
              serverControlVC (2),
              pointToMultiPointVC (3)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "Control VC type used to specify a particular connection.
              pointToPointVC (1):
                used by the ATM Clients for the registration and
                queries.  This VC or the initial signalling path is
                set up from the source MCS to a MARS. It is
                bi-directional.
              serverControlVC (2):
                used by a MARS to issue asynchronous updates to an
                ATM Client.  This VC is established from the MARS
                to the MCS.
              pointToMultiPointVC (3):
                used by the client to transfer multicast data
                packets from layer 3.  This VC is established from
                this VC to a cluster member."
       ::= { marsMcsVcEntry 8 }

   marsMcsVcIdleTimer OBJECT-TYPE
       SYNTAX  INTEGER (1..2147483647)
       UNITS   "minutes"
       MAX-ACCESS read-create





       STATUS  current
       DESCRIPTION
           "The idle timer associated with this VC. The minimum
            suggested value is 1 minute and the recommended
            default value is 20 minutes."
       DEFVAL { 20 }
       ::= { marsMcsVcEntry 9 }

   marsMcsVcRevalidate OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "A flag associated with an open and active multipoint
            VC. It is checked every time a packet is queued for
            transmission on that VC. The object has the value of
            true (1) if revalidate is required and the value
            false (2) otherwise."
       ::= { marsMcsVcEntry 10 }

   marsMcsVcEncapsType OBJECT-TYPE
       SYNTAX  INTEGER {
             other (1),
             llcSnap (2)
           }
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The encapsulation type used when communicating over
            this VC."
       ::= { marsMcsVcEntry 11 }

   marsMcsVcNegotiatedMtu OBJECT-TYPE
       SYNTAX  INTEGER (1..65535)
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The negotiated MTU when communicating over this VC."
       ::= { marsMcsVcEntry 12 }

   marsMcsVcRowStatus OBJECT-TYPE
       SYNTAX  RowStatus
       MAX-ACCESS read-create
       STATUS  current
       DESCRIPTION
           "The object is used to create, delete or modify a
            row in this table.






            A row cannot be made 'active' until instances of
            all corresponding columns in the row of this table
            are appropriately configured.

            While objects: marsMcsVcIdleTimer and
            marsMcsVcRevalidate in this conceptual row can
            be modified irrespective of the value of this
            object, all other objects in the row can not be
            modified when this object has a value of 'active'.

            It is possible for an SNMP management station
            to set the row to 'notInService' and modify
            the entry and then set it back to 'active'
            with the following exception. That is, rows
            for which the corresponding instance of
            marsMcsVcType has a value of 'svc' can not
            be modified or deleted."
       ::= { marsMcsVcEntry 13 }

   --***************************************************************
   --  IP ATM MARS MCS Statistics Definition Table
   --***************************************************************

   marsMcsStatTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF MarsMcsStatEntry
       MAX-ACCESS  not-accessible
       STATUS current
       DESCRIPTION
           "The table contains statistics collected at MARS MCSs."
       ::= {  marsMcsObjects 5 }

   marsMcsStatEntry OBJECT-TYPE
       SYNTAX  MarsMcsStatEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "Each entry contains statistics collected at one
            MARS MCS."
       INDEX { marsMcsIndex, marsMcsIfIndex }
       ::= { marsMcsStatTable 1 }

   MarsMcsStatEntry ::=
       SEQUENCE {
           marsMcsStatTxReqMsgs       Counter32,
           marsMcsStatTxMservMsgs     Counter32,
           marsMcsStatTxUnservMsgs    Counter32,
           marsMcsStatRxMultiMsgs     Counter32,
           marsMcsStatRxSjoinMsgs     Counter32,





           marsMcsStatRxSleaveMsgs    Counter32,
           marsMcsStatRxNakMsgs       Counter32,
           marsMcsStatRxMigrateMsgs   Counter32,
           marsMcsStatFailMultiMsgs   Counter32
       }

   marsMcsStatTxReqMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_REQUEST messages transmitted
            from this MCS."
       ::= { marsMcsStatEntry 1 }

   marsMcsStatTxMservMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MSERV messages transmitted from
            this MCS."
       ::= { marsMcsStatEntry 2 }

   marsMcsStatTxUnservMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_UNSERV messages transmitted from
            this MCS."
       ::= { marsMcsStatEntry 3 }

   marsMcsStatRxMultiMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MULTI messages received by
            this MCS."
       ::= { marsMcsStatEntry 4 }

   marsMcsStatRxSjoinMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_SJOIN messages received by





            this MCS."
       ::= { marsMcsStatEntry 5 }

   marsMcsStatRxSleaveMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_SLEAVE messages received
            by this MCS."
       ::= { marsMcsStatEntry 6 }

   marsMcsStatRxNakMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_NAK messages received
            by this MCS."
       ::= { marsMcsStatEntry 7 }

   marsMcsStatRxMigrateMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of MARS_MIGRATE messages received
            by this MCS."
       ::= { marsMcsStatEntry 8 }

   marsMcsStatFailMultiMsgs OBJECT-TYPE
       SYNTAX  Counter32
       MAX-ACCESS read-only
       STATUS  current
       DESCRIPTION
           "Total number of timeouts occurred indicating
            failure of the last MARS_MULTI to arrive."
       ::= { marsMcsStatEntry 9 }

   --***************************************************************
   --  IP ATM MARS Notification Definitions
   --***************************************************************

   marsTrapInfo OBJECT IDENTIFIER ::= { marsMIB 0 }

   marsFaultTrap NOTIFICATION-TYPE
       OBJECTS {
           marsAddr,





           marsServStatus
          }
       STATUS  current
       DESCRIPTION
           "This trap/inform is sent to the manager whenever
            there is a fault condition occurred on a MARS."
       ::= { marsTrapInfo 1 }

   --***************************************************************
   --  IP ATM MARS Conformance Definitions
   --***************************************************************

   marsConformance       OBJECT IDENTIFIER ::= { marsMIB 4 }
   marsClientConformance OBJECT IDENTIFIER ::= { marsConformance 1 }
   marsServerConformance OBJECT IDENTIFIER ::= { marsConformance 2 }
   marsMcsConformance    OBJECT IDENTIFIER ::= { marsConformance 3 }

   marsClientCompliances OBJECT IDENTIFIER ::= { marsClientConformance 1 }
   marsClientGroups      OBJECT IDENTIFIER ::= { marsClientConformance 2 }

   marsServerCompliances OBJECT IDENTIFIER ::= { marsServerConformance 1 }


   marsServerGroups      OBJECT IDENTIFIER ::= { marsServerConformance 2 }

   marsMcsCompliances    OBJECT IDENTIFIER ::= { marsMcsConformance 1 }
   marsMcsGroups         OBJECT IDENTIFIER ::= { marsMcsConformance 2 }

   --***************************************************************
   -- MARS Client Compliance Statements
   --***************************************************************

   marsClientCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
           "The compliance statement for entities that are required
            for the management of MARS clients."
       MODULE
           MANDATORY-GROUPS {
            marsClientGroup
           }

       OBJECT marsClientAddr
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientDefaultMarsAddr





       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientHsn
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientRegistration
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientCmi
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientDefaultMtu
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."


       OBJECT marsClientFailureTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientRetranDelayTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientRdmMulReqAddRetrTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientRdmVcRevalidateTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientJoinLeaveRetrInterval
       MIN-ACCESS read-only
       DESCRIPTION





         "Write access is not required."

       OBJECT marsClientJoinLeaveRetrLimit
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientRegWithMarsRdmTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientForceWaitTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientLmtToMissRedirMapTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientIdleTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientMcGrpRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientBackupMarsRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientVcType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientVcCtrlType





       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientVcIdleTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientVcRevalidate
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientVcEncapsType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientVcNegotiatedMtu
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsClientVcRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       ::= { marsClientCompliances 1 }

   marsClientGroup OBJECT-GROUP
       OBJECTS {
           marsClientAddr,
           marsClientDefaultMarsAddr,
           marsClientHsn,
           marsClientRegistration,
           marsClientCmi,
           marsClientDefaultMtu,
           marsClientFailureTimer,
           marsClientRetranDelayTimer,
           marsClientRdmMulReqAddRetrTimer,
           marsClientRdmVcRevalidateTimer,
           marsClientJoinLeaveRetrInterval,
           marsClientJoinLeaveRetrLimit,
           marsClientRegWithMarsRdmTimer,
           marsClientForceWaitTimer,
           marsClientIdleTimer,





           marsClientLmtToMissRedirMapTimer,
           marsClientRowStatus,
           marsClientMcGrpRowStatus,
           marsClientBackupMarsRowStatus,
           marsClientVcPartyAddrType,
           marsClientVcType,
           marsClientVcCtrlType,
           marsClientVcIdleTimer,
           marsClientVcRevalidate,
           marsClientVcEncapsType,
           marsClientVcNegotiatedMtu,
           marsClientVcRowStatus,
           marsClientStatTxReqMsgs,
           marsClientStatTxJoinMsgs,
           marsClientStatTxLeaveMsgs,
           marsClientStatTxGrpLstReqMsgs,
           marsClientStatRxJoinMsgs,
           marsClientStatRxLeaveMsgs,
           marsClientStatRxMultiMsgs,
           marsClientStatRxNakMsgs,
           marsClientStatRxGrpLstRplyMsgs,
           marsClientStatRxMigrateMsgs,
           marsClientStatFailMultiMsgs
          }
       STATUS  current
       DESCRIPTION
           "A collection of objects to be implemented in a MIB
            for the management of MARS clients."
       ::= { marsClientGroups 1 }

   --***************************************************************
   -- MARS Server Compliance Statements
   --***************************************************************

   marsServerCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
           "The compliance statement for entities that are required
            for the management of MARS servers."
       MODULE -- this module
           MANDATORY-GROUPS {
            marsServerGroup,
            marsServerEventGroup
           }

       OBJECT marsAddr
       MIN-ACCESS read-only
       DESCRIPTION





         "Write access is not required."

       OBJECT marsLocal
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsServStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsServType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsServPriority
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsRedirMapMsgTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsCsn
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsSsn
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcGrpAddrUsage
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcGrpRowStatus





       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsHostMapRowType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsHostMapRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsServerMapRowType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsServerMapRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsVcPartyAddrType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsVcType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsVcCtrlType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsVcIdleTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsVcCmi
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."





       OBJECT marsVcEncapsType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsVcNegotiatedMtu
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsVcRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       ::= { marsServerCompliances 1 }

   marsServerGroup OBJECT-GROUP
         OBJECTS {
           marsAddr,
           marsLocal,
           marsServStatus,
           marsServType,
           marsServPriority,
           marsRedirMapMsgTimer,
           marsCsn,
           marsSsn,
           marsRowStatus,
           marsMcGrpAddrUsage,
           marsMcGrpRxLayer3GrpSets,
           marsMcGrpRxLayer3GrpResets,
           marsMcGrpRowStatus,
           marsHostMapRowType,
           marsHostMapRowStatus,
           marsServerMapRowType,
           marsServerMapRowStatus,
           marsVcPartyAddrType,
           marsVcType,
           marsVcCtrlType,
           marsVcIdleTimer,
           marsVcCmi,
           marsVcEncapsType,
           marsVcNegotiatedMtu,
           marsVcRowStatus,
           marsRegClientAtmAddr,
           marsRegMcsAtmAddr,
           marsStatTxMultiMsgs,
           marsStatTxGrpLstRplyMsgs,





           marsStatTxRedirectMapMsgs,
           marsStatTxMigrateMsgs,
           marsStatTxNakMsgs,
           marsStatTxJoinMsgs,
           marsStatTxLeaveMsgs,
           marsStatTxSjoinMsgs,
           marsStatTxSleaveMsgs,
           marsStatTxMservMsgs,
           marsStatTxUnservMsgs,
           marsStatRxReqMsgs,
           marsStatRxGrpLstReqMsgs,
           marsStatRxJoinMsgs,
           marsStatRxLeaveMsgs,
           marsStatRxMservMsgs,
           marsStatRxUnservMsgs,
           marsStatRxBlkJoinMsgs,
           marsStatRegMemGroups,
           marsStatRegMcsGroups
          }
       STATUS  current
       DESCRIPTION
           "A collection of objects to be implemented in a MIB
            for the management of MARS servers."
       ::= { marsServerGroups 1 }

   marsServerEventGroup NOTIFICATION-GROUP
       NOTIFICATIONS { marsFaultTrap }
       STATUS  current
       DESCRIPTION
           "A collection of events that can be generated from
            a MARS server."
       ::= { marsServerGroups 2 }

   --***************************************************************
   -- MARS Multicast Server (MCS) Compliance Statements
   --***************************************************************

   marsMcsCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
           "The compliance statement for entities that are required
            for the management of MARS multicast servers (MCS)."
       MODULE
           MANDATORY-GROUPS {
            marsMcsGroup
           }

       OBJECT marsMcsAddr





       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsDefaultMarsAddr
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsRegistration
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsSsn
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsDefaultMtu
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsFailureTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsRetranDelayTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsRdmMulReqAddRetrTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsRdmVcRevalidateTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsRegisterRetrInterval
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."





       OBJECT marsMcsRegisterRetrLimit
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsForceWaitTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsLmtToMissRedirMapTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsIdleTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsMcGrpRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsBackupMarsRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsVcPartyAddrType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsVcType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsVcCtrlType
       MIN-ACCESS read-only
       DESCRIPTION





         "Write access is not required."

       OBJECT marsMcsVcIdleTimer
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsVcRevalidate
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsVcEncapsType
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsVcNegotiatedMtu
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       OBJECT marsMcsVcRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
         "Write access is not required."

       ::= { marsMcsCompliances 1 }

   marsMcsGroup OBJECT-GROUP
       OBJECTS {
           marsMcsAddr,
           marsMcsDefaultMarsAddr,
           marsMcsRegistration,
           marsMcsSsn ,
           marsMcsDefaultMtu,
           marsMcsFailureTimer,
           marsMcsRetranDelayTimer,
           marsMcsRdmMulReqAddRetrTimer,
           marsMcsRdmVcRevalidateTimer,
           marsMcsRegisterRetrInterval,
           marsMcsRegisterRetrLimit,
           marsMcsRegWithMarsRdmTimer,
           marsMcsForceWaitTimer,
           marsMcsIdleTimer,
           marsMcsLmtToMissRedirMapTimer,
           marsMcsRowStatus,
           marsMcsMcGrpRowStatus,





           marsMcsVcPartyAddrType,
           marsMcsBackupMarsRowStatus,
           marsMcsVcType,
           marsMcsVcCtrlType,
           marsMcsVcIdleTimer,
           marsMcsVcRevalidate,
           marsMcsVcEncapsType,
           marsMcsVcNegotiatedMtu,
           marsMcsVcRowStatus,
           marsMcsStatTxReqMsgs,
           marsMcsStatTxMservMsgs,
           marsMcsStatTxUnservMsgs,
           marsMcsStatRxMultiMsgs,
           marsMcsStatRxSjoinMsgs,
           marsMcsStatRxSleaveMsgs,
           marsMcsStatRxNakMsgs,
           marsMcsStatRxMigrateMsgs,
           marsMcsStatFailMultiMsgs
          }
       STATUS  current
       DESCRIPTION
           "A collection of objects to be implemented in a MIB
            for the management of MARS multicast servers (MCS)."
       ::= { marsMcsGroups 1 }

      END


