CAPWAP-DOT11-MIB DEFINITIONS ::= BEGIN


IMPORTS
   RowStatus, TEXTUAL-CONVENTION
       FROM SNMPv2-TC
   OBJECT-GROUP, MODULE-COMPLIANCE
       FROM SNMPv2-CONF
   MODULE-IDENTITY, OBJECT-TYPE, mib-2, Unsigned32
       FROM SNMPv2-SMI
   ifIndex, InterfaceIndex
       FROM IF-MIB
   CapwapBaseMacTypeTC, CapwapBaseTunnelModeTC
       FROM CAPWAP-BASE-MIB;

capwapDot11MIB MODULE-IDENTITY
    LAST-UPDATED "201004300000Z"        -- 30 April 2010
    ORGANIZATION "IETF Control And Provisioning of Wireless Access
                  Points (CAPWAP) Working Group
                  http://www.ietf.org/html.charters/capwap-charter.html"
    CONTACT-INFO
        "General Discussion: capwap@frascone.com
         To Subscribe: http://lists.frascone.com/mailman/listinfo/capwap

         Yang Shi (editor)
         Hangzhou H3C Tech. Co., Ltd.
         Beijing R&D Center of H3C, Digital Technology Plaza
         NO. 9 Shangdi 9th Street, Haidian District
         Beijing  100085
         China
         Phone: +86 010 82775276
         Email: rishyang@gmail.com

         David T. Perkins (editor)
         228 Bayview Dr.
         San Carlos, CA  94070
         USA
         Phone: +1 408 394-8702
         Email:  dperkins@dsperkins.com

         Chris Elliott (editor)
         1516 Kent St.
         Durham, NC  27707
         USA
         Phone: +1 919-308-1216
         Email: chelliot@pobox.com






         Yong Zhang (editor)
         Fortinet, Inc.
         1090 Kifer Road
         Sunnyvale, CA  94086
         USA
         Email: yzhang@fortinet.com"

   DESCRIPTION
       "Copyright (c) 2010 IETF Trust and the persons identified as
        authors of the code.  All rights reserved.

        Redistribution and use in source and binary forms, with or
        without modification, is permitted pursuant to, and subject
        to the license terms contained in, the Simplified BSD License
        set forth in Section 4.c of the IETF Trust's Legal Provisions
        Relating to IETF Documents
        (http://trustee.ietf.org/license-info).

        This version of this MIB module is part of RFC 5834;
        see the RFC itself for full legal notices.

        This MIB module contains managed object definitions for
        CAPWAP Protocol binding for IEEE 802.11."
   REVISION    "201004300000Z"
   DESCRIPTION
       "Initial version, published as RFC 5834"
        ::= { mib-2 195 }

-- Textual conventions

CapwapDot11WlanIdTC ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
        "Represents the unique identifier of a Wireless Local Area
         Network (WLAN)."
    SYNTAX      Unsigned32 (1..16)

CapwapDot11WlanIdProfileTC ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS      current
    DESCRIPTION
        "Represents the unique identifier of a WLAN profile."
    SYNTAX      Unsigned32 (1..512)

-- Top level components of this MIB module

-- Tables, Scalars





capwapDot11Objects OBJECT IDENTIFIER
    ::= { capwapDot11MIB 1 }
-- Conformance
capwapDot11Conformance OBJECT IDENTIFIER
    ::= { capwapDot11MIB 2 }

-- capwapDot11WlanTable Table

capwapDot11WlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CapwapDot11WlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that allows the operator to display and configure
         WLAN profiles, such as specifying the MAC type and tunnel mode
         for a WLAN.  Also, it helps the AC to configure a WLAN through
         the IEEE 802.11 MIB module.
         Values of all objects in this table are persistent at
         restart/reboot."
    ::= { capwapDot11Objects 1 }

capwapDot11WlanEntry  OBJECT-TYPE
    SYNTAX      CapwapDot11WlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A set of objects that stores the settings of a WLAN profile."
    INDEX { capwapDot11WlanProfileId }
    ::= { capwapDot11WlanTable 1 }

CapwapDot11WlanEntry ::=
    SEQUENCE {
      capwapDot11WlanProfileId          CapwapDot11WlanIdProfileTC,
      capwapDot11WlanProfileIfIndex     InterfaceIndex,
      capwapDot11WlanMacType            CapwapBaseMacTypeTC,
      capwapDot11WlanTunnelMode         CapwapBaseTunnelModeTC,
      capwapDot11WlanRowStatus          RowStatus
    }

capwapDot11WlanProfileId OBJECT-TYPE
    SYNTAX      CapwapDot11WlanIdProfileTC
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Represents the identifier of a WLAN profile that has a
         corresponding capwapDot11WlanProfileIfIndex."
    ::= { capwapDot11WlanEntry 1 }






capwapDot11WlanProfileIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Represents the index value that uniquely identifies a
         WLAN Profile Interface.  The interface identified by a
         particular value of this index is the same interface as
         identified by the same value of the ifIndex.
         The creation of a row object in the capwapDot11WlanTable
         triggers the AC to automatically create an WLAN Profile
         Interface identified by an ifIndex without manual
         intervention.
         Most MIB tables in the IEEE 802.11 MIB module
         [IEEE.802-11.2007] use an ifIndex to identify an interface
         to facilitate the configuration and maintenance, for example,
         dot11AuthenticationAlgorithmsTable.
         Using the ifIndex of a WLAN Profile Interface, the Operator
         could configure a WLAN through the IEEE 802.11 MIB module."
    ::= { capwapDot11WlanEntry 2 }

capwapDot11WlanMacType OBJECT-TYPE
    SYNTAX      CapwapBaseMacTypeTC
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Represents whether the WTP SHOULD support the WLAN in
         Local or Split MAC modes."
    REFERENCE
        "Section 6.1 of CAPWAP Protocol Binding for IEEE 802.11,
         RFC 5416."
    ::= { capwapDot11WlanEntry 3 }

capwapDot11WlanTunnelMode OBJECT-TYPE
    SYNTAX      CapwapBaseTunnelModeTC
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Represents the frame tunneling mode to be used for IEEE 802.11
         data frames from all stations associated with the WLAN.
         Bits are exclusive with each other for a specific WLAN profile,
         and only one tunnel mode could be configured.
         If the operator set more than one bit, the value of the
         Response-PDU's error-status field is set to 'wrongValue',
         and the value of its error-index field is set to the index of
         the failed variable binding."
    REFERENCE
        "Section 6.1 of CAPWAP Protocol Binding for IEEE 802.11,





         RFC 5416."
    ::= { capwapDot11WlanEntry 4 }

capwapDot11WlanRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable is used to create, modify, and/or delete a row
         in this table.
         All the objects in a row can be modified only when the value
         of this object in the corresponding conceptual row is not
         'active'.  Thus, to modify one or more of the objects in
         this conceptual row:
              a. change the row status to 'notInService',
              b. change the values of the row
              c. change the row status to 'active'
         The capwapDot11WlanRowStatus may be changed to 'active'
         if all the managed objects in the conceptual row with
         MAX-ACCESS read-create have been assigned valid values.

         When the operator deletes a WLAN profile, the AC SHOULD
         check whether the WLAN profile is bound with a radio.
         If yes, the value of the Response-PDU's error-status field
         is set to 'inconsistentValue', and the value of its
         error-index field is set to the index of the failed variable
         binding.  If not, the row object could be deleted."
    ::= { capwapDot11WlanEntry 5 }

-- End of capwapDot11WlanTable Table


-- capwapDot11WlanBindTable Table

capwapDot11WlanBindTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CapwapDot11WlanBindEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that stores bindings between WLAN profiles
         (identified by capwapDot11WlanProfileId) and WTP Virtual Radio
         Interfaces.  The WTP Virtual Radio Interfaces on the AC
         correspond to physical layer (PHY) radios on the WTPs.
         It also stores the mappings between WLAN IDs and WLAN
         Basic Service Set (BSS) Interfaces.
         Values of all objects in this table are persistent at
         restart/reboot."
    REFERENCE





        "Section 6.1 of CAPWAP Protocol Binding for IEEE 802.11,
         RFC 5416."
    ::= { capwapDot11Objects 2 }

capwapDot11WlanBindEntry OBJECT-TYPE
    SYNTAX      CapwapDot11WlanBindEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A set of objects that stores the binding of a WLAN profile
         to a WTP Virtual Radio Interface.  It also stores the mapping
         between WLAN ID and WLAN BSS Interface.
         The INDEX object ifIndex is the ifIndex of a WTP Virtual
         Radio Interface."
    INDEX { ifIndex, capwapDot11WlanProfileId }
    ::= { capwapDot11WlanBindTable 1 }

CapwapDot11WlanBindEntry ::=
    SEQUENCE {
      capwapDot11WlanBindWlanId        CapwapDot11WlanIdTC,
      capwapDot11WlanBindBssIfIndex    InterfaceIndex,
      capwapDot11WlanBindRowStatus     RowStatus
    }

capwapDot11WlanBindWlanId OBJECT-TYPE
    SYNTAX      CapwapDot11WlanIdTC
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Represents the WLAN ID of a WLAN.
         During a binding operation, the AC MUST select an unused
         WLAN ID from between 1 and 16 [RFC5416].  For example, to bind
         another WLAN profile to a radio that has been bound with
         a WLAN profile, WLAN ID 2 should be assigned."
    REFERENCE
        "Section 6.1 of CAPWAP Protocol Binding for IEEE 802.11,
         RFC 5416."
    ::= { capwapDot11WlanBindEntry 1 }

capwapDot11WlanBindBssIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Represents the index value that uniquely identifies a
         WLAN BSS Interface.  The interface identified by a
         particular value of this index is the same interface as
         identified by the same value of the ifIndex.





         The ifIndex here is for a WLAN BSS Interface.
         The creation of a row object in the capwapDot11WlanBindTable
         triggers the AC to automatically create a WLAN BSS Interface
         identified by an ifIndex without manual intervention.
         The PHY address of the capwapDot11WlanBindBssIfIndex is the
         BSSID.  While manufacturers are free to assign BSSIDs by using
         any arbitrary mechanism, it is advised that where possible the
         BSSIDs are assigned as a contiguous block.
         When assigned as a block, implementations can still assign
         any of the available BSSIDs to any WLAN.  One possible method
         is for the WTP to assign the address using the following
         algorithm: base BSSID address + WLAN ID."
    REFERENCE
        "Section 2.4 of CAPWAP Protocol Binding for IEEE 802.11,
         RFC 5416."
    ::= { capwapDot11WlanBindEntry 2 }

capwapDot11WlanBindRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable is used to create, modify, and/or delete a row
         in this table.
         All the objects in a row can be modified only when the value
         of this object in the corresponding conceptual row is not
         'active'.  Thus, to modify one or more of the objects in
         this conceptual row:
              a. change the row status to 'notInService',
              b. change the values of the row
              c. change the row status to 'active'"
    ::= { capwapDot11WlanBindEntry 3 }

-- End of capwapDot11WlanBindTable Table


-- Module compliance

capwapDot11Groups OBJECT IDENTIFIER
    ::= { capwapDot11Conformance 1 }

capwapDot11Compliances OBJECT IDENTIFIER
    ::= { capwapDot11Conformance 2 }

capwapDot11Compliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
        "Describes the requirements for conformance to the





         CAPWAP-DOT11-MIB module."

    MODULE -- this module
      MANDATORY-GROUPS {
        capwapDot11WlanGroup,
        capwapDot11WlanBindGroup
      }
    ::= { capwapDot11Compliances 1 }

capwapDot11WlanGroup    OBJECT-GROUP
    OBJECTS {
      capwapDot11WlanProfileIfIndex,
      capwapDot11WlanMacType,
      capwapDot11WlanTunnelMode,
      capwapDot11WlanRowStatus
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects that is used to configure
         the properties of a WLAN profile."
    ::= { capwapDot11Groups 1 }

capwapDot11WlanBindGroup    OBJECT-GROUP
    OBJECTS {
      capwapDot11WlanBindWlanId,
      capwapDot11WlanBindBssIfIndex,
      capwapDot11WlanBindRowStatus
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects that is used to bind the
         WLAN profiles with a radio."
    ::= { capwapDot11Groups 2 }

END


