TED-MIB DEFINITIONS ::= BEGIN


   IMPORTS
      MODULE-IDENTITY, OBJECT-TYPE, Integer32, Unsigned32, transmission,
      NOTIFICATION-TYPE
        FROM SNMPv2-SMI                            -- RFC 2578
      MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF                           -- RFC 2580
      TEXTUAL-CONVENTION, RowPointer
        FROM SNMPv2-TC                             -- RFC 2579
      IANAGmplsLSPEncodingTypeTC, IANAGmplsSwitchingTypeTC
        FROM IANA-GMPLS-TC-MIB                     -- RFC 4802
      InetAddress, InetAddressType
        FROM INET-ADDRESS-MIB                      -- RFC 4001
      Float32TC
        FROM FLOAT-TC-MIB                          -- RFC 6340
      ;

   tedMIB MODULE-IDENTITY
      LAST-UPDATED "201212210000Z"  -- 21 Dec. 2012 00:00:00 GMT
      ORGANIZATION "IETF CCAMP Working Group."
      CONTACT-INFO
         "          Tomohiro Otani
                    Tm-otani@kddi.com

                    Masanori Miyazawa
                    ma-miyazawa@kddilabs.jp

                    Thomas D. Nadeau
                    tnadeau@juniper.net

                    Kenji Kumaki
                    ke-kumaki@kddi.com

                    Comments and discussion to ccamp@ietf.org"










   DESCRIPTION
     "This MIB module contains managed object definitions for TED in
     support of MPLS/GMPLS TE Database.

     Copyright (c) 2013 IETF Trust and the persons identified as
     authors of the code.  All rights reserved.

     Redistribution and use in source and binary forms, with or without
     modification, is permitted pursuant to, and subject to the license
     terms contained in, the Simplified BSD License set forth in
     Section 4.c of the IETF Trust's Legal Provisions Relating to IETF
     Documents (http://trustee.ietf.org/license-info)."
   -- Revision history.
      REVISION
        "201212210000Z"  -- 21 Dec. 2012 00:00:00 GMT
      DESCRIPTION
        "Initial version.  Published as RFC 6825."
      ::= { transmission 273 }
   -- assigned by IANA; see Section 9 for details.

   -- Textual Conventions.

   TedAreaIdTC ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
        "The area identifier of the IGP.  If OSPF is used to advertise
        LSA, this represents an ospfArea.  If IS-IS is used, this
        represents an area address."
       SYNTAX       OCTET STRING (SIZE (0..20))

   TedRouterIdTC ::= TEXTUAL-CONVENTION
      STATUS       current
       DESCRIPTION
        "The router identifier.  If OSPF is used to advertise LSA, this
        represents a Router ID.  If IS-IS is used, this represents a
        System ID."
       SYNTAX       OCTET STRING (SIZE (0..6))

   TedLinkIndexTC ::= TEXTUAL-CONVENTION
      STATUS       current
      DESCRIPTION
        "The link identifier.  If OSPF is used, this represents an
        ospfLsdbID.  If IS-IS is used, this represents an isisLSPID.
        If a locally configured link is used, this object represents an
        arbitrary value, which is locally defined in a router."
       SYNTAX       OCTET STRING (SIZE (0..8))







   -- Top-level components of this MIB module.

   tedNotifications OBJECT IDENTIFIER ::= { tedMIB 0 }
   tedObjects       OBJECT IDENTIFIER ::= { tedMIB 1 }
   tedConformance   OBJECT IDENTIFIER ::= { tedMIB 2 }

   --  TED Table

   tedTable OBJECT-TYPE
      SYNTAX       SEQUENCE OF TedEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
        "This table indicates multiple TED information, which has been
        supported by RFC 3630 and RFC 5305."
   ::= { tedObjects 1 }

   tedEntry OBJECT-TYPE
       SYNTAX       TedEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This entry contains TED information commonly utilized in both
        MPLS and GMPLS."
      INDEX { tedLocalRouterId, tedRemoteRouterId,
      tedLinkInformationSource, tedLinkIndex }

   ::= { tedTable 1 }

   TedEntry ::= SEQUENCE {
       tedLinkInformationSource     INTEGER,
       tedLocalRouterId             TedRouterIdTC,
       tedRemoteRouterId            TedRouterIdTC,
       tedLinkIndex                 TedLinkIndexTC,
       tedLinkInformationData       RowPointer,
       tedLinkState                 INTEGER,
       tedAreaId                    TedAreaIdTC,
       tedLinkType                  INTEGER,
       tedTeRouterIdAddrType        InetAddressType,
       tedTeRouterIdAddr            InetAddress,
       tedLinkIdAddrType            InetAddressType,
       tedLinkIdAddr                InetAddress,
       tedMetric                    Integer32,
       tedMaxBandwidth              Float32TC,
       tedMaxReservableBandwidth    Float32TC,
       tedUnreservedBandwidthPri0   Float32TC,
       tedUnreservedBandwidthPri1   Float32TC,
       tedUnreservedBandwidthPri2   Float32TC,





       tedUnreservedBandwidthPri3   Float32TC,
       tedUnreservedBandwidthPri4   Float32TC,
       tedUnreservedBandwidthPri5   Float32TC,
       tedUnreservedBandwidthPri6   Float32TC,
       tedUnreservedBandwidthPri7   Float32TC,
       tedAdministrativeGroup       Integer32,
       tedLocalId                   Integer32,
       tedRemoteId                  Integer32,
       tedLinkProtectionType        BITS
       }

   tedLinkInformationSource OBJECT-TYPE
       SYNTAX       INTEGER {
                    unknown(0),
                    locallyConfigured(1),
                    ospfv2(2),
                    ospfv3(3),
                    isis(4),
                    other(5)
                    }
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This object indicates the source of the information about the
        TE link."
     ::= { tedEntry 1 }

   tedLocalRouterId OBJECT-TYPE
       SYNTAX       TedRouterIdTC
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This object represents the Router ID of the router originating
        the LSA.  If OSPF is used to advertise LSA, this represents a
        Router ID.  If IS-IS is used, this represents a System ID.
        Otherwise, this represents zero."
       REFERENCE
         "OSPF Version 2, RFC 2328, Appendix C.1
           OSPF for IPv6, RFC 5340, Appendix C.1
           ISO10589, Section 7.1"
   ::= { tedEntry 2 }












   tedRemoteRouterId OBJECT-TYPE
       SYNTAX       TedRouterIdTC
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This object indicates the router at the remote end of the link
        from the originating router.  If OSPF is used to advertise LSA,
        this represents a Link ID in the Link TLV.  If IS-IS is used,
        this represents a neighbor System ID defined in RFC 5305.
        Otherwise, this represents zero."
       REFERENCE
         "OSPF Version 2, RFC 2328, Appendix C.1
           OSPF for IPv6, RFC 5340, Appendix C.1
           ISO10589, Section 7.1"
   ::= { tedEntry 3 }

   tedLinkIndex OBJECT-TYPE
       SYNTAX       TedLinkIndexTC
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This object indicates the link state identifier.  If OSPF is
        used, this represents an ospfLsdbID.  If IS-IS is used, this
        represents an isisLSPID.  Otherwise, this represents a unique
        identifier within a node."
       REFERENCE
         "OSPF Version 2, RFC 2328, Appendix A.4.1,
           OSPF for IPv6, RFC 5340, Appendix A.4.2
           ISO10589, Section 9.8 "
   ::= { tedEntry 4 }

   tedLinkInformationData OBJECT-TYPE
       SYNTAX       RowPointer
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "If tedLinkInformationSource has the value unknown(0), this
        object MUST contain a value of zeroDotZero.

        If tedLinkInformationSource has the value locallyConfigured(1),
        an implementation can use this object to supply the identifier
        of the corresponding row entry in the teLinkTable of TE-LINK-
        STD-MIB (RFC 4220), the identifier of the corresponding row in
        a local proprietary TE link MIB module, or the value of
        zeroDotZero.

        If tedLinkInformationSource has the value ospfv2(2) and
        ospfv3(3), an implementation can use this object to supply the





        identifier of the corresponding row entry in the
        ospfLocalLsdbTable (OSPFv2-MIB) and the ospfv3AreaLsdbTable
        (OSPFv3-MIB), or the value of zeroDotZero.

        If tedLinkInformationSource has the value isis(4), an
        implementation can use this object to supply the identifier of
        the corresponding row entry in the isisAreaAddr of ISIS-MIB
        (RFC 4444), or the value of zeroDotZero.

        If tedLinkInformationSource has the value other(5), an
        implementation can use this object to supply the identifier of
        the corresponding row entry in the local proprietary MIB module,
        or the value of zeroDotZero."
   ::= { tedEntry 5 }

   tedLinkState OBJECT-TYPE
        SYNTAX       INTEGER {
                     unknown (0),
                     up (1),
                     down (2)
                     }
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
         "This object represents the actual operational state of this TE
         link.  For instance, if a row is created in the TED table, but
         the actual TE link is not available for some reason (e.g., when
         there is not yet a physical link or the link has been manually
         disabled), then the object would be down(2) state.
         In contrast, if a row is added and the TE link is available,
         this would be operationally up(1)."
   ::= { tedEntry 6 }

   tedAreaId OBJECT-TYPE
       SYNTAX       TedAreaIdTC
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the area identifier of the IGP.  If OSPF
        is used to advertise LSA, this represents an ospfArea.  If IS-IS
        is used, this represents an area address.  Otherwise, this
        represents zero."
       REFERENCE
         "OSPF Version 2, RFC 2328, Appendix C.2
           OSPF for IPv6, RFC 5340, Appendix C.2
           ISO10589, Section 9.8"
   ::= { tedEntry 7 }






   tedLinkType OBJECT-TYPE
       SYNTAX       INTEGER {
                    pointToPoint (1),
                    multiAccess (2)
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the type of the link, such as point to point or
        multi-access."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.1"
   ::= { tedEntry 8 }

   tedTeRouterIdAddrType OBJECT-TYPE
       SYNTAX       InetAddressType
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the TE-Router ID address type.  Only
        values unknown(0), ipv4(1), or ipv6(2) are supported."
   ::= { tedEntry 9 }

   tedTeRouterIdAddr OBJECT-TYPE
       SYNTAX       InetAddress
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
         "This object indicates the TE-Router ID."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.4.1
          IS-IS extensions for TE, RFC 5305, Section 4.3"
   ::= { tedEntry 10 }

   tedLinkIdAddrType OBJECT-TYPE
       SYNTAX       InetAddressType
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the address type of the TE Link ID.  Only
        values unknown(0), ipv4(1), or ipv6(2) are supported."
   ::= { tedEntry 11 }

   tedLinkIdAddr OBJECT-TYPE
       SYNTAX       InetAddress
       MAX-ACCESS   read-only





       STATUS       current
       DESCRIPTION
        "This indicates the Router ID of the neighbor in the case of
        point-to-point links.  This also indicates the interface
        address of the designated router in the case of multi-access
        links."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.2
          IS-IS extensions for TE, RFC 5305, Section 4.3"
   ::= { tedEntry 12 }

   tedMetric OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the traffic engineering metric value of the TE
        link."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.5
          IS-IS extensions for TE, RFC 5305, Section 3.7"
   ::= { tedEntry 13 }

   tedMaxBandwidth OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the maximum bandwidth that can be used on this
        link in this direction."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.6
          IS-IS extensions for TE, RFC 5305, Section 3.4"
   ::= { tedEntry 14 }

   tedMaxReservableBandwidth OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the maximum bandwidth that may be reserved on
        this link in this direction."






       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.7
          IS-IS extensions for TE, RFC 5305, Section 3.5"
   ::= { tedEntry 15 }

   tedUnreservedBandwidthPri0 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the amount of bandwidth not yet reserved at the
        priority 0."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.8
          IS-IS extensions for TE, RFC 5305, Section 3.6"
   ::= { tedEntry 16 }

   tedUnreservedBandwidthPri1 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the amount of bandwidth not yet reserved at the
        priority 1."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.8
          IS-IS extensions for TE, RFC 5305, Section 3.6"
   ::= { tedEntry 17 }

   tedUnreservedBandwidthPri2 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the amount of bandwidth not yet reserved at the
        priority 2."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.8
          IS-IS extensions for TE, RFC 5305, Section 3.6"
   ::= { tedEntry 18 }






   tedUnreservedBandwidthPri3 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the amount of bandwidth not yet reserved at the
        priority 3."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.8
          IS-IS extensions for TE, RFC 5305, Section 3.6"
   ::= { tedEntry 19 }

   tedUnreservedBandwidthPri4 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the amount of bandwidth not yet reserved at the
        priority 4."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.8
          IS-IS extensions for TE, RFC 5305, Section 3.6"
   ::= { tedEntry 20 }

   tedUnreservedBandwidthPri5 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the amount of bandwidth not yet reserved at the
        priority 5."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.8
          IS-IS extensions for TE, RFC 5305, Section 3.6"
   ::= { tedEntry 21 }

   tedUnreservedBandwidthPri6 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current






       DESCRIPTION
        "This indicates the amount of bandwidth not yet reserved at the
        priority 6."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.8
          IS-IS extensions for TE, RFC 5305, 3.6"
   ::= { tedEntry 22 }

   tedUnreservedBandwidthPri7 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the amount of bandwidth not yet reserved at the
        priority 7."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.8
          IS-IS extensions for TE, RFC 5305, Section 3.6"
   ::= { tedEntry 23 }

   tedAdministrativeGroup OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the Administrative Group to which the link
        belongs.  Since the value is a bit mask, the link can belong
        to multiple groups.  This is also called Resource Class/Color."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.9
          IS-IS extensions for TE, RFC 5305, Section 3.1"
   ::= { tedEntry 24 }

   tedLocalId OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the Link Local Identifier of an unnumbered
        link."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.1
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.1"
   ::= { tedEntry 25 }





   tedRemoteId OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This indicates the Link Remote Identifier of an unnumbered
        link."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.1
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.1"
   ::= { tedEntry 26 }

   tedLinkProtectionType OBJECT-TYPE
       SYNTAX       BITS {
                    extraTraffic(0),
                    unprotected(1),
                    shared (2),
                    dedicatedOneToOne (3),
                    dedicatedOnePlusOne(4),
                    enhanced(5)
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
         "This object indicates the protection type of the TE link."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.2
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.2"
   ::= { tedEntry 27 }

   --  TED Local Interface IP Address Table

   tedLocalIfAddrTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF TedLocalIfAddrEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This table contains the IP address information of a local TE
        link."
   ::= { tedObjects 2 }

   tedLocalIfAddrEntry OBJECT-TYPE
       SYNTAX       TedLocalIfAddrEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This entry contains the IP address information of the local TE
        link."





       INDEX { tedLinkIndex, tedLocalIfAddr }
   ::= { tedLocalIfAddrTable 1 }

   TedLocalIfAddrEntry ::= SEQUENCE {
       tedLocalIfAddrType    InetAddressType,
       tedLocalIfAddr        InetAddress
       }

   tedLocalIfAddrType OBJECT-TYPE
       SYNTAX       InetAddressType
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the address type of the local TE link.
        Only values unknown(0), ipv4(1), or ipv6(2) have to be
        supported."
   ::= { tedLocalIfAddrEntry 1 }

   tedLocalIfAddr OBJECT-TYPE
       SYNTAX       InetAddress (SIZE (1..20))
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This object indicates the address of the local TE link."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.3,
         Traffic Engineering Extensions to OSPF Version 3, RFC 5329,
         Section 4.3
          IS-IS extensions for TE, RFC 5305, Section 3.4"
   ::= { tedLocalIfAddrEntry 2 }

   --  TED Remote Interface IP Address Table

   tedRemoteIfAddrTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF TedRemoteIfAddrEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This table contains the IP address information of a remote TE
        link."
   ::= { tedObjects 3 }

   tedRemoteIfAddrEntry OBJECT-TYPE
       SYNTAX       TedRemoteIfAddrEntry
       MAX-ACCESS   not-accessible
       STATUS       current






       DESCRIPTION
        "This entry contains the IP address information of the remote
        TE link."
   INDEX { tedLinkIndex, tedRemoteIfAddr }
       ::= { tedRemoteIfAddrTable 1 }

   TedRemoteIfAddrEntry ::= SEQUENCE {
       tedRemoteIfAddrType    InetAddressType,
       tedRemoteIfAddr        InetAddress
       }

   tedRemoteIfAddrType OBJECT-TYPE
       SYNTAX       InetAddressType
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
         "This object indicates the address type of the remote TE link."
   ::= { tedRemoteIfAddrEntry 1 }

   tedRemoteIfAddr OBJECT-TYPE
       SYNTAX       InetAddress(SIZE (1..20))
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This object indicates the address of the remote TE link."
       REFERENCE
        "Traffic Engineering (TE) Extensions to OSPF Version 2,
         RFC 3630, Section 2.5.4,
         Traffic Engineering Extensions to OSPF Version3, RFC 5329,
         Section 4.4
          IS-IS extensions for TE, RFC 5305, Section 3.3"
   ::= { tedRemoteIfAddrEntry 2 }

   --  TED Switching Capability Table

   tedSwCapTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF TedSwCapEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This table contains the GMPLS TED switching capability
        information."
   ::= { tedObjects 4 }

   tedSwCapEntry OBJECT-TYPE
       SYNTAX       TedSwCapEntry
       MAX-ACCESS   not-accessible
       STATUS       current





       DESCRIPTION
        "This entry relates each TE link with its GMPLS TE switching
        capability information.  If the MIB module deals with only OSPF-
        TE information, the value of each object related with GMPLS TE
        extensions should be null."
       INDEX { tedLinkIndex, tedSwCapIndex }
   ::= { tedSwCapTable 1 }

   TedSwCapEntry ::= SEQUENCE {
       tedSwCapIndex                 Unsigned32,
       tedSwCapType         IANAGmplsSwitchingTypeTC,
       tedSwCapEncoding              IANAGmplsLSPEncodingTypeTC,
       tedSwCapMaxLspBandwidthPri0   Float32TC,
       tedSwCapMaxLspBandwidthPri1   Float32TC,
       tedSwCapMaxLspBandwidthPri2   Float32TC,
       tedSwCapMaxLspBandwidthPri3   Float32TC,
       tedSwCapMaxLspBandwidthPri4   Float32TC,
       tedSwCapMaxLspBandwidthPri5   Float32TC,
       tedSwCapMaxLspBandwidthPri6   Float32TC,
       tedSwCapMaxLspBandwidthPri7   Float32TC,
       tedSwCapMinLspBandwidth       Float32TC,
       tedSwCapIfMtu                 Integer32,
       tedSwCapIndication            INTEGER
       }

   tedSwCapIndex OBJECT-TYPE
       SYNTAX       Unsigned32 (1..255)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This index is utilized to identify multiple switching
        functions on a local or remote TE link according to definitions
        of textual conventions of GMPLS, RFC 4801."
   ::= { tedSwCapEntry 1 }

   tedSwCapType OBJECT-TYPE
       SYNTAX       IANAGmplsSwitchingTypeTC
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the GMPLS switching capability assigned
        to the TE link according to definitions of textual conventions
        of GMPLS, RFC 4801."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 2 }






   tedSwCapEncoding OBJECT-TYPE
       SYNTAX       IANAGmplsLSPEncodingTypeTC
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the GMPLS encoding type assigned to the
        TE link."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 3 }

   tedSwCapMaxLspBandwidthPri0 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the maximum bandwidth of the TE link at
        the priority 0 for GMPLS LSP creation."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 4 }

   tedSwCapMaxLspBandwidthPri1 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the maximum bandwidth of the TE link at
        the priority 1 for GMPLS LSP creation."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 5 }

   tedSwCapMaxLspBandwidthPri2  OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the maximum bandwidth of the TE link at
        the priority 2 for GMPLS LSP creation."







       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 6 }

   tedSwCapMaxLspBandwidthPri3 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the maximum bandwidth of the TE link at
        the priority 3 for GMPLS LSP creation."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 7 }

   tedSwCapMaxLspBandwidthPri4 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the maximum bandwidth of the TE link at
        the priority 4 for GMPLS LSP creation."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 8 }

   tedSwCapMaxLspBandwidthPri5  OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the maximum bandwidth of the TE link at
        the priority 5 for GMPLS LSP creation."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 9 }

   tedSwCapMaxLspBandwidthPri6 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only





       STATUS       current
       DESCRIPTION
        "This object indicates the maximum bandwidth of the TE link at
        the priority 6 for GMPLS LSP creation."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 10 }

   tedSwCapMaxLspBandwidthPri7 OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the maximum bandwidth of the TE link at
        the priority 7 for GMPLS LSP creation."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 11 }

   tedSwCapMinLspBandwidth OBJECT-TYPE
       SYNTAX       Float32TC
       UNITS        "Byte per second"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the minimum bandwidth of the TE link for
        GMPLS LSP creation if the switching capability field is TDM,
        PSC-1, PSC-2, PSC-3, or PSC-4."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 12 }

   tedSwCapIfMtu OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
         "This object indicates the MTU of the local or remote TE link."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 13 }







   tedSwCapIndication OBJECT-TYPE
       SYNTAX       INTEGER {
                    standard (0),
                    arbitrary (1)
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates whether the interface supports Standard
        or Arbitrary SONET/SDH."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.4
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.3"
   ::= { tedSwCapEntry 14 }

   --  TED SRLG Table

   tedSrlgTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF TedSrlgEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
         "This table contains the SRLG information of the TE link."
   ::= { tedObjects 5 }

   tedSrlgEntry OBJECT-TYPE
       SYNTAX       TedSrlgEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
         "This entry relates each TE link with its SRLG information."
       INDEX { tedLinkIndex, tedSrlgIndex }
   ::= { tedSrlgTable 1 }

   TedSrlgEntry ::= SEQUENCE {
       tedSrlgIndex   Unsigned32,
       tedSrlg        Integer32
       }

   tedSrlgIndex OBJECT-TYPE
       SYNTAX       Unsigned32(1..255)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This index is utilized to identify multiple SRLG values on a
        local or remote TE link.  This object represents an arbitrary
        value, which is locally defined in a router."






       REFERENCE
        "OSPF Extensions in support of GMPLS, RFC 4203, Section 1.3
          IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.4"
   ::= { tedSrlgEntry 1 }

   tedSrlg OBJECT-TYPE
       SYNTAX       Integer32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "This object indicates the SRLG value assigned to a local or
        remote TE link."
       REFERENCE
         "OSPF Extensions in Support of GMPLS, RFC 4203, Section 1.3
           IS-IS Extensions in Support of GMPLS, RFC 5307, Section 1.4"
   ::= { tedSrlgEntry 2 }

   -- Notification Configuration

   tedStatusChangeNotificationMaxRate OBJECT-TYPE
       SYNTAX        Unsigned32
       MAX-ACCESS    read-write
       STATUS        current
       DESCRIPTION
        "A lot of notifications relating to the status change are
        expected to generate in a node, especially when a network
        failure occurs and might cause a performance degradation of the
        node itself.  To avoid such a defect, this object provides the
        maximum number of notifications generated per minute.  If
        events occur more rapidly, the implementation may simply fail
        to emit these notifications during that period, or may queue
        them until an appropriate time.  A value of 0 means no
        throttling is applied and events may be notified at the rate at
        which they occur."
       DEFVAL        {1}
   ::= { tedObjects 6 }

   tedCreatedDeletedNotificationMaxRate OBJECT-TYPE
       SYNTAX        Unsigned32
       MAX-ACCESS    read-write
       STATUS        current
       DESCRIPTION
        "A lot of notifications relating to new registration in the TED
        table by receiving new TE link information or deletion of
        existing entries in the TED table are expected to generate in a
        node.  This object provides the maximum number of notifications
        generated per minute."






       DEFVAL        {1}
   ::= { tedObjects 7 }

   -- Notifications

   tedStatusChange NOTIFICATION-TYPE
       OBJECTS  {
         tedLinkState
         }
       STATUS   current
       DESCRIPTION
        "This notification signifies that there has been change in the
        TE information of tedTable, tedLocalIfAddrTable,
        tedRemoteIfAddrTable, tedSwCapTable, and/or tedSrlgTable.  For
        example, this should be generated when tedUnreservedBandwidth is
        changed to create or delete LSP using the registered TE link."
   ::= { tedNotifications 1 }

   tedEntryCreated NOTIFICATION-TYPE
       OBJECTS  {
         tedLinkState
         }
       STATUS   current
       DESCRIPTION
        "This notification signifies that there has been new
        registration in the TED table by receiving new TE link
        information.  For example, this should be generated when a new
        index (tedLinkIndex) is registered in the TED table."
   ::= { tedNotifications 2 }

   tedEntryDeleted NOTIFICATION-TYPE
       OBJECTS  {
         tedLinkState
         }
       STATUS      current
      DESCRIPTION
        "This notification signifies that there has been deletion of an
        entry in the TED table.  For example, this should be generated
        when one of the existing entries is deleted in the TED table."
   ::= { tedNotifications 3 }

   -- Conformance Statement

   tedCompliances
       OBJECT IDENTIFIER ::= { tedConformance 1 }
   tedGroups
       OBJECT IDENTIFIER ::= { tedConformance 2 }






   -- Module Compliance

   tedModuleFullCompliance MODULE-COMPLIANCE
       STATUS   current
       DESCRIPTION
         "Compliance statement for agents provides full support for the
         TED MIB."
       MODULE -- this module
       MANDATORY-GROUPS   { tedMainGroup,
                            tedObjectsGroup,
                            tedNotificationGroup
                          }

   GROUP tedUnnumberedLinkGroup
      DESCRIPTION
        "This group is mandatory for TE links that support the
        unnumbered links."

   GROUP tedNumberedLinkGroup
      DESCRIPTION
        "This group is mandatory for TE links that support the
        numbered links."

   GROUP tedSwCapGroup
      DESCRIPTION
        "This group is mandatory for TE links that support GMPLS
        switching capability."

   GROUP tedSwCapMinLspBandwidthGroup
      DESCRIPTION
        "This group is mandatory for TE links if the switching
        capability field is TDM, PSC-1, PSC-2, PSC-3, or PSC-4."

   GROUP tedSwCapIfMtuGroup
      DESCRIPTION
        "This group is mandatory for TE links that support the MTU of
        the local or remote TE link."

   GROUP tedSwCapIndicationGroup
      DESCRIPTION
        "This group is mandatory for TE links that support Standard or
        Arbitrary SONET/SDH."











   GROUP tedSrlgGroup
      DESCRIPTION
        "This group is mandatory for TE links that support SRLG
        information."

   ::= { tedCompliances 1 }

   --
   -- ReadOnly Compliance
   --

   tedModuleReadOnlyCompliance MODULE-COMPLIANCE
      STATUS current
       DESCRIPTION
        "Compliance requirement for implementations only provides read-
        only support for TED.  Such devices can then be monitored but
        cannot be configured using this MIB module."
       MODULE -- this module
       MANDATORY-GROUPS   { tedMainGroup
                          }

   GROUP tedUnnumberedLinkGroup
      DESCRIPTION
        "This group is mandatory for TE links that support the
        unnumbered links."

   GROUP tedNumberedLinkGroup
      DESCRIPTION
        "This group is mandatory for TE links that support the
        numbered links."

   GROUP tedSwCapGroup
      DESCRIPTION
        "This group is mandatory for TE links that support some GMPLS
        switching capabilities."

   GROUP tedSwCapMinLspBandwidthGroup
      DESCRIPTION
        "This group is mandatory for TE links if the switching
        capability field is TDM, PSC-1, PSC-2, PSC-3, or PSC-4."

   GROUP tedSwCapIfMtuGroup
      DESCRIPTION
        "This group is mandatory for TE links that support the MTU of
        the local or remote TE link."








   GROUP tedSwCapIndicationGroup
      DESCRIPTION
        "This group is mandatory for TE links that support Standard or
        Arbitrary SONET/SDH."

   GROUP tedSrlgGroup
      DESCRIPTION
        "This group is mandatory for TE links that support SRLG
        information."

   ::= { tedCompliances 2 }

   -- Units of conformance

   tedMainGroup OBJECT-GROUP
       OBJECTS {
               tedLinkState,
               tedAreaId,
               tedLinkType,
               tedTeRouterIdAddrType,
               tedTeRouterIdAddr,
               tedLinkIdAddrType,
               tedLinkIdAddr,
               tedMetric,
               tedMaxBandwidth,
               tedMaxReservableBandwidth,
               tedUnreservedBandwidthPri0,
               tedUnreservedBandwidthPri1,
               tedUnreservedBandwidthPri2,
               tedUnreservedBandwidthPri3,
               tedUnreservedBandwidthPri4,
               tedUnreservedBandwidthPri5,
               tedUnreservedBandwidthPri6,
               tedUnreservedBandwidthPri7,
               tedAdministrativeGroup,
               tedLinkProtectionType,
               tedLinkInformationData
               }
       STATUS   current
       DESCRIPTION
        "Collection of objects for TED management"
   ::= { tedGroups 1 }

   tedObjectsGroup OBJECT-GROUP
       OBJECTS {
            tedStatusChangeNotificationMaxRate,
            tedCreatedDeletedNotificationMaxRate
       }





       STATUS  current
       DESCRIPTION
        "The objects needed to implement notification."
   ::= { tedGroups 2 }

   tedNotificationGroup NOTIFICATION-GROUP
       NOTIFICATIONS {
            tedStatusChange,
            tedEntryCreated,
            tedEntryDeleted
            }
       STATUS  current
       DESCRIPTION
        "This group is mandatory for those implementations that can
        implement the notifications contained in this group."
   ::= { tedGroups 3 }

   tedUnnumberedLinkGroup OBJECT-GROUP
       OBJECTS {
            tedLocalId,
            tedRemoteId
       }
       STATUS  current
       DESCRIPTION
        "The objects needed to implement the unnumbered links."
   ::= { tedGroups 4 }

   tedNumberedLinkGroup OBJECT-GROUP
       OBJECTS {
            tedLocalIfAddrType,
            tedRemoteIfAddrType
       }
       STATUS  current
       DESCRIPTION
        "The objects needed to implement the numbered links."
   ::= { tedGroups 5 }

   tedSwCapGroup OBJECT-GROUP
       OBJECTS {
            tedSwCapType,
            tedSwCapEncoding,
            tedSwCapMaxLspBandwidthPri0,
            tedSwCapMaxLspBandwidthPri1,
            tedSwCapMaxLspBandwidthPri2,
            tedSwCapMaxLspBandwidthPri3,
            tedSwCapMaxLspBandwidthPri4,







            tedSwCapMaxLspBandwidthPri5,
            tedSwCapMaxLspBandwidthPri6,
            tedSwCapMaxLspBandwidthPri7
       }
       STATUS  current
       DESCRIPTION
        "The objects needed to implement the TE links with GMPLS TE
        switching capability information."
   ::= { tedGroups 6 }

   tedSwCapMinLspBandwidthGroup OBJECT-GROUP
       OBJECTS {
            tedSwCapMinLspBandwidth
       }
       STATUS  current
       DESCRIPTION
        "The objects needed to implement the minimum bandwidth of the
        TE link for GMPLS LSP creation."
   ::= { tedGroups 7 }

   tedSwCapIfMtuGroup OBJECT-GROUP
       OBJECTS {
            tedSwCapIfMtu
       }
       STATUS  current
       DESCRIPTION
        "The objects needed to implement the MTU information of the
        local or remote TE link."
   ::= { tedGroups 8 }

   tedSwCapIndicationGroup OBJECT-GROUP
       OBJECTS {
            tedSwCapIndication
       }
       STATUS  current
       DESCRIPTION
        "The objects needed to implement the indication of whether the
        interface supports Standard or Arbitrary SONET/SDH."
   ::= { tedGroups 9 }














   tedSrlgGroup OBJECT-GROUP
       OBJECTS {
            tedSrlg
       }
       STATUS  current
       DESCRIPTION
         "The objects needed to implement multiple SRLG values with
         GMPLS TE information."
   ::= { tedGroups 10 }

   END


