Printer-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, experimental, Counter32, Integer32,
        TimeTicks, NOTIFICATION-TYPE, OBJECT-IDENTITY FROM SNMPv2-SMI
    TEXTUAL-CONVENTION FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP FROM SNMPv2-CONF
    hrDeviceIndex, hrStorageIndex FROM HOST-RESOURCES-MIB;

printmib MODULE-IDENTITY
    LAST-UPDATED "9411250000Z"
    ORGANIZATION "IETF Printer MIB Working Group"
    CONTACT-INFO
            "        Steven Waldbusser
         Postal: Carnegie Mellon University
                     4910 Forbes Ave
                  Pittsburgh, PA, 15213

                Tel: 412-268-6628
                Fax: 412-268-4987
             E-mail: waldbusser@cmu.edu"
    DESCRIPTION
            "The MIB module for management of printers."
    ::= { mib-2 43 }

-- Textual conventions for this MIB module

MediaUnit ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
            "Units of measure for media dimensions."
    -- This is a type 1 enumeration.
    SYNTAX       INTEGER {
                     tenThousandthsOfInches(3),  -- .0001
                     micrometers(4)





                 }

CapacityUnit ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
            "Units of measure for media capacity."
    -- This is a type 1 enumeration.
    SYNTAX       INTEGER {
                     tenThousandthsOfInches(3),  -- .0001
                     micrometers(4),
                     sheets(8),
                     feet(16),
                     meters(17)
                 }

SubUnitStatus ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
            "Status of a printer sub-unit.

             The SubUnitStatus is an integer that is the sum of 5
             distinct values, Availability, Non-Critical, Critical,
             On-line, and Transitioning. These values are:

     Availability                           value

            Available and Idle              0       000'b
            Available and Standby           2       010'b
            Available and Active            4       100'b
            Available and Busy              6       110'b
            Unavailable and OnRequest       1       001'b
            Unavailable because Broken      3       011'b
            Unknown                         5       101'b

    Non-Critical

            No Non-Critical Alerts          0
            Non-Critical Alerts             8

    Critical

            No Critical Alerts              0
            Critical Alerts                 16

    On-Line

            Intended state is On-Line       0
            Intended state is Off-Line      32





    Transitioning

            At intended state               0
            Transitioning to intended state 64
    "

    SYNTAX       INTEGER (0..126)

PresentOnOff ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
            "Presence and configuration of a device or feature."
    -- This is a type 1 enumeration.
    SYNTAX       INTEGER {
                     other(1),
                     on(3),
                     off(4),
                     notPresent(5)
                 }

  CodedCharSet ::= TEXTUAL-CONVENTION
      STATUS     current
      DESCRIPTION
         "A coded character set value that specifies both a set of
          characters that may be used and an encoding (as one or more
          octets) that is used to represent the characters in the
          set. These values are to be used to identify the encoding
          employed for strings in the MIB where this is not fixed by
          the MIB.

          Some objects that allow a choice of coded character set
          are: the prtLocalizationCharacterSet object in the
          LocalizationTable and prtInterpreterDefaultCharSetIn.
          The prtGeneralCurrentLocalization and prtConsoleLocalization
          objects in turn contain the index in the LocalizationTable
          of the current localization (country, language, and coded
          character set) of the `description' objects and the console,
          respectively.

          The space of the coded character set enumeration has been
          divide into three regions. The first region (3-999) consists
          of coded character sets that have been standardized by some
          standard setting organization. This region is intended for
          standards that do not have subset implementations. The
          second region (1000-1999) is for the Unicode and ISO/IEC 10646
          coded character sets together with a specification of a (set
          of) sub-repetoires that may occur.  The third region (>1999)
          is intended for vendor specific coded character sets.





          NOTE: Unicode and ISO 10646 character coded data may be
          processed and stored in either Big Endian (most significant
          octet first) or Little Endian (least significant octet
          first) order.  Intel x86, VAX, and Alpha/AXP architectures are
          examples of Little Endian processor architectures.
          Furthermore, in environments where either order may occur,
          so-called Unicode BYTE ORDER MARK (BOM) character (which is
          ISO 10646 ZERO WIDTH NO BREAK SPACE), coded as FEFF in two
          octets and 0000FEFF in four octets is used at the beginning
          of the data as a signature to indicate the order of the
          following data (See ISO 10646 Annex F).  Thus either
          ordering and BOM may occur in print data streams sent to the
          interpreter.  However, ISO 8824/8825 (ASN.1/BER) used by
          SNMP is quite clear that Big Endian order shall be used and
          BOM shall NOT be used in transmission in the protocol.
          Transmitting Unicode in Big Endian order in SNMP should
          not prove to be a hardship for Little Endian machines,
          since SNMP ASN.1/BER requires integers to be transmitted
          in Big Endian order as well.  So SNMP implementations on
          Little Endian machines are already reversing the order of
          integers to make them Big Endian for transmission via
          SNMP.  Also Unicode characters are usually treated as
          two-octet integers, not short text strings, so that it will
          be straightforward for Little Endian machines to reverse the
          order of Unicode character octets as well before
          transmitting them and after receiving them via the SNMP
          protocol.

          Where a given coded character set may be known by more than
          one name, the most commonly known name is used as the name
          of the enumeration and other names are shown in the
          comments.  The comments also indicate where to find detailed
          information on the coded character set and briefly
          characterize its relationship to other similar coded
          character sets.

          The current list of character sets and their enumerated
          values used to reference them is contained in the IANA
          Character Set registry.  The enum value is indicated by
          the MIBenum entry in the registry.  The enum symbol is
          indicated by the Alias that starts with `cs' for character
          set.

          The IANA character sets registry is available via
          anonymous ftp.

          The ftp server is ftp.isi.edu.
          The subdirectory is /in-notes/iana/assignments/.





          The file name is character-sets.

          To add a character set to the IANA Registry:

             1. Format an entry like those in the current list,
                omitting the MIBenum value.
             2. Send the entry with a request to add the entry
                to the character set list to iana@ISI.EDU.
             3. The IANA will supply a unique MIBenum value
                and update the list."

      -- This is a type 3 enumeration.

      SYNTAX     INTEGER {
        other(1)               -- used if the designated coded
                               -- character set is not currently in
                               -- the enumeration

      -- See IANA Registry for standard character sets in the
      -- MIBenum range of 3-999.

      -- See IANA Registry for Unicode and vendor-supplied
      -- combinations of ISO collections and character sets based
      -- on Unicode in the MIBenum range of 1000-1999.
      -- See IANA Registry for vendor developed character sets
      -- in the MIBenum range of 2000-xxxx.
   }


-- The General Printer Group
--
-- The general printer sub-unit is responsible for the overall control
-- and status of the printer.  There is exactly one general printer
-- sub-unit in a printer.
--
-- Implementation of every object in this group is mandatory.

prtGeneral  OBJECT IDENTIFIER ::= { printmib 5 }

prtGeneralTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtGeneralEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of general information per printer.
        Objects in this table are defined in various
        places in the MIB, nearby the groups to
        which they apply.  They are all defined





        here to minimize the number of tables that would
        otherwise need to exist."
    ::= { prtGeneral 1 }

prtGeneralEntry OBJECT-TYPE
    SYNTAX      PrtGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry exists in this table for each
        device entry in the hostmib device table who's type
        is `printer'"
    INDEX  { hrDeviceIndex }
    ::= { prtGeneralTable 1 }

PrtGeneralEntry ::= SEQUENCE {
    -- Note that not all of the objects in this sequence are in the
    -- general printer group.
    prtGeneralConfigChanges         Counter32,
    prtGeneralCurrentLocalization   Integer32,
    prtGeneralReset                 INTEGER,
    prtGeneralCurrentOperator       OCTET STRING,
    prtGeneralServicePerson         OCTET STRING,
    prtInputDefaultIndex            Integer32,
    prtOutputDefaultIndex           Integer32,
    prtMarkerDefaultIndex           Integer32,
    prtMediaPathDefaultIndex        Integer32,
    prtConsoleLocalization          Integer32,
    prtConsoleNumberOfDisplayLines  Integer32,
    prtConsoleNumberOfDisplayChars  Integer32,
    prtConsoleDisable               INTEGER
}

prtGeneralConfigChanges OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Counts configuration changes that change the capabilities of
        a printer, such as the addition/deletion of input/output bins,
        the addition/deletion of interpreters, or changes in media
        size.  Such changes will often affect the capability of the
        printer to service certain types of print jobs.

        Management applications may cache infrequently changed
        configuration  information about sub-units on the printer.
        This object should be incremented whenever the agent wishes
        such applications to invalidate that cache and re-download





        all of this configuration information, thereby signalling a
        change in the printer's configuration.

        For example, if an input tray that contained paper of
        different dimensions was added, this counter would be
        incremented.

        As an additional example, this counter would not be
        incremented when an input tray is removed or the level of an
        input device changes."
    ::= { prtGeneralEntry 1 }

prtGeneralCurrentLocalization OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of the prtLocalizationIndex corresponding to the
        current language, country, and character set to be used for
        localized string values that are identified as being dependent
        on the value of this object.  Note that this object does not
        apply to localized strings in the prtConsole group or any
        object that is not identified as above."
    ::= { prtGeneralEntry 2 }

prtGeneralReset OBJECT-TYPE
    -- This value is a type 3 enumeration
    SYNTAX     INTEGER {
                   notResetting(3),
                   powerCycleReset(4), -- Cold Start
                   resetToNVRAM(5), -- Warm Start
                   resetToFactoryDefaults(6) -- Reset contents of
                                             -- NVRAM to factory defaults
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Setting this value to `powerCycleReset', `resetToNVRAM', or
        `resetToFactoryDefaults' will result in the resetting of the
        printer.  When read, this object will always have the value
        `notResetting(3)', and a SET of the value `notResetting' shall
        have no effect on the printer.  Some of the defined values are
        optional.  However, every implementation must support at least
        the values `notResetting' and resetToNVRAM'."
    ::= { prtGeneralEntry 3 }








-- The Cover Table
--
-- The cover portion of the General print sub-unit describes the
-- covers and interlocks of the printer.  The Cover Table has an
-- entry for each cover and interlock.

prtCover    OBJECT IDENTIFIER ::= { printmib 6 }

prtCoverTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtCoverEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of the covers and interlocks of the printer."
    ::= { prtCover 1 }

prtCoverEntry OBJECT-TYPE
    SYNTAX     PrtCoverEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Information about a cover or interlock.
        Entries may exist in the table for each device
        index whose device type is `printer'."
    INDEX  { hrDeviceIndex, prtCoverIndex }
    ::= { prtCoverTable 1 }

PrtCoverEntry ::= SEQUENCE {
    prtCoverIndex            Integer32,
    prtCoverDescription      OCTET STRING,
    prtCoverStatus           INTEGER
}

prtCoverIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this Cover
        sub-unit.  Although these values may change due to a major
        reconfiguration of the device (e.g. the addition of new
        cover sub-units to the printer), values are expected to
        remain stable across successive printer power cycles."
    ::= { prtCoverEntry 1 }

prtCoverDescription OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only





    STATUS     current
    DESCRIPTION
        "The manufacturer provided cover sub-mechanism  name in the
        localization specified by prtGeneralCurrentLocalization."
    ::= { prtCoverEntry 2 }

prtCoverStatus  OBJECT-TYPE
    --  This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   doorOpen(3),
                   doorClosed(4),
                   interlockOpen(5),
                   interlockClosed(6)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The status of this cover sub-unit."
    ::= { prtCoverEntry 3 }

-- The Localization Table
--

-- The localization portion of the General printer sub-unit is

-- responsible for identifying the natural language, country, and
-- character set in which character strings are expressed. There
-- may be one or more localizations supported per printer. The
-- available localizations are represented by the Localization table.

prtLocalization  OBJECT IDENTIFIER ::= { printmib 7 }

prtLocalizationTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtLocalizationEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The available localizations in this printer."
    ::= { prtLocalization 1 }

prtLocalizationEntry OBJECT-TYPE
    SYNTAX     PrtLocalizationEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A description of a localization.






        Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtLocalizationIndex }
    ::= { prtLocalizationTable 1 }

PrtLocalizationEntry ::= SEQUENCE {
        prtLocalizationIndex                Integer32,
        prtLocalizationLanguage             OCTET STRING,
        prtLocalizationCountry              OCTET STRING,
        prtLocalizationCharacterSet         CodedCharSet
}

prtLocalizationIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this
        localization entry.  Although these values may change due to a
        major reconfiguration of the device (e.g., the addition of new
        Cover sub-units to the printer), values are expected to remain
        stable across successive printer power cycles."
    ::= { prtLocalizationEntry 1 }

prtLocalizationLanguage OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..2))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A two character language code from ISO 639.  Examples EN, GB,
        CA, FR, DE."
    ::= { prtLocalizationEntry 2 }

prtLocalizationCountry OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..2))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A two character country code from ISO 3166, a blank string
        (two space characters) shall indicate that the country is
        not defined.  Examples: US, FR, DE, ..."
    ::= { prtLocalizationEntry 3 }

prtLocalizationCharacterSet OBJECT-TYPE
    SYNTAX     CodedCharSet
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION





        "The coded character set used for this localization."
    ::= { prtLocalizationEntry 4 }

-- The System Resources Tables

-- The Printer MIB makes use of the Host MIB to
-- define system resources by referencing the storage
-- and device groups of the print group.  In order to
-- determine, amongst multiple printers serviced by
-- one agent, which printer owns a particular
-- resource, the prtStorageRef and prtDeviceRef tables
-- associate particular storage and device entries to
-- printers.

prtStorageRefTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtStorageRefEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtGeneral 2 }

prtStorageRefEntry OBJECT-TYPE
    SYNTAX     PrtStorageRefEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table will have an entry for each entry in
        the host MIB storage table that represents storage associated
        with a printer managed by this agent."
    INDEX      { hrStorageIndex, prtStorageRefSeqNumber }
    ::= { prtStorageRefTable 1 }

PrtStorageRefEntry ::= SEQUENCE {
    prtStorageRefSeqNumber  Integer32,
    prtStorageRefIndex      Integer32
}

prtStorageRefSeqNumber OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This value will be unique amongst all entries with a common
        value of hrStorageIndex.

        This object allows a storage entry to point to the multiple
        printer devices with which it is associated."





    ::= { prtStorageRefEntry 1 }

prtStorageRefIndex OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of the hrDeviceIndex of the printer device that this
        storageEntry is associated with."
    ::= { prtStorageRefEntry 2 }

prtDeviceRefTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtDeviceRefEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtGeneral 3 }

prtDeviceRefEntry OBJECT-TYPE
    SYNTAX     PrtDeviceRefEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table will have an entry for each entry in
        the host MIB device table that represents a device associated
        with a printer managed by this agent."
    INDEX      { hrDeviceIndex, prtDeviceRefSeqNumber }
    ::= { prtDeviceRefTable 1 }

PrtDeviceRefEntry ::= SEQUENCE {
    prtDeviceRefSeqNumber   Integer32,
    prtDeviceRefIndex       Integer32
}

prtDeviceRefSeqNumber OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This value will be unique amongst all entries with a common
        value of hrDeviceIndex.

        This object allows a device entry to point to the multiple
        printer devices with which it is associated."
    ::= { prtDeviceRefEntry 1 }

prtDeviceRefIndex OBJECT-TYPE





    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of the hrDeviceIndex of the printer device that this
        deviceEntry is associated with."
    ::= { prtDeviceRefEntry 2 }

-- The Responsible Party group
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.

prtGeneralCurrentOperator OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name of the current human operator responsible for
        operating this printer. It is suggested that this string
        include information that would enable other humans to reach
        the operator, such as a phone number."
    ::= { prtGeneralEntry 4 }

prtGeneralServicePerson OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name of the last human responsible for servicing
        this printer. It is suggested that this string
        include information that would enable other humans to reach
        the service person, such as a phone number."
    ::= { prtGeneralEntry 5 }

-- The Input Group
--
-- Input sub-units are managed as a tabular, indexed collection of
-- possible devices capable of providing media for input to the printing
-- process.  Input sub-units typically have a location, a type, an
-- identifier, a set of constraints on possible media sizes and
-- potentially other media characteristics, and may be capable of
-- indicating current status or capacity.
--
-- Implementation of every object in this group is mandatory.


prtInput   OBJECT IDENTIFIER ::= { printmib 8 }





prtInputDefaultIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "The value of prtInputIndex corresponding to the default input
        sub-unit: that is, this object selects the default source of
        input media."
    ::= { prtGeneralEntry 6 }

prtInputTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtInputEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of the devices capable of providing media for input
        to the printing process."
    ::= { prtInput 2 }

prtInputEntry OBJECT-TYPE
    SYNTAX     PrtInputEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Attributes of a device capable of providing media for input
        to the printing process.

        Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtInputIndex }
    ::= { prtInputTable 1 }

PrtInputEntry ::= SEQUENCE {
        prtInputIndex                     Integer32,
        prtInputType                      INTEGER,
        prtInputDimUnit                   MediaUnit,
        prtInputMediaDimFeedDirDeclared   Integer32,
        prtInputMediaDimXFeedDirDeclared  Integer32,
        prtInputMediaDimFeedDirChosen     Integer32,
        prtInputMediaDimXFeedDirChosen    Integer32,
        prtInputCapacityUnit              CapacityUnit,
        prtInputMaxCapacity               Integer32,
        prtInputCurrentLevel              Integer32,
        prtInputStatus                    SubUnitStatus,
        prtInputMediaName                 OCTET STRING,
        prtInputName                      OCTET STRING,
        prtInputVendorName                OCTET STRING,
        prtInputModel                     OCTET STRING,





        prtInputVersion                   OCTET STRING,
        prtInputSerialNumber              OCTET STRING,
        prtInputDescription               OCTET STRING,
        prtInputSecurity                  PresentOnOff,
        prtInputMediaWeight               Integer32,
        prtInputMediaType                 OCTET STRING,
        prtInputMediaColor                OCTET STRING,
        prtInputMediaFormParts            Integer32
}

prtInputIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this input
        sub-unit. Although these values may change due to a major
        reconfiguration of the device (e.g. the addition of new
        input sub-units to the printer), values are expected to
        remain stable across successive printer power cycles."
    ::= { prtInputEntry 1 }

prtInputType OBJECT-TYPE
    --  This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   unknown(2),
                   sheetFeedAutoRemovableTray(3),
                   sheetFeedAutoNonRemovableTray(4),
                   sheetFeedManual(5),
                   continuousRoll(6),
                   continuousFanFold(7)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of technology (discriminated primarily according to
        feeder mechanism type) employed by the input sub-unit.  Note,
        the Optional Input Class provides for a descriptor field to
        further qualify the other choice."
    ::= { prtInputEntry 2 }

prtInputDimUnit OBJECT-TYPE
    SYNTAX     MediaUnit
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measurement for use calculating and relaying





        dimensional values for this input sub-unit."
    ::= { prtInputEntry 3 }

prtInputMediaDimFeedDirDeclared OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object provides the value of the declared dimension, in
        the feed direction, of the media that is (or, if empty, was or
        will be) in this input sub-unit.  The feed direction is the
        direction in which the media is fed on this sub-unit.  This
        dimension is measured in input sub-unit dimensional units
        (prtInputDimUnit).  If this input sub-unit can reliably sense
        this value, the value is sensed by the printer and may not be
        changed by management requests.  Otherwise, the value may be
        changed. The value (-1) means other and specifically means
        that this sub-unit places no restriction on this parameter.
        The value (-2) indicates unknown."
    ::= { prtInputEntry 4 }

prtInputMediaDimXFeedDirDeclared OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object provides the value of the declared dimension, in
        the cross feed direction, of the media that is (or, if empty,
        was or will be) in this input sub-unit.  The cross  feed
        direction is ninety degrees relative to the feed direction
        associated with this sub-unit. This dimension is measured in
        input sub-unit dimensional units (prtInputDimUnit).  If this
        input sub-unit can reliably sense this value, the value is
        sensed by the printer and may not be changed by management
        requests. Otherwise, the value may be changed. The value (-1)
        means other and specifically means that this sub-unit places
        no restriction on this parameter. The value (-2) indicates
        unknown."
    ::= { prtInputEntry 5 }

prtInputMediaDimFeedDirChosen OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The printer will act as if media of the chosen dimension (in
        the feed direction) is present in this input source.  Note
        that this value will be used even if the input tray is empty.





        Feed dimension measurements
        are taken parallel relative to the feed direction
        associated with that sub-unit and are in input sub-unit
        dimensional units (DimUnit). If the printer supports the
        declared dimension, the granted dimension is the same as
        the declared dimension. If not, the granted dimension is
        set to the closest dimension that the printer supports
        when the declared dimension is set. The value (-1) means
        other and specifically indicates that this sub-unit
        places no restriction on this parameter. The value (-2)
        indicates unknown."
    ::= { prtInputEntry 6 }

prtInputMediaDimXFeedDirChosen OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The printer will act as if media of the chosen dimension (in
        the cross feed direction) is present in this input source.
        Note that this value will be used even if the input tray is
        empty.  The cross feed direction is ninety degrees relative
        to the feed direction associated with this sub-unit. This
        dimension is measured in input sub-unit dimensional units
        (DimUnit).  If the printer supports the declared
        dimension, the granted dimension is the same as the
        declared dimension. If not, the granted dimension is set
        to the closest dimension that the printer supports when
        the declared dimension is set. The value (-1) means other
        and specifically indicates that this sub-unit places no
        restriction on this parameter.  The value (-2) indicates
        unknown."
    ::= { prtInputEntry 7 }

prtInputCapacityUnit OBJECT-TYPE
    SYNTAX     CapacityUnit
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measurement for use in calculating and relaying
        capacity values for this input sub-unit."
    ::= { prtInputEntry 8 }

prtInputMaxCapacity OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION





        "The maximum capacity of the input sub-unit in input
        sub-unit capacity units (CapacityUnit).  There is no
        convention associated with the media itself so this value
        reflects claimed capacity. If this input sub-unit can
        reliably sense this value, the value is sensed by the
        printer and may not be changed by management requests;
        otherwise, the value may be written (by a Remote
        Contol Panel or a Management Application).
        The value (-1) means other and specifically
        indicates that the sub-unit places no restrictions
        on this parameter.  The value (-2) means unknown."
    ::= { prtInputEntry 9 }

prtInputCurrentLevel OBJECT-TYPE
    SYNTAX     Integer32 --    in capacity units (CapacityUnit).
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The current capacity of the input sub-unit in input
        sub-unit capacity units (CapacityUnit). If this input
        sub-unit can reliably sense this value, the value is
        sensed by the printer and may not be changed by
        management requests; otherwise, the value may
        be written (by a Remote Contol Panel or a
        Management Application).  The value (-1) means other and
        specifically indicates that the sub-unit places no
        restrictions on this parameter. The value (-2) means unknown.
        The value (-3) means that the printer knows that at least one
        unit remains."
    ::= { prtInputEntry 10 }

prtInputStatus OBJECT-TYPE
    SYNTAX     SubUnitStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current status of this input sub-unit."
    ::= { prtInputEntry 11 }

prtInputMediaName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "A description of the media contained in this input sub-unit;
        This description is intended for display to a human operator.
        This description is not processed by the printer.  It is used
        to provide information not expressible in terms of the other





        media attributes (e.g. prtInputMediaDimFeedDirChosen,
        prtInputMediaDimXFeedDirChosen, prtInputMediaWeight,
        prtInputMediaType). An example would be `legal tender bond
        paper'."
    ::= { prtInputEntry 12 }

--               INPUT MEASUREMENT
--
--     _______ |                     |
--      ^      |                     |
--      |      |                     |                    |
--      |      |_ _ _ _ _ _ _ _ _ _ _| _________________  |direction
--      |      |                     |      ^             v
-- MaxCapacity |                     |      |
--      |      | Sheets left in tray | CurrentLevel
--      |      |                     |      |
--      v      |                     |      v
--     _______ +_____________________+ _______

-- The Extended Input Group
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.


prtInputName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name assigned to this input sub-unit."
    ::= { prtInputEntry 13 }

prtInputVendorName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The vendor name of this input sub-unit."
    ::= { prtInputEntry 14 }

prtInputModel OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The model name of this input sub-unit."
    ::= { prtInputEntry 15 }





prtInputVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The version of this input sub-unit."
    ::= { prtInputEntry 16 }

prtInputSerialNumber OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..32))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The serial number assigned to this input sub-unit."
    ::= { prtInputEntry 17 }

prtInputDescription OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A free-form text description of this input
        sub-unit in the localization specified by
        prtGeneralCurrentLocalization."
    ::= { prtInputEntry 18 }

prtInputSecurity OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Indicates if this input sub-unit has some security
        associated with it."
    ::= { prtInputEntry 19 }

-- The Input Media Group
--
-- The Input Media Group supports identification of media installed
-- or available for use on a printing device. Medium resources are
-- identified by name, and include a collection of characteristic
-- attributes that may further be used for selection and management
-- of them. The Input Media group consists of a set of optional
-- "columns" in the Input Table. In this manner, a minimally
-- conforming implementation may choose to not support reporting
-- of media resources if it cannot do so.
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.





prtInputMediaWeight  OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The weight of the medium associated with this input
        sub-unit in grams / per meter squared. The value (-2) means
        unknown."
    ::= { prtInputEntry 20 }

prtInputMediaType OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name of the type of medium associated with this input
        sub-unit. This name need not be processed by the printer; it
        might simply be displayed to an operator. The standardized
        string values from ISO 10175 (DPA) and ISO 10180 (SPDL) are:

        stationery       Separately cut sheets of an opaque material
        transparency     Separately cut sheets of a transparent material
        envelope         Envelopes that can be used for conventional
        mailing purposes
        envelope-plain   Envelopes that are not preprinted and have no
                         windows
        envelope-window  Envelopes that have windows for addressing
                         purposes
        continuous-long  Continuously connected sheets of an opaque
                         material connected along the long edge
        continuous-short Continuously connected sheets of an opaque
                         material connected along the short edge
        tab-stock        Media with tabs
        multi-part-form  Form medium composed of multiple layers not
                         pre-attached to one another; each sheet may be
                         drawn separately from an input source
        labels           Label stock
        multi-layer      Form medium composed of multiple layers which
                         are pre-attached to one another; e.g., for
                         use with impact printers"
    ::= { prtInputEntry 21 }

prtInputMediaColor OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name of the color of the medium associated with





        this input sub-unit using standardized string values
        from ISO 10175 (DPA) and ISO 10180 (SPDL) which are:

        other
        unknown
        white
        pink
        yellow
        buff
        goldenrod
        blue
        green
        transparent

        Implementors may add additional string values. The naming
        conventions in ISO 9070 are recommended in order to avoid
        potential name clashes."
    ::= { prtInputEntry 22 }

prtInputMediaFormParts OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "The number of parts associated with the medium
         associated with this input sub-unit if the medium is a
         multi-part form.  The value (-1) means other and
         specifically indicates that the device places no
         restrictions on this parameter.  The value (-2) means
         unknown."
    ::= { prtInputEntry 23 }

-- The Output Group
--
-- Output sub-units are managed as a tabular, indexed collection of
-- possible devices capable of receiving media delivered from the
-- printing process.  Output sub-units typically have a location,
-- a type, an identifier, a set of constraints on possible media
-- sizes and potentially other characteristics, and may be capable
-- of indicating current status or capacity.
--
-- Implementation of every object in this group is mandatory.

prtOutput  OBJECT IDENTIFIER ::= { printmib 9 }

prtOutputDefaultIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write





    STATUS     current
    DESCRIPTION
        "The  value of prtOutputIndex  corresponding to the default
        output sub-unit; that is, this object selects the default
        output destination."
    ::= { prtGeneralEntry 7 }

prtOutputTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtOutputEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of the devices capable of receiving media delivered
        from the printing process."
    ::= { prtOutput 2 }

prtOutputEntry OBJECT-TYPE
    SYNTAX     PrtOutputEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Attributes of a device capable of receiving media delivered
        from the printing process.

        Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtOutputIndex }
    ::= { prtOutputTable 1 }

PrtOutputEntry ::= SEQUENCE {
        prtOutputIndex                    Integer32,
        prtOutputType                     INTEGER,
        prtOutputCapacityUnit             CapacityUnit,
        prtOutputMaxCapacity              Integer32,
        prtOutputRemainingCapacity        Integer32,
        prtOutputStatus                   SubUnitStatus,
        prtOutputName                     OCTET STRING,
        prtOutputVendorName               OCTET STRING,
        prtOutputModel                    OCTET STRING,
        prtOutputVersion                  OCTET STRING,
        prtOutputSerialNumber             OCTET STRING,
        prtOutputDescription              OCTET STRING,
        prtOutputSecurity                 PresentOnOff,
        prtOutputDimUnit                  MediaUnit,
        prtOutputMaxDimFeedDir            Integer32,
        prtOutputMaxDimXFeedDir           Integer32,
        prtOutputMinDimFeedDir            Integer32,
        prtOutputMinDimXFeedDir           Integer32,





        prtOutputStackingOrder            INTEGER,
        prtOutputPageDeliveryOrientation  INTEGER,
        prtOutputBursting                 PresentOnOff,
        prtOutputDecollating              PresentOnOff,
        prtOutputPageCollated             PresentOnOff,
        prtOutputOffsetStacking           PresentOnOff
}

prtOutputIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by this printer to identify this
        output sub-unit. Although these values may change due
        to a major reconfiguration of the sub-unit (e.g.  the
        addition of new output devices to the printer), values
        are expected to remain stable across successive printer
        power cycles."
    ::= { prtOutputEntry 1 }

prtOutputType OBJECT-TYPE
    -- This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   unknown(2),
                   removableBin(3),
                   unRemovableBin(4),
                   continuousRollDevice(5),
                   mailBox(6),
                   continuousFanFold(7)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of technology supported by this output sub-unit."
    ::= { prtOutputEntry 2 }

prtOutputCapacityUnit OBJECT-TYPE
    SYNTAX     CapacityUnit
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measurement for use in calculating and relaying
        capacity values for this output sub-unit."
    ::= { prtOutputEntry 3 }

prtOutputMaxCapacity OBJECT-TYPE





    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The maximum capacity of this output sub-unit in output
        sub-unit capacity units (CapacityUnit). There is no
        convention associated with the media itself so this value
        essentially reflects claimed capacity. If this output
        sub-unit can reliably sense this value, the value is
        sensed by the printer and may not be changed by management
        requests; otherwise, the value may be written
        (by a Remote Contol Panel or a Management Application).
        The value (-1) means other and specifically indicates
        that the sub-unit places no restrictions on this parameter.
        The value (-2) means unknown."
    ::= { prtOutputEntry 4 }

prtOutputRemainingCapacity OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The remaining capacity of the possible output sub-unit
        capacity in output sub-unit capacity units (CapacityUnit)
        of this output sub-unit. If this output sub-unit can
        reliably sense this value, the value is sensed by the
        printer and may not be modified by management requests;
        otherwise, the value may be written (by
        a Remote Contol Panel or a Management
        Application).  The value (-1) means other and
        specifically indicates that the sub-unit places no
        restrictions on this parameter.  The value (-2) means
        unknown.  The value (-3) means that the printer knows that
        there remains capacity for at least one unit."
    ::= { prtOutputEntry 5 }

prtOutputStatus OBJECT-TYPE
    SYNTAX     SubUnitStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current status of this output sub-unit."
    ::= { prtOutputEntry 6 }










--               OUTPUT MEASUREMENT
--
--     _______ |                     | _______
--      ^      |                     |      ^
--      |      |                     |      |
--      |      |                     | RemainingCapacity
-- MaxCapacity |                     |      |
--      |      |                     |      v               ^
--      |      |_ _ _ _ _ _ _ _ _ _ _| ___________________  |direction
--      |      |                     |                      |
--      |      |  Sheets in output   |
--      v      |                     |
--     _______ +_____________________+

-- The Extended Output Group
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.

prtOutputName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The name assigned to this output sub-unit."
    ::= { prtOutputEntry 7 }

prtOutputVendorName OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The vendor name of this output sub-unit."
    ::= { prtOutputEntry 8 }

prtOutputModel OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The name assigned to this output sub-unit."
    ::= { prtOutputEntry 9 }

prtOutputVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION





        "The version of this output sub-unit."
    ::= { prtOutputEntry 10 }

prtOutputSerialNumber OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The serial number assigned to this output sub-unit."
    ::= { prtOutputEntry 11 }

prtOutputDescription OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "  A free-form text description of this output sub-unit in the
        localization specified by prtGeneralCurrentLocalization."
    ::= { prtOutputEntry 12 }

prtOutputSecurity OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Indicates if this output sub-unit has some security associated
        with it and if that security is enabled or not."
    ::= { prtOutputEntry 13 }

-- The Output Dimensions Group
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.

prtOutputDimUnit OBJECT-TYPE
    SYNTAX     MediaUnit
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measurement for use in calculating and relaying
        dimensional values for this output sub-unit."
    ::= { prtOutputEntry 14 }

prtOutputMaxDimFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION





        "The maximum dimensions supported by this output sub-unit
        for measurements taken parallel relative to the feed
        direction associated with that sub-unit in output
        sub-unit dimensional units (DimUnit). If this output
        sub-unit can reliably sense this value, the value is
        sensed by the printer and may not be changed with
        management protocol operations."
    ::= { prtOutputEntry 15 }

prtOutputMaxDimXFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The maximum dimensions supported by this output sub-unit
        for measurements taken ninety degrees relative to the
        feed direction associated with that sub-unit in output
        sub-unit dimensional units (DimUnit). If this output
        sub-unit can reliably sense this value, the value is
        sensed by the printer and may not be changed with
        management protocol operations."
    ::= { prtOutputEntry 16 }

prtOutputMinDimFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The minimum dimensions supported by this output sub-unit
        for measurements taken parallel relative to the feed
        direction associated with that sub-unit in output
        sub-unit dimensional units (DimUnit).  If this output
        sub-unit can reliably sense this value, the value is
        sensed by the printer and may not be changed with
        management protocol operations."
    ::= { prtOutputEntry 17 }

prtOutputMinDimXFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The minimum dimensions supported by this output sub-unit
        for measurements taken ninety degrees relative to the
        feed direction associated with that sub-unit in output
        sub-unit dimensional units (DimUnit). If this output
        sub-unit can reliably sense this value, the value is
        sensed by the printer and may not be changed with





        management protocol operations."
    ::= { prtOutputEntry 18 }

-- The Output Features Group
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.

prtOutputStackingOrder OBJECT-TYPE
    --  This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   unknown(2),
                   firstToLast(3),
                   lastToFirst(4)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The current state of the stacking order for the
        associated output sub-unit. `FirstToLast' means
        that as pages are output the front of the next page is
        placed against the back of the previous page.
        `LasttoFirst' means that as pages are output the back
        of the next page is placed against the front of the
        previous page."
    ::= { prtOutputEntry 19 }

prtOutputPageDeliveryOrientation OBJECT-TYPE
    --   This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   faceUp(3),
                   faceDown(4)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The reading surface that will be `up' when pages are
        delivered to the associated output sub-unit. Values are
        Face-Up and Face-Down. (Note: interpretation of these
        values is in general context-dependent based on locale;
        presentation of these values to an end-user should be
        normalized to the expectations of the user)."
    ::= { prtOutputEntry 20 }

prtOutputBursting OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current





    DESCRIPTION
        "This object indicates that the outputing sub-unit
        supports bursting, and if so, whether the feature is enabled.
        Bursting is the process by which continuous media is separated
        into individual sheets, typically by bursting along pre-formed
        perforations."
    ::= { prtOutputEntry 21 }

prtOutputDecollating OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object indicates that the output supports
        supports decollating, and if so, whether the feature
        is enabled. Decollating is the process by which the
        individual parts within a multi-part form are separated
        and sorted into separate stacks for each part."
    ::= { prtOutputEntry 22 }

prtOutputPageCollated OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object indicates that the output sub-unit
        supports page collation, and if so, whether the feature is
        enabled."
    ::= { prtOutputEntry 23 }

prtOutputOffsetStacking OBJECT-TYPE
    SYNTAX     PresentOnOff
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object indicates that the output supports
        supports offset stacking, and if so, whether the feature is
        enabled."
    ::= { prtOutputEntry 24 }

-- The Marker Group
--
-- A marker is the mechanism that produces marks on the print media.  The
-- marker sub-units and their associated supplies are represented by the
-- Marker Group in the model.  A printer can contain one or more marking
-- mechanisms.  Some examples of multiple marker sub-units are: a printer
-- with separate markers for normal and magnetic ink or an imagesetter
-- that can output to both a proofing device and final film. Each marking





-- device can have its own set of  characteristics associated with it,
-- such as marking technology and resolution.
--
-- Implementation of every object in this group is mandatory.


prtMarker OBJECT IDENTIFIER ::= { printmib 10 }

prtMarkerDefaultIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtMarkerIndex  corresponding to the
        default markersub-unit; that is, this object selects the
        default marker."
    ::= { prtGeneralEntry 8 }

-- The printable area margins as listed below define an area of the print
-- media which is guaranteed to be printable for all combinations of
-- input, media paths, and interpreters for this marker.

prtMarkerTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtMarkerEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtMarker 2 }

prtMarkerEntry OBJECT-TYPE
    SYNTAX     PrtMarkerEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtMarkerIndex }
    ::= { prtMarkerTable 1 }

PrtMarkerEntry ::= SEQUENCE {
        prtMarkerIndex                  Integer32,
        prtMarkerMarkTech               INTEGER,
        prtMarkerCounterUnit            INTEGER,
        prtMarkerLifeCount              Counter32,
        prtMarkerPowerOnCount           Counter32,
        prtMarkerProcessColorants       Integer32,
        prtMarkerSpotColorants          Integer32,





        prtMarkerAddressabilityUnit     INTEGER,
        prtMarkerAddressabilityFeedDir  Integer32,
        prtMarkerAddressabilityXFeedDir Integer32,
        prtMarkerNorthMargin            Integer32,
        prtMarkerSouthMargin            Integer32,
        prtMarkerWestMargin             Integer32,
        prtMarkerEastMargin             Integer32,
        prtMarkerStatus                 SubUnitStatus
}


prtMarkerIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this marking
        SubUnitStatus.  Although these values may change due to a major
        reconfiguration of the device (e.g. the addition of new marking
        sub-units to the printer), values are expected to remain
        stable across successive printer power cycles."
    ::= { prtMarkerEntry 1 }

prtMarkerMarkTech OBJECT-TYPE
    -- This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   unknown(2),
                   electrophotographicLED(3),
                   electrophotographicLaser(4),
                   electrophotographicOther(5),
                   impactMovingHeadDotMatrix9pin(6),
                   impactMovingHeadDotMatrix24pin(7),
                   impactMovingHeadDotMatrixOther(8),
                   impactMovingHeadFullyFormed(9),
                   impactBand(10),
                   impactOther(11),
                   inkjetAqueous(12),
                   inkjetSolid(13),
                   inkjetOther(14),
                   pen(15),
                   thermalTransfer(16),
                   thermalSensitive(17),
                   thermalDiffusion(18),
                   thermalOther(19),
                   electroerosion(20),
                   electrostatic(21),
                   photographicMicrofiche(22),





                   photographicImagesetter(23),
                   photographicOther(24),
                   ionDeposition(25),
                   eBeam(26),
                   typesetter(27)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of marking technology used for this marking sub-unit."
    ::= { prtMarkerEntry 2 }

prtMarkerCounterUnit OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   tenThousandthsOfInches(3),  -- .0001
                   micrometers(4),
                   characters(5),
                   lines(6),
                   impressions(7),
                   sheets(8),
                   dotRow(9),
                   hours(11),
                   feet(16),
                   meters(17)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit that will be used by the printer when reporting
        counter values for this marking sub-unit.  The
        time units of measure are provided for a device like a
        strip recorder that does not or cannot track the physical
        dimensions of the media and does not use characters,
        lines or sheets."
    ::= { prtMarkerEntry 3}

prtMarkerLifeCount OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The count of the number of units of measure counted during
        the life of printer using units of measure as specified by
        CounterUnit."
    ::= { prtMarkerEntry 4 }

prtMarkerPowerOnCount OBJECT-TYPE





    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The count of the number of units of measure counted since the
        equipment was most recently powered on using units of measure as
        specified by CounterUnit."
    ::= { prtMarkerEntry 5 }

prtMarkerProcessColorants OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of process colors supported by this marker.  A
        process color of 1 implies monochrome.  The value of this
        object and SpotColorants cannot both be 0.  Must be 0 or
        greater."
    ::= { prtMarkerEntry 6 }

prtMarkerSpotColorants OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of spot colors supported by this marker.  The
        value of this object and ProcessColorants cannot
        both be 0.  Must be 0 or greater."
    ::= { prtMarkerEntry 7 }

prtMarkerAddressabilityUnit OBJECT-TYPE
    --   This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   tenThousandthsOfInches(3),  -- .0001
                   micrometers(4)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The unit of measure of distances."
    ::= { prtMarkerEntry 8 }

prtMarkerAddressabilityFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The  number of addressable marking positions in the feed





        direction per 10000 units of measure specified by
        AddressabilityUnit.  A value of (-1) implies 'other' or
        'infinite' while a value of (-2) implies 'unknown'."
    ::= { prtMarkerEntry 9 }

prtMarkerAddressabilityXFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of addressable marking positions in the cross
        feed direction in 10000 units of measure specified by
        AddressabilityUnit.  A value of (-1) implies 'other' or
        'infinite' while a value of (-2) implies 'unknown'."
    ::= { prtMarkerEntry 10 }

prtMarkerNorthMargin OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The margin, in units identified by AddressabilityUnit,
        from the leading edge of the medium as the medium flows
        throught the marking engine with the side to be imaged
        facing the observer. The leading edge is the North edge
        and the other edges are defined by the normal compass
        layout of  directions with the compass facing the
        observer.  Printing within the area bounded by all four
        margins is guaranteed for all interpreters.   The value
        (-2) means unknown."
    ::= { prtMarkerEntry 11 }

prtMarkerSouthMargin OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The margin from the South edge  (see NorthMargin)
        of the medium in units identified by
        AddressabilityUnit.  Printing within the area bounded by
        all four margins  is guaranteed for all interpreters.
        The value (-2) means unknown."
    ::= { prtMarkerEntry 12 }

prtMarkerWestMargin OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current





    DESCRIPTION
        "The margin from the West edge (see NorthMargin) of the
        medium in units identified by AddressabilityUnit.
        Printing within the area bouned by all four margins is
        guaranteed for all interpreters.   The value (-2) means
        unknown."
    ::= { prtMarkerEntry 13 }

prtMarkerEastMargin OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The margin from the East edge (see NorthMargin) of the
        medium in units identified by AddressabilityUnit.
        Printing within the area bounded by all four margins is
        guaranteed for all interpreters. The value (-2) means
        unknown."
    ::= { prtMarkerEntry 14 }

prtMarkerStatus OBJECT-TYPE
    SYNTAX     SubUnitStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current status of this marker sub-unit."
        ::= { prtMarkerEntry 15 }

-- The Marker Supplies Group
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.

prtMarkerSupplies OBJECT IDENTIFIER ::= { printmib 11 }

prtMarkerSuppliesTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtMarkerSuppliesEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of the marker supplies available on this printer."
    ::= { prtMarkerSupplies 1 }

prtMarkerSuppliesEntry OBJECT-TYPE
    SYNTAX     PrtMarkerSuppliesEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION





        "Attributes of a marker supply.

        Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtMarkerSuppliesIndex }
    ::= { prtMarkerSuppliesTable 1 }

PrtMarkerSuppliesEntry ::= SEQUENCE {
        prtMarkerSuppliesIndex          Integer32,
        prtMarkerSuppliesMarkerIndex    Integer32,
        prtMarkerSuppliesColorantIndex  Integer32,
        prtMarkerSuppliesClass          INTEGER,
        prtMarkerSuppliesType           INTEGER,
        prtMarkerSuppliesDescription    OCTET STRING,
        prtMarkerSuppliesSupplyUnit     INTEGER,
        prtMarkerSuppliesMaxCapacity    Integer32,
        prtMarkerSuppliesLevel          Integer32
}


prtMarkerSuppliesIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this marker
        supply.  Although these values may change due to a major
        reconfiguration of the device (e.g. the addition of new marker
        supplies to the printer), values are expected to remain stable
        across successive printer power cycles."
    ::= { prtMarkerSuppliesEntry 1 }

prtMarkerSuppliesMarkerIndex OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of prtMarkerIndex corresponding to the
        marking sub-unit with which this marker supply
        sub-unit is associated."
    ::= { prtMarkerSuppliesEntry 2 }

prtMarkerSuppliesColorantIndex OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of prtMarkerColorantIndex





        corresponding to the colorant with which this
        marker supply sub-unit is associated.  This value
        shall be 0 if there is no colorant table."
    ::= { prtMarkerSuppliesEntry 3 }

prtMarkerSuppliesClass OBJECT-TYPE
    --  This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   supplyThatIsConsumed(3),
                   receptacleThatIsFilled(4)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Indicates whether this supply entity represents a supply
        container that is consumed or a receptacle that is filled."
    ::= { prtMarkerSuppliesEntry 4 }

prtMarkerSuppliesType OBJECT-TYPE
    --   This value is a type 3 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   unknown(2),
                   toner(3),
                   wasteToner(4),
                   ink(5),
                   inkCartridge(6),
                   inkRibbon(7),
                   wasteInk(8),
                   opc(9),
                   developer(10),
                   fuserOil(11),
                   solidWax(12),
                   ribbonWax(13),
                   wasteWax(14)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of this supply."
    ::= { prtMarkerSuppliesEntry 5 }

prtMarkerSuppliesDescription OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION





        "The description of this supply container/receptacle in the
        localization specified by prtGeneralCurrentLocalization."
    ::= { prtMarkerSuppliesEntry 6 }

prtMarkerSuppliesSupplyUnit OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   tenThousandthsOfInches(3),  -- .0001
                   micrometers(4),
                   thousandthsOfOunces(12),
                   tenthsOfGrams(13),
                   hundrethsOfFluidOunces(14),
                   tenthsOfMilliliters(15)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Unit of this marker supply container/receptacle."
    ::= { prtMarkerSuppliesEntry 7 }

prtMarkerSuppliesMaxCapacity OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The maximum capacity of this supply container/receptacle
        expressed in SupplyUnit. If this supply
        container/receptacle can reliably sense this value, the
        value is sensed by the printer and is read-only;
        otherwise, the value may be written (by a Remote Contol
        Panel or a Management Application). The value (-1) means
        other and specifically indicates that the sub-unit places
        no restrictions on this parameter. The value (-2) means
        unknown."
    ::= { prtMarkerSuppliesEntry 8 }

prtMarkerSuppliesLevel OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The current level if this supply is a container; the
        remaining space if this supply is a receptacle. If this
        supply container/receptacle can reliably sense this
        value, the value is sensed by the printer and is
        read-only; otherwise, the value may be written (by a
        Remote Contol Panel or a Management Application). The
        value (-1) means other and specifically indicates that





        the sub-unit places no restrictions on this parameter.
        The value (-2) means unknown.  A value of (-3) means that the
        printer knows that there is some supply/remaining space,
        respectively."
    ::= { prtMarkerSuppliesEntry 9 }

-- The Marker Colorant Group
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.

prtMarkerColorant OBJECT IDENTIFIER ::= { printmib 12 }

prtMarkerColorantTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtMarkerColorantEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of all of the colorants available on the printer."
    ::= { prtMarkerColorant 1 }

prtMarkerColorantEntry OBJECT-TYPE
    SYNTAX     PrtMarkerColorantEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Attributes of a colorant available on the printer.

        Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX { hrDeviceIndex, prtMarkerColorantIndex }
    ::= { prtMarkerColorantTable 1 }

PrtMarkerColorantEntry ::= SEQUENCE {
        prtMarkerColorantIndex          Integer32,
        prtMarkerColorantMarkerIndex    Integer32,
        prtMarkerColorantRole           INTEGER,
        prtMarkerColorantValue          OCTET STRING,
        prtMarkerColorantTonality       Integer32
}

prtMarkerColorantIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this colorant.
        Although these values may change due to a major





        reconfiguration of the device (e.g. the addition of new
        colorants to the printer), values are expected to remain
        stable across successive printer power cycles."
    ::= { prtMarkerColorantEntry 1 }

prtMarkerColorantMarkerIndex OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of prtMarkerIndex corresponding to the
        marker sub-unit with which this colorant entry is
        associated."
    ::= { prtMarkerColorantEntry 2 }

prtMarkerColorantRole OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER { --  Colorant Role
                   other(1),
                   process(3),
                   spot(4)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The role played by this colorant."
    ::= { prtMarkerColorantEntry 3 }

prtMarkerColorantValue OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The name of the color of this The name of the color of this
        colorant using standardized string names from ISO 10175 (DPA)
        and ISO 10180 (SPDL) which are:
          other
          unknown
          white
          red
          green
          blue
          cyan
          magenta
          yellow
          black
        Implementors may add additional string values. The naming
        conventions in ISO 9070 are recommended in order to avoid





        potential name clashes"
    ::= { prtMarkerColorantEntry 4 }

prtMarkerColorantTonality OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The distinct levels of tonality realizable by a marking
        sub-unit when using this colorant.  This value does not
        include the number of levels of tonal difference that an
        interpreter can obtain by techniques such as half toning.
        This value must be at least 2."
    ::= { prtMarkerColorantEntry 5 }

-- The Media Path Group
--
-- The media paths encompass the mechanisms in the printer that move the
-- media through the printer and connect all other media related sub-
-- units: inputs, outputs, markers and finishers. A printer contains one
-- or more media paths. These are represented by the Media Path Group in
-- the model. The Media Path group has some attributes that apply to all
-- paths plus a table of the separate media paths.

prtMediaPath OBJECT IDENTIFIER ::= { printmib 13 }

prtMediaPathDefaultIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtMediaPathIndex corresponding to
        the default media path; that is, the selection of the
        default media path."
    ::= { prtGeneralEntry 9 }

prtMediaPathTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtMediaPathEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtMediaPath 4 }

prtMediaPathEntry OBJECT-TYPE
    SYNTAX     PrtMediaPathEntry
    MAX-ACCESS not-accessible
    STATUS     current





    DESCRIPTION
        "Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtMediaPathIndex }
    ::= { prtMediaPathTable 1 }

PrtMediaPathEntry ::= SEQUENCE {
    prtMediaPathIndex               Integer32,
    prtMediaPathMaxSpeedPrintUnit   INTEGER,
    prtMediaPathMediaSizeUnit       MediaUnit,
    prtMediaPathMaxSpeed            Integer32,
    prtMediaPathMaxMediaFeedDir     Integer32,
    prtMediaPathMaxMediaXFeedDir    Integer32,
    prtMediaPathMinMediaFeedDir     Integer32,
    prtMediaPathMinMediaXFeedDir    Integer32,
    prtMediaPathType                INTEGER,
    prtMediaPathDescription         OCTET STRING,
    prtMediaPathStatus              SubUnitStatus
}


prtMediaPathIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this media
        path. Although these values may change due to a major
        reconfiguration of the device (e.g. the addition of new
        media paths to the printer), values are expected to remain
        stable across successive printer power
        cycles."
    ::= { prtMediaPathEntry 1 }

prtMediaPathMaxSpeedPrintUnit OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   tenThousandthsOfInchesPerHour(3),   -- .0001/hour
                   micrometersPerHour(4),
                   charactersPerHour(5),
                   linesPerHour(6),
                   impressionsPerHour(7),
                   sheetsPerHour(8),
                   dotRowPerHour(9),
                   feetPerHour(16),
                   metersPerHour(17)
               }
    MAX-ACCESS read-only





    STATUS     current
    DESCRIPTION
        "The unit of measure used in specifying the speed of all media
        paths in the printer."
    ::= { prtMediaPathEntry 2 }

prtMediaPathMediaSizeUnit OBJECT-TYPE
    SYNTAX     MediaUnit
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The units of measure of media size for use in calculating and
        relaying dimensional values for all media paths in the printer."
    ::= { prtMediaPathEntry 3 }

prtMediaPathMaxSpeed OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum printing speed of this media path expressed in
        prtMediaPathMaxSpeedUnit's.  A value of (-1) implies
        'other'."
    ::= { prtMediaPathEntry 4 }

prtMediaPathMaxMediaFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum physical media size in the feed direction of this
        media path expressed in units of measure specified by
        MediaSizeUnit.  A value of (-1) implies 'unlimited'.  A value
        of (-2) implies 'unknown'"
    ::= { prtMediaPathEntry 5 }

prtMediaPathMaxMediaXFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum physical media size across the feed direction of
        this media path expressed in units of measure specified by
        MediaSizeUnit.  A value of (-2) implies 'unknown'."
    ::= { prtMediaPathEntry 6 }

prtMediaPathMinMediaFeedDir OBJECT-TYPE
    SYNTAX     Integer32





    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The minimum physical media size in the feed direction of this
        media path expressed in units of measure specified by
        MediaSizeUnit. A value of (-2) implies 'unknown'."
    ::= { prtMediaPathEntry 7 }

prtMediaPathMinMediaXFeedDir OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The minimum physical media size across the feed direction of
        this media path expressed in units of measure specified by
        MediaSizeUnit.  A value of (-2) implies 'unknown'."
    ::= { prtMediaPathEntry 8 }

prtMediaPathType OBJECT-TYPE
    --   This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   unknown(2),
                   longEdgeBindingDuplex(3),
                   shortEdgeBindingDuplex(4),
                   simplex(5)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of the media path for this media path."
    ::= { prtMediaPathEntry 9 }

prtMediaPathDescription OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The manufacturer-provided description of this media path in
        the localization specified by prtGeneralCurrentLocalization."
    ::= { prtMediaPathEntry 10 }

prtMediaPathStatus OBJECT-TYPE
    SYNTAX     SubUnitStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current status of this media path."





    ::= { prtMediaPathEntry 11 }

-- The Channel Group
--
-- Implementation of every object in this group is mandatory.

-- Channels are independent sources of print data. Here,
-- print data is the term used for the information that is
-- used to construct printed pages and may have both data
-- and control aspects. The output of a channel is in a form
-- suitable for input to one of the interpreters as a
-- stream. A channel may be independently enabled (allowing
-- print data to flow) or disabled (stopping the flow of
-- print data). A printer may have one or more channels.
--
-- Basically, the channel abstraction is intended to cover
-- all the aspects of getting the print data to an
-- interpreter. This might include transporting the data
-- from one place to another, it might include (invisible)
-- compression, it might include encoding or packetizing to
-- provide multiple information sources over a single
-- physical interface and it might include filtering
-- characters that were destined for another kind of
-- channel. All of these aspects are hidden in the channel
-- abstraction.(Note some Page Description Languages have
-- compression built into them so "invisible" compression
-- refers to compression done by the transport medium and
-- removed before the data is presented to the interpreter.)
--
-- There are many kinds of channels;some of which are based
-- on networks and others which are not. For example, a
-- channel can be a serial (or parallel) connection; it can
-- be a service, such as the Unix Line Printer Daemon (LPD),
-- offering itself over a network connection (interface); or
-- it could be a disk drive into which a floppy disks with
-- the print data is inserted. Each channel is typically
-- identified by the electronic path and/or service protocol
-- used to deliver print data to the printer.
--
-- Channel example                   Implementation
--
-- serial port channel            bi-directional data channel
-- parallel port channel          often uni-directional channel
-- IEEE 1284 port channel         bi-directional channel
-- SCSI port channel              bi-directional
-- Apple PAP channel              may be based on Local-, Ether-or
--                                TokenTalk
-- LPD Server channel             typically TCP/IP based, port 515





-- Novell Remote Printer          typically SPX/IPX based channel
-- Novell Print Server            typically SPX/IPX based channel
-- port 9100 channel              HP and friends
-- Adobe AppSocket(9101) channel  a bi-directional extension of LPD
--
-- It is easy to note that this is a mixed bag.  There are
-- some physical connections over which no (or very meager)
-- protocols are run (e.g. the serial or old parallel ports)
-- and there are services which often have elaborate
-- protocols that run over a number of protocol stacks. In
-- the end what is important is the delivery of print data
-- thru the channel.
--
-- The channel sub-units are represented by the Channel
-- Group in the Model. It has a current Control Language
-- which can be used to specify which interpreter is to be
-- used for the print data and to query and change
-- environment variables used by the interpreters (and
-- Mangement Applications). There is also a default
-- interpreter that is to be used if an interpreter is not
-- explicitly specified using the Control Language. Channel
-- sub-units are based on an underlying interface.

--       The channel table and its underlying structure
--
-- The first seven items in the Channel Table define the
-- "channel" itself.  A channel typically depends on other
-- protocols and interfaces to provide the data that flows
-- thru the channel. It is necessary to provide control of
-- the (perhaps complex) process by which print data arrives
-- at an interpreter. Control is largely limited to enabling
-- or disabling the whole channel. It is likely, however,
-- that more control of the process of accessing print data
-- will be needed over time. Thus, the ChannelType will
-- allow type specific data to be associated with each
-- channel (using ChannelType specific groups in a fashion
-- analogous to the media specific MIBs that are associated
-- with the IANAIfType in the Interfaces Table). As a first
-- step in this direction, each channel will identify the
-- underlying Interface on which it is based. This is the
-- eighth object in each row of the table.

-- Some examples of the kind of control are where
-- compression or encoding is used; and whether the data is
-- filtered to remove file storage anomolies such as those
-- created by using MS-DOS/PC-DOS LPT1:.
--






-- The Channel Table
--
-- The prtChannelTable represents the set of input data sources which
-- can provide print data to one or more of the interpreters
-- available on a printer


prtChannel OBJECT IDENTIFIER ::= { printmib 14 }

prtChannelTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtChannelEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtChannel 1 }

prtChannelEntry OBJECT-TYPE
    SYNTAX     PrtChannelEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtChannelIndex }
    ::= { prtChannelTable 1 }

PrtChannelEntry ::= SEQUENCE {
    prtChannelIndex                     Integer32,
    prtChannelType                      INTEGER,
    prtChannelProtocolVersion           OCTET STRING,
    prtChannelCurrentJobCntlLangIndex   Integer32,
    prtChannelDefaultPageDescLangIndex  Integer32,
    prtChannelState                     INTEGER,
    prtChannelIfIndex                   Integer32,
    prtChannelStatus                    SubUnitStatus
}

prtChannelIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this data
        channel.  Although these values may change due to a major
        reconfiguration of the device (e.g. the addition of new data
        channels to the printer), values are expected to remain
        stable across successive printer power cycles."





    ::= { prtChannelEntry 1 }

prtChannelType OBJECT-TYPE
    -- This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   chSerialPort(3),
                   chParallelPort(4),
                   chIEEE1284Port(5),
                   chSCSIPort(6),
                   chAppleTalkPAP(7), -- AppleTalk Printer Achess Protocol
                   chLPDServer(8),
                   chNetwareRPrinter(9),  -- Netware
                   chNetwarePServer(10),  -- Netware
                   chPort9100(11),
                   chAppSocket(12),       -- a bi-directional, LPD-like
                                          -- protocol using 9101 for
                                          -- control and 9100 for data.
                                          -- Adobe Systems, Inc.
                   chFTP(13),             -- FTP "PUT" to printer
                   chTFTP(14),
                   chDLCLLCPort(15),
                   chIBM3270(16),
                   chIBM5250(17),
                   chFax(18),
                   chIEEE1394(19),
                   chTransport1(20),      -- port 35
                   chCPAP(21),            -- port 170
                   chDCERemoteProcCall(22), -- OSF
                   chONCRemoteProcCall(23), -- Sun Microsystems
                   chOLE(24),               -- Microsoft
                   chNamedPipe(25),
                   chPCPrint(26),           -- Banyan
                   chServerMessageBlock(27),
                        -- File/Print sharing protocol used by
                        -- various network operating systems
                        -- from IBM 3Com, Microsoft and others
                   chDPMF(28),  -- Distributed Print Mgt. Framework, IBM
                   chDLLAPI(29), -- Microsoft
                   chVxDAPI(30), -- Microsoft
                   chSystemObjectManager(31), -- IBM
                   chDECLAT(32),          -- Digital Equipment Corp.
                   chNPAP(33)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of this print data channel.  This





        object provides the linkage to ChannelType-specific
        groups that may (conceptually) extend the prtChannelTable
        with additional details about that channel."
    ::= { prtChannelEntry 2 }

prtChannelProtocolVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..63))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The version of the protocol used on this
        channel.  The format used for version numbering depends
        on prtChannelType."
    ::= { prtChannelEntry 3 }

prtChannelCurrentJobCntlLangIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtInterpreterIndex  corresponding to the
        Control Language Interpreter for this channel. This
        interpreter defines the syntax used for control
        functions, such as querying or changing environment
        variables and identifying job boundaries (e.g. PJL,
        PostScript, NPAP). Must be 1 or greater."
    ::= { prtChannelEntry 4 }

prtChannelDefaultPageDescLangIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of prtInterpreterIndex  corresponding to the
        Page Description Language Interpreter for this channel.
        This interpreter defines the default Page Description
        Language interpreter to be used for the print data unless
        the Control Language is used to select a specific
        interpreter (e.g.,  PCL, PostScript Language,
        auto-sense). Must be 1 or greater."
    ::= { prtChannelEntry 5 }

prtChannelState OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   printDataAccepted(3),
                   noDataAccepted(4)





               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The state of this print data channel.  The value determines
        whether control information and print data is allowed through
        this channel or not."
    ::= { prtChannelEntry 6 }

prtChannelIfIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of ifIndex (in the ifTable; see the interface
        section of MIB-2/RFC 1213) which corresponds to this channel.
        When more than one row of the ifTable is relevant, this is
        the index of the row representing the topmost layer in the
        interface hierarchy.  A value of zero indicates that no
        interface is associated with this channel."
    ::= { prtChannelEntry 7 }

prtChannelStatus OBJECT-TYPE
    SYNTAX     SubUnitStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current status of the channel."
    ::= { prtChannelEntry 8 }

-- The Interpreter Group
--
-- The interpreter sub-units are responsible for the conversion of a
-- description of intended print instances into images that are to be
-- marked on the media. A printer may have one or more interpreters. The
-- interpreter sub-units are represented by the Interpreter Group in the
-- Model. Each interpreter is generally implemented with software running
-- on the System Controller sub-unit. The Interpreter Table has one entry
-- per interpreter where the interpreters include both Page Description
-- Language (PDL) Interpreters and Control Language Interpreters.
--
-- Implementation of every object in this group is mandatory.


prtInterpreter OBJECT IDENTIFIER ::= { printmib 15 }

--       Interpreter Table
--





-- The prtInterpreterTable is a table representing the interpreters in
-- the printer.  An entry shall be placed in the interpreter table for
-- each interpreter on the printer.

prtInterpreterTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtInterpreterEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtInterpreter 1 }

prtInterpreterEntry OBJECT-TYPE
    SYNTAX     PrtInterpreterEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtInterpreterIndex }
    ::= { prtInterpreterTable 1 }

PrtInterpreterEntry ::= SEQUENCE {
    prtInterpreterIndex                 Integer32,
    prtInterpreterLangFamily            INTEGER,
    prtInterpreterLangLevel             OCTET STRING,
    prtInterpreterLangVersion           OCTET STRING,
    prtInterpreterDescription           OCTET STRING,
    prtInterpreterVersion               OCTET STRING,
    prtInterpreterDefaultOrientation    INTEGER,
    prtInterpreterFeedAddressability    Integer32,
    prtInterpreterXFeedAddressability   Integer32,
    prtInterpreterDefaultCharSetIn      CodedCharSet,
    prtInterpreterDefaultCharSetOut     CodedCharSet,
    prtInterpreterTwoWay                INTEGER
}

prtInterpreterIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value for each PDL or control language for which
        there exists an interpreter or emulator in the printer.  The
        value is used to identify this interpreter. Although these
        values may change due to a major reconfiguration of the device
        (e.g. the addition of new interpreters to the printer), values
        are expected to remain stable across successive printer power





        cycles."
    ::= { prtInterpreterEntry 1 }

prtInterpreterLangFamily OBJECT-TYPE
    -- This value is a type 2 enumeration
    SYNTAX     INTEGER {
          other(1),
          langPCL(3),        -- PCL.  Starting with PCL version 5,
                             -- HP-GL/2 is included as part of the
                             -- PCL language.
                             -- PCL and HP-GL/2 are registered
                             -- trademarks of Hewlett-Packard Company.
          langHPGL(4),       -- Hewlett-Packard Graphics Language.
                             -- HP-GL is a registered trademark of
                             -- Hewlett-Packard Company.
          langPJL(5),        -- Peripheral Job Language. Appears in the
                             -- data stream between data intended for a
                             -- page description language.
                             -- Hewlett-Packard Co.
          langPS(6),         -- PostScript Language (tm)
                             -- Postscript - a trademark of Adobe
                             -- Systems Incorporated which may be
                             -- registered in certain jurisdictions
          langPSPrinter(42), -- The PostScript Language used for
                             -- control (with any PDLs)
                             -- Adobe Systems Incorporated
          langIPDS(7),       -- Intelligent Printer Data Stream
                             -- Bi-directional print data stream for
                             -- documents consisting of data objects
                             -- (text, image, graphics, bar codes),
                             -- resources (fonts, overlays) and page,
                             -- form and finishing instructions.
                             -- Facilitates system level device
                             -- control, document tracking and error
                             -- recovery throughout the print process.
                             -- Pennant Systems, IBM
          langPPDS(8),       -- IBM Personal Printer Data Stream.
                             -- Originally called IBM ASCII, the name
                             -- was changed to PPDS when the Laser
                             -- Printer was introduced in 1989.
                             -- Lexmark International, Inc.
          langEscapeP(9),
          langEpson(10),
          langDDIF(11),      -- Digital Document Interchange Format
                             -- Digital Equipment Corp., Maynard MA
          langInterpress(12),
          langISO6429(13),   -- ISO 6429.  Control functions for Coded
                             -- Character Sets (has ASCII control





                             -- characters, plus additional controls for
                             -- character imaging devices.)
                             -- ISO Standard, Geneva, Switzerland
          langLineData(14),  -- line-data:  Lines of data as separate
                             -- ASCII or EBCDIC records and containing
                             -- no control functions (no CR, LF, HT, FF,
                             -- etc.). For use with traditional line
                             -- printers.  May use CR and/or LF to
                             -- delimit lines, instead of records.  See
                             -- ISO 10175 Document Printing Application
                             -- (DPA)
                             -- ISO standard, Geneva, Switzerland
          langMODCA(15),     -- Mixed Object Document Content Architecture
                             -- Definitions that allow the composition,
                             -- interchange, and presentation of final
                             -- form documents as a collection of data
                             -- objects (text, image, graphics, bar
                             -- codes), resources (fonts, overlays) and
                             -- page, form and finishing instructions.
                             -- Pennant Systems, IBM
          langREGIS(16),     -- Remote Graphics Instruction Set,
                             -- Digital Equipment Corp., Maynard MA
          langSCS(17),       -- SNA Character String
                             -- Bi-directional print data stream for SNA
                             -- LU-1 mode of communications
                             -- IBM
          langSPDL(18),      -- ISO 10180 Standard Page Description
                             -- Language
                             -- ISO Standard
          langTEK4014(19),
          langPDS(20),
          langIGP(21),
          langCodeV(22),     -- Magnum Code-V, Image and printer control
                             -- language used to control impact/dot-
                             -- matrix printers.
                             -- QMS, Inc., Mobile AL
          langDSCDSE(23),    -- DSC-DSE:  Data Stream Compatible and
                             -- Emulation Bi-directional print data
                             -- stream for non-SNA (DSC) and SNA LU-3
                             -- 3270 controller (DSE) communications
                             -- IBM
          langWPS(24),       -- Windows Printing System, Resource based
                             -- command/data stream used by Microsoft At
                             -- Work Peripherals.
                             -- Developed by the Microsoft Corporation.
          langLN03(25),      -- Early DEC-PPL3, Digital Equipment Corp.
          langCCITT(26),
          langQUIC(27),      -- QUIC (Quality Information Code), Page





                             -- Description Language for laser printers.
                             -- Included graphics, printer control
                             -- capability and emulation of other well-
                             -- known printer .
                             -- QMS, Inc.
          langCPAP(28),      -- Common Printer Access Protocol
                             -- Digital Equipment Corp.
          langDecPPL(29),    -- Digital ANSI-Compliant Printing Protocol
                             -- (DEC-PPL)
                             -- Digital Equipment Corp.
          langSimpleText(30),-- simple-text:  character coded data,
                             -- including NUL, CR , LF, HT, and FF
                             -- control characters.  See ISO 10175
                             -- Document Printing Application (DPA)
                             -- ISO standard, Geneva, Switzerland
          langNPAP(31),      -- Network Printer Alliance Protocol
                             -- IEEE 1284.1
          langDOC(32),       -- Document Option Commands, Appears in the
                             -- data stream between data intended for a
                             -- page description .
                             -- QMS, Inc.
          langimPress(33),   -- imPRESS, Page description language
                             -- originally developed for the ImageServer
                             -- line of systems. A binary language
                             -- providing representations for text,
                             -- simple graphics (rules, lines, conic
                             -- sections), and some large forms (simple
                             -- bit-map and CCITT group 3/4 encoded).The
                             -- language was intended to be sent over an
                             -- 8-bit channel and supported early
                             -- document preparation languages (e.g. TeX
                             -- and TROFF).
                             -- QMS, Inc.
          langPinwriter(34), -- 24 wire dot matrix printer  for
                             -- USA, Europe, and Asia except Japan.
                             -- More widely used in Germany, and some
                             -- Asian countries than in US.
                             -- NEC
          langNPDL(35),      -- Page printer  for Japanese
                             -- market.
                             -- NEC
          langNEC201PL(36),  -- Serial printer language used in the
                             -- Japanese market.
                             -- NEC
          langAutomatic(37), -- Automatic PDL sensing.  Automatic
                             -- sensing of the interpreter language
                             -- family by the printer examining the
                             -- document content.  Which actual





                             -- interpreter language families are sensed
                             -- depends on the printer implementation.
          langPages(38),     -- Page printer Advanced Graphic Escape Set
                             -- IBM Japan
          langLIPS(39),      -- LBP Image Processing System
          langTIFF(40),      -- Tagged Image File Format (Aldus)
          langDiagnostic(41),-- A hex dump of the input to the
                             -- interpreter
          langCaPSL(43),     -- Canon Print Systems Language
          langEXCL(44),      -- Extended Command Language
                             -- Talaris Systems Inc.
          langLCDS(45),      -- Line Conditioned Data Stream
                             -- Xerox Corporation
          langXES(46)        -- Xerox Escape Sequences
                             -- Xerox Corporation
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The family name of a Page Description Language (PDL) or
        control language which this interpreter in the printer can
        interpret or emulate.  This type 2 list of enumerations
        requires review before additional entries are made."
    ::= { prtInterpreterEntry 2 }

prtInterpreterLangLevel OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..31))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The level of the language which this interpreter is
        interpreting or emulating.  This might contain a value like
        '5e' for an interpreter which is emulating level 5e of the PCL
        language.  It might contain '2' for an interpreter which is
        emulating level 2 of the PostScript language.  Similarly it
        might contain '2' for an interpreter which is emulating level
        2 of the HPGL language."
    ::= { prtInterpreterEntry 3 }

prtInterpreterLangVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..31))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The date code or version of the language which this interpreter
        is interpreting or emulating."
    ::= { prtInterpreterEntry 4 }






prtInterpreterDescription OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A string to identify this interpreter in the localization
        specified by prtGeneralCurrentLocalization as opposed to the
        language which is being interpreted.  It is anticipated that
        this string will allow manufacturers to unambiguously identify
        their interpreters."
    ::= { prtInterpreterEntry 5 }

prtInterpreterVersion OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..31))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The date code, version number, or other product specific
        information tied to this interpreter.  This value is
        associated with the interpreter, rather than with the version
        of the language which is being interpreted or emulated."
    ::= { prtInterpreterEntry 6 }

prtInterpreterDefaultOrientation OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   portrait(3),
                   landscape(4)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The current orientation default for this interpreter.  This
        value may be overridden for a particular job (e.g., by a
        command in the input data stream)."
    ::= { prtInterpreterEntry 7 }

prtInterpreterFeedAddressability OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum interpreter addressability in the feed
        direction in 10000 prtMarkerAddressabilityUnit s (see
        prtMarkerAddressabilityFeedDir ) for this interpreter.
        The value (-1) means other and specifically indicates
        that the sub-unit places no restrictions on this parameter."





    ::= { prtInterpreterEntry 8 }

prtInterpreterXFeedAddressability OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The maximum interpreter addressability in the cross feed
        direction in 10000 prtMarkerAddressabilityUnit s (see
        prtMarkerAddressabilityXFeedDir) for this interpreter.
        The value (-1) means other and specifically indicates
        that the sub-unit places no restrictions on this
        parameter."
    ::= { prtInterpreterEntry 9 }

prtInterpreterDefaultCharSetIn OBJECT-TYPE
    SYNTAX     CodedCharSet
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The default coded character set for input octets
        encountered outside a context in which the Page
        Description Language established the interpretation
        of the octets.

        This value shall be (2) if there is no default."
    ::= { prtInterpreterEntry 10 }

prtInterpreterDefaultCharSetOut OBJECT-TYPE
    SYNTAX     CodedCharSet
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The default character set for data coming from this interpreter
        through the printer's output channel.


        This value shall be (2) if there is no default."
    ::= { prtInterpreterEntry 11 }

prtInterpreterTwoWay OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   yes(3),
                   no(4)
               }
    MAX-ACCESS read-only
    STATUS     current





    DESCRIPTION
        "Indicates whether or not this interpreter returns information
        back to the host."
    ::= { prtInterpreterEntry 12 }

-- The Console Group
--
-- Many printers have a console on the printer, the operator console,
-- that is used to display and modify the state of the printer. The
-- console can be as simple as a few indicators and switches or as
-- complicated as full screen displays and keyboards. There can be
-- at most one such console.
--
-- Implementation of every object in this group is mandatory.

prtConsoleLocalization OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The value of the prtLocalizationIndex corresponding to
        the language, country, and character set to be used for the
        console.  This localization applies both to the actual display
        on the console as well as the encoding of these console
        objects in management operations."
    ::= { prtGeneralEntry 10 }

prtConsoleNumberOfDisplayLines OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of lines on the printer's physical
        display.  This value is 0 if there are no lines on the
        physical display or if there is no physical display"
    ::= { prtGeneralEntry 11 }

prtConsoleNumberOfDisplayChars OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of characters per line displayed on the physical
        display.  This value is 0 if there are no lines on the
        physical display or if there is no physical display"
    ::= { prtGeneralEntry 12 }

prtConsoleDisable OBJECT-TYPE





    SYNTAX     INTEGER {
                   enabled(3),
                   disabled(4)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This object enables or disables manual input from the
        operators console."
    ::= { prtGeneralEntry 13 }

-- The Display Buffer Table

prtConsoleDisplayBuffer OBJECT IDENTIFIER ::= { printmib 16 }

prtConsoleDisplayBufferTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtConsoleDisplayBufferEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtConsoleDisplayBuffer 5 }

prtConsoleDisplayBufferEntry OBJECT-TYPE
    SYNTAX     PrtConsoleDisplayBufferEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table contains one entry for each physical line on
        the display.  Lines cannot be added or deleted.

        Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtConsoleDisplayBufferIndex }
    ::= { prtConsoleDisplayBufferTable 1 }

PrtConsoleDisplayBufferEntry ::= SEQUENCE {
    prtConsoleDisplayBufferIndex    Integer32,
    prtConsoleDisplayBufferText     OCTET STRING
}

prtConsoleDisplayBufferIndex OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value for each console line in the printer.  The
        value is used to identify this console line. Although





        these values may change due to a major reconfiguration of
        the device (e.g. the addition of new console lines to the
        printer), values are expected to remain stable across
        successive printer power cycles."
    ::= { prtConsoleDisplayBufferEntry 1 }

prtConsoleDisplayBufferText OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The content of a line in the logical display buffer of
        the operator's console of the printer.  When a write
        operation occurs, normally a critical message, to one of
        the LineText strings, the agent should make that line
        displayable if a physical display is present.  Writing
        a zero length string clears the line.  It is an
        implementation-specific matter as to whether the agent allows
        a line to be overwritten before it has been cleared.
        Printer generated strings shall be in the localization
        specified by ConsoleLocalization.  Management Application
        generated strings should be localized by the Management
        Application."
    ::= { prtConsoleDisplayBufferEntry 2 }

-- The Console Light Table

prtConsoleLights OBJECT IDENTIFIER ::= { printmib 17 }

prtConsoleLightTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtConsoleLightEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtConsoleLights 6 }

prtConsoleLightEntry OBJECT-TYPE
    SYNTAX     PrtConsoleLightEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtConsoleLightIndex }
    ::= { prtConsoleLightTable 1 }

PrtConsoleLightEntry ::= SEQUENCE {





    prtConsoleLightIndex            Integer32,
    prtConsoleOnTime                Integer32,
    prtConsoleOffTime               Integer32,
    prtConsoleColor                 INTEGER,
    prtConsoleDescription           OCTET STRING
}

prtConsoleLightIndex OBJECT-TYPE
    SYNTAX     Integer32 (0..65535)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A unique value used by the printer to identify this light.
        Although these values may change due to a major
        reconfiguration of the device (e.g. the addition of new lights
        to the printer), values are expected to remain stable across
        successive printer power cycles."
    ::= { prtConsoleLightEntry 1 }

prtConsoleOnTime OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The on time in milliseconds of blinking of this light; 0
        indicates off always.  If both prtConsoleOnTime
        and prtConsoleOffTime are 0, then the light is
        always off."
    ::= { prtConsoleLightEntry 2 }

prtConsoleOffTime OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The off time in milliseconds of blinking of this light; 0
        indicates on always.  If both prtConsoleOnTime
        and prtConsoleOffTime are 0, then the light is
        always off."
    ::= { prtConsoleLightEntry 3 }

prtConsoleColor OBJECT-TYPE
    -- This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   unknown(2),
                   white(3),
                   red(4),





                   green(5),
                   blue(6),
                   cyan(7),
                   magenta(8),
                   yellow(9)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The color of this light."
    ::= { prtConsoleLightEntry 4 }

prtConsoleDescription OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The vendor description or label of this light in the
        localization specified by prtConsoleLocalization."
    ::= { prtConsoleLightEntry 5 }


-- The Alerts Group
--
-- The prtAlertTable lists all the critical and non-critical alerts
-- currently active in the printer.  A critical alert is one that stops
-- the printer from printing immediately and printing can not continue
-- until the critical alert condition is eliminated.  Non-critical
-- alerts are those items that do not stop printing but may at some
-- future time.
-- The table contains information on the severity, component, detail
-- location within the component, alert code and description of each
-- critical alert that is currently active within the printer.  See
-- 2.2.13 for a more complete description of the alerts table and
-- its management.
--
-- Implementation of every object in this group is mandatory.

prtAlert OBJECT IDENTIFIER ::= { printmib 18 }

prtAlertTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF PrtAlertEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        ""
    ::= { prtAlert 1 }






prtAlertEntry OBJECT-TYPE
    SYNTAX     PrtAlertEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entries may exist in the table for each device
        index who's device type is `printer'."
    INDEX  { hrDeviceIndex, prtAlertIndex }
    ::= { prtAlertTable 1 }

PrtAlertEntry ::= SEQUENCE {
    prtAlertIndex               Integer32,
    prtAlertSeverityLevel       INTEGER,
    prtAlertTrainingLevel       INTEGER,
    prtAlertGroup               INTEGER,
    prtAlertGroupIndex          Integer32,
    prtAlertLocation            Integer32,
    prtAlertCode                INTEGER,
    prtAlertDescription         OCTET STRING,
    prtAlertTime                TimeTicks
}

prtAlertIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The index value used to determine which alerts
        have been added or removed from the alert table.
        This is an incrementing integer starting from zero
        every time the printer is reset.  When the printer
        adds an alert to the table, that alert is assigned
        the next higher integer value from the last item
        entered into the table.  If the index value reaches
        its maximum value, the next item entered will cause
        the index value to roll over and start at zero
        again.  The first event placed in the alert table
        after a reset of the printer shall
        have an index value of 1.  NOTE: The management
        application will read the alert table when a trap
        or event notification occurs or at a periodic rate
        and then parse the table to determine if any new
        entries were added by comparing the last known index
        value with the current highest index value. The
        management application will then update its copy of
        the alert table.  When the printer discovers that
        an alert is no longer active, the printer shall
        remove the row for that alert from the table and





        shall reduce the number of rows in the table.  The
        printer may add or delete any number of rows from
        the table at any time.  The management station
        can detect when binary alerts have been deleted by
        requesting an attribute of each alert, and noting
        alerts as deleted when that retrieval is not possible."
    ::= { prtAlertEntry 1 }

prtAlertSeverityLevel OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   critical(3),
                   warning(4)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The level of severity of this alert table entry.  The printer
        determines the severity level assigned to each entry into the
        table."
    ::= { prtAlertEntry 2 }

prtAlertTrainingLevel OBJECT-TYPE
    -- This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   unknown(2),
                   untrained(3),
                   trained(4),
                   fieldService(5),
                   management(6)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The level of training required to handle this alert. The
        training level is an enumeration that is determined and
        assigned by the printer manufacturer based on the information
        or the training required to handle this alert.  The printer
        will break alerts into these different training levels.  It is
        the responsibility of the management application in the system
        to determine how a particular alert is handled and how and to
        whom that alert is routed.  The following are the four
        training levels of alerts:

               Field Service - Alerts that typically require advanced
                      training and technical knowledge of the printer





                      and its sub-units. An example of a technical
                      person would be a manufacture's Field Service
                      representative, or other person formally
                      trained by the manufacturer or similar
                      representative.
               Trained - Alerts that require an intermediate or moderate
                      level of knowledge of the printer and its
                      sub-units. A typical examples of alerts that
                      a trained operator can handle is replacing
                      toner cartridges.
               Untrained - Alerts that can be fixed without prior
                      training either because the action to correct
                      the alert is obvious or the printer can help the
                      untrained person fix the problem. A typical
                      example of such an alert is reloading paper
                      trays and emptying output bins on a low end
                      printer.
               Management - Alerts that have to do with overall
                      operation of and configuration of the printer.
                      Examples of management events are configuration
                      change of sub-units."
    ::= { prtAlertEntry 3 }

prtAlertGroup OBJECT-TYPE
    -- This value is a type 1 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   hostResourcesMIBStorageTable(3),
                   hostResourcesMIBDeviceTable(4),
                   generalPrinter(5),
                   cover(6),
                   localization(7),
                   input(8),
                   output(9),
                   marker(10),
                   markerSupplies(11),
                   markerColorant(12),
                   mediaPath(13),
                   channel(14),
                   interpreter(15),
                   consoleDisplayBuffer(16),
                   consoleLights(17)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The type of sub-unit within the printer model that this alert
        is related.  Input, output, and markers are examples of





        printer model groups, i.e., examples of types of sub-units.

        Whereever possible, these enumerations match the
        sub-identifier that identifies the relevant table in the
        printmib."
    ::= { prtAlertEntry 4 }

prtAlertGroupIndex OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "An index of the row within the principle table in the
        group identified by prtAlertGroup that represents the
        sub-unit of the printer that caused this alert.  The
        combination of the Group and the GroupIndex defines
        exactly which printer sub-unit caused the alert.; for
        example, Input #3, Output #2, and Marker #1.

        Every object in this MIB is indexed with hrDeviceIndex and
        optionally, another index variable.  If this other index
        variable is present in the table that generated the alert, it
        will be used as the value for this object.  Otherwise, this
        value shall be -1."
    ::= { prtAlertEntry 5 }

prtAlertLocation OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The sub-unit location that is defined by the printer
        manufacturer to further refine the location of this alert
        within the designated sub-unit.  The location is used in
        conjunction with the Group and GroupIndex values; for
        example, there is an alert in Input #2 at location number 7."
    ::= { prtAlertEntry 6 }

prtAlertCode OBJECT-TYPE
    -- This value is a type 2 enumeration
    SYNTAX     INTEGER {
                   other(1),
                   unknown(2),
                        -- codes common to serveral groups
                   coverOpen(3),
                   coverClosed(4),
                   interlockOpen(5),
                   interlockClosed(6),





                   configurationChange(7),
                   jam(8),
                        -- general Printer group
                   doorOpen(501),
                   doorClosed(502),
                   powerUp(503),
                   powerDown(504),
                        -- Input Group
                   inputMediaTrayMissing(801),
                   inputMediaSizeChange(802),
                   inputMediaWeightChange(803),
                   inputMediaTypeChange(804),
                   inputMediaColorChange(805),
                   inputMediaFormPartsChange(806),
                   inputMediaSupplyLow(807),
                   inputMediaSupplyEmpty(808),
                        -- Output Group
                   outputMediaTrayMissing(901),
                   outputMediaTrayAlmostFull(902),
                   outputMediaTrayFull(903),
                        -- Marker group
                   markerFuserUnderTemperature(1001),
                   markerFuserOverTemperature(1002),
                        -- Marker Supplies group
                   markerTonerEmpty(1101),
                   markerInkEmpty(1102),
                   markerPrintRibbonEmpty(1103),
                   markerTonerAlmostEmpty(1104),
                   markerInkAlmostEmpty(1105),
                   markerPrintRibbonAlmostEmpty(1106),
                   markerWasteTonerReceptacleAlmostFull(1107),
                   markerWasteInkReceptacleAlmostFull(1108),
                   markerWasteTonerReceptacleFull(1109),
                   markerWasteInkReceptacleFull(1110),
                   markerOpcLifeAlmostOver(1111),
                   markerOpcLifeOver(1112),
                   markerDeveloperAlmostEmpty(1113),
                   markerDeveloperEmpty(1114),
                        -- Media Path Device Group
                   mediaPathMediaTrayMissing(1301),
                   mediaPathMediaTrayAlmostFull(1302),
                   mediaPathMediaTrayFull(1303),
                        -- interpreter Group
                   interpreterMemoryIncrease(1501),
                   interpreterMemoryDecrease(1502),
                   interpreterCartridgeAdded(1503),
                   interpreterCartridgeDeleted(1504),
                   interpreterResourceAdded(1505),





                   interpreterResourceDeleted(1506),
                   interpreterResourceUnavailable(1507)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The code that describes the type of alert for this entry in
        the table.  There are different codes for each
        sub-unit type: for example, Media Supply Low and Media
        Supply Empty are Aler codes for the Input sub-unit."
    ::= { prtAlertEntry 7}

prtAlertDescription OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..255))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A description of this alert entry in the localization
        specified by prtGeneralCurrentLocalization.  The description is
        provided by the printer to further elaborate on the enumerated
        alert or provide information in the case where the code is
        classified ask `other' or `unknown'.  The printer is required
        to return a description string but the string may be a null
        string."
    ::= { prtAlertEntry 8 }

printerV1Alert OBJECT-IDENTITY
    STATUS  current
    DESCRIPTION
        "The value of the enterprise-specific oid in a SNMPv1 trap sent
        signalling a critical event in the prtAlertTable."
    ::= { prtAlert 2 }

printerV2AlertPrefix OBJECT IDENTIFIER ::= { printerV1Alert 0 }

printerV2Alert NOTIFICATION-TYPE
    OBJECTS { prtAlertIndex, prtAlertSeverityLevel, prtAlertGroup,
              prtAlertGroupIndex, prtAlertLocation, prtAlertCode }
    STATUS  current
    DESCRIPTION
        "This trap is sent whenever a critical event is added to the
        prtAlertTable."
    ::= { printerV2AlertPrefix 1 }

-- Note that the SNMPv2 to SNMPv1 translation rules dictate that the
-- preceding structure will result in SNMPv1 traps of the following
-- form:
--





-- printerAlert TRAP-TYPE
--     ENTERPRISE printerV1Alert
--     VARIABLES { prtAlertIndex, prtAlertSeverityLevel, prtAlertGroup,
--                 prtAlertGroupIndex, prtAlertLocation, prtAlertCode }
--     DESCRIPTION
--        "This trap is sent whenever a critical event is added to the
--        prtAlertTable."
--     ::= 1



-- The Alert Time Group
--
-- This group is optional.  However, to claim conformance to this
-- group, it is necessary to implement every object in the group.

prtAlertTime OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The value of sysUpTime at the time that this alert was
        generated."
    ::= { prtAlertEntry 9 }


-- Conformance Information

prtMIBConformance OBJECT IDENTIFIER ::= { printmib 2 }

-- compliance statements
prtMIBCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
        "The compliance statement for agents that implement the
        printer MIB."
    MODULE -- this module
    MANDATORY-GROUPS { prtGeneralGroup, prtInputGroup, prtOutputGroup,
                       prtMarkerGroup, prtMediaPathGroup,
                       prtChannelGroup, prtInterpreterGroup,
                       prtConsoleGroup, prtAlertTableGroup }

        OBJECT      prtGeneralReset
        SYNTAX      INTEGER {
                        notResetting(3),
                        resetToNVRAM(5)
                    }
        DESCRIPTION





            "It is conformant to implement just these two states in
            this object.  Any additional states are optional."

        OBJECT      prtConsoleOnTime
        MIN-ACCESS  read-only
        DESCRIPTION
            "It is conformant to implement this object as read-only."

        OBJECT      prtConsoleOffTime
        MIN-ACCESS  read-only
        DESCRIPTION
            "It is conformant to implement this object as read-only."

    -- the prtResponsiblePartyGroup, prtExtendedInputGroup,
    -- prtInputMediaGroup, prtExtendedOutputGroup,
    -- prtOutputDimensionsGroup, prtOutputFeaturesGroup,
    -- prtMarkerSuppliesGroup, prtMarkerColorantGroup,
    -- and the prtAlertTimeGroup are completely optional.
    ::= { prtMIBConformance 1 }

prtMIBGroups      OBJECT IDENTIFIER ::= { prtMIBConformance 2 }

prtGeneralGroup OBJECT-GROUP
    OBJECTS { prtGeneralConfigChanges, prtGeneralCurrentLocalization,
              prtGeneralReset, prtCoverDescription, prtCoverStatus,
              prtLocalizationLanguage, prtLocalizationCountry,
              prtLocalizationCharacterSet, prtStorageRefIndex,
              prtDeviceRefIndex }
    STATUS  current
    DESCRIPTION
        "The general printer group."
    ::= { prtMIBGroups 1 }

prtResponsiblePartyGroup OBJECT-GROUP
    OBJECTS { prtGeneralCurrentOperator, prtGeneralServicePerson }
    STATUS  current
    DESCRIPTION
        "The responsible party group contains contact information for
        humans responsible for the printer."
    ::= { prtMIBGroups 2 }

prtInputGroup OBJECT-GROUP
    OBJECTS { prtInputDefaultIndex, prtInputType, prtInputDimUnit,
              prtInputMediaDimFeedDirDeclared,
              prtInputMediaDimXFeedDirDeclared,
              prtInputMediaDimFeedDirChosen,
              prtInputMediaDimXFeedDirChosen, prtInputCapacityUnit,
              prtInputMaxCapacity, prtInputCurrentLevel,





              prtInputStatus, prtInputMediaName }
    STATUS  current
    DESCRIPTION
        "The input group."
    ::= { prtMIBGroups 3 }

prtExtendedInputGroup OBJECT-GROUP
    OBJECTS { prtInputName, prtInputVendorName, prtInputModel,
              prtInputVersion, prtInputSerialNumber,
              prtInputDescription, prtInputSecurity }
    STATUS  current
    DESCRIPTION
        "The extended input group."
    ::= { prtMIBGroups 4 }

prtInputMediaGroup OBJECT-GROUP
    OBJECTS { prtInputMediaWeight, prtInputMediaType,
              prtInputMediaColor, prtInputMediaFormParts }
    STATUS  current
    DESCRIPTION
        "The input media group."
    ::= { prtMIBGroups 5 }

prtOutputGroup OBJECT-GROUP
    OBJECTS { prtOutputDefaultIndex, prtOutputType,
              prtOutputCapacityUnit, prtOutputMaxCapacity,
              prtOutputRemainingCapacity,  prtOutputStatus }
    STATUS  current
    DESCRIPTION
        "The output group."
    ::= { prtMIBGroups 6 }

prtExtendedOutputGroup OBJECT-GROUP
    OBJECTS { prtOutputName, prtOutputVendorName, prtOutputModel,
              prtOutputVersion, prtOutputSerialNumber,
              prtOutputDescription, prtOutputSecurity }
    STATUS  current
    DESCRIPTION
        "The extended output group."
    ::= { prtMIBGroups 7 }

prtOutputDimensionsGroup OBJECT-GROUP
    OBJECTS { prtOutputDimUnit, prtOutputMaxDimFeedDir,
              prtOutputMaxDimXFeedDir, prtOutputMinDimFeedDir,
              prtOutputMinDimXFeedDir }
    STATUS  current
    DESCRIPTION
        "The output dimensions group"





    ::= { prtMIBGroups 8 }

prtOutputFeaturesGroup OBJECT-GROUP
    OBJECTS { prtOutputStackingOrder,
              prtOutputPageDeliveryOrientation, prtOutputBursting,
              prtOutputDecollating, prtOutputPageCollated,
              prtOutputOffsetStacking }
    STATUS  current
    DESCRIPTION
        "The output features group."
    ::= { prtMIBGroups 9 }

prtMarkerGroup OBJECT-GROUP
    OBJECTS { prtMarkerDefaultIndex, prtMarkerMarkTech,
              prtMarkerCounterUnit, prtMarkerLifeCount,
              prtMarkerPowerOnCount, prtMarkerProcessColorants,
              prtMarkerSpotColorants, prtMarkerAddressabilityUnit,
              prtMarkerAddressabilityFeedDir,
              prtMarkerAddressabilityXFeedDir, prtMarkerNorthMargin,
              prtMarkerSouthMargin, prtMarkerWestMargin,
              prtMarkerEastMargin, prtMarkerStatus }
    STATUS  current
    DESCRIPTION
        "The marker group."
    ::= { prtMIBGroups 10 }

prtMarkerSuppliesGroup OBJECT-GROUP
    OBJECTS { prtMarkerSuppliesMarkerIndex,
              prtMarkerSuppliesColorantIndex, prtMarkerSuppliesClass,
              prtMarkerSuppliesType, prtMarkerSuppliesDescription,
              prtMarkerSuppliesSupplyUnit,
              prtMarkerSuppliesMaxCapacity, prtMarkerSuppliesLevel }
    STATUS  current
    DESCRIPTION
        "The marker supplies group."
    ::= { prtMIBGroups 11 }

prtMarkerColorantGroup OBJECT-GROUP
    OBJECTS { prtMarkerColorantMarkerIndex, prtMarkerColorantRole,
              prtMarkerColorantValue, prtMarkerColorantTonality }
    STATUS  current
    DESCRIPTION
        "The marker colorant group."
    ::= { prtMIBGroups 12 }

prtMediaPathGroup OBJECT-GROUP
    OBJECTS { prtMediaPathDefaultIndex, prtMediaPathMaxSpeedPrintUnit,
              prtMediaPathMediaSizeUnit, prtMediaPathMaxSpeed,





              prtMediaPathMaxMediaFeedDir,
              prtMediaPathMaxMediaXFeedDir,
              prtMediaPathMinMediaFeedDir,
              prtMediaPathMinMediaXFeedDir, prtMediaPathType,
              prtMediaPathDescription, prtMediaPathStatus}
    STATUS  current
    DESCRIPTION
        "The media path group."
    ::= { prtMIBGroups 13 }

prtChannelGroup OBJECT-GROUP
    OBJECTS { prtChannelType, prtChannelProtocolVersion,
              prtChannelCurrentJobCntlLangIndex,
              prtChannelDefaultPageDescLangIndex, prtChannelState,
              prtChannelIfIndex, prtChannelStatus }
    STATUS  current
    DESCRIPTION
        "The channel group."
    ::= { prtMIBGroups 14 }

prtInterpreterGroup OBJECT-GROUP
    OBJECTS { prtInterpreterLangFamily, prtInterpreterLangLevel,
              prtInterpreterLangVersion, prtInterpreterDescription,
              prtInterpreterVersion, prtInterpreterDefaultOrientation,
              prtInterpreterFeedAddressability,
              prtInterpreterXFeedAddressability,
              prtInterpreterDefaultCharSetIn,
              prtInterpreterDefaultCharSetOut, prtInterpreterTwoWay }
    STATUS  current
    DESCRIPTION
        "The interpreter group."
    ::= { prtMIBGroups 15 }

prtConsoleGroup OBJECT-GROUP
    OBJECTS { prtConsoleLocalization, prtConsoleNumberOfDisplayLines,
              prtConsoleNumberOfDisplayChars, prtConsoleDisable,
              prtConsoleDisplayBufferText, prtConsoleOnTime,
              prtConsoleOffTime, prtConsoleColor,
              prtConsoleDescription }
    STATUS  current
    DESCRIPTION
        "The console group."
    ::= { prtMIBGroups 16 }

prtAlertTableGroup OBJECT-GROUP
    OBJECTS { prtAlertSeverityLevel, prtAlertTrainingLevel,
              prtAlertGroup, prtAlertGroupIndex, prtAlertLocation,
              prtAlertCode, prtAlertDescription }





    STATUS  current
    DESCRIPTION
        "The alert table group."
    ::= { prtMIBGroups 17 }

prtAlertTimeGroup OBJECT-GROUP
    OBJECTS { prtAlertTime }
    STATUS  current
    DESCRIPTION
        "The alert time group."
    ::= { prtMIBGroups 18 }


END






































