ARC-MIB DEFINITIONS ::= BEGIN


IMPORTS
  MODULE-IDENTITY, OBJECT-TYPE, Unsigned32, mib-2
          FROM SNMPv2-SMI                           -- [RFC2578]
  TEXTUAL-CONVENTION, RowStatus, StorageType
          FROM SNMPv2-TC                            -- [RFC2579]
  MODULE-COMPLIANCE, OBJECT-GROUP
          FROM SNMPv2-CONF                          -- [RFC2580]
  ResourceId
          FROM ALARM-MIB;                           -- [RFC3877]

arcMibModule MODULE-IDENTITY
  LAST-UPDATED "200409090000Z"  -- September 09, 2004
  ORGANIZATION "IETF Distributed Management Working Group"
  CONTACT-INFO
       "WG EMail:  disman@ietf.org
              Subscribe: disman-request@ietf.org
              http://www.ietf.org/html.charters/disman-charter.html

        Chair:     Randy Presuhn
                   E-mail: randy_presuhn@mindspring.com

        Editor:    Hing-Kam Lam
                   Lucent Technologies, 4C-616
                   101 Crawfords Corner Road





                   Holmdel, NJ 07733
                   USA
                   Tel: +1 732 949 8338
                   E-mail: hklam@lucent.com"

  DESCRIPTION
    "The MIB module describes the objects for controlling a resource
     in reporting alarm conditions that it detects.

     Copyright (C) The Internet Society (2004).  This version
     of this MIB module is part of RFC 3878;  see the RFC
     itself for full legal notices."

  REVISION  "200409090000Z"  -- September 09, 2004
  DESCRIPTION
       "Initial version, published as RFC 3878."
  ::={ mib-2 117 }

------------------
-- TEXTUAL-CONVENTION
------------------

IANAItuProbableCauseOrZero ::= TEXTUAL-CONVENTION
  STATUS  current
  DESCRIPTION
    "This TC can take any value of IANAItuProbableCause or 0.
     IANAItuProbableCause is defined in the IANA-ITU-ALARM-TC
     module, which is maintained at the IANA web site and
     published in the Alarm MIB document (see RFC 3877)."
  REFERENCE
    "IANA-ITU-ALARM-TC MIB module as maintained at the IANA web site.
     The initial module was also published in RFC 3877."
--
  SYNTAX  INTEGER (0..2147483647)

------------------
-- MIB Objects
------------------

arcTimeIntervals   OBJECT IDENTIFIER ::= { arcMibModule 1 }
arcObjects         OBJECT IDENTIFIER ::= { arcMibModule 2 }

arcTITimeInterval OBJECT-TYPE
  SYNTAX  Unsigned32
  UNITS       "seconds"
  MAX-ACCESS  read-write
  STATUS  current
  DESCRIPTION





    "This variable indicates the time interval used for the nalmTI
     state, in units of second.  It is a pre-defined length of time
     in which the resource will stay in the nalmTI state before
     transition into the alm state.

     Instances of this object SHOULD persist across agent restarts."
  ::= { arcTimeIntervals 1 }

arcCDTimeInterval OBJECT-TYPE
  SYNTAX  Unsigned32
  UNITS       "seconds"
  MAX-ACCESS  read-write
  STATUS  current
  DESCRIPTION
    "This variable indicates the time interval used for the nalmQICD
     state, in units of second.  It is a pre-defined length of time
     in which the resource will stay in the nalmQICD state before
     transition into the alm state after it is problem-free.

     Instances of this object SHOULD persist across agent restarts."
  ::= { arcTimeIntervals 2 }

arcTable OBJECT-TYPE
  SYNTAX  SEQUENCE OF ArcEntry
  MAX-ACCESS  not-accessible
  STATUS  current
  DESCRIPTION
    "A table of Alarm Reporting Control (ARC) settings on the system.

     Alarm Reporting Control is a feature that provides an automatic
     in-service provisioning capability.  Alarm reporting is turned
     off on a per-resource basis for a selective set of potential
     alarm conditions to allow sufficient time for customer testing
     and other maintenance activities in an 'alarm free' state.
     Once a resource is ready for service, alarm reporting is
     automatically or manually turned on.

     Functional description and requirements of Alarm Reporting
     Control are defined in ITU-T Recommendation M.3100 Amendment 3
     [M.3100 Amd3]."

  REFERENCE
        "ITU Recommendation M.3100 Amendment 3, 'Generic Network
         Information Model', January 2001."
  ::= { arcObjects 1 }

arcEntry OBJECT-TYPE
  SYNTAX  ArcEntry





  MAX-ACCESS  not-accessible
  STATUS  current
  DESCRIPTION
    "A conceptual row that contains information about an ARC setting
     of a resource in the system.

     Implementation need to be aware that if the total size of
     arcIndex and arcNotificationId exceeds 114 sub-IDs, then OIDs
     of column instances in this table will have more than 128
     sub-IDs and cannot be access using SNMPv1, SNMPv2c, or snmpv3."

  INDEX  { arcIndex, arcAlarmType, arcNotificationId }
  ::= { arcTable 1 }

ArcEntry ::=
  SEQUENCE {
    arcIndex                      ResourceId,
    arcAlarmType                  IANAItuProbableCauseOrZero,
    arcNotificationId             OBJECT IDENTIFIER,
    arcState                      INTEGER,
    arcNalmTimeRemaining          Unsigned32,
    arcRowStatus                  RowStatus,
    arcStorageType                StorageType
    }

arcIndex OBJECT-TYPE
  SYNTAX  ResourceId
  MAX-ACCESS  not-accessible
  STATUS  current
  DESCRIPTION
    "This object uniquely identifies a resource, which is under the
     arcState's control for the associated arcAlarmType.

     For example, if the resource is an interface, this object will
     point to an instance of interface, e.g., ifIndex.1."
  ::= { arcEntry 1 }

arcAlarmType OBJECT-TYPE
  SYNTAX  IANAItuProbableCauseOrZero
  MAX-ACCESS  not-accessible
  STATUS  current
  DESCRIPTION
    "This object identifies the alarm condition type controlled by the
     arcState.  It specifies the value 0 or a value of
     IANAItuProbableCause that is applicable to the resource.
     IANAItuProbableCause is defined in the IANA-ITU-ALARM-TC
     module in the Alarm MIB document.






     The value of zero (0) implies any probable causes that are
     applicable to the resource.  Usually, the applicable probable
     causes of a resource are specified in the resource-specific mib."
  ::= { arcEntry 2 }

arcNotificationId OBJECT-TYPE
  SYNTAX  OBJECT IDENTIFIER
  MAX-ACCESS  not-accessible
  STATUS  current
  DESCRIPTION
    "This object identifies the type of notification to be suppressed.
     The notification type identified should be the one normally used
     by the resource for reporting its alarms.  When the value of 0.0 is
     specified for this object, it implies all applicable notification
     types."
  ::= { arcEntry 3 }

arcState OBJECT-TYPE
  SYNTAX  INTEGER {
            nalm (1),
            nalmQI (2),
            nalmTI (3),
            nalmQICD (4)
            }
  MAX-ACCESS  read-create
  STATUS  current
  DESCRIPTION
    "Defined in M.3100 Amendment 3 [M.3100 Amd3], there are five
     ARC states: alm, nalm, nalmQI, nalmQICD, and nalmTI.

        alm:        Alarm reporting is turned on (i.e., is allowed).
        nalm:       Alarm reporting is turned off (i.e., not allowed).
        nalmQI:     nalm - Qualified Inhibit. Alarm reporting is
                    turned off until the managed entity is qualified
                    problem-free for an optional persistence interval.
                    Problem-free means that the condition corresponding
                    to the specified alarm type is cleared.
        nalmQICD:   nalmQI - Count down.  This is a substate of nalmQI
                    and performs the persistence timing countdown
                    function after the managed entity is qualified
                    problem-free.
        nalmTI:     nalm - Timed Inhibit.  Alarm reporting is turned
                    off for a specified time interval.

     alm may transition to nalm, nalmQI or nalmTI by management request.

     nalm may transition to alm, nalmQI or nalmTI by management request.






     nalmQI may transition to nalm or alm by management request.

     nalmQI may transition to alm automatically
             if qualified problem-free (if nalmQICD is not supported) or
             if the CD timer expired (if nalmQICD is supported)

     nalmTI may transition to alm or nalm by management request.

     nalmTI may transition to alm automatically if the TI timer expired.

     Further details of ARC state transitions are defined in Figure 3
     of M.3100 Amd3 [M.3100 Amd3].

     According to the requirements in M.3100 Amd3, a resource
     supporting the ARC feature shall support the alm state and at
     least one of the nalm, nalmTI, and nalmQI states. The nalmQICD
     state is an optional substate of nalmQI.

     The arcState object controls the alarm reporting state of a
     resource. Note that the state alm (alarm reporting is allowed) is
     not listed in the enumeration of the value of this object. However,
     this state is implicitly supported by the mib.
     Once a resource enters the normal reporting mode (i.e., in the alm
     state) for the specified alarm type, the corresponding
     row will be automatically deleted from the arc table.
     Also the manual setting of arcState to alm can be achieved through
     setting the RowStatus object to 'destroy'.

     The nalamQICD state is a transitional state from nalmQI to alm. It
     is optional depending on the resource type and the implementation
     of the resource.  If it is supported, before the state
     transitions from nalmQI to alm, a count down period is activated
     for a duration set by the object arcNalmCDTimeInterval.  When the
     time is up, the arcState transitions to alm."

  ::= { arcEntry 4 }

arcNalmTimeRemaining OBJECT-TYPE
  SYNTAX  Unsigned32
  UNITS       "seconds"
  MAX-ACCESS  read-create
  STATUS  current
  DESCRIPTION
    "This variable indicates the time remaining in the nalmTI state
     or the nalmQICD state, in units of second.

     At the moment the resource enters the nalmTI state, this variable
     will have the initial value equal to the value of





     arcNalmTITimeInterval and then starts decrementing as time goes by.

     Similarly at the moment the resource enters the nalmQICD state,
     this variable will have the initial value equal to the value of
     arcNalmCDTimeInterval and then starts decrementing as time goes by.

     This variable is read-create and thus will allow the manager to
     write (extend or shorten), as needed, the remaining time when the
     resource is in the nalmTI or nalmQICD state.

     If this variable is supported and the resource is currently not in
     the nalmTI nor nalmQICD state, the value of this variable shall
     equal to zero."
  ::= { arcEntry 5 }

arcRowStatus OBJECT-TYPE
  SYNTAX  RowStatus
  MAX-ACCESS  read-create
  STATUS  current
  DESCRIPTION
    "This columnar object is used for creating and deleting a conceptual
     row of the arcTable.  It is used to create and delete an arc
     setting.

     Setting RowStatus to createAndGo or createAndWait implies creating
     a new ARC setting for the specified resource and alarm type.
     Setting RowStatus to destroy implies removing the ARC setting and
     thus has the effect of resuming normal reporting behaviour of the
     resource for the alarm type.

     Only the objects arcState, arcNalmTimeRemaining, and arcRowStatus
     can be updated when a row is active. All the objects, except
     arcNalmTimeRemaining, must be set before the row can be activated."
  ::= { arcEntry 6 }

arcStorageType OBJECT-TYPE
  SYNTAX       StorageType
  MAX-ACCESS   read-create
  STATUS       current
  DESCRIPTION
    "The storage type for this conceptual row.
     Conceptual rows having the value 'permanent' must
     allow write-access at a minimum to arcState.
     Note that arcState must allow change by management request.
     Therefore, no row can be created with 'readOnly'.
     If a set operation tries to set the value to 'readOnly',
     then an 'inconsistentValue' error must be returned."
  DEFVAL      { nonVolatile }





  ::= { arcEntry 7}

--------------------------
-- conformance information
--------------------------

arcConformance OBJECT IDENTIFIER ::= { arcMibModule 3 }

arcCompliances OBJECT IDENTIFIER ::= { arcConformance 1 }

arcCompliance MODULE-COMPLIANCE
  STATUS  current
    DESCRIPTION
      "The compliance statement for systems supporting
       the ARC MIB module."

  MODULE -- this module
           MANDATORY-GROUPS {
            arcSettingGroup
           }

  OBJECT arcStorageType
    WRITE-SYNTAX StorageType {
                         volatile(2),
                         nonVolatile(3),
                         permanent(4)
                         }
    DESCRIPTION
      "Support for value 'other' is not required.
       The arcState object must allow change by management
       request.  Therefore, no row can be created with
       'readOnly'."

  GROUP  arcTIGroup
  DESCRIPTION
    "This group is REQUIRED for ARC settings
     that provide the Time Inhibit (TI) function."

  GROUP  arcQICDGroup
  DESCRIPTION
    "This group is REQUIRED for ARC settings
     that provide the Quality Inhibit (QI) Count Down (CD)
     function."

  ::= { arcCompliances 1 }

arcGroups OBJECT IDENTIFIER ::= { arcConformance 2 }






arcSettingGroup OBJECT-GROUP
  OBJECTS {
          arcState,
          arcRowStatus,
          arcStorageType
          }
   STATUS   current
   DESCRIPTION
     "A collection of objects applicable to
      basic ARC setting."
   ::= { arcGroups 1}

arcTIGroup OBJECT-GROUP
  OBJECTS {
          arcTITimeInterval,
          arcNalmTimeRemaining
          }
   STATUS   current
   DESCRIPTION
     "A collection of objects applicable to
      ARC setting that support the Time Inhibit (TI)
      function."
   ::= { arcGroups 2}

arcQICDGroup OBJECT-GROUP
  OBJECTS {
          arcCDTimeInterval,
          arcNalmTimeRemaining
          }
  STATUS   current
  DESCRIPTION
    "A collection of objects applicable to
     ARC setting that support the Quality Inhibit (QI)
     Count Down (CD) function."
  ::= { arcGroups 3}

END















