APS-MIB DEFINITIONS ::= BEGIN


IMPORTS
        MODULE-IDENTITY, NOTIFICATION-TYPE, OBJECT-TYPE,
        Gauge32, Counter32, Integer32, transmission
                FROM SNMPv2-SMI

        TEXTUAL-CONVENTION, RowStatus,
        TimeStamp, StorageType
                FROM SNMPv2-TC

        SnmpAdminString
                FROM SNMP-FRAMEWORK-MIB







        ifIndex, InterfaceIndex
                FROM IF-MIB

        MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
                FROM SNMPv2-CONF;

apsMIB MODULE-IDENTITY
    LAST-UPDATED        "200302280000Z"  -- February 28, 2003
    ORGANIZATION        "IETF AToMMIB Working Group"
    CONTACT-INFO
        "       Jim Kuhfeld
                Postal: RedBack Networks. Inc.
                300 Holger Way
                San Jose, CA 95134-1362
                Tel: +1 408 750 5465
                Email: jkuhfeld@redback.com

                Jeff Johnson
                Postal: RedBack Networks. Inc.
                300 Holger Way
                San Jose, CA 95134-1362
                Tel: +1 408 750 5460
                Email: jeff@redback.com

                Michael Thatcher
                Postal: RedBack Networks. Inc.
                300 Holger Way
                San Jose, CA 95134-1362
                Tel: +1 408 750 5449
                Email: thatcher@redback.com"
    DESCRIPTION
        "This management information module supports the configuration
         and management of SONET linear APS groups. The definitions and
         descriptions used in this MIB have been derived from
         Synchronous Optical Network (SONET) Transport Systems:
         Common Generic Criteria, GR-253-CORE Issue 3, September 2000,
         section 5.3. The MIB is also consistent with the Multiplex
         Section Protection (MSP) protocol as specified in ITU-T
         Recommendation G.783, Characteristics of synchronous digital
         hierarchy (SDH) equipment function blocks, Annex A and B.

         Copyright (C) The Internet Society (2003).  This version of
         this MIB module is part of RFC 3498; see the RFC itself for
         full legal notices.
         "








    REVISION      "200302280000Z"  -- February 28, 2003
    DESCRIPTION
          "Initial version of this MIB, published as RFC 3498."
        ::= { transmission 49 }

apsMIBObjects OBJECT IDENTIFIER
        ::= { apsMIB 1 }

apsMIBNotifications OBJECT IDENTIFIER
        ::= { apsMIB 2 }

apsMIBConformance OBJECT IDENTIFIER
        ::= { apsMIB 3 }

ApsK1K2 ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "This Textual Convention describes an object that stores
         a SONET K1 and K2 byte APS protocol field.

         K1 is located in the first octet, K2 is located in
         the second octet. Bits are numbered from left to right.

         Bits 1-4 of the K1 byte indicate a request.

         1111  Lockout of Protection
         1110  Forced Switch
         1101  SF - High Priority
         1100  SF - Low Priority
         1011  SD - High Priority
         1010  SD - Low Priority
         1001  not used
         1000  Manual Switch
         0111  not used
         0110  Wait-to-Restore
         0101  not used
         0100  Exercise
         0011  not used
         0010  Reverse Request
         0001  Do Not Revert
         0000  No Request

         Bits 5-8 of the K1 byte indicate the channel associated with
         the request defined in bits 1-4.

         0000 is the Null channel.







         1-14 are working channels.
         15   is the extra traffic channel

         Bits 1-4 of the K2 byte indicate a channel. The channel is
         defined with the same syntax as K1 Bits 5-8.

         Bit 5 of the K2 byte indicates the
         architecture.

         0 if the architecture is 1+1
         1 if the architecture is 1:n

         Bits 6-8 of the K2 byte indicates the mode.

         000 - 011 are reserved for future use
         100  indicates the mode is unidirectional
         101  indicates the mode is bidirectional
         110  RDI-L
         111  AIS-L
        "
    REFERENCE
        "Bellcore (Telcordia Technologies) GR-253-CORE, Issue 3,
        September 2000, 5.3.5."
    SYNTAX      OCTET STRING (SIZE (2))

ApsSwitchCommand ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
        "An APS switch command allows a user to perform protection
         switch actions.

         If the APS switch command cannot be executed because an
         equal or higher priority request is in effect, an
         inconsistentValue error is returned.

         The Switch command values are:

         noCmd

         This value should be returned by a read request when no switch
         command has been written to the object in question since
         initialization. This value may not be used in a write
         operation.  If noCmd is used in a write operation a wrongValue
         error is returned.









         clear

         Clears all of the switch commands listed below for the
         specified channel.

         lockoutOfProtection

         Prevents any of the working channels from switching to the
         protection line. The specified channel should be the protection
         channel, otherwise an inconsistentValue error is returned.

         forcedSwitchWorkToProtect

         Switches the specified working channel to the protection line.
         If the protection channel is specified an inconsistentValue
         error is returned.

         forcedSwitchProtectToWork

         Switches the working channel back from the protection
         line to the working line. The specified channel should be
         the protection channel, otherwise an inconsistentValue
         error is returned.

         manualSwitchWorkToProtect

         Switches the specified working channel to the protection line.
         If the protection channel is specified an inconsistentValue
         error is returned.

         manualSwitchProtectToWork

         Switches the working channel back from the protection
         line to the working line. The specified channel should be
         the protection channel, otherwise an inconsistentValue
         error is returned.

         exercise

         Exercises the protocol for a protection switch of the specified
         channel by issuing an Exercise request for that channel and
         checking the response on the APS channel. "
    SYNTAX       INTEGER {
                     noCmd(1),
                     clear(2),
                     lockoutOfProtection(3),
                     forcedSwitchWorkToProtect(4),
                     forcedSwitchProtectToWork(5),





                     manualSwitchWorkToProtect(6),
                     manualSwitchProtectToWork(7),
                     exercise(8)
                 }

ApsControlCommand ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
        "An APS control command applies only to LTE that support the
         1:n architecture and performs the following actions.

         The Control command values are:

         noCmd

         This value should be returned by a read request when no control
         command has been written to the object in question since
         initialization. This value may not be used in a write
         operation.  If noCmd is used in a write operation a wrongValue
         error is returned.

         lockoutWorkingChannel

         Prevents the specified working channel from switching to the
         protection line. If the protection line is specified an
         inconsistentValue error is returned.

         clearLockoutWorkingChannel

         Clears the lockout a working channel command for the channel
         specified. If the protection line is specified an
         inconsistentValue error is returned."
    SYNTAX       INTEGER {
                     noCmd(1),
                     lockoutWorkingChannel(2),
                     clearLockoutWorkingChannel(3)
                 }

--
-- APS Configuration Table
--
-- This table supports the addition, configuration and deletion of APS
-- groups.
--

apsConfig     OBJECT IDENTIFIER ::= { apsMIBObjects 1 }







apsConfigGroups OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The count of APS groups. This count includes all rows in
         apsConfigTable, regardless of the value of apsConfigRowStatus."
    ::= { apsConfig 1 }

apsConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ApsConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table lists the APS groups that have been configured
         on the system."
    ::= { apsConfig 2 }

apsConfigEntry OBJECT-TYPE
    SYNTAX      ApsConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row in the apsConfigTable."
    INDEX { IMPLIED apsConfigName }
    ::= { apsConfigTable  1 }

ApsConfigEntry ::= SEQUENCE {
    apsConfigName                  SnmpAdminString,
    apsConfigRowStatus             RowStatus,
    apsConfigMode                  INTEGER,
    apsConfigRevert                INTEGER,
    apsConfigDirection             INTEGER,
    apsConfigExtraTraffic          INTEGER,
    apsConfigSdBerThreshold        Integer32,
    apsConfigSfBerThreshold        Integer32,
    apsConfigWaitToRestore         Integer32,
    apsConfigCreationTime          TimeStamp,
    apsConfigStorageType           StorageType
}

apsConfigName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE (1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A textual name for the APS group."
    ::= { apsConfigEntry 1 }





apsConfigRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this APS group entry.

        An entry may not exist in the active state unless all
        objects in the entry have an appropriate value. Also,
        all associated apsChanConfigEntry rows must represent
        a set of consecutive channel numbers beginning with
        0 or 1, depending on the selected architecture.

        When set to notInService changes may be made to apsConfigMode,
        apsConfigRevert, apsConfigDirection, apsConfigExtraTraffic,
        apsConfigSdBerThreshold, apsConfigSfBerThreshold,
        and apsConfigWaitToRestore. Also, associated apsChanConfigTable
        objects may be added, deleted and modified."
    ::= { apsConfigEntry 2 }

apsConfigMode OBJECT-TYPE
    SYNTAX      INTEGER {
                        onePlusOne(1),
                        oneToN(2),
                        onePlusOneCompatible(3),
                        onePlusOneOptimized(4)
                        }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The architecture of the APS group.

        onePlusOne

        The 1+1 architecture permanently bridges the working
        line to the protection line.

        oneToN

        The 1:n architecture allows one protection channel to
        protect up to n working channels. When a fault is detected
        on one of the n working channels that channel is bridged
        over the protection channel.

        onePlusOneCompatible








        This refers to 1 + 1 bidirectional switching compatible with
        1:n bidirectional switching as specified in ITU-T
        Recommendation G.783 (04/97) section A.3.4.1. Since this
        mode necessitates bidirectional switching, apsConfigDirection
        must be set to bidirectional whenever onePlusOneCompatible
        is set.

        onePlusOneOptimized

        This refers to 1 + 1 bidirectional switching optimized
        for a network using predominantly 1 + 1 bidirectional
        switching as specified in ITU-T Recommendation G.783 (04/97)
        section B.1. Since this mode necessitates bidirectional
        switching, apsConfigDirection must be set to bidirectional
        whenever onePlusOneOptimized is set.

        This object may not be modified if the associated
        apsConfigRowStatus object is equal to active(1)."
    DEFVAL {onePlusOne}
    ::= { apsConfigEntry 3 }

apsConfigRevert OBJECT-TYPE
    SYNTAX      INTEGER { nonrevertive(1), revertive(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The revertive mode of the APS group.

        nonrevertive

        Traffic remains on the protection line until another switch
        request is received.

        revertive

        When the condition that caused a switch to the protection
        line has been cleared the signal is switched back to the
        working line. Since switching is revertive with the 1:n
        architecture, apsConfigRevert must be set to revertive if
        apsConfigMode is set to oneToN.

        Switching may optionally be revertive with the 1+1 architecture.

        This object may not be modified if the associated
        apsConfigRowStatus object is equal to active(1). "
    DEFVAL { nonrevertive }
    ::= { apsConfigEntry 4 }






apsConfigDirection OBJECT-TYPE
    SYNTAX      INTEGER { unidirectional(1), bidirectional(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The directional mode of the APS group.

        unidirectional

        The unidirectional mode provides protection in one direction.

        bidirectional

        The bidirectional mode provides protection in both
        directions.

        This object may not be modified if the associated
        apsConfigRowStatus object is equal to active(1). "
    DEFVAL {unidirectional}
    ::= { apsConfigEntry 5 }

apsConfigExtraTraffic OBJECT-TYPE
    SYNTAX      INTEGER { enabled(1), disabled(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "This object enables or disables the transfer of extra traffic
        on the protection channel in a 1:n architecture. This object
        must be set to disabled if the architecture is 1+1. It may be
        necessary to disable this in order to interwork with other SONET
        network elements that don't support extra traffic.

        This object may not be modified if the associated
        apsConfigRowStatus object is equal to active(1). "
    DEFVAL { disabled }
    ::= { apsConfigEntry 6 }

apsConfigSdBerThreshold OBJECT-TYPE
    SYNTAX      Integer32 (5..9)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Signal Degrade Bit Error Rate.

         The negated value of this number is used as the exponent of
         10 for computing the threshold value for the Bit Error Rate
         (BER). For example, a value of 5 indicates a BER threshold of
         10^-5.





         This object may be modified if the associated
         apsConfigRowStatus object is equal to active(1)."
    DEFVAL { 5 }
    ::= { apsConfigEntry 7 }

apsConfigSfBerThreshold OBJECT-TYPE
    SYNTAX      Integer32 (3..5)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Signal Failure Bit Error Rate.

         The negated value of this number is used as the exponent of
         10 for computing the threshold value for the Bit Error Rate
         (BER). For example, a value of 5 indicates a BER threshold of
         10^-5.

         This object may be modified if the associated
         apsConfigRowStatus object is equal to active(1)."
    DEFVAL { 3 }
    ::= { apsConfigEntry 8 }

apsConfigWaitToRestore OBJECT-TYPE
    SYNTAX      Integer32 (0..720)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Wait To Restore period in seconds.

         After clearing of a condition that necessitated an
         automatic switch, the wait to restore period must elapse
         before reverting. This is intended to avoid rapid switch
         oscillations.

         GR-253-CORE specifies a Wait To Restore range of 5 to 12
         minutes. G.783 defines a 5 to 12 minute Wait To Restore
         range in section 5.4.1.1.3, but also allows for a shorter
         WTR period in  Table 2-1,
         WaitToRestore value (MI_WTRtime: 0..(5)..12 minutes).

         This object may not be modified if the associated
         apsConfigRowStatus object is equal to active(1)."
    DEFVAL { 300 }
    ::= { apsConfigEntry 9 }








apsConfigCreationTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime at the time the row was
         created"
    ::= { apsConfigEntry 10 }

apsConfigStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this conceptual row.
         Conceptual rows having the value 'permanent' need not
         allow write-access to any columnar objects in the row."
    DEFVAL      { nonVolatile }
    ::= { apsConfigEntry 11 }

--
-- APS Status Table
--
-- This table provides APS group statistics.
--

apsStatusTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ApsStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides status information about APS groups
         that have been configured on the system."
    ::= { apsMIBObjects 2 }

apsStatusEntry OBJECT-TYPE
    SYNTAX      ApsStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row in the apsStatusTable."
    AUGMENTS { apsConfigEntry }
    ::= { apsStatusTable  1 }

ApsStatusEntry ::= SEQUENCE {
    apsStatusK1K2Rcv               ApsK1K2,
    apsStatusK1K2Trans             ApsK1K2,
    apsStatusCurrent               BITS,





    apsStatusModeMismatches        Counter32,
    apsStatusChannelMismatches     Counter32,
    apsStatusPSBFs                 Counter32,
    apsStatusFEPLFs                Counter32,
    apsStatusSwitchedChannel       Integer32,
    apsStatusDiscontinuityTime     TimeStamp
}

apsStatusK1K2Rcv OBJECT-TYPE
    SYNTAX      ApsK1K2
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current value of the K1 and K2 bytes received on the
         protection channel."
    ::= { apsStatusEntry 1 }

apsStatusK1K2Trans OBJECT-TYPE
    SYNTAX        ApsK1K2
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The current value of the K1 and K2 bytes transmitted on the
         protection channel."
    ::= { apsStatusEntry 2 }

apsStatusCurrent OBJECT-TYPE
    SYNTAX      BITS {
                  modeMismatch(0),
                  channelMismatch(1),
                  psbf(2),
                  feplf(3),
                  extraTraffic(4)
                 }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current status of the APS group.

         modeMismatch

         Modes other than 1+1 unidirectional monitor protection line
         K2 bit 5, which indicates the architecture and K2 bits
         6-8, which indicate if the mode is unidirectional or
         bidirectional. A conflict between the current local mode
         and the received K2 mode information constitutes a
         mode mismatch.






         channelMismatch

         This bit indicates a  mismatch between the transmitted K1
         channel and the received K2 channel has been detected.

         psbf

         This bit indicates a Protection Switch Byte Failure (PSBF) is
         in effect. This condition occurs when either an inconsistent
         APS byte or an invalid code is detected. An inconsistent APS
         byte occurs when no three consecutive K1 bytes of the last 12
         successive frames are identical, starting with the last frame
         containing a previously consistent byte. An invalid code occurs
         when the incoming K1 byte contains an unused code or a code
         irrelevant for the specific switching operation (e.g., Reverse
         Request while no switching request is outstanding) in three
         consecutive frames. An invalid code also occurs when the
         incoming K1 byte contains an invalid channel number in three
         consecutive frames.

         feplf

         Modes other than 1+1 unidirectional monitor the K1 byte
         for Far-End Protection-Line failures. A Far-End
         Protection-Line defect is declared based on receiving
         SF on the protection line.

         extraTraffic

         This bit indicates whether extra traffic is currently being
         accepted on the protection line. "
    ::= { apsStatusEntry 3 }

apsStatusModeMismatches OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A count of Mode Mismatch conditions.

         Discontinuities in the value of this counter can occur at
         re-initialization of the management system, and at other
         times as indicated by the value of
         apsStatusDiscontinuityTime."
    ::= { apsStatusEntry 4 }








apsStatusChannelMismatches OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A count of Channel Mismatch conditions.

         Discontinuities in the value of this counter can occur at
         re-initialization of the management system, and at other
         times as indicated by the value of
         apsStatusDiscontinuityTime."
    ::= { apsStatusEntry 5 }

apsStatusPSBFs OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A count of Protection Switch Byte Failure conditions.
         This condition occurs when either an inconsistent APS
         byte or an invalid code is detected. An inconsistent APS
         byte occurs when no three consecutive K1 bytes of the last
         12 successive frames are identical, starting with the last
         frame containing a previously consistent byte. An invalid
         code occurs when the incoming K1 byte contains an unused
         code or a code irrelevant for the specific switching
         operation (e.g., Reverse Request while no switching request
         is outstanding) in three consecutive frames. An invalid code
         also occurs when the incoming K1 byte contains an invalid
         channel number in three consecutive frames.

         Discontinuities in the value of this counter can occur at
         re-initialization of the management system, and at other
         times as indicated by the value of
         apsStatusDiscontinuityTime."
    ::= { apsStatusEntry 6 }

apsStatusFEPLFs OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A count of Far-End Protection-Line Failure conditions.
         This condition is declared based on receiving SF on
         the protection line in the K1 byte.








         Discontinuities in the value of this counter can occur at
         re-initialization of the management system, and at other
         times as indicated by the value of
         apsStatusDiscontinuityTime."
    ::= { apsStatusEntry 7 }

apsStatusSwitchedChannel OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This field is set to the number of the channel that is
         currently switched to protection. The value 0 indicates no
         channel is switched to protection. The values 1-14 indicate
         that working channel is switched to protection."
    ::= { apsStatusEntry 8 }

apsStatusDiscontinuityTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime on the most recent occasion at which
         any one or more of this APS group's counters suffered a
         discontinuity.  The relevant counters are the specific
         instances associated with this APS group of any Counter32
         object contained in apsStatusTable. If no such
         discontinuities have occurred since the last re-initialization
         of the local management subsystem, then this object contains
         a zero value."
    ::= { apsStatusEntry 9 }

--
-- APS Map Group
--
-- Lists the SONET LTE interfaces that may be used to create APS groups.
--

apsMap      OBJECT IDENTIFIER ::= { apsMIBObjects 3 }

apsChanLTEs OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The count of SONET LTE interfaces on the system.
         Each interface that is included has an ifType value of
         sonet(39)."





    ::= { apsMap 1 }

apsMapTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ApsMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table lists the SONET LTE interfaces on the system.
         Each interface that is listed has an ifType value of
         sonet(39)."
    ::= { apsMap 2 }

apsMapEntry OBJECT-TYPE
    SYNTAX      ApsMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row in the apsMapTable."
    INDEX { ifIndex }
    ::= { apsMapTable  1 }

ApsMapEntry ::= SEQUENCE {
    apsMapGroupName             SnmpAdminString,
    apsMapChanNumber            Integer32
}

apsMapGroupName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A textual name for the APS group which this channel is
         included in. If the channel is not part of an APS group
         this value is set to a string of size 0.

         When an instance of apsChanConfigIfIndex is set equal to an
         instance of ifIndex that has an ifType value of sonet(39),
         apsMapGroupName is set equal to the corresponding value of
         apsChanConfigGroupName.

         If an instance of ifIndex that has an ifType value of
         sonet(39) ceases to be equal to an instance of
         apsChanConfigIfIndex, either because of a change in the value
         of apsChanConfigIfIndex, or because of row deletion in the
         ApsChanConfigTable, apsMapGroupName is set to a string of
         size 0."
    ::= { apsMapEntry 2 }






apsMapChanNumber OBJECT-TYPE
    SYNTAX     Integer32 (-1..14)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This field is set to a unique channel number within an APS
         group.  The value 0 indicates the null channel. The values
         1-14 define a working channel. If the SONET LTE is not part
         of an APS group this value is set to -1.

         When an instance of apsChanConfigIfIndex is set equal to an
         instance of ifIndex that has an  ifType value of sonet(39),
         apsMapChanNumber is set equal to the corresponding value of
         apsChanConfigNumber.

         If an instance of ifIndex that has an  ifType value of
         sonet(39) ceases to be equal to an instance of
         apsChanConfigIfIndex, either because of a change in the
         value of apsChanConfigIfIndex, or because of row deletion
         in the ApsChanConfigTable, apsMapChanNumber is set to -1."
    ::= { apsMapEntry 3 }

--
-- APS Channel Configuration Table
--
-- This table supports the addition, configuration and deletion of
-- channels in APS groups.
--

apsChanConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ApsChanConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table lists the APS channels that have been configured
         in APS groups."
    ::= { apsMIBObjects 4 }

apsChanConfigEntry OBJECT-TYPE
    SYNTAX      ApsChanConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row in the apsChanConfigTable."
    INDEX {apsChanConfigGroupName, apsChanConfigNumber}
    ::= { apsChanConfigTable  1 }







ApsChanConfigEntry ::= SEQUENCE {
    apsChanConfigGroupName             SnmpAdminString,
    apsChanConfigNumber                Integer32,
    apsChanConfigRowStatus             RowStatus,
    apsChanConfigIfIndex               InterfaceIndex,
    apsChanConfigPriority              INTEGER,
    apsChanConfigStorageType           StorageType
}

apsChanConfigGroupName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE (1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A textual name for the APS group which this channel is
         included in."
    ::= { apsChanConfigEntry 1 }

apsChanConfigNumber OBJECT-TYPE
    SYNTAX     Integer32 (0..14)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This field is set to a unique channel number within an APS
         group.  The value 0 indicates the null channel.  The values
         1-14 define a working channel.

         This field must be assigned a unique number within the group."
    ::= { apsChanConfigEntry 2 }

apsChanConfigRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this APS channel entry.

         An entry may not exist in the active state unless all
         objects in the entry have an appropriate value.

         A row in the apsChanConfigTable may not be created,
         deleted, set to notInService or otherwise modified
         if the apsChanConfigGroupName value is equal to an
         apsConfigName value and the associated apsConfigRowStatus
         object is equal to active. However, if the apsConfigRowStatus
         object is equal to notInService, a row may be created, deleted
         or modified. In other words, a channel may not be added,
         deleted or modified if the group is active.





         A row may be created with an apsChanConfigGroupName value
         that is not equal to any existing instance of apsConfigName.
         This action is the initial step in adding a SONET LTE to a
         new APS group.

         If this object is set to destroy, the associated instance
         of apsMapGroupName will be set to a string of size 0 and
         the apsMapChanNumber will be set to -1. The channel status
         entry will also be deleted by this action.

         apsChanConfigNumber must be set to a unique channel number
         within the APS group. The value 0 indicates the null channel.
         The values 1-14 define a working channel. When an attempt is
         made to set the  corresponding apsConfigRowStatus field to
         active the apsChanConfigNumber values of all entries with equal
         apsChanConfigGroupName fields must represent a set of
         consecutive integer values beginning with 0 or 1, depending on
         the architecture of the group, and ending with n, where n is
         greater than or equal to 1 and less than or equal to 14.
         Otherwise, the error inconsistentValue is returned to the
         apsConfigRowStatus set attempt."
    ::= { apsChanConfigEntry 3 }

apsChanConfigIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "The Interface Index assigned to a SONET LTE. This is an
         interface with ifType sonet(39). The value of this object
         must be unique among all instances of apsChanConfigIfIndex.
         In other words, a particular SONET LTE can only be configured
         in one APS group.

         This object cannot be set if the apsChanConfigGroupName
         instance associated with this row is equal to an instance of
         apsConfigName and the corresponding apsConfigRowStatus object
         is set to active.  In other words this value cannot be changed
         if the APS group is active. However, this value may be changed
         if the apsConfigRowStatus value is equal to notInService."
    ::= { apsChanConfigEntry 4 }

apsChanConfigPriority OBJECT-TYPE
    SYNTAX     INTEGER {low(1), high(2)}
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "The priority of the channel.





         This field determines whether high or low priority
         SD and SF codes are used in K1 requests.

         This field is only applicable if the channel is to be included
         in a group using the 1:n architecture. It is not applicable if
         the channel is to be included in a group using the 1+1
         architecture, and is ignored in that case.

         This object cannot be set if the apsChanConfigGroupName
         instance associated with this row is equal to an instance of
         apsConfigName and the corresponding apsConfigRowStatus object
         is set to active.  In other words this value cannot be changed
         if the APS group is active.  However, this value may be changed
         if the apsConfigRowStatus value is equal to notInService."
    DEFVAL { low }
    ::= { apsChanConfigEntry 5 }

apsChanConfigStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this conceptual row.
         Conceptual rows having the value 'permanent' need not
         allow write-access to any columnar objects in the row."
    DEFVAL { nonVolatile }
    ::= { apsChanConfigEntry 6 }

--
-- APS Command Table
--
-- This table provides the ability to initiate APS commands.
--

apsCommandTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ApsCommandEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table allows commands to be sent to configured APS
          groups."
    ::= { apsMIBObjects 5 }

apsCommandEntry OBJECT-TYPE
    SYNTAX      ApsCommandEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION





        "A conceptual row in the apsCommandTable. This row exists only
         if the associated apsConfigEntry is active."
    INDEX {apsChanConfigGroupName, apsChanConfigNumber}
    ::= { apsCommandTable  1 }

ApsCommandEntry ::= SEQUENCE {
    apsCommandSwitch         ApsSwitchCommand,
    apsCommandControl        ApsControlCommand
}

apsCommandSwitch OBJECT-TYPE
    SYNTAX      ApsSwitchCommand
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Allows the initiation of an APS switch command on the
         APS group and channel specified by the index values.

         When read this object returns the last command written
         or noCmd if no command has been written to this
         channel since initialization. The return of the last command
         written does not imply that this command is currently in
         effect.  This request may have been preempted by a higher
         priority local or remote request. In order to determine the
         current state of the APS group it is necessary to read
         the objects apsStatusK1K2Rcv and apsStatusK1K2Trans.

         The value lockoutOfProtection should only be applied to the
         protection line channel since that switch command prevents any
         of the working channels from switching to the protection line.
         Following the same logic, forcedSwitchProtectToWork and
         manualSwitchProtectToWork should only be applied to the
         protection line channel.

         forcedSwitchWorkToProtect and manualSwitchWorkToProtect
         should only be applied to a working channel."
    ::= { apsCommandEntry 1 }

apsCommandControl OBJECT-TYPE
    SYNTAX      ApsControlCommand
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Allows the initiation of an APS control command on the
         APS group and channel specified by the index values.








         When read this object returns the last command written or
         noCmd if no command has been written to this channel since
         initialization.

         This object does not apply to the protection line."
    ::= { apsCommandEntry 2 }

--
-- APS Channel Status Table
--
-- This table provides APS channel statistics.
--

apsChanStatusTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ApsChanStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains status information for all SONET LTE
         interfaces that are included in APS groups."
    ::= { apsMIBObjects 6 }

apsChanStatusEntry OBJECT-TYPE
    SYNTAX      ApsChanStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row in the apsChanStatusTable."
    AUGMENTS { apsChanConfigEntry }
    ::= { apsChanStatusTable  1 }

ApsChanStatusEntry ::= SEQUENCE {
    apsChanStatusCurrent               BITS,
    apsChanStatusSignalDegrades        Counter32,
    apsChanStatusSignalFailures        Counter32,
    apsChanStatusSwitchovers           Counter32,
    apsChanStatusLastSwitchover        TimeStamp,
    apsChanStatusSwitchoverSeconds     Counter32,
    apsChanStatusDiscontinuityTime     TimeStamp
}

apsChanStatusCurrent OBJECT-TYPE
    SYNTAX     BITS {
               lockedOut(0),
               sd(1),
               sf(2),
               switched(3),
               wtr(4)





            }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Indicates the current state of the port.

         lockedOut

         This bit, when applied to a working channel, indicates that
         the channel is prevented from switching to the protection
         line.  When applied to the null channel, this bit indicates
         that no working channel may switch to the protection line.

         sd

         A signal degrade condition is in effect.

         sf

         A signal failure condition is in effect.

         switched

         The switched bit is applied to a working channel if that
         channel is currently switched to the protection line.

         wtr

         A Wait-to-Restore state is in effect."
    ::= { apsChanStatusEntry 1 }

apsChanStatusSignalDegrades OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A count of Signal Degrade conditions. This condition
         occurs when the line Bit Error Rate exceeds the currently
         configured value of the relevant instance of
         apsConfigSdBerThreshold.

         Discontinuities in the value of this counter can occur at
         re-initialization of the management system, and at other
         times as indicated by the value of
         apsChanStatusDiscontinuityTime."

    ::= { apsChanStatusEntry 2 }






apsChanStatusSignalFailures OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A count of Signal Failure conditions that have been
         detected on the incoming signal. This condition occurs
         when a loss of signal, loss of frame, AIS-L or a Line
         bit error rate exceeding the currently configured value of
         the relevant instance of apsConfigSfBerThreshold.

         Discontinuities in the value of this counter can occur at
         re-initialization of the management system, and at other
         times as indicated by the value of
         apsChanStatusDiscontinuityTime."

    ::= { apsChanStatusEntry 3 }

apsChanStatusSwitchovers OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "When queried with index value apsChanConfigNumber other than
         0, this object will return the number of times this channel
         has switched to the protection line.

         When queried with index value apsChanConfigNumber set to 0,
         which is the protection line, this object will return the
         number of times that any working channel has been switched
         back to the working line from this protection line.

         Discontinuities in the value of this counter can occur at
         re-initialization of the management system, and at other
         times as indicated by the value of
         apsChanStatusDiscontinuityTime."

    ::= { apsChanStatusEntry 4 }

apsChanStatusLastSwitchover OBJECT-TYPE
    SYNTAX     TimeStamp
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "When queried with index value apsChanConfigNumber other than
         0, this object will return the value of sysUpTime when this
         channel last completed a switch to the protection line. If






         this channel has never switched to the protection line, the
         value 0 will be returned.

         When queried with index value apsChanConfigNumber set to 0,
         which is the protection line, this object will return the
         value of sysUpTime the last time that a working channel was
         switched back to the working line from this protection line.
         If no working channel has ever switched back to the working
         line from this protection line, the value 0 will be returned."

    ::= { apsChanStatusEntry 5 }

apsChanStatusSwitchoverSeconds OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The cumulative Protection Switching Duration (PSD) time in
         seconds. For a working channel, this is the cumulative number
         of seconds that service was carried on the protection line.
         For the protection line, this is the cumulative number of
         seconds that the protection line has been used to carry any
         working channel traffic. This information is only valid if
         revertive switching is enabled. The value 0 will be returned
         otherwise.

         Discontinuities in the value of this counter can occur at
         re-initialization of the management system, and at other
         times as indicated by the value of
         apsChanStatusDiscontinuityTime. For example, if the value
         of an instance of apsChanStatusSwitchoverSeconds changes
         from a non-zero value to zero due to revertive switching
         being disabled, it is expected that the corresponding
         value of apsChanStatusDiscontinuityTime will be updated
         to reflect the time of the configuration change.
         "
    ::= { apsChanStatusEntry 6 }

apsChanStatusDiscontinuityTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime on the most recent occasion at which
         any one or more of this channel's counters suffered a
         discontinuity.  The relevant counters are the specific
         instances associated with this channel of any Counter32
         object contained in apsChanStatusTable. If no such





         discontinuities have occurred since the last re-initialization
         of the local management subsystem, then this object contains
         a zero value."
    ::= { apsChanStatusEntry 7 }

apsNotificationEnable OBJECT-TYPE
    SYNTAX     BITS {
               switchover(0),
               modeMismatch(1),
               channelMismatch(2),
               psbf(3),
               feplf(4)
            }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Provides the ability to enable and disable notifications
         defined in this MIB.

         switchover

         Indicates  apsEventSwitchover notifications
         should be generated.

         modeMismatch

         Indicates  apsEventModeMismatch notifications
         should be generated.

         channelMismatch

         Indicates  apsEventChannelMismatch notifications
         should be generated.

         psbf

         Indicates  apsEventPSBF notifications
         should be generated.

         feplf

         Indicates  apsEventFEPLF notifications
         should be generated. "
    DEFVAL { { } }
    ::= { apsMIBObjects 7 }

--
-- APS EVENTS





--

apsNotificationsPrefix OBJECT IDENTIFIER
        ::= { apsMIBNotifications 0 }

apsEventSwitchover NOTIFICATION-TYPE
    OBJECTS { apsChanStatusSwitchovers, apsChanStatusCurrent }
    STATUS  current
    DESCRIPTION
        "An apsEventSwitchover notification is sent when the
        value of an instance of apsChanStatusSwitchovers increments."
    ::= { apsNotificationsPrefix 1 }

apsEventModeMismatch NOTIFICATION-TYPE
    OBJECTS { apsStatusModeMismatches, apsStatusCurrent }
    STATUS  current
    DESCRIPTION
        "An apsEventModeMismatch notification is sent when the
        value of an instance of apsStatusModeMismatches increments."
    ::= { apsNotificationsPrefix 2 }

apsEventChannelMismatch NOTIFICATION-TYPE
    OBJECTS { apsStatusChannelMismatches, apsStatusCurrent }
    STATUS  current
    DESCRIPTION
        "An apsEventChannelMismatch notification is sent when the
        value of an instance of apsStatusChannelMismatches increments."
    ::= { apsNotificationsPrefix 3 }

apsEventPSBF NOTIFICATION-TYPE
    OBJECTS { apsStatusPSBFs, apsStatusCurrent }
    STATUS  current
    DESCRIPTION
        "An apsEventPSBF notification is sent when the
        value of an instance of apsStatusPSBFs increments."
    ::= { apsNotificationsPrefix 4 }

apsEventFEPLF NOTIFICATION-TYPE
    OBJECTS { apsStatusFEPLFs, apsStatusCurrent }
    STATUS  current
    DESCRIPTION
        "An apsEventFEPLFs notification is sent when the
        value of an instance of apsStatusFEPLFs increments."
    ::= { apsNotificationsPrefix 5 }

-- conformance information







apsGroups      OBJECT IDENTIFIER ::= { apsMIBConformance 1 }
apsCompliances OBJECT IDENTIFIER ::= { apsMIBConformance 2 }

apsFullCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
        "When this MIB is implemented with support for read-create, then
        such an implementation can claim read/write compliance. Linear
        APS groups can then be both monitored and configured with this
        MIB.

        Note that An agent is not required to process SNMP Set Requests
        that affect multiple control objects within this MIB. This is
        intended to simplify the processing of Set Requests for the
        various control tables by eliminating the possibility that a
        single Set PDU will contain multiple varbinds which are in
        conflict. "

    MODULE
    MANDATORY-GROUPS { apsConfigGeneral, apsStatusGeneral,
                       apsChanGeneral }

        OBJECT  apsConfigRowStatus
        SYNTAX INTEGER { active(1) }
        WRITE-SYNTAX INTEGER { createAndGo(4), destroy(6) }
        DESCRIPTION
            "Support for createAndWait and notInService is not
             required."

        OBJECT  apsChanConfigRowStatus
        SYNTAX INTEGER { active(1) }
        WRITE-SYNTAX INTEGER { createAndGo(4), destroy(6) }
        DESCRIPTION
            "Support for createAndWait and notInService is not
             required."

        GROUP       apsConfigWtr
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations. The information is
             applicable to groups supporting a configurable
             WTR period."

        GROUP       apsCommandOnePlusOne
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations. The information is
             applicable to groups implementing the linear





             APS 1+1 architecture and supporting set operations."

       GROUP       apsCommandOneToN
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations. The information is
             applicable to groups implementing the linear
             APS 1:n architecture and supporting set operations."

       GROUP       apsChanOneToN
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations. The information is
             applicable to groups implementing the linear
             APS 1:n architecture."

       GROUP       apsTotalsGroup
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations."

       GROUP       apsMapGroup
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations."

       GROUP       apsEventGroup
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations."

    ::= { apsCompliances 1 }

--
-- Read-Only Compliance
--

apsReadOnlyCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
        "When this MIB is implemented without support for read-create
         (i.e. in read-only mode), then that implementation can claim
         read-only compliance. In that case, linear APS groups can be
         monitored but cannot be configured with this MIB."

    MODULE
    MANDATORY-GROUPS { apsConfigGeneral, apsStatusGeneral,
                       apsChanGeneral }





        OBJECT  apsConfigMode
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsConfigRevert
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsConfigDirection
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsConfigExtraTraffic
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsConfigSdBerThreshold
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsConfigSfBerThreshold
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsConfigWaitToRestore
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsConfigRowStatus
        SYNTAX  INTEGER { active(1) }
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required, and active is the only status
             that needs to be supported."

        OBJECT  apsConfigStorageType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsChanConfigIfIndex





        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsChanConfigPriority
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsChanConfigRowStatus
        SYNTAX  INTEGER { active(1) }
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required, and active is the only status
             that needs to be supported."

        OBJECT  apsChanConfigStorageType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT  apsNotificationEnable
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required."

        GROUP       apsConfigWtr
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations. The information is
             applicable to groups supporting a configurable
             WTR period."

        GROUP       apsCommandOnePlusOne
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations. The information is
             applicable to groups implementing the linear
             APS 1+1 architecture and supporting set operations."

       GROUP       apsCommandOneToN
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations. The information is
             applicable to groups implementing the linear
             APS 1:n architecture and supporting set operations."

       GROUP       apsChanOneToN





        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations. The information is
             applicable to groups implementing the linear
             APS 1:n architecture."

       GROUP       apsTotalsGroup
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations."

       GROUP       apsMapGroup
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations."

       GROUP       apsEventGroup
        DESCRIPTION
            "Implementation of this group is optional for all
             linear APS implementations."

    ::= { apsCompliances 2 }

-- units of conformance

apsConfigGeneral    OBJECT-GROUP
    OBJECTS
    {
        apsConfigMode,
        apsConfigRevert,
        apsConfigDirection,
        apsConfigExtraTraffic,
        apsConfigSdBerThreshold,
        apsConfigSfBerThreshold,
        apsConfigCreationTime,
        apsConfigRowStatus,
        apsConfigStorageType,
        apsNotificationEnable
    }
    STATUS  current
    DESCRIPTION
        "A collection of apsConfigTable objects providing configuration
         information applicable to all linear APS groups."
    ::= { apsGroups 1 }

apsConfigWtr    OBJECT-GROUP
    OBJECTS
    {





        apsConfigWaitToRestore
    }
    STATUS  current
    DESCRIPTION
        "The apsConfigTable object that provides information which is
         applicable to groups supporting a configurable WTR period."
    ::= { apsGroups 2 }

--  If set operations are not supported neither of the following two
--  groups are implemented. If sets are supported only one of these
--  groups is implemented for a linear APS group instance.

apsCommandOnePlusOne    OBJECT-GROUP
    OBJECTS
    {
        apsCommandSwitch
    }
    STATUS  current
    DESCRIPTION
        "The  apsCommandTable object which is applicable to groups
         implementing the linear APS 1+1 architecture. Also, set
         operations must be supported."
    ::= { apsGroups 3 }

apsCommandOneToN    OBJECT-GROUP
    OBJECTS
    {
        apsCommandSwitch,
        apsCommandControl
    }
    STATUS  current
    DESCRIPTION
        "A collection of apsCommandTable objects which are applicable to
         groups implementing the linear APS 1:n architecture. Also, set
         operations must be supported."
    ::= { apsGroups 4 }

apsStatusGeneral    OBJECT-GROUP
    OBJECTS
    {
        apsStatusK1K2Rcv,
        apsStatusK1K2Trans,
        apsStatusCurrent,
        apsStatusModeMismatches,
        apsStatusChannelMismatches,
        apsStatusPSBFs,
        apsStatusFEPLFs,
        apsStatusSwitchedChannel,





        apsStatusDiscontinuityTime
    }
    STATUS  current
    DESCRIPTION
        "A collection of apsStatusTable objects providing status
         information applicable to all linear APS groups."
    ::= { apsGroups 5 }

apsChanGeneral    OBJECT-GROUP
    OBJECTS
    {
        apsChanConfigIfIndex,
        apsChanConfigRowStatus,
        apsChanConfigStorageType,
        apsChanStatusCurrent,
        apsChanStatusSignalDegrades,
        apsChanStatusSignalFailures,
        apsChanStatusSwitchovers,
        apsChanStatusLastSwitchover,
        apsChanStatusSwitchoverSeconds,
        apsChanStatusDiscontinuityTime
   }
    STATUS  current
    DESCRIPTION
        "A collection of channel objects providing information
         applicable to all linear APS channels."
    ::= { apsGroups 6 }

apsChanOneToN    OBJECT-GROUP
    OBJECTS
    {
        apsChanConfigPriority
    }
    STATUS  current
    DESCRIPTION
        "The apsChanConfigTable object that provides information which
         is only applicable to groups implementing the linear APS 1:n
         architecture."
    ::= { apsGroups 7 }

apsTotalsGroup OBJECT-GROUP
    OBJECTS
    {
        apsConfigGroups,
        apsChanLTEs
    }
    STATUS  current
    DESCRIPTION





        "A collection of objects providing optional counts of configured
         APS groups and SONET LTE interfaces."
    ::= { apsGroups 8 }

apsMapGroup OBJECT-GROUP
    OBJECTS
    {
        apsMapGroupName,
        apsMapChanNumber
    }
    STATUS  current
    DESCRIPTION
        "A collection of apsMapTable objects providing a mapping
         from sonet(39) InterfaceIndex to group name and channel
         number for assigned APS channels and a list of unassigned
         sonet(39) interfaces."
    ::= { apsGroups 9 }

apsEventGroup NOTIFICATION-GROUP
    NOTIFICATIONS {apsEventSwitchover, apsEventModeMismatch,
                   apsEventChannelMismatch, apsEventPSBF,
                   apsEventFEPLF }
    STATUS    current
    DESCRIPTION
        "A collection of SONET linear APS notifications."
    ::= { apsGroups 10 }

END


