CIRCUIT-IF-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    mib-2, Gauge32                          FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, RowStatus,
    TimeStamp, RowPointer, StorageType      FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP         FROM SNMPv2-CONF
    ifIndex, InterfaceIndex                 FROM IF-MIB;

    circuitIfMIB MODULE-IDENTITY
        LAST-UPDATED "200201030000Z" -- January 3, 2002
        ORGANIZATION "IETF Frame Relay Service MIB Working Group"
        CONTACT-INFO





          "IETF Frame Relay Service MIB (frnetmib) Working Group

           WG Charter:    http://www.ietf.org/html.charters/
                                 frnetmib-charter.html
           WG-email:      frnetmib@sunroof.eng.sun.com
           Subscribe:     frnetmib-request@sunroof.eng.sun.com
           Email Archive: ftp://ftp.ietf.org/ietf-mail-archive/frnetmib

           Chair:      Andy Malis
                       Vivace Networks
           Email:      Andy.Malis@vivacenetworks.com

           WG editor:  Robert Steinberger
                       Paradyne Networks and
                       Fujitsu Network Communications
           Email:      robert.steinberger@fnc.fujitsu.com

           Co-author:  Orly Nicklass
                       RAD Data Communications Ltd.
           EMail:      Orly_n@rad.co.il"
        DESCRIPTION
            "The MIB module to allow insertion of selected circuit into
             the ifTable."
        REVISION "200201030000Z" -- January 3, 2002
        DESCRIPTION
            "Initial version, published as RFC 3201"
        ::= { mib-2 94 }

    -- Textual Conventions

    CiFlowDirection ::= TEXTUAL-CONVENTION
        STATUS  current
        DESCRIPTION
            "The direction of data flow thru a circuit.

                transmit(1) - Only transmitted data
                receive(2)  - Only received data
                both(3)     - Both transmitted and received data."
        SYNTAX  INTEGER {
                  transmit(1),
                  receive(2),
                  both(3)
                }

    ciObjects      OBJECT IDENTIFIER ::= { circuitIfMIB 1 }
    ciCapabilities OBJECT IDENTIFIER ::= { circuitIfMIB 2 }
    ciConformance  OBJECT IDENTIFIER ::= { circuitIfMIB 3 }






    -- The Circuit Interface Circuit Table
    --
    -- This table is used to define and display the circuits that
    -- are added to the ifTable.  It maps circuits to their respective
    -- ifIndex values.

    ciCircuitTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF CiCircuitEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The Circuit Interface Circuit Table."
        ::= { ciObjects 1 }

    ciCircuitEntry OBJECT-TYPE
        SYNTAX      CiCircuitEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the Circuit Interface Circuit Table."
        INDEX    { ciCircuitObject, ciCircuitFlow }
        ::= { ciCircuitTable 1 }

    CiCircuitEntry ::=
        SEQUENCE {
            --
            -- Index Control Variables
            --
            ciCircuitObject      RowPointer,
            ciCircuitFlow        CiFlowDirection,
            ciCircuitStatus      RowStatus,
            --
            -- Data variables
            --
            ciCircuitIfIndex     InterfaceIndex,
            ciCircuitCreateTime  TimeStamp,
            --
            -- Data Persistence
            --
            ciCircuitStorageType StorageType
        }

    ciCircuitObject OBJECT-TYPE
        SYNTAX      RowPointer
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This value contains the RowPointer that uniquely





             describes the circuit that is to be added to this table.
             Any RowPointer that will force the size of OBJECT
             IDENTIFIER of the row to grow beyond the legal limit
             MUST be rejected.

             The purpose of this object is to point a network manager
             to the table in which the circuit was created as well as
             define the circuit on which the interface is defined.

             Valid tables for this object include the frCircuitTable
             from the Frame Relay DTE MIB(FRAME-RELAY-DTE-MIB), the
             frPVCEndptTable from the Frame Relay Service MIB
             (FRNETSERV-MIB), and the aal5VccTable from the ATM MIB
             (ATM MIB).  However, including circuits from other MIB
             tables IS NOT prohibited."
        ::= { ciCircuitEntry 1 }

    ciCircuitFlow OBJECT-TYPE
        SYNTAX      CiFlowDirection
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The direction of data flow through the circuit for which
             the virtual interface is defined.  The following define
             the information that the virtual interface will report.

                transmit(1) - Only transmitted frames
                receive(2)  - Only received frames
                both(3)     - Both transmitted and received frames.

             It is recommended that the ifDescr of the circuit
             interfaces that are not both(3) SHOULD have text warning
             the operators that the particular interface represents
             only half the traffic on the circuit."
        ::= { ciCircuitEntry 2 }

    ciCircuitStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The status of the current row.  This object is
             used to add, delete, and disable rows in this
             table.  When the status changes to active(1), a row
             will also be added to the interface map table below
             and a row will be added to the ifTable.  These rows
             SHOULD not be removed until the status is changed
             from active(1).  The value of ifIndex for the row that





             is added to the ifTable is determined by the agent
             and MUST follow the rules of the ifTable.  The value
             of ifType for that interface will be frDlciEndPt(193)
             for a frame relay circuit, atmVciEndPt(194) for an
             ATM circuit, or another ifType defining the circuit
             type for any other circuit.

             When this object is set to destroy(6), the associated
             row in the interface map table will be removed and the
             ifIndex will be removed from the ifTable.  Removing
             the ifIndex MAY initiate a chain of events that causes
             changes to other tables as well.

             The rows added to this table MUST have a valid object
             identifier for ciCircuitObject.  This means that the
             referenced object must exist and it must be in a table
             that supports circuits.

             The object referenced by ciCircuitObject MUST exist
             prior to transitioning a row to active(1).  If at any
             point the object referenced by ciCircuitObject does not
             exist or the row containing it is not in the active(1)
             state, the status SHOULD either age out the row or
             report notReady(3).  The effects transitioning from
             active(1) to notReady(3) are the same as those caused
             by setting the status to destroy(6).

             Each row in this table relies on information from other
             MIB modules.  The rules persistence of data SHOULD follow
             the same rules as those of the underlying MIB module.
             For example, if the circuit defined by ciCircuitObject
             would normally be stored in non-volatile memory, then
             the row SHOULD also be non-volatile."
        ::= { ciCircuitEntry 3 }

    ciCircuitIfIndex OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The ifIndex that the agent assigns to this row."
        ::= { ciCircuitEntry 4 }

    ciCircuitCreateTime OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION





            "This object returns the value of sysUpTime at the time
             the value of ciCircuitStatus last transitioned to
             active(1).  If ciCircuitStatus has never been active(1),
             this object SHOULD return 0."
        ::= { ciCircuitEntry 5 }

    ciCircuitStorageType OBJECT-TYPE
        SYNTAX      StorageType
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The storage type used for this row."
    ::= { ciCircuitEntry 6 }

    -- The Circuit Interface Map Table
    --
    -- This table maps the ifIndex values that are assigned to
    -- rows in the circuit table back to the objects that define
    -- the circuits.

    ciIfMapTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF CiIfMapEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The Circuit Interface Map Table."
        ::= { ciObjects 2 }

    ciIfMapEntry OBJECT-TYPE
        SYNTAX      CiIfMapEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the Circuit Interface Map Table."
        INDEX    { ifIndex }
        ::= { ciIfMapTable 1 }

    CiIfMapEntry ::=
        SEQUENCE {
            --
            -- Mapped Object Variables
            --
            ciIfMapObject      RowPointer,
            ciIfMapFlow        CiFlowDirection
        }

    ciIfMapObject OBJECT-TYPE
        SYNTAX      RowPointer





        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This value contains the value of RowPointer that
             corresponds to the current ifIndex."
        ::= { ciIfMapEntry 1 }

    ciIfMapFlow   OBJECT-TYPE
        SYNTAX      CiFlowDirection
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The value contains the value of ciCircuitFlow that
             corresponds to the current ifIndex."
        ::= { ciIfMapEntry 2 }

    -- Change tracking metrics

    ciIfLastChange OBJECT-TYPE
        SYNTAX       TimeStamp
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The value of sysUpTime at the most recent change to
             ciCircuitStatus for any row in ciCircuitTable."
        ::= { ciObjects 3 }

    ciIfNumActive      OBJECT-TYPE
        SYNTAX         Gauge32
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
            "The number of active rows in ciCircuitTable."
        ::= { ciObjects 4 }

    -- Conformance Information

    ciMIBGroups      OBJECT IDENTIFIER ::= { ciConformance 1 }
    ciMIBCompliances OBJECT IDENTIFIER ::= { ciConformance 2 }

    --
    -- Compliance Statements
    --

    ciCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
            "The compliance statement for SNMP entities





             which support of the Circuit Interfaces MIB module.
             This group defines the minimum level of support
             required for compliance."
        MODULE -- this module
            MANDATORY-GROUPS { ciCircuitGroup,
                               ciIfMapGroup,
                               ciStatsGroup }

            OBJECT      ciCircuitStatus
            SYNTAX      INTEGER { active(1) } -- subset of RowStatus
            MIN-ACCESS  read-only
            DESCRIPTION
               "Row creation can be done outside of the scope of
                the SNMP protocol.  If this object is implemented with
                max-access of read-only, then the only value that MUST
                be returned is active(1)."

            OBJECT      ciCircuitStorageType
            MIN-ACCESS  read-only
            DESCRIPTION
               "It is legal to support ciCircuitStorageType as read-
                only as long as the value reported in consistent
                with the actual storage mechanism employed within the
                agent."

    ::= { ciMIBCompliances 1 }

    --
    -- Units of Conformance
    --
    ciCircuitGroup  OBJECT-GROUP
       OBJECTS {
            ciCircuitStatus,
            ciCircuitIfIndex,
            ciCircuitCreateTime,
            ciCircuitStorageType
       }
       STATUS  current
       DESCRIPTION
           "A collection of required objects providing
            information from the circuit table."
       ::= { ciMIBGroups 1 }

    ciIfMapGroup OBJECT-GROUP
       OBJECTS {
            ciIfMapObject,
            ciIfMapFlow
       }





       STATUS  current
       DESCRIPTION
           "A collection of required objects providing
            information from the interface map table."
       ::= { ciMIBGroups 2 }

    ciStatsGroup OBJECT-GROUP
       OBJECTS {
            ciIfLastChange,
            ciIfNumActive
       }
       STATUS  current
       DESCRIPTION
           "A collection of statistical metrics used to help manage
            the ciCircuitTable."
       ::= { ciMIBGroups 3 }
END


