
DEFINITIONS ::= BEGIN

-- object identifier definitions
sc6 OBJECT IDENTIFIER ::= {joint-iso-ccitt sc6(?)}
-- value to be assigned by SC21 secretariat
isisoi OBJECT IDENTIFIER ::= {sc6 iSO10589(?)}
-- value to be assigned by SC6 secretariat
moi OBJECT IDENTIFIER ::= {isisoi objectClass (3)}
poi OBJECT IDENTIFIER ::= {isisoi package (4)}
proi OBJECT IDENTIFIER ::= {isisoi parameter (5)}
nboi OBJECT IDENTIFIER ::= {isisoi nameBinding (6)}
aoi OBJECT IDENTIFIER ::= {isisoi attribute (7)}
agoi OBJECT IDENTIFIER ::= {isisoi attributeGroup 
(8)}
acoi OBJECT IDENTIFIER ::= {isisoi action (10)}
noi OBJECT IDENTIFIER ::= {isisoi notification (11)}
 
 
ActionFailureReason ::= ENUMERATED{
reason1(0),
reason2(1)}
-- Note: actual reasons TBS
ActionInfo ::= SET OF Parameter
ActionReply ::= SEQUENCE{
responseCode OBJECT IDENTIFIER,
responseArgs SET OF Parameter OPTIONAL}
AddressPrefix ::=  OCTETSTRING(SIZE(0..20))
AdjacencyState ::= ENUMERATED{
initializing(0),
up(1),
failed(2)}-- was 4 in N5821 , is it required at all?
AreaAddress ::=  OCTETSTRING(SIZE(1..20))
AreaAddresses ::= SET OF AreaAddress
Boolean ::= BOOLEAN
CircuitID ::=  OCTETSTRING(SIZE(1..10))
CompleteSNPInterval ::= INTEGER(1..600)
ConstraintViolationReason ::= OBJECT IDENTIFIER;
DRISISHelloTimer ::= INTEGER(1..65535)
DatabaseState ::= ENUMERATED{
off(0),
on(1),
waiting(2)}
DesignatedISChange ::= ENUMERATED{
resigned(0),
elected(1)}
DefaultESHelloTimer ::= INTEGER(1..65535)
EndSystemIDs ::= SET OF SystemID
GraphicString ::=  GRAPHICSTRING
HelloTimer ::= INTEGER(1..65535)
HoldingTimer ::= INTEGER(1..65535)
HopMetric ::= INTEGER(0..63)
ISISHelloTimer ::= INTEGER(1..65535)
IDLength ::= INTEGER(0..9)
IdleTimer ::= INTEGER(1..65535)
InitialMinimumTimer ::= INTEGER(1..65535)
IntermediateSystemPriority ::= INTEGER(1..127)
ISType ::= ENUMERATED{
level1IS(1),
level2IS(2)}
LANAddress ::=  OCTETSTRING(SIZE(6))
AdjacencyUsageType::= ENUMERATED{
undefined(0),
level1(1),
level2(2),
level1and2(3)}
LocalDistinguishedName ::= CMIP-1.ObjectInstance
-- A suitable free standing definition is requred
LSPID ::=  OCTETSTRING(SIZE(2..11))
MappingType ::= ENUMERATED{
manual(0),
x121(1)}
MaximumBuffers ::= INTEGER(1..65535)
MaximumCallAttempts ::= INTEGER(1..65535)
MaximumLSPGenerationInterval ::= INTEGER(1..65535)
MaximumPathSplits ::= INTEGER(1..32)
MaximumSVCAdjacencies ::= INTEGER(1..65535)
MaximumVirtualAdjacencies ::= INTEGER(0..32)
MetricIncrement ::= INTEGER(0..63)
MetricType ::= ENUMERATED{
internal(0),
external(1)}
MinimumBroadcastLSPTransmissionInterval ::= 
INTEGER(1..65535)
MinimumLSPGenerationInterval ::= INTEGER(1..65535)
MinimumLSPTransmissionInterval ::= 
 
INTEGER(1..65535)
NeighbourSystemType ::= ENUMERATED{
unknown(0),
endSystem(1),
intermediateSystem(2),
l1IntermediateSystem(3),
l2IntermediateSystem(4)}
NetworkEntityTitle ::=  OCTETSTRING(SIZE(1..19))
NewAdjacencyState ::= ENUMERATED{
down(0),
up(1)}
NewCircuitState ::= ENUMERATED{
off(0),
on(1)}
NonWrappingCounter ::= INTEGER(0..264-1)
NotificationInfo ::= SET OF Parameter
NSAPAddress ::=  OCTETSTRING(SIZE(1..20))
OctetString ::=  OCTETSTRING
OriginatingLSPBufferSize ::= INTEGER(512..1492)
OutputAdjacencies ::= SET OF LocalDistinguishedName
OverloadStateChange ::= ENUMERATED{
on(0),
waiting(1)}
Parameter ::= SEQUENCE{
paramIdOBJECT IDENTIFIER,
paramInfoANY DEFINED BY paramID}
PartialSNPInterval ::= INTEGER(1..65535)
Password ::=  OCTETSTRING(SIZE(0..254)
Passwords ::= SET OF Password
PathMetric ::= INTEGER(0..1023)
PDUHeader ::=  OCTETSTRING(SIZE(0..255))
PollESHelloRate ::= INTEGER(1..65535)
Reason ::= ENUMERATED{
holdingTimerExpired(0),
checksumError(1),
oneWayConnectivity(2),
callRejected(3),
reserveTimerExpired(4),
circuitDisabled(5),
versionSkew(6),
areaMismatch(7),
maximumBroadcastIntermediateSystemsExceeded(8),
maximumBroadcastEndSystemsExceeded(9),
wrongSystemType(10)}
ResponseCode ::= OBJECT IDENTIFIER
RecallTimer ::= INTEGER(1..65535)
ReserveTimer ::= INTEGER(1..65535)
SNPAAddress ::=  
NUMERICSTRING(FROM("0"|"1"|"2"|"3"|"4"|"5"|
"6"|"7"|"8"|"9"))(SIZE(0..15))
-- Up to 15 Digits 0..9
SNPAAddresses ::= SET OF SNPAAddress
CircuitType ::= ENUMERATED{
broadcast(0),
ptToPt(1),
staticIN(2),
staticOut(3),
dA(4)}
SourceID ::=  OCTETSTRING(SIZE(1..10))
SystemID ::=  OCTETSTRING(SIZE(0..9))
VirtualLinkChange ::= ENUMERATED{
deleted(0),
created(1)}
Version ::=  GRAPHICSTRING
WaitingTime ::= INTEGER(1..65535)
maximumPathSplits-Default INTEGER ::= 2
MaximumPathSplits-Permitted ::= INTEGER(1..32)
 
maximumBuffers-Default INTEGER ::= ImpSpecific
MaximumBuffers-Permitted ::= INTEGER(1..ImpSpecific)
minimumLSPTransmissionInterval-Default INTEGER ::= 
5
MinimumLSPTransmissionInterval-Permitted ::= 
INTEGER(5..30)
maximumLSPGenerationInterval-Default INTEGER ::= 
900
MaximumLSPGenerationInterval-Permitted ::= 
INTEGER(60..900)
minimumBroadcastLSPTransmissionInterval-Default 
INTEGER ::=33
MinimumBroadcastLSPTransmissionInterval-Permitted ::= 
INTEGER(1..65535)
completeSNPInterval-Default INTEGER ::= 10
CompleteSNPInterval-Permitted ::= INTEGER(1..600)
originatingL1LSPBufferSize-Default INTEGER ::= 
receiveLSPBufferSize
OriginatingL1LSPBufferSize-Permitted ::= 
INTEGER(512..receiveLSPBufferSize)
manualAreaAddresses-Default AreaAddresses ::= {}
ManualAreaAddresses-Permitted ::= AreaAddresses 
(SIZE(0..MaximumAreaAddresses))
minimumLSPGenerationInterval-Default INTEGER ::= 30
MinimumLSPGenerationInterval-Permitted ::= 
INTEGER(5..300)
defaultESHelloTime-Default INTEGER ::= 600
DefaultESHelloTime-Permitted ::= INTEGER(1..65535)
pollESHelloRate-Default INTEGER ::= 50
PollESHelloRate-Permitted ::= INTEGER(1..65535)
partialSNPInterval-Default INTEGER ::= 2
PartialSNPInterval-Permitted ::= INTEGER(1..65535)
waitingTime-Default INTEGER ::= 60
WaitingTime-Permitted ::= INTEGER(1..65535)
dRISISHelloTimer-Default INTEGER ::= 1
DRISISHelloTimer-Permitted ::=  INTEGER(1..65535)
originatingL2LSPBufferSize-Default INTEGER ::= 
receiveLSPBufferSize
OriginatingL2LSPBufferSize-Permitted ::= 
INTEGER(512..receiveLSPBufferSize)
maximumVirtualAdjacencies-Default INTEGER ::= 2
MaximumVirtualAdjacencies-Permitted ::= 
INTEGER(0..32)
helloTimer-Default INTEGER ::= 10
HelloTimer-Permitted ::= INTEGER(1..21845)
defaultMetric-Default INTEGER ::= 20
DefaultMetric-Permitted ::= INTEGER(1..MaxLinkMetric)
optionalMetric-Default INTEGER ::= 0
OptionalMetric-Permitted ::= 
INTEGER(0..MaxLinkMetric)
metricType-Default MetricType ::= Internal
iSISHelloTimer-Default INTEGER ::= 3
ISISHelloTimer-Permitted ::= INTEGER(1..21845)
externalDomain-Default BOOLEAN ::= TRUE
l1IntermediateSystemPriority-Default INTEGER ::= 64
L1IntermediateSystemPriority-Permitted ::= 
INTEGER(1..127)
callEstablishmentMetricIncrement-Default INTEGER ::= 0
CallEstablishmentMetricIncrement-Permitted ::= 
INTEGER(0..MaxLinkMetric)
idleTimer-Default INTEGER ::= 30
IdleTimer-Permitted ::= INTEGER(0..65535)
initialMinimumTimer-Default INTEGER ::= 55
InitialMinimumTimer-Permitted ::= INTEGER(1..65535)
reserveTimer-Default INTEGER ::= 600
ReserveTimer-Permitted ::= INTEGER(1..65535)
maximumSVCAdjacencies-Default INTEGER ::= 1
 
MaximumSVCAdjacencies-Permitted ::= 
INTEGER(1..65535)
reservedAdjacency-Default BOOLEAN ::= FALSE
neighbourSNPAAddress-Default INTEGER ::= 0
recallTimer-Default INTEGER ::= 60
RecallTimer-Permitted ::= INTEGER(0..65535)
maximumCallAttempts-Default INTEGER ::= 10
MaximumCallAttempts-Permitted ::= INTEGER(0..255)
manualL2OnlyMode-Default BOOLEAN ::= FALSE
l2IntermediateSystemPriority-Default INTEGER ::= 64
L2IntermediateSystemPriority-Permitted ::= 
INTEGER(1..127)
lANAddress-Default LANAddress ::= 000000000000
sNPAAddresses-Default SNPAAddresses::= {}
password-Default Password ::= {}
passwords-Default Passwords ::= {} -- The empty set
END


