COFFEE-POT-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
       TimeStamp, TimeInterval,
       Counter32, Integer32
           FROM SNMPv2-SMI
       InterfaceIndex
           FROM IF-MIB
       transmission
           FROM RFC1213-MIB
       MODULE-COMPLIANCE, OBJECT-GROUP
           FROM SNMPv2-CONF;

   coffee MODULE-IDENTITY
        LAST-UPDATED "9803231700Z"
        ORGANIZATION "Networked Appliance Management Working Group"

        CONTACT-INFO
               "        Michael Slavitch
                        Loran Technologies,
                        955 Green Valley Crescent
                        Ottawa, Ontario Canada K2A 0B6

                   Tel: 613-723-7505
                   Fax: 613-723-7209
                E-mail: slavitch@loran.com"
        DESCRIPTION
               "The MIB Module for coffee vending devices."
       ::= { transmission 132 }

   potName OBJECT-TYPE
        SYNTAX     DisplayString (SIZE (0..255))
        MAX-ACCESS read-only





        STATUS current
        DESCRIPTION
                "The vendor description of the pot under management"
        ::= { coffee 1 }


   potCapacity OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
           "The number of units of beverage supported by this device
            (regardless of its current state) ."
       ::= { coffee 2 }


   potType OBJECT-TYPE
        SYNTAX     INTEGER {
           automatic-drip(1),
           percolator(2),
           french-press(3),
           espresso(4),
           }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "The brew type of the coffee pot."
        ::= { coffee 3 }

   potLocation OBJECT-TYPE {
        SYNTAX     DisplayString (SIZE (0..255))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "The physical location of the pot in question"
        ::= { coffee 4 }


   potMonitor            OBJECT IDENTIFIER ::= { coffee 6 }


   potOperStatus
        SYNTAX     Integer {
                        off(1),
                        brewing(2),
                        holding(3),
                        other(4),
                        waiting(5)





                        }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "The operating status of the pot in question. Note
                 that this is a read-only feature. Current hardware
                 prevents us from changing the port state via SNMP."
        ::= { potMonitor 1 }

    potLevel OBJECT-TYPE
        SYNTAX     Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "The number of units of coffee under management. The
                 units of level are defined in potMetric below."
        ::= { potMonitor 2 }

    potMetric  OBJECT-TYPE
        SYNTAX     Integer {
                    espresso(1),
                    demi-tasse(2),
                    cup(3),
                    mug(4),
                    bucket(5)
                    }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "The vendor description of the pot under management"
        ::= { potMonitor 3 }


   potStartTime OBJECT-TYPE
       SYNTAX     Integer64
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "The time in seconds since Jan 1 1970 to start the pot
                if and only if potOperStatus is waiting(5)"
       ::= { potMonitor 4 }


    lastStartTime OBJECT-TYPE
       SYNTAX     TimeInterval
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION





               "The amount of time, in TimeTicks, since the coffee
               making process was initiated."
       ::= { potMonitor 5 }


    potTemperature OBJECT-TYPE
       SYNTAX     Integer32
       UNITS      "degrees Centigrade"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "The ambient temperature of the coffee within the pot"

      ::= { potMonitor 6 }

   END


