FRSLD-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Counter32, Gauge32, Integer32,
    Counter64, TimeTicks, mib-2             FROM SNMPv2-SMI
    CounterBasedGauge64                     FROM HCNUM-TC
    TEXTUAL-CONVENTION, RowStatus,
    TimeStamp                               FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP         FROM SNMPv2-CONF
    ifIndex                                 FROM IF-MIB
    DLCI                                    FROM FRAME-RELAY-DTE-MIB;

    frsldMIB MODULE-IDENTITY
        LAST-UPDATED "200201030000Z" -- January 3, 2002
        ORGANIZATION "IETF Frame Relay Service MIB Working Group"
        CONTACT-INFO
          "IETF Frame Relay Service MIB (frnetmib) Working Group

           WG Charter:    http://www.ietf.org/html.charters/
                                 frnetmib-charter.html
           WG-email:      frnetmib@sunroof.eng.sun.com
           Subscribe:     frnetmib-request@sunroof.eng.sun.com
           Email Archive: ftp://ftp.ietf.org/ietf-mail-archive/frnetmib





           Chair:      Andy Malis
                       Vivace Networks
           Email:      Andy.Malis@vivacenetworks.com

           WG editor:  Robert Steinberger
                       Paradyne Networks and
                       Fujitsu Network Communications
           Email:      robert.steinberger@fnc.fujitsu.com

           Co-author:  Orly Nicklass
                       RAD Data Communications Ltd.
           EMail:      Orly_n@rad.co.il"
        DESCRIPTION
            "The MIB module to describe generic objects for
             FRF.13 Frame Relay Service Level Definitions."
        REVISION "200201030000Z" -- January 3, 2002
        DESCRIPTION
            "Initial version, published as RFC 3202"
        ::= { mib-2 95 }

    --
    -- Textual Conventions
    --
    FrsldTxRP ::= TEXTUAL-CONVENTION
        STATUS  current
        DESCRIPTION
            "The reference point a PVC uses for calculation
             of transmitter related statistics.

             The valid values for this type of object are as follows:
               - srcLocalRP(1) for the local source
               - ingTxLocalRP(2) for the local ingress queue input
               - tpTxLocalRP(3) for the local traffic policing
               - eqiTxLocalRP(4) for the local egress queue input
               - eqoTxLocalRP(5) for the local egress queue output
               - otherTxLocalRP(6) for any other local transmit point
               - srcRemoteRP(7) for the remote source
               - ingTxLocalRP(8) for the remote ingress queue input
               - tpTxLocalRP(9) for the remote traffic policing
               - eqiTxRemoteRP(10) for the remote egress queue input
               - eqoTxRemoteRP(11) for the remote egress queue output
               - otherTxRemoteRP(12) for any other remote xmit point"
        REFERENCE
            "FRF.13: Section 2.3"
        SYNTAX      INTEGER {
                      srcLocalRP(1),
                      ingTxLocalRP(2),
                      tpTxLocalRP(3),





                      eqiTxLocalRP(4),
                      eqoTxLocalRP(5),
                      otherTxLocalRP(6),
                      srcRemoteRP(7),
                      ingTxRemoteRP(8),
                      tpTxRemoteRP(9),
                      eqiTxRemoteRP(10),
                      eqoTxRemoteRP(11),
                      otherTxRemoteRP(12)
                    }

    FrsldRxRP ::= TEXTUAL-CONVENTION
        STATUS      current
        DESCRIPTION
            "The reference point a PVC uses for calculation
             of receiver related statistics.

             The valid values for this object are as follows:
               - desLocalRP(1) for the local destination
               - ingRxLocalRP(2) for the local ingress queue input
               - tpRxLocalRP(3) for the local traffic policing
               - eqiRxLocalRP(4) for the local egress queue input
               - eqoRxLocalRP(5) for the local egress queue output
               - otherRxLocalRP(6) for any other local receive point
               - desRemoteRP(7) for the remote destination
               - ingRxRemoteRP(8) for the remote ingress input
               - tpRxRemoteRP(9) for the remote traffic policing
               - eqiRxRemoteRP(10) for the remote egress queue input
               - eqoRxRemoteRP(11) for the remote egress queue output
               - otherRxRemoteRP(12) for any other remote receive point"
        REFERENCE
            "FRF.13: Section 2.3"
        SYNTAX      INTEGER {
                      desLocalRP(1),
                      ingRxLocalRP(2),
                      tpRxLocalRP(3),
                      eqiRxLocalRP(4),
                      eqoRxLocalRP(5),
                      otherRxLocalRP(6),
                      desRemoteRP(7),
                      ingRxRemoteRP(8),
                      tpRxRemoteRP(9),
                      eqiRxRemoteRP(10),
                      eqoRxRemoteRP(11),
                      otherRxRemoteRP(12)
                    }

    --





    -- Base Objects
    ---

    frsldObjects      OBJECT IDENTIFIER ::= { frsldMIB 1 }
    frsldCapabilities OBJECT IDENTIFIER ::= { frsldMIB 2 }
    frsldConformance  OBJECT IDENTIFIER ::= { frsldMIB 3 }

    -- The Frame Relay Service Level Definitions PVC Control Table
    --
    -- This table is used to define and display the parameters of
    -- service level definitions on individual PVCs.

    frsldPvcCtrlTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF FrsldPvcCtrlEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The Frame Relay Service Level Definitions
             PVC control table."
        ::= { frsldObjects 1 }

    frsldPvcCtrlEntry OBJECT-TYPE
        SYNTAX      FrsldPvcCtrlEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the Frame Relay Service Level
             Definitions PVC control table."
        INDEX    { ifIndex, frsldPvcCtrlDlci,
                   frsldPvcCtrlTransmitRP, frsldPvcCtrlReceiveRP}
        ::= { frsldPvcCtrlTable 1 }

    FrsldPvcCtrlEntry ::=
        SEQUENCE {
            --
            -- Index Control Variables
            --
            frsldPvcCtrlDlci                DLCI,
            frsldPvcCtrlTransmitRP          FrsldTxRP,
            frsldPvcCtrlReceiveRP           FrsldRxRP,
            frsldPvcCtrlStatus              RowStatus,
            --
            -- Service Level Definitions Setup Variables
            --
            frsldPvcCtrlPacketFreq          Integer32,
            --
            -- Delay Specific Setup Variables
            --





            frsldPvcCtrlDelayFrSize         Integer32,
            frsldPvcCtrlDelayType           INTEGER,
            frsldPvcCtrlDelayTimeOut        Integer32,
            --
            -- Data Persistence Control Variables
            --
            frsldPvcCtrlPurge               Integer32,
            frsldPvcCtrlDeleteOnPurge       INTEGER,
            frsldPvcCtrlLastPurgeTime       TimeStamp
        }

    frsldPvcCtrlDlci OBJECT-TYPE
        SYNTAX      DLCI
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The value of this object is equal to the DLCI
             value for this PVC."
        ::= { frsldPvcCtrlEntry 1 }

    frsldPvcCtrlTransmitRP OBJECT-TYPE
        SYNTAX      FrsldTxRP
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The reference point this PVC uses for calculation
             of transmitter related statistics.  This object
             together with frsldPvcCtrlReceiveRP define the
             measurement domain."
        REFERENCE
            "FRF.13: Section 2.3"
        ::= { frsldPvcCtrlEntry 2 }

    frsldPvcCtrlReceiveRP OBJECT-TYPE
        SYNTAX      FrsldRxRP
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The reference point this PVC uses for calculation
             of receiver related statistics.  This object
             together with frsldPvcCtrlTransmitRP define the
             measurement domain."
        ::= { frsldPvcCtrlEntry 3 }

    frsldPvcCtrlStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current





        DESCRIPTION
            "The status of the current row.  This object is
             used to add, delete, and disable rows in this
             table.  When the status changes to active(1) for the
             first time, a row will also be added to the data
             table below.  This row SHOULD not be removed until
             the status is changed to deleted.

             When this object is set to destroy(6), all associated
             sample and data table rows will also be deleted.
             When this object is changed from active(1) to any
             other valid value, the defined purge behavior will
             affect the data and sample tables.

             The rows added to this table MUST have a valid
             ifIndex and an ifType related to frame relay.  Further,
             the reference points referred to by frsldPvcCtrlTransmitRP
             and frsldPvcCtrlReceiveRP MUST be supported (see the
             frsldRPCaps object).

             If at any point the row is not in the active(1) state
             and the DLCI no longer exists, the state SHOULD
             report notReady(3).

             The data in this table SHOULD persist through power
             cycles.  The symantics of readiness for the rows still
             applies.  This means that it is possible for a row to be
             reprovisioned as notReady(3) if the underlying DLCI does
             not persist."
        ::= { frsldPvcCtrlEntry 4 }

    frsldPvcCtrlPacketFreq OBJECT-TYPE
        SYNTAX      Integer32 (0..3600)
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The frequency in seconds between initiation of
             specialized packets used to collect delay and / or
             delivery information as supported by the device.
             A value of zero indicates that no packets will
             be sent."
        DEFVAL { 60 }
        ::= { frsldPvcCtrlEntry 5 }

    frsldPvcCtrlDelayFrSize OBJECT-TYPE
        SYNTAX      Integer32 (1..8188)
        UNITS       "octets"





        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The size of the payload in the frame used for
             calculation of network delay."
        DEFVAL { 128 }
        ::= { frsldPvcCtrlEntry 6 }

    frsldPvcCtrlDelayType OBJECT-TYPE
        SYNTAX      INTEGER {
                      oneWay(1),
                      roundTrip(2)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
                "The type of delay measurement performed."
        REFERENCE
            "FRF.13: Section 3"
        ::= { frsldPvcCtrlEntry 7 }

    frsldPvcCtrlDelayTimeOut OBJECT-TYPE
        SYNTAX      Integer32 (1..3600)
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "A delay frame will count as a missed poll if
             it is not updated in the time specified by
             frsldPvcCtrlDelayTimeOut."
        DEFVAL { 60 }
        ::= { frsldPvcCtrlEntry 8 }

    frsldPvcCtrlPurge OBJECT-TYPE
        SYNTAX      Integer32 (0..172800) -- up to 48 hours
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "This object defines the amount of time the device
             will wait, after discovering that a DLCI does not exist,
             the DLCI was deleted or the value of frsldPvcCtrlStatus
             changes from active(1) to either notInService(2) or
             notReady(3), prior to automatically purging the history
             in the sample tables and resetting the data in the data
             tables to all zeroes.  If frsldPvcCtrlStatus is manually
             set to destroy(6), this object does not apply."
        DEFVAL { 0 }





        ::= { frsldPvcCtrlEntry 9 }

    frsldPvcCtrlDeleteOnPurge OBJECT-TYPE
        SYNTAX      INTEGER {
                      none(1),
                      sampleContols(2),
                      all(3)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "This object defines whether rows will
             automatically be deleted from the tables
             when the information is purged.

             - A value of none(1) indicates that no rows
               will deleted.  The last known values will
               be preserved.
             - A value of sampleControls(2) indicates
               that all associated sample control rows
               will be deleted.
             - A value of all(3) indicates that all
               associated rows SHOULD be deleted."
        DEFVAL { all }
        ::= { frsldPvcCtrlEntry 10 }

    frsldPvcCtrlLastPurgeTime OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This object returns the value of sysUpTime
             at the time the information was last purged.
             This value SHOULD be set to the sysUpTime
             upon setting frsldPvcCtrlStatus to active(1)
             for the first time.  Each time a
             discontinuity in the counters occurs, this
             value MUST be set to the sysUpTime.

             If frsldPvcCtrlStatus has never been active(1),
             this object SHOULD return 0.

             This object SHOULD be used as the discontinuity
             timer for the counters in frsldPvcDataTable."
        ::= { frsldPvcCtrlEntry 11 }

    -- The Frame Relay Service Level Definitions Sampling Control
    -- Table





    --
    -- This table is used to define the sample control parameters
    -- of service level definitions on individual PVCs.

    frsldSmplCtrlTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF FrsldSmplCtrlEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The Frame Relay Service Level Definitions
             sampling control table."
        ::= { frsldObjects 2 }

    frsldSmplCtrlEntry OBJECT-TYPE
        SYNTAX      FrsldSmplCtrlEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the Frame Relay Service Level
             Definitions sample control table."
        INDEX    { ifIndex, frsldPvcCtrlDlci,
                   frsldPvcCtrlTransmitRP, frsldPvcCtrlReceiveRP,
                   frsldSmplCtrlIdx }
        ::= { frsldSmplCtrlTable 1 }

    FrsldSmplCtrlEntry ::=
        SEQUENCE {
            --
            -- Index Control Variables
            --
            frsldSmplCtrlIdx                Integer32,
            frsldSmplCtrlStatus             RowStatus,
            --
            -- Collection Control Variables
            --
            frsldSmplCtrlColPeriod          Integer32,
            frsldSmplCtrlBuckets            Integer32,
            frsldSmplCtrlBucketsGranted     Integer32
        }

    frsldSmplCtrlIdx OBJECT-TYPE
        SYNTAX  Integer32 (1..256)
        MAX-ACCESS not-accessible
        STATUS  current
        DESCRIPTION
            "The unique index for this row in the
             sample control table."
        ::= { frsldSmplCtrlEntry 1 }





    frsldSmplCtrlStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The status of the current row.  This object is
             used to add, delete, and disable rows in this
             table.  This row SHOULD NOT be removed until the
             status is changed to destroy(6).  When the status
             changes to active(1), the collection in the sample
             tables below will be activated.

             The rows added to this table MUST have a valid
             ifIndex, an ifType related to frame relay,
             frsldPvcCtrlDlci MUST exist for the specified
             ifIndex and frsldPvcCtrlStatus MUST have a
             value of active(1).

             The value of frsldPvcCtrlStatus MUST be active(1)
             to transition this object to active(1).  If
             the value of frsldPvcCtrlStatus becomes anything
             other than active(1) when the state of this object
             is not active(1), this object SHOULD be set to
             notReady(3).

             The data in this table SHOULD persist through power
             cycles.  The symantics of readiness for the rows still
             applies.  This means that it is possible for a row to be
             reprovisioned as notReady(3) if the underlying DLCI does
             not persist."
        ::= { frsldSmplCtrlEntry 2 }

    frsldSmplCtrlColPeriod OBJECT-TYPE
        SYNTAX      Integer32 (1..2147483647)
        UNITS       "seconds"
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The amount of time in seconds that defines a
             period of collection for the statistics.
             At the end of each period, the statistics will be
             sampled and a row is added to the sample table."
        ::= { frsldSmplCtrlEntry 3 }

    frsldSmplCtrlBuckets OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-create
        STATUS      current





        DESCRIPTION
            "The number of discrete buckets over which the
             data statistics are sampled.

             When this object is created or modified, the device
             SHOULD attempt to set the frsldSmplCtrlBuckets-
             Granted to a value as close as is possible
             depending upon the implementation and the available
             resources."
        DEFVAL { 60 }
        ::= { frsldSmplCtrlEntry 4 }

    frsldSmplCtrlBucketsGranted OBJECT-TYPE
        SYNTAX      Integer32 (0..65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of discrete buckets granted.  This
             object will return 0 until frsldSmplCtrlStatus is
             set to active(1).  At that time the buckets will be
             allocated depending upon implementation and
             available resources."
        ::= { frsldSmplCtrlEntry 5 }

    -- The Frame Relay Service Level Definitions PVC Data Table
    --
    -- This table contains the accumulated values of
    -- the collected data.  This table is the table that should
    -- be referenced by external polling mechanisms if time
    -- based polling be desired.

     frsldPvcDataTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF FrsldPvcDataEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The Frame Relay Service Level Definitions
             data table.

             This table contains accumulated values of the
             collected data.  It is the table that should be
             referenced by external polling mechanisms if
             time based polling be desired."
        ::= { frsldObjects 3 }

    frsldPvcDataEntry OBJECT-TYPE
        SYNTAX      FrsldPvcDataEntry
        MAX-ACCESS  not-accessible





        STATUS      current
        DESCRIPTION
            "An entry in the Frame Relay Service Level
             Definitions data table."
        INDEX    { ifIndex, frsldPvcCtrlDlci,
                  frsldPvcCtrlTransmitRP, frsldPvcCtrlReceiveRP}
        ::= { frsldPvcDataTable 1 }

    FrsldPvcDataEntry ::=
        SEQUENCE {
            frsldPvcDataMissedPolls       Counter32,
            frsldPvcDataFrDeliveredC      Counter32,
            frsldPvcDataFrDeliveredE      Counter32,
            frsldPvcDataFrOfferedC        Counter32,
            frsldPvcDataFrOfferedE        Counter32,
            frsldPvcDataDataDeliveredC    Counter32,
            frsldPvcDataDataDeliveredE    Counter32,
            frsldPvcDataDataOfferedC      Counter32,
            frsldPvcDataDataOfferedE      Counter32,
            frsldPvcDataHCFrDeliveredC    Counter64,
            frsldPvcDataHCFrDeliveredE    Counter64,
            frsldPvcDataHCFrOfferedC      Counter64,
            frsldPvcDataHCFrOfferedE      Counter64,
            frsldPvcDataHCDataDeliveredC  Counter64,
            frsldPvcDataHCDataDeliveredE  Counter64,
            frsldPvcDataHCDataOfferedC    Counter64,
            frsldPvcDataHCDataOfferedE    Counter64,
            frsldPvcDataUnavailableTime   TimeTicks,
            frsldPvcDataUnavailables      Counter32
        }

    frsldPvcDataMissedPolls OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of polls that have been determined
             to be missed.  These polls are typically associated
             with the calculation of delay but may also be
             used for the calculation of other statistics.  If an
             anticipated poll is not received in a reasonable
             amount of time, it should be counted as missed.
             The value used to determine the reasonable amount
             of time is contained in frsldPvcCtrlDelayTimeOut.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by





             frsldPvcCtrlLastPurgeTime."
        ::= { frsldPvcDataEntry 1 }

    frsldPvcDataFrDeliveredC OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent within CIR.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 4.1 (FramesDeliveredc)"
        ::= { frsldPvcDataEntry 2 }

    frsldPvcDataFrDeliveredE OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent in excess of the CIR.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 4.1 (FramesDeliverede)"
        ::= { frsldPvcDataEntry 3 }

    frsldPvcDataFrOfferedC OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were offered through
             frsldPvcCtrlTransmitRP within CIR.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by





             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 4.1 (FramesOfferedc)"
        ::= { frsldPvcDataEntry 4 }

    frsldPvcDataFrOfferedE OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were offered through
             frsldPvcCtrlTransmitRP in excess of the CIR.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 4.1 (FramesOfferede)"
        ::= { frsldPvcDataEntry 5 }

    frsldPvcDataDataDeliveredC OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent within CIR.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 5.1 (DataDeliveredc)"
        ::= { frsldPvcDataEntry 6 }

    frsldPvcDataDataDeliveredE OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent in excess of the CIR.

             Discontinuities in the value of this counter can





             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 5.1 (DataDeliverede)"
        ::= { frsldPvcDataEntry 7 }

    frsldPvcDataDataOfferedC OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were offered through
             frsldPvcCtrlTransmitRP within CIR.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 5.1 (DataOfferedc)"
        ::= { frsldPvcDataEntry 8 }

    frsldPvcDataDataOfferedE OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were offered through
             frsldPvcCtrlTransmitRP in excess of the CIR.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 5.1 (DataOfferede)"
        ::= { frsldPvcDataEntry 9 }

    frsldPvcDataHCFrDeliveredC OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent within CIR.  This object is a 64-bit version
             of frsldPvcDataFrDeliveredC.





             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 4.1 (FramesDeliveredc)"
        ::= { frsldPvcDataEntry 10 }

    frsldPvcDataHCFrDeliveredE OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent in excess of the CIR.  This object is a 64-bit
             version of frsldPvcDataFrDeliveredE.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 4.1 (FramesDeliverede)"
        ::= { frsldPvcDataEntry 11 }

    frsldPvcDataHCFrOfferedC OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were offered through
             frsldPvcCtrlTransmitRP within CIR.  This object is
             a 64-bit version of frsldPvcDataFrOfferedC.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 4.1 (FramesOfferedc)"
        ::= { frsldPvcDataEntry 12 }

    frsldPvcDataHCFrOfferedE OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION





            "The number of frames that were offered through
             frsldPvcCtrlTransmitRP in excess of the CIR.  This
             object is a 64-bit version of frsldPvcDataFrOfferedE.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 4.1 (FramesOfferede)"
        ::= { frsldPvcDataEntry 13 }

    frsldPvcDataHCDataDeliveredC OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent within CIR.  This object is a 64-bit version of
             frsldPvcDataDataDeliveredC.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 5.1 (DataDeliveredc)"
        ::= { frsldPvcDataEntry 14 }

    frsldPvcDataHCDataDeliveredE OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent in excess of the CIR.  This object is a 64-bit
             version of frsldPvcDataDataDeliveredE.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 5.1 (DataDeliverede)"
        ::= { frsldPvcDataEntry 15 }






    frsldPvcDataHCDataOfferedC OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were offered through
             frsldPvcCtrlTransmitRP within CIR.  This object is
             a 64-bit version of frsldPvcDataDataOfferedC.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 5.1 (DataOfferedc)"
        ::= { frsldPvcDataEntry 16 }

    frsldPvcDataHCDataOfferedE OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were offered through
             frsldPvcCtrlTransmitRP in excess of the CIR.
             This object is a 64-bit version of
             frsldPvcDataDataOfferedE.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 5.1 (DataOfferede)"
        ::= { frsldPvcDataEntry 17 }

    frsldPvcDataUnavailableTime OBJECT-TYPE
        SYNTAX      TimeTicks
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of time this PVC was declared unavailable
             for any reason since this row was created."
        REFERENCE
            "FRF.13: Section 6.1 (OutageTime)"
        ::= { frsldPvcDataEntry 18 }

    frsldPvcDataUnavailables OBJECT-TYPE
        SYNTAX      Counter32





        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of times this PVC was declared unavailable
             for any reason since this row was created.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system
             and at other times as indicated by
             frsldPvcCtrlLastPurgeTime."
        REFERENCE
            "FRF.13: Section 6.1 (OutageCount)"
        ::= { frsldPvcDataEntry 19 }

    -- The Frame Relay Service Level Definitions PVC Sample Table
    --
    -- This table contains the sampled delay, delivery and
    -- availability information.

    frsldPvcSampleTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF FrsldPvcSampleEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The Frame Relay Service Level Definitions
             sample table."
        ::= { frsldObjects 4 }

    frsldPvcSampleEntry OBJECT-TYPE
        SYNTAX      FrsldPvcSampleEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the Frame Relay Service Level
             Definitions data sample table."
        INDEX    { ifIndex, frsldPvcCtrlDlci,
                   frsldPvcCtrlTransmitRP, frsldPvcCtrlReceiveRP,
                   frsldSmplCtrlIdx, frsldPvcSmplIdx }
        ::= { frsldPvcSampleTable 1 }

    FrsldPvcSampleEntry ::=
        SEQUENCE {
            frsldPvcSmplIdx              Integer32,
            frsldPvcSmplDelayMin         Gauge32,
            frsldPvcSmplDelayMax         Gauge32,
            frsldPvcSmplDelayAvg         Gauge32,
            frsldPvcSmplMissedPolls      Gauge32,
            frsldPvcSmplFrDeliveredC     Gauge32,





            frsldPvcSmplFrDeliveredE     Gauge32,
            frsldPvcSmplFrOfferedC       Gauge32,
            frsldPvcSmplFrOfferedE       Gauge32,
            frsldPvcSmplDataDeliveredC   Gauge32,
            frsldPvcSmplDataDeliveredE   Gauge32,
            frsldPvcSmplDataOfferedC     Gauge32,
            frsldPvcSmplDataOfferedE     Gauge32,
            frsldPvcSmplHCFrDeliveredC   CounterBasedGauge64,
            frsldPvcSmplHCFrDeliveredE   CounterBasedGauge64,
            frsldPvcSmplHCFrOfferedC     CounterBasedGauge64,
            frsldPvcSmplHCFrOfferedE     CounterBasedGauge64,
            frsldPvcSmplHCDataDeliveredC CounterBasedGauge64,
            frsldPvcSmplHCDataDeliveredE CounterBasedGauge64,
            frsldPvcSmplHCDataOfferedC   CounterBasedGauge64,
            frsldPvcSmplHCDataOfferedE   CounterBasedGauge64,
            frsldPvcSmplUnavailableTime  TimeTicks,
            frsldPvcSmplUnavailables     Gauge32,
            frsldPvcSmplStartTime        TimeStamp,
            frsldPvcSmplEndTime          TimeStamp
        }

    frsldPvcSmplIdx OBJECT-TYPE
        SYNTAX      Integer32 (1..2147483647)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The bucket index of the current sample.  This
             increments once for each new bucket in the
             table."
        ::= { frsldPvcSampleEntry 1 }

    frsldPvcSmplDelayMin OBJECT-TYPE
        SYNTAX      Gauge32
        UNITS       "microseconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The minimum delay reported in microseconds measured
             for any information packet that arrived during this
             interval.

             A value of zero means that no data is available."
        REFERENCE
            "FRF.13: Section 3.1 (FTD)"
        ::= { frsldPvcSampleEntry 2 }

    frsldPvcSmplDelayMax OBJECT-TYPE
        SYNTAX      Gauge32





        UNITS       "microseconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The largest delay reported in microseconds measured
             for any information packet that arrived during this
             interval.

             A value of zero means that no data is available."
        REFERENCE
            "FRF.13: Section 3.1 (FTD)"
        ::= { frsldPvcSampleEntry 3 }

    frsldPvcSmplDelayAvg OBJECT-TYPE
        SYNTAX      Gauge32
        UNITS       "microseconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The average delay reported in microseconds measured
             for all delay packets that arrived during this
             interval.

             A value of zero means that no data is available."
        REFERENCE
            "FRF.13: Section 3.1 (FTD)"
        ::= { frsldPvcSampleEntry 4 }

    frsldPvcSmplMissedPolls OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of polls that were missed during
             this interval."
        ::= { frsldPvcSampleEntry 5 }

    frsldPvcSmplFrDeliveredC OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent within CIR during this interval.

             If it is the case that the high capacity counters
             are also used, this MUST report the value of the





             lower 32 bits of the CounterBasedGauge64 value of
             frsldPvcSmplHCFrDeliveredC."
        REFERENCE
            "FRF.13: Section 4.1 (FramesDeliveredc)"
        ::= { frsldPvcSampleEntry 6 }

    frsldPvcSmplFrDeliveredE OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent in excess of the CIR during this interval.

             If it is the case that the high capacity counters
             are also used, this MUST report the value of the
             lower 32 bits of the CounterBasedGauge64 value of
             frsldPvcSmplHCFrDeliveredE."
        REFERENCE
            "FRF.13: Section 4.1 (FramesDeliverede))"
        ::= { frsldPvcSampleEntry 7 }

    frsldPvcSmplFrOfferedC OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were offered through
             frsldPvcCtrlTransmitRP within CIR during this
             interval.

             If it is the case that the high capacity counters
             are also used, this MUST report the value of the
             lower 32 bits of the CounterBasedGauge64 value of
             frsldPvcSmplHCFrOfferedC."
        REFERENCE
            "FRF.13: Section 4.1 (FramesOfferedc)"
        ::= { frsldPvcSampleEntry 8 }

    frsldPvcSmplFrOfferedE OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were offered through
             frsldPvcCtrlTransmitRP in excess of the CIR
             during this interval.





             If it is the case that the high capacity counters
             are also used, this MUST report the value of the
             lower 32 bits of the CounterBasedGauge64 value of
             frsldPvcSmplHCFrOfferedE."
        REFERENCE
            "FRF.13: Section 4.1 (FramesOfferede)"
        ::= { frsldPvcSampleEntry 9 }

    frsldPvcSmplDataDeliveredC OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent within CIR during this interval.

             If it is the case that the high capacity counters
             are also used, this MUST report the value of the
             lower 32 bits of the CounterBasedGauge64 value of
             frsldPvcSmplHCDataDeliveredC."
        REFERENCE
            "FRF.13: Section 5.1 (DataDeliveredc)"
        ::= { frsldPvcSampleEntry 10 }

    frsldPvcSmplDataDeliveredE OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were received at
             frsldPvcCtrlDeliveredRP and determined to have been
             sent in excess of the CIR during this interval.

             If it is the case that the high capacity counters
             are also used, this MUST report the value of the
             lower 32 bits of the CounterBasedGauge64 value of
             frsldPvcSmplHCDataDeliveredE."
        REFERENCE
            "FRF.13: Section 5.1 (DataDeliverede)"
        ::= { frsldPvcSampleEntry 11 }

    frsldPvcSmplDataOfferedC OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were offered through





             frsldPvcCtrlTransmitRP within CIR during this
             interval.

             If it is the case that the high capacity counters
             are also used, this MUST report the value of the
             lower 32 bits of the CounterBasedGauge64 value of
             frsldPvcSmplHCDataOfferredC."
        REFERENCE
            "FRF.13: Section 5.1 (DataOfferedc)"
        ::= { frsldPvcSampleEntry 12 }

    frsldPvcSmplDataOfferedE OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were offered through
             frsldPvcCtrlTransmitRP in excess of the CIR
             during this interval.

             If it is the case that the high capacity counters
             are also used, this MUST report the value of the
             lower 32 bits of the CounterBasedGauge64 value of
             frsldPvcSmplHCDataOfferedE."
        REFERENCE
            "FRF.13: Section 5.1 (DataOfferede)"
        ::= { frsldPvcSampleEntry 13 }

    frsldPvcSmplHCFrDeliveredC OBJECT-TYPE
        SYNTAX      CounterBasedGauge64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent within CIR during this interval.  This object
             is a 64-bit version of frsldPvcSmplFrDeliveredC."
        REFERENCE
            "FRF.13: Section 4.1 (FramesDeliveredc)"
        ::= { frsldPvcSampleEntry 14 }

    frsldPvcSmplHCFrDeliveredE OBJECT-TYPE
        SYNTAX      CounterBasedGauge64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were received at
             frsldPvcCtrlReceiveRP and determined to have been





             sent in excess of the CIR during this interval.
             This object is a 64-bit version of frsldPvcSmpl-
             FrDeliveredE."
        REFERENCE
            "FRF.13: Section 4.1 (FramesDeliverede)"
       ::= { frsldPvcSampleEntry 15 }

    frsldPvcSmplHCFrOfferedC OBJECT-TYPE
        SYNTAX      CounterBasedGauge64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were offered through
             frsldPvcCtrlTransmitRP within CIR during this
             interval.  This object is a 64-bit version of
             frsldPvcSmplFrOfferedC."
        REFERENCE
            "FRF.13: Section 4.1 (FramesOfferedc)"
        ::= { frsldPvcSampleEntry 16 }

    frsldPvcSmplHCFrOfferedE OBJECT-TYPE
        SYNTAX      CounterBasedGauge64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of frames that were offered through
             frsldPvcCtrlTransmitRP in excess of the CIR
             during this interval.  This object is a 64-bit
             version of frsldPvcSmplFrOfferedE."
        REFERENCE
            "FRF.13: Section 4.1 (FramesOfferede)"
        ::= { frsldPvcSampleEntry 17 }

    frsldPvcSmplHCDataDeliveredC OBJECT-TYPE
        SYNTAX      CounterBasedGauge64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent within CIR during this interval.  This value
             is a 64-bit version of frsldPvcSmplDataDeliveredC."
        REFERENCE
            "FRF.13: Section 5.1 (DataDeliveredc)"
        ::= { frsldPvcSampleEntry 18 }

    frsldPvcSmplHCDataDeliveredE OBJECT-TYPE
        SYNTAX      CounterBasedGauge64





        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were received at
             frsldPvcCtrlReceiveRP and determined to have been
             sent in excess of the CIR during this interval.  This
             value is a 64-bit version of frsldPvcSmplData-
             DeliveredE."
        REFERENCE
            "FRF.13: Section 5.1 (DataDeliverede)"
        ::= { frsldPvcSampleEntry 19 }

    frsldPvcSmplHCDataOfferedC OBJECT-TYPE
        SYNTAX      CounterBasedGauge64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were offered through
             frsldPvcCtrlTransmitRP within CIR during this
             interval.  This value is a 64-bit version of
             frsldPvcSmplDataOfferedC."
        REFERENCE
            "FRF.13: Section 5.1 (DataOfferedc)"
        ::= { frsldPvcSampleEntry 20 }

    frsldPvcSmplHCDataOfferedE OBJECT-TYPE
        SYNTAX      CounterBasedGauge64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of octets that were offered through
             frsldPvcCtrlTransmitRP in excess of the CIR
             during this interval.  This object is a 64-bit
             version of frsldPvcSmplDataOfferedE."
        REFERENCE
            "FRF.13: Section 5.1 (DataOfferede)"
        ::= { frsldPvcSampleEntry 21 }

    frsldPvcSmplUnavailableTime OBJECT-TYPE
        SYNTAX  TimeTicks
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
            "The amount of time this PVC was declared
             unavailable for any reason during this interval."
        REFERENCE
            "FRF.13: Section 6.1 (OutageTime)"
        ::= { frsldPvcSampleEntry 22 }





    frsldPvcSmplUnavailables OBJECT-TYPE
        SYNTAX  Gauge32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
            "The number of times this PVC was declared
             unavailable for any reason during this interval."
        REFERENCE
            "FRF.13: Section 6.1 (OutageCount)"
        ::= { frsldPvcSampleEntry 23 }

    frsldPvcSmplStartTime OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The value of sysUpTime when this sample interval
             started."
        ::= { frsldPvcSampleEntry 24 }

    frsldPvcSmplEndTime OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The value of sysUpTime when this sample interval
             ended.  No data will be reported and the row will
             not appear in the table until the sample has
             been collected."
        ::= { frsldPvcSampleEntry 25 }

    -- Capabilities Group
    -- This group provides capabilities objects for the tables
    -- that control configuration.

    frsldPvcCtrlWriteCaps OBJECT-TYPE
        SYNTAX  BITS {
               frsldPvcCtrlStatus(0),
               frsldPvcCtrlPacketFreq(1),
               frsldPvcCtrlDelayFrSize(2),
               frsldPvcCtrlDelayType(3),
               frsldPvcCtrlDelayTimeOut(4),
               frsldPvcCtrlPurge(5),
               frsldPvcCtrlDeleteOnPurge(6)
        }
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION





            "This object specifies the write capabilities
             for the read-create objects of the PVC Control
             table.  If the corresponding bit is enabled (1),
             the agent supports writes to that object."
        ::= { frsldCapabilities 1 }

    frsldSmplCtrlWriteCaps OBJECT-TYPE
        SYNTAX  BITS {
               frsldSmplCtrlStatus(0),
               frsldSmplCtrlBuckets(1)
        }
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
            "This object specifies the write capabilities
             for the read-create objects of the Sample Control
             table.  If the corresponding bit is enabled (1),
             the agent supports writes to that object."
        ::= { frsldCapabilities 2 }

    frsldRPCaps OBJECT-TYPE
        SYNTAX  BITS {
               srcLocalRP(0),
               ingTxLocalRP(1),
               tpTxLocalRP(2),
               eqiTxLocalRP(3),
               eqoTxLocalRP(4),
               otherTxLocalRP(5),
               srcRemoteRP(6),
               ingTxRemoteRP(7),
               tpTxRemoteRP(8),
               eqiTxRemoteRP(9),
               eqoTxRemoteRP(10),
               otherTxRemoteRP(11),
               desLocalRP(12),
               ingRxLocalRP(13),
               tpRxLocalRP(14),
               eqiRxLocalRP(15),
               eqoRxLocalRP(16),
               otherRxLocalRP(17),
               desRemoteRP(18),
               ingRxRemoteRP(19),
               tpRxRemoteRP(20),
               eqiRxRemoteRP(21),
               eqoRxRemoteRP(22),
               otherRxRemoteRP(23)
        }
        MAX-ACCESS  read-only





        STATUS  current
        DESCRIPTION
            "This object specifies the reference points that
             the agent supports.  This object allows the management
             application to discover which rows can be created on
             a specific device."
        ::= { frsldCapabilities 3 }

    frsldMaxPvcCtrls   OBJECT-TYPE
        SYNTAX      Integer32 (0..2147483647)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The maximum number of control rows that can be created
             in frsldPvcCtrlTable.  Sets to this object lower than
             the current value of frsldNumPvcCtrls should result in
             inconsistentValue."
        ::= { frsldCapabilities 4 }

    frsldNumPvcCtrls   OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current number of rows in frsldPvcCtrlTable."
        ::= { frsldCapabilities 5 }


    frsldMaxSmplCtrls   OBJECT-TYPE
        SYNTAX      Integer32 (0..2147483647)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The maximum number of control rows that can be created
             in frsldSmplCtrlTable.  Sets to this object lower than
             the current value of frsldNumSmplCtrls should result in
             inconsistentValue."
        ::= { frsldCapabilities 6 }

    frsldNumSmplCtrls   OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current number of rows in frsldSmplCtrlTable."
        ::= { frsldCapabilities 7 }

    -- Conformance Information





    frsldMIBGroups      OBJECT IDENTIFIER ::= { frsldConformance 1 }
    frsldMIBCompliances OBJECT IDENTIFIER ::= { frsldConformance 2 }

    --
    -- Compliance Statements
    --

    frsldCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
            "The compliance statement for SNMP entities
             which support with Frame Relay Service Level
             Definitions.  This group defines the minimum
             level of support required for compliance."
        MODULE -- this module
            MANDATORY-GROUPS { frsldPvcReqCtrlGroup,
                               frsldPvcReqDataGroup,
                               frsldCapabilitiesGroup}

            GROUP       frsldPvcHCFrameDataGroup
            DESCRIPTION
               "This group is mandatory only for those network
                interfaces with corresponding instance of ifSpeed
                 greater than 650,000,000 bits/second."

            GROUP       frsldPvcHCOctetDataGroup
            DESCRIPTION
               "This group is mandatory only for those network
                interfaces with corresponding instance of ifSpeed
                greater than 650,000,000 bits/second."

            GROUP       frsldPvcPacketGroup
            DESCRIPTION
               "This group is optional.  Network interfaces that
                allow control of the packets used to collect
                information are encouraged to implement this
                group."

            GROUP       frsldPvcDelayCtrlGroup
            DESCRIPTION
               "This group is optional.  Network interfaces that
                offer control of the delay measurement are
                strongly encouraged to implement this group."


            GROUP       frsldPvcSampleCtrlGroup
            DESCRIPTION
               "This group is mandatory only for those network





                interfaces that allow data sampling."

            GROUP       frsldPvcDelayDataGroup
            DESCRIPTION
               "This group is only mandatory when
                frsldPvcDelayCtrlGroup is implemented.  It is
                strongly encouraged that any device capable
                of measuring delay implement this group."

            GROUP       frsldPvcSampleDelayGroup
            DESCRIPTION
               "This group is only mandatory when both
                frsldPvcSampleCtrlGroup and frsldPvcDelayDataGroup
                are supported."

            GROUP       frsldPvcSampleDataGroup
            DESCRIPTION
               "This group is mandatory whenever
                frsldPvcSampleCtrlGroup is supported."

            GROUP       frsldPvcSampleHCFrameGroup
            DESCRIPTION
               "This group is mandatory whenever both
                frsldPvcSampleCtrlGroup and frsldPvcHCFrameDataGroup
                are supported."

            GROUP       frsldPvcSampleHCDataGroup
            DESCRIPTION
               "This group is mandatory whenever both
                frsldPvcSampleCtrlGroup and frsldPvcHCOctetDataGroup
                are supported."

            GROUP       frsldPvcSampleAvailGroup
            DESCRIPTION
               "This group is mandatory whenever
                frsldPvcSampleCtrlGroup is supported."

            GROUP       frsldPvcSampleGeneralGroup
            DESCRIPTION
               "This group is mandatory whenever
                frsldPvcSampleCtrlGroup is supported."

            OBJECT      frsldPvcCtrlStatus
            SYNTAX      RowStatus { active(1) } -- subset of RowStatus
            MIN-ACCESS  read-only
            DESCRIPTION
               "Row creation can be done outside of the scope of
                the SNMP protocol.  If this object is implemented





                with max-access of read-only, then the only value
                that MUST be returned is active(1) and
                frsldPvcCtrlWriteCaps MUST return 0 for the
                frsldPvcCtrlStatus(0) bit."

            OBJECT      frsldPvcCtrlPurge
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required.  If this object is
                 implemented with a max-access of read-only, then
                 the frsldPvcCtrlPurge(5) bit must return 0."

            OBJECT      frsldPvcCtrlDeleteOnPurge
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required.  If this object is
                 implemented with a max-access of read-only, then
                 the frsldPvcCtrlDeleteOnPurge(6) bit must return
                 0."

            OBJECT      frsldMaxPvcCtrls
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required if the device either
                 dynamically allocates memory or statically allocates
                 a fixed number of entries.  In the case of static
                 allocation, the device should always report the
                 correct maximum number of controls.  In the case
                 of dynamic allocation, the device SHOULD always
                 report a number greater than frsldNumPvcCtrls
                 when allocation is possible and a number equal to
                 frsldNumPvcCtrls when allocation is not possible."
            OBJECT      frsldMaxSmplCtrls
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required if the device either
                 dynamically allocates memory or statically allocates
                 a fixed number of entries.  In the case of static
                 allocation, the device should always report the
                 correct maximum number of controls.  In the case
                 of dynamic allocation, the device SHOULD always
                 report a number greater than frsldNumSmplCtrls
                 when allocation is possible and a number equal to
                 frsldNumSmplCtrls when allocation is not possible."

    ::= { frsldMIBCompliances 1 }

    --





    -- Units of Conformance
    --
    frsldPvcReqCtrlGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcCtrlStatus,
            frsldPvcCtrlPurge,
            frsldPvcCtrlDeleteOnPurge,
            frsldPvcCtrlLastPurgeTime
       }
       STATUS  current
       DESCRIPTION
           "A collection of required objects providing
            control information applicable to a PVC which
            implements Service Level Definitions."
       ::= { frsldMIBGroups 1 }

    frsldPvcPacketGroup OBJECT-GROUP
       OBJECTS {
            frsldPvcCtrlPacketFreq
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing packet
            level control information applicable to a PVC which
            implements Service Level Definitions."
       ::= { frsldMIBGroups 2 }

    frsldPvcDelayCtrlGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcCtrlDelayFrSize,
            frsldPvcCtrlDelayType,
            frsldPvcCtrlDelayTimeOut
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing delay
            control information applicable to a PVC which
            implements Service Level Definitions.

            If this group is implemented, frsldPvcPacketGroup
            and frsldPvcDelayDataGroup MUST also be implemented."
       ::= { frsldMIBGroups 3 }

    frsldPvcSampleCtrlGroup  OBJECT-GROUP
       OBJECTS {
            frsldSmplCtrlStatus,
            frsldSmplCtrlColPeriod,
            frsldSmplCtrlBuckets,





            frsldSmplCtrlBucketsGranted
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing sample
            control information applicable to a PVC which
            implements Service Level Definitions.

            If this group is implemented, frsldPvcReqDataGroup
            and frsldPvcSampleGeneralGroup MUST also be
            implemented."
       ::= { frsldMIBGroups 4 }

    frsldPvcReqDataGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcDataFrDeliveredC,
            frsldPvcDataFrDeliveredE,
            frsldPvcDataFrOfferedC,
            frsldPvcDataFrOfferedE,
            frsldPvcDataDataDeliveredC,
            frsldPvcDataDataDeliveredE,
            frsldPvcDataDataOfferedC,
            frsldPvcDataDataOfferedE,
            frsldPvcDataUnavailableTime,
            frsldPvcDataUnavailables
       }
       STATUS  current
       DESCRIPTION
           "A collection of required objects providing data
            collected on a PVC which implements Service
            Level Definitions."
       ::= { frsldMIBGroups 5 }

    frsldPvcDelayDataGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcDataMissedPolls
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing delay
            data collected on a PVC which implements Service
            Level Definitions.

            If this group is implemented, frsldPvcDelayCtrlGroup
            MUST also be implemented."
       ::= { frsldMIBGroups 6 }

    frsldPvcHCFrameDataGroup  OBJECT-GROUP





       OBJECTS {
            frsldPvcDataHCFrDeliveredC,
            frsldPvcDataHCFrDeliveredE,
            frsldPvcDataHCFrOfferedC,
            frsldPvcDataHCFrOfferedE
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing high
            capacity frame data collected on a PVC which
            implements Service Level Definitions."
       ::= { frsldMIBGroups 7 }

    frsldPvcHCOctetDataGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcDataHCDataDeliveredC,
            frsldPvcDataHCDataDeliveredE,
            frsldPvcDataHCDataOfferedC,
            frsldPvcDataHCDataOfferedE
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing high
            capacity octet data collected on a PVC which
            implements Service Level Definitions."
       ::= { frsldMIBGroups 8 }

    frsldPvcSampleDelayGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcSmplDelayMin,
            frsldPvcSmplDelayMax,
            frsldPvcSmplDelayAvg,
            frsldPvcSmplMissedPolls
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing delay
            sample data collected on a PVC which implements
            Service Level Definitions.

            If this group is implemented, frsldPvcDelayCtrlGroup
            MUST also be implemented."
       ::= { frsldMIBGroups 9 }

    frsldPvcSampleDataGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcSmplFrDeliveredC,
            frsldPvcSmplFrDeliveredE,





            frsldPvcSmplFrOfferedC,
            frsldPvcSmplFrOfferedE,
            frsldPvcSmplDataDeliveredC,
            frsldPvcSmplDataDeliveredE,
            frsldPvcSmplDataOfferedC,
            frsldPvcSmplDataOfferedE
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing data
            and frame delivery sample data collected on a PVC
            which implements Service Level Definitions.

            If this group is implemented, frsldPvcReqDataGroup
            MUST also be implemented."
       ::= { frsldMIBGroups 10 }

    frsldPvcSampleHCFrameGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcSmplHCFrDeliveredC,
            frsldPvcSmplHCFrDeliveredE,
            frsldPvcSmplHCFrOfferedC,
            frsldPvcSmplHCFrOfferedE
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing high
            capacity frame delivery sample data collected on a PVC
            which implements Service Level Definitions.

            If this group is implemented, frsldPvcHCFrameDataGroup
            MUST also be implemented."
       ::= { frsldMIBGroups 11 }

    frsldPvcSampleHCDataGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcSmplHCDataDeliveredC,
            frsldPvcSmplHCDataDeliveredE,
            frsldPvcSmplHCDataOfferedC,
            frsldPvcSmplHCDataOfferedE
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing high
            capacity data delivery sample data collected on a PVC
            which implements Service Level Definitions.

            If this group is implemented, frsldPvcHCOctetDataGroup





            MUST also be implemented."
       ::= { frsldMIBGroups 12 }

    frsldPvcSampleAvailGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcSmplUnavailableTime,
            frsldPvcSmplUnavailables
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing
            availability sample data collected on a PVC which
            implements Service Level Definitions.

            If this group is implemented, frsldPvcReqDataGroup
            MUST also be implemented."
       ::= { frsldMIBGroups 13 }

    frsldPvcSampleGeneralGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcSmplStartTime,
            frsldPvcSmplEndTime
       }
       STATUS  current
       DESCRIPTION
           "A collection of optional objects providing
            general sample data collected on a PVC which
            implements Service Level Definitions."
       ::= { frsldMIBGroups 14 }

    frsldCapabilitiesGroup  OBJECT-GROUP
       OBJECTS {
            frsldPvcCtrlWriteCaps,
            frsldSmplCtrlWriteCaps,
            frsldRPCaps,
            frsldMaxPvcCtrls,
            frsldNumPvcCtrls,
            frsldMaxSmplCtrls,
            frsldNumSmplCtrls
       }
       STATUS  current
       DESCRIPTION
           "A collection of required objects providing
            capability information and control for this
            MIB module."
       ::= { frsldMIBGroups 15 }
END





