DNS-SERVER-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       mib-2
           FROM RFC-1213
       MODULE-IDENTITY, OBJECT-TYPE, OBJECT-IDENTITY,
       IpAddress, Counter32, Gauge32
           FROM SNMPv2-SMI
       TEXTUAL-CONVENTION, RowStatus, DisplayString, TruthValue
           FROM SNMPv2-TC
       MODULE-COMPLIANCE, OBJECT-GROUP
           FROM SNMPv2-CONF;

   dns OBJECT-IDENTITY
       STATUS  current
       DESCRIPTION
               "The OID assigned to DNS MIB work by the IANA."
       ::= { mib-2 32 }

   dnsServMIB MODULE-IDENTITY
       LAST-UPDATED "9401282251Z"
       ORGANIZATION "IETF DNS Working Group"
       CONTACT-INFO
               "       Rob Austein
               Postal: Epilogue Technology Corporation
                       268 Main Street, Suite 283
                       North Reading, MA 10864
                       US
                  Tel: +1 617 245 0804
                  Fax: +1 617 245 8122
               E-Mail: sra@epilogue.com

                       Jon Saperia
               Postal: Digital Equipment Corporation
                       110 Spit Brook Road
                       ZKO1-3/H18
                       Nashua, NH 03062-2698
                       US
                  Tel: +1 603 881 0480
                  Fax: +1 603 881 0120
                Email: saperia@zko.dec.com"
       DESCRIPTION
               "The MIB module for entities implementing the server side
               of the Domain Name System (DNS) protocol."
       ::= { dns 1 }






   dnsServMIBObjects       OBJECT IDENTIFIER ::= { dnsServMIB 1 }

   -- (Old-style) groups in the DNS server MIB.

   dnsServConfig           OBJECT IDENTIFIER ::= { dnsServMIBObjects 1 }
   dnsServCounter          OBJECT IDENTIFIER ::= { dnsServMIBObjects 2 }
   dnsServOptCounter       OBJECT IDENTIFIER ::= { dnsServMIBObjects 3 }
   dnsServZone             OBJECT IDENTIFIER ::= { dnsServMIBObjects 4 }


   -- Textual conventions

   DnsName ::= TEXTUAL-CONVENTION
       -- A DISPLAY-HINT would be nice, but difficult to express.
       STATUS  current
       DESCRIPTION
               "A DNS name is a sequence of labels.  When DNS names are
               displayed, the boundaries between labels are typically
               indicated by dots (e.g. `Acme' and `COM' are labels in
               the name `Acme.COM').  In the DNS protocol, however, no
               such separators are needed because each label is encoded
               as a length octet followed by the indicated number of
               octets of label.  For example, `Acme.COM' is encoded as
               the octet sequence { 4, 'A', 'c', 'm', 'e', 3, 'C', 'O',
               'M', 0 } (the final 0 is the length of the name of the
               root domain, which appears implicitly at the end of any
               DNS name).  This MIB uses the same encoding as the DNS
               protocol.

               A DnsName must always be a fully qualified name.  It is
               an error to encode a relative domain name as a DnsName
               without first making it a fully qualified name."
       REFERENCE
               "RFC-1034 section 3.1."
       SYNTAX  OCTET STRING (SIZE (0..255))

   DnsNameAsIndex ::= TEXTUAL-CONVENTION
       STATUS  current
       DESCRIPTION
               "This textual convention is like a DnsName, but is used
               as an index componant in tables.  Alphabetic characters
               in names of this type are restricted to uppercase: the
               characters 'a' through 'z' are mapped to the characters
               'A' through 'Z'.  This restriction is intended to make
               the lexical ordering imposed by SNMP useful when applied
               to DNS names.

               Note that it is theoretically possible for a valid DNS





               name to exceed the allowed length of an SNMP object
               identifer, and thus be impossible to represent in tables
               in this MIB that are indexed by DNS name.  Sampling of
               DNS names in current use on the Internet suggests that
               this limit does not pose a serious problem in practice."
       REFERENCE
               "RFC-1034 section 3.1, RFC-1448 section 4.1."
       SYNTAX  DnsName

   DnsClass ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "2d"
       STATUS  current
       DESCRIPTION
               "This data type is used to represent the class values
               which appear in Resource Records in the DNS.  A 16-bit
               unsigned integer is used to allow room for new classes
               of records to be defined.  Existing standard classes are
               listed in the DNS specifications."
       REFERENCE
               "RFC-1035 section 3.2.4."
       SYNTAX  INTEGER (0..65535)

   DnsType ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "2d"
       STATUS  current
       DESCRIPTION
               "This data type is used to represent the type values
               which appear in Resource Records in the DNS.  A 16-bit
               unsigned integer is used to allow room for new record
               types to be defined.  Existing standard types are listed
               in the DNS specifications."
       REFERENCE
               "RFC-1035 section 3.2.2."
       SYNTAX  INTEGER (0..65535)

   DnsQClass ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "2d"
       STATUS  current
       DESCRIPTION
               "This data type is used to represent the QClass values
               which appear in Resource Records in the DNS.  A 16-bit
               unsigned integer is used to allow room for new QClass
               records to be defined.  Existing standard QClasses are
               listed in the DNS specification."
       REFERENCE
               "RFC-1035 section 3.2.5."
       SYNTAX  INTEGER (0..65535)






   DnsQType ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "2d"
       STATUS  current
       DESCRIPTION
               "This data type is used to represent the QType values
               which appear in Resource Records in the DNS.  A 16-bit
               unsigned integer is used to allow room for new QType
               records to be defined.  Existing standard QTypes are
               listed in the DNS specification."
       REFERENCE
               "RFC-1035 section 3.2.3."
       SYNTAX  INTEGER (0..65535)

   DnsTime ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "4d"
       STATUS  current
       DESCRIPTION
               "DnsTime values are 32-bit unsigned integers which
               measure time in seconds."
       REFERENCE
               "RFC-1035."
       SYNTAX  Gauge32


   DnsOpCode ::= TEXTUAL-CONVENTION
       STATUS  current
       DESCRIPTION
               "This textual convention is used to represent the DNS
               OPCODE values used in the header section of DNS
               messages.  Existing standard OPCODE values are listed in
               the DNS specifications."
       REFERENCE
               "RFC-1035 section 4.1.1."
       SYNTAX  INTEGER (0..15)

   DnsRespCode ::= TEXTUAL-CONVENTION
       STATUS  current
       DESCRIPTION
               "This data type is used to represent the DNS RCODE value
               in DNS response messages.  Existing standard RCODE
               values are listed in the DNS specifications."
       REFERENCE
               "RFC-1035 section 4.1.1."
       SYNTAX  INTEGER (0..15)









   -- Server Configuration Group

   dnsServConfigImplementIdent OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "The implementation identification string for the DNS
               server software in use on the system, for example;
               `FNS-2.1'"
       ::= { dnsServConfig 1 }

   dnsServConfigRecurs  OBJECT-TYPE
       SYNTAX      INTEGER { available(1),
                             restricted(2),
                             unavailable(3) }
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "This represents the recursion services offered by this
               name server.  The values that can be read or written
               are:

               available(1) - performs recursion on requests from
               clients.

               restricted(2) - recursion is performed on requests only
               from certain clients, for example; clients on an access
               control list.

               unavailable(3) - recursion is not available."
        ::= { dnsServConfig 2 }

   dnsServConfigUpTime OBJECT-TYPE
       SYNTAX      DnsTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "If the server has a persistent state (e.g., a process),
               this value will be the time elapsed since it started.
               For software without persistant state, this value will
               be zero."
       ::= { dnsServConfig 3 }

   dnsServConfigResetTime OBJECT-TYPE
       SYNTAX      DnsTime
       MAX-ACCESS  read-only
       STATUS      current





       DESCRIPTION
               "If the server has a persistent state (e.g., a process)
               and supports a `reset' operation (e.g., can be told to
               re-read configuration files), this value will be the
               time elapsed since the last time the name server was
               `reset.'  For software that does not have persistence or
               does not support a `reset' operation, this value will be
               zero."
       ::= { dnsServConfig 4 }

   dnsServConfigReset OBJECT-TYPE
       SYNTAX      INTEGER { other(1),
                             reset(2),
                             initializing(3),
                             running(4) }
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "Status/action object to reinitialize any persistant name
               server state.  When set to reset(2), any persistant
               name server state (such as a process) is reinitialized as
               if the name server had just been started.  This value
               will never be returned by a read operation.  When read,
               one of the following values will be returned:
                   other(1) - server in some unknown state;
                   initializing(3) - server (re)initializing;
                   running(4) - server currently running."
       ::= { dnsServConfig 5 }


   -- Server Counter Group

   dnsServCounterAuthAns OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries which were authoritatively answered."
       ::= { dnsServCounter 2 }

   dnsServCounterAuthNoNames OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries for which `authoritative no such name'
               responses were made."
       ::= { dnsServCounter 3 }





   dnsServCounterAuthNoDataResps OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries for which `authoritative no such data'
               (empty answer) responses were made."
       ::= { dnsServCounter 4 }

   dnsServCounterNonAuthDatas OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries which were non-authoritatively
               answered (cached data)."
       ::= { dnsServCounter 5 }

   dnsServCounterNonAuthNoDatas OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries which were non-authoritatively
               answered with no data (empty answer)."
       ::= { dnsServCounter 6 }

   dnsServCounterReferrals OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests that were referred to other servers."
       ::= { dnsServCounter 7 }

   dnsServCounterErrors OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests the server has processed that were
               answered with errors (RCODE values other than 0 and 3)."
       REFERENCE
               "RFC-1035 section 4.1.1."
       ::= { dnsServCounter 8 }

   dnsServCounterRelNames OBJECT-TYPE
       SYNTAX      Counter32





       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests received by the server for names that
               are only 1 label long (text form - no internal dots)."
       ::= { dnsServCounter 9 }

   dnsServCounterReqRefusals OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of DNS requests refused by the server."
       ::= { dnsServCounter 10 }

   dnsServCounterReqUnparses OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests received which were unparseable."
       ::= { dnsServCounter 11 }

   dnsServCounterOtherErrors OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests which were aborted for other (local)
               server errors."
       ::= { dnsServCounter 12 }

   -- DNS Server Counter Table

   dnsServCounterTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF DnsServCounterEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "Counter information broken down by DNS class and type."
       ::= { dnsServCounter 13 }

   dnsServCounterEntry OBJECT-TYPE
       SYNTAX      DnsServCounterEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "This table contains count information for each DNS class





               and type value known to the server.  The index allows
               management software to to create indices to the table to
               get the specific information desired, e.g., number of
               queries over UDP for records with type value `A' which
               came to this server.  In order to prevent an
               uncontrolled expansion of rows in the table; if
               dnsServCounterRequests is 0 and dnsServCounterResponses
               is 0, then the row does not exist and `no such' is
               returned when the agent is queried for such instances."
       INDEX     { dnsServCounterOpCode,
                   dnsServCounterQClass,
                   dnsServCounterQType,
                   dnsServCounterTransport }
       ::= { dnsServCounterTable 1 }

   DnsServCounterEntry ::=
       SEQUENCE {
           dnsServCounterOpCode
               DnsOpCode,
           dnsServCounterQClass
               DnsClass,
           dnsServCounterQType
               DnsType,
           dnsServCounterTransport
               INTEGER,
           dnsServCounterRequests
               Counter32,
           dnsServCounterResponses
               Counter32
           }

   dnsServCounterOpCode OBJECT-TYPE
       SYNTAX      DnsOpCode
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "The DNS OPCODE being counted in this row of the table."
       ::= { dnsServCounterEntry 1 }

   dnsServCounterQClass OBJECT-TYPE
       SYNTAX      DnsClass
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "The class of record being counted in this row of the
               table."
       ::= { dnsServCounterEntry 2 }






   dnsServCounterQType OBJECT-TYPE
       SYNTAX      DnsType
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "The type of record which is being counted in this row in
               the table."
       ::= { dnsServCounterEntry 3 }

   dnsServCounterTransport OBJECT-TYPE
       SYNTAX      INTEGER { udp(1), tcp(2), other(3) }
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "A value of udp(1) indicates that the queries reported on
               this row were sent using UDP.

               A value of tcp(2) indicates that the queries reported on
               this row were sent using TCP.

               A value of other(3) indicates that the queries reported
               on this row were sent using a transport that was neither
               TCP nor UDP."
       ::= { dnsServCounterEntry 4 }

   dnsServCounterRequests OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests (queries) that have been recorded in
               this row of the table."
       ::= { dnsServCounterEntry 5 }

   dnsServCounterResponses OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of responses made by the server since
               initialization for the kind of query identified on this
               row of the table."
       ::= { dnsServCounterEntry 6 }










   -- Server Optional Counter Group

   -- The Server Optional Counter Group is intended for those systems
   -- which make distinctions between the different sources of the DNS
   -- queries as defined below.
   --
   -- Objects in this group are implemented on servers which distinguish
   -- between queries which originate from the same host as the server,
   -- queries from one of an arbitrary group of hosts that are on an
   -- access list defined by the server, and queries from hosts that do
   -- not fit either of these descriptions.
   --
   -- The objects found in the Server Counter group are totals.  Thus if
   -- one wanted to identify, for example, the number of queries from
   -- `remote' hosts which have been given authoritative answers, one
   -- would subtract the current values of ServOptCounterFriendsAuthAns
   -- and ServOptCounterSelfAuthAns from servCounterAuthAns.
   --
   -- The purpose of these distinctions is to allow for implementations
   -- to group queries and responses on this basis.  One way in which
   -- servers may make these distinctions is by looking at the source IP
   -- address of the DNS query.  If the source of the query is `your
   -- own' then the query should be counted as `yourself' (local host).
   -- If the source of the query matches an `access list,' the query
   -- came from a friend.  What constitutes an `access list' is
   -- implementation dependent and could be as simple as a rule that all
   -- hosts on the same IP network as the DNS server are classed
   -- `friends.'
   --
   -- In order to avoid double counting, the following rules apply:
   --
   -- 1. No host is in more than one of the three groups defined above.
   --
   -- 2. All queries from the local host are always counted in the
   --    `yourself' group regardless of what the access list, if any,
   --    says.
   --
   -- 3. The access list should not define `your friends' in such a way
   --    that it includes all hosts.   That is, not everybody is your
   --    `friend.'

   dnsServOptCounterSelfAuthAns OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests the server has processed which
               originated from a resolver on the same host for which





               there has been an authoritative answer."
       ::= { dnsServOptCounter 1 }

   dnsServOptCounterSelfAuthNoNames OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests the server has processed which
               originated from a resolver on the same host for which
               there has been an authoritative no such name answer
               given."
       ::= { dnsServOptCounter 2 }

   dnsServOptCounterSelfAuthNoDataResps OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests the server has processed which
               originated from a resolver on the same host for which
               there has been an authoritative no such data answer
               (empty answer) made."
       ::= { dnsServOptCounter 3 }

   dnsServOptCounterSelfNonAuthDatas OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests the server has processed which
               originated from a resolver on the same host for which a
               non-authoritative answer (cached data) was made."
       ::= { dnsServOptCounter 4 }

   dnsServOptCounterSelfNonAuthNoDatas OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests the server has processed which
               originated from a resolver on the same host for which a
               `non-authoritative, no such data' response was made
               (empty answer)."
       ::= { dnsServOptCounter 5 }

   dnsServOptCounterSelfReferrals OBJECT-TYPE
       SYNTAX      Counter32





       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries the server has processed which
               originated from a resolver on the same host and were
               referred to other servers."
       ::= { dnsServOptCounter 6 }

   dnsServOptCounterSelfErrors OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests the server has processed which
               originated from a resolver on the same host which have
               been answered with errors (RCODEs other than 0 and 3)."
       REFERENCE
               "RFC-1035 section 4.1.1."
       ::= { dnsServOptCounter 7 }

   dnsServOptCounterSelfRelNames OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests received for names that are only 1
               label long (text form - no internal dots) the server has
               processed which originated from a resolver on the same
               host."
       ::= { dnsServOptCounter 8 }

   dnsServOptCounterSelfReqRefusals OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of DNS requests refused by the server which
               originated from a resolver on the same host."
       ::= { dnsServOptCounter 9 }

   dnsServOptCounterSelfReqUnparses OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests received which were unparseable and
               which originated from a resolver on the same host."
       ::= { dnsServOptCounter 10 }





   dnsServOptCounterSelfOtherErrors OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests which were aborted for other (local)
               server errors and which originated on the same host."
       ::= { dnsServOptCounter 11 }

   dnsServOptCounterFriendsAuthAns OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries originating from friends which were
               authoritatively answered.  The definition of friends is
               a locally defined matter."
       ::= { dnsServOptCounter 12 }

   dnsServOptCounterFriendsAuthNoNames OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries originating from friends, for which
               authoritative `no such name' responses were made.  The
               definition of friends is a locally defined matter."
       ::= { dnsServOptCounter 13 }

   dnsServOptCounterFriendsAuthNoDataResps OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries originating from friends for which
               authoritative no such data (empty answer) responses were
               made.  The definition of friends is a locally defined
               matter."
       ::= { dnsServOptCounter 14 }

   dnsServOptCounterFriendsNonAuthDatas OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries originating from friends which were
               non-authoritatively answered (cached data). The
               definition of friends is a locally defined matter."





       ::= { dnsServOptCounter 15 }

   dnsServOptCounterFriendsNonAuthNoDatas OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of queries originating from friends which were
               non-authoritatively answered with no such data (empty
               answer)."
       ::= { dnsServOptCounter 16 }

   dnsServOptCounterFriendsReferrals OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests which originated from friends that
               were referred to other servers.  The definition of
               friends is a locally defined matter."
       ::= { dnsServOptCounter 17 }

   dnsServOptCounterFriendsErrors OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests the server has processed which
               originated from friends and were answered with errors
               (RCODE values other than 0 and 3).  The definition of
               friends is a locally defined matter."
       REFERENCE
               "RFC-1035 section 4.1.1."
       ::= { dnsServOptCounter 18 }

   dnsServOptCounterFriendsRelNames OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests received for names from friends that
               are only 1 label long (text form - no internal dots) the
               server has processed."
       ::= { dnsServOptCounter 19 }

   dnsServOptCounterFriendsReqRefusals OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only





       STATUS      current
       DESCRIPTION
               "Number of DNS requests refused by the server which were
               received from `friends'."
       ::= { dnsServOptCounter 20 }

   dnsServOptCounterFriendsReqUnparses OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests received which were unparseable and
               which originated from `friends'."
       ::= { dnsServOptCounter 21 }

   dnsServOptCounterFriendsOtherErrors OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Number of requests which were aborted for other (local)
               server errors and which originated from `friends'."
       ::= { dnsServOptCounter 22 }


   -- Server Zone Group

   -- DNS Management Zone Configuration Table

   -- This table contains zone configuration information.

   dnsServZoneTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF DnsServZoneEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "Table of zones for which this name server provides
               information.  Each of the zones may be loaded from stable
               storage via an implementation-specific mechanism or may
               be obtained from another name server via a zone transfer.

               If name server doesn't load any zones, this table is
               empty."
       ::= { dnsServZone 1 }

   dnsServZoneEntry OBJECT-TYPE
       SYNTAX      DnsServZoneEntry
       MAX-ACCESS  not-accessible





       STATUS      current
       DESCRIPTION
               "An entry in the name server zone table.  New rows may be
               added either via SNMP or by the name server itself."
       INDEX     { dnsServZoneName,
                   dnsServZoneClass }
       ::= { dnsServZoneTable 1 }

   DnsServZoneEntry ::=
       SEQUENCE {
           dnsServZoneName
               DnsNameAsIndex,
           dnsServZoneClass
               DnsClass,
           dnsServZoneLastReloadSuccess
               DnsTime,
           dnsServZoneLastReloadAttempt
               DnsTime,
           dnsServZoneLastSourceAttempt
               IpAddress,
           dnsServZoneStatus
               RowStatus,
           dnsServZoneSerial
               Counter32,
           dnsServZoneCurrent
               TruthValue,
           dnsServZoneLastSourceSuccess
               IpAddress
       }

   dnsServZoneName OBJECT-TYPE
       SYNTAX      DnsNameAsIndex
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "DNS name of the zone described by this row of the table.
               This is the owner name of the SOA RR that defines the
               top of the zone. This is name is in uppercase:
               characters 'a' through 'z' are mapped to 'A' through 'Z'
               in order to make the lexical ordering useful."
       ::= { dnsServZoneEntry 1 }

   dnsServZoneClass OBJECT-TYPE
       SYNTAX      DnsClass
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "DNS class of the RRs in this zone."





       ::= { dnsServZoneEntry 2 }

   dnsServZoneLastReloadSuccess OBJECT-TYPE
       SYNTAX      DnsTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Elapsed time in seconds since last successful reload of
               this zone."
       ::= { dnsServZoneEntry 3 }

   dnsServZoneLastReloadAttempt OBJECT-TYPE
       SYNTAX      DnsTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Elapsed time in seconds since last attempted reload of
               this zone."
       ::= { dnsServZoneEntry 4 }

   dnsServZoneLastSourceAttempt OBJECT-TYPE
       SYNTAX      IpAddress
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "IP address of host from which most recent zone transfer
               of this zone was attempted.  This value should match the
               value of dnsServZoneSourceSuccess if the attempt was
               succcessful.  If zone transfer has not been attempted
               within the memory of this name server, this value should
               be 0.0.0.0."
       ::= { dnsServZoneEntry 5 }

   dnsServZoneStatus OBJECT-TYPE
       SYNTAX      RowStatus
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
               "The status of the information represented in this row of
               the table."
       ::= { dnsServZoneEntry 6 }

   dnsServZoneSerial OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Zone serial number (from the SOA RR) of the zone





               represented by this row of the table.  If the zone has
               not been successfully loaded within the memory of this
               name server, the value of this variable is zero."
       ::= { dnsServZoneEntry 7 }

   dnsServZoneCurrent OBJECT-TYPE
       SYNTAX      TruthValue
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "Whether the server's copy of the zone represented by
               this row of the table is currently valid.  If the zone
               has never been successfully loaded or has expired since
               it was last succesfully loaded, this variable will have
               the value false(2), otherwise this variable will have
               the value true(1)."
       ::= { dnsServZoneEntry 8 }

   dnsServZoneLastSourceSuccess OBJECT-TYPE
       SYNTAX      IpAddress
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "IP address of host which was the source of the most
               recent successful zone transfer for this zone.  If
               unknown (e.g., zone has never been successfully
               transfered) or irrelevant (e.g., zone was loaded from
               stable storage), this value should be 0.0.0.0."
       ::= { dnsServZoneEntry 9 }

   -- DNS Zone Source Table

   dnsServZoneSrcTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF DnsServZoneSrcEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "This table is a list of IP addresses from which the
               server will attempt to load zone information using DNS
               zone transfer operations.  A reload may occur due to SNMP
               operations that create a row in dnsServZoneTable or a
               SET to object dnsServZoneReload.  This table is only
               used when the zone is loaded via zone transfer."
       ::= { dnsServZone 2 }

   dnsServZoneSrcEntry OBJECT-TYPE
       SYNTAX      DnsServZoneSrcEntry
       MAX-ACCESS  not-accessible





       STATUS      current
       DESCRIPTION
               "An entry in the name server zone source table."
       INDEX     { dnsServZoneSrcName,
                   dnsServZoneSrcClass,
                   dnsServZoneSrcAddr }
       ::= { dnsServZoneSrcTable 1 }

   DnsServZoneSrcEntry ::=
       SEQUENCE {
           dnsServZoneSrcName
               DnsNameAsIndex,
           dnsServZoneSrcClass
               DnsClass,
           dnsServZoneSrcAddr
               IpAddress,
           dnsServZoneSrcStatus
               RowStatus
       }

   dnsServZoneSrcName OBJECT-TYPE
       SYNTAX      DnsNameAsIndex
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "DNS name of the zone to which this entry applies."
       ::= { dnsServZoneSrcEntry 1 }

   dnsServZoneSrcClass OBJECT-TYPE
       SYNTAX      DnsClass
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "DNS class of zone to which this entry applies."
       ::= { dnsServZoneSrcEntry 2 }

   dnsServZoneSrcAddr OBJECT-TYPE
       SYNTAX      IpAddress
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "IP address of name server host from which this zone
               might be obtainable."
       ::= { dnsServZoneSrcEntry 3 }

   dnsServZoneSrcStatus OBJECT-TYPE
       SYNTAX      RowStatus
       MAX-ACCESS  read-create





       STATUS      current
       DESCRIPTION
               "The status of the information represented in this row of
               the table."
       ::= { dnsServZoneSrcEntry 4 }


   -- SNMPv2 groups.

   dnsServMIBGroups        OBJECT IDENTIFIER ::= { dnsServMIB 2 }

   dnsServConfigGroup OBJECT-GROUP
       OBJECTS   { dnsServConfigImplementIdent,
                   dnsServConfigRecurs,
                   dnsServConfigUpTime,
                   dnsServConfigResetTime,
                   dnsServConfigReset }
       STATUS      current
       DESCRIPTION
               "A collection of objects providing basic configuration
               control of a DNS name server."
       ::= { dnsServMIBGroups 1 }

   dnsServCounterGroup OBJECT-GROUP
       OBJECTS   { dnsServCounterAuthAns,
                   dnsServCounterAuthNoNames,
                   dnsServCounterAuthNoDataResps,
                   dnsServCounterNonAuthDatas,
                   dnsServCounterNonAuthNoDatas,
                   dnsServCounterReferrals,
                   dnsServCounterErrors,
                   dnsServCounterRelNames,
                   dnsServCounterReqRefusals,
                   dnsServCounterReqUnparses,
                   dnsServCounterOtherErrors,
                   dnsServCounterOpCode,
                   dnsServCounterQClass,
                   dnsServCounterQType,
                   dnsServCounterTransport,
                   dnsServCounterRequests,
                   dnsServCounterResponses }
       STATUS      current
       DESCRIPTION
               "A collection of objects providing basic instrumentation
               of a DNS name server."
       ::= { dnsServMIBGroups 2 }







   dnsServOptCounterGroup OBJECT-GROUP
       OBJECTS   { dnsServOptCounterSelfAuthAns,
                   dnsServOptCounterSelfAuthNoNames,
                   dnsServOptCounterSelfAuthNoDataResps,
                   dnsServOptCounterSelfNonAuthDatas,
                   dnsServOptCounterSelfNonAuthNoDatas,
                   dnsServOptCounterSelfReferrals,
                   dnsServOptCounterSelfErrors,
                   dnsServOptCounterSelfRelNames,
                   dnsServOptCounterSelfReqRefusals,
                   dnsServOptCounterSelfReqUnparses,
                   dnsServOptCounterSelfOtherErrors,
                   dnsServOptCounterFriendsAuthAns,
                   dnsServOptCounterFriendsAuthNoNames,
                   dnsServOptCounterFriendsAuthNoDataResps,
                   dnsServOptCounterFriendsNonAuthDatas,
                   dnsServOptCounterFriendsNonAuthNoDatas,
                   dnsServOptCounterFriendsReferrals,
                   dnsServOptCounterFriendsErrors,
                   dnsServOptCounterFriendsRelNames,
                   dnsServOptCounterFriendsReqRefusals,
                   dnsServOptCounterFriendsReqUnparses,
                   dnsServOptCounterFriendsOtherErrors }
       STATUS      current
       DESCRIPTION
               "A collection of objects providing extended
               instrumentation of a DNS name server."
       ::= { dnsServMIBGroups 3 }

   dnsServZoneGroup OBJECT-GROUP
       OBJECTS   { dnsServZoneName,
                   dnsServZoneClass,
                   dnsServZoneLastReloadSuccess,
                   dnsServZoneLastReloadAttempt,
                   dnsServZoneLastSourceAttempt,
                   dnsServZoneLastSourceSuccess,
                   dnsServZoneStatus,
                   dnsServZoneSerial,
                   dnsServZoneCurrent,
                   dnsServZoneSrcName,
                   dnsServZoneSrcClass,
                   dnsServZoneSrcAddr,
                   dnsServZoneSrcStatus }
       STATUS      current
       DESCRIPTION
               "A collection of objects providing configuration control
               of a DNS name server which loads authoritative zones."
       ::= { dnsServMIBGroups 4 }





   -- Compliances.

   dnsServMIBCompliances OBJECT IDENTIFIER ::= { dnsServMIB 3 }

   dnsServMIBCompliance MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
               "The compliance statement for agents implementing the DNS
               name server MIB extensions."
       MODULE -- This MIB module
           MANDATORY-GROUPS { dnsServConfigGroup, dnsServCounterGroup }
           GROUP   dnsServOptCounterGroup
           DESCRIPTION
               "The server optional counter group is unconditionally
               optional."
           GROUP   dnsServZoneGroup
           DESCRIPTION
               "The server zone group is mandatory for any name server
               that acts as an authoritative server for any DNS zone."
           OBJECT  dnsServConfigRecurs
           MIN-ACCESS      read-only
           DESCRIPTION
               "This object need not be writable."
           OBJECT  dnsServConfigReset
           MIN-ACCESS      read-only
           DESCRIPTION
               "This object need not be writable."
       ::= { dnsServMIBCompliances 1 }

   END






















