FRAMEWORK-PIB PIB-DEFINITIONS ::= BEGIN


  IMPORTS
      Unsigned32, Integer32, MODULE-IDENTITY,
      MODULE-COMPLIANCE, OBJECT-TYPE, OBJECT-GROUP, pib
              FROM COPS-PR-SPPI
      InstanceId, Prid
              FROM COPS-PR-SPPI-TC
      RoleCombination, PrcIdentifierOid, AttrIdentifierOrZero,
      ClientType, ClientHandle
              FROM FRAMEWORK-TC-PIB
      InetAddress, InetAddressType,
      InetAddressPrefixLength, InetPortNumber
              FROM INET-ADDRESS-MIB
      InterfaceIndex
              FROM IF-MIB
      DscpOrAny
              FROM DIFFSERV-DSCP-TC
      TruthValue, PhysAddress
              FROM SNMPv2-TC
      SnmpAdminString
              FROM SNMP-FRAMEWORK-MIB;

  frameworkPib  MODULE-IDENTITY
      SUBJECT-CATEGORIES { all }
      LAST-UPDATED "200302130000Z"  -- 13 Feb 2003
      ORGANIZATION "IETF RAP WG"
      CONTACT-INFO "
                    Keith McCloghrie
                    Cisco Systems, Inc.
                    170 West Tasman Drive,
                    San Jose, CA 95134-1706 USA
                    Phone: +1 408 526 5260
                    Email: kzm@cisco.com

                    John Seligson
                    Nortel Networks, Inc.
                    4401 Great America Parkway
                    Santa Clara, CA 95054 USA
                    Phone: +1 408 495 2992
                    Email: jseligso@nortelnetworks.com






                    Ravi Sahita
                    Intel Labs.
                    2111 NE 25th Ave.

                    Hillsboro, OR 97124 USA
                    Phone: +1 503 712 1554
                    Email: ravi.sahita@intel.com

                    RAP WG Mailing list: rap@ops.ietf.org"

      DESCRIPTION
           "A PIB module containing the base set of PRCs that
           provide support for management of multiple PIB contexts,
           association of roles to device capabilities and other
           reusable PRCs. PEPs are required for to implement this
           PIB if the above features are desired. This PIB defines
           PRCs applicable to 'all' subject-categories.

           Copyright (C) The Internet Society (2003). This version
           of this PIB module is part of RFC 3318; see the RFC
           itself for full legal notices."
      REVISION     "200302130000Z"  -- 13 Feb 2003
      DESCRIPTION
           "Initial version, published in RFC 3318."

      ::= { pib 2 }

  --
  -- The root OID for PRCs in the Framework PIB
  --

  frwkBasePibClasses
               OBJECT IDENTIFIER ::= { frameworkPib 1 }

  --
  -- PRC Support Table
  --
















  frwkPrcSupportTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkPrcSupportEntry
      PIB-ACCESS     notify
      STATUS         current
      DESCRIPTION
          "Each instance of this PRC specifies a PRC that the device
          supports and a bit string to indicate the attributes of the
          class that are supported.  These PRIs are sent to the PDP to
          indicate to the PDP which PRCs, and which attributes of
          these PRCs, the device supports.

          All install and install-notify PRCs supported by the device
          must be represented in this PRC. Notify PRCs may be
          represented for informational purposes."

      ::= { frwkBasePibClasses 1 }

  frwkPrcSupportEntry OBJECT-TYPE
      SYNTAX         FrwkPrcSupportEntry
      STATUS         current
      DESCRIPTION
          "An instance of the frwkPrcSupport class that identifies a
          specific PRC and associated attributes as supported
          by the device."

      PIB-INDEX { frwkPrcSupportPrid }
      UNIQUENESS { frwkPrcSupportSupportedPrc }

      ::= { frwkPrcSupportTable 1 }

  FrwkPrcSupportEntry ::= SEQUENCE {
          frwkPrcSupportPrid           InstanceId,
          frwkPrcSupportSupportedPrc   PrcIdentifierOid,
          frwkPrcSupportSupportedAttrs OCTET STRING
  }

  frwkPrcSupportPrid OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "An arbitrary integer index that uniquely identifies an
          instance of the frwkPrcSupport class."

      ::= { frwkPrcSupportEntry 1 }









  frwkPrcSupportSupportedPrc OBJECT-TYPE
      SYNTAX         PrcIdentifierOid
      STATUS         current
      DESCRIPTION
          "The object identifier of a supported PRC. The value is the
           OID of the Entry object of the PRC definition. The Entry
           Object definition of a PRC has an OID with value XxxTable.1
           Where, XxxTable is the OID assigned to the PRC Table
           Object definition. There may not be more than one instance
           of the frwkPrcSupport class with the same value of
           frwkPrcSupportSupportedPrc."

      ::= { frwkPrcSupportEntry 2 }

  frwkPrcSupportSupportedAttrs OBJECT-TYPE
      SYNTAX         OCTET STRING
      STATUS         current
      DESCRIPTION
          "A bit string representing the supported attributes of the
          class that is identified by the frwkPrcSupportSupportedPrc
          object.

          Each bit of this bit string corresponds to a class
          attribute, with the most significant bit of the i-th octet
          of this octet string corresponding to the (8*i - 7)-th
          attribute, and the least significant bit of the i-th octet
          corresponding to the (8*i)-th class attribute. Each bit
          specifies whether or not the corresponding class attribute
          is currently supported, with a '1' indicating support and a
          '0' indicating no support.

          If the value of this bit string is N bits long and there are
          more than N class attributes then the bit string is
          logically extended with 0's to the required length.
          On the other hand, If the PDP receives a bit string of
          length N and there are less that N class attributes then the
          PDP should ignore the extra bits in the bit string, i.e.,
          assume those attributes are unsupported."
        REFERENCE
          "COPS Usage for Policy Provisioning.  RFC 3084, section
          2.2.1."

      ::= { frwkPrcSupportEntry 3 }

  --
  -- PIB Incarnation Table
  --






  frwkPibIncarnationTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkPibIncarnationEntry
      PIB-ACCESS     install-notify
      STATUS         current
      DESCRIPTION
          "This PRC contains a single PRovisioning Instance per
          installed context that identifies the current incarnation
          of the PIB and the PDP or network manager that installed
          this incarnation.  The instance of this PRC is reported to
          the PDP in the REQ message so that the PDP can (attempt to)
          ascertain the current state of the PIB. A network manager
          may use the instance to determine the state of the device."

      ::= { frwkBasePibClasses 2 }

  frwkPibIncarnationEntry OBJECT-TYPE
      SYNTAX         FrwkPibIncarnationEntry
      STATUS         current
      DESCRIPTION
          "An instance of the frwkPibIncarnation class. Only
          one instance of this PRC is ever instantiated per context"

      PIB-INDEX { frwkPibIncarnationPrid }

      ::= { frwkPibIncarnationTable 1 }

  FrwkPibIncarnationEntry ::= SEQUENCE {
          frwkPibIncarnationPrid                InstanceId,
          frwkPibIncarnationName                SnmpAdminString,
          frwkPibIncarnationId                  OCTET STRING,
          frwkPibIncarnationLongevity           INTEGER,
          frwkPibIncarnationTtl                 Unsigned32,
          frwkPibIncarnationInCtxtSet           TruthValue,
          frwkPibIncarnationActive              TruthValue,
          frwkPibIncarnationFullState           TruthValue
  }

  frwkPibIncarnationPrid OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "An index to uniquely identify an instance of this PRC."

      ::= { frwkPibIncarnationEntry 1 }









  frwkPibIncarnationName OBJECT-TYPE
      SYNTAX         SnmpAdminString (SIZE (0..255))
      STATUS         current
      DESCRIPTION
          "The name of the PDP that installed the current incarnation
          of the PIB into the device.  A zero-length string value for
          this type implies the PDP has not assigned this type any
          value. By default, it is the zero length string."

      ::= { frwkPibIncarnationEntry 2 }

  frwkPibIncarnationId OBJECT-TYPE
      SYNTAX         OCTET STRING (SIZE (0..255))
      STATUS         current
      DESCRIPTION
          "An ID to identify the current incarnation.  It has meaning
          to the PDP/manager that installed the PIB and perhaps its
          standby PDPs/managers. A zero-length string value for
          this type implies the PDP has not assigned this type any
          value. By default, it is the zero-length string."

      ::= { frwkPibIncarnationEntry 3 }

  frwkPibIncarnationLongevity OBJECT-TYPE
      SYNTAX         INTEGER {
                          expireNever(1),
                          expireImmediate(2),
                          expireOnTimeout(3)
                     }
      STATUS         current
      DESCRIPTION
          "This attribute controls what the PEP does with the
          downloaded policy on a Client Close message or a loss of
          connection to the PDP.

          If set to expireNever, the PEP continues to operate with the
          installed policy indefinitely.  If set to expireImmediate,
          the PEP immediately expires the policy obtained from the PDP
          and installs policy from local configuration.  If set to
          expireOnTimeout, the PEP continues to operate with the
          policy installed by the PDP for a period of time specified
          by frwkPibIncarnationTtl.  After this time (and it has not
          reconnected to the original or new PDP) the PEP expires this
          policy and reverts to local configuration.

          For all cases, it is the responsibility of the PDP to check
          the incarnation and download new policy, if necessary, on a
          reconnect. On receiving a Remove-State for the active





          context, this attribute value MUST be ignored and the PEP
          should expire the policy in that active context immediately.
          Policy enforcement timing only applies to policies that have
          been installed dynamically (e.g., by a PDP via COPS)."
      REFERENCE
          "COPS Usage for Policy Provisioning. RFC 3084."

      ::= { frwkPibIncarnationEntry 4 }

  frwkPibIncarnationTtl OBJECT-TYPE
      SYNTAX         Unsigned32
      UNITS          "seconds"
      STATUS         current
      DESCRIPTION
          "The number of seconds after a Client Close or TCP timeout
          for which the PEP continues to enforce the policy in the
          PIB. After this interval, the PIB is considered expired and
          the device no longer enforces the policy installed in the
          PIB.

          This attribute is only meaningful if
          frwkPibIncarnationLongevity is set to expireOnTimeout."

      ::= { frwkPibIncarnationEntry 5 }

  frwkPibIncarnationInCtxtSet OBJECT-TYPE
      SYNTAX        TruthValue
      STATUS         current
      DESCRIPTION
          "When the PDP installs a PRI with this flag set to 'true' it
          implies this context belongs to the set of contexts out of
          which at the most one context can be active at a given time.
          If this attribute is set to 'false' this context is one of
          the outsourcing (simultaneous active) contexts on the PEP.

          This attribute is 'true' for all contexts belong to the set
          of configuration contexts. Within the configuration context
          set, one context can be active identified by the
          frwkPibIncarnationActive attribute."
      REFERENCE
          "TruthValue Textual Convention, defined in RFC 2579."
      ::= { frwkPibIncarnationEntry 6 }











  frwkPibIncarnationActive OBJECT-TYPE
      SYNTAX         TruthValue
      STATUS         current
      DESCRIPTION
          "When the PDP installs a PRI on the PEP with this attribute
          set to 'true' and if this context belongs to the
          'configuration contexts' set, i.e., the
          frwkPibIncarnationInCtxtSet is set to 'true', then the PIB
          instance to which this PRI belongs must become the active
          PIB instance. In this case, the previous active instance
          from this set MUST become inactive and the
          frwkPibIncarnationActive attribute in that PIB instance MUST
          be set to 'false'.

          When the PDP installs an attribute frwkPibIncarnationActive
          on the PEP  that is 'true' in one PIB instance and if the
          context belongs to the 'configuration contexts' set, the PEP
          must ensure, re-setting the attribute if necessary, that the
          frwkPibIncarnationActive attribute is  'false' in all other
          contexts which belong to the 'configuration contexts' set."

      ::= { frwkPibIncarnationEntry 7 }

  frwkPibIncarnationFullState OBJECT-TYPE
      SYNTAX         TruthValue
      STATUS         current
      DESCRIPTION
          "This attribute is interpreted only when sent in a COPS
          request message from the PEP to the PDP. It does not have
          any meaning when sent from the PDP to the PEP.

          If this attribute is set to 'true' by the PEP, then the
          request that the PEP sends to the PDP must be interpreted as
          the complete configuration request for the PEP. The PDP must
          in this case refresh the request information for the
          handle that the request containing this PRI was received on.
          If this attribute is set to 'false', then the
             request PRIs sent in the request must be interpreted as
          updates to the previous request PRIs sent using that handle.
          See section 3.3 for details on updating request state
          information."
      REFERENCE
          "RFC 3318 Section 2.3"

      ::= { frwkPibIncarnationEntry 8 }

  --
  -- Device Identification Table





  --

  frwkDeviceIdTable OBJECT-TYPE

      SYNTAX         SEQUENCE OF FrwkDeviceIdEntry
      PIB-ACCESS     notify
      STATUS         current
      DESCRIPTION
          "This PRC contains a single PRovisioning Instance that
          contains general purpose device-specific information that is
          used to facilitate efficient policy communication by a PDP.
          The  instance of this PRC is reported to the PDP in a COPS
          request message so that the PDP can take into account
          certain device characteristics during policy installation."

      ::= { frwkBasePibClasses 3 }

  frwkDeviceIdEntry OBJECT-TYPE
      SYNTAX         FrwkDeviceIdEntry
      STATUS         current
      DESCRIPTION
          "An instance of the frwkDeviceId class. Only one instance of
          this PRC is ever instantiated."

      PIB-INDEX { frwkDeviceIdPrid }

      ::= { frwkDeviceIdTable 1 }

  FrwkDeviceIdEntry ::= SEQUENCE {
          frwkDeviceIdPrid        InstanceId,
          frwkDeviceIdDescr       SnmpAdminString,
          frwkDeviceIdMaxMsg      Unsigned32,
          frwkDeviceIdMaxContexts Unsigned32
  }

  frwkDeviceIdPrid OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "An index to uniquely identify an instance of this PRC."

      ::= { frwkDeviceIdEntry 1 }











  frwkDeviceIdDescr OBJECT-TYPE
      SYNTAX         SnmpAdminString (SIZE (1..255))
      STATUS         current
      DESCRIPTION
          "A textual description of the PEP. This value should include
          the name and version identification of the PEP's hardware
          and software."

      ::= { frwkDeviceIdEntry 2 }

  frwkDeviceIdMaxMsg OBJECT-TYPE
      SYNTAX         Unsigned32 (64..4294967295)
      UNITS          "octets"
      STATUS         current
      DESCRIPTION
          "The maximum COPS-PR message size, in octets, that the
          device is capable of processing. Received messages with a
          size in excess of this value must cause the PEP to return an
          error to the PDP containing the global error code
          'maxMsgSizeExceeded'. This is an additional error-avoidance
          mechanism to allow the administrator to know the maximum
          message size supported so that they have the ability to
          control the message size of messages sent to the device.
          This attribute must have a non-zero value. The device should
          send the MAX value for Unsigned32 for this attribute if it
          not defined."
      DEFVAL { 4294967295 }

      ::= { frwkDeviceIdEntry 3 }

  frwkDeviceIdMaxContexts OBJECT-TYPE
     SYNTAX         Unsigned32 (1..4294967295)
     UNITS          "contexts"
     STATUS         current
     DESCRIPTION
         "The maximum number of unique contexts supported by
          the device. This is an additional error-avoidance mechanism
          to allow the administrators to have the ability to know the
          maximum number of contexts supported so that they can
          control the number of configuration contexts they install on
          the device. This attribute must have a non-zero value. The
          device should send the MAX value for Unsigned32 for this
          attribute if it not defined."
      DEFVAL { 4294967295 }

     ::= { frwkDeviceIdEntry 4 }

  --





  -- Component Limitations Table
  --

  frwkCompLimitsTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkCompLimitsEntry
      PIB-ACCESS     notify
      STATUS         current
      DESCRIPTION
          "This PRC supports the ability to export information
          detailing PRC/attribute implementation limitations to the
          policy management system. Instances of this PRC apply only
          for PRCs with access type 'install' or 'install-notify'.

          Each instance of this PRC identifies a PRovisioning Class
          or attribute and a limitation related to the implementation
          of the class/attribute in the device. Additional information
          providing guidance related to the limitation may also be
          present. These PRIs are sent to the PDP to indicate which
          PRCs or PRC attributes the device supports in a restricted
          manner."

      ::= { frwkBasePibClasses 4 }

  frwkCompLimitsEntry OBJECT-TYPE
      SYNTAX         FrwkCompLimitsEntry
      STATUS         current
      DESCRIPTION
          "An instance of the frwkCompLimits class that identifies
          a PRC or PRC attribute and a limitation related to the PRC
          or PRC attribute implementation supported by the device.
          COPS-PR lists the error codes that MUST be returned (if
          applicable)for policy installation that don't abide by the
          restrictions indicated by the limitations exported. [SPPI]
          defines an INSTALL-ERRORS clause that allows PIB designers
          to define PRC specific error codes that can be returned for
          policy installation. This allows efficient debugging of PIB
          implementations."
      REFERENCE
          "COPS Usage for Policy Provisioning. RFC 3084."

      PIB-INDEX { frwkCompLimitsPrid }
      UNIQUENESS { frwkCompLimitsComponent,
                   frwkCompLimitsAttrPos,
                   frwkCompLimitsNegation,
                   frwkCompLimitsType,
                   frwkCompLimitsSubType,
                   frwkCompLimitsGuidance }






      ::= { frwkCompLimitsTable 1 }

  FrwkCompLimitsEntry ::= SEQUENCE {
          frwkCompLimitsPrid           InstanceId,
          frwkCompLimitsComponent      PrcIdentifierOid,
          frwkCompLimitsAttrPos        AttrIdentifierOrZero,
          frwkCompLimitsNegation       TruthValue,
          frwkCompLimitsType           INTEGER,
          frwkCompLimitsSubType        INTEGER,
          frwkCompLimitsGuidance       OCTET STRING
  }

  frwkCompLimitsPrid OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "An arbitrary integer index that uniquely identifies an
          instance of the frwkCompLimits class."

      ::= { frwkCompLimitsEntry 1 }

  frwkCompLimitsComponent OBJECT-TYPE
      SYNTAX         PrcIdentifierOid
      STATUS         current
      DESCRIPTION
          "The value is the OID of a PRC (the table entry) which is
          supported in some limited fashion or contains an attribute
          that is supported in some limited fashion with regard to
          it's definition in the associated PIB module. The same OID
          may appear in the table several times, once for each
          implementation limitation acknowledged by the device."

      ::= { frwkCompLimitsEntry 2 }

  frwkCompLimitsAttrPos OBJECT-TYPE
      SYNTAX         AttrIdentifierOrZero
      STATUS         current
      DESCRIPTION
          "The relative position of the attribute within the PRC
          specified by the frwkCompLimitsComponent. A value of 1 would
          represent the first columnar object in the PRC and a value
          of N would represent the Nth columnar object in the PRC. A
          value of zero (0) indicates that the limit applies to the
          PRC itself and not to a specific attribute."

      ::= { frwkCompLimitsEntry 3 }







  frwkCompLimitsNegation OBJECT-TYPE
      SYNTAX        TruthValue
      STATUS        current
      DESCRIPTION
           "A boolean value ,if 'true', negates the component limit
           exported."

      ::= { frwkCompLimitsEntry 4 }

  frwkCompLimitsType OBJECT-TYPE
      SYNTAX    INTEGER {
                           priSpaceLimited(1),
                           attrValueSupLimited(2),
                           attrEnumSupLimited(3),
                           attrLengthLimited(4),
                           prcLimitedNotify(5)
                        }
      STATUS   current
      DESCRIPTION
          "A value describing an implementation limitation for the
          device related to the PRC or PRC attribute identified by
          the frwkCompLimitsComponent and the frwkCompLimitsAttrPos
          attributes.

          Values for this object are one of the following:

          priSpaceLimited(1) - No more instances than that specified
          by the guidance value may be installed in the given class.
          The component identified MUST be a valid PRC. The SubType
          used MUST be valueOnly(9).

          attrValueSupLimited(2) - Limited values are acceptable for
          the identified component. The component identified MUST be a
          valid PRC attribute. The guidance OCTET STRING will be
          decoded according to the attribute type.

          attrEnumSupLimited(3) - Limited enumeration values are legal
          for the identified component. The attribute identified MUST
          be a valid enum type.

          attrLengthLimited(4) - The length of the specified
          value for the identified component is limited. The component
          identified MUST be a valid PRC attribute of base-type OCTET
          STRING.

          prcLimitedNotify (5) - The component is currently limited
          for use by request or report messages prohibiting decision
          installation. The component identified must be a valid PRC."





      ::= { frwkCompLimitsEntry 5 }

     frwkCompLimitsSubType OBJECT-TYPE
      SYNTAX         INTEGER {
                                  none(1),
                                  lengthMin(2),
                                  lengthMax(3),
                                  rangeMin(4),
                                  rangeMax(5),
                                  enumMin(6),
                                  enumMax(7),
                                  enumOnly(8),
                                  valueOnly(9),
                                  bitMask(10)
                              }
      STATUS         current
      DESCRIPTION
          "This object indicates the type of guidance related
          to the noted limitation (as indicated by the
          frwkCompLimitsType attribute) that is provided
          in the frwkCompLimitsGuidance attribute.

          A value of 'none(1)' means that no additional
          guidance is provided for the noted limitation type.

          A value of 'lengthMin(2)' means that the guidance
          attribute provides data related to the minimum
          acceptable length for the value of the identified
          component. A corresponding class instance
          specifying the 'lengthMax(3)' value is required
          in conjunction with this sub-type.

          A value of 'lengthMax(3)' means that the guidance
          attribute provides data related to the maximum
          acceptable length for the value of the identified
          component. A corresponding class instance
          specifying the 'lengthMin(2)' value is required
          in conjunction with this sub-type.

          A value of 'rangeMin(4)' means that the guidance
          attribute provides data related to the lower bound
          of the range for the value of the identified
          component. A corresponding class instance
          specifying the 'rangeMax(5)' value is required
          in conjunction with this sub-type.

          A value of 'rangeMax(5)' means that the guidance
          attribute provides data related to the upper bound





          of the range for the value of the identified
          component. A corresponding class instance
          specifying the 'rangeMin(4)' value is required
          in conjunction with this sub-type.

          A value of 'enumMin(6)' means that the guidance
          attribute provides data related to the lowest
          enumeration acceptable for the value of the
          identified component. A corresponding
          class instance specifying the 'enumMax(7)'
          value is required in conjunction with this sub-type.

          A value of 'enumMax(7)' means that the guidance
          attribute provides data related to the largest
          enumeration acceptable for the value of the
          identified component. A corresponding
          class instance specifying the 'enumMin(6)'
          value is required in conjunction with this sub-type.

          A value of 'enumOnly(8)' means that the guidance
          attribute provides data related to a single
          enumeration acceptable for the value of the
          identified component.

          A value of 'valueOnly(9)' means that the guidance
          attribute provides data related to a single
          value that is acceptable for the identified
          component.

          A value of 'bitMask(10)' means that the guidance
          attribute is a bit mask such that all the combinations of
          bits set in the bitmask are acceptable values for the
          identified component which should be an attribute of type

          'BITS'.

          For example, an implementation of the frwkIpFilter class may
          be limited in several ways, such as address mask, protocol
          and Layer 4 port options. These limitations could be
          exported using this PRC with the following instances:

          Component        Type                 Sub-Type   Guidance
          ------------------------------------------------------------
          DstPrefixLength  attrValueSupLimited  valueOnly   24
          SrcPrefixLength  attrValueSupLimited  valueOnly   24
          Protocol         attrValueSupLimited  rangeMin    10
          Protocol         attrValueSupLimited  rangeMax    20






          The above entries describe a number of limitations that
          may be in effect for the frwkIpFilter class on a given
          device. The limitations include restrictions on acceptable
          values for certain attributes.

          Also, an implementation of a PRC may be limited in the ways
          it can be accessed. For instance, for a fictitious PRC
          dscpMapEntry, which has a PIB-ACCESS of 'install-notify':

          Component    Type              SubType  Guidance
          ------------------------------------------------------------
          dscpMapEntry prcLimitedNotify  none     zero-length string."

         ::= { frwkCompLimitsEntry 6 }

   frwkCompLimitsGuidance OBJECT-TYPE
         SYNTAX         OCTET STRING
         STATUS         current
         DESCRIPTION
             "A value used to convey additional information related
             to the implementation limitation. Note that a guidance
             value will not necessarily be provided for all exported
             limitations. If a guidance value is not provided, the
             value must be a zero-length string.

             The format of the guidance value, if one is present as
             indicated by the frwkCompLimitsSubType attribute,
             is described by the following table. Note that the
             format of guidance value is dictated by the base-type of
             the component whose limitation is being exported,
             interpreted in the context of the frwkCompLimitsType and
             frwkCompLimitsSubType values. Any other restrictions
             (such as size/range/enumerated value) on the guidance
             value MUST be complied with according to the definition
             of the component for which guidance is being specified.

             Note that numbers are encoded in network byte order.

             Base Type                      Value
             ---------                      -----
             Unsigned32/Integer32/INTEGER   32-bit value.
             Unsigned64/Integer64        64-bit Value.
             OCTET STRING                octets of data.
             OID                         32-bit OID components.
             BITS                        Binary octets of length
                                         same as Component specified."

         ::= { frwkCompLimitsEntry 7 }





  --
  -- Complete Reference specification table
  --

  frwkReferenceTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkReferenceEntry
      PIB-ACCESS     install-notify
      STATUS         current
      DESCRIPTION
          "Each instance of this PRC specifies a reference to a PRI
          in a specific PIB context (handle) for a specific client-
          type. This table gives the PDP the ability to set up
          policies that span installed contexts and the PEP the
          ability to reference instances in another, perhaps
          configured context. The PEP must send a
          'attrReferenceUnknown' COPS-PR error to the PDP if it
          encounters an invalid reference. "
      REFERENCE
          "COPS Usage for Policy Provisioning. RFC 3084, error
          codes section 4.5."

      ::= { frwkBasePibClasses 5 }

  frwkReferenceEntry OBJECT-TYPE
      SYNTAX         FrwkReferenceEntry
      STATUS         current
      DESCRIPTION
          "Entry specification for the frwkReferenceTable."

      PIB-INDEX { frwkReferencePrid }
      UNIQUENESS { }

      ::= { frwkReferenceTable 1 }

  FrwkReferenceEntry ::= SEQUENCE {
          frwkReferencePrid           InstanceId,
          frwkReferenceClientType     ClientType,
          frwkReferenceClientHandle   ClientHandle,
          frwkReferenceInstance       Prid
  }

  frwkReferencePrid  OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "An arbitrary integer index that uniquely identifies an
          instance of the frwkReference class."






      ::= { frwkReferenceEntry 1 }

  frwkReferenceClientType OBJECT-TYPE
      SYNTAX         ClientType
      STATUS         current
      DESCRIPTION
          "Is unused if set to zero else specifies a client-type for
           which the reference is to be interpreted. This non-zero
           client-type must be activated explicitly via a separate
           COPS client-open else this attribute is not valid."

      ::= { frwkReferenceEntry 2 }

  frwkReferenceClientHandle OBJECT-TYPE
      SYNTAX         ClientHandle
      STATUS         current
      DESCRIPTION
          "Must be set to specify a valid client-handle in the scope
          of the client-type specified."

      ::= { frwkReferenceEntry 3 }

  frwkReferenceInstance OBJECT-TYPE
      SYNTAX         Prid
      STATUS         current
      DESCRIPTION
          "References a PRI in the context identified by
           frwkReferenceClientHandle for client-type identified by
           frwkReferenceClientType."

      ::= { frwkReferenceEntry 4 }

  --
  -- Error specification table
  --

  frwkErrorTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkErrorEntry
      PIB-ACCESS     install
      STATUS         current
      DESCRIPTION
          "Each instance of this PRC specifies a class specific
          error object. Instances of this PRC are transient, i.e.,
          instances received in a COPS decision message must not be
          maintained by the PEP in its copy of the PIB instances. This
          PRC allows a PDP to send error information to the PEP if the
          PDP cannot process updates to a Request successfully."






      ::= { frwkBasePibClasses 6 }

  frwkErrorEntry OBJECT-TYPE
      SYNTAX         FrwkErrorEntry
      STATUS         current
      DESCRIPTION
          "Entry specification for the frwkErrorTable."

      PIB-INDEX { frwkErrorPrid }
      UNIQUENESS {
                   frwkErrorCode,
                   frwkErrorSubCode,
                   frwkErrorPrc,
                   frwkErrorInstance
                 }

      ::= { frwkErrorTable 1 }

  FrwkErrorEntry ::= SEQUENCE {
          frwkErrorPrid        InstanceId,
          frwkErrorCode        Unsigned32,
          frwkErrorSubCode     Unsigned32,
          frwkErrorPrc         PrcIdentifierOid,
          frwkErrorInstance    InstanceId
  }

  frwkErrorPrid  OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "An arbitrary integer index that uniquely identifies an
          instance of the frwkError class."

      ::= { frwkErrorEntry 1 }

  frwkErrorCode OBJECT-TYPE
      SYNTAX         Unsigned32 (0..65535)
      STATUS         current
      DESCRIPTION
          "Error code defined in COPS-PR CPERR object."
      REFERENCE
          "COPS Usage for Policy Provisioning. RFC 3084."

      ::= { frwkErrorEntry 2 }

  frwkErrorSubCode OBJECT-TYPE
      SYNTAX         Unsigned32 (0..65535)
      STATUS         current





      DESCRIPTION
          "The class-specific error object is used to communicate
          errors relating to specific PRCs."

      ::= { frwkErrorEntry 3 }

  frwkErrorPrc OBJECT-TYPE
      SYNTAX         PrcIdentifierOid
      STATUS         current
      DESCRIPTION
          "The PRC due to which the error specified by codes
          (frwkErrorCode , frwkErrorSubCode) occurred."

      ::= { frwkErrorEntry 4 }

  frwkErrorInstance OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "The PRI of the identified PRC (frwkErrorPrc) due to which
          the error specified by codes (frwkErrorCode ,
          frwkErrorSubCode) occurred. Must be set to zero if unused."

      ::= { frwkErrorEntry 5 }

  --
  -- The device capabilities and role combo classes group
  --

  frwkDeviceCapClasses
              OBJECT IDENTIFIER ::= { frameworkPib 2 }
  --
  -- Capability Set Table
  --

  frwkCapabilitySetTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkCapabilitySetEntry
      PIB-ACCESS     notify
      STATUS         current
      DESCRIPTION

          "This PRC describes the capability sets that exist on the
          interfaces on the device. The capability set is given a
          unique name that identifies a set. These capability set
          names are used by the PDP to determine policy information to
          be associated with interfaces that possess similar sets of
          capabilities."






      ::= { frwkDeviceCapClasses 1 }

  frwkCapabilitySetEntry OBJECT-TYPE
      SYNTAX         FrwkCapabilitySetEntry
      STATUS         current
      DESCRIPTION
          "An instance of this PRC describes a particular set of
          capabilities and associates a unique name with the set."

      PIB-INDEX { frwkCapabilitySetPrid }
      UNIQUENESS { frwkCapabilitySetName,
                   frwkCapabilitySetCapability }

      ::= { frwkCapabilitySetTable 1 }

  FrwkCapabilitySetEntry ::= SEQUENCE {
          frwkCapabilitySetPrid           InstanceId,
          frwkCapabilitySetName           SnmpAdminString,
          frwkCapabilitySetCapability     Prid
  }

  frwkCapabilitySetPrid OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "An arbitrary integer index that uniquely identifies a
          instance of the class."

      ::= { frwkCapabilitySetEntry 1 }

  frwkCapabilitySetName OBJECT-TYPE
      SYNTAX         SnmpAdminString (SIZE (1..255))
      STATUS         current
      DESCRIPTION
          "The name for the capability set.  This name  is the unique
          identifier of a set of capabilities. This attribute must not
          be assigned a zero-length string."

      ::= { frwkCapabilitySetEntry 2 }

  frwkCapabilitySetCapability OBJECT-TYPE
      SYNTAX      Prid
      STATUS      current
      DESCRIPTION

          "The complete PRC OID and instance identifier specifying the
          capability PRC instance for the interface. This attribute
          references a specific instance of a capability table. The





          capability table whose instance is referenced must be
          defined in the client type specific PIB that this PIB is
          used with. The referenced capability instance becomes a part
          of the set of capabilities associated with the specified
          frwkCapabilitySetName."

      ::= { frwkCapabilitySetEntry 3 }

  --
  -- Interface and Role Combination Tables
  --

  frwkRoleComboTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkRoleComboEntry
      PIB-ACCESS     install-notify
      STATUS         current
      DESCRIPTION
          "This is an abstract PRC that may be extended or referenced
          to enumerate the role combinations, capability set names
          assigned to any interface on a PEP. The identification of
          the interface is to be defined by its extensions or
          referencing PRCs."

      ::= { frwkDeviceCapClasses 2 }

  frwkRoleComboEntry OBJECT-TYPE
      SYNTAX         FrwkRoleComboEntry
      STATUS         current
      DESCRIPTION
          "An instance of this PRC describes one association of an
          interface to a role-combination and capability set name .
          Note that an interface can have multiple associations. This
          constraint is controlled by the extending or referencing
          PRC's uniqueness clause."

      PIB-INDEX { frwkRoleComboPrid }
      UNIQUENESS { }

      ::= { frwkRoleComboTable 1 }

  FrwkRoleComboEntry ::= SEQUENCE {
          frwkRoleComboPrid         InstanceId,
          frwkRoleComboRoles        RoleCombination,
          frwkRoleComboCapSetName   SnmpAdminString
  }

  frwkRoleComboPrid OBJECT-TYPE
      SYNTAX         InstanceId





      STATUS         current
      DESCRIPTION
          "An arbitrary integer index that uniquely identifies an
          instance of the class."

      ::= { frwkRoleComboEntry 1 }

  frwkRoleComboRoles OBJECT-TYPE
      SYNTAX         RoleCombination
      STATUS         current
      DESCRIPTION
          "The role combination assigned to a specific interface."

      ::= { frwkRoleComboEntry 2 }

  frwkRoleComboCapSetName OBJECT-TYPE
      SYNTAX         SnmpAdminString (SIZE (0..255))
      STATUS         current
      DESCRIPTION
          "The name of the capability set associated with
          the Role Combination specified in frwkRoleComboRoles. If
          this is a zero length string it implies the PEP is not
          exporting any capability set information for this
          RoleCombination. The PDP must then use the RoleCombinations
          provided as the only means of assigning policies
          If a non-zero length string is specified, the name must
          exist in frwkCapabilitySetTable."

      ::= { frwkRoleComboEntry 3 }

  --
  -- Interface, Role Combination association via IfIndex
  --

  frwkIfRoleComboTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkIfRoleComboEntry
      PIB-ACCESS     install-notify
      STATUS         current
      DESCRIPTION
          "This PRC enumerates the interface to role combination and
          frwkRoleComboCapSetName mapping for all policy managed
          interfaces of a device. Policy for an interface depends not
          only on the capability set of an interface but also on its
          roles. This  table specifies all the <interface index,
          interface capability set name, role combination> tuples
          currently on the device"

      ::= { frwkDeviceCapClasses 3 }





  frwkIfRoleComboEntry OBJECT-TYPE
      SYNTAX         FrwkIfRoleComboEntry
      STATUS         current
      DESCRIPTION
          "An instance of this PRC describes the association of
          a interface to an capability set name and a role
          combination.
          Note that a capability set name can have multiple role
          combinations assigned to it, but an IfIndex can have only
          one role combination associated."

      EXTENDS { frwkRoleComboEntry }
      UNIQUENESS { frwkIfRoleComboIfIndex,
                   frwkRoleComboCapSetName   }

      ::= { frwkIfRoleComboTable 1 }

  FrwkIfRoleComboEntry ::= SEQUENCE {
          frwkIfRoleComboIfIndex      InterfaceIndex
  }

  frwkIfRoleComboIfIndex OBJECT-TYPE
      SYNTAX         InterfaceIndex
      STATUS         current
      DESCRIPTION
          "The value of this attribute is the ifIndex which is
          associated with the specified RoleCombination and interface
          capability set name."

      ::= { frwkIfRoleComboEntry 1 }

  --
  -- The Classification classes group
  --

  frwkClassifierClasses
             OBJECT IDENTIFIER ::= { frameworkPib 3 }
  --
  -- The Base Filter Table
  --

  frwkBaseFilterTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkBaseFilterEntry
      PIB-ACCESS     install
      STATUS         current








      DESCRIPTION
          "The Base Filter class.  A packet has to match all
          fields in an Filter.  Wildcards may be specified for those
          fields that are not relevant."

      ::= { frwkClassifierClasses 1 }

  frwkBaseFilterEntry OBJECT-TYPE
      SYNTAX         FrwkBaseFilterEntry
      STATUS         current
      DESCRIPTION
          "An instance of the frwkBaseFilter class."

      PIB-INDEX { frwkBaseFilterPrid }

      ::= { frwkBaseFilterTable 1 }

  FrwkBaseFilterEntry ::= SEQUENCE {
          frwkBaseFilterPrid         InstanceId,
          frwkBaseFilterNegation     TruthValue
  }

  frwkBaseFilterPrid OBJECT-TYPE
      SYNTAX         InstanceId
      STATUS         current
      DESCRIPTION
          "An integer index to uniquely identify this Filter among all
          the Filters."

      ::= { frwkBaseFilterEntry 1 }

  frwkBaseFilterNegation OBJECT-TYPE
      SYNTAX         TruthValue
      STATUS         current
      DESCRIPTION
          "This attribute behaves like a logical NOT for the filter.
          If the packet matches this filter and the value of this
          attribute is 'true', the action associated with this filter
          is not applied to the packet.  If the value of this
          attribute is 'false', then the action is applied to the
          packet."

      ::= { frwkBaseFilterEntry 2 }

  --
  -- The IP Filter Table
  --






  frwkIpFilterTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF FrwkIpFilterEntry
      PIB-ACCESS     install
      STATUS         current
      DESCRIPTION
          "Filter definitions.  A packet has to match all fields in a
          filter.  Wildcards may be specified for those fields that
          are not relevant."

      INSTALL-ERRORS {
          invalidDstL4PortData(1),
          invalidSrcL4PortData(2)
          }
      ::= { frwkClassifierClasses 2 }

  frwkIpFilterEntry OBJECT-TYPE
      SYNTAX         FrwkIpFilterEntry
      STATUS         current
      DESCRIPTION
          "An instance of the frwkIpFilter class."

      EXTENDS { frwkBaseFilterEntry }
      UNIQUENESS { frwkBaseFilterNegation,
                   frwkIpFilterAddrType,
                   frwkIpFilterDstAddr,
                   frwkIpFilterDstPrefixLength,
                   frwkIpFilterSrcAddr,
                   frwkIpFilterSrcPrefixLength,
                   frwkIpFilterDscp,
                   frwkIpFilterFlowId,
                   frwkIpFilterProtocol,
                   frwkIpFilterDstL4PortMin,
                   frwkIpFilterDstL4PortMax,
                   frwkIpFilterSrcL4PortMin,
                   frwkIpFilterSrcL4PortMax }

      ::= { frwkIpFilterTable 1 }

  FrwkIpFilterEntry ::= SEQUENCE {
          frwkIpFilterAddrType         InetAddressType,
          frwkIpFilterDstAddr          InetAddress,
          frwkIpFilterDstPrefixLength  InetAddressPrefixLength,
          frwkIpFilterSrcAddr          InetAddress,
          frwkIpFilterSrcPrefixLength  InetAddressPrefixLength,
          frwkIpFilterDscp             DscpOrAny,
          frwkIpFilterFlowId           Integer32,
          frwkIpFilterProtocol         Unsigned32,
          frwkIpFilterDstL4PortMin     InetPortNumber,





          frwkIpFilterDstL4PortMax     InetPortNumber,
          frwkIpFilterSrcL4PortMin     InetPortNumber,
          frwkIpFilterSrcL4PortMax     InetPortNumber
  }

  frwkIpFilterAddrType OBJECT-TYPE

      SYNTAX         InetAddressType
      STATUS         current
      DESCRIPTION
          "The address type enumeration value to specify the type of
          the packet's IP address.

          While other types of addresses are defined in the
          InetAddressType textual convention, an IP filter can only
          use IPv4 and IPv6 addresses directly to classify traffic.
          All other InetAddressTypes require mapping to the
          corresponding Ipv4 or IPv6 address before being used to
          classify traffic. Therefore, this object as such is not
          limited to IPv4 and IPv6 addresses, i.e., it can be assigned
          any of the valid values defined in the InetAddressType TC,
          but the mapping of the address values to IPv4 or IPv6
          addresses for the address attributes (frwkIpFilterDstAddr
          and frwkIpFilterSrcAddr) must be done by the PEP. For
          example when dns (16) is used, the PEP must resolve
          the address to IPv4 or IPv6 at install time."
      REFERENCE
          "Textual Conventions for Internet Network Addresses.
          RFC 3291."

      ::= { frwkIpFilterEntry 1 }

  frwkIpFilterDstAddr OBJECT-TYPE

      SYNTAX         InetAddress
      STATUS         current
      DESCRIPTION
          "The IP address to match against the packet's
           destination IP address. If the address type is 'ipv4',
           'ipv6', 'ipv4z' or 'ipv6z' then, the attribute
           frwkIpFilterDstPrefixLength indicates the number of bits
           that are relevant. "
      REFERENCE
          "Textual Conventions for Internet Network Addresses.
          RFC 3291."

      ::= { frwkIpFilterEntry 2 }






  frwkIpFilterDstPrefixLength OBJECT-TYPE
      SYNTAX         InetAddressPrefixLength
      STATUS         current
      DESCRIPTION
          "The length of a mask for the matching of the destination
           IP address. This attribute is interpreted only if the
           InetAddressType is 'ipv4', 'ipv4z', 'ipv6' or 'ipv6z'.
           Masks are constructed by setting bits in sequence from the
           most-significant bit downwards for
           frwkIpFilterDstPrefixLength bits length. All other bits in
           the mask, up to the  number needed to fill the length of
           the address frwkIpFilterDstAddr are cleared to zero. A zero
           bit in the mask then means that the corresponding bit in
           the address always matches.

           In IPv4 addresses, a length of 0 indicates a match of any
           address; a length of 32 indicates a match of a single host
           address, and a length between 0 and 32 indicates the use of
           a CIDR Prefix. IPv6 is similar, except that prefix lengths
           range from 0..128."
      REFERENCE
          "Textual Conventions for Internet Network Addresses.
          RFC 3291."
      DEFVAL { 0 }

      ::= { frwkIpFilterEntry 3 }

  frwkIpFilterSrcAddr OBJECT-TYPE
      SYNTAX         InetAddress
      STATUS         current
      DESCRIPTION
          "The IP address to match against the packet's source IP
          address. If the address type is 'ipv4', 'ipv6', 'ipv4z' or
          'ipv6z' then, the attribute frwkIpFilterSrcPrefixLength
          indicates the number of bits that are relevant."
      REFERENCE
          "Textual Conventions for Internet Network Addresses.
          RFC 3291."

      ::= { frwkIpFilterEntry 4 }

  frwkIpFilterSrcPrefixLength OBJECT-TYPE
      SYNTAX         InetAddressPrefixLength
      UNITS          "bits"
      STATUS         current
      DESCRIPTION
          "The length of a mask for the matching of the source IP
           address. This attribute is interpreted only if the





           InetAddressType is 'ipv4', 'ipv4z', 'ipv6' or 'ipv6z'.
           Masks are constructed by setting bits in sequence from the
           most-significant bit downwards for
           frwkIpFilterSrcPrefixLength bits length. All other bits in
           the mask, up to the  number needed to fill the length of
           the address frwkIpFilterSrcAddr are cleared to zero.  A
           zero bit in the mask then means that the corresponding bit
           in the address always matches.

           In IPv4 addresses, a length of 0 indicates a match of any
           address; a length of 32 indicates a match of a single host
           address, and a length between 0 and 32 indicates the use of
           a CIDR Prefix. IPv6 is similar, except that prefix lengths
           range from 0..128."
      REFERENCE
          "Textual Conventions for Internet Network Addresses.
          RFC 3291."
      DEFVAL { 0 }

      ::= { frwkIpFilterEntry 5 }

  frwkIpFilterDscp OBJECT-TYPE
      SYNTAX         DscpOrAny
      STATUS         current
      DESCRIPTION
          "The value that the DSCP in the packet can have and
           match this filter. A value of -1 indicates that a specific
           DSCP value has not been defined and thus all DSCP values
           are considered a match."
      REFERENCE
          "Management Information Base for the Differentiated Services
           Architecture. RFC 3289."
      DEFVAL { -1 }

      ::= { frwkIpFilterEntry 6 }

  frwkIpFilterFlowId OBJECT-TYPE
      SYNTAX        Integer32 (-1 | 0..1048575)
      STATUS         current
      DESCRIPTION
          "The flow label or flow identifier in an IPv6 header
           that may be used to discriminate traffic flows.
           The value of -1 for this attribute MUST imply that
           any flow label value in the IPv6 header will match,
           resulting in the flow label field of the IPv6 header
           being ignored for matching this filter entry."

      ::= { frwkIpFilterEntry 7 }






  frwkIpFilterProtocol OBJECT-TYPE
      SYNTAX         Unsigned32 (0..255)
      STATUS         current
      DESCRIPTION
          "The layer-4 protocol Id to match against the IPv4 protocol
          number or the IPv6 Next-Header number in the packet. A value
          of 255 means match all. Note the protocol number of 255 is
          reserved by IANA, and Next-Header number of 0 is used in
          IPv6."
      DEFVAL { 255 }

      ::= { frwkIpFilterEntry 8 }

  frwkIpFilterDstL4PortMin OBJECT-TYPE
      SYNTAX         InetPortNumber
      STATUS         current
      DESCRIPTION
          "The minimum value that the packet's layer 4 destination
          port number can have and match this filter. This value must
          be equal to or lesser that the value specified for this
          filter in frwkIpFilterDstL4PortMax.

          COPS-PR error code 'attrValueInvalid' must be returned if
          the frwkIpFilterSrcL4PortMin is greater than
          frwkIpFilterSrcL4PortMax"
      REFERENCE
          "COPS Usage for Policy Provisioning.  RFC 3084, error
          codes section 4.5."
      DEFVAL { 0 }

     ::= { frwkIpFilterEntry 9 }

  frwkIpFilterDstL4PortMax OBJECT-TYPE
      SYNTAX         InetPortNumber
      STATUS         current
      DESCRIPTION
          "The maximum value that the packet's layer 4 destination
          port number can have and match this filter. This value must
          be equal to or greater that the value specified for this
          filter in frwkIpFilterDstL4PortMin.

          COPS-PR error code 'attrValueInvalid' must be returned if
          the frwkIpFilterDstL4PortMax is less than
          frwkIpFilterDstL4PortMin"
      REFERENCE
          "COPS Usage for Policy Provisioning.  RFC 3084, error
          codes section 4.5."





      DEFVAL { 65535 }

      ::= { frwkIpFilterEntry 10 }

  frwkIpFilterSrcL4PortMin OBJECT-TYPE
      SYNTAX         InetPortNumber
      STATUS         current
      DESCRIPTION
          "The minimum value that the packet's layer 4 source port
          number can have and match this filter. This value must
          be equal to or lesser that the value specified for this
          filter in frwkIpFilterSrcL4PortMax.

          COPS-PR error code 'attrValueInvalid' must be returned if
          the frwkIpFilterSrcL4PortMin is greated than
          frwkIpFilterSrcL4PortMax"
      REFERENCE
          "COPS Usage for Policy Provisioning.  RFC 3084, error
          codes section 4.5."
      DEFVAL { 0 }

      ::= { frwkIpFilterEntry 11 }

  frwkIpFilterSrcL4PortMax OBJECT-TYPE
      SYNTAX         InetPortNumber
      STATUS         current
      DESCRIPTION
          "The maximum value that the packet's layer 4 source port
          number can have and match this filter.  This value must be
          equal to or greater that the value specified for this filter
          in frwkIpFilterSrcL4PortMin.

          COPS-PR error code 'attrValueInvalid' must be returned if
          the frwkIpFilterSrcL4PortMax is less than
          frwkIpFilterSrcL4PortMin"
      REFERENCE
          "COPS Usage for Policy Provisioning.  RFC error codes
          section 4.5."
      DEFVAL { 65535 }

      ::= { frwkIpFilterEntry 12 }

  --
  -- The IEEE 802 Filter Table
  --

  frwk802FilterTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF Frwk802FilterEntry





      PIB-ACCESS     install
      STATUS         current
      DESCRIPTION
          "IEEE 802-based filter definitions. A class that contains
          attributes of IEEE 802 (e.g., 802.3) traffic that form
          filters that are used to perform traffic classification."
      REFERENCE
          "IEEE Standards for Local and Metropolitan Area Networks.
          Overview and Architecture, ANSI/IEEE Std 802, 1990."
      ::= { frwkClassifierClasses 3 }

  frwk802FilterEntry OBJECT-TYPE
      SYNTAX         Frwk802FilterEntry
      STATUS         current
      DESCRIPTION
          "IEEE 802-based filter definitions.  An entry specifies
          (potentially) several distinct matching components. Each
          component is tested against the data in a frame
          individually. An overall match occurs when all of the
          individual components match the data they are compared
          against in the frame being processed. A failure of any
          one test causes the overall match to fail.

          Wildcards may be specified for those fields that are not
          relevant."

      EXTENDS { frwkBaseFilterEntry }
      UNIQUENESS { frwkBaseFilterNegation,
                   frwk802FilterDstAddr,
                   frwk802FilterDstAddrMask,
                   frwk802FilterSrcAddr,
                   frwk802FilterSrcAddrMask,
                   frwk802FilterVlanId,
                   frwk802FilterVlanTagRequired,
                   frwk802FilterEtherType,
                   frwk802FilterUserPriority }

      ::= { frwk802FilterTable 1 }

  Frwk802FilterEntry ::= SEQUENCE {
          frwk802FilterDstAddr         PhysAddress,
          frwk802FilterDstAddrMask     PhysAddress,
          frwk802FilterSrcAddr         PhysAddress,
          frwk802FilterSrcAddrMask     PhysAddress,
          frwk802FilterVlanId          Integer32,
          frwk802FilterVlanTagRequired INTEGER,
          frwk802FilterEtherType       Integer32,
          frwk802FilterUserPriority    BITS





  }

  frwk802FilterDstAddr OBJECT-TYPE
      SYNTAX         PhysAddress
      STATUS         current
      DESCRIPTION
          "The 802 address against which the 802 DA of incoming
          traffic streams will be compared. Frames whose 802 DA
          matches the physical address specified by this object,
          taking into account address wildcarding as specified by the
          frwk802FilterDstAddrMask object, are potentially subject to
          the processing guidelines that are associated with this
          entry through the related action class."
      REFERENCE
          "Textual Conventions for SMIv2, RFC 2579."

      ::= { frwk802FilterEntry 1 }

  frwk802FilterDstAddrMask OBJECT-TYPE
      SYNTAX         PhysAddress
      STATUS         current
      DESCRIPTION
          "This object specifies the bits in a 802 destination address
          that should be considered when performing a 802 DA
          comparison against the address specified in the
          frwk802FilterDstAddr object.

          The value of this object represents a mask that is logically
          and'ed with the 802 DA in received frames to derive the
          value to be compared against the frwk802FilterDstAddr
          address. A zero bit in the mask thus means that the
          corresponding bit in the address always matches. The
          frwk802FilterDstAddr value must also be masked using this
          value prior to any comparisons.

          The length of this object in octets must equal the length in
          octets of the frwk802FilterDstAddr. Note that a mask with no
          bits set (i.e., all zeroes) effectively wildcards the
          frwk802FilterDstAddr object."

      ::= { frwk802FilterEntry 2 }

  frwk802FilterSrcAddr OBJECT-TYPE
      SYNTAX         PhysAddress
      STATUS         current
      DESCRIPTION
          "The 802 MAC address against which the 802 MAC SA of
          incoming traffic streams will be compared. Frames whose 802





          MAC SA matches the physical address specified by this
          object, taking into account address wildcarding as specified
          by the frwk802FilterSrcAddrMask object, are potentially
          subject to the processing guidelines that are associated
          with this entry through the related action class."

      ::= { frwk802FilterEntry 3 }

  frwk802FilterSrcAddrMask OBJECT-TYPE
      SYNTAX         PhysAddress
      STATUS         current
      DESCRIPTION
          "This object specifies the bits in a 802 MAC source address
          that should be considered when performing a 802 MAC SA
          comparison against the address specified in the
          frwk802FilterSrcAddr object.

          The value of this object represents a mask that is logically
          and'ed with the 802 MAC SA in received frames to derive the
          value to be compared against the frwk802FilterSrcAddr
          address. A zero bit in the mask thus means that the
          corresponding bit in the address always matches. The
          frwk802FilterSrcAddr value must also be masked using this
          value prior to any comparisons.

          The length of this object in octets must equal the length in
          octets of the frwk802FilterSrcAddr. Note that a mask with no
          bits set (i.e., all zeroes) effectively wildcards the
          frwk802FilterSrcAddr object."

      ::= { frwk802FilterEntry 4 }

  frwk802FilterVlanId OBJECT-TYPE
      SYNTAX         Integer32 (-1 | 1..4094)
      STATUS         current
      DESCRIPTION
          "The VLAN ID (VID) that uniquely identifies a VLAN
          within the device. This VLAN may be known or unknown
          (i.e., traffic associated with this VID has not yet
          been seen by the device) at the time this entry
          is instantiated.

          Setting the frwk802FilterVlanId object to -1 indicates that
          VLAN data should not be considered during traffic
          classification."

      ::= { frwk802FilterEntry 5 }






  frwk802FilterVlanTagRequired OBJECT-TYPE
      SYNTAX         INTEGER {
                         taggedOnly(1),
                         priorityTaggedPlus(2),
                         untaggedOnly(3),
                         ignoreTag(4)
                     }
      STATUS         current
      DESCRIPTION
          "This object indicates whether the presence of an
          IEEE 802.1Q VLAN tag in data link layer frames must
          be considered when determining if a given frame
          matches this 802 filter entry.

          A value of 'taggedOnly(1)' means that only frames
          containing a VLAN tag with a non-Null VID (i.e., a
          VID in the range 1..4094) will be considered a match.

          A value of 'priorityTaggedPlus(2)' means that only
          frames containing a VLAN tag, regardless of the value
          of the VID, will be considered a match.

          A value of 'untaggedOnly(3)' indicates that only
          untagged frames will match this filter component.

          The presence of a VLAN tag is not taken into
          consideration in terms of a match if the value is
          'ignoreTag(4)'."

      ::= { frwk802FilterEntry 6 }

  frwk802FilterEtherType OBJECT-TYPE
      SYNTAX         Integer32 (-1 | 0..'ffff'h)
      STATUS         current
      DESCRIPTION
          "This object specifies the value that will be compared
          against the value contained in the EtherType field of an
          IEEE 802 frame. Example settings would include 'IP'
          (0x0800), 'ARP' (0x0806) and 'IPX' (0x8137).

          Setting the frwk802FilterEtherTypeMin object to -1 indicates
          that EtherType data should not be considered during traffic
          classification.

          Note that the position of the EtherType field depends on
          the underlying frame format. For Ethernet-II encapsulation,
          the EtherType field follows the 802 MAC source address. For
          802.2 LLC/SNAP encapsulation, the EtherType value follows





          the Organization Code field in the 802.2 SNAP header. The
        value that is tested with regard to this filter component
        therefore depends on the data link layer frame format being
        used. If this 802 filter component is active when there is
        no EtherType field in a frame (e.g., 802.2 LLC), a match is
        implied."

    ::= { frwk802FilterEntry 7 }

frwk802FilterUserPriority OBJECT-TYPE
    SYNTAX         BITS {
                        matchPriority0(0),
                        matchPriority1(1),
                        matchPriority2(2),
                        matchPriority3(3),
                        matchPriority4(4),
                        matchPriority5(5),
                        matchPriority6(6),
                        matchPriority7(7)
                   }
    STATUS         current
    DESCRIPTION
        "The set of values, representing the potential range
        of user priority values, against which the value contained
        in the user priority field of a tagged 802.1 frame is
        compared. A test for equality is performed when determining
        if a match exists between the data in a data link layer
        frame and the value of this 802 filter component. Multiple
        values may be set at one time such that potentially several
        different user priority values may match this 802 filter
        component.

        Setting all of the bits that are associated with this
        object causes all user priority values to match this
        attribute. This essentially makes any comparisons
        with regard to user priority values unnecessary. Untagged
        frames are treated as an implicit match."

    ::= { frwk802FilterEntry 8 }

--
-- The Internal label filter extension
--

frwkILabelFilterTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF FrwkILabelFilterEntry
    PIB-ACCESS     install
    STATUS         current





    DESCRIPTION
        "Internal label filter Table. This PRC is used to achieve
         classification based on the internal flow label set by the
         PEP possibly after ingress classification to avoid
         re-classification at the egress interface on the same PEP."

    ::= { frwkClassifierClasses 4 }

frwkILabelFilterEntry OBJECT-TYPE
    SYNTAX         FrwkILabelFilterEntry
    STATUS         current
    DESCRIPTION
        "Internal label filter entry definition."

    EXTENDS { frwkBaseFilterEntry }
    UNIQUENESS { frwkBaseFilterNegation,
                 frwkILabelFilterILabel }

    ::= { frwkILabelFilterTable 1 }

FrwkILabelFilterEntry ::= SEQUENCE {
   frwkILabelFilterILabel      OCTET STRING
}

frwkILabelFilterILabel      OBJECT-TYPE
    SYNTAX       OCTET STRING
    STATUS       current
    DESCRIPTION
       "The Label that this flow uses for differentiating traffic
        flows.  The flow labeling is meant for network device
       internal usage. A value of zero length string matches all
       internal labels."
    ::= { frwkILabelFilterEntry 1 }

--
-- The Marker classes group
--

frwkMarkerClasses
           OBJECT IDENTIFIER ::= { frameworkPib 4 }
--
-- The 802 Marker Table
--

frwk802MarkerTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF Frwk802MarkerEntry
    PIB-ACCESS     install
    STATUS         current





    DESCRIPTION
        "The 802 Marker class. An 802 packet can be marked with the
         specified VLAN id, priority level."

    ::= { frwkMarkerClasses 1 }

frwk802MarkerEntry OBJECT-TYPE
    SYNTAX         Frwk802MarkerEntry
    STATUS         current
    DESCRIPTION
        "frwk802Marker entry definition."

    PIB-INDEX { frwk802MarkerPrid }
    UNIQUENESS { frwk802MarkerVlanId,
                 frwk802MarkerPriority }

    ::= { frwk802MarkerTable 1 }

Frwk802MarkerEntry::= SEQUENCE {
        frwk802MarkerPrid          InstanceId,
        frwk802MarkerVlanId        Unsigned32,
        frwk802MarkerPriority      Unsigned32
}

frwk802MarkerPrid  OBJECT-TYPE
    SYNTAX         InstanceId
    STATUS         current
    DESCRIPTION
        "An integer index to uniquely identify this 802 Marker."

    ::= { frwk802MarkerEntry 1 }

frwk802MarkerVlanId  OBJECT-TYPE
    SYNTAX         Unsigned32 (1..4094)
    STATUS         current
    DESCRIPTION
        "The VLAN ID (VID) that uniquely identifies a VLAN within
         the device."

    ::= { frwk802MarkerEntry 2 }

frwk802MarkerPriority  OBJECT-TYPE
    SYNTAX         Unsigned32 (0..7)
    STATUS         current
    DESCRIPTION
        "The user priority field of a tagged 802.1 frame."

    ::= { frwk802MarkerEntry 3 }






--
-- The Internal Label Marker Table
--

frwkILabelMarkerTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF FrwkILabelMarkerEntry
    PIB-ACCESS     install
    STATUS         current
    DESCRIPTION
        "The Internal Label Marker class. A flow in a PEP can be
        marked with an internal label using this PRC."

    ::= { frwkMarkerClasses 2 }

frwkILabelMarkerEntry OBJECT-TYPE
    SYNTAX         FrwkILabelMarkerEntry
    STATUS         current
    DESCRIPTION
        "frwkILabelkMarker entry definition."

    PIB-INDEX { frwkILabelMarkerPrid }
    UNIQUENESS { frwkILabelMarkerILabel }

    ::= { frwkILabelMarkerTable 1 }

FrwkILabelMarkerEntry::= SEQUENCE {
        frwkILabelMarkerPrid          InstanceId,
        frwkILabelMarkerILabel        OCTET STRING
}

frwkILabelMarkerPrid  OBJECT-TYPE
    SYNTAX         InstanceId
    STATUS         current
    DESCRIPTION
        "An integer index to uniquely identify this Label Marker."

    ::= { frwkILabelMarkerEntry 1 }

frwkILabelMarkerILabel  OBJECT-TYPE
    SYNTAX         OCTET STRING
    STATUS         current
    DESCRIPTION
        "This internal label is implementation specific and may be
         used for other policy related functions like flow
         accounting purposes and/or other data path treatments."

    ::= { frwkILabelMarkerEntry 2 }






--
-- Conformance Section
--

frwkBasePibConformance
                OBJECT IDENTIFIER ::= { frameworkPib 5 }

frwkBasePibCompliances
                OBJECT IDENTIFIER ::= { frwkBasePibConformance 1 }

frwkBasePibGroups
                OBJECT IDENTIFIER ::= { frwkBasePibConformance 2 }

frwkBasePibCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "Describes the requirements for conformance to the
            Framework PIB."

    MODULE  -- this module
        MANDATORY-GROUPS { frwkPrcSupportGroup,
                           frwkPibIncarnationGroup,
                           frwkDeviceIdGroup,
                           frwkCompLimitsGroup,
                           frwkCapabilitySetGroup,
                           frwkRoleComboGroup,
                           frwkIfRoleComboGroup }

        OBJECT          frwkPibIncarnationLongevity
        PIB-MIN-ACCESS  notify
        DESCRIPTION
           "Install support is required if policy expiration is to
           be supported."

        OBJECT          frwkPibIncarnationTtl
        PIB-MIN-ACCESS  notify
        DESCRIPTION
           "Install support is required if policy expiration is to
           be supported."

        OBJECT          frwkPibIncarnationInCtxtSet
        PIB-MIN-ACCESS  notify
        DESCRIPTION
           "Install support is required if configuration contexts
           and outsourcing contexts are both to be supported."

        OBJECT          frwkPibIncarnationFullState





        PIB-MIN-ACCESS  notify
        DESCRIPTION
            "Install support is required if incremental updates to
            request states is to be supported."

    GROUP   frwkReferenceGroup
        DESCRIPTION
            "The frwkReferenceGroup is mandatory if referencing
            across PIB contexts for specific client-types is to be
            supported."

    GROUP   frwkErrorGroup
        DESCRIPTION
            "The frwkErrorGroup is mandatory sending errors in
             decisions is to be supported."

    GROUP   frwkBaseFilterGroup
        DESCRIPTION
            "The frwkBaseFilterGroup is mandatory if filtering
             based on traffic components is to be supported."

    GROUP   frwkIpFilterGroup
        DESCRIPTION
            "The frwkIpFilterGroup is mandatory if filtering
             based on IP traffic components is to be supported."

    GROUP   frwk802FilterGroup
        DESCRIPTION
            "The frwk802FilterGroup is mandatory if filtering
            based on 802 traffic criteria is to be supported."

    GROUP   frwkILabelFilterGroup
        DESCRIPTION
            "The frwkILabelFilterGroup is mandatory if filtering
            based on PEP internal label is to be supported."

    GROUP   frwk802MarkerGroup
        DESCRIPTION
            "The frwk802MarkerGroup is mandatory if marking a packet
            with 802 traffic criteria is to be supported."

    GROUP   frwkILabelMarkerGroup
        DESCRIPTION
            "The frwkILabelMarkerGroup is mandatory if marking a
            flow with internal labels is to be supported."

    ::= { frwkBasePibCompliances 1 }






frwkPrcSupportGroup OBJECT-GROUP
    OBJECTS {
             frwkPrcSupportPrid,
             frwkPrcSupportSupportedPrc,
             frwkPrcSupportSupportedAttrs }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkPrcSupportTable."

    ::= { frwkBasePibGroups 1 }

frwkPibIncarnationGroup OBJECT-GROUP
    OBJECTS {
             frwkPibIncarnationPrid,
             frwkPibIncarnationName,
             frwkPibIncarnationId,
             frwkPibIncarnationLongevity,
             frwkPibIncarnationTtl,
             frwkPibIncarnationInCtxtSet,
             frwkPibIncarnationActive,
             frwkPibIncarnationFullState
            }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkDevicePibIncarnationTable."

    ::= { frwkBasePibGroups 2 }

frwkDeviceIdGroup OBJECT-GROUP
    OBJECTS {
             frwkDeviceIdPrid,
             frwkDeviceIdDescr,
             frwkDeviceIdMaxMsg,
             frwkDeviceIdMaxContexts }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkDeviceIdTable."

    ::= { frwkBasePibGroups 3 }

frwkCompLimitsGroup OBJECT-GROUP
    OBJECTS {
             frwkCompLimitsPrid,
             frwkCompLimitsComponent,
             frwkCompLimitsAttrPos,
             frwkCompLimitsNegation,
             frwkCompLimitsType,
             frwkCompLimitsSubType,





             frwkCompLimitsGuidance }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkCompLimitsTable."

    ::= { frwkBasePibGroups 4 }

frwkReferenceGroup OBJECT-GROUP
    OBJECTS {
             frwkReferencePrid,
             frwkReferenceClientType,
             frwkReferenceClientHandle,
             frwkReferenceInstance }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkReferenceTable."

    ::= { frwkBasePibGroups 5 }

frwkErrorGroup OBJECT-GROUP
    OBJECTS {
             frwkErrorPrid,
             frwkErrorCode,
             frwkErrorSubCode,
             frwkErrorPrc,
             frwkErrorInstance }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkErrorTable."

    ::= { frwkBasePibGroups 6 }

frwkCapabilitySetGroup OBJECT-GROUP
    OBJECTS {
             frwkCapabilitySetPrid,
             frwkCapabilitySetName,
             frwkCapabilitySetCapability }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkCapabilitySetTable."

    ::= { frwkBasePibGroups 7 }

frwkRoleComboGroup OBJECT-GROUP
    OBJECTS {
             frwkRoleComboPrid,
             frwkRoleComboRoles,
             frwkRoleComboCapSetName }





    STATUS  current
    DESCRIPTION
            "Objects from the frwkRoleComboTable."

    ::= { frwkBasePibGroups 8 }

frwkIfRoleComboGroup OBJECT-GROUP
    OBJECTS { frwkIfRoleComboIfIndex }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkIfRoleComboTable."

    ::= { frwkBasePibGroups 9 }

frwkBaseFilterGroup OBJECT-GROUP
    OBJECTS {
             frwkBaseFilterPrid,
             frwkBaseFilterNegation }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkBaseFilterTable."

    ::= { frwkBasePibGroups 10 }

frwkIpFilterGroup OBJECT-GROUP
    OBJECTS {
             frwkIpFilterAddrType,
             frwkIpFilterDstAddr,
             frwkIpFilterDstPrefixLength,
             frwkIpFilterSrcAddr,
             frwkIpFilterSrcPrefixLength,
             frwkIpFilterDscp,
             frwkIpFilterFlowId,
             frwkIpFilterProtocol,
             frwkIpFilterDstL4PortMin,
             frwkIpFilterDstL4PortMax,
             frwkIpFilterSrcL4PortMin,
             frwkIpFilterSrcL4PortMax }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkIpFilterTable."

    ::= { frwkBasePibGroups 11 }

frwk802FilterGroup OBJECT-GROUP
    OBJECTS {
             frwk802FilterDstAddr,
             frwk802FilterDstAddrMask,





             frwk802FilterSrcAddr,
             frwk802FilterSrcAddrMask,
             frwk802FilterVlanId,
             frwk802FilterVlanTagRequired,
             frwk802FilterEtherType,
             frwk802FilterUserPriority }
    STATUS  current
    DESCRIPTION
            "Objects from the frwk802FilterTable."

    ::= { frwkBasePibGroups 12 }

frwkILabelFilterGroup OBJECT-GROUP
    OBJECTS { frwkILabelFilterILabel }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkILabelFilterTable."

    ::= { frwkBasePibGroups 13 }

frwk802MarkerGroup OBJECT-GROUP
    OBJECTS {
             frwk802MarkerPrid,
             frwk802MarkerVlanId,
             frwk802MarkerPriority }
    STATUS  current
    DESCRIPTION
            "Objects from the frwk802MarkerTable."

    ::= { frwkBasePibGroups 14 }

frwkILabelMarkerGroup OBJECT-GROUP
    OBJECTS {
             frwkILabelMarkerPrid,
             frwkILabelMarkerILabel }
    STATUS  current
    DESCRIPTION
            "Objects from the frwkILabelMarkerTable."

    ::= { frwkBasePibGroups 15 }

END










