T11-FC-FSPF-MIB DEFINITIONS ::= BEGIN

--
-- For management of FSPF, the Fibre Channel routing protocol.
--

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
    Counter32, Integer32, Unsigned32, TimeTicks,
    Gauge32, mib-2                     FROM SNMPv2-SMI   -- [RFC2578]
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP                 FROM SNMPv2-CONF  -- [RFC2580]
    TEXTUAL-CONVENTION, RowStatus, StorageType,
    TruthValue                         FROM SNMPv2-TC    -- [RFC2579]
    ifIndex, InterfaceIndex            FROM IF-MIB       -- [RFC2863]
    fcmInstanceIndex, fcmSwitchIndex,
    FcDomainIdOrZero                   FROM FC-MGMT-MIB  -- [FC-MGMT]
    T11FabricIndex                     FROM T11-TC-MIB   -- [RFC4439]
    t11FamConfigDomainId
                       FROM T11-FC-FABRIC-ADDR-MGR-MIB;  -- [RFC4439]

t11FcFspfMIB MODULE-IDENTITY
    LAST-UPDATED "200608140000Z"
    ORGANIZATION "T11"
    CONTACT-INFO
                   "Claudio DeSanti
                    Cisco Systems, Inc.
                    170 West Tasman Drive
                    San Jose, CA 95134 USA
                    EMail: cds@cisco.com






                    Keith McCloghrie
                    Cisco Systems, Inc.
                    170 West Tasman Drive
                    San Jose, CA USA 95134
                    Email: kzm@cisco.com"
    DESCRIPTION
           "The MIB module for managing the Fabric Shortest Path
           First (FSPF) protocol.  FSPF is specified in FC-SW-4.

           Copyright (C) The Internet Society (2006).  This version of
           this MIB module is part of RFC 4626;  see the RFC itself for
           full legal notices."
    REVISION   "200608140000Z"
    DESCRIPTION
           "Initial version of this MIB module published as RFC4626."

    ::= { mib-2 143 }

t11FspfNotifications      OBJECT IDENTIFIER ::= { t11FcFspfMIB 0 }
t11FspfObjects            OBJECT IDENTIFIER ::= { t11FcFspfMIB 1 }
t11FspfConformance        OBJECT IDENTIFIER ::= { t11FcFspfMIB 2 }
t11FspfConfiguration      OBJECT IDENTIFIER ::= { t11FspfObjects 1 }
t11FspfDatabase           OBJECT IDENTIFIER ::= { t11FspfObjects 2 }

--
-- TEXTUAL CONVENTIONS

T11FspfLsrType ::= TEXTUAL-CONVENTION
    STATUS    current
    DESCRIPTION
           "Type of the Link State Record.

           FC-SW-4 defines two types of LSRs and allows for the
           possibility for more will be defined in the future:

               01      - Switch Link Record
               02      - Obsolete
               240 - 255 - Vendor Specific
               others  - Reserved.
           "
    REFERENCE
           "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
            ANSI INCITS 418-2006, section 6.1.9.3."
    SYNTAX    Integer32 (0..255)

T11FspfLinkType ::= TEXTUAL-CONVENTION
    STATUS    current
    DESCRIPTION





           "Type of an the FSPF Link.  Presently defined values:

               1           - Point-to-Point
               240-255     - Vendor Specific
               all others  - Reserved.
           "
    REFERENCE
           "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
           ANSI INCITS 418-2006, section 6.1.9.4."
    SYNTAX    Integer32 (0..255)

T11FspfInterfaceState ::= TEXTUAL-CONVENTION
    STATUS    current
    DESCRIPTION
           "The state of the FSPF Neighbor Finite State Machine
           for the neighbor (switch) on a particular interface.
           Possible values are :

                down(1)         - Down
                init(2)         - Init
                dbExchange(3)   - Database Exchange
                dbAckwait(4)    - Database AckWait
                dbWait(5)       - Database Wait
                full(6)         - Full (Connected)
           "
    REFERENCE
           "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
           ANSI INCITS 418-2006, section 8.7."
    SYNTAX  INTEGER {
                   down(1),
                   init(2),
                   dbExchange(3),
                   dbAckwait(4),
                   dbWait(5),
                   full(6)
            }

T11FspfLastCreationTime ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
           "This TC describes an object that stores the last time
           it, and the row containing it, was created.

           This can be used by management applications to determine
           that a row has been deleted and re-created between reads,
           causing an otherwise undetectable discontinuity in the
           data."
    SYNTAX  TimeTicks





--
-- t11FspfTable

t11FspfTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF T11FspfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "This table allows the users to configure and monitor FSPF's
           per-Fabric parameters and statistics on all Fabrics known to
           locally managed switches.

           Entries are created/removed by the agent if and when
           (Virtual) Fabrics are created/deleted."
    ::= { t11FspfConfiguration 1 }

t11FspfEntry OBJECT-TYPE
    SYNTAX      T11FspfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "An entry containing FSPF variables, parameters, and
           statistics on a particular switch (identified by values
           of fcmInstanceIndex and fcmSwitchIndex) for a particular
           Fabric (identified by a t11FspfFabricIndex value).

           (Note that the local switch's per-fabric Domain-ID is
           available in t11FamConfigDomainId, which is defined in
           T11-FC-FABRIC-ADDR-MGR-MIB.)"
    INDEX      { fcmInstanceIndex, fcmSwitchIndex, t11FspfFabricIndex }
    ::= { t11FspfTable 1 }

T11FspfEntry ::= SEQUENCE  {
    t11FspfFabricIndex                 T11FabricIndex,
    t11FspfMinLsArrival                Unsigned32,
    t11FspfMinLsInterval               Unsigned32,
    t11FspfLsRefreshTime               Unsigned32,
    t11FspfMaxAge                      Unsigned32,
    t11FspfMaxAgeDiscards              Counter32,
    t11FspfPathComputations            Counter32,
    t11FspfChecksumErrors              Counter32,
    t11FspfLsrs                        Gauge32,
    t11FspfCreateTime                  T11FspfLastCreationTime,
    t11FspfAdminStatus                 INTEGER,
    t11FspfOperStatus                  INTEGER,
    t11FspfNbrStateChangNotifyEnable   TruthValue,
    t11FspfSetToDefault                INTEGER,
    t11FspfStorageType                 StorageType





}

t11FspfFabricIndex OBJECT-TYPE
    SYNTAX      T11FabricIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "A unique index value that uniquely identifies a
           particular Fabric.

           In a Fabric conformant to FC-SW-4, multiple Virtual Fabrics
           can operate within one (or more) physical infrastructures.
           In such a case, index value is used to uniquely identify a
           particular Fabric within a physical infrastructure.

           In a Fabric that has (can have) only a single Fabric
           operating within the physical infrastructure, the
           value of this Fabric Index will always be 1."
    ::= { t11FspfEntry 1 }

t11FspfMinLsArrival OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    UNITS       "milliSeconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
           "The minimum time after accepting a Link State Record
           (LSR) on this Fabric before accepting another update of
           the same LSR on the same Fabric.

           An LSR update that is not accepted because of this time
           interval is discarded."
    REFERENCE  "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
               ANSI INCITS 418-2006, sections 8.6.4.5 & 15.1."
    DEFVAL     {1000}
    ::= { t11FspfEntry 2 }

t11FspfMinLsInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    UNITS       "milliSeconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
           "The minimum time after this switch sends an LSR on this
           Fabric before it will send another update of the same LSR
           on the same Fabric."
    REFERENCE  "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
               ANSI INCITS 418-2006, section 15.1."





    DEFVAL     {5000}
    ::= { t11FspfEntry 3 }

t11FspfLsRefreshTime OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "Minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The interval between transmission of refresh LSRs on this
           Fabric."
    REFERENCE  "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
               ANSI INCITS 418-2006, sections 8.5.1 & 15.1."
    DEFVAL     {30}
    ::= { t11FspfEntry 4 }

t11FspfMaxAge OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "Minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The maximum age an LSR will be retained in the FSPF
           database on this Fabric.  An LSR is removed from the
           database after MaxAge is reached."
    REFERENCE  "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
               ANSI INCITS 418-2006, section 15.1."
    DEFVAL     {60}
    ::= { t11FspfEntry 5 }

t11FspfMaxAgeDiscards OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The number of LSRs discarded due to their age reaching
           t11FspfMaxAge in this Fabric.  The last discontinuity of
           this counter is indicated by t11FspfCreateTime."
    ::= { t11FspfEntry 6 }

t11FspfPathComputations OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The number of times that the path computation algorithm
           has been invoked by this Switch on this Fabric to compute
           a set of minimum cost paths for this Fabric.  The last





           discontinuity of this counter is indicated by
           t11FspfCreateTime."
    REFERENCE  "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
               ANSI INCITS 418-2006, section 8.1.1."
    ::= { t11FspfEntry 7 }

t11FspfChecksumErrors OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The number of FSPF checksum errors that were detected
           locally (and therefore discarded) on this Fabric.
           The last discontinuity of this counter is indicated by
           t11FspfCreateTime."
    REFERENCE  "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
               ANSI INCITS 418-2006, section 8.5.4."
    ::= { t11FspfEntry 8 }

t11FspfLsrs OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The current number of entries for this Fabric in the
           t11FspfLsrTable."
    ::= { t11FspfEntry 9 }

t11FspfCreateTime OBJECT-TYPE
    SYNTAX      T11FspfLastCreationTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The value of sysUpTime when this entry was last created."
    ::= { t11FspfEntry 10 }

t11FspfAdminStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    up(1),
                    down(2)
                    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
           "The desired state of FSPF in this Fabric.  If value of
           this object is set to 'up', then FSPF is enabled in
           this Fabric.  If set to 'down', then FSPF is disabled
           in this Fabric -- when FSPF is disabled, FSPF provides





           no routes to be included in the T11-FC-ROUTE-MIB module.
           (see the T11-FC-ROUTE-MIB)."
    REFERENCE  "T11-FC-ROUTE-MIB, The Fibre Channel Routing
                Information MIB, RFC4625."
    DEFVAL {up}
    ::= { t11FspfEntry 11 }

t11FspfOperStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                      up(1),
                      down(2)
                     }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "State of FSPF in this Fabric.  If 't11FspfAdminStatus' is
           'down', then the 't11FspfOperStatus' should be 'down'.
           If 't11FspfAdminStatus' is changed to 'up', then
           't11FspfOperStatus' should change to 'up' as and when
           FSPF is active in this Fabric."
    ::= { t11FspfEntry 12 }

t11FspfNbrStateChangNotifyEnable OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
           "Specifies whether or not the local agent should
           issue the notification 't11FspfNbrStateChangNotify'
           when the local switch learns of a change of state
           in the FSPF Neighbor Finite State Machine on an
           interface in this Fabric.
           If the value of the object is 'true, then the
           notification is generated.  If the value is 'false',
           notification is not generated."
    DEFVAL { false }
    ::= { t11FspfEntry 13 }

t11FspfSetToDefault OBJECT-TYPE
    SYNTAX      INTEGER {
                     default(1),
                     noOp(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
           "Setting this value to 'default' changes the value of each
           and every writable object in this row to its default





           value.

           No action is taken if this object is set to 'noOp'.
           The value of the object, when read, is always 'noOp'."
    ::= { t11FspfEntry 14 }

t11FspfStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
           "The storage type for read-write objects in this
           conceptual row.

           Conceptual rows having the value 'permanent' need not
           allow write-access to any columnar objects in the row."
    DEFVAL { nonVolatile }
    ::= { t11FspfEntry 15 }

--
-- t11FspfIfTable

t11FspfIfTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FspfIfEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "This table allows the users to configure and monitor
           the FSPF parameters that are per-interface (identified
           by a t11FspfIfIndex value), per-Fabric (identified by a
           t11FspfFabricIndex value), and per-switch (identified by
           values of fcmInstanceIndex and fcmSwitchIndex).

           Creating a row in this table via t11FspfIfRowStatus
           provides the means to specify non-default parameter value(s)
           for an interface at a time when the relevant row in this
           table would not otherwise exist because the interface is
           either down or it is not an E_Port, but the corresponding
           row in the t11FspfTable must already exist.

           After the non-default values have been specified for a
           port's parameters, they need to be retained in this table,
           even when the port becomes 'isolated'.  However, having
           unnecessary rows in this table clutters it up and makes
           those rows that are useful harder for an NMS to find.
           Therefore, when an E_Port becomes isolated, its row gets
           deleted if and only if all of its parameter values are the
           default values; also, when an E_Port becomes non-isolated





           in a particular Fabric, a row in this table needs to exist
           and is automatically created, if necessary.

           The specific conditions for an automated/implicit deletion
           of a row are:
           a) if the corresponding interface is no longer an E_Port
              (e.g., a G_Port which is dynamically determined to be an
              F_Port), and all configurable parameters have default
              values; or
           b) if the interface identified by t11FspfIfIndex no longer
              exists (e.g., because a line-card is physically removed);
              or
           c) if the corresponding row in the t11FspfTable is deleted.
           "
    ::= { t11FspfConfiguration 2 }

t11FspfIfEntry OBJECT-TYPE
    SYNTAX      T11FspfIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "An entry containing FSPF information for the interface
           identified by t11FspfIfIndex, on the fabric identified
           by t11FspfFabricIndex, on the switch identified by
           fcmSwitchIndex."
    INDEX       { fcmInstanceIndex, fcmSwitchIndex,
                  t11FspfFabricIndex, t11FspfIfIndex }
    ::= { t11FspfIfTable 1 }

T11FspfIfEntry ::= SEQUENCE {
    t11FspfIfIndex                     InterfaceIndex,
    t11FspfIfHelloInterval             Unsigned32,
    t11FspfIfDeadInterval              Unsigned32,
    t11FspfIfRetransmitInterval        Unsigned32,
    t11FspfIfInLsuPkts                 Counter32,
    t11FspfIfInLsaPkts                 Counter32,
    t11FspfIfOutLsuPkts                Counter32,
    t11FspfIfOutLsaPkts                Counter32,
    t11FspfIfOutHelloPkts              Counter32,
    t11FspfIfInHelloPkts               Counter32,
    t11FspfIfRetransmittedLsuPkts      Counter32,
    t11FspfIfInErrorPkts               Counter32,
    t11FspfIfNbrState                  T11FspfInterfaceState,
    t11FspfIfNbrDomainId               FcDomainIdOrZero,
    t11FspfIfNbrPortIndex              Unsigned32,
    t11FspfIfAdminStatus               INTEGER,
    t11FspfIfCreateTime                T11FspfLastCreationTime,
    t11FspfIfSetToDefault              INTEGER,





    t11FspfIfLinkCostFactor            Unsigned32,
    t11FspfIfStorageType               StorageType,
    t11FspfIfRowStatus                 RowStatus
}

t11FspfIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The value of ifIndex that identifies the local
           Fibre Channel interface for which this entry
           contains FSPF information."
    ::= { t11FspfIfEntry 1 }

t11FspfIfHelloInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    UNITS       "Seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "Interval between the periodic HELLO messages sent on this
           interface in this Fabric to verify the link health.  Note
           that this value must be same at both ends of a link in
           this Fabric."
    DEFVAL {20}
    ::= { t11FspfIfEntry 2 }

t11FspfIfDeadInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (2..65535)
    UNITS       "Seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "Maximum time for which no HELLO messages can be received
           on this interface in this Fabric.  After this time, the
           interface is assumed to be broken and removed from the
           database.  Note that this value must be greater than the
           HELLO interval specified on this interface in this Fabric."
    DEFVAL {80}
    ::= { t11FspfIfEntry 3 }

t11FspfIfRetransmitInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    UNITS       "Seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION





           "The time after which an unacknowledged LSR is
           retransmitted on this interface in this Fabric."
    DEFVAL {5}
    ::= { t11FspfIfEntry 4 }

t11FspfIfInLsuPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "Number of Link State Update (LSU) packets received on
           this interface in this Fabric.  The last discontinuity
           of this counter is indicated by t11FspfIfCreateTime."
    ::= { t11FspfIfEntry 5 }

t11FspfIfInLsaPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "Number of Link State Acknowledgement (LSA) packets
           received on this interface in this Fabric.  The last
           discontinuity of this counter is indicated by
           t11FspfIfCreateTime."
    ::= { t11FspfIfEntry 6 }

t11FspfIfOutLsuPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "Number of Link State Update (LSU) packets transmitted
           on this interface in this Fabric.  The last
           discontinuity of this counter is indicated by
           t11FspfIfCreateTime."
    ::= { t11FspfIfEntry 7 }

t11FspfIfOutLsaPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "Number of Link State Acknowledgement (LSA) packets
           transmitted on this interface in this Fabric.  The
           last discontinuity of this counter is indicated by
           t11FspfIfCreateTime."
    ::= { t11FspfIfEntry 8 }






t11FspfIfOutHelloPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "Number of HELLO packets transmitted on this interface in
           this Fabric.  The last discontinuity of this counter is
           indicated by t11FspfIfCreateTime."
    ::= { t11FspfIfEntry 9 }

t11FspfIfInHelloPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "Number of HELLO packets received on this interface in
           this Fabric.  The last discontinuity of this counter is
           indicated by t11FspfIfCreateTime."
    ::= { t11FspfIfEntry 10 }

t11FspfIfRetransmittedLsuPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The number of LSU packets that contained one or more
           retransmitted LSRs, and that were transmitted on this
           interface in this Fabric.  The last discontinuity of
           this counter is indicated by t11FspfIfCreateTime."
    ::= { t11FspfIfEntry 11 }

t11FspfIfInErrorPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "Number of invalid FSPF control packets received on this
           interface in this Fabric.  The last discontinuity of
           this counter is indicated by t11FspfIfCreateTime."
    ::= { t11FspfIfEntry 12 }

t11FspfIfNbrState OBJECT-TYPE
    SYNTAX      T11FspfInterfaceState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The state of FSPF's 'neighbor state machine', which is
           the operational state of the interaction with the





           neighbor's interface that is connected to this interface.

           If the 't11FspfIfAdminStatus' is 'down', then this object
           should be 'down'.  If the 't11FspfIfAdminStatus' is 'up',
           then this object's value depends on the state of FSPF's
           'neighbor state machine' on this interface in this
           Fabric."
    REFERENCE  "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
               ANSI INCITS 418-2006, section 8.7"
    ::= { t11FspfIfEntry 13 }

t11FspfIfNbrDomainId OBJECT-TYPE
    SYNTAX      FcDomainIdOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The Domain Id of the neighbor in this Fabric."
    ::= { t11FspfIfEntry 14 }

t11FspfIfNbrPortIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (0..16777215)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The index, as known by the neighbor, of the neighbor's
           interface that is connected to this interface in this
           Fabric."
    REFERENCE  "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
               ANSI INCITS 418-2006, section 6.1.9.4."
    ::= { t11FspfIfEntry 15 }

t11FspfIfAdminStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                up(1),
                down(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The desired state of FSPF on this interface in this
           Fabric, whenever 't11FspfAdminStatus' is 'up'.
           If the value of this object is set to 'up', then FSPF is
           enabled on this interface in this Fabric.  If set to
           'down', then FSPF is disabled on this interface in this
           Fabric.  Note that the operational state of FSPF on an
           interface is given by t11FspfIfNbrState."
    DEFVAL  {up}
    ::= { t11FspfIfEntry 16 }





t11FspfIfCreateTime OBJECT-TYPE
    SYNTAX      T11FspfLastCreationTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The value of sysUpTime when this entry was last
           created."
    ::= { t11FspfIfEntry 17 }

t11FspfIfSetToDefault OBJECT-TYPE
    SYNTAX      INTEGER {
                     default(1),
                     noOp(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "Setting this value to 'default' changes the value of each
           and every writable object in this row to its default
           value.

           If all the configuration parameters have their default
           values, and if the interface is down, then the row is
           deleted automatically.

           No action is taken if this object is set to 'noOp'.
           The value of the object, when read, is always 'noOp'."
    ::= { t11FspfIfEntry 18 }

t11FspfIfLinkCostFactor OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The administrative factor used in calculating the cost
           of sending a frame on this interface in this Fabric.

           The formula used to calculate the link cost is:

                    Link Cost = S * (1.0625e12 / ifSpeed)
           where:
             S = (the value of this object / 100)
             ifSpeed = interface speed (as defined in the IF-MIB).
           "
    REFERENCE
           "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
            ANSI INCITS 418-2006, section 8.5.5; and
            IF-MIB, RFC 2863."





    DEFVAL { 100 }
    ::= { t11FspfIfEntry 19 }

t11FspfIfStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The storage type for this conceptual row.
            Conceptual rows having the value 'permanent' need not
            allow write-access to any columnar objects in the row."
       DEFVAL { nonVolatile }
    ::= { t11FspfIfEntry 20 }

t11FspfIfRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
           "The status of the conceptual row.

           This object can be used to create an entry only if there
           is an entry in the t11FspfTable for the corresponding
           Fabric, and if the interface is either isolated or is a
           non-E_port.

           Setting this object to 'destroy' will typically fail;
           to reverse the creation process, set the corresponding
           instance of t11FspfIfSetToDefault to 'default'."
    ::= { t11FspfIfEntry 21 }

--
-- t11FspfLsrTable

t11FspfLsrTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FspfLsrEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "This table is the database of all the latest
           incarnations of the Link State Records (LSRs) that
           are currently contained in the topology database,
           for all interfaces on all Fabrics known to
           locally managed switches.

           A Fabric's topology database contains the LSRs that
           have been either issued or received by a local switch on
           that Fabric, and that have not reached t11FspfMaxAge."





    ::= { t11FspfDatabase 1 }

t11FspfLsrEntry OBJECT-TYPE
    SYNTAX      T11FspfLsrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "This gives information for the most recent update of an
           LSR.  There is one entry for every LSR issued or received
           by a locally managed switch (identified by
           fcmInstanceIndex and fcmSwitchIndex) in a Fabric
           (identified by t11FspfFabricIndex)."
    INDEX      { fcmInstanceIndex, fcmSwitchIndex, t11FspfFabricIndex,
                 t11FspfLsrDomainId, t11FspfLsrType }
    ::= { t11FspfLsrTable 1 }

T11FspfLsrEntry ::= SEQUENCE {
    t11FspfLsrDomainId           FcDomainIdOrZero,
    t11FspfLsrType               T11FspfLsrType,
    t11FspfLsrAdvDomainId        FcDomainIdOrZero,
    t11FspfLsrAge                Unsigned32,
    t11FspfLsrIncarnationNumber  Unsigned32,
    t11FspfLsrCheckSum           Unsigned32,
    t11FspfLsrLinks              Unsigned32
}

t11FspfLsrDomainId OBJECT-TYPE
    SYNTAX      FcDomainIdOrZero
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "Domain Id of the LSR owner in this Fabric.  It is the
           Link State Id of this LSR."
    ::= { t11FspfLsrEntry 1 }

t11FspfLsrType OBJECT-TYPE
    SYNTAX      T11FspfLsrType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "Type of this LSR."
    ::= { t11FspfLsrEntry 2 }

t11FspfLsrAdvDomainId OBJECT-TYPE
    SYNTAX      FcDomainIdOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION





           "Domain Id of the switch that is advertising the LSR on
           the behalf of the switch owning it."
    ::= { t11FspfLsrEntry 3 }

t11FspfLsrAge OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    UNITS       "Seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The time since this LSR was inserted into the database."
    ::= { t11FspfLsrEntry 4 }

t11FspfLsrIncarnationNumber OBJECT-TYPE
    SYNTAX      Unsigned32 (0..4294967295)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The link state incarnation number of this LSR.  This is
           used to identify most recent instance of an LSR while
           updating the topology database when an LSR is received.
           The updating of an LSR includes incrementing its
           incarnation number prior to transmission of the updated
           LSR.  So, the most recent LSR is the one with the
           largest incarnation number."
    ::= { t11FspfLsrEntry 5 }

t11FspfLsrCheckSum OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The checksum of the LSR."
    ::= { t11FspfLsrEntry 6 }

t11FspfLsrLinks OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65355)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "Number of entries in the t11FspfLinkTable associated with
           this LSR."
    ::= { t11FspfLsrEntry 7 }
--
-- t11FspfLinkTable

t11FspfLinkNumber  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..2147483647)





    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The number of rows in the t11FspfLinkTable."
        ::= { t11FspfDatabase 3 }

t11FspfLinkTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FspfLinkEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "This table contains the list of Inter-Switch Links and
           their information that is part of an LSR, either
           received or transmitted."
    ::= { t11FspfDatabase 4 }

t11FspfLinkEntry OBJECT-TYPE
    SYNTAX      T11FspfLinkEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "An entry that contains information about a link
           contained in an LSR in this Fabric.  An entry is created
           whenever a new link appears in an (issued or received)
           LSR.  An entry is deleted when a link no longer appears
           in an (issued or received) LSR."
    INDEX      { fcmInstanceIndex, fcmSwitchIndex, t11FspfFabricIndex,
                 t11FspfLsrDomainId, t11FspfLsrType, t11FspfLinkIndex}
    ::= { t11FspfLinkTable 1 }

T11FspfLinkEntry ::= SEQUENCE {
    t11FspfLinkIndex             Unsigned32,
    t11FspfLinkNbrDomainId       FcDomainIdOrZero,
    t11FspfLinkPortIndex         Unsigned32,
    t11FspfLinkNbrPortIndex      Unsigned32,
    t11FspfLinkType              T11FspfLinkType,
    t11FspfLinkCost              Integer32
}

t11FspfLinkIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "An arbitrary index of this link."
    ::= { t11FspfLinkEntry 1 }

t11FspfLinkNbrDomainId OBJECT-TYPE





    SYNTAX      FcDomainIdOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The Domain Id of the neighbor on the other end of this
           link in this Fabric."
    ::= { t11FspfLinkEntry 2 }

t11FspfLinkPortIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (0..16777215)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The source E_port of this link, as indicated by the index
           value in the LSR received from the switch identified by
           't11FspfLsrDomainId'."
    ::= { t11FspfLinkEntry 3 }

t11FspfLinkNbrPortIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (0..16777215)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The destination E_port of this link, as indicated by the
           index value in the LSR received from the switch identified
           by 't11FspfLinkNbrDomainId'."
    ::= { t11FspfLinkEntry 4 }

t11FspfLinkType OBJECT-TYPE
    SYNTAX      T11FspfLinkType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The type of this link."
    ::= { t11FspfLinkEntry 5 }

t11FspfLinkCost OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
           "The cost of sending a frame on this link in this Fabric.
           Link cost is calculated using the formula:

                 link cost = S * (1.0625e12 / Signalling Rate)

           For issued LSRs, S is determined by the value of
           t11FspfIfLinkCostFactor for the corresponding interface





           and Fabric."
    ::= { t11FspfLinkEntry 6 }

--
-- Notification-related object

t11FspfIfPrevNbrState OBJECT-TYPE
    SYNTAX      T11FspfInterfaceState
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
           "The previous state of FSPF's Neighbor Finite State
           Machine on an interface.

           This object is only used in the
           't11FspfNbrStateChangNotify' notification."
    ::= { t11FspfConfiguration 3 }

--
-- Notifications

t11FspfNbrStateChangNotify NOTIFICATION-TYPE
    OBJECTS     { ifIndex,
                  t11FamConfigDomainId,
                  t11FspfIfNbrDomainId,
                  t11FspfIfNbrState,
                  t11FspfIfPrevNbrState
    }
    STATUS      current
    DESCRIPTION
           "This notification signifies that there has been a change in
           the state of an FSPF neighbor.  This is generated when the
           FSPF state changes to a terminal state, through either
           regression (i.e., goes from Full to Init or Down) or
           progression (i.e., from any state to Full).  The value of
           't11FspfIfNbrState' is the state of the neighbor after the
           change."
    ::= { t11FspfNotifications 1 }

--
-- Conformance

t11FspfMIBCompliances
    OBJECT IDENTIFIER ::= { t11FspfConformance 1 }

t11FspfMIBGroups
    OBJECT IDENTIFIER ::= { t11FspfConformance 2 }






t11FspfMIBCompliance MODULE-COMPLIANCE
    STATUS     current
    DESCRIPTION
           "The compliance statement for entities that
           implement the FSPF."
    MODULE -- this module
        MANDATORY-GROUPS { t11FspfGeneralGroup,
                           t11FspfIfGroup,
                           t11FspfDatabaseGroup,
                           t11FspfNotificationGroup }

        GROUP      t11FspfIfCounterGroup
        DESCRIPTION
               "These counters, for particular FSPF-packet
               occurrences on an interface, are mandatory only
               for those systems that count such events."

        OBJECT     t11FspfIfRowStatus
        SYNTAX     INTEGER { active(1) }
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required, so only
               one value needs to be supported."

        OBJECT     t11FspfIfStorageType
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfNbrStateChangNotifyEnable
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfMinLsArrival
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfMinLsInterval
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfAdminStatus
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."





        OBJECT     t11FspfSetToDefault
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfStorageType
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfIfHelloInterval
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfIfDeadInterval
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfIfRetransmitInterval
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfIfAdminStatus
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfIfSetToDefault
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        OBJECT     t11FspfIfLinkCostFactor
        MIN-ACCESS read-only
        DESCRIPTION
               "Write access is not required."

        ::= { t11FspfMIBCompliances 1 }

-- Units of Conformance

t11FspfGeneralGroup OBJECT-GROUP
    OBJECTS  { t11FspfMinLsArrival,
               t11FspfMinLsInterval,
               t11FspfLsRefreshTime,





               t11FspfMaxAge,
               t11FspfMaxAgeDiscards,
               t11FspfPathComputations,
               t11FspfChecksumErrors,
               t11FspfLsrs,
               t11FspfCreateTime,
               t11FspfAdminStatus,
               t11FspfOperStatus,
               t11FspfNbrStateChangNotifyEnable,
               t11FspfSetToDefault,
               t11FspfStorageType }
    STATUS   current
    DESCRIPTION
           "A collection of objects for displaying and
           configuring FSPF parameters."
    ::= { t11FspfMIBGroups 1 }

t11FspfIfGroup OBJECT-GROUP
    OBJECTS  { t11FspfIfHelloInterval,
               t11FspfIfDeadInterval,
               t11FspfIfRetransmitInterval,
               t11FspfIfNbrState,
               t11FspfIfNbrDomainId,
               t11FspfIfNbrPortIndex,
               t11FspfIfAdminStatus,
               t11FspfIfCreateTime,
               t11FspfIfSetToDefault,
               t11FspfIfLinkCostFactor,
               t11FspfIfRowStatus,
               t11FspfIfStorageType,
               t11FspfIfPrevNbrState }
    STATUS   current
    DESCRIPTION
           "A collection of objects for displaying the FSPF
           interface information."
    ::= { t11FspfMIBGroups 2 }

t11FspfIfCounterGroup OBJECT-GROUP
    OBJECTS  { t11FspfIfInLsuPkts,
               t11FspfIfInLsaPkts,
               t11FspfIfOutLsuPkts,
               t11FspfIfOutLsaPkts,
               t11FspfIfOutHelloPkts,
               t11FspfIfInHelloPkts,
               t11FspfIfRetransmittedLsuPkts,
               t11FspfIfInErrorPkts  }
    STATUS   current
    DESCRIPTION





            "A collection of objects for counting particular
            FSPF-packet occurrences on an interface."
    ::= { t11FspfMIBGroups 3 }

t11FspfDatabaseGroup OBJECT-GROUP
    OBJECTS  { t11FspfLsrAdvDomainId,
               t11FspfLsrAge,
               t11FspfLsrIncarnationNumber,
               t11FspfLsrCheckSum,
               t11FspfLsrLinks,
               t11FspfLinkNbrDomainId,
               t11FspfLinkPortIndex,
               t11FspfLinkNbrPortIndex,
               t11FspfLinkType,
               t11FspfLinkCost,
               t11FspfLinkNumber }
    STATUS   current
    DESCRIPTION
           "A collection of objects for displaying the FSPF
           topology database information."
    ::= { t11FspfMIBGroups 4 }
t11FspfNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS  { t11FspfNbrStateChangNotify }
    STATUS   current
    DESCRIPTION
           "A collection of notifications for FSPF."
    ::= { t11FspfMIBGroups 5 }
END


