RFC1317-MIB DEFINITIONS ::= BEGIN


                    IMPORTS
                       Counter
                               FROM RFC1155-SMI
                       transmission
                               FROM RFC1213-MIB
                       OBJECT-TYPE
                               FROM RFC-1212;

       -- this is the MIB module for RS-232-like hardware devices

       rs232    OBJECT IDENTIFIER ::= { transmission 33 }


       -- the generic RS-232-like group

       -- Implementation of this group is mandatory for all
       -- systems that have RS-232-like hardware ports
       -- supporting higher level services such as character
       -- streams or network interfaces

       rs232Number OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The number of ports (regardless of their current
               state) in the RS-232-like general port table."
           ::= { rs232 1 }


       -- the RS-232-like general Port table

       rs232PortTable OBJECT-TYPE
           SYNTAX SEQUENCE OF Rs232PortEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "A list of port entries.  The number of entries is
               given by the value of rs232Number."
           ::= { rs232 2 }

       rs232PortEntry OBJECT-TYPE
           SYNTAX Rs232PortEntry
           ACCESS not-accessible





           STATUS mandatory
           DESCRIPTION
               "Status and parameter values for a port."
           INDEX { rs232PortIndex }
           ::= { rs232PortTable 1 }

       Rs232PortEntry ::=
           SEQUENCE {
               rs232PortIndex
                   INTEGER,
               rs232PortType
                   INTEGER,
               rs232PortInSigNumber
                   INTEGER,
               rs232PortOutSigNumber
                   INTEGER,
               rs232PortInSpeed
                   INTEGER,
               rs232PortOutSpeed
                   INTEGER    }

       rs232PortIndex OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "A unique value for each port.  Its value ranges
               between 1 and the value of rs232Number.  By
               convention and if possible, hardware port numbers
               map directly to external connectors.  The value for
               each port must remain constant at least from one
               re-initialization of the network management agent to
               the next."
           ::= { rs232PortEntry 1 }

       rs232PortType OBJECT-TYPE
           SYNTAX INTEGER { other(1), rs232(2), rs422(3),
                            rs423(4), v35(5) }
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The port's hardware type."
           ::= { rs232PortEntry 2 }

       rs232PortInSigNumber OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory





           DESCRIPTION
               "The number of input signals for the port in the
               input signal table (rs232PortInSigTable).  The table
               contains entries only for those signals the software
               can detect."
           ::= { rs232PortEntry 3 }

       rs232PortOutSigNumber OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The number of output signals for the port in the
               output signal table (rs232PortOutSigTable).  The
               table contains entries only for those signals the
               software can assert."
           ::= { rs232PortEntry 4 }

       rs232PortInSpeed OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-write
           STATUS mandatory
           DESCRIPTION
               "The port's input speed in bits per second."
           ::= { rs232PortEntry 5 }

       rs232PortOutSpeed OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-write
           STATUS mandatory
           DESCRIPTION
               "The port's output speed in bits per second."
           ::= { rs232PortEntry 6 }


       -- the RS-232-like Asynchronous Port group

       -- Implementation of this group is mandatory if the system
       -- has any asynchronous ports.  Otherwise it is not
       -- present.

       rs232AsyncPortTable OBJECT-TYPE
           SYNTAX SEQUENCE OF Rs232AsyncPortEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "A list of asynchronous port entries.  The maximum
               entry number is given by the value of rs232Number.





               Entries need not exist for synchronous ports."
           ::= { rs232 3 }

       rs232AsyncPortEntry OBJECT-TYPE
           SYNTAX Rs232AsyncPortEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "Status and parameter values for an asynchronous
               port."
           INDEX { rs232AsyncPortIndex }
           ::= { rs232AsyncPortTable 1 }

       Rs232AsyncPortEntry ::=
           SEQUENCE {
               rs232AsyncPortIndex
                   INTEGER,
               rs232AsyncPortBits
                   INTEGER,
               rs232AsyncPortStopBits
                   INTEGER,
               rs232AsyncPortParity
                   INTEGER,
               rs232AsyncPortAutobaud
                   INTEGER,
               rs232AsyncPortParityErrs
                   Counter,
               rs232AsyncPortFramingErrs
                   Counter,
               rs232AsyncPortOverrunErrs
                   Counter

           }

       rs232AsyncPortIndex OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "A unique value for each port.  Its value is the
               same as rs232PortIndex for the port."
           ::= { rs232AsyncPortEntry 1 }

       rs232AsyncPortBits OBJECT-TYPE
           SYNTAX INTEGER (5..8)
           ACCESS read-write
           STATUS mandatory
           DESCRIPTION





               "The port's number of bits in a character."
           ::= { rs232AsyncPortEntry 2 }

       rs232AsyncPortStopBits OBJECT-TYPE
           SYNTAX INTEGER { one(1), two(2),
                            one-and-half(3), dynamic(4) }
           ACCESS read-write
           STATUS mandatory
           DESCRIPTION
               "The port's number of stop bits."
           ::= { rs232AsyncPortEntry 3 }

       rs232AsyncPortParity OBJECT-TYPE
           SYNTAX INTEGER { none(1), odd(2), even(3),
                            mark(4), space(5) }
           ACCESS read-write
           STATUS mandatory
           DESCRIPTION
               "The port's sense of a character parity bit."
           ::= { rs232AsyncPortEntry 4 }

       rs232AsyncPortAutobaud OBJECT-TYPE
           SYNTAX INTEGER { enabled(1), disabled(2) }
           ACCESS read-write
           STATUS mandatory
           DESCRIPTION
               "A control for the port's ability to automatically
               sense input speed.

               When rs232PortAutoBaud is 'enabled', a port may
               autobaud to values different from the set values for
               speed, parity, and character size.  As a result a
               network management system may temporarily observe
               values different from what was previously set."
           ::= { rs232AsyncPortEntry 5 }

       rs232AsyncPortParityErrs OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Total number of characters with a parity error,
               input from the port since system re-initialization
               and while the port state was 'up' or 'test'."
           ::= { rs232AsyncPortEntry 6 }

       rs232AsyncPortFramingErrs OBJECT-TYPE
           SYNTAX Counter





           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Total number of characters with a framing error,
               input from the port since system re-initialization
               and while the port state was 'up' or 'test'."
           ::= { rs232AsyncPortEntry 7 }

       rs232AsyncPortOverrunErrs OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Total number of characters with an overrun error,
               input from the port since system re-initialization
               and while the port state was 'up' or 'test'."
           ::= { rs232AsyncPortEntry 8 }


       -- the RS-232-like Synchronous Port group

       -- Implementation of this group is mandatory if the system
       -- has any synchronous ports.  Otherwise it is not
       -- present.

       rs232SyncPortTable OBJECT-TYPE
           SYNTAX SEQUENCE OF Rs232SyncPortEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "A list of synchronous port entries.  The maximum
               entry number is given by the value of rs232Number.
               Entries need not exist for asynchronous ports."
           ::= { rs232 4 }

       rs232SyncPortEntry OBJECT-TYPE
           SYNTAX Rs232SyncPortEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "Status and parameter values for a synchronous
               port."
           INDEX { rs232SyncPortIndex }
           ::= { rs232SyncPortTable 1 }

       Rs232SyncPortEntry ::=
           SEQUENCE {
               rs232SyncPortIndex





                   INTEGER,
               rs232SyncPortClockSource
                   INTEGER,
               rs232SyncPortFrameCheckErrs
                   Counter,
               rs232SyncPortTransmitUnderrunErrs
                   Counter,
               rs232SyncPortReceiveOverrunErrs
                   Counter,
               rs232SyncPortInterruptedFrames
                   Counter,
               rs232SyncPortAbortedFrames
                   Counter
           }

       rs232SyncPortIndex OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "A unique value for each port.  Its value is the
               same as rs232PortIndex for the port."
           ::= { rs232SyncPortEntry 1 }

       rs232SyncPortClockSource OBJECT-TYPE
           SYNTAX INTEGER  { internal(1), external(2), split(3) }
           ACCESS read-write
           STATUS mandatory
           DESCRIPTION
               "Source of the port's bit rate clock. 'split' means
               the tranmit clock is internal and the receive clock
               is external."
           ::= { rs232SyncPortEntry 2 }

       rs232SyncPortFrameCheckErrs OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Total number of frames with an invalid frame check
               sequence, input from the port since system
               re-initialization and while the port state was 'up'
               or 'test'."
           ::= { rs232SyncPortEntry 3 }

       rs232SyncPortTransmitUnderrunErrs OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only





           STATUS mandatory
           DESCRIPTION
               "Total number of frames that failed to be
               transmitted on the port since system
               re-initialization and while the port state was 'up'
               or 'test' because data was not available to the
               transmitter in time."
           ::= { rs232SyncPortEntry 4 }

       rs232SyncPortReceiveOverrunErrs OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Total number of frames that failed to be received
               on the port since system re-initialization and while
               the port state was 'up' or 'test' because the
               receiver did not accept the data in time."
           ::= { rs232SyncPortEntry 5 }

       rs232SyncPortInterruptedFrames OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Total number of frames that failed to be received
               or transmitted on the port due to loss of modem
               signals since system re-initialization and while the
               port state was 'up' or 'test'."
           ::= { rs232SyncPortEntry 6 }

       rs232SyncPortAbortedFrames OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Number of frames aborted on the port due to
               receiving an abort sequence since system
               re-initialization and while the port state was 'up'
               or 'test'."
           ::= { rs232SyncPortEntry 7 }


       -- the Input Signal table

       rs232InSigTable OBJECT-TYPE
           SYNTAX SEQUENCE OF Rs232InSigEntry
           ACCESS not-accessible





           STATUS mandatory
           DESCRIPTION
               "A list of port input control signal entries."
           ::= { rs232 5 }

       rs232InSigEntry OBJECT-TYPE
           SYNTAX Rs232InSigEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "Input control signal status for a hardware port."
           INDEX { rs232InSigPortIndex, rs232InSigName }
           ::= { rs232InSigTable 1 }

       Rs232InSigEntry ::=
           SEQUENCE {
               rs232InSigPortIndex
                   INTEGER,
               rs232InSigName
                   INTEGER,
               rs232InSigState
                   INTEGER,
               rs232InSigChanges
                   Counter
           }

       rs232InSigPortIndex OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The value of rs232PortIndex for the port to which
               this entry belongs."
           ::= { rs232InSigEntry 1 }

       rs232InSigName OBJECT-TYPE
           SYNTAX INTEGER { rts(1), cts(2), dsr(3), dtr(4), ri(5),
                            dcd(6), sq(7), srs(8), srts(9),
                            scts(10), sdcd(11) }
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Identification of a hardware signal, as follows:

                   rts    Request to Send
                   cts    Clear to Send
                   dsr    Data Set Ready
                   dtr    Data Terminal Ready





                   ri     Ring Indicator
                   dcd    Received Line Signal Detector
                   sq     Signal Quality Detector
                   srs    Data Signaling Rate Selector
                   srts   Secondary Request to Send
                   scts   Secondary Clear to Send
                   sdcd   Secondary Received Line Signal Detector
               "
           REFERENCE
               "EIA Standard RS-232-C, August 1969."
           ::= { rs232InSigEntry 2 }

       rs232InSigState OBJECT-TYPE
           SYNTAX INTEGER { none(1), on(2), off(3) }
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The current signal state."
           ::= { rs232InSigEntry 3 }

       rs232InSigChanges OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The number of times the signal has changed from
               'on' to 'off' or from 'off' to 'on'."
           ::= { rs232InSigEntry 4 }


       -- the Output Signal table

       rs232OutSigTable OBJECT-TYPE
           SYNTAX SEQUENCE OF Rs232OutSigEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "A list of port output control signal entries."
           ::= { rs232 6 }

       rs232OutSigEntry OBJECT-TYPE
           SYNTAX Rs232OutSigEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "Output control signal status for a hardware port."
           INDEX { rs232OutSigPortIndex, rs232OutSigName }
           ::= { rs232OutSigTable 1 }





       Rs232OutSigEntry ::=
           SEQUENCE {
               rs232OutSigPortIndex
                   INTEGER,
               rs232OutSigName
                   INTEGER,
               rs232OutSigState
                   INTEGER,
               rs232OutSigChanges
                   Counter
           }

       rs232OutSigPortIndex OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The value of rs232PortIndex for the port to which
               this entry belongs."
           ::= { rs232OutSigEntry 1 }

       rs232OutSigName OBJECT-TYPE
           SYNTAX INTEGER { rts(1), cts(2), dsr(3), dtr(4), ri(5),
                            dcd(6), sq(7), srs(8), srts(9),
                            scts(10), sdcd(11) }
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "Identification of a hardware signal, as follows:

                   rts    Request to Send
                   cts    Clear to Send
                   dsr    Data Set Ready
                   dtr    Data Terminal Ready
                   ri     Ring Indicator
                   dcd    Received Line Signal Detector
                   sq     Signal Quality Detector
                   srs    Data Signaling Rate Selector
                   srts   Secondary Request to Send
                   scts   Secondary Clear to Send
                   sdcd   Secondary Received Line Signal Detector
               "
           REFERENCE
               "EIA Standard RS-232-C, August 1969."
           ::= { rs232OutSigEntry 2 }








       rs232OutSigState OBJECT-TYPE
           SYNTAX INTEGER { none(1), on(2), off(3) }
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The current signal state."
           ::= { rs232OutSigEntry 3 }

       rs232OutSigChanges OBJECT-TYPE
           SYNTAX Counter
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The number of times the signal has changed from
               'on' to 'off' or from 'off' to 'on'."
           ::= { rs232OutSigEntry 4 }

       END


